**3GPP TSG-CT WG4 Meeting #130C4-253589**

**Göteborg, Sweden; 25th – 29th August 2025**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.2* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  |  | **CR** |  | **rev** |  | **Current version:** |  |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **X** |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | 29.175 Rel-19 API version and External doc update | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** |  | | | | | | | | | |
| ***Source to TSG:*** | CT4 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | TEI19 | | | | |  | ***Date:*** | | |  |
|  |  | | | |  | |  | | |  |
| ***Category:*** |  |  | | | | | ***Release:*** | | | -19 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-16 (Release 16) Rel-17 (Release 17) Rel-18 (Release 18) Rel-19 (Release 19)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | The following CRs modifying the Nimsas\_Nimsas\_ImsSessionManagement API have been agreed and version number of the corresponding OpenAPI file needs to be incremented following the rules in TS29.501, subclause 4.3.1.   * TS29.175 CR#0092: backwards compatible correction. * TS29.510 CR#1226: backwards compatible features.   The following CRs modifying the Nimsas\_MediaControl API have been agreed and version number of the corresponding OpenAPI file needs to be incremented following the rules in TS29.501, subclause 4.3.1.   * TS29.175 CR#0073: backwards compatible correction. * TS29.175 CR#0083: backwards compatible features. * TS29.510 CR#1226: backwards compatible features. * TS29.175 CR#0091: backwards compatible features.   The following CRs modifying the Nimsas\_SessionEventControl API have been agreed and version number of the corresponding OpenAPI file needs to be incremented following the rules in TS29.501, subclause 4.3.1.   * TS29.510 CR#1226: backwards compatible features. * TS29.175 CR#0091: backwards compatible features.   The following CRs modifying the Nimsas\_ImsEE API have been agreed and version number of the corresponding OpenAPI file needs to be incremented following the rules in TS29.501, subclause 4.3.1.   * TS29.571 CR#0666: backwards compatible correction. * TS29.510 CR#1226: backwards compatible features.   externalDocs needs also to be updated to refer to the new version of the specification. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | The Nimsas\_SessionEventControl API version number is incremented to 1.1.0-alpha.4.  externalDocs updated to V19.3.0.  The Nimsas\_MediaControl API version number is incremented to 1.1.1-alpha.3.  externalDocs updated to V19.3.0.  The Nimsas\_ImsSessionManagement API version number is incremented to 1.0.0-alpha.2.  externalDocs updated to V19.3.0.  The Nimsas\_ImsEE API version number is incremented to 1.0.0-alpha.2.  externalDocs updated to V19.3.0. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | Incorrect API version number and externalDocs field. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | A.2, A.3, A.4, A.5 | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  | **X** | Other core specifications | | | | TS/TR ... CR ... | | |
| ***affected:*** | |  | **X** | Test specifications | | | | TS/TR ... CR ... | | |
| ***(show related CRs)*** | |  | **X** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | |  | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | |  | | | | | | | | |

\* \* \* First Change \* \* \* \*

# A.2 Nimsas\_SessionEventControl API

openapi: 3.0.0

info:

title: 'IMS AS SessionEventControl Service'

version: 1.1.0-alpha.4

description: |

Nimsas\_SessionEventControl Service.

© 2025, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

All rights reserved.

externalDocs:

description: >

3GPP TS 29.175 V19.3.0; IP Multimedia Subsystem; IP Multimedia Subsystem (IMS) Application

Server (AS) Services; Stage 3

url: 'https://www.3gpp.org/ftp/Specs/archive/29\_series/29.175/'

servers:

- url: '{apiRoot}/nimsas-sec/v1'

variables:

apiRoot:

default: https://example.com

description: apiRoot as defined in clause 4.4 of 3GPP TS 29.501

\* \* \* Next Change \* \* \* \*

# A.3 Nimsas\_MediaControl API

openapi: 3.0.0

info:

title: 'IMS AS MediaControl Service'

version: 1.1.1-alpha.3

description: |

Nimsas\_MediaControl Service.

© 2025, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

All rights reserved.

externalDocs:

description: >

3GPP TS 29.175 V19.3.0; IP Multimedia Subsystem; IP Multimedia Subsystem (IMS) Application

Server (AS) Services; Stage 3

url: 'https://www.3gpp.org/ftp/Specs/archive/29\_series/29.175'

servers:

- url: '{apiRoot}/nimsas-mc/v1'

variables:

apiRoot:

default: https://example.com

description: apiRoot as defined in clause 4.4 of 3GPP TS 29.501

\* \* \* Next Change \* \* \* \*

# A.4 Nimsas\_ImsSessionManagement API

openapi: 3.0.0  
  
info:  
 title: 'IMS AS ImsSessionManagement Service'  
 version: 1.0.0-alpha.2  
 description: |  
 Nimsas\_ImsSessionManagement Service.   
 © 2025, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).   
 All rights reserved.  
  
externalDocs:  
 description: >  
 3GPP TS 29.175 V19.3.0; IP Multimedia Subsystem; IP Multimedia Subsystem (IMS) Application  
 Server (AS) Services; Stage 3  
 url: 'https://www.3gpp.org/ftp/Specs/archive/29\_series/29.175'  
  
servers:  
 - url: '{apiRoot}/nimsas-ism/v1'  
 variables:  
 apiRoot:  
 default: https://example.com  
 description: apiRoot as defined in clause 4.4 of 3GPP TS 29.501

\* \* \* Next Change \* \* \* \*

# A.5 Nimsas\_ImsEE API

openapi: 3.0.0

info:

title: 'IMS AS ImsEventExposure Service'

version: 1.0.0-alpha.2

description: |

Nimsas\_ImsEE Service.

© 2025, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

All rights reserved.

externalDocs:

description: >

3GPP TS 29.175 V19.3.0; IP Multimedia Subsystem; IP Multimedia Subsystem (IMS) Application

Server (AS) Services; Stage 3

url: 'https://www.3gpp.org/ftp/Specs/archive/29\_series/29.175'

servers:

- url: '{apiRoot}/nimsas-ee/v1'

variables:

apiRoot:

default: https://example.com

description: apiRoot as defined in clause 4.4 of 3GPP TS 29.501

\* \* \* End of Changes \* \* \* \*