**3GPP TSG-CT WG4 Meeting #130C4-253589**

**Göteborg, Sweden; 25th – 29th August 2025**

|  |
| --- |
| *CR-Form-v12.2* |
| **CHANGE REQUEST** |
|  |
|  |  | **CR** |  | **rev** |  | **Current version:** |  |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **X** |

|  |
| --- |
|  |
| ***Title:***  | 29.175 Rel-19 API version and External doc update |
|  |  |
| ***Source to WG:*** |  |
| ***Source to TSG:*** | CT4 |
|  |  |
| ***Work item code:*** | TEI19 |  | ***Date:*** |  |
|  |  |  |  |  |
| ***Category:*** |  |  | ***Release:*** | -19 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)Rel-19 (Release 19)* |
|  |  |
| ***Reason for change:*** | The following CRs modifying the Nimsas\_Nimsas\_ImsSessionManagement API have been agreed and version number of the corresponding OpenAPI file needs to be incremented following the rules in TS29.501, subclause 4.3.1.* TS29.175 CR#0092: backwards compatible correction.
* TS29.510 CR#1226: backwards compatible features.

The following CRs modifying the Nimsas\_MediaControl API have been agreed and version number of the corresponding OpenAPI file needs to be incremented following the rules in TS29.501, subclause 4.3.1.* TS29.175 CR#0073: backwards compatible correction.
* TS29.175 CR#0083: backwards compatible features.
* TS29.510 CR#1226: backwards compatible features.
* TS29.175 CR#0091: backwards compatible features.

The following CRs modifying the Nimsas\_SessionEventControl API have been agreed and version number of the corresponding OpenAPI file needs to be incremented following the rules in TS29.501, subclause 4.3.1.* TS29.510 CR#1226: backwards compatible features.
* TS29.175 CR#0091: backwards compatible features.

The following CRs modifying the Nimsas\_ImsEE API have been agreed and version number of the corresponding OpenAPI file needs to be incremented following the rules in TS29.501, subclause 4.3.1.* TS29.571 CR#0666: backwards compatible correction.
* TS29.510 CR#1226: backwards compatible features.

externalDocs needs also to be updated to refer to the new version of the specification. |
|  |  |
| ***Summary of change:*** | The Nimsas\_SessionEventControl API version number is incremented to 1.1.0-alpha.4.externalDocs updated to V19.3.0.The Nimsas\_MediaControl API version number is incremented to 1.1.1-alpha.3.externalDocs updated to V19.3.0.The Nimsas\_ImsSessionManagement API version number is incremented to 1.0.0-alpha.2.externalDocs updated to V19.3.0.The Nimsas\_ImsEE API version number is incremented to 1.0.0-alpha.2.externalDocs updated to V19.3.0. |
|  |  |
| ***Consequences if not approved:*** | Incorrect API version number and externalDocs field. |
|  |  |
| ***Clauses affected:*** | A.2, A.3, A.4, A.5 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

\* \* \* First Change \* \* \* \*

# A.2 Nimsas\_SessionEventControl API

openapi: 3.0.0

info:

 title: 'IMS AS SessionEventControl Service'

 version: 1.1.0-alpha.4

 description: |

 Nimsas\_SessionEventControl Service.

 © 2025, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

 All rights reserved.

externalDocs:

 description: >

 3GPP TS 29.175 V19.3.0; IP Multimedia Subsystem; IP Multimedia Subsystem (IMS) Application

 Server (AS) Services; Stage 3

 url: 'https://www.3gpp.org/ftp/Specs/archive/29\_series/29.175/'

servers:

 - url: '{apiRoot}/nimsas-sec/v1'

 variables:

 apiRoot:

 default: https://example.com

 description: apiRoot as defined in clause 4.4 of 3GPP TS 29.501

\* \* \* Next Change \* \* \* \*

# A.3 Nimsas\_MediaControl API

openapi: 3.0.0

info:

 title: 'IMS AS MediaControl Service'

 version: 1.1.1-alpha.3

 description: |

 Nimsas\_MediaControl Service.

 © 2025, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

 All rights reserved.

externalDocs:

 description: >

 3GPP TS 29.175 V19.3.0; IP Multimedia Subsystem; IP Multimedia Subsystem (IMS) Application

 Server (AS) Services; Stage 3

 url: 'https://www.3gpp.org/ftp/Specs/archive/29\_series/29.175'

servers:

 - url: '{apiRoot}/nimsas-mc/v1'

 variables:

 apiRoot:

 default: https://example.com

 description: apiRoot as defined in clause 4.4 of 3GPP TS 29.501

\* \* \* Next Change \* \* \* \*

# A.4 Nimsas\_ImsSessionManagement API

openapi: 3.0.0

info:
 title: 'IMS AS ImsSessionManagement Service'
 version: 1.0.0-alpha.2
 description: |
 Nimsas\_ImsSessionManagement Service.
 © 2025, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).
 All rights reserved.

externalDocs:
 description: >
 3GPP TS 29.175 V19.3.0; IP Multimedia Subsystem; IP Multimedia Subsystem (IMS) Application
 Server (AS) Services; Stage 3
 url: 'https://www.3gpp.org/ftp/Specs/archive/29\_series/29.175'

servers:
 - url: '{apiRoot}/nimsas-ism/v1'
 variables:
 apiRoot:
 default: https://example.com
 description: apiRoot as defined in clause 4.4 of 3GPP TS 29.501

\* \* \* Next Change \* \* \* \*

# A.5 Nimsas\_ImsEE API

openapi: 3.0.0

info:

 title: 'IMS AS ImsEventExposure Service'

 version: 1.0.0-alpha.2

 description: |

 Nimsas\_ImsEE Service.

 © 2025, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

 All rights reserved.

externalDocs:

 description: >

 3GPP TS 29.175 V19.3.0; IP Multimedia Subsystem; IP Multimedia Subsystem (IMS) Application

 Server (AS) Services; Stage 3

 url: 'https://www.3gpp.org/ftp/Specs/archive/29\_series/29.175'

servers:

 - url: '{apiRoot}/nimsas-ee/v1'

 variables:

 apiRoot:

 default: https://example.com

 description: apiRoot as defined in clause 4.4 of 3GPP TS 29.501

\* \* \* End of Changes \* \* \* \*