UECap Comments file

Template:

# O002

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| RIL Id | WI | Class | Title | Tdoc | Delegate | Misc | File version | Status |
| O002 | UECap, for NR\_ENDC\_RF\_Ph4 | 2 | Merging of 46-4, 46-5 | R2-25xxxxx | OPPO (Qianxi) |  | V002 | ToDo |

**[Description]**: Clearly, 46-4 is a subset of 46-5, in the sense that 46-4 supports a smaller number of MPR reduction combination compared to 46-5. So, there is no need for UE to simultaneously report the support of 46-4 and 46-5.

**[Proposed Change]**: R2 implement 46-4 and 46-5 as two enumerate values of a same capability. If R2 cannot converge, ask R4 whether there is a reason that UE has to report the support of both 46-4 and 46-5 other than 46-5 only using a LS.

**[Comments]**:

# E038

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| RIL Id | WI | Class | Title | Tdoc | Delegate | Misc | File version | Status |
| E037 | LPWUS | 1 or 2 | Clarify the *minimumTimeGap-r19* capability signalling | R2-25xxx | Ericsson (Martin) |  | V006 | ToDo |

**[Description]**:

RAN1 agreed:

Agreement

The 3 capabilities for UE’s wake-up delay in idle/inactive mode are defined as follows:

|  |  |  |  |
| --- | --- | --- | --- |
| SSB periodicity (ms) | Wake-up delay (ms)  UE capability 1 | Wake-up delay (ms)  UE capability 2 | Wake-up delay (ms)  UE capability 3 |
| 5/10/20 | 70 | 500 | 900 |
| 40 | 130 | 600 | 1000 |
| 80 | 250 | 800 | 1200 |
| 160 | 490 | 1200 | 1600 |

The MEGA 38.306 and 38.331 include:

- *minimumTimeGap-r19* indicates the minimum time gap between LP-WUS reception and UE to start PDCCH monitoring.

LPWUS-SupportedBandInfo-r19 ::= SEQUENCE {

supportedBandIndicator-r19 FreqBandIndicatorNR,

-- R1 62-1: LP-WUS operation in IDLE/INACTIVE mode based on OOK signal

lpwus-OOK-r19 ENUMERATED {supported} OPTIONAL,

-- R1 62-1a: LP-WUS operation in IDLE/INACTIVE mode based on OFDM overlaid sequence

lpwus-OFDM-r19 ENUMERATED {supported} OPTIONAL,

-- R1 62-1b: LP-SS based RRM measurement in IDLE/INACTIVE mode when LP-SS overlaid sequence is configured

lpwus-LP-SS-r19 ENUMERATED {supported} OPTIONAL,

minimumTimeGap-r19 SEQUENCE {

wakeUpDelay-SSB-Periodicity-LessThan20ms-r19 ENUMERATED {ms70, ms500, ms900} OPTIONAL,

wakeUpDelay-SSB-Periodicity-40ms-r19 ENUMERATED {ms130, ms600, ms1000} OPTIONAL,

wakeUpDelay-SSB-Periodicity-80ms-r19 ENUMERATED {ms250, ms800, ms1200} OPTIONAL,

wakeUpDelay-SSB-Periodicity-160ms-r19 ENUMERATED {ms490, ms1200, ms1600} OPTIONAL

}

}

It is not clear whether the UE is required to send at least one wake-up delay for one SSB periodicity, or a wake-up delay for each possible SSB periodicity. Furthermore, what is the implication when the UE did not signal a wake-up delay for the configured SSB periodicity in the cell?

**[Proposed Change]**:

Based on offline discussion a proposal will be provided in a Tdoc.

**[Comments]**:

Instructions:

1. Copy the template RIL comments fields above (including the Heading Xnnn)
2. Paste the RIL comments fields at its position while **respecting the order of the RILs in the Review file (i.e. keep the order of the spec).**
3. Fill in the fields, see R19 ASN.1 Guideline.
4. Companies may comment whether they agree or disagree.
5. Can copy spec text and use Word “Track changes”, etc.
6. Do not delete text added by other companies.