**UECap Review file**

**3GPP TSG- Meeting #131**

**Bengaluru, IN, - Aug, 2025**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.3* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  |  | **CR** | **5403** | **rev** | **1** | **Current version:** | **6.0** |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network | **X** | Core Network |  |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | Introduction of Rel-19 UE capability, including [TN32HARQ], [Pos\_SRSHop], [SRTrig\_SSSGSwitch], [SRSCS\_ULTxSwitch], [SimCSI\_count], [SimCSI\_countNES], [TxSwitch\_R19] | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | Xiaomi | | | | | | | | | |
| ***Source to TSG:*** |  | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | NR\_AIML\_air, NR\_Mob\_Ph4, NR-NR\_MIMO\_Ph5, NR\_duplex\_evo, Netw\_Energy\_NR\_enh, NR\_LPWUS, NR\_XR\_Ph3, NR\_NTN\_Ph3, NR\_ENDC\_RF\_Ph4, NR\_ATG\_enh, NR\_RRM\_Ph5, NonCol\_intraB\_ENDC\_NR\_CA\_Ph2, NR\_SL\_relay\_multihop, NR\_ENDC\_SON\_MDT\_Ph4, TEI19 | | | | |  | ***Date:*** | | | 09 |
|  |  | | | |  | |  | | |  |
| ***Category:*** | **B** |  | | | | | ***Release:*** | | | Rel-19 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-17 (Release 17) Rel-18 (Release 18) Rel-19 (Release 19)  Rel-20 (Release 20)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | Capture Release-19 UE capabilities  All the entries that are not concluded in the feature lists from RAN1/4 feature lists and those that are highlighted (or has pre-requisite with features that are highlighted) in R1 feature list are not considered as part of this CR. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | New Release-19 capabilities from RAN1/4 are added based on the latest RAN1/4 feature lists.   * R1-2506627 Updated RAN1 UE features list for Rel-19 NR after RAN1 #122 * R4-2511883 Rel-19 RAN4 UE feature list for NR (version 2)   The following RAN2 endorsed CRs are included:   * R2-2506525 Introduction of AI air UE capability * R2-2506223 Introduction of UE capability for network energy saving enhancement in TS 38.331 * R2-2506227 Draft 331 running CR for UE capability for Mob Ph4 * R2-2505137 Draft 38.331 CR for Rel-19 XR UE capabilities * R2-2506531 Draft CR for Rel-19 NR NTN UE capabilities * R2-2506377 Introduction of SONMDT UE Capabilities * R2-2506330 Introduction of multi-hop sidelink relay capability * R2-2506009 Introduction of signaling support for intra-band non-collocated EN-DC/NR-CA deployment Phase 2: new receiver type(s) * R2-2506590 Introduction of 3Tx UL switching [TxSwitch\_R19] | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | Rel-19 UE capabilities will not be captured in specifications | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | 6.3.3, 11 | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | | **X** |  | Other core specifications | | | | TS/TR 38.306 CR 1321 | | |
| ***affected:*** | |  | **X** | Test specifications | | | | TS/TR ... CR ... | | |
| ***(show related CRs)*** | |  | **X** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | |  | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | |  | | | | | | | | |

START OF CHANGE

# 6 Protocol data units, formats and parameters (ASN.1)

## 6.3 RRC information elements

### 6.3.3 UE capability information elements

#### – *AccessStratumRelease*

The IE *AccessStratumRelease* indicates the release supported by the UE.

*AccessStratumRelease* information element

-- ASN1START

-- TAG-ACCESSSTRATUMRELEASE-START

AccessStratumRelease ::= ENUMERATED {

rel15, rel16, rel17, rel18, rel19, spare3, spare2, spare1, ... }

-- TAG-ACCESSSTRATUMRELEASE-STOP

-- ASN1STOP

#### – *AerialParameters*

The IE *AerialParameters* is used to convey the capabilities supported by the UE for aerial operation.

*AerialParameters* information element

-- ASN1START

-- TAG-AERIALPARAMETERS-START

AerialParameters-r18 ::= SEQUENCE {

-- Support of Aerial UE features

aerialUE-Capability-r18 ENUMERATED {supported} OPTIONAL,

-- Support of altitude measurement and event H1/H2-triggered reporting

altitudeMeas-r18 ENUMERATED {supported} OPTIONAL,

-- Support of altitude based measurement configuration of SSB-ToMeasure

altitudeBasedSSB-ToMeasure-r18 ENUMERATED {supported} OPTIONAL,

-- Support of events A3H1, A3H2, A4H1, A4H2, A5H1, A5H2

eventAxHy-r18 ENUMERATED {supported} OPTIONAL,

-- Support of flight path reporting

flightPathReporting-r18 ENUMERATED {supported} OPTIONAL,

-- Support of flight path availability indication via UAI

flightPathAvailabilityIndicationUAI-r18 ENUMERATED {supported} OPTIONAL,

-- Support of numberOfTriggeringCells for eventA3, eventA4, and eventA5, and additionally, if the UE supports eventAxHy-r18,

-- support of numberOfTriggeringCells for eventA3H1, eventA3H2, eventA4H1, eventA4H2, eventA5H1, and eventA5H2

multipleCellsMeasExtension-r18 ENUMERATED {supported} OPTIONAL,

-- Support of handling aerial-specific Ns value(s) and Pmax list broadcasted by the cell

nr-NS-PmaxListAerial-r18 ENUMERATED {supported} OPTIONAL,

-- Support of reporting only the measurement report corresponding to the event with the smallest value between the

-- altitude of the UAV and the altitude threshold for which the altitude-related entering condition e.g. A3H1-2 is satisfied, when

-- multiple events of the same type (Hx or AxHy) for the same MO (for AxHy) are triggered simultaneously.

simulMultiTriggerSingleMeasReport-r18 ENUMERATED {supported} OPTIONAL,

-- Support of A2X service(s) using PC5 Sidelink and dedicated resource pool for A2X service(s)

sl-A2X-Service-r18 ENUMERATED {brid, daa, bridAndDAA} OPTIONAL,

...

}

-- TAG-AERIALPARAMETERS-STOP

-- ASN1STOP

#### – *AIML-Parameters*

The IE *AIML-Parameters* is used to convey the capabilities supported by the UE for AI/ML beam management and AI/ML CSI prediction.

*AIML-Parameters* information element

-- ASN1START

-- TAG-AIML-PARAMETERS-START

AIML-Parameters-r19 ::= SEQUENCE {

applicabilityReportingCSI-r19 ENUMERATED {supported} OPTIONAL,

applicabilityReportingOther-r19 ENUMERATED {supported} OPTIONAL,

loggedDataCollection-r19 ENUMERATED {supported} OPTIONAL,

eventBasedLoggedDataCollection-r19 ENUMERATED {supported} OPTIONAL,

dataThresholdAvailabilityIndication-r19 ENUMERATED {supported} OPTIONAL

}

-- TAG-AIML-PARAMETERS-STOP

-- ASN1STOP

#### – *AppLayerMeasParameters*

The IE *AppLayerMeasParameters* is used to convey the capabilities supported by the UE for application layer measurements.

*AppLayerMeasParameters* information element

-- ASN1START

-- TAG-APPLAYERMEASPARAMETERS-START

AppLayerMeasParameters-r17 ::= SEQUENCE {

qoe-Streaming-MeasReport-r17 ENUMERATED {supported} OPTIONAL,

qoe-MTSI-MeasReport-r17 ENUMERATED {supported} OPTIONAL,

qoe-VR-MeasReport-r17 ENUMERATED {supported} OPTIONAL,

ran-VisibleQoE-Streaming-MeasReport-r17 ENUMERATED {supported} OPTIONAL,

ran-VisibleQoE-VR-MeasReport-r17 ENUMERATED {supported} OPTIONAL,

ul-MeasurementReportAppLayer-Seg-r17 ENUMERATED {supported} OPTIONAL,

...,

[[

qoe-IdleInactiveMeasReport-r18 ENUMERATED {supported} OPTIONAL,

qoe-NRDC-MeasReport-r18 ENUMERATED {supported} OPTIONAL,

qoe-AdditionalMemoryMeasReport-r18 ENUMERATED {kB128, kB256, kB512, kB1024} OPTIONAL,

qoe-PriorityBasedDiscarding-r18 ENUMERATED {supported} OPTIONAL,

srb5-r18 ENUMERATED {supported} OPTIONAL

]]

}

-- TAG-APPLAYERMEASPARAMETERS-STOP

-- ASN1STOP

#### – *BandCombinationList*

The IE *BandCombinationList* contains a list of NR CA, NR non-CA and/or MR-DC band combinations (also including DL only or UL only band).

*BandCombinationList* information element

-- ASN1START

-- TAG-BANDCOMBINATIONLIST-START

BandCombinationList ::= SEQUENCE (SIZE (1..maxBandComb)) OF BandCombination

BandCombinationList-v1540 ::= SEQUENCE (SIZE (1..maxBandComb)) OF BandCombination-v1540

BandCombinationList-v1550 ::= SEQUENCE (SIZE (1..maxBandComb)) OF BandCombination-v1550

BandCombinationList-v1560 ::= SEQUENCE (SIZE (1..maxBandComb)) OF BandCombination-v1560

BandCombinationList-v1570 ::= SEQUENCE (SIZE (1..maxBandComb)) OF BandCombination-v1570

BandCombinationList-v1580 ::= SEQUENCE (SIZE (1..maxBandComb)) OF BandCombination-v1580

BandCombinationList-v1590 ::= SEQUENCE (SIZE (1..maxBandComb)) OF BandCombination-v1590

BandCombinationList-v15g0 ::= SEQUENCE (SIZE (1..maxBandComb)) OF BandCombination-v15g0

BandCombinationList-v15n0 ::= SEQUENCE (SIZE (1..maxBandComb)) OF BandCombination-v15n0

BandCombinationList-v1610 ::= SEQUENCE (SIZE (1..maxBandComb)) OF BandCombination-v1610

BandCombinationList-v1630 ::= SEQUENCE (SIZE (1..maxBandComb)) OF BandCombination-v1630

BandCombinationList-v1640 ::= SEQUENCE (SIZE (1..maxBandComb)) OF BandCombination-v1640

BandCombinationList-v1650 ::= SEQUENCE (SIZE (1..maxBandComb)) OF BandCombination-v1650

BandCombinationList-v1680 ::= SEQUENCE (SIZE (1..maxBandComb)) OF BandCombination-v1680

BandCombinationList-v1690 ::= SEQUENCE (SIZE (1..maxBandComb)) OF BandCombination-v1690

BandCombinationList-v16a0 ::= SEQUENCE (SIZE (1..maxBandComb)) OF BandCombination-v16a0

BandCombinationList-v16j0 ::= SEQUENCE (SIZE (1..maxBandComb)) OF BandCombination-v16j0

BandCombinationList-v1700 ::= SEQUENCE (SIZE (1..maxBandComb)) OF BandCombination-v1700

BandCombinationList-v1720 ::= SEQUENCE (SIZE (1..maxBandComb)) OF BandCombination-v1720

BandCombinationList-v1730 ::= SEQUENCE (SIZE (1..maxBandComb)) OF BandCombination-v1730

BandCombinationList-v1740 ::= SEQUENCE (SIZE (1..maxBandComb)) OF BandCombination-v1740

BandCombinationList-v1760 ::= SEQUENCE (SIZE (1..maxBandComb)) OF BandCombination-v1760

BandCombinationList-v1770 ::= SEQUENCE (SIZE (1..maxBandComb)) OF BandCombination-v1770

BandCombinationList-v1780 ::= SEQUENCE (SIZE (1..maxBandComb)) OF BandCombination-v1780

BandCombinationList-v1790 ::= SEQUENCE (SIZE (1..maxBandComb)) OF BandCombination-v1790

BandCombinationList-v17b0 ::= SEQUENCE (SIZE (1..maxBandComb)) OF BandCombination-v17b0

BandCombinationList-v1800 ::= SEQUENCE (SIZE (1..maxBandComb)) OF BandCombination-v1800

BandCombinationList-v1830 ::= SEQUENCE (SIZE (1..maxBandComb)) OF BandCombination-v1830

BandCombinationList-v1840 ::= SEQUENCE (SIZE (1..maxBandComb)) OF BandCombination-v1840

BandCombinationList-v1860 ::= SEQUENCE (SIZE (1..maxBandComb)) OF BandCombination-v1860

BandCombinationList-v1900 ::= SEQUENCE (SIZE (1..maxBandComb)) OF BandCombination-v1900

BandCombinationList-UplinkTxSwitch-r16 ::= SEQUENCE (SIZE (1..maxBandComb)) OF BandCombination-UplinkTxSwitch-r16

BandCombinationList-UplinkTxSwitch-v1630 ::= SEQUENCE (SIZE (1..maxBandComb)) OF BandCombination-UplinkTxSwitch-v1630

BandCombinationList-UplinkTxSwitch-v1640 ::= SEQUENCE (SIZE (1..maxBandComb)) OF BandCombination-UplinkTxSwitch-v1640

BandCombinationList-UplinkTxSwitch-v1650 ::= SEQUENCE (SIZE (1..maxBandComb)) OF BandCombination-UplinkTxSwitch-v1650

BandCombinationList-UplinkTxSwitch-v1670 ::= SEQUENCE (SIZE (1..maxBandComb)) OF BandCombination-UplinkTxSwitch-v1670

BandCombinationList-UplinkTxSwitch-v1690 ::= SEQUENCE (SIZE (1..maxBandComb)) OF BandCombination-UplinkTxSwitch-v1690

BandCombinationList-UplinkTxSwitch-v16a0 ::= SEQUENCE (SIZE (1..maxBandComb)) OF BandCombination-UplinkTxSwitch-v16a0

BandCombinationList-UplinkTxSwitch-v16e0 ::= SEQUENCE (SIZE (1..maxBandComb)) OF BandCombination-UplinkTxSwitch-v16e0

BandCombinationList-UplinkTxSwitch-v16j0 ::= SEQUENCE (SIZE (1..maxBandComb)) OF BandCombination-UplinkTxSwitch-v16j0

BandCombinationList-UplinkTxSwitch-v1700 ::= SEQUENCE (SIZE (1..maxBandComb)) OF BandCombination-UplinkTxSwitch-v1700

BandCombinationList-UplinkTxSwitch-v1720 ::= SEQUENCE (SIZE (1..maxBandComb)) OF BandCombination-UplinkTxSwitch-v1720

BandCombinationList-UplinkTxSwitch-v1730 ::= SEQUENCE (SIZE (1..maxBandComb)) OF BandCombination-UplinkTxSwitch-v1730

BandCombinationList-UplinkTxSwitch-v1740 ::= SEQUENCE (SIZE (1..maxBandComb)) OF BandCombination-UplinkTxSwitch-v1740

BandCombinationList-UplinkTxSwitch-v1760 ::= SEQUENCE (SIZE (1..maxBandComb)) OF BandCombination-UplinkTxSwitch-v1760

BandCombinationList-UplinkTxSwitch-v1770 ::= SEQUENCE (SIZE (1..maxBandComb)) OF BandCombination-UplinkTxSwitch-v1770

BandCombinationList-UplinkTxSwitch-v1780 ::= SEQUENCE (SIZE (1..maxBandComb)) OF BandCombination-UplinkTxSwitch-v1780

BandCombinationList-UplinkTxSwitch-v1790 ::= SEQUENCE (SIZE (1..maxBandComb)) OF BandCombination-UplinkTxSwitch-v1790

BandCombinationList-UplinkTxSwitch-v17b0 ::= SEQUENCE (SIZE (1..maxBandComb)) OF BandCombination-UplinkTxSwitch-v17b0

BandCombinationList-UplinkTxSwitch-v1800 ::= SEQUENCE (SIZE (1..maxBandComb)) OF BandCombination-UplinkTxSwitch-v1800

BandCombinationList-UplinkTxSwitch-v1830 ::= SEQUENCE (SIZE (1..maxBandComb)) OF BandCombination-UplinkTxSwitch-v1830

BandCombinationList-UplinkTxSwitch-v1840 ::= SEQUENCE (SIZE (1..maxBandComb)) OF BandCombination-UplinkTxSwitch-v1840

BandCombinationList-UplinkTxSwitch-v1860 ::= SEQUENCE (SIZE (1..maxBandComb)) OF BandCombination-UplinkTxSwitch-v1860

BandCombinationList-UplinkTxSwitch-v1900 ::= SEQUENCE (SIZE (1..maxBandComb)) OF BandCombination-UplinkTxSwitch-v1900

BandCombination ::= SEQUENCE {

bandList SEQUENCE (SIZE (1..maxSimultaneousBands)) OF BandParameters,

featureSetCombination FeatureSetCombinationId,

ca-ParametersEUTRA CA-ParametersEUTRA OPTIONAL,

ca-ParametersNR CA-ParametersNR OPTIONAL,

mrdc-Parameters MRDC-Parameters OPTIONAL,

supportedBandwidthCombinationSet BIT STRING (SIZE (1..32)) OPTIONAL,

powerClass-v1530 ENUMERATED {pc2} OPTIONAL

}

BandCombination-v1540::= SEQUENCE {

bandList-v1540 SEQUENCE (SIZE (1..maxSimultaneousBands)) OF BandParameters-v1540,

ca-ParametersNR-v1540 CA-ParametersNR-v1540 OPTIONAL

}

BandCombination-v1550 ::= SEQUENCE {

ca-ParametersNR-v1550 CA-ParametersNR-v1550

}

BandCombination-v1560::= SEQUENCE {

ne-DC-BC ENUMERATED {supported} OPTIONAL,

ca-ParametersNRDC CA-ParametersNRDC OPTIONAL,

ca-ParametersEUTRA-v1560 CA-ParametersEUTRA-v1560 OPTIONAL,

ca-ParametersNR-v1560 CA-ParametersNR-v1560 OPTIONAL

}

BandCombination-v1570 ::= SEQUENCE {

ca-ParametersEUTRA-v1570 CA-ParametersEUTRA-v1570

}

BandCombination-v1580 ::= SEQUENCE {

mrdc-Parameters-v1580 MRDC-Parameters-v1580

}

BandCombination-v1590::= SEQUENCE {

supportedBandwidthCombinationSetIntraENDC BIT STRING (SIZE (1..32)) OPTIONAL,

mrdc-Parameters-v1590 MRDC-Parameters-v1590

}

BandCombination-v15g0::= SEQUENCE {

ca-ParametersNR-v15g0 CA-ParametersNR-v15g0 OPTIONAL,

ca-ParametersNRDC-v15g0 CA-ParametersNRDC-v15g0 OPTIONAL,

mrdc-Parameters-v15g0 MRDC-Parameters-v15g0 OPTIONAL

}

BandCombination-v15n0::= SEQUENCE {

mrdc-Parameters-v15n0 MRDC-Parameters-v15n0

}

BandCombination-v1610 ::= SEQUENCE {

bandList-v1610 SEQUENCE (SIZE (1..maxSimultaneousBands)) OF BandParameters-v1610 OPTIONAL,

ca-ParametersNR-v1610 CA-ParametersNR-v1610 OPTIONAL,

ca-ParametersNRDC-v1610 CA-ParametersNRDC-v1610 OPTIONAL,

powerClass-v1610 ENUMERATED {pc1dot5} OPTIONAL,

powerClassNRPart-r16 ENUMERATED {pc1, pc2, pc3, pc5} OPTIONAL,

featureSetCombinationDAPS-r16 FeatureSetCombinationId OPTIONAL,

mrdc-Parameters-v1620 MRDC-Parameters-v1620 OPTIONAL

}

BandCombination-v1630 ::= SEQUENCE {

ca-ParametersNR-v1630 CA-ParametersNR-v1630 OPTIONAL,

ca-ParametersNRDC-v1630 CA-ParametersNRDC-v1630 OPTIONAL,

mrdc-Parameters-v1630 MRDC-Parameters-v1630 OPTIONAL,

supportedTxBandCombListPerBC-Sidelink-r16 BIT STRING (SIZE (1..maxBandComb)) OPTIONAL,

supportedRxBandCombListPerBC-Sidelink-r16 BIT STRING (SIZE (1..maxBandComb)) OPTIONAL,

scalingFactorTxSidelink-r16 SEQUENCE (SIZE (1..maxBandComb)) OF ScalingFactorSidelink-r16 OPTIONAL,

scalingFactorRxSidelink-r16 SEQUENCE (SIZE (1..maxBandComb)) OF ScalingFactorSidelink-r16 OPTIONAL

}

BandCombination-v1640 ::= SEQUENCE {

ca-ParametersNR-v1640 CA-ParametersNR-v1640 OPTIONAL,

ca-ParametersNRDC-v1640 CA-ParametersNRDC-v1640 OPTIONAL

}

BandCombination-v1650 ::= SEQUENCE {

ca-ParametersNRDC-v1650 CA-ParametersNRDC-v1650 OPTIONAL

}

BandCombination-v1680 ::= SEQUENCE {

intrabandConcurrentOperationPowerClass-r16 SEQUENCE (SIZE (1..maxBandComb)) OF IntraBandPowerClass-r16 OPTIONAL

}

BandCombination-v1690 ::= SEQUENCE {

dummy CA-ParametersNR-v1690 OPTIONAL

}

BandCombination-v16a0 ::= SEQUENCE {

ca-ParametersNR-v16a0 CA-ParametersNR-v16a0 OPTIONAL,

ca-ParametersNRDC-v16a0 CA-ParametersNRDC-v16a0 OPTIONAL

}

BandCombination-v16j0::= SEQUENCE {

ca-ParametersNR-v16j0 CA-ParametersNR-v1690 OPTIONAL,

ca-ParametersNRDC-v16j0 CA-ParametersNRDC-v16j0 OPTIONAL

}

BandCombination-v1700 ::= SEQUENCE {

ca-ParametersNR-v1700 CA-ParametersNR-v1700 OPTIONAL,

ca-ParametersNRDC-v1700 CA-ParametersNRDC-v1700 OPTIONAL,

mrdc-Parameters-v1700 MRDC-Parameters-v1700 OPTIONAL,

bandList-v1710 SEQUENCE (SIZE (1..maxSimultaneousBands)) OF BandParameters-v1710 OPTIONAL,

supportedBandCombListPerBC-SL-RelayDiscovery-r17 BIT STRING (SIZE (1..maxBandComb)) OPTIONAL,

supportedBandCombListPerBC-SL-NonRelayDiscovery-r17 BIT STRING (SIZE (1..maxBandComb)) OPTIONAL

}

BandCombination-v1720 ::= SEQUENCE {

ca-ParametersNR-v1720 CA-ParametersNR-v1720 OPTIONAL,

ca-ParametersNRDC-v1720 CA-ParametersNRDC-v1720 OPTIONAL

}

BandCombination-v1730 ::= SEQUENCE {

ca-ParametersNR-v1730 CA-ParametersNR-v1730 OPTIONAL,

ca-ParametersNRDC-v1730 CA-ParametersNRDC-v1730 OPTIONAL,

bandList-v1730 SEQUENCE (SIZE (1..maxSimultaneousBands)) OF BandParameters-v1730 OPTIONAL

}

BandCombination-v1740 ::= SEQUENCE {

dummy CA-ParametersNR-v1740 OPTIONAL

}

BandCombination-v1760 ::= SEQUENCE {

ca-ParametersNR-v1760 CA-ParametersNR-v1760,

ca-ParametersNRDC-v1760 CA-ParametersNRDC-v1760

}

BandCombination-v1770::= SEQUENCE {

bandList-v1770 SEQUENCE (SIZE (1..maxSimultaneousBands)) OF BandParameters-v1770,

mrdc-Parameters-v1770 MRDC-Parameters-v1770 OPTIONAL,

ca-ParametersNR-v1770 CA-ParametersNR-v1770 OPTIONAL

}

BandCombination-v1780 ::= SEQUENCE {

ca-ParametersNR-v1780 CA-ParametersNR-v1780 OPTIONAL,

ca-ParametersNRDC-v1780 CA-ParametersNRDC-v1780 OPTIONAL,

bandList-v1780 SEQUENCE (SIZE (1..maxSimultaneousBands)) OF BandParameters-v1780 OPTIONAL,

mrdc-Parameters-v1780 MRDC-Parameters-v1770 OPTIONAL

}

BandCombination-v1790 ::= SEQUENCE {

supportedIntraENDC-BandCombinationList-r17 SEQUENCE (SIZE (1..maxNrofIntraEndc-Components-r17)) OF SupportedIntraENDC-BandCombination-r17 OPTIONAL

}

BandCombination-v17b0::= SEQUENCE {

ca-ParametersNR-v17b0 CA-ParametersNR-v1740 OPTIONAL,

ca-ParametersNRDC-v17b0 CA-ParametersNRDC-v17b0 OPTIONAL

}

BandCombination-v1800 ::= SEQUENCE {

ca-ParametersNR-v1800 CA-ParametersNR-v1800 OPTIONAL,

ca-ParametersNRDC-v1800 CA-ParametersNRDC-v1800 OPTIONAL,

supportedBandCombListPerBC-SL-U2U-RelayDiscovery-r18 BIT STRING (SIZE (1..maxBandComb)) OPTIONAL,

bandList-v1810 SEQUENCE (SIZE (1..maxSimultaneousBands)) OF BandParameters-v1810 OPTIONAL

}

BandCombination-v1830 ::= SEQUENCE {

ca-ParametersNR-v1830 CA-ParametersNR-v1830 OPTIONAL,

ca-ParametersNRDC-v1830 CA-ParametersNRDC-v1830 OPTIONAL

}

BandCombination-v1840 ::= SEQUENCE {

mrdc-Parameters-v1840 MRDC-Parameters-v1840 OPTIONAL

}

BandCombination-v1860 ::= SEQUENCE {

ca-ParametersNR-v1860 CA-ParametersNR-v1860 OPTIONAL

}

BandCombination-v1900 ::= SEQUENCE {

ca-ParametersNR-v1900 CA-ParametersNR-v1900 OPTIONAL,

ca-ParametersNRDC-v1900 CA-ParametersNRDC-v1900 OPTIONAL,

mrdc-Parameters-v1900 MRDC-Parameters-v1900 OPTIONAL,

bandList-v1900 SEQUENCE (SIZE (1..maxSimultaneousBands)) OF BandParameters-v1900 OPTIONAL

}

BandCombination-UplinkTxSwitch-r16 ::= SEQUENCE {

bandCombination-r16 BandCombination,

bandCombination-v1540 BandCombination-v1540 OPTIONAL,

bandCombination-v1560 BandCombination-v1560 OPTIONAL,

bandCombination-v1570 BandCombination-v1570 OPTIONAL,

bandCombination-v1580 BandCombination-v1580 OPTIONAL,

bandCombination-v1590 BandCombination-v1590 OPTIONAL,

bandCombination-v1610 BandCombination-v1610 OPTIONAL,

supportedBandPairListNR-r16 SEQUENCE (SIZE (1..maxULTxSwitchingBandPairs)) OF ULTxSwitchingBandPair-r16,

uplinkTxSwitching-OptionSupport-r16 ENUMERATED {switchedUL, dualUL, both} OPTIONAL,

uplinkTxSwitching-PowerBoosting-r16 ENUMERATED {supported} OPTIONAL,

...,

[[

-- R4 16-5 UL-MIMO coherence capability for dynamic Tx switching between 3CC 1Tx-2Tx switching

uplinkTxSwitching-PUSCH-TransCoherence-r16 ENUMERATED {nonCoherent, fullCoherent} OPTIONAL

]]

}

BandCombination-UplinkTxSwitch-v1630 ::= SEQUENCE {

bandCombination-v1630 BandCombination-v1630 OPTIONAL

}

BandCombination-UplinkTxSwitch-v1640 ::= SEQUENCE {

bandCombination-v1640 BandCombination-v1640 OPTIONAL

}

BandCombination-UplinkTxSwitch-v1650 ::= SEQUENCE {

bandCombination-v1650 BandCombination-v1650 OPTIONAL

}

BandCombination-UplinkTxSwitch-v1670 ::= SEQUENCE {

bandCombination-v15g0 BandCombination-v15g0 OPTIONAL

}

BandCombination-UplinkTxSwitch-v1690 ::= SEQUENCE {

bandCombination-v1690 BandCombination-v1690 OPTIONAL

}

BandCombination-UplinkTxSwitch-v16a0 ::= SEQUENCE {

bandCombination-v16a0 BandCombination-v16a0 OPTIONAL

}

BandCombination-UplinkTxSwitch-v16e0 ::= SEQUENCE {

bandCombination-v15n0 BandCombination-v15n0 OPTIONAL

}

BandCombination-UplinkTxSwitch-v16j0 ::= SEQUENCE {

bandCombination-v16j0 BandCombination-v16j0 OPTIONAL

}

BandCombination-UplinkTxSwitch-v1700 ::= SEQUENCE {

bandCombination-v1700 BandCombination-v1700 OPTIONAL,

-- R4 16-1/16-2/16-3 Dynamic Tx switching between 2CC/3CC 2Tx-2Tx/1Tx-2Tx switching

supportedBandPairListNR-v1700 SEQUENCE (SIZE (1..maxULTxSwitchingBandPairs)) OF ULTxSwitchingBandPair-v1700 OPTIONAL,

-- R4 16-6: UL-MIMO coherence capability for dynamic Tx switching between 2Tx-2Tx switching

uplinkTxSwitchingBandParametersList-v1700 SEQUENCE (SIZE (1.. maxSimultaneousBands)) OF UplinkTxSwitchingBandParameters-v1700 OPTIONAL

}

BandCombination-UplinkTxSwitch-v1720 ::= SEQUENCE {

bandCombination-v1720 BandCombination-v1720 OPTIONAL,

uplinkTxSwitching-OptionSupport2T2T-r17 ENUMERATED {switchedUL, dualUL, both} OPTIONAL

}

BandCombination-UplinkTxSwitch-v1730 ::= SEQUENCE {

bandCombination-v1730 BandCombination-v1730 OPTIONAL

}

BandCombination-UplinkTxSwitch-v1740 ::= SEQUENCE {

bandCombination-v1740 BandCombination-v1740 OPTIONAL

}

BandCombination-UplinkTxSwitch-v1760 ::= SEQUENCE {

bandCombination-v1760 BandCombination-v1760 OPTIONAL

}

BandCombination-UplinkTxSwitch-v1770 ::= SEQUENCE {

bandCombination-v1770 BandCombination-v1770 OPTIONAL

}

BandCombination-UplinkTxSwitch-v1780 ::= SEQUENCE {

bandCombination-v1780 BandCombination-v1780 OPTIONAL

}

BandCombination-UplinkTxSwitch-v1790 ::= SEQUENCE {

bandCombination-v1790 BandCombination-v1790 OPTIONAL

}

BandCombination-UplinkTxSwitch-v17b0 ::= SEQUENCE {

bandCombination-v17b0 BandCombination-v17b0 OPTIONAL

}

BandCombination-UplinkTxSwitch-v1800 ::= SEQUENCE {

bandCombination-v1800 BandCombination-v1800 OPTIONAL,

supportedBandPairListNR-r18 SEQUENCE (SIZE (1..maxULTxSwitchingBandPairs)) OF ULTxSwitchingBandPair-r18 OPTIONAL,

-- R1 49-Y: Minimum separation time for two uplink switching on more than 2 bands within any two consecutive reference slots

uplinkTxSwitchingMinimumSeparationTime-r18 ENUMERATED {n0us, n500us} OPTIONAL,

-- R4 38-4: Switching Period for unaffected Band for Dual UL

uplinkTxSwitchingAdditionalPeriodDualUL-List-r18 SEQUENCE (SIZE (1..maxULTxSwitchingBetweenBandPairs-r18)) OF

UplinkTxSwitchingAdditionalPeriodDualUL-r18 OPTIONAL,

-- R4 38-6: Switching period restriction for fallback band combination

switchingPeriodRestriction-r18 ENUMERATED {true} OPTIONAL

}

BandCombination-UplinkTxSwitch-v1830 ::= SEQUENCE {

bandCombination-v1830 BandCombination-v1830 OPTIONAL

}

BandCombination-UplinkTxSwitch-v1840 ::= SEQUENCE {

bandCombination-v1840 BandCombination-v1840 OPTIONAL,

supportedBandPairListNR-v1840 SEQUENCE (SIZE (1..maxULTxSwitchingBandPairs)) OF ULTxSwitchingBandPair-v1840 OPTIONAL

}

BandCombination-UplinkTxSwitch-v1860 ::= SEQUENCE {

bandCombination-v1860 BandCombination-v1860 OPTIONAL

}

BandCombination-UplinkTxSwitch-v1900 ::=SEQUENCE {

bandCombination-v1900 BandCombination-v1900 OPTIONAL,

-- R1 67-5: Enhanced handling of simultaneous SRS carrier switching and uplink Tx switching

simultaneousSRS-UplinkTxSwitch-r19 ENUMERATED {max, sum} OPTIONAL,

supportedBandPairListNR-v1900 SEQUENCE (SIZE (1..maxULTxSwitchingBandPairs)) OF ULTxSwitchingBandPair-v1900 OPTIONAL,

uplinkTxSwitchingBandParametersList-v1900 SEQUENCE (SIZE (1..maxSimultaneousBands)) OF UplinkTxSwitchingBandParameters-v1900 OPTIONAL

}

ULTxSwitchingBandPair-r16 ::= SEQUENCE {

bandIndexUL1-r16 INTEGER(1..maxSimultaneousBands),

bandIndexUL2-r16 INTEGER(1..maxSimultaneousBands),

uplinkTxSwitchingPeriod-r16 ENUMERATED {n35us, n140us, n210us},

uplinkTxSwitching-DL-Interruption-r16 BIT STRING (SIZE(1..maxSimultaneousBands)) OPTIONAL

}

ULTxSwitchingBandPair-v1700 ::= SEQUENCE {

uplinkTxSwitchingPeriod2T2T-r17 ENUMERATED {n35us, n140us, n210us} OPTIONAL

}

ULTxSwitchingBandPair-r18 ::= SEQUENCE {

bandIndexUL1-r18 INTEGER(1..maxSimultaneousBands),

bandIndexUL2-r18 INTEGER(1..maxSimultaneousBands),

-- R1 49-X: Supported switching option for each band pair in the band combination for UL Tx switching across more than 2 bands

uplinkTxSwitchingOptionForBandPair-r18 ENUMERATED {switchedUL, dualUL, both},

-- R4 38-1: Switching period for dynamic UL Tx switching across up to 4 bands in case of inter-band CA, SUL up to two TAGs

uplinkTxSwitchingPeriodForBandPair-r18 SEQUENCE {

switchingPeriodFor2T-r18 ENUMERATED {n35us, n140us, n210us} OPTIONAL,

switchingPeriodFor1T-r18 ENUMERATED {n35us, n140us, n210us}

},

-- R4 38-2: Application of DL interruptions due to dynamic UL Tx switching

uplinkTxSwitching-DL-Interruption-r18 BIT STRING (SIZE(1..maxSimultaneousBands)) OPTIONAL,

-- R4 38-3: Switching Period for unaffected Band for Dual UL

uplinkTxSwitchingPeriodUnaffectedBandDualUL-List-r18 SEQUENCE (SIZE (1..maxSimultaneousBands-2-r18)) OF

SwitchingPeriodUnaffectedBandDualUL-r18 OPTIONAL

}

ULTxSwitchingBandPair-v1840 ::= SEQUENCE {

-- R1 49-Z: Support of 2-band configuration of 1T-1T UL Tx switching by using Rel-18 UL Tx switching configurations

configured1T1T-OnTwoBands-r18 ENUMERATED {supported} OPTIONAL

}

ULTxSwitchingBandPair-v1900 ::= SEQUENCE {

-- R4 57-1: Switch period for dynamic UL Tx switching between 2 bands for 3Tx UE with up to 2Tx per band

uplink3TxSwitchingPeriodUpTo2TPerBandDualUL-v1900 ENUMERATED {n35us, n140us, n210us},

-- R4 57-2: Application of DL interruptions due to dynamic UL Tx switching between 2 bands for 3Tx UE with up to 2Tx per band

uplinkTxSwitching-DL-Interruption-DualUL-v1900 BIT STRING (SIZE(1..maxSimultaneousBands)) OPTIONAL

}

UplinkTxSwitchingBandParameters-v1700 ::= SEQUENCE {

bandIndex-r17 INTEGER(1..maxSimultaneousBands),

-- R4 38-5: UL-MIMO coherence capability for dynamic Tx switching between 2Tx-2Tx switching among up to 4 bands

uplinkTxSwitching2T2T-PUSCH-TransCoherence-r17 ENUMERATED {nonCoherent, fullCoherent} OPTIONAL

}

UplinkTxSwitchingAdditionalPeriodDualUL-r18::= SEQUENCE {

uplinkTxSwitchingBetweenBandPairs-r18 SEQUENCE {

bandPairIndex1-r18 INTEGER(1.. maxULTxSwitchingBandPairs),

anotherBandPairOrBand-r18 CHOICE {

bandPairIndex2-r18 INTEGER(1.. maxULTxSwitchingBandPairs),

bandIndex-r18 INTEGER(1..maxSimultaneousBands)

}

},

-- R4 38-4: Additional switching Period for switching case across three or four bands for Dual UL

switchingAdditionalPeriodDualUL-r18 ENUMERATED {n35us, n140us, n210us}

}

UplinkTxSwitchingBandParameters-v1900 ::= SEQUENCE {

bandIndex-r19 INTEGER(1..maxSimultaneousBands),

-- R4 57-3: UL-MIMO coherence capability for dynamic UL Tx switching between 2 bands for 3Tx UE with up to 2Tx per band

uplinkTxSwitching3Tx-PUSCH-TransCoherence-DualUL-v1900 ENUMERATED {nonCoherent, fullCoherent} OPTIONAL

}

SwitchingPeriodUnaffectedBandDualUL-r18::= SEQUENCE {

bandIndexUnaffected-r18 INTEGER(1..maxSimultaneousBands),

periodUnaffectedBandDualUL-r18 CHOICE {

maintainedUL-Trans-r18 NULL,

periodOnULBands-r18 ENUMERATED {n35us, n140us, n210us}

}

}

BandParameters ::= CHOICE {

eutra SEQUENCE {

bandEUTRA FreqBandIndicatorEUTRA,

ca-BandwidthClassDL-EUTRA CA-BandwidthClassEUTRA OPTIONAL,

ca-BandwidthClassUL-EUTRA CA-BandwidthClassEUTRA OPTIONAL

},

nr SEQUENCE {

bandNR FreqBandIndicatorNR,

ca-BandwidthClassDL-NR CA-BandwidthClassNR OPTIONAL,

ca-BandwidthClassUL-NR CA-BandwidthClassNR OPTIONAL

}

}

BandParameters-v1540 ::= SEQUENCE {

srs-CarrierSwitch CHOICE {

nr SEQUENCE {

srs-SwitchingTimesListNR SEQUENCE (SIZE (1..maxSimultaneousBands)) OF SRS-SwitchingTimeNR

},

eutra SEQUENCE {

srs-SwitchingTimesListEUTRA SEQUENCE (SIZE (1..maxSimultaneousBands)) OF SRS-SwitchingTimeEUTRA

}

} OPTIONAL,

srs-TxSwitch SEQUENCE {

supportedSRS-TxPortSwitch ENUMERATED {t1r2, t1r4, t2r4, t1r4-t2r4, t1r1, t2r2, t4r4, notSupported},

txSwitchImpactToRx INTEGER (1..32) OPTIONAL,

txSwitchWithAnotherBand INTEGER (1..32) OPTIONAL

} OPTIONAL

}

BandParameters-v1610 ::= SEQUENCE {

srs-TxSwitch-v1610 SEQUENCE {

supportedSRS-TxPortSwitch-v1610 ENUMERATED {t1r1-t1r2, t1r1-t1r2-t1r4, t1r1-t1r2-t2r2-t2r4, t1r1-t1r2-t2r2-t1r4-t2r4,

t1r1-t2r2, t1r1-t2r2-t4r4}

} OPTIONAL

}

BandParameters-v1710 ::= SEQUENCE {

-- R1 23-8-3 SRS Antenna switching for >4Rx

srs-AntennaSwitchingBeyond4RX-r17 SEQUENCE {

-- 1. Support of SRS antenna switching xTyR with y>4

supportedSRS-TxPortSwitchBeyond4Rx-r17 BIT STRING (SIZE (11)),

-- 2. Report the entry number of the first-listed band with UL in the band combination that affects this DL

entryNumberAffectBeyond4Rx-r17 INTEGER (1..32) OPTIONAL,

-- 3. Report the entry number of the first-listed band with UL in the band combination that switches together with this UL

entryNumberSwitchBeyond4Rx-r17 INTEGER (1..32) OPTIONAL

} OPTIONAL

}

BandParameters-v1730 ::= SEQUENCE {

-- R1 39-3-2 Affected bands for inter-band CA during SRS carrier switching

srs-SwitchingAffectedBandsListNR-r17 SEQUENCE (SIZE (1..maxSimultaneousBands)) OF SRS-SwitchingAffectedBandsNR-r17

}

BandParameters-v1770 ::= SEQUENCE {

ca-BandwidthClassDL-NR-r17 CA-BandwidthClassNR-r17 OPTIONAL,

ca-BandwidthClassUL-NR-r17 CA-BandwidthClassNR-r17 OPTIONAL

}

BandParameters-v1780 ::= SEQUENCE {

ca-BandwidthClassDL-NR-r17 CA-BandwidthClassNR-r17 OPTIONAL,

ca-BandwidthClassUL-NR-r17 CA-BandwidthClassNR-r17 OPTIONAL,

supportedAggBW-FR2-r17 SEQUENCE {

supportedAggBW-DL-r17 SupportedAggBandwidth-r17 OPTIONAL,

supportedAggBW-UL-r17 SupportedAggBandwidth-r17 OPTIONAL

} OPTIONAL

}

BandParameters-v1810 ::= SEQUENCE {

-- R1 40-5-4: SRS 8 Tx ports-antenna switching

srs-AntennaSwitching8T8R-r18 SEQUENCE {

antennaSwitch8T8R-r18 ENUMERATED {noTdm, tdmAndNoTdm} OPTIONAL,

downgradeConfig-r18 CHOICE {

empty-r18 NULL,

downgrade-r18 BIT STRING (SIZE (11))

} OPTIONAL,

entryNumberAffect-r18 INTEGER (1..32) OPTIONAL,

entryNumberSwitch-r18 INTEGER (1..32) OPTIONAL

} OPTIONAL

}

BandParameters-v1900 ::= SEQUENCE {

-- R1 59-3-3: 3T6R Antenna switching

srs-AntennaSwitching3T6R-r19 SEQUENCE {

entryNumberAffect-r19 INTEGER (1..32) OPTIONAL,

entryNumberSwitch-r19 INTEGER (1..32) OPTIONAL

} OPTIONAL,

-- R1 59-3-3a: 3T3R Antenna switching

srs-AntennaSwitching3T3R-r19 SEQUENCE {

entryNumberAffect-r19 INTEGER (1..32) OPTIONAL,

entryNumberSwitch-r19 INTEGER (1..32) OPTIONAL

} OPTIONAL

}

ScalingFactorSidelink-r16 ::= ENUMERATED {f0p4, f0p75, f0p8, f1}

IntraBandPowerClass-r16 ::= ENUMERATED {pc2, pc3, spare6, spare5, spare4, spare3, spare2, spare1}

SRS-SwitchingAffectedBandsNR-r17 ::= BIT STRING (SIZE (1..maxSimultaneousBands))

SupportedIntraENDC-BandCombination-r17 ::= SEQUENCE {

supportedBandwidthCombinationSetIntraENDC-v1790 BIT STRING (SIZE (1..32)) OPTIONAL,

mrdc-Parameters-v1790 MRDC-Parameters-v1790 OPTIONAL

}

-- TAG-BANDCOMBINATIONLIST-STOP

-- ASN1STOP

|  |
| --- |
| *BandCombination* field descriptions |
| ***BandCombinationList-v1540, BandCombinationList-v1550, BandCombinationList-v1560, BandCombinationList-v1570, BandCombinationList-v1580, BandCombinationList-v1590, BandCombinationList-v15g0, BandCombinationList-v15n0, BandCombinationList-v1610*, *BandCombinationList-v1630*, *BandCombinationList-v1640*, *BandCombinationList-v1650, BandCombinationList-v1680, BandCombinationList-v1690, BandCombinationList-v16a0, BandCombinationList-v16j0, BandCombinationList-v1700, BandCombinationList-v1720, BandCombinationList-v1730, BandCombinationList-v1760, BandCombinationList-v1780, BandCombinationList-v1790, BandCombinationList-v17b0, BandCombinationList-v1800, BandCombinationList-v1830, BandCombinationList-v1840, BandCombinationList-v1860, BandCombinationList-v1900***  The UE shall include the same number of entries, and listed in the same order, as in *BandCombinationList* (without suffix). If the field is included in *supportedBandCombinationListNEDC-Only-v1610*, the UE shall include the same number of entries, and listed in the same order, as in *BandCombinationList* of *supportedBandCombinationListNEDC-Only* (without suffix) field.  If the field is included in *supportedBandCombinationListNEDC-Only-v15a0*, the UE shall include the same number of entries, and listed in the same order, as in *BandCombinationList* (without suffix) of *supportedBandCombinationListNEDC-Only* (without suffix) field. |
| ***BandCombinationList-UplinkTxSwitch-r16, BandCombinationList-UplinkTxSwitch-v1630, BandCombinationList-UplinkTxSwitch-v1640, BandCombinationList-UplinkTxSwitch-v1650, BandCombinationList-UplinkTxSwitch-v1690, BandCombinationList-UplinkTxSwitch-v16a0, BandCombinationList-UplinkTxSwitch-v16e0, BandCombinationList-UplinkTxSwitch-v16j0, BandCombinationList-UplinkTxSwitch-v1700, BandCombinationList-UplinkTxSwitch-v1720, BandCombinationList-UplinkTxSwitch-v1730, BandCombinationList-UplinkTxSwitch-v1760, BandCombinationList-UplinkTxSwitch-v1780, BandCombinationList-UplinkTxSwitch-v1790, BandCombinationList-UplinkTxSwitch-v17b0, BandCombinationList-UplinkTxSwitch-v1800, BandCombinationList-UplinkTxSwitch-v1830, BandCombinationList-UplinkTxSwitch-v1840, BandCombinationList-UplinkTxSwitch-v1860, BandCombinationList-UplinkTxSwitch-v1900***  The UE shall include the same number of entries, and listed in the same order, as in *BandCombinationList-UplinkTxSwitch-r16*.  For the field of *supportedBandCombinationList-UplinkTxSwitch-v1700*, if the UE does not support 2Tx-2Tx switching for a given band combination, the field of *supportedBandPairListNR-v1700* in the corresponding entry is absent. |
| ***ca-ParametersNRDC***  If the field (without suffix) is included for a band combination in the NR capability container, the field (without suffix) indicates support of NR-DC. Otherwise, the field is absent. If a version of the field (with suffix) is absent for a band combination, *ca-ParametersNR* field version in *BandCombination* corresponding to the *ca-ParametersNR-ForDC* field version in the field (with suffix) is applicable to the UE configured with NR-DC for the band combination. |
| ***featureSetCombinationDAPS***  If this field is present for a band combination, it reports the feature set combination supported for the band combination when any DAPS bearer is configured. |
| ***ne-DC-BC***  If the field is included for a band combination in the MR-DC capability container, the field indicates support of NE-DC. Otherwise, the field is absent. |
| ***supportedBandPairListNR-r16, supportedBandPairListNR-v1700, supportedBandPairListNR-v1900***  Indicates a list of band pair supporting UL Tx switching as defined in TS 38.101-1 [15] for a given band combination.  A UE supporting 2Tx-2Tx switching should include both of *supportedBandPairListNR-r16* and *supportedBandPairListNR-v1700*. And the UE shall include the same number of entries listed in the same order as in *supportedBandPairListNR-r16*.  If the UE does not support 2Tx-2Tx switching for a given band pair, the field of *uplinkTxSwitchingPeriod2T2T* in the corresponding entry is absent.  A 3Tx UE supporting Tx switching between 2 UL bands with up to 2Tx per band should indicate both of *supportedBandPairListNR-r16* and *supportedBandPairListNR-v19xy*. And the UE shall include the same number of entries listed in the same order as in *supportedBandPairListNR-r16*. |
| ***supportedBandPairListNR-r18*, *supportedBandPairListNR-v1840***  Indicates a list of band pair supporting UL Tx switching up to 4 bands as defined in TS 38.101-1 [15] for a given band combination. The UE shall include all the possible band pairs. If *supportedBandPairListNR-v1840* is included, the UE shall include the same number of entries listed in the same order as in *supportedBandPairListNR-r18*.  For a band pair only supporting 1Tx-1Tx switching, the UE should include *switchingPeriodFor1T* in *ULTxSwitchingBandPair-r18*.  For a band pair supporting 1Tx-2Tx switching, the UE always supports 1Tx-1Tx switching, and the UE should include *switchingPeriodFor1T* in *ULTxSwitchingBandPair-r18*.  For a band pair supporting 2Tx-2Tx switching, the UE always supports 1Tx-2Tx switching and 1Tx-1Tx switching, the UE should include *switchingPeriodFor2T* as well as *switchingPeriodFor1T* in *ULTxSwitchingBandPair-r18*. |
| ***srs-SwitchingTimesListNR***  Indicates, for a particular pair of NR bands, the RF retuning time when switching between a NR carrier corresponding to this band entry and another (PUSCH-less) NR carrier corresponding to the band entry in the order indicated below:  - For the first NR band, the UE shall include the same number of entries for NR bands as in *bandList*, i.e. first entry corresponds to first NR band in *bandList* and so on,  - For the second NR band, the UE shall include one entry less, i.e. first entry corresponds to the second NR band in *bandList* and so on  - And so on |
| ***srs-SwitchingTimesListEUTRA***  Indicates, for a particular pair of E-UTRA bands, the RF retuning time when switching between an E-UTRA carrier corresponding to this band entry and another (PUSCH-less) E-UTRA carrier corresponding to the band entry in the order indicated below:  - For the first E-UTRA band, the UE shall include the same number of entries for E-UTRA bands as in *bandList,* i.e. first entry corresponds to first E-UTRA band in *bandList* and so on,  - For the second E-UTRA band, the UE shall include one entry less, i.e. first entry corresponds to the second E-UTRA band in *bandList* and so on  - And so on |
| ***srs-TxSwitch***  Indicates supported SRS antenna switch capability for the associated band. If the UE indicates support of *SRS-SwitchingTimeNR*, the UE is allowed to set this field for a band with associated *FeatureSetUplinkId* set to 0 for SRS carrier switching. |
| ***supportedIntraENDC-BandCombinationList***  Indicates BCS and/or spectrum contiguity capability for each entry in a list of intra-band (NG)EN-DC components in an inter-band (NG)EN-DC band combination. The UE shall include the entries in the order corresponding to the order of NR band entries of the intra-band (NG)EN-DC components in the *bandList* in the inter-band (NG)EN-DC band combination (i.e., *BandCombination* without suffix). |
| ***uplinkTxSwitchingBandParametersList-v1700, uplinkTxSwitchingBandParametersList-v1900***  Indicates a list of per band per band combination capabilities for UL Tx switching. |

#### – *BandCombinationListSidelinkEUTRA-NR*

The IE *BandCombinationListSidelinkEUTRA-NR* contains a list of V2X sidelink and NR sidelink band combinations.

BandCombinationListSidelinkEUTRA-NR information element

-- ASN1START

-- TAG-BANDCOMBINATIONLISTSIDELINKEUTRANR-START

BandCombinationListSidelinkEUTRA-NR-r16 ::= SEQUENCE (SIZE (1..maxBandComb)) OF BandCombinationParametersSidelinkEUTRA-NR-r16

BandCombinationListSidelinkEUTRA-NR-v1630 ::= SEQUENCE (SIZE (1..maxBandComb)) OF BandCombinationParametersSidelinkEUTRA-NR-v1630

BandCombinationListSidelinkEUTRA-NR-v1710 ::= SEQUENCE (SIZE (1..maxBandComb)) OF BandCombinationParametersSidelinkEUTRA-NR-v1710

BandCombinationParametersSidelinkEUTRA-NR-r16 ::= SEQUENCE (SIZE (1..maxSimultaneousBands)) OF BandParametersSidelinkEUTRA-NR-r16

BandCombinationParametersSidelinkEUTRA-NR-v1630 ::= SEQUENCE (SIZE (1..maxSimultaneousBands)) OF BandParametersSidelinkEUTRA-NR-v1630

BandCombinationParametersSidelinkEUTRA-NR-v1710 ::= SEQUENCE (SIZE (1..maxSimultaneousBands)) OF BandParametersSidelinkEUTRA-NR-v1710

BandParametersSidelinkEUTRA-NR-r16 ::= CHOICE {

eutra SEQUENCE {

bandParametersSidelinkEUTRA1-r16 OCTET STRING OPTIONAL,

bandParametersSidelinkEUTRA2-r16 OCTET STRING OPTIONAL

},

nr SEQUENCE {

bandParametersSidelinkNR-r16 BandParametersSidelink-r16

}

}

BandParametersSidelinkEUTRA-NR-v1630 ::= CHOICE {

eutra NULL,

nr SEQUENCE {

tx-Sidelink-r16 ENUMERATED {supported} OPTIONAL,

rx-Sidelink-r16 ENUMERATED {supported} OPTIONAL,

sl-CrossCarrierScheduling-r16 ENUMERATED {supported} OPTIONAL

}

}

BandParametersSidelinkEUTRA-NR-v1710 ::= CHOICE {

eutra NULL,

nr SEQUENCE {

--32-4

sl-TransmissionMode2-PartialSensing-r17 SEQUENCE {

harq-TxProcessModeTwoSidelink-r17 ENUMERATED {n8, n16},

scs-CP-PatternTxSidelinkModeTwo-r17 CHOICE {

fr1-r17 SEQUENCE {

scs-15kHz-r17 BIT STRING (SIZE (16)) OPTIONAL,

scs-30kHz-r17 BIT STRING (SIZE (16)) OPTIONAL,

scs-60kHz-r17 BIT STRING (SIZE (16)) OPTIONAL

},

fr2-r17 SEQUENCE {

scs-60kHz-r17 BIT STRING (SIZE (16)) OPTIONAL,

scs-120kHz-r17 BIT STRING (SIZE (16)) OPTIONAL

}

} OPTIONAL,

extendedCP-Mode2PartialSensing-r17 ENUMERATED {supported} OPTIONAL,

dl-openLoopPC-Sidelink-r17 ENUMERATED {supported} OPTIONAL

} OPTIONAL,

--32-2a: Receiving NR sidelink of PSFCH

rx-sidelinkPSFCH-r17 ENUMERATED {n5, n15, n25, n32, n35, n45, n50, n64} OPTIONAL,

--32-5a-1

tx-IUC-Scheme1-Mode2Sidelink-r17 ENUMERATED {supported} OPTIONAL,

--32-5b-1

tx-IUC-Scheme2-Mode2Sidelink-r17 ENUMERATED {n4, n8, n16} OPTIONAL

}

}

BandParametersSidelink-r16 ::= SEQUENCE {

freqBandSidelink-r16 FreqBandIndicatorNR

}

-- TAG-BANDCOMBINATIONLISTSIDELINKEUTRANR-STOP

-- ASN1STOP

|  |
| --- |
| *BandParametersSidelinkEUTRA-NR* field descriptions |
| ***bandParametersSidelinkEUTRA1,*** ***bandParametersSidelinkEUTRA2***  This field includes the *V2X-BandParameters-r14* and *V2X-BandParameters-v1530* IE as specified in 36.331 [10]. It is used for reporting the per-band capability for V2X sidelink communication. |

#### – *BandCombinationListSL-Discovery*

The IE *BandCombinationListSL-Discovery* contains a list of NR Sidelink discovery band combinations.

*BandCombinationListSidelinkSL-Discovery* information element

-- ASN1START

-- TAG-BANDCOMBINATIONLISTSLDISCOVERY-START

BandCombinationListSL-Discovery-r17 ::= SEQUENCE (SIZE (1..maxSimultaneousBands)) OF BandParametersSidelinkDiscovery-r17

BandParametersSidelinkDiscovery-r17 ::= SEQUENCE {

sl-CrossCarrierScheduling-r17 ENUMERATED {supported} OPTIONAL,

--R1 32-4: Transmitting NR sidelink mode 2 with partial sensing

sl-TransmissionMode2-PartialSensing-r17 SEQUENCE {

harq-TxProcessModeTwoSidelink-r17 ENUMERATED {n8, n16},

scs-CP-PatternTxSidelinkModeTwo-r17 CHOICE {

fr1-r17 SEQUENCE {

scs-15kHz-r17 BIT STRING (SIZE (16)) OPTIONAL,

scs-30kHz-r17 BIT STRING (SIZE (16)) OPTIONAL,

scs-60kHz-r17 BIT STRING (SIZE (16)) OPTIONAL

},

fr2-r17 SEQUENCE {

scs-60kHz-r17 BIT STRING (SIZE (16)) OPTIONAL,

scs-120kHz-r17 BIT STRING (SIZE (16)) OPTIONAL

}

} OPTIONAL,

extendedCP-Mode2PartialSensing-r17 ENUMERATED {supported} OPTIONAL,

dl-openLoopPC-Sidelink-r17 ENUMERATED {supported} OPTIONAL

} OPTIONAL,

--R1 32-5a-1: Transmitting Inter-UE coordination scheme 1 in NR sidelink mode 2

tx-IUC-Scheme1-Mode2Sidelink-r17 ENUMERATED {supported} OPTIONAL

}

-- TAG-BANDCOMBINATIONLISTSLDISCOVERY-STOP

-- ASN1STOP

#### – *CA-BandwidthClassEUTRA*

The IE *CA-BandwidthClassEUTRA* indicates the E-UTRA CA bandwidth class as defined in TS 36.101 [22], table 5.6A-1.

*CA-BandwidthClassEUTRA* information element

-- ASN1START

-- TAG-CA-BANDWIDTHCLASSEUTRA-START

CA-BandwidthClassEUTRA ::= ENUMERATED {a, b, c, d, e, f, ...}

-- TAG-CA-BANDWIDTHCLASSEUTRA-STOP

-- ASN1STOP

#### – *CA-BandwidthClassNR*

The IE *CA-BandwidthClassNR* indicates the NR CA bandwidth class as defined in TS 38.101-1 [15], table 5.3A.5-1 and TS 38.101-2 [39], table 5.3A.4-1.

*CA-BandwidthClassNR* information element

-- ASN1START

-- TAG-CA-BANDWIDTHCLASSNR-START

-- R4 17-6: new CA BW Classes R2-R12

-- R4 17-7: new CA BW Classes V, W

CA-BandwidthClassNR ::= ENUMERATED {a, b, c, d, e, f, g, h, i, j, k, l, m, n, o, p, q, ...,r2-v1730, r3-v1730, r4-v1730, r5-v1730, r6-v1730, r7-v1730, r8-v1730, r9-v1730, r10-v1730, r11-v1730, r12-v1730,v-v1770, w-v1770 }

CA-BandwidthClassNR-r17 ::= ENUMERATED {r, s, t, u, ...}

-- TAG-CA-BANDWIDTHCLASSNR-STOP

-- ASN1STOP

#### – *CA-ParametersEUTRA*

The IE *CA-ParametersEUTRA* contains the E-UTRA part of band combination parameters for a given MR-DC band combination.

NOTE: If additional E-UTRA band combination parameters are defined in TS 36.331 [10], which are supported for MR-DC, they will be defined here as well.

*CA-ParametersEUTRA* information element

-- ASN1START

-- TAG-CA-PARAMETERSEUTRA-START

CA-ParametersEUTRA ::= SEQUENCE {

multipleTimingAdvance ENUMERATED {supported} OPTIONAL,

simultaneousRx-Tx ENUMERATED {supported} OPTIONAL,

supportedNAICS-2CRS-AP BIT STRING (SIZE (1..8)) OPTIONAL,

additionalRx-Tx-PerformanceReq ENUMERATED {supported} OPTIONAL,

ue-CA-PowerClass-N ENUMERATED {class2} OPTIONAL,

supportedBandwidthCombinationSetEUTRA-v1530 BIT STRING (SIZE (1..32)) OPTIONAL,

...

}

CA-ParametersEUTRA-v1560 ::= SEQUENCE {

fd-MIMO-TotalWeightedLayers INTEGER (2..128) OPTIONAL

}

CA-ParametersEUTRA-v1570 ::= SEQUENCE {

dl-1024QAM-TotalWeightedLayers INTEGER (0..10) OPTIONAL

}

-- TAG-CA-PARAMETERSEUTRA-STOP

-- ASN1STOP

#### – *CA-ParametersNR*

The IE *CA-ParametersNR* contains carrier aggregation and inter-frequency DAPS handover related capabilities that are defined per band combination.

*CA-ParametersNR* information element

-- ASN1START

-- TAG-CA-PARAMETERSNR-START

CA-ParametersNR ::= SEQUENCE {

dummy ENUMERATED {supported} OPTIONAL,

parallelTxSRS-PUCCH-PUSCH ENUMERATED {supported} OPTIONAL,

parallelTxPRACH-SRS-PUCCH-PUSCH ENUMERATED {supported} OPTIONAL,

simultaneousRxTxInterBandCA ENUMERATED {supported} OPTIONAL,

simultaneousRxTxSUL ENUMERATED {supported} OPTIONAL,

diffNumerologyAcrossPUCCH-Group ENUMERATED {supported} OPTIONAL,

diffNumerologyWithinPUCCH-GroupSmallerSCS ENUMERATED {supported} OPTIONAL,

supportedNumberTAG ENUMERATED {n2, n3, n4} OPTIONAL,

...

}

CA-ParametersNR-v1540 ::= SEQUENCE {

simultaneousSRS-AssocCSI-RS-AllCC INTEGER (5..32) OPTIONAL,

csi-RS-IM-ReceptionForFeedbackPerBandComb SEQUENCE {

maxNumberSimultaneousNZP-CSI-RS-ActBWP-AllCC INTEGER (1..64) OPTIONAL,

totalNumberPortsSimultaneousNZP-CSI-RS-ActBWP-AllCC INTEGER (2..256) OPTIONAL

} OPTIONAL,

simultaneousCSI-ReportsAllCC INTEGER (5..32) OPTIONAL,

dualPA-Architecture ENUMERATED {supported} OPTIONAL

}

CA-ParametersNR-v1550 ::= SEQUENCE {

dummy ENUMERATED {supported} OPTIONAL

}

CA-ParametersNR-v1560 ::= SEQUENCE {

diffNumerologyWithinPUCCH-GroupLargerSCS ENUMERATED {supported} OPTIONAL

}

CA-ParametersNR-v15g0 ::= SEQUENCE {

simultaneousRxTxInterBandCAPerBandPair SimultaneousRxTxPerBandPair OPTIONAL,

simultaneousRxTxSULPerBandPair SimultaneousRxTxPerBandPair OPTIONAL

}

CA-ParametersNR-v1610 ::= SEQUENCE {

-- R1 9-3: Parallel MsgA and SRS/PUCCH/PUSCH transmissions across CCs in inter-band CA

parallelTxMsgA-SRS-PUCCH-PUSCH-r16 ENUMERATED {supported} OPTIONAL,

-- R1 9-4: MsgA operation in a band combination including SUL

msgA-SUL-r16 ENUMERATED {supported} OPTIONAL,

-- R1 10-9c: Joint search space group switching across multiple cells

jointSearchSpaceSwitchAcrossCells-r16 ENUMERATED {supported} OPTIONAL,

-- R1 14-5: Half-duplex UE behaviour in TDD CA for same SCS

half-DuplexTDD-CA-SameSCS-r16 ENUMERATED {supported} OPTIONAL,

-- R1 18-4: SCell dormancy within active time

scellDormancyWithinActiveTime-r16 ENUMERATED {supported} OPTIONAL,

-- R1 18-4a: SCell dormancy outside active time

scellDormancyOutsideActiveTime-r16 ENUMERATED {supported} OPTIONAL,

-- R1 18-6: Cross-carrier A-CSI RS triggering with different SCS

crossCarrierA-CSI-trigDiffSCS-r16 ENUMERATED {higherA-CSI-SCS,lowerA-CSI-SCS,both} OPTIONAL,

-- R1 18-6a: Default QCL assumption for cross-carrier A-CSI-RS triggering

defaultQCL-CrossCarrierA-CSI-Trig-r16 ENUMERATED {diffOnly, both} OPTIONAL,

-- R1 18-7: CA with non-aligned frame boundaries for inter-band CA

interCA-NonAlignedFrame-r16 ENUMERATED {supported} OPTIONAL,

simul-SRS-Trans-BC-r16 ENUMERATED {n2} OPTIONAL,

interFreqDAPS-r16 SEQUENCE {

interFreqAsyncDAPS-r16 ENUMERATED {supported} OPTIONAL,

interFreqDiffSCS-DAPS-r16 ENUMERATED {supported} OPTIONAL,

interFreqMultiUL-TransmissionDAPS-r16 ENUMERATED {supported} OPTIONAL,

interFreqSemiStaticPowerSharingDAPS-Mode1-r16 ENUMERATED {supported} OPTIONAL,

interFreqSemiStaticPowerSharingDAPS-Mode2-r16 ENUMERATED {supported} OPTIONAL,

interFreqDynamicPowerSharingDAPS-r16 ENUMERATED {short, long} OPTIONAL,

interFreqUL-TransCancellationDAPS-r16 ENUMERATED {supported} OPTIONAL

} OPTIONAL,

codebookParametersPerBC-r16 CodebookParameters-v1610 OPTIONAL,

-- R1 16-2a-10 Value of R for BD/CCE

blindDetectFactor-r16 INTEGER (1..2) OPTIONAL,

-- R1 11-2a: Capability on the number of CCs for monitoring a maximum number of BDs and non-overlapped CCEs per span when configured

-- with DL CA with Rel-16 PDCCH monitoring capability on all the serving cells

pdcch-MonitoringCA-r16 SEQUENCE {

maxNumberOfMonitoringCC-r16 INTEGER (2..16),

supportedSpanArrangement-r16 ENUMERATED {alignedOnly, alignedAndNonAligned}

} OPTIONAL,

-- R1 11-2c: Number of carriers for CCE/BD scaling with DL CA with mix of Rel. 16 and Rel. 15 PDCCH monitoring capabilities on

-- different carriers

pdcch-BlindDetectionCA-Mixed-r16 SEQUENCE {

pdcch-BlindDetectionCA1-r16 INTEGER (1..15),

pdcch-BlindDetectionCA2-r16 INTEGER (1..15),

supportedSpanArrangement-r16 ENUMERATED {alignedOnly, alignedAndNonAligned}

} OPTIONAL,

-- R1 11-2d: Capability on the number of CCs for monitoring a maximum number of BDs and non-overlapped CCEs per span for MCG and for

-- SCG when configured for NR-DC operation with Rel-16 PDCCH monitoring capability on all the serving cells

pdcch-BlindDetectionMCG-UE-r16 INTEGER (1..14) OPTIONAL,

pdcch-BlindDetectionSCG-UE-r16 INTEGER (1..14) OPTIONAL,

-- R1 11-2e: Number of carriers for CCE/BD scaling for MCG and for SCG when configured for NR-DC operation with mix of Rel. 16 and

-- Rel. 15 PDCCH monitoring capabilities on different carriers

pdcch-BlindDetectionMCG-UE-Mixed-r16 SEQUENCE {

pdcch-BlindDetectionMCG-UE1-r16 INTEGER (0..15),

pdcch-BlindDetectionMCG-UE2-r16 INTEGER (0..15)

} OPTIONAL,

pdcch-BlindDetectionSCG-UE-Mixed-r16 SEQUENCE {

pdcch-BlindDetectionSCG-UE1-r16 INTEGER (0..15),

pdcch-BlindDetectionSCG-UE2-r16 INTEGER (0..15)

} OPTIONAL,

-- R1 18-5 cross-carrier scheduling with different SCS in DL CA

crossCarrierSchedulingDL-DiffSCS-r16 ENUMERATED {low-to-high, high-to-low, both} OPTIONAL,

-- R1 18-5a Default QCL assumption for cross-carrier scheduling

crossCarrierSchedulingDefaultQCL-r16 ENUMERATED {diff-only, both} OPTIONAL,

-- R1 18-5b cross-carrier scheduling with different SCS in UL CA

crossCarrierSchedulingUL-DiffSCS-r16 ENUMERATED {low-to-high, high-to-low, both} OPTIONAL,

-- R1 13.19a Simultaneous positioning SRS and MIMO SRS transmission for a given BC

simul-SRS-MIMO-Trans-BC-r16 ENUMERATED {n2} OPTIONAL,

-- R1 16-3a, 16-3a-1, 16-3b, 16-3b-1: New Individual Codebook

codebookParametersAdditionPerBC-r16 CodebookParametersAdditionPerBC-r16 OPTIONAL,

-- R1 16-8: Mixed codebook

codebookComboParametersAdditionPerBC-r16 CodebookComboParametersAdditionPerBC-r16 OPTIONAL

}

CA-ParametersNR-v1630 ::= SEQUENCE {

-- R1 22-5b: Simultaneous transmission of SRS for antenna switching and SRS for CB/NCB /BM for inter-band UL CA

-- R1 22-5d: Simultaneous transmission of SRS for antenna switching for inter-band UL CA

simulTX-SRS-AntSwitchingInterBandUL-CA-r16 SimulSRS-ForAntennaSwitching-r16 OPTIONAL,

-- R4 8-5: supported beam management type for inter-band CA

beamManagementType-r16 ENUMERATED {ibm, dummy} OPTIONAL,

-- R4 7-3a: UL frequency separation class with aggregate BW and Gap BW

intraBandFreqSeparationUL-AggBW-GapBW-r16 ENUMERATED {classI, classII, classIII} OPTIONAL,

-- RAN 89: Case B in case of Inter-band CA with non-aligned frame boundaries

interCA-NonAlignedFrame-B-r16 ENUMERATED {supported} OPTIONAL

}

CA-ParametersNR-v1640 ::= SEQUENCE {

-- R4 7-5: Support of reporting UL Tx DC locations for uplink intra-band CA.

uplinkTxDC-TwoCarrierReport-r16 ENUMERATED {supported} OPTIONAL,

-- RAN 22-6: Support of up to 3 different numerologies in the same NR PUCCH group for NR part of EN-DC, NGEN-DC, NE-DC and NR-CA

-- where UE is not configured with two NR PUCCH groups

maxUpTo3Diff-NumerologiesConfigSinglePUCCH-grp-r16 PUCCH-Grp-CarrierTypes-r16 OPTIONAL,

-- RAN 22-6a: Support of up to 4 different numerologies in the same NR PUCCH group for NR part of EN-DC, NGEN-DC, NE-DC and NR-CA

-- where UE is not configured with two NR PUCCH groups

maxUpTo4Diff-NumerologiesConfigSinglePUCCH-grp-r16 PUCCH-Grp-CarrierTypes-r16 OPTIONAL,

-- RAN 22-7: Support two PUCCH groups for NR-CA with 3 or more bands with at least two carrier types

twoPUCCH-Grp-ConfigurationsList-r16 SEQUENCE (SIZE (1..maxTwoPUCCH-Grp-ConfigList-r16)) OF TwoPUCCH-Grp-Configurations-r16 OPTIONAL,

-- R1 22-7a: Different numerology across NR PUCCH groups

diffNumerologyAcrossPUCCH-Group-CarrierTypes-r16 ENUMERATED {supported} OPTIONAL,

-- R1 22-7b: Different numerologies across NR carriers within the same NR PUCCH group, with PUCCH on a carrier of smaller SCS

diffNumerologyWithinPUCCH-GroupSmallerSCS-CarrierTypes-r16 ENUMERATED {supported} OPTIONAL,

-- R1 22-7c: Different numerologies across NR carriers within the same NR PUCCH group, with PUCCH on a carrier of larger SCS

diffNumerologyWithinPUCCH-GroupLargerSCS-CarrierTypes-r16 ENUMERATED {supported} OPTIONAL,

-- R1 11-2f: add the replicated FGs of 11-2a/c with restriction for non-aligned span case

-- with DL CA with Rel-16 PDCCH monitoring capability on all the serving cells

pdcch-MonitoringCA-NonAlignedSpan-r16 INTEGER (2..16) OPTIONAL,

-- R1 11-2g: add the replicated FGs of 11-2a/c with restriction for non-aligned span case

pdcch-BlindDetectionCA-Mixed-NonAlignedSpan-r16 SEQUENCE {

pdcch-BlindDetectionCA1-r16 INTEGER (1..15),

pdcch-BlindDetectionCA2-r16 INTEGER (1..15)

} OPTIONAL

}

CA-ParametersNR-v1690 ::= SEQUENCE {

csi-ReportingCrossPUCCH-Grp-r16 SEQUENCE {

computationTimeForA-CSI-r16 ENUMERATED {sameAsNoCross, relaxed},

additionalSymbols-r16 SEQUENCE {

scs-15kHz-additionalSymbols-r16 ENUMERATED {s14, s28} OPTIONAL,

scs-30kHz-additionalSymbols-r16 ENUMERATED {s14, s28} OPTIONAL,

scs-60kHz-additionalSymbols-r16 ENUMERATED {s14, s28, s56} OPTIONAL,

scs-120kHz-additionalSymbols-r16 ENUMERATED {s14, s28, s56} OPTIONAL

} OPTIONAL,

sp-CSI-ReportingOnPUCCH-r16 ENUMERATED {supported} OPTIONAL,

sp-CSI-ReportingOnPUSCH-r16 ENUMERATED {supported} OPTIONAL,

carrierTypePairList-r16 SEQUENCE (SIZE (1..maxCarrierTypePairList-r16)) OF CarrierTypePair-r16

} OPTIONAL

}

CA-ParametersNR-v16a0 ::= SEQUENCE {

pdcch-BlindDetectionMixedList-r16 SEQUENCE(SIZE(1..maxNrofPdcch-BlindDetectionMixed-1-r16)) OF PDCCH-BlindDetectionMixedList-r16

}

CA-ParametersNR-v1700 ::= SEQUENCE {

-- R1 23-9-1: Basic Features of Further Enhanced Port-Selection Type II Codebook (FeType-II) per band combination information

codebookParametersfetype2PerBC-r17 CodebookParametersfetype2PerBC-r17 OPTIONAL,

-- R4 18-4: Support of enhanced Demodulation requirements for CA in HST SFN FR1

demodulationEnhancementCA-r17 ENUMERATED {supported} OPTIONAL,

-- R4 20-1: Maximum uplink duty cycle for NR inter-band CA power class 2

maxUplinkDutyCycle-interBandCA-PC2-r17 ENUMERATED {n50, n60, n70, n80, n90, n100} OPTIONAL,

-- R4 20-2: Maximum uplink duty cycle for NR SUL combination power class 2

maxUplinkDutyCycle-SULcombination-PC2-r17 ENUMERATED {n50, n60, n70, n80, n90, n100} OPTIONAL,

beamManagementType-CBM-r17 ENUMERATED {supported} OPTIONAL,

-- R1 25-18: Parallel PUCCH and PUSCH transmission across CCs in inter-band CA

parallelTxPUCCH-PUSCH-r17 ENUMERATED {supported} OPTIONAL,

-- R1 23-9-5 Active CSI-RS resources and ports for mixed codebook types in any slot per band combination

codebookComboParameterMixedTypePerBC-r17 CodebookComboParameterMixedTypePerBC-r17 OPTIONAL,

-- R1 23-7-1 Basic Features of CSI Enhancement for Multi-TRP

mTRP-CSI-EnhancementPerBC-r17 SEQUENCE {

maxNumNZP-CSI-RS-r17 INTEGER (2..8),

cSI-Report-mode-r17 ENUMERATED {mode1, mode2, both},

supportedComboAcrossCCs-r17 SEQUENCE (SIZE (1..16)) OF CSI-MultiTRP-SupportedCombinations-r17,

codebookMode-NCJT-r17 ENUMERATED{mode1,mode1And2}

} OPTIONAL,

-- R1 23-7-1b Active CSI-RS resources and ports in the presence of multi-TRP CSI

codebookComboParameterMultiTRP-PerBC-r17 CodebookComboParameterMultiTRP-PerBC-r17 OPTIONAL,

-- R1 24-8b: 32 DL HARQ processes for FR 2-2 - maximum number of component carriers

maxCC-32-DL-HARQ-ProcessFR2-2-r17 ENUMERATED {n1, n2, n3, n4, n6, n8, n16, n32} OPTIONAL,

-- R1 24-9b: 32 UL HARQ processes for FR 2-2 - maximum number of component carriers

maxCC-32-UL-HARQ-ProcessFR2-2-r17 ENUMERATED {n1, n2, n3, n4, n5, n8, n16, n32} OPTIONAL,

-- R1 34-2: Cross-carrier scheduling from SCell to PCell/PSCell (Type B)

crossCarrierSchedulingSCell-SpCellTypeB-r17 CrossCarrierSchedulingSCell-SpCell-r17 OPTIONAL,

-- R1 34-1: Cross-carrier scheduling from SCell to PCell/PSCell with search space restrictions (Type A)

crossCarrierSchedulingSCell-SpCellTypeA-r17 CrossCarrierSchedulingSCell-SpCell-r17 OPTIONAL,

-- R1 34-1a: DCI formats on PCell/PSCell USS set(s) support

dci-FormatsPCellPSCellUSS-Sets-r17 ENUMERATED {supported} OPTIONAL,

-- R1 34-3: Disabling scaling factor alpha when sSCell is deactivated

disablingScalingFactorDeactSCell-r17 ENUMERATED {supported} OPTIONAL,

-- R1 34-4: Disabling scaling factor alpha when sSCell is deactivated

disablingScalingFactorDormantSCell-r17 ENUMERATED {supported} OPTIONAL,

-- R1 34-5: Non-aligned frame boundaries between PCell/PSCell and sSCell

non-AlignedFrameBoundaries-r17 SEQUENCE {

scs15kHz-15kHz-r17 BIT STRING (SIZE (1..496)) OPTIONAL,

scs15kHz-30kHz-r17 BIT STRING (SIZE (1..496)) OPTIONAL,

scs15kHz-60kHz-r17 BIT STRING (SIZE (1..496)) OPTIONAL,

scs30kHz-30kHz-r17 BIT STRING (SIZE (1..496)) OPTIONAL,

scs30kHz-60kHz-r17 BIT STRING (SIZE (1..496)) OPTIONAL,

scs60kHz-60kHz-r17 BIT STRING (SIZE (1..496)) OPTIONAL

} OPTIONAL

}

CA-ParametersNR-v1720 ::= SEQUENCE {

-- R1 39-1: Parallel SRS and PUCCH/PUSCH transmission across CCs in intra-band non-contiguous CA

parallelTxSRS-PUCCH-PUSCH-intraBand-r17 ENUMERATED {supported} OPTIONAL,

-- R1 39-2: Parallel PRACH and SRS/PUCCH/PUSCH transmissions across CCs in intra-band non-contiguous CA

parallelTxPRACH-SRS-PUCCH-PUSCH-intraBand-r17 ENUMERATED {supported} OPTIONAL,

-- R1 25-9: Semi-static PUCCH cell switching for a single PUCCH group only

semiStaticPUCCH-CellSwitchSingleGroup-r17 SEQUENCE {

pucch-Group-r17 ENUMERATED {primaryGroupOnly, secondaryGroupOnly, eitherPrimaryOrSecondaryGroup},

pucch-Group-Config-r17 PUCCH-Group-Config-r17

} OPTIONAL,

-- R1 25-9a: Semi-static PUCCH cell switching for two PUCCH groups

semiStaticPUCCH-CellSwitchTwoGroups-r17 SEQUENCE (SIZE (1..maxTwoPUCCH-Grp-ConfigList-r17)) OF TwoPUCCH-Grp-Configurations-r17 OPTIONAL,

-- R1 25-10: PUCCH cell switching based on dynamic indication for same length of overlapping PUCCH slots/sub-slots for a single

-- PUCCH group only

dynamicPUCCH-CellSwitchSameLengthSingleGroup-r17 SEQUENCE {

pucch-Group-r17 ENUMERATED {primaryGroupOnly, secondaryGroupOnly, eitherPrimaryOrSecondaryGroup},

pucch-Group-Config-r17 PUCCH-Group-Config-r17

} OPTIONAL,

-- R1 25-10a: PUCCH cell switching based on dynamic indication for different length of overlapping PUCCH slots/sub-slots

-- for a single PUCCH group only

dynamicPUCCH-CellSwitchDiffLengthSingleGroup-r17 SEQUENCE {

pucch-Group-r17 ENUMERATED {primaryGroupOnly, secondaryGroupOnly, eitherPrimaryOrSecondaryGroup},

pucch-Group-Config-r17 PUCCH-Group-Config-r17

} OPTIONAL,

-- R1 25-10b: PUCCH cell switching based on dynamic indication for same length of overlapping PUCCH slots/sub-slots for two PUCCH

-- groups

dynamicPUCCH-CellSwitchSameLengthTwoGroups-r17 SEQUENCE (SIZE (1..maxTwoPUCCH-Grp-ConfigList-r17)) OF TwoPUCCH-Grp-Configurations-r17

OPTIONAL,

-- R1 25-10c: PUCCH cell switching based on dynamic indication for different length of overlapping PUCCH slots/sub-slots for two

-- PUCCH groups

dynamicPUCCH-CellSwitchDiffLengthTwoGroups-r17 SEQUENCE (SIZE (1..maxTwoPUCCH-Grp-ConfigList-r17)) OF TwoPUCCH-Grp-Configurations-r17

OPTIONAL,

-- R1 33-2a: ACK/NACK based HARQ-ACK feedback and RRC-based enabling/disabling ACK/NACK-based

-- feedback for dynamic scheduling for multicast

ack-NACK-FeedbackForMulticast-r17 ENUMERATED {supported} OPTIONAL,

-- R1 33-2d: PTP retransmission for multicast dynamic scheduling

ptp-Retx-Multicast-r17 ENUMERATED {supported} OPTIONAL,

-- R1 33-4: NACK-only based HARQ-ACK feedback for RRC-based enabling/disabling multicast with ACK/NACK transforming

nack-OnlyFeedbackForMulticast-r17 ENUMERATED {supported} OPTIONAL,

-- R1 33-4a: NACK-only based HARQ-ACK feedback for multicast corresponding to a specific sequence or a PUCCH transmission

nack-OnlyFeedbackSpecificResourceForMulticast-r17 ENUMERATED {supported} OPTIONAL,

-- R1 33-5-1a: ACK/NACK based HARQ-ACK feedback and RRC-based enabling/disabling ACK/NACK-based feedback

-- for SPS group-common PDSCH for multicast

ack-NACK-FeedbackForSPS-Multicast-r17 ENUMERATED {supported} OPTIONAL,

-- R1 33-5-1d: PTP retransmission for SPS group-common PDSCH for multicast

ptp-Retx-SPS-Multicast-r17 ENUMERATED {supported} OPTIONAL,

-- R4 26-1: Higher Power Limit CA DC

higherPowerLimit-r17 ENUMERATED {supported} OPTIONAL,

-- R1 39-4: Parallel MsgA and SRS/PUCCH/PUSCH transmissions across CCs in intra-band non-contiguous CA

parallelTxMsgA-SRS-PUCCH-PUSCH-intraBand-r17 ENUMERATED {supported} OPTIONAL,

-- R1 24-11a: Capability on the number of CCs for monitoring a maximum number of BDs and non-overlapped CCEs per span when

-- configured with DL CA with Rel-17 PDCCH monitoring capability on all the serving cells

pdcch-MonitoringCA-r17 INTEGER (4..16) OPTIONAL,

-- R1 24-11f: Capability on the number of CCs for monitoring a maximum number of BDs and non-overlapped CCEs for MCG and for SCG

-- when configured for NR-DC operation with Rel-17 PDCCH monitoring capability on all the serving cells

pdcch-BlindDetectionMCG-SCG-List-r17 SEQUENCE(SIZE(1..maxNrofPdcch-BlindDetection-r17)) OF PDCCH-BlindDetectionMCG-SCG-r17

OPTIONAL,

-- R1 24-11c: Number of carriers for CCE/BD scaling with DL CA with mix of Rel. 17 and Rel. 15 PDCCH monitoring capabilities on

-- different Carriers

-- R1 24-11g: Number of carriers for CCE/BD scaling for MCG and for SCG when configured for NR-DC operation with mix of Rel. 17 and

-- Rel. 15 PDCCH monitoring capabilities on different carriers

pdcch-BlindDetectionMixedList1-r17 SEQUENCE(SIZE(1..maxNrofPdcch-BlindDetection-r17)) OF PDCCH-BlindDetectionMixed-r17

OPTIONAL,

-- R1 24-11d: Number of carriers for CCE/BD scaling with DL CA with mix of Rel. 17 and Rel. 16 PDCCH monitoring capabilities on

-- different Carriers

-- R1 24-11h: Number of carriers for CCE/BD scaling for MCG and for SCG when configured for NR-DC operation with mix of Rel. 17 and

-- Rel. 16 PDCCH monitoring capabilities on different carriers

pdcch-BlindDetectionMixedList2-r17 SEQUENCE(SIZE(1..maxNrofPdcch-BlindDetection-r17)) OF PDCCH-BlindDetectionMixed-r17

OPTIONAL,

-- R1 24-11e: Number of carriers for CCE/BD scaling with DL CA with mix of Rel. 17, Rel. 16 and Rel. 15 PDCCH monitoring

-- capabilities on different carriers

-- R1 24-11i: Number of carriers for CCE/BD scaling for MCG and for SCG when configured for NR-DC operation with mix of Rel. 17,

-- Rel. 16 and Rel. 15 PDCCH monitoring capabilities on different carriers

pdcch-BlindDetectionMixedList3-r17 SEQUENCE(SIZE(1..maxNrofPdcch-BlindDetection-r17)) OF PDCCH-BlindDetectionMixed1-r17

OPTIONAL

}

CA-ParametersNR-v1730 ::= SEQUENCE {

-- R1 30-4a: DM-RS bundling for PUSCH repetition type A (per BC)

dmrs-BundlingPUSCH-RepTypeAPerBC-r17 ENUMERATED {supported} OPTIONAL,

-- R1 30-4b: DM-RS bundling for PUSCH repetition type B(per BC)

dmrs-BundlingPUSCH-RepTypeBPerBC-r17 ENUMERATED {supported} OPTIONAL,

-- R1 30-4c: DM-RS bundling for TB processing over multi-slot PUSCH(per BC)

dmrs-BundlingPUSCH-multiSlotPerBC-r17 ENUMERATED {supported} OPTIONAL,

-- R1 30-4d: DMRS bundling for PUCCH repetitions(per BC)

dmrs-BundlingPUCCH-RepPerBC-r17 ENUMERATED {supported} OPTIONAL,

-- R1 30-4g: Restart DM-RS bundling (per BC)

dmrs-BundlingRestartPerBC-r17 ENUMERATED {supported} OPTIONAL,

-- R1 30-4h: DM-RS bundling for non-back-to-back transmission (per BC)

dmrs-BundlingNonBackToBackTX-PerBC-r17 ENUMERATED {supported} OPTIONAL,

-- R1 39-3-1: Stay on the target CC for SRS carrier switching

stayOnTargetCC-SRS-CarrierSwitch-r17 ENUMERATED {supported} OPTIONAL,

-- R1 33-3-3a: FDM-ed Type-1 and Type-2 HARQ-ACK codebooks for multiplexing HARQ-ACK for unicast and HARQ-ACK for multicast

fdm-CodebookForMux-UnicastMulticastHARQ-ACK-r17 ENUMERATED {supported} OPTIONAL,

-- R1 33-3-3b: Mode 2 TDM-ed Type-1 and Type-2 HARQ-ACK codebook for multiplexing HARQ-ACK for unicast and HARQ-ACK for multicast

mode2-TDM-CodebookForMux-UnicastMulticastHARQ-ACK-r17 ENUMERATED {supported} OPTIONAL,

-- R1 33-3-4: Mode 1 for type1 codebook generation

mode1-ForType1-CodebookGeneration-r17 ENUMERATED {supported} OPTIONAL,

-- R1 33-5-1j: NACK-only based HARQ-ACK feedback for multicast corresponding to a specific sequence or a PUCCH transmission

-- for SPS group-commmon PDSCH for multicast

nack-OnlyFeedbackSpecificResourceForSPS-Multicast-r17 ENUMERATED {supported} OPTIONAL,

-- R1 33-8-2: Up to 2 PUCCH resources configuration for multicast feedback for dynamically scheduled multicast

multiPUCCH-ConfigForMulticast-r17 ENUMERATED {supported} OPTIONAL,

-- R1 33-8-3: PUCCH resource configuration for multicast feedback for SPS GC-PDSCH

pucch-ConfigForSPS-Multicast-r17 ENUMERATED {supported} OPTIONAL,

-- The following parameter is associated with R1 33-2a, R1 33-3-3a, and R1 33-3-3b, and is not a RAN1 FG.

maxNumberG-RNTI-HARQ-ACK-Codebook-r17 INTEGER (1..4) OPTIONAL,

-- R1 33-3-5: Feedback multiplexing for unicast PDSCH and group-common PDSCH for multicast with same priority and different codebook

-- type

mux-HARQ-ACK-UnicastMulticast-r17 ENUMERATED {supported} OPTIONAL

}

CA-ParametersNR-v1740 ::= SEQUENCE {

-- R1 33-5-1f: NACK-only based HARQ-ACK feedback for multicast RRC-based enabling/disabling NACK-only based feedback

-- for SPS group-common PDSCH for multicast

nack-OnlyFeedbackForSPS-Multicast-r17 ENUMERATED {supported} OPTIONAL,

-- R1 33-8-1: PUCCH resource configuration for multicast feedback for dynamically scheduled multicast

singlePUCCH-ConfigForMulticast-r17 ENUMERATED {supported} OPTIONAL

}

CA-ParametersNR-v1760 ::= SEQUENCE {

prioSCellPRACH-OverSP-PeriodicSRS-Support-r17 ENUMERATED {supported} OPTIONAL

}

CA-ParametersNR-v1770 ::= SEQUENCE {

parallelTxPUCCH-PUSCH-SamePriority-r17 ENUMERATED {supported} OPTIONAL

}

CA-ParametersNR-v1780 ::= SEQUENCE {

parallelTxPUCCH-PUSCH-SamePriority-r17 ENUMERATED {supported} OPTIONAL,

supportedAggBW-FR1-r17 SEQUENCE {

scalingFactorSCS-r17 ENUMERATED {true} OPTIONAL,

supportedAggBW-FDD-DL-r17 SupportedAggBandwidth-r17 OPTIONAL,

supportedAggBW-FDD-UL-r17 SupportedAggBandwidth-r17 OPTIONAL,

supportedAggBW-TDD-DL-r17 SupportedAggBandwidth-r17 OPTIONAL,

supportedAggBW-TDD-UL-r17 SupportedAggBandwidth-r17 OPTIONAL,

supportedAggBW-TotalDL-r17 SupportedAggBandwidth-r17 OPTIONAL,

supportedAggBW-TotalUL-r17 SupportedAggBandwidth-r17 OPTIONAL

} OPTIONAL

}

CA-ParametersNR-v1800 ::= SEQUENCE {

codebookParametersetype2DopplerCSI-PerBC-r18 CodebookParametersetype2DopplerCSI-r18 OPTIONAL,

codebookParametersfetype2DopplerCSI-PerBC-r18 CodebookParametersfetype2DopplerCSI-r18 OPTIONAL,

codebookParametersetype2CJT-PerBC-r18 CodebookParametersetype2CJT-r18 OPTIONAL,

codebookParametersfetype2CJT-PerBC-r18 CodebookParametersfetype2CJT-r18 OPTIONAL,

codebookComboParametersCJT-PerBC-r18 CodebookComboParametersCJT-r18 OPTIONAL,

codebookParametersHARQ-ACK-PUSCH-PerBC-r18 CodebookParametersHARQ-ACK-PUSCH-r18 OPTIONAL,

-- R1 40-2-8: Maximum number of TAGs across all CCs

maxNumberTAG-AcrossCC-r18 INTEGER (2..4) OPTIONAL,

-- R1 40-3-3-1: TDCP (Time Domain Channel Properties) report

tdcp-ReportPerBC-r18 SEQUENCE {

valueX-r18 INTEGER (1..2),

maxNumberActiveResource-r18 INTEGER (2..32)

} OPTIONAL,

-- R1 40-3-3-5: Number of CSI-RS resources for TDCP

tdcp-ResourcePerBC-r18 SEQUENCE {

maxNumberConfigPerCC-r18 ENUMERATED {n2,n4,n6,n8,n10,n12},

maxNumberConfigAcrossCC-r18 INTEGER (1..32),

maxNumberSimultaneousPerCC-r18 ENUMERATED {n2, n4, n6, n8, n12, n16, n20, n24, n28, n32}

} OPTIONAL,

-- R1 40-3-1-24: Timeline for regular eType-II-CJT CSI, or for port selection FeType-II-CJT CSI

timelineRelax-CJT-CSI-CA-r18 ENUMERATED {n0,n2} OPTIONAL,

-- R1 42-1: Spatial domain adaptation with CSI feedback based on CSI report sub-configuration(s) for periodic CSI reporting

spatialAdaptation-CSI-FeedbackPerBC-r18 SEQUENCE {

maxNumberCSI-ResourceAcrossCC-r18 SEQUENCE {

sdType1-Resource-r18 ENUMERATED {n5, n6, n7, n8, n9, n10, n12, n14, n16, n18, n20, n22,

n24, n26, n28, n30, n32, n34, n36, n38, n40, n42, n44,

n46, n48, n50, n52, n54, n56, n58, n60, n62, n64},

sdType2-Resource-r18 ENUMERATED {n5, n6, n7, n8, n9, n10, n12, n14, n16, n18, n20, n22,

n24, n26, n28, n30, n32, n34, n36, n38, n40, n42, n44,

n46, n48, n50, n52, n54, n56, n58, n60, n62, n64}

},

maxNumberPortsAcrossCC-r18 SEQUENCE {

sdType1-Resource-r18 INTEGER (1..32),

sdType2-Resource-r18 INTEGER (1..32)

}

} OPTIONAL,

-- R1 40-7-2a: Association between CSI-RS and SRS for non-codebook case

nonCodebook-CSI-RS-SRS-PerBC-r18 SEQUENCE (SIZE (1.. maxNrofCSI-RS-Resources)) OF SupportedCSI-RS-Resource OPTIONAL,

-- R1 42-1a: Spatial domain adaptation with CSI feedback based on CSI report sub-configuration(s) for periodic CSI reporting on

-- PUSCH

spatialAdaptation-CSI-FeedbackPUSCH-PerBC-r18 SEQUENCE {

maxNumberCSI-ResourceAcrossCC-r18 ENUMERATED {n5, n6, n7, n8, n9, n10, n12, n14, n16, n18, n20, n22, n24, n26, n28,

n30, n32, n34, n36, n38, n40, n42, n44, n46, n48, n50, n52, n54,

n56, n58, n60, n62, n64},

maxNumberPortsAcrossCC-r18 INTEGER (1..32)

} OPTIONAL,

-- R1 42-1b: Spatial domain adaptation with CSI feedback based on CSI report sub-configuration(s) for aperiodic CSI reporting

spatialAdaptation-CSI-FeedbackAperiodicPerBC-r18 SEQUENCE {

maxNumberCSI-ResourceAcrossCC-r18 SEQUENCE {

sdType1-Resource-r18 ENUMERATED {n5, n6, n7, n8, n9, n10, n12, n14, n16, n18, n20, n22,

n24, n26, n28, n30, n32, n34, n36, n38, n40, n42, n44,

n46, n48, n50, n52, n54, n56, n58, n60, n62, n64},

sdType2-Resource-r18 ENUMERATED {n5, n6, n7, n8, n9, n10, n12, n14, n16, n18, n20, n22,

n24, n26, n28, n30, n32, n34, n36, n38, n40, n42, n44,

n46, n48, n50, n52, n54, n56, n58, n60, n62, n64}

},

maxNumberPortsAcrossCC-r18 SEQUENCE {

sdType1-Resource-r18 INTEGER (1..32),

sdType2-Resource-r18 INTEGER (1..32) }

} OPTIONAL,

-- R1 42-1c: Spatial domain adaptation with CSI feedback based on CSI report sub-configuration(s) for semi-persistent CSI

-- reporting on PUCCH

spatialAdaptation-CSI-FeedbackPUCCH-PerBC-r18 SEQUENCE {

maxNumberCSI-ResourceAcrossCC-r18 ENUMERATED {n5, n6, n7, n8, n9, n10, n12, n14, n16, n18, n20, n22, n24, n26, n28,

n30, n32, n34, n36, n38, n40, n42, n44, n46, n48, n50, n52, n54,

n56, n58, n60, n62, n64},

maxNumberPortsAcrossCC-r18 INTEGER (1..32)

} OPTIONAL,

-- R1 42-2: Spatial domain adaptation with CSI feedback based on CSI report sub-configuration(s) for periodic CSI reporting

powerAdaptation-CSI-FeedbackPerBC-r18 SEQUENCE {

maxNumberCSI-ResourceAcrossCC-r18 ENUMERATED {n5, n6, n7, n8, n9, n10, n12, n14, n16, n18, n20, n22, n24, n26, n28,

n30, n32, n34, n36, n38, n40, n42, n44, n46, n48, n50, n52, n54,

n56, n58, n60, n62, n64},

maxNumberPortsAcrossCC-r18 INTEGER (1..32)

} OPTIONAL,

-- R1 42-2a: Spatial domain adaptation with CSI feedback based on CSI report sub-configuration(s) for periodic CSI reporting on PUSCH

powerAdaptation-CSI-FeedbackPUSCH-PerBC-r18 SEQUENCE {

maxNumberCSI-ResourceAcrossCC-r18 ENUMERATED {n5, n6, n7, n8, n9, n10, n12, n14, n16, n18, n20, n22, n24, n26, n28,

n30, n32, n34, n36, n38, n40, n42, n44, n46, n48, n50, n52, n54,

n56, n58, n60, n62, n64},

maxNumberPortsAcrossCC-r18 INTEGER (1..32)

} OPTIONAL,

-- R1 42-2b: Spatial domain adaptation with CSI feedback based on CSI report sub-configuration(s) for aperiodic CSI reporting

powerAdaptation-CSI-FeedbackAperiodicPerBC-r18 SEQUENCE {

maxNumberCSI-ResourceAcrossCC-r18 ENUMERATED {n5, n6, n7, n8, n9, n10, n12, n14, n16, n18, n20, n22, n24, n26, n28,

n30, n32, n34, n36, n38, n40, n42, n44, n46, n48, n50, n52, n54,

n56, n58, n60, n62, n64},

maxNumberPortsAcrossCC-r18 INTEGER (1..32)

} OPTIONAL,

-- R1 42-2c: Spatial domain adaptation with CSI feedback based on CSI report sub-configuration(s) for semi-persistent CSI

-- reporting on PUCCH

powerAdaptation-CSI-FeedbackPUCCH-PerBC-r18 SEQUENCE {

maxNumberCSI-ResourceAcrossCC-r18 ENUMERATED {n5, n6, n7, n8, n9, n10, n12, n14, n16, n18, n20, n22, n24, n26, n28,

n30, n32, n34, n36, n38, n40, n42, n44, n46, n48, n50, n52, n54,

n56, n58, n60, n62, n64},

maxNumberPortsAcrossCC-r18 INTEGER (1..32)

} OPTIONAL,

-- R1 42-7: Mixed codebook combination for spatial domain adaptation with CSI feedback based on CSI report sub-configuration(s),

-- each containing one port subset configuration

mixCodeBookSpatialAdaptationPerBC-r18 SEQUENCE (SIZE (1.. maxNrofCSI-RS-Resources)) OF SupportedCSI-RS-Resource OPTIONAL,

-- R1 42-9: Indicates whether the UE supports CSI report framework and the number of CSI report(s) which the UE can

-- simultaneously process across all CCs, and across MCG and SCG in case of NR-DC.

simultaneousCSI-SubReportsAllCC-r18 INTEGER (5..32) OPTIONAL,

-- R1 49-1: Multi-cell PDSCH scheduling by DCI format 1\_3 on a scheduling cell with same SCS between scheduling

-- cell and cells in the set

multiCell-PDSCH-DCI-1-3-SameSCS-r18 SEQUENCE {

coScheduledCellSCS-r18 SEQUENCE {

nonSharedSpectrum-fdd-fr1 ENUMERATED {supported} OPTIONAL,

nonSharedSpectrum-tdd-fr1 ENUMERATED {supported} OPTIONAL,

sharedSpectrum-tdd-fr1 ENUMERATED {supported} OPTIONAL,

fr2-1 ENUMERATED {supported} OPTIONAL,

fr2-2 ENUMERATED {supported} OPTIONAL

},

maxNumberCoScheduledCell-r18 INTEGER (2..4),

maxNumberSetsOfCellAcrossPUCCH-Group-r18 INTEGER (1..8),

maxNumberSetsOfCellScheduling-r18 INTEGER (1..4),

harqFeedbackType-r18 ENUMERATED {type1, type2, type1And2},

coScheduledCellIndicationScheme-r18 ENUMERATED {fdra,cellInd, both},

supportOfSearchSpace-r18 ENUMERATED {supported} OPTIONAL,

licensed-fdd-tdd-fr1-r18 ENUMERATED {supported} OPTIONAL

} OPTIONAL,

-- R1 49-1b: Multi-cell PDSCH scheduling by DCI format 1\_3 on a scheduling cell not included in a set of cells with different

-- SCS/carrier type between scheduling cell and cells in the set

multiCell-PDSCH-DCI-1-3-DiffSCS-r18 SEQUENCE {

coScheduledCellSCS-r18 ENUMERATED {lowScheduling-highScheduled, highScheduling-lowScheduled, both},

combinationCarrierType-r18 SEQUENCE (SIZE(1..maxSchedulingBandCombination-r18)) OF

CombinationCarrierType-r18,

maxNumberCoScheduledCell-r18 INTEGER (2..4),

maxNumberSetsOfCellAcrossPUCCH-Group-r18 INTEGER (1..8),

maxNumberSetsOfCellScheduling-r18 INTEGER (1..4),

harqFeedbackType-r18 ENUMERATED {type1, type2, type1And2},

coScheduledCellIndicationScheme-r18 ENUMERATED {fdra,cellInd, both}

} OPTIONAL,

-- R1 49-2: Multi-cell PUSCH scheduling by DCI format 0\_3 on a scheduling cell with same SCS between scheduling cell

-- and cells in the set

multiCell-PUSCH-DCI-0-3-SameSCS-r18 SEQUENCE {

coScheduledCellSCS-r18 SEQUENCE {

nonSharedSpectrum-fdd-fr1 ENUMERATED {supported} OPTIONAL,

nonSharedSpectrum-tdd-fr1 ENUMERATED {supported} OPTIONAL,

sharedSpectrum-tdd-fr1 ENUMERATED {supported} OPTIONAL,

fr2-1 ENUMERATED {supported} OPTIONAL,

fr2-2 ENUMERATED {supported} OPTIONAL

},

maxNumberCoScheduledCell-r18 INTEGER (2..4),

maxNumberSetsOfCellAcrossPUCCH-Group-r18 INTEGER (1..8),

maxNumberSetsOfCellScheduling-r18 INTEGER (1..4),

coScheduledCellIndicationScheme-r18 ENUMERATED {fdra,cellInd, both},

supportOfSearchSpace-r18 ENUMERATED {supported} OPTIONAL,

licensed-fdd-tdd-fr1-r18 ENUMERATED {supported} OPTIONAL

} OPTIONAL,

-- R1 49-2b: Multi-cell PUSCH scheduling by DCI format 0\_3 on a scheduling cell not included in a set of cells with

-- different SCS/carrier type between scheduling cell and cells in the set

multiCell-PUSCH-DCI-0-3-DiffSCS-r18 SEQUENCE {

coScheduledCellSCS-r18 ENUMERATED {lowScheduling-highScheduled, highScheduling-lowScheduled, both},

combinationCarrierType-r18 SEQUENCE (SIZE(1..maxSchedulingBandCombination-r18)) OF

CombinationCarrierType-r18,

maxNumberCoScheduledCell-r18 INTEGER (2..4),

maxNumberSetsOfCellAcrossPUCCH-Group-r18 INTEGER (1..8),

maxNumberSetsOfCellScheduling-r18 INTEGER (1..4),

coScheduledCellIndicationScheme-r18 ENUMERATED {fdra,cellInd, both}

} OPTIONAL,

-- R1 49-3x: Advanced UE capability for larger number of unicast DL DCI

advUnicastDCI-DL-r18 SEQUENCE {

scs-15kHz-120kHz-r18 ENUMERATED {n2, n4} OPTIONAL,

scs-15kHz-60kHz-r18 ENUMERATED {n2, n4} OPTIONAL,

scs-30kHz-120kHz-r18 ENUMERATED {n2, n4} OPTIONAL,

scs-15kHz-30kHz-r18 ENUMERATED {n2} OPTIONAL,

scs-30kHz-60kHz-r18 ENUMERATED {n2} OPTIONAL,

scs-60kHz-120kHz-r18 ENUMERATED {n2} OPTIONAL

} OPTIONAL,

-- R1 49-3y: Advanced UE capability for larger number of unicast UL DCI

advUnicastDCI-UL-r18 SEQUENCE {

scs-15kHz-120kHz-r18 ENUMERATED {n2, n4} OPTIONAL,

scs-15kHz-60kHz-r18 ENUMERATED {n2, n4} OPTIONAL,

scs-30kHz-120kHz-r18 ENUMERATED {n2, n4} OPTIONAL,

scs-15kHz-30kHz-r18 ENUMERATED {n2} OPTIONAL,

scs-30kHz-60kHz-r18 ENUMERATED {n2} OPTIONAL,

scs-60kHz-120kHz-r18 ENUMERATED {n2} OPTIONAL

} OPTIONAL,

-- R1 49-5a: Trigger Type 3 HARQ CB based feedback using DCI format 1\_3

type3HARQ-CB-DCI-1-3-r18 ENUMERATED {supported} OPTIONAL,

-- R1 49-5b: Trigger enhanced Type 3 HARQ CB based feedback using DCI format 1\_3

type3EnhHARQ-CB-DCI-1-3-r18 SEQUENCE {

numberOfCodebook-r18 ENUMERATED {n1, n2, n4, n8},

maxNumberPUCCH-Trans-r18 INTEGER (1..7)

} OPTIONAL,

-- R1 49-9: SCell dormancy indication within active time in DCI format 0\_3/1\_3

scellDormancyWithinActiveTime-DCI-0-3-And-1-3-r18 ENUMERATED {supported} OPTIONAL,

pdcch-MonitoringCA-Ext-r18 CHOICE {

-- R1 55-6a: Capability on the number of CCs for monitoring a maximum number of BDs and non-overlapped CCEs per span when

-- configured with DL CA with Rel-16 PDCCH monitoring capability on all the serving cells

pdcch-MonitoringCA-r18 SEQUENCE {

maxNumberOfMonitoringCC-r18 INTEGER (2..16),

supportedSpanArrangement-r18 ENUMERATED {alignedOnly, alignedAndNonAligned}

},

-- R1 55-6f: Capability on the number of CCs for monitoring a maximum number of BDs and non-overlapped CCEs per span when

-- configured with DL CA with Rel-16 PDCCH monitoring capability on all the serving cells with restriction for non-aligned

-- span case

pdcch-MonitoringCA-NonAlignedSpan-r18 INTEGER (2..16)

} OPTIONAL,

pdcch-BlindDetectionCA-MixedExt-r18 CHOICE {

-- R1 55-6c: Number of carriers for CCE/BD scaling with DL CA with mix of Rel. 16 and Rel. 15 PDCCH monitoring capabilities on

-- different carriers

pdcch-BlindDetectionCA-Mixed-r18 SEQUENCE {

blindDetectionCA-Mixed-r18 SEQUENCE(SIZE (1..maxNrofPdcch-BlindDetectionMixed-1-r16)) OF

PDCCH-BlindDetectionCA-MixedExt-r16,

supportedSpanArrangement-r18 ENUMERATED{ alignedOnly, alignedAndNonAligned }

},

-- R1 55-6g: Number of carriers for CCE/BD scaling with DL CA with mix of Rel. 16 and Rel. 15 PDCCH monitoring capabilities on

-- different carriers with restriction for non-aligned span case

pdcch-BlindDetectionCA-Mixed-NonAlignedSpan-r18 SEQUENCE(SIZE (1..maxNrofPdcch-BlindDetectionMixed-1-r16)) OF

PDCCH-BlindDetectionCA-MixedExt-r16

} OPTIONAL,

-- R1 55-6e: Number of carriers for CCE/BD scaling for MCG and for SCG when configured for NR-DC operation with mix of Rel. 16

-- and Rel. 15 PDCCH monitoring capabilities on different carriers

pdcch-BlindDetectionMCG-SCG-List-r18 SEQUENCE(SIZE (1..maxNrofPdcch-BlindDetectionMixed-1-r16)) OF

PDCCH-BlindDetectionMixed2-r18 OPTIONAL,

-- R4 33-1: Support of intra-band non-collocated NR CA operation

intraBandNR-CA-non-collocated-r18 ENUMERATED {supported} OPTIONAL

}

CA-ParametersNR-v1830 ::= SEQUENCE {

-- R1 45-1: Intra-frequency L1 measurement and reports for L1-L2 Triggered Mobility (LTM) procedure

intraFreqL1-MeasConfig-r18 SEQUENCE {

supportedMaxIntraFreqCellsConfig-r18 INTEGER (1..8),

supportedMaxIntraFreqCellsPerReport-r18 INTEGER (1..4),

supportedMaxReportBeamsPerReportedCell-r18 INTEGER (1..4),

supportedMaxReportBeamsReports-r18 ENUMERATED {n1,n2,n3,n4,n6,n8,n9,n12,n16},

supportedMaxAperiodic-LTM-CSI-ReportConfig-r18 INTEGER (0..4),

supportedMaxPeriodic-LTM-CSI-ReportConfig-r18 INTEGER (1..4),

supportedMaxSemiPersistent-LTM-CSI-ReportConfig-r18 INTEGER (0..4)

} OPTIONAL,

-- R1 45-1a: Inter-frequency L1 measurement and reports for L1-L2 Triggered Mobility (LTM) procedure

interFreqL1-MeasConfig-r18 SEQUENCE {

supportedMaxIntraInterFreqCellsConfig-r18 INTEGER (1..8),

supportedMaxIntraInterFreqCellsPerReport-r18 INTEGER (1..4),

supportedMaxIntraInterFreqBeamsPerCellReports-r18 INTEGER (1..4),

supportedMaxIntraInterFreqBeamsReports-r18 ENUMERATED {n1,n2,n3,n4,n6,n8,n9,n12,n16}

} OPTIONAL,

-- R1 45-2: Inclusion of current SpCell in the L1 measurement report

currentSpCellInclL1-Report-r18 ENUMERATED {supported} OPTIONAL,

-- R4 39-1: SSB based L1-RSRP measurements for multiple cells with RTD > CP

multiCellL1-measRTD-greaterThan-CP-r18 ENUMERATED {supported} OPTIONAL,

-- R4 39-2: SSB based inter-frequency L1-RSRP measurements without measurement gaps

interFreqSSB-L1-MeasWithoutGaps-r18 ENUMERATED {supported} OPTIONAL,

-- R4 39-3-1: Number of frequency layers for L1-RSRP measurement

maxFreqLayersL1-Meas-r18 SEQUENCE {

supportedMaxIntraInterFreqLayersWithoutGaps-r18 INTEGER (1..8) OPTIONAL,

supportedMaxInterFreqLayersWithGaps-r18 INTEGER (1..8) OPTIONAL

} OPTIONAL,

-- R4 39-3-2: Number of neighbour cells to be measured per frequency layer

maxNeighCellsPerFreqLayerL1-Meas-r18 SEQUENCE {

supportedMaxNeighCellsPerFreqLayersWithoutGaps-r18 INTEGER (1..8) OPTIONAL,

supportedMaxNeighCellsPerFreqLayersWithGaps-r18 INTEGER (1..8) OPTIONAL

} OPTIONAL,

-- R4 39-3-3: Number of total cells to be measured

supportedMaxCellsWithoutGapsL1-Meas-r18 INTEGER (1..24) OPTIONAL,

-- R4 39-3-4: Number of SSB resources for L1-RSRP measurement within a slot

supportedMaxSSB-WithinSlotL1-Meas-r18 ENUMERATED {n1,n2,n3,n4,n5,n6,n7,n8,n16,n32,n48,n64} OPTIONAL,

dummy SEQUENCE {

supportedMaxSSB-PerFreqLayerWithoutGaps-r18 INTEGER (1..8) OPTIONAL,

supportedMaxSSB-PerFreqLayerWithGaps-r18 INTEGER (1..8) OPTIONAL

} OPTIONAL,

-- R4 39-3-6: Number of total SSB resources to be measured

supportedMaxSSB-L1-Meas-r18 ENUMERATED {n2,n4,n8,n12,n16,n32,n64} OPTIONAL,

-- R1 49-13: Default QCL assumption for multi-cell scheduling by DCI format 1\_3

qcl-MultiCellDCI-1-3-r18 ENUMERATED {diff, both} OPTIONAL,

-- R1 49-14: Support of BWP switch indication by DCI format 0\_3/1\_3

bwp-SwitchingDCI-0-3-And-1-3-r18 ENUMERATED {supported} OPTIONAL

}

CA-ParametersNR-v1860 ::= SEQUENCE {

-- R4 39-3-5: Number of SSB resources for L1-RSRP measurement per frequency layer

maxSSB-PerFreqLayerL1-Meas-r18 SEQUENCE {

supportedMaxSSB-PerFreqLayerWithoutGaps-r18 ENUMERATED {n1,n2,n3,n4,n5,n6,n7,n8,n12,n16,n20,n24} OPTIONAL,

supportedMaxSSB-PerFreqLayerWithGaps-r18 INTEGER (1..8) OPTIONAL

} OPTIONAL

}

CA-ParametersNR-v1900 ::= SEQUENCE {

codebookParametersType1SP-SchemeA-PerBC-r19 CodebookParametersType1SP-SchemeA-r19 OPTIONAL,

codebookParametersType1SP-SchemeB-PerBC-r19 CodebookParametersType1SP-SchemeB-r19 OPTIONAL,

codebookParametersType1MP-PerBC-r19 CodebookParametersType1MP-r19 OPTIONAL,

codebookParameterseType2ExtPerBC-r19 CodebookParameterseType2Ext-r19 OPTIONAL,

codebookParametersfeType2ExtPerBC-r19 CodebookParametersfeType2Ext-r19 OPTIONAL,

codebookParameterseType2DopplerExtPerBC-r19 CodebookParameterseType2DopplerExt-r19 OPTIONAL,

codebookParametersHybridBF-Type1SP-PerBC-r19 CodebookParametersHybridBF-Type1SP-r19 OPTIONAL,

codebookParametersHybridBF-eType2PerBC-r19 CodebookParametersHybridBF-eType2-r19 OPTIONAL,

-- R1 58-3-1: CSI prediction for UE-sided inference when N4=1

aiml-CSI-PredictionPerBC-r19 ENUMERATED {supported} OPTIONAL,

-- R1 59-1-6: First PUCCH and second PUSCH from different PUCCH groups

diffGroupPUCCH-PUSCH-r19 ENUMERATED {supported} OPTIONAL,

-- R1 59-2-1-6: CSI-RS resource time domain restriction for Type-I and Type II codebook enhancement for up to 128 ports

timeRestriction128PortPerBC-r19 ENUMERATED {supported} OPTIONAL,

-- R1 59-2-1-7: Group-specific 3-bit scaling factors for up to 128 ports

groupScalingFactorPerBC-r19 ENUMERATED {rank1, rank1and2} OPTIONAL,

-- R1 59-2-2-3a: Configuration of MR always-reported resources with Rel-15 Type-I SP codebook

mr-AlwaysReportedType1SP-PerBC-r19 ENUMERATED {supported} OPTIONAL,

-- R1 59-2-2-3b: Configuration of MR always-reported resources with Rel-16 eType-II codebook with R=1

mr-AlwaysReported-eType2PerBC-r19 ENUMERATED {supported} OPTIONAL,

-- R1 59-2-3-1: CJTC Dd report

cjtc-DdReportPerBC-r19 SEQUENCE {

minRangeDdInCyclicPrefix-r19 ENUMERATED {half, full},

maxResolutionDd-r19 ENUMERATED {n32,n64,n128,n256},

scalingFactor-r19 INTEGER (1..2)

} OPTIONAL,

-- R1 59-2-3-1a: CJTC Dd report processing

cjtc-DdReportProcessingPerBC-r19 SEQUENCE {

maxNumberTRS-Resource-r19 ENUMERATED {n2,n4,n6,n8,n10,n12},

maxNumberTRS-ResourceAcrossCC-r19 ENUMERATED {n2,n4,n6,n8,n12,n64},

maxNumberCSI-RS-ResourcePerCC-r19 ENUMERATED {n2,n4,n6,n8,n12,n16,n20,n24,n28,n32},

maxNumberCSI-RS-ResourceAcrossCC-r19 ENUMERATED {n2,n4,n6,n8,n12,n16,n20,n24,n28,n32,n64},

valueX-r19 INTEGER (1..2)

} OPTIONAL,

-- R1 59-2-3-2: CJTC FO report

cjtc-FO-ReportPerBC-r19 SEQUENCE {

minRangeFO-r19 ENUMERATED {ppmDot1, ppmDot2},

maxResolutionFO-r19 ENUMERATED {n16,n32,n256},

scalingFactor-r19 INTEGER (1..2)

} OPTIONAL,

-- R1 59-2-3-2a: CJTC FO report processing

cjtc-FO-ReportProcessingPerBC-r19 SEQUENCE {

maxNumberTRS-Resource-r19 ENUMERATED {n2,n4,n6,n8,n10,n12},

maxNumberTRS-ResourceAcrossCC-r19 ENUMERATED {n2,n4,n6,n8,n12,n64},

maxNumberCSI-RS-ResourcePerCC-r19 ENUMERATED {n2,n4,n6,n8,n12,n16,n20,n24,n28,n32},

maxNumberCSI-RS-ResourceAcrossCC-r19 ENUMERATED {n2,n4,n6,n8,n12,n16,n20,n24,n28,n32,n64},

valueX-r19 INTEGER (1..2)

} OPTIONAL,

-- R1 59-2-3-3: CJTC wideband PO report

cjtc-PO-ReportWidebandPerBC-r19 SEQUENCE {

maxResolution-r19 ENUMERATED {n16, n32},

scalingFactor-r19 INTEGER (1..2),

maxSlotDuration-r19 INTEGER (1..2)

} OPTIONAL,

-- R1 59-2-3-3a: CJTC wideband PO report processing

cjtc-PO-ReportWidebandProcessingPerBC-r19 SEQUENCE {

maxNumberCSI-RS-Configured-r19 ENUMERATED {n2,n4,n6,n8,n10,n12},

maxNumberCSI-RS-ConfiguredAcrossCC-r19 ENUMERATED {n2,n4,n6,n8,n12,n64},

maxNumberCSI-RS-ResourcePerCC-r19 ENUMERATED {n2,n4,n6,n8,n12,n16,n20,n24,n28,n32},

maxNumberCSI-RS-ResourceAcrossCC-r19 ENUMERATED {n2,n4,n6,n8,n12,n16,n20,n24,n28,n32,n64},

valueX-r19 INTEGER (1..2)

} OPTIONAL,

-- R1 59-2-3-4: CJTC subband PO report

cjtc-PO-ReportSubbandPerBC-r19 SEQUENCE {

maxResolution-r19 ENUMERATED {n16, n32},

minSubbandSize-r19 ENUMERATED {n1,n2,n4,n8,n16},

scalingFactor-r19 INTEGER (1..2),

maxSlotDuration-r19 INTEGER (1..2)

} OPTIONAL,

-- R1 59-2-3-5: CJTC Dd+FO report

cjtc-DdFO-ReportPerBC-r19 SEQUENCE {

minRangeDdInCyclicPrefix-r19 ENUMERATED {half, full},

maxResolutionDd-r19 ENUMERATED {n32,n64,n128,n256},

minRangeFO-r19 ENUMERATED {ppmDot1, ppmDot2},

maxResolutionFO-r19 ENUMERATED {n16,n32,n256},

scalingFactor-r19 INTEGER (1..2)

} OPTIONAL,

-- R1 59-2-3-5a: CJTC Dd+FO report processing

cjtc-DdFO-ReportProcessingPerBC-r19 SEQUENCE {

maxNumberTRS-Resource-r19 ENUMERATED {n2,n4,n6,n8,n10,n12},

maxNumberTRS-ResourceAcrossCC-r19 ENUMERATED {n2,n4,n6,n8,n12,n64},

maxNumberCSI-RS-ResourcePerCC-r19 ENUMERATED {n2,n4,n6,n8,n12,n16,n20,n24,n28,n32},

maxNumberCSI-RS-ResourceAcrossCC-r19 ENUMERATED {n2,n4,n6,n8,n12,n16,n20,n24,n28,n32,n64},

valueX-r19 INTEGER (1..2)

} OPTIONAL,

-- R1 59-2-3-7: Linkage of CJTC Dd and Rel-18 eType-II CJT with joint triggering

linked-CJTC-Dd-eType2CJT-JointPerBC-r19 ENUMERATED {supported} OPTIONAL,

-- R1 59-2-3-7a: Linkage of CJTC Dd and Rel-18 eType-II CJT with joint triggering

linked-CJTC-Dd-eType2CJT-SeparatePerBC-r19 ENUMERATED {supported} OPTIONAL,

-- R1 59-2-3-8: Separate triggering with configuration of 1-bit indicator per CSI trigger state

linked-CJTC-Dd-eType2CJT-SeparatePerStatePerBC-r19 ENUMERATED {supported} OPTIONAL,

-- R1 59-2-3-10: Relaxed timeline for joint triggering of CJTC Dd and Rel-18 eType-II CJT

timelineRelax-CJTC-Dd-eType2CJT-PerBC-r19 SEQUENCE {

scs15kHz-r19 ENUMERATED {n2,n4,n8} OPTIONAL,

scs30kHz-r19 ENUMERATED {n4,n8,n14,n28} OPTIONAL,

scs60kHz-r19 ENUMERATED {n8,n14,n28} OPTIONAL,

scs120kHz-r19 ENUMERATED {n14,n28,n56} OPTIONAL,

scs480kHz-r19 ENUMERATED {n56,n112,n224} OPTIONAL,

scs960kHz-r19 ENUMERATED {n112,n224,n448} OPTIONAL

} OPTIONAL,

-- R1 59-2-4: Association up to 128 CSI-RS ports and SRS for non-codebook-based PUSCH

nonCodebook-CSI-RS-SRS-PerBC-Enh-r19 SEQUENCE (SIZE (1.. maxNrofCSI-RS-ResourcesExt-r16))

OF INTEGER(0..maxNrofCSI-RS-ResourcesAlt-1-r16) OPTIONAL, -- R1 63-1: NW triggered intra-frequency L1-RSRP measurement based on periodic CSI-RS (s) for

-- L1-L2 Triggered Mobility (LTM) procedure

intraFreqL1-MeasConfigPeriodicCSI-RS-r19 SEQUENCE {

supportedMaxIntraFreqCellsConfig-r19 INTEGER (1..8),

supportedMaxIntraFreqCellsPerReport-r19 INTEGER (1..4),

supportedMaxReportBeamsPerReportedCell-r19 INTEGER (1..4),

supportedMaxReportBeamsReports-r19 ENUMERATED {n1,n2,n3,n4,n6,n8,n9,n12,n16},

supportedMaxAperiodic-LTM-CSI-ReportConfig-r19 INTEGER (0..4),

supportedMaxPeriodic-LTM-CSI-ReportConfig-r19 INTEGER (1..4),

supportedMaxSemiPersistent-LTM-CSI-ReportConfig-r19 INTEGER (0..4)

} OPTIONAL,

-- R1 63-2: NW triggered intra-frequency L1-RSRP measurement based on semi-persistent CSI-RS (s) for

-- L1-L2 Triggered Mobility (LTM) procedure

intraFreqL1-MeasConfigSP-CSI-RS-r19 SEQUENCE {

supportedMaxAperiodic-LTM-CSI-ReportConfig-r19 INTEGER (0..4),

supportedMaxSemiPersistent-LTM-CSI-ReportConfig-r19 INTEGER (0..4)

} OPTIONAL,

-- R1 63-8: Inclusion of current SpCell in the L1 measurement report based on CSI-RS(s)

currentSpCellInclL1-ReportCSI-RS-r19 ENUMERATED {supported} OPTIONAL,

-- R1 67-6: Simultaneous NZP-CSI-RS resource counting

simultaneousNZP-CSI-RS-r19 ENUMERATED {supported} OPTIONAL,

-- R1 67-8: Simultaneous NZP-CSI-RS resource counting NES

simultaneousNZP-CSI-RS-NES-r19 ENUMERATED {supported} OPTIONAL,

-- R4 46-1: MPR enhancement for activated carrier

mpr-ActiveCarrierEnh-r19 ENUMERATED {supported} OPTIONAL,

-- R4 46-2: FR2 MPR-Improvement Downlink Independent

mpr-DL-Independent-r19 ENUMERATED {supported} OPTIONAL,

-- R4 46-3: FR2 MPR Improvement Activation Dependent

mpr-ActivateDependent-r19 ENUMERATED {supported} OPTIONAL,

-- R4 47-1: Support network control of requirement for UE supporting intraBandNR-CA-non-collocated-r19

intraBandNR-CA-non-collocated-r19 ENUMERATED {supported} OPTIONAL,

-- R4 48-1: Rx beam Type

atg-RxBeamType-r19 ENUMERATED {rxType1, rxType2} OPTIONAL,

-- R4 50-1: Lower bound of measurement periodicity of 10ms for the deactivated measurement requirement in

-- fast measurement window on OD-SSB SCell

od-SSB-FastMeasWinLowerBound-r19 ENUMERATED {supported} OPTIONAL,

-- R4 52-1: Number of CSI-RS resources for L1-RSRP measurement within a slot

maxCSI-RS-ResourceL1-Meas-r19 ENUMERATED {n1,n2,n3,n4,n5,n6,n7,n8,n16,n32,n48,n64} OPTIONAL,

-- R4 52-2: Number of total CSI-RS resources to be measured

totalCSI-RS-ResourceL1-Meas-r19 ENUMERATED {n2,n4,n8,n12,n16,n32,n64} OPTIONAL

}

CrossCarrierSchedulingSCell-SpCell-r17 ::= SEQUENCE {

supportedSCS-Combinations-r17 SEQUENCE {

scs15kHz-15kHz-r17 ENUMERATED {supported} OPTIONAL,

scs15kHz-30kHz-r17 ENUMERATED {supported} OPTIONAL,

scs15kHz-60kHz-r17 ENUMERATED {supported} OPTIONAL,

scs30kHz-30kHz-r17 BIT STRING (SIZE (1..496)) OPTIONAL,

scs30kHz-60kHz-r17 BIT STRING (SIZE (1..496)) OPTIONAL,

scs60kHz-60kHz-r17 BIT STRING (SIZE (1..496)) OPTIONAL

},

pdcch-MonitoringOccasion-r17 ENUMERATED {val1, val2}

}

PDCCH-BlindDetectionMixedList-r16::= SEQUENCE {

pdcch-BlindDetectionCA-MixedExt-r16 CHOICE {

pdcch-BlindDetectionCA-Mixed-v16a0 PDCCH-BlindDetectionCA-MixedExt-r16,

pdcch-BlindDetectionCA-Mixed-NonAlignedSpan-v16a0 PDCCH-BlindDetectionCA-MixedExt-r16

} OPTIONAL,

pdcch-BlindDetectionCG-UE-MixedExt-r16 SEQUENCE{

pdcch-BlindDetectionMCG-UE-Mixed-v16a0 PDCCH-BlindDetectionCG-UE-MixedExt-r16,

pdcch-BlindDetectionSCG-UE-Mixed-v16a0 PDCCH-BlindDetectionCG-UE-MixedExt-r16

} OPTIONAL

}

PDCCH-BlindDetectionCA-MixedExt-r16 ::= SEQUENCE {

pdcch-BlindDetectionCA1-r16 INTEGER (1..15),

pdcch-BlindDetectionCA2-r16 INTEGER (1..15)

}

PDCCH-BlindDetectionCG-UE-MixedExt-r16 ::= SEQUENCE {

pdcch-BlindDetectionCG-UE1-r16 INTEGER (0..15),

pdcch-BlindDetectionCG-UE2-r16 INTEGER (0..15)

}

PDCCH-BlindDetectionMCG-SCG-r17 ::= SEQUENCE {

pdcch-BlindDetectionMCG-UE-r17 INTEGER (1..15),

pdcch-BlindDetectionSCG-UE-r17 INTEGER (1..15)

}

PDCCH-BlindDetectionMixed-r17::= SEQUENCE {

pdcch-BlindDetectionCA-Mixed-r17 PDCCH-BlindDetectionCA-Mixed-r17 OPTIONAL,

pdcch-BlindDetectionCG-UE-Mixed-r17 SEQUENCE{

pdcch-BlindDetectionMCG-UE-Mixed-v17 PDCCH-BlindDetectionCG-UE-Mixed-r17,

pdcch-BlindDetectionSCG-UE-Mixed-v17 PDCCH-BlindDetectionCG-UE-Mixed-r17

} OPTIONAL

}

PDCCH-BlindDetectionCG-UE-Mixed-r17 ::= SEQUENCE {

pdcch-BlindDetectionCG-UE1-r17 INTEGER (0..15),

pdcch-BlindDetectionCG-UE2-r17 INTEGER (0..15)

}

PDCCH-BlindDetectionCA-Mixed-r17 ::= SEQUENCE {

pdcch-BlindDetectionCA1-r17 INTEGER (1..15) OPTIONAL,

pdcch-BlindDetectionCA2-r17 INTEGER (1..15) OPTIONAL

}

PDCCH-BlindDetectionMixed1-r17::= SEQUENCE {

pdcch-BlindDetectionCA-Mixed1-r17 PDCCH-BlindDetectionCA-Mixed1-r17 OPTIONAL,

pdcch-BlindDetectionCG-UE-Mixed1-r17 SEQUENCE{

pdcch-BlindDetectionMCG-UE-Mixed1-v17 PDCCH-BlindDetectionCG-UE-Mixed1-r17,

pdcch-BlindDetectionSCG-UE-Mixed1-v17 PDCCH-BlindDetectionCG-UE-Mixed1-r17

} OPTIONAL

}

PDCCH-BlindDetectionCG-UE-Mixed1-r17 ::= SEQUENCE {

pdcch-BlindDetectionCG-UE1-r17 INTEGER (0..15),

pdcch-BlindDetectionCG-UE2-r17 INTEGER (0..15),

pdcch-BlindDetectionCG-UE3-r17 INTEGER (0..15)

}

PDCCH-BlindDetectionCA-Mixed1-r17 ::= SEQUENCE {

pdcch-BlindDetectionCA1-r17 INTEGER (1..15) OPTIONAL,

pdcch-BlindDetectionCA2-r17 INTEGER (1..15) OPTIONAL,

pdcch-BlindDetectionCA3-r17 INTEGER (1..15) OPTIONAL

}

PDCCH-BlindDetectionMixed2-r18 ::= SEQUENCE{

pdcch-BlindDetectionMCG-UE-Mixed-r18 PDCCH-BlindDetectionCG-UE-MixedExt-r16,

pdcch-BlindDetectionSCG-UE-Mixed-r18 PDCCH-BlindDetectionCG-UE-MixedExt-r16

}

SimulSRS-ForAntennaSwitching-r16 ::= SEQUENCE {

supportSRS-xTyR-xLessThanY-r16 ENUMERATED {supported} OPTIONAL,

supportSRS-xTyR-xEqualToY-r16 ENUMERATED {supported} OPTIONAL,

supportSRS-AntennaSwitching-r16 ENUMERATED {supported} OPTIONAL

}

TwoPUCCH-Grp-Configurations-r16 ::= SEQUENCE {

pucch-PrimaryGroupMapping-r16 TwoPUCCH-Grp-ConfigParams-r16,

pucch-SecondaryGroupMapping-r16 TwoPUCCH-Grp-ConfigParams-r16

}

TwoPUCCH-Grp-Configurations-r17 ::= SEQUENCE {

primaryPUCCH-GroupConfig-r17 PUCCH-Group-Config-r17,

secondaryPUCCH-GroupConfig-r17 PUCCH-Group-Config-r17

}

TwoPUCCH-Grp-ConfigParams-r16 ::= SEQUENCE {

pucch-GroupMapping-r16 PUCCH-Grp-CarrierTypes-r16,

pucch-TX-r16 PUCCH-Grp-CarrierTypes-r16

}

CarrierTypePair-r16 ::= SEQUENCE {

carrierForCSI-Measurement-r16 PUCCH-Grp-CarrierTypes-r16,

carrierForCSI-Reporting-r16 PUCCH-Grp-CarrierTypes-r16

}

PUCCH-Grp-CarrierTypes-r16 ::= SEQUENCE {

fr1-NonSharedTDD-r16 ENUMERATED {supported} OPTIONAL,

fr1-SharedTDD-r16 ENUMERATED {supported} OPTIONAL,

fr1-NonSharedFDD-r16 ENUMERATED {supported} OPTIONAL,

fr2-r16 ENUMERATED {supported} OPTIONAL

}

PUCCH-Group-Config-r17 ::= SEQUENCE {

fr1-FR1-NonSharedTDD-r17 ENUMERATED {supported} OPTIONAL,

fr2-FR2-NonSharedTDD-r17 ENUMERATED {supported} OPTIONAL,

fr1-FR2-NonSharedTDD-r17 ENUMERATED {supported} OPTIONAL

}

CombinationCarrierType-r18 ::= SEQUENCE {

schedulingCellCarrierType-r18 ENUMERATED {licensed-fdd-fr1, licensed-tdd-fr1, unlicensed-tdd-fr1, fr2-1, fr2-2},

scheduledCellCarrierType-r18 ENUMERATED {licensed-fdd-fr1, licensed-tdd-fr1, unlicensed-tdd-fr1, fr2-1, fr2-2}

}

-- TAG-CA-PARAMETERSNR-STOP

-- ASN1STOP

|  |
| --- |
| *CA-ParametersNR* field description |
| ***codebookParametersPerBC***  For a given supported band combination, this field indicates the alternative list of *SupportedCSI-RS-Resource* supported for each codebook type, amongst the supported CSI-RS resources included in *codebookParametersPerBand* in *MIMO-ParametersPerBand*. |
| ***dummy***  The field is not used in the specification and the network ignores the received value. |

#### – *CA-ParametersNRDC*

The IE *CA-ParametersNRDC* contains dual connectivity related capabilities that are defined per band combination.

*CA-ParametersNRDC* information element

-- ASN1START

-- TAG-CA-PARAMETERS-NRDC-START

CA-ParametersNRDC ::= SEQUENCE {

ca-ParametersNR-ForDC CA-ParametersNR OPTIONAL,

ca-ParametersNR-ForDC-v1540 CA-ParametersNR-v1540 OPTIONAL,

ca-ParametersNR-ForDC-v1550 CA-ParametersNR-v1550 OPTIONAL,

ca-ParametersNR-ForDC-v1560 CA-ParametersNR-v1560 OPTIONAL,

featureSetCombinationDC FeatureSetCombinationId OPTIONAL

}

CA-ParametersNRDC-v15g0 ::= SEQUENCE {

ca-ParametersNR-ForDC-v15g0 CA-ParametersNR-v15g0 OPTIONAL

}

CA-ParametersNRDC-v1610 ::= SEQUENCE {

-- R1 18-1: Semi-static power sharing mode1 between MCG and SCG cells of same FR for NR dual connectivity

intraFR-NR-DC-PwrSharingMode1-r16 ENUMERATED {supported} OPTIONAL,

-- R1 18-1a: Semi-static power sharing mode 2 between MCG and SCG cells of same FR for NR dual connectivity

intraFR-NR-DC-PwrSharingMode2-r16 ENUMERATED {supported} OPTIONAL,

-- R1 18-1b: Dynamic power sharing between MCG and SCG cells of same FR for NR dual connectivity

intraFR-NR-DC-DynamicPwrSharing-r16 ENUMERATED {short, long} OPTIONAL,

asyncNRDC-r16 ENUMERATED {supported} OPTIONAL

}

CA-ParametersNRDC-v1630 ::= SEQUENCE {

ca-ParametersNR-ForDC-v1610 CA-ParametersNR-v1610 OPTIONAL,

ca-ParametersNR-ForDC-v1630 CA-ParametersNR-v1630 OPTIONAL

}

CA-ParametersNRDC-v1640 ::= SEQUENCE {

ca-ParametersNR-ForDC-v1640 CA-ParametersNR-v1640 OPTIONAL

}

CA-ParametersNRDC-v1650 ::= SEQUENCE {

supportedCellGrouping-r16 BIT STRING (SIZE (1..maxCellGroupings-r16)) OPTIONAL

}

CA-ParametersNRDC-v16a0 ::= SEQUENCE {

ca-ParametersNR-ForDC-v16a0 CA-ParametersNR-v16a0 OPTIONAL

}

CA-ParametersNRDC-v16j0 ::= SEQUENCE {

ca-ParametersNR-ForDC-v16j0 CA-ParametersNR-v1690 OPTIONAL

}

CA-ParametersNRDC-v1700 ::= SEQUENCE {

-- R1 31-9: Indicates the support of simultaneous transmission and reception of an IAB-node from multiple parent nodes

simultaneousRxTx-IAB-MultipleParents-r17 ENUMERATED {supported} OPTIONAL,

condPSCellAdditionNRDC-r17 ENUMERATED {supported} OPTIONAL,

scg-ActivationDeactivationNRDC-r17 ENUMERATED {supported} OPTIONAL,

scg-ActivationDeactivationResumeNRDC-r17 ENUMERATED {supported} OPTIONAL,

beamManagementType-CBM-r17 ENUMERATED {supported} OPTIONAL

}

CA-ParametersNRDC-v1720 ::= SEQUENCE {

ca-ParametersNR-ForDC-v1700 CA-ParametersNR-v1700 OPTIONAL,

ca-ParametersNR-ForDC-v1720 CA-ParametersNR-v1720 OPTIONAL

}

CA-ParametersNRDC-v1730 ::= SEQUENCE {

ca-ParametersNR-ForDC-v1730 CA-ParametersNR-v1730 OPTIONAL

}

CA-ParametersNRDC-v1760 ::= SEQUENCE {

ca-ParametersNR-ForDC-v1760 CA-ParametersNR-v1760

}

CA-ParametersNRDC-v1780 ::= SEQUENCE {

ca-ParametersNR-ForDC-v1780 CA-ParametersNR-v1780 OPTIONAL

}

CA-ParametersNRDC-v17b0 ::= SEQUENCE {

ca-ParametersNR-ForDC-v17b0 CA-ParametersNR-v1740 OPTIONAL

}

CA-ParametersNRDC-v1800 ::= SEQUENCE {

ca-ParametersNR-ForDC-v1800 CA-ParametersNR-v1800 OPTIONAL,

-- R1 55-6d: Capability on the number of CCs for monitoring a maximum number of BDs and non-overlapped CCEs per span for MCG and for

-- SCG when configured for NR-DC operation with Rel-16 PDCCH monitoring on all the serving cells

pdcch-BlindDetectionNRDC-r18 SEQUENCE(SIZE (1..maxNrofPdcch-BlindDetectionMixed-1-r16)) OF

PDCCH-BlindDetectionMixed1-r18 OPTIONAL

}

CA-ParametersNRDC-v1830 ::= SEQUENCE {

ca-ParametersNR-ForDC-v1830 CA-ParametersNR-v1830 OPTIONAL

}

CA-ParametersNRDC-v1900 ::= SEQUENCE {

ca-ParametersNR-ForDC-v1900 CA-ParametersNR-v1900 OPTIONAL

}

PDCCH-BlindDetectionMixed1-r18::= SEQUENCE {

pdcch-BlindDetectionCG-UE-Mixed-r18 SEQUENCE{

pdcch-BlindDetectionMCG-UE-Mixed-r18 INTEGER (1..15),

pdcch-BlindDetectionSCG-UE-Mixed-r18 INTEGER (1..15)

}

}

-- TAG-CA-PARAMETERS-NRDC-STOP

-- ASN1STOP

|  |
| --- |
| *CA-ParametersNRDC* field descriptions |
| ***ca-ParametersNR-forDC (with and without suffix)***  If this field is present for a band combination, it reports the UE capabilities when NR-DC is configured with the band combination. If a version of this field (i.e., with or without suffix) is absent for a band combination, the corresponding *ca-ParametersNR* field version in *BandCombination* is applicable to the UE configured with NR-DC for the band combination. If a version of this field (i.e., with or without suffix) is present for a band combination but does not contain any parameters, the UE does not support the corresponding field version when configured with NR-DC for the band combination. |
| ***featureSetCombinationDC***  If this field is present for a band combination, it reports the feature set combination supported for the band combination when NR-DC is configured. If this field is absent for a band combination, the *featureSetCombination* in *BandCombination* (without suffix) is applicable to the UE configured with NR-DC for the band combination. |

#### – *CarrierAggregationVariant*

The IE *CarrierAggregationVariant* informs the network about supported "placement" of the SpCell in an NR cell group.

*CarrierAggregationVariant* information element

-- ASN1START

-- TAG-CARRIERAGGREGATIONVARIANT-START

CarrierAggregationVariant ::= SEQUENCE {

fr1fdd-FR1TDD-CA-SpCellOnFR1FDD ENUMERATED {supported} OPTIONAL,

fr1fdd-FR1TDD-CA-SpCellOnFR1TDD ENUMERATED {supported} OPTIONAL,

fr1fdd-FR2TDD-CA-SpCellOnFR1FDD ENUMERATED {supported} OPTIONAL,

fr1fdd-FR2TDD-CA-SpCellOnFR2TDD ENUMERATED {supported} OPTIONAL,

fr1tdd-FR2TDD-CA-SpCellOnFR1TDD ENUMERATED {supported} OPTIONAL,

fr1tdd-FR2TDD-CA-SpCellOnFR2TDD ENUMERATED {supported} OPTIONAL,

fr1fdd-FR1TDD-FR2TDD-CA-SpCellOnFR1FDD ENUMERATED {supported} OPTIONAL,

fr1fdd-FR1TDD-FR2TDD-CA-SpCellOnFR1TDD ENUMERATED {supported} OPTIONAL,

fr1fdd-FR1TDD-FR2TDD-CA-SpCellOnFR2TDD ENUMERATED {supported} OPTIONAL

}

-- TAG-CARRIERAGGREGATIONVARIANT-STOP

-- ASN1STOP

#### – *CodebookParameters*

The IE *CodebookParameters* is used to convey codebook related parameters.

*CodebookParameters* information element

-- ASN1START

-- TAG-CODEBOOKPARAMETERS-START

CodebookParameters ::= SEQUENCE {

type1 SEQUENCE {

singlePanel SEQUENCE {

supportedCSI-RS-ResourceList SEQUENCE (SIZE (1.. maxNrofCSI-RS-Resources)) OF SupportedCSI-RS-Resource,

modes ENUMERATED {mode1, mode1andMode2},

maxNumberCSI-RS-PerResourceSet INTEGER (1..8)

},

multiPanel SEQUENCE {

supportedCSI-RS-ResourceList SEQUENCE (SIZE (1.. maxNrofCSI-RS-Resources)) OF SupportedCSI-RS-Resource,

modes ENUMERATED {mode1, mode2, both},

nrofPanels ENUMERATED {n2, n4},

maxNumberCSI-RS-PerResourceSet INTEGER (1..8)

} OPTIONAL

},

type2 SEQUENCE {

supportedCSI-RS-ResourceList SEQUENCE (SIZE (1.. maxNrofCSI-RS-Resources)) OF SupportedCSI-RS-Resource,

parameterLx INTEGER (2..4),

amplitudeScalingType ENUMERATED {wideband, widebandAndSubband},

amplitudeSubsetRestriction ENUMERATED {supported} OPTIONAL

} OPTIONAL,

type2-PortSelection SEQUENCE {

supportedCSI-RS-ResourceList SEQUENCE (SIZE (1.. maxNrofCSI-RS-Resources)) OF SupportedCSI-RS-Resource,

parameterLx INTEGER (2..4),

amplitudeScalingType ENUMERATED {wideband, widebandAndSubband}

} OPTIONAL

}

CodebookParameters-v1610 ::= SEQUENCE {

supportedCSI-RS-ResourceListAlt-r16 SEQUENCE {

type1-SinglePanel-r16 SEQUENCE (SIZE (1..maxNrofCSI-RS-Resources)) OF INTEGER (0..maxNrofCSI-RS-ResourcesAlt-1-r16) OPTIONAL,

type1-MultiPanel-r16 SEQUENCE (SIZE (1..maxNrofCSI-RS-Resources)) OF INTEGER (0..maxNrofCSI-RS-ResourcesAlt-1-r16) OPTIONAL,

type2-r16 SEQUENCE (SIZE (1..maxNrofCSI-RS-Resources)) OF INTEGER (0..maxNrofCSI-RS-ResourcesAlt-1-r16) OPTIONAL,

type2-PortSelection-r16 SEQUENCE (SIZE (1..maxNrofCSI-RS-Resources)) OF INTEGER (0..maxNrofCSI-RS-ResourcesAlt-1-r16) OPTIONAL

} OPTIONAL

}

CodebookParametersAddition-r16 ::= SEQUENCE {

etype2-r16 SEQUENCE {

-- R1 16-3a Regular eType 2 R=1

etype2R1-r16 SEQUENCE {

supportedCSI-RS-ResourceListAdd-r16 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF

INTEGER (0..maxNrofCSI-RS-ResourcesAlt-1-r16)

},

-- R1 16-3a-1 Regular eType 2 R=2

etype2R2-r16 SEQUENCE {

supportedCSI-RS-ResourceListAdd-r16 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF

INTEGER (0..maxNrofCSI-RS-ResourcesAlt-1-r16)

} OPTIONAL,

-- R1 16-3a-2: Support of parameter combinations 7-8

paramComb7-8-r16 ENUMERATED {supported} OPTIONAL,

-- R1 16-3a-3: Support of rank 3,4

rank3-4-r16 ENUMERATED {supported} OPTIONAL,

-- R1 16-3a-4: CBSR with soft amplitude restriction

amplitudeSubsetRestriction-r16 ENUMERATED {supported} OPTIONAL

} OPTIONAL,

etype2-PS-r16 SEQUENCE {

-- R1 16-3b Regular eType 2 R=1 PortSelection

etype2R1-PortSelection-r16 SEQUENCE {

supportedCSI-RS-ResourceListAdd-r16 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF

INTEGER (0..maxNrofCSI-RS-ResourcesAlt-1-r16)

},

-- R1 16-3b-1 Regular eType 2 R=2 PortSelection

etype2R2-PortSelection-r16 SEQUENCE {

supportedCSI-RS-ResourceListAdd-r16 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF

INTEGER (0..maxNrofCSI-RS-ResourcesAlt-1-r16)

} OPTIONAL,

-- R1 16-3b-2: Support of rank 3,4

rank3-4-r16 ENUMERATED {supported} OPTIONAL

} OPTIONAL

}

CodebookComboParametersAddition-r16 ::= SEQUENCE {

-- R1 16-8 Mixed codebook types

type1SP-Type2-null-r16 SEQUENCE {

supportedCSI-RS-ResourceListAdd-r16 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER (0..maxNrofCSI-RS-ResourcesAlt-1-r16)

} OPTIONAL,

type1SP-Type2PS-null-r16 SEQUENCE {

supportedCSI-RS-ResourceListAdd-r16 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER (0..maxNrofCSI-RS-ResourcesAlt-1-r16)

} OPTIONAL,

type1SP-eType2R1-null-r16 SEQUENCE {

supportedCSI-RS-ResourceListAdd-r16 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER (0..maxNrofCSI-RS-ResourcesAlt-1-r16)

} OPTIONAL,

type1SP-eType2R2-null-r16 SEQUENCE {

supportedCSI-RS-ResourceListAdd-r16 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER (0..maxNrofCSI-RS-ResourcesAlt-1-r16)

} OPTIONAL,

type1SP-eType2R1PS-null-r16 SEQUENCE {

supportedCSI-RS-ResourceListAdd-r16 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER (0..maxNrofCSI-RS-ResourcesAlt-1-r16)

} OPTIONAL,

type1SP-eType2R2PS-null-r16 SEQUENCE {

supportedCSI-RS-ResourceListAdd-r16 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER (0..maxNrofCSI-RS-ResourcesAlt-1-r16)

} OPTIONAL,

type1SP-Type2-Type2PS-r16 SEQUENCE {

supportedCSI-RS-ResourceListAdd-r16 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER (0..maxNrofCSI-RS-ResourcesAlt-1-r16)

} OPTIONAL,

type1MP-Type2-null-r16 SEQUENCE {

supportedCSI-RS-ResourceListAdd-r16 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER (0..maxNrofCSI-RS-ResourcesAlt-1-r16)

} OPTIONAL,

type1MP-Type2PS-null-r16 SEQUENCE {

supportedCSI-RS-ResourceListAdd-r16 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER (0..maxNrofCSI-RS-ResourcesAlt-1-r16)

} OPTIONAL,

type1MP-eType2R1-null-r16 SEQUENCE {

supportedCSI-RS-ResourceListAdd-r16 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER (0..maxNrofCSI-RS-ResourcesAlt-1-r16)

} OPTIONAL,

type1MP-eType2R2-null-r16 SEQUENCE {

supportedCSI-RS-ResourceListAdd-r16 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER (0..maxNrofCSI-RS-ResourcesAlt-1-r16)

} OPTIONAL,

type1MP-eType2R1PS-null-r16 SEQUENCE {

supportedCSI-RS-ResourceListAdd-r16 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER (0..maxNrofCSI-RS-ResourcesAlt-1-r16)

} OPTIONAL,

type1MP-eType2R2PS-null-r16 SEQUENCE {

supportedCSI-RS-ResourceListAdd-r16 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER (0..maxNrofCSI-RS-ResourcesAlt-1-r16)

} OPTIONAL,

type1MP-Type2-Type2PS-r16 SEQUENCE {

supportedCSI-RS-ResourceListAdd-r16 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER (0..maxNrofCSI-RS-ResourcesAlt-1-r16)

} OPTIONAL

}

CodebookParametersfetype2-r17 ::= SEQUENCE {

-- R1 23-9-1 Basic Features of Further Enhanced Port-Selection Type II Codebook (FeType-II)

fetype2basic-r17 SEQUENCE (SIZE (1.. maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER (0..maxNrofCSI-RS-ResourcesAlt-1-r16),

-- R1 23-9-2 Support of M=2 and R=1 for FeType-II

fetype2R1-r17 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r17)) OF INTEGER (0.. maxNrofCSI-RS-ResourcesAlt-1-r16)

OPTIONAL,

-- R1 23-9-4 Support of R = 2 for FeType-II

fetype2R2-r17 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r17)) OF INTEGER (0.. maxNrofCSI-RS-ResourcesAlt-1-r16)

OPTIONAL,

-- R1 23-9-3 Support of rank 3, 4 for FeType-II

fetype2Rank3Rank4-r17 ENUMERATED {supported} OPTIONAL

}

CodebookComboParameterMixedType-r17 ::= SEQUENCE {

-- R1 23-9-5 Active CSI-RS resources and ports for mixed codebook types in any slot

type1SP-feType2PS-null-r17 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER (0..maxNrofCSI-RS-ResourcesAlt-1-r16)

OPTIONAL,

type1SP-feType2PS-M2R1-null-r17 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER (0..maxNrofCSI-RS-ResourcesAlt-1-r16)

OPTIONAL,

type1SP-feType2PS-M2R2-null-r1 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER (0..maxNrofCSI-RS-ResourcesAlt-1-r16)

OPTIONAL,

type1SP-Type2-feType2-PS-M1-r17 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER (0..maxNrofCSI-RS-ResourcesAlt-1-r16)

OPTIONAL,

type1SP-Type2-feType2-PS-M2R1-r17 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER (0..maxNrofCSI-RS-ResourcesAlt-1-r16)

OPTIONAL,

type1SP-eType2R1-feType2-PS-M1-r17 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER (0..maxNrofCSI-RS-ResourcesAlt-1-r16)

OPTIONAL,

type1SP-eType2R1-feType2-PS-M2R1-r17 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER (0..maxNrofCSI-RS-ResourcesAlt-1-r16)

OPTIONAL,

type1MP-feType2PS-null-r17 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER (0..maxNrofCSI-RS-ResourcesAlt-1-r16)

OPTIONAL,

type1MP-feType2PS-M2R1-null-r17 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER (0..maxNrofCSI-RS-ResourcesAlt-1-r16)

OPTIONAL,

type1MP-feType2PS-M2R2-null-r17 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER (0..maxNrofCSI-RS-ResourcesAlt-1-r16)

OPTIONAL,

type1MP-Type2-feType2-PS-M1-r17 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER (0..maxNrofCSI-RS-ResourcesAlt-1-r16)

OPTIONAL,

type1MP-Type2-feType2-PS-M2R1-r17 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER (0..maxNrofCSI-RS-ResourcesAlt-1-r16)

OPTIONAL,

type1MP-eType2R1-feType2-PS-M1-r17 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER (0..maxNrofCSI-RS-ResourcesAlt-1-r16)

OPTIONAL,

type1MP-eType2R1-feType2-PS-M2R1-r17 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER (0..maxNrofCSI-RS-ResourcesAlt-1-r16)

OPTIONAL

}

CodebookComboParameterMultiTRP-r17::= SEQUENCE {

-- R1 23-7-1b Active CSI-RS resources and ports in the presence of multi-TRP CSI

-- {Codebook 2, Codebook 3} =(NULL, NULL}

nCJT-null-null SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER (0..maxNrofCSI-RS-ResourcesAlt-1-r16)

OPTIONAL,

nCJT1SP-null-null SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER (0..maxNrofCSI-RS-ResourcesAlt-1-r16)

OPTIONAL,

-- {Codebook 2, Codebook 3} = {( {"Rel 16 combinations in FG 16-8"}

nCJT-Type2-null-r16 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER (0..maxNrofCSI-RS-ResourcesAlt-1-r16)

OPTIONAL,

nCJT-Type2PS-null-r16 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER (0..maxNrofCSI-RS-ResourcesAlt-1-r16)

OPTIONAL,

nCJT-eType2R1-null-r16 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER (0..maxNrofCSI-RS-ResourcesAlt-1-r16)

OPTIONAL,

nCJT-eType2R2-null-r16 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER (0..maxNrofCSI-RS-ResourcesAlt-1-r16)

OPTIONAL,

nCJT-eType2R1PS-null-r16 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER (0..maxNrofCSI-RS-ResourcesAlt-1-r16)

OPTIONAL,

nCJT-eType2R2PS-null-r16 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER (0..maxNrofCSI-RS-ResourcesAlt-1-r16)

OPTIONAL,

nCJT-Type2-Type2PS-r16 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER (0..maxNrofCSI-RS-ResourcesAlt-1-r16)

OPTIONAL,

nCJT1SP-Type2-null-r16 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER (0..maxNrofCSI-RS-ResourcesAlt-1-r16)

OPTIONAL,

nCJT1SP-Type2PS-null-r16 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER (0..maxNrofCSI-RS-ResourcesAlt-1-r16)

OPTIONAL,

nCJT1SP-eType2R1-null-r16 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER (0..maxNrofCSI-RS-ResourcesAlt-1-r16)

OPTIONAL,

nCJT1SP-eType2R2-null-r16 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER (0..maxNrofCSI-RS-ResourcesAlt-1-r16)

OPTIONAL,

nCJT1SP-eType2R1PS-null-r16 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER (0..maxNrofCSI-RS-ResourcesAlt-1-r16)

OPTIONAL,

nCJT1SP-eType2R2PS-null-r16 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER (0..maxNrofCSI-RS-ResourcesAlt-1-r16)

OPTIONAL,

nCJT1SP-Type2-Type2PS-r16 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER (0..maxNrofCSI-RS-ResourcesAlt-1-r16)

OPTIONAL,

-- {Codebook 2, Codebook 3} = {"New Rel17 combinations in FG 23-9-5"}

nCJT-feType2PS-null-r17 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER (0..maxNrofCSI-RS-ResourcesAlt-1-r16)

OPTIONAL,

nCJT-feType2PS-M2R1-null-r17 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER (0..maxNrofCSI-RS-ResourcesAlt-1-r16)

OPTIONAL,

nCJT-feType2PS-M2R2-null-r17 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER (0..maxNrofCSI-RS-ResourcesAlt-1-r16)

OPTIONAL,

nCJT-Type2-feType2-PS-M1-r17 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER (0..maxNrofCSI-RS-ResourcesAlt-1-r16)

OPTIONAL,

nCJT-Type2-feType2-PS-M2R1-r17 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER (0..maxNrofCSI-RS-ResourcesAlt-1-r16)

OPTIONAL,

nCJT-eType2R1-feType2-PS-M1-r17 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER (0..maxNrofCSI-RS-ResourcesAlt-1-r16)

OPTIONAL,

nCJT-eType2R1-feType2-PS-M2R1-r17 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER (0..maxNrofCSI-RS-ResourcesAlt-1-r16)

OPTIONAL,

nCJT1SP-feType2PS-null-r17 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER (0..maxNrofCSI-RS-ResourcesAlt-1-r16)

OPTIONAL,

nCJT1SP-feType2PS-M2R1-null-r17 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER (0..maxNrofCSI-RS-ResourcesAlt-1-r16)

OPTIONAL,

nCJT1SP-feType2PS-M2R2-null-r1 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER (0..maxNrofCSI-RS-ResourcesAlt-1-r16)

OPTIONAL,

nCJT1SP-Type2-feType2-PS-M1-r17 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER (0..maxNrofCSI-RS-ResourcesAlt-1-r16)

OPTIONAL,

nCJT1SP-Type2-feType2-PS-M2R1-r17 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER (0..maxNrofCSI-RS-ResourcesAlt-1-r16)

OPTIONAL,

nCJT1SP-eType2R1-feType2-PS-M1-r17 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER (0..maxNrofCSI-RS-ResourcesAlt-1-r16)

OPTIONAL,

nCJT1SP-eType2R1-feType2-PS-M2R1-r17 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER (0..maxNrofCSI-RS-ResourcesAlt-1-r16)

OPTIONAL

}

CodebookParametersAdditionPerBC-r16::= SEQUENCE {

-- R1 16-3a Regular eType 2 R=1

etype2R1-r16 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER (0..maxNrofCSI-RS-ResourcesAlt-1-r16)

OPTIONAL,

-- R1 16-3a-1 Regular eType 2 R=2

etype2R2-r16 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER (0..maxNrofCSI-RS-ResourcesAlt-1-r16)

OPTIONAL,

-- R1 16-3b Regular eType 2 R=1 PortSelection

etype2R1-PortSelection-r16 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER (0..maxNrofCSI-RS-ResourcesAlt-1-r16)

OPTIONAL,

-- R1 16-3b-1 Regular eType 2 R=2 PortSelection

etype2R2-PortSelection-r16 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER (0..maxNrofCSI-RS-ResourcesAlt-1-r16)

OPTIONAL

}

CodebookComboParametersAdditionPerBC-r16::= SEQUENCE {

-- R1 16-8 Mixed codebook types

type1SP-Type2-null-r16 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER (0..maxNrofCSI-RS-ResourcesAlt-1-r16)

OPTIONAL,

type1SP-Type2PS-null-r16 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER (0..maxNrofCSI-RS-ResourcesAlt-1-r16)

OPTIONAL,

type1SP-eType2R1-null-r16 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER (0..maxNrofCSI-RS-ResourcesAlt-1-r16)

OPTIONAL,

type1SP-eType2R2-null-r16 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER (0..maxNrofCSI-RS-ResourcesAlt-1-r16)

OPTIONAL,

type1SP-eType2R1PS-null-r16 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER (0..maxNrofCSI-RS-ResourcesAlt-1-r16)

OPTIONAL,

type1SP-eType2R2PS-null-r16 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER (0..maxNrofCSI-RS-ResourcesAlt-1-r16)

OPTIONAL,

type1SP-Type2-Type2PS-r16 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER (0..maxNrofCSI-RS-ResourcesAlt-1-r16)

OPTIONAL,

type1MP-Type2-null-r16 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER (0..maxNrofCSI-RS-ResourcesAlt-1-r16)

OPTIONAL,

type1MP-Type2PS-null-r16 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER (0..maxNrofCSI-RS-ResourcesAlt-1-r16)

OPTIONAL,

type1MP-eType2R1-null-r16 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER (0..maxNrofCSI-RS-ResourcesAlt-1-r16)

OPTIONAL,

type1MP-eType2R2-null-r16 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER (0..maxNrofCSI-RS-ResourcesAlt-1-r16)

OPTIONAL,

type1MP-eType2R1PS-null-r16 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER (0..maxNrofCSI-RS-ResourcesAlt-1-r16)

OPTIONAL,

type1MP-eType2R2PS-null-r16 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER (0..maxNrofCSI-RS-ResourcesAlt-1-r16)

OPTIONAL,

type1MP-Type2-Type2PS-r16 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER (0..maxNrofCSI-RS-ResourcesAlt-1-r16)

OPTIONAL

}

CodebookParametersfetype2PerBC-r17 ::= SEQUENCE {

-- R1 23-9-1 Basic Features of Further Enhanced Port-Selection Type II Codebook (FeType-II)

fetype2basic-r17 SEQUENCE (SIZE (1.. maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER (0..maxNrofCSI-RS-ResourcesAlt-1-r16),

-- R1 23-9-2 Support of M=2 and R=1 for FeType-II

fetype2R1-r17 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r17)) OF INTEGER (0.. maxNrofCSI-RS-ResourcesAlt-1-r16)

OPTIONAL,

-- R1 23-9-4 Support of R = 2 for FeType-II

fetype2R2-r17 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r17)) OF INTEGER (0.. maxNrofCSI-RS-ResourcesAlt-1-r16)

OPTIONAL

}

CodebookComboParameterMixedTypePerBC-r17 ::= SEQUENCE {

-- R1 23-9-5 Active CSI-RS resources and ports for mixed codebook types in any slot

type1SP-feType2PS-null-r17 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER (0..maxNrofCSI-RS-ResourcesAlt-1-r16)

OPTIONAL,

type1SP-feType2PS-M2R1-null-r17 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER (0..maxNrofCSI-RS-ResourcesAlt-1-r16)

OPTIONAL,

type1SP-feType2PS-M2R2-null-r17 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER (0..maxNrofCSI-RS-ResourcesAlt-1-r16)

OPTIONAL,

type1SP-Type2-feType2-PS-M1-r17 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER (0..maxNrofCSI-RS-ResourcesAlt-1-r16)

OPTIONAL,

type1SP-Type2-feType2-PS-M2R1-r17 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER (0..maxNrofCSI-RS-ResourcesAlt-1-r16)

OPTIONAL,

type1SP-eType2R1-feType2-PS-M1-r17 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER (0..maxNrofCSI-RS-ResourcesAlt-1-r16)

OPTIONAL,

type1SP-eType2R1-feType2-PS-M2R1-r17 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER (0..maxNrofCSI-RS-ResourcesAlt-1-r16)

OPTIONAL,

type1MP-feType2PS-null-r17 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER (0..maxNrofCSI-RS-ResourcesAlt-1-r16)

OPTIONAL,

type1MP-feType2PS-M2R1-null-r17 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER (0..maxNrofCSI-RS-ResourcesAlt-1-r16)

OPTIONAL,

type1MP-feType2PS-M2R2-null-r17 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER (0..maxNrofCSI-RS-ResourcesAlt-1-r16)

OPTIONAL,

type1MP-Type2-feType2-PS-M1-r17 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER (0..maxNrofCSI-RS-ResourcesAlt-1-r16)

OPTIONAL,

type1MP-Type2-feType2-PS-M2R1-r17 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER (0..maxNrofCSI-RS-ResourcesAlt-1-r16)

OPTIONAL,

type1MP-eType2R1-feType2-PS-M1-r17 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER (0..maxNrofCSI-RS-ResourcesAlt-1-r16)

OPTIONAL,

type1MP-eType2R1-feType2-PS-M2R1-r17 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER (0..maxNrofCSI-RS-ResourcesAlt-1-r16)

OPTIONAL

}

CodebookComboParameterMultiTRP-PerBC-r17::= SEQUENCE {

-- R1 23-7-1b Active CSI-RS resources and ports in the presence of multi-TRP CSI

-- {Codebook 2, Codebook 3} =(NULL, NULL}

nCJT-null-null SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER (0..maxNrofCSI-RS-ResourcesAlt-1-r16)

OPTIONAL,

nCJT1SP-null-null SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER (0..maxNrofCSI-RS-ResourcesAlt-1-r16)

OPTIONAL,

-- {Codebook 2, Codebook 3} = {( {"Rel 16 combinations in FG 16-8"}

nCJT-Type2-null-r16 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER (0..maxNrofCSI-RS-ResourcesAlt-1-r16)

OPTIONAL,

nCJT-Type2PS-null-r16 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER (0..maxNrofCSI-RS-ResourcesAlt-1-r16)

OPTIONAL,

nCJT-eType2R1-null-r16 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER (0..maxNrofCSI-RS-ResourcesAlt-1-r16)

OPTIONAL,

nCJT-eType2R2-null-r16 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER (0..maxNrofCSI-RS-ResourcesAlt-1-r16)

OPTIONAL,

nCJT-eType2R1PS-null-r16 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER (0..maxNrofCSI-RS-ResourcesAlt-1-r16)

OPTIONAL,

nCJT-eType2R2PS-null-r16 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER (0..maxNrofCSI-RS-ResourcesAlt-1-r16)

OPTIONAL,

nCJT-Type2-Type2PS-r16 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER (0..maxNrofCSI-RS-ResourcesAlt-1-r16)

OPTIONAL,

nCJT1SP-Type2-null-r16 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER (0..maxNrofCSI-RS-ResourcesAlt-1-r16)

OPTIONAL,

nCJT1SP-Type2PS-null-r16 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER (0..maxNrofCSI-RS-ResourcesAlt-1-r16)

OPTIONAL,

nCJT1SP-eType2R1-null-r16 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER (0..maxNrofCSI-RS-ResourcesAlt-1-r16)

OPTIONAL,

nCJT1SP-eType2R2-null-r16 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER (0..maxNrofCSI-RS-ResourcesAlt-1-r16)

OPTIONAL,

nCJT1SP-eType2R1PS-null-r16 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER (0..maxNrofCSI-RS-ResourcesAlt-1-r16)

OPTIONAL,

nCJT1SP-eType2R2PS-null-r16 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER (0..maxNrofCSI-RS-ResourcesAlt-1-r16)

OPTIONAL,

nCJT1SP-Type2-Type2PS-r16 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER (0..maxNrofCSI-RS-ResourcesAlt-1-r16)

OPTIONAL,

-- {Codebook 2, Codebook 3} = {"New Rel17 combinations in FG 23-9-5"}

nCJT-feType2PS-null-r17 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER (0..maxNrofCSI-RS-ResourcesAlt-1-r16)

OPTIONAL,

nCJT-feType2PS-M2R1-null-r17 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER (0..maxNrofCSI-RS-ResourcesAlt-1-r16)

OPTIONAL,

nCJT-feType2PS-M2R2-null-r17 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER (0..maxNrofCSI-RS-ResourcesAlt-1-r16)

OPTIONAL,

nCJT-Type2-feType2-PS-M1-r17 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER (0..maxNrofCSI-RS-ResourcesAlt-1-r16)

OPTIONAL,

nCJT-Type2-feType2-PS-M2R1-r17 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER (0..maxNrofCSI-RS-ResourcesAlt-1-r16)

OPTIONAL,

nCJT-eType2R1-feType2-PS-M1-r17 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER (0..maxNrofCSI-RS-ResourcesAlt-1-r16)

OPTIONAL,

nCJT-eType2R1-feType2-PS-M2R1-r17 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER (0..maxNrofCSI-RS-ResourcesAlt-1-r16)

OPTIONAL,

nCJT1SP-feType2PS-null-r17 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER (0..maxNrofCSI-RS-ResourcesAlt-1-r16)

OPTIONAL,

nCJT1SP-feType2PS-M2R1-null-r17 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER (0..maxNrofCSI-RS-ResourcesAlt-1-r16)

OPTIONAL,

nCJT1SP-feType2PS-M2R2-null-r1 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER (0..maxNrofCSI-RS-ResourcesAlt-1-r16)

OPTIONAL,

nCJT1SP-Type2-feType2-PS-M1-r17 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER (0..maxNrofCSI-RS-ResourcesAlt-1-r16)

OPTIONAL,

nCJT1SP-Type2-feType2-PS-M2R1-r17 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER (0..maxNrofCSI-RS-ResourcesAlt-1-r16)

OPTIONAL,

nCJT1SP-eType2R1-feType2-PS-M1-r17 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER (0..maxNrofCSI-RS-ResourcesAlt-1-r16)

OPTIONAL,

nCJT1SP-eType2R1-feType2-PS-M2R1-r17 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER (0..maxNrofCSI-RS-ResourcesAlt-1-r16)

OPTIONAL

}

CodebookParametersetype2DopplerCSI-r18 ::= SEQUENCE {

-- R1 40-3-2-1: Support of Rel-16-based doppler CSI

eType2Doppler-r18 SEQUENCE {

supportedCSI-RS-ResourceList-r18 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER

(0..maxNrofCSI-RS-ResourcesAlt-1-r16),

valueY-P-SP-CSI-RS-r18 INTEGER (1..3),

valueY-A-CSI-RS-r18 INTEGER (1..3),

scalingfactor-r18 ENUMERATED {n1, n2, n4}

},

-- R1 40-3-2-1a: Support of Rel-16-based doppler measurement with N4>1

eType2DopplerN4-r18 SEQUENCE {

supportedCSI-RS-ReportSettingList1-r18 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF

SupportedCSI-RS-ReportSetting-r18,

supportedCSI-RS-ReportSettingList2-r18 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF

SupportedCSI-RS-ReportSetting-r18

} OPTIONAL,

-- R1 40-3-2-1a-1: DD unit size when A-CSI-RS is configured for CMR N4>1

ddUnitSize-A-CSI-RS-CMR-r18 ENUMERATED {supported} OPTIONAL,

-- R1 40-3-2-1b: Maximum number of aperiodic CSI-RS resources that can be configured in the same CSI report setting for

-- Rel-16-based doppler measurement

maxNumberAperiodicCSI-RS-Resource-r18 ENUMERATED {n4, n8, n12} OPTIONAL,

-- R1 40-3-2-2: Support R=2 for Rel-16-based doppler codebook

eType2DopplerR2-r18 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER (0..maxNrofCSI-RS-ResourcesAlt-1-r16)

OPTIONAL,

-- R1 40-3-2-3: Support X=1 based on first and last slot of WCSI, for Rel-16-based doppler codebook

eType2DopplerX1-r18 ENUMERATED {supported} OPTIONAL,

-- R1 40-3-2-3a: Support X=2 CQI based on 2 slots for Rel-16-based doppler codebook

eType2DopplerX2-r18 ENUMERATED {supported} OPTIONAL,

--R1 40-3-2-7: support of l = (n - nCSI,ref ) for CSI reference slot for Rel-16 based doppler codebook

eType2DopplerL-N4D1-r18 ENUMERATED {supported} OPTIONAL,

-- R1 40-3-2-8: Support of L=6 for Rel-16 based doppler codebook

eType2DopplerL6-r18 ENUMERATED {supported} OPTIONAL,

-- R1 40-3-2-9: Support of rank equals 3 and 4 for Rel-16 based doppler codebook

eType2DopplerR3R4-r18 ENUMERATED {supported} OPTIONAL

}

CodebookParametersfetype2DopplerCSI-r18 ::= SEQUENCE {

-- R1 40-3-2-4: Support of Rel-17-based doppler CSI

feType2Doppler-r18 SEQUENCE {

supportedCSI-RS-ResourceList-r18 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER

(0..maxNrofCSI-RS-ResourcesAlt-1-r16),

valueY-A-CSI-RS-r18 INTEGER (1..3),

scalingfactor-r18 ENUMERATED {n1, n2, n4}

},

-- R1 40-3-2-4b: Maximum number of aperiodic CSI-RS resources that can be configured in the same CSI report setting for

-- Rel-17-based doppler CSI

maxNumberAperiodicCSI-RS-Resource-r18 ENUMERATED {n4, n8, n12} OPTIONAL,

-- R1 40-3-2-5: Support of M=2 and R=1 for Rel-17-based doppler codebook

feType2DopplerM2R1-r18 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER

(0..maxNrofCSI-RS-ResourcesAlt-1-r16)

OPTIONAL,

-- R1 40-3-2-6: Support R=2 for Rel-17-based doppler codebook

feType2DopplerR2-r18 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER (0..maxNrofCSI-RS-ResourcesAlt-1-r16)

OPTIONAL,

--R1 40-3-2-7a: Support of l = (n - nCSI,ref ) for CSI reference slot for Rel-17 based doppler codebook

feType2DopplerL-N4D1-r18 ENUMERATED {supported} OPTIONAL,

-- R1 40-3-2-10: Support of rank equals 3 and 4 for Rel-17 based doppler codebook

feType2DopplerR3R4-r18 ENUMERATED {supported} OPTIONAL

}

CodebookParametersetype2CJT-r18 ::= SEQUENCE {

-- R1 40-3-1-1: Basic feature for Rel-16-based CJT type-II codebook

eType2CJT-r18 SEQUENCE {

supportedCSI-RS-ResourceList-r18 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER

(0..maxNrofCSI-RS-ResourcesAlt-1-r16),

scalingfactor-r18 ENUMERATED {n1, n1dot5, n2},

maxNumberNZP-CSI-RS-MultiTRP-CJT-r18 INTEGER (2..4)

},

-- R1 40-3-1-1a: Support of mode 1 for Rel-16-based CJT type-II codebook with FD basis selection integer frequency offset

eType2CJT-FD-IO-r18 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER

(0..maxNrofCSI-RS-ResourcesAlt-1-r16) OPTIONAL,

-- R1 40-3-1-2: Support for FD basis selection fractional offset mode for Rel-16-based CJT codebook with mode1

eType2CJT-FD-FO-r18 ENUMERATED {supported} OPTIONAL,

-- R1 40-3-1-3: Support R=2 for Rel-16-based CJT codebook

eType2CJT-R2-r18 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER

(0..maxNrofCSI-RS-ResourcesAlt-1-r16) OPTIONAL,

-- R1 40-3-1-4: Support pv={1/2,1/2,1/2,1/2} and beta=1/2 for Rel-16-based CJT codebook

eType2CJT-PV-Beta-r18 ENUMERATED {supported} OPTIONAL,

-- R1 40-3-1-9: Support for 2NN1N2 >32 for Rel-16 based CJT codebook

eType2CJT-2NN1N2-r18 ENUMERATED {n64,n96,n128} OPTIONAL,

-- R1 40-3-1-12: Support of Rank 3 and 4 for Rel-16-based CJT type-II codebook

eType2CJT-Rank3Rank4-r18 ENUMERATED {supported} OPTIONAL,

-- R1 40-3-1-14: Support of Support of L=6 for Rel-16-based CJT type-II codebook

eType2CJT-L6-r18 ENUMERATED {supported} OPTIONAL,

-- R1 40-3-1-15: dynamic selection of N<=N\_TRP for Rel-16-based CJT type-II codebook

eType2CJT-NN-r18 ENUMERATED {supported} OPTIONAL,

-- R1 40-3-1-17: Support for N\_L>1 combinations of number of SD basis across CSI-RS resources for Rel-16-based CJT

-- type-II codebook

eType2CJT-NL-SD-r18 ENUMERATED {n2,n4} OPTIONAL,

-- R1 40-3-1-23: Unequal number of spatial basis selection configuration for multi-TRP CJT

eType2CJT-Unequal-r18 ENUMERATED {supported} OPTIONAL

}

CodebookParametersfetype2CJT-r18 ::= SEQUENCE {

-- R1 40-3-1-5: Basic feature for Rel-17-based CJT type-II codebook

feType2CJT-r18 SEQUENCE {

supportedCSI-RS-ResourceList-r18 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER

(0..maxNrofCSI-RS-ResourcesAlt-1-r16),

scalingfactor-r18 ENUMERATED {n1, n1dot5, n2},

maxNumberNZP-CSI-RS-MultiTRP-CJT-r18 INTEGER (2..4)

},

-- R1 40-3-1-5a: Support of mode 1 for Rel-17-based CJT type-II codebook with FD basis selection integer frequency offset

feType2CJT-FD-IO-r18 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER

(0..maxNrofCSI-RS-ResourcesAlt-1-r16) OPTIONAL,

-- R1 40-3-1-6: Support for FD basis selection fractional offset mode for Rel-17-based CJT codebook with mode1

feType2CJT-FD-FO-r18 ENUMERATED {supported} OPTIONAL,

-- R1 40-3-1-7: Support of M=2 and R=1 for Rel-17-based CJT codebook

feType2CJT-M2R1-r18 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER

(0..maxNrofCSI-RS-ResourcesAlt-1-r16) OPTIONAL,

-- R1 40-3-1-8: Support of R=2 for Rel-17-based CJT codebook

feType2CJT-R2-r18 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER

(0..maxNrofCSI-RS-ResourcesAlt-1-r16) OPTIONAL,

-- R1 40-3-1-9a: Support for 2NN1N2 >32 for Rel-17 based CJT codebook

feType2CJT-2NN1N2-r18 ENUMERATED {n64,n96,n128} OPTIONAL,

-- R1 40-3-1-13: Support of Rank 3 and 4 for Rel-17-based CJT type-II codebook

feType2CJT-Rank3Rank4-r18 ENUMERATED {supported} OPTIONAL,

-- R1 40-3-1-16: dynamic selection of N<=N\_TRP for Rel-17-based CJT type-II codebook

feType2CJT-NN-r18 ENUMERATED {supported} OPTIONAL,

-- R1 40-3-1-18: Support for N\_L>1 combinations of number of SD basis across CSI-RS resources for Rel-17-based CJT

-- type-II codebook

feType2CJT-NL-r18 ENUMERATED {n2,n4} OPTIONAL,

-- R1 40-3-1-23a: Unequal number of port selection configuration for multi-TRP CJT

feType2CJT-Unequal-r18 ENUMERATED {supported} OPTIONAL

}

CodebookComboParametersCJT-r18::= SEQUENCE {

-- R1 40-3-1-11: Active CSI-RS resources and ports for mixed codebook types including Type-II-CJT in any slot

-- {Codebook 1} = Type I SP

cjt-Type1SP-eType2R1-null SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER (0..maxNrofCSI-RS-ResourcesAlt-1-r16)

OPTIONAL,

cjt-Type1SP-eType2R2-null SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER (0..maxNrofCSI-RS-ResourcesAlt-1-r16)

OPTIONAL,

cjt-Type1SP-feType2R1M1-null SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER (0..maxNrofCSI-RS-ResourcesAlt-1-r16)

OPTIONAL,

cjt-Type1SP-feType2R1M2-null SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER (0..maxNrofCSI-RS-ResourcesAlt-1-r16)

OPTIONAL,

cjt-Type1SP-feType2R2M2-null SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER (0..maxNrofCSI-RS-ResourcesAlt-1-r16)

OPTIONAL,

-- {Codebook 1} = Type I MP

cjt-Type1MP-eType2R1-null SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER (0..maxNrofCSI-RS-ResourcesAlt-1-r16)

OPTIONAL,

cjt-Type1MP-eType2R2-null SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER (0..maxNrofCSI-RS-ResourcesAlt-1-r16)

OPTIONAL,

cjt-Type1MP-feType2R1M1-null SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER (0..maxNrofCSI-RS-ResourcesAlt-1-r16)

OPTIONAL,

cjt-Type1MP-feType2R1M2-null SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER (0..maxNrofCSI-RS-ResourcesAlt-1-r16)

OPTIONAL,

cjt-Type1MP-feType2R2M2-null SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER (0..maxNrofCSI-RS-ResourcesAlt-1-r16)

OPTIONAL

}

CodebookParametersHARQ-ACK-PUSCH-r18::= SEQUENCE {

-- R1 55-4a: Multiplexing Type-1 HARQ-ACK codebook in a PUSCH for PDSCH scheduled after UL grant

multiplexingType1-r18 ENUMERATED {supported} OPTIONAL,

-- R1 55-4b: Multiplexing Type-2 HARQ-ACK codebook in a PUSCH for PDSCH scheduled after UL grant

multiplexingType2-r18 ENUMERATED {supported} OPTIONAL,

-- R1 55-4c: Multiplexing Type-3 HARQ-ACK codebook in a PUSCH for PDSCH scheduled after UL grant

multiplexingType3-r18 ENUMERATED {supported} OPTIONAL,

-- R1 55-4d: Determining a different PUCCH resource to transmit HARQ-ACK for PDSCH scheduled after UL grant

pucch-DiffResource-PDSCH-r18 ENUMERATED {supported} OPTIONAL,

-- R1 55-4e: Determining different codebook size to transmit HARQ-ACK for PDSCH scheduled after UL grant

diffCB-Size-PDSCH-r18 ENUMERATED {supported} OPTIONAL

}

CodebookParametersType1SP-SchemeA-r19 ::= SEQUENCE {

-- R1 59-2-1-1: Enhanced Type-I SP codebook for 64 ports – Scheme-A

enhType1SP64PortsSchemeA-r19 SEQUENCE {

supportedCSI-RS-ResourceExtList-r19 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER

(0..maxNrofCSI-RS-ResourcesAlt-1-r16),

maxRank-r19 INTEGER (4..8),

maxNumberResource-r19 ENUMERATED {n2, n4},

processingCapability-r19 ENUMERATED {cap1, cap2},

supportedCSI-RS-ResourceListPerCC-r19 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER

(0..maxNrofCSI-RS-ResourcesAlt-1-r16)

},

-- R1 59-2-1-1a: Enhanced Type-I SP codebook for 48 ports – Scheme-A

enhType1SP48PortsSchemeA-r19 SEQUENCE {

supportedCSI-RS-ResourceExtList-r19 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER

(0..maxNrofCSI-RS-ResourcesAlt-1-r16),

maxRank-r19 INTEGER (4..8),

maxNumberResource-r19 INTEGER (1..8),

processingCapability-r19 ENUMERATED {cap1, cap2},

supportedCSI-RS-ResourceListPerCC-r19 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER

(0..maxNrofCSI-RS-ResourcesAlt-1-r16)

} OPTIONAL,

-- R1 59-2-1-1b: Enhanced Type-I SP codebook for 128 ports – Scheme-A

enhType1SP128PortsSchemeA-r19 SEQUENCE {

supportedCSI-RS-ResourceExtList-r19 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER

(0..maxNrofCSI-RS-ResourcesAlt-1-r16),

maxRank-r19 INTEGER (4..8),

processingCapability-r19 ENUMERATED {cap1, cap2},

supportedCSI-RS-ResourceListPerCC-r19 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER

(0..maxNrofCSI-RS-ResourcesAlt-1-r16)

} OPTIONAL

}

CodebookParametersType1SP-SchemeB-r19 ::= SEQUENCE {

-- R1 59-2-1-1c: Enhanced Type-I SP codebook for 64 ports – Scheme-B

enhType1SP64PortsSchemeB-r19 SEQUENCE {

supportedCSI-RS-ResourceExtList-r19 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER

(0..maxNrofCSI-RS-ResourcesAlt-1-r16),

maxRank-r19 INTEGER (4..8),

maxNumberResource-r19 ENUMERATED {n2, n4},

processingCapability-r19 ENUMERATED {cap1, cap2},

supportedCSI-RS-ResourceListPerCC-r19 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER

(0..maxNrofCSI-RS-ResourcesAlt-1-r16)

},

-- R1 59-2-1-1d: Enhanced Type-I SP codebook for 48 ports – Scheme-B

enhType1SP48PortsSchemeB-r19 SEQUENCE {

supportedCSI-RS-ResourceExtList-r19 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER

(0..maxNrofCSI-RS-ResourcesAlt-1-r16),

maxRank-r19 INTEGER (4..8),

maxNumberResource-r19 ENUMERATED {n2,n3},

processingCapability-r19 ENUMERATED {cap1, cap2},

supportedCSI-RS-ResourceListPerCC-r19 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER

(0..maxNrofCSI-RS-ResourcesAlt-1-r16)

} OPTIONAL,

-- R1 59-2-1-1e: Enhanced Type-I SP codebook for 128 ports – Scheme-B

enhType1SP128PortsSchemeB-r19 SEQUENCE {

supportedCSI-RS-ResourceExtList-r19 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER

(0..maxNrofCSI-RS-ResourcesAlt-1-r16),

maxRank-r19 INTEGER (4..8),

processingCapability-r19 ENUMERATED {cap1, cap2},

supportedCSI-RS-ResourceListPerCC-r19 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER

(0..maxNrofCSI-RS-ResourcesAlt-1-r16)

} OPTIONAL

}

CodebookParametersType1MP-r19 ::= SEQUENCE {

-- R1 59-2-1-2: Enhanced Type-I MP codebook for 64 ports

enhType1MP64Ports-r19 SEQUENCE {

supportedCSI-RS-ResourceExtList-r19 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER

(0..maxNrofCSI-RS-ResourcesAlt-1-r16),

maxPanel-r19 ENUMERATED {n2, n4},

maxNumberResource-r19 ENUMERATED {n2, n4},

processingCapability-r19 ENUMERATED {cap1, cap2},

supportedCSI-RS-ResourceListPerCC-r19 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER

(0..maxNrofCSI-RS-ResourcesAlt-1-r16)

},

-- R1 59-2-1-2a: Enhanced Type-I MP codebook for 48 ports

enhType1MP48Ports-r19 SEQUENCE {

supportedCSI-RS-ResourceExtList-r19 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER

(0..maxNrofCSI-RS-ResourcesAlt-1-r16),

maxPanel-r19 ENUMERATED {n2, n4},

maxNumberResource-r19 ENUMERATED {n2,n3},

processingCapability-r19 ENUMERATED {cap1, cap2},

supportedCSI-RS-ResourceListPerCC-r19 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER

(0..maxNrofCSI-RS-ResourcesAlt-1-r16)

} OPTIONAL,

-- R1 59-2-1-2b: Enhanced Type-I MP codebook for 128 ports

enhType1MP128Ports-r19 SEQUENCE {

supportedCSI-RS-ResourceExtList-r19 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER

(0..maxNrofCSI-RS-ResourcesAlt-1-r16),

maxPanel-r19 ENUMERATED {n2, n4},

processingCapability-r19 ENUMERATED {cap1, cap2},

supportedCSI-RS-ResourceListPerCC-r19 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER

(0..maxNrofCSI-RS-ResourcesAlt-1-r16)

} OPTIONAL

}

CodebookParameterseType2Ext-r19 ::= SEQUENCE {

-- R1 59-2-1-3: Extended Rel-16 eType-II codebook for 64 Tx ports

eType2-64PortExt-r19 SEQUENCE {

supportedCSI-RS-ResourceExtList-r19 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER

(0..maxNrofCSI-RS-ResourcesAlt-1-r16),

processingCapability-r19 ENUMERATED {cap1, cap2},

maxNumberResource-r19 ENUMERATED {n2, n4},

supportedCSI-RS-ResourceListPerCC-r19 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER

(0..maxNrofCSI-RS-ResourcesAlt-1-r16)

},

-- R1 59-2-1-3a: Extended Rel-16 eType-II codebook for 48 Tx ports

eType2-48PortExt-r19 SEQUENCE {

supportedCSI-RS-ResourceExtList-r19 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER

(0..maxNrofCSI-RS-ResourcesAlt-1-r16),

processingCapability-r19 ENUMERATED {cap1, cap2},

maxNumberResource-r19 ENUMERATED {n2,n3},

supportedCSI-RS-ResourceListPerCC-r19 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER

(0..maxNrofCSI-RS-ResourcesAlt-1-r16)

} OPTIONAL,

-- R1 59-2-1-3b: Extended Rel-16 eType-II codebook for 128 Tx ports

eType2-128PortExt-r19 SEQUENCE {

supportedCSI-RS-ResourceExtList-r19 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER

(0..maxNrofCSI-RS-ResourcesAlt-1-r16),

processingCapability-r19 ENUMERATED {cap1, cap2},

supportedCSI-RS-ResourceListPerCC-r19 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER

(0..maxNrofCSI-RS-ResourcesAlt-1-r16)

} OPTIONAL,

-- R1 59-2-1-3-1: PMI sub-bands with R=2 for extended Rel-16 eType-II codebook for up to 128 ports

eType2R2Ext-r19 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER

(0..maxNrofCSI-RS-ResourcesAlt-1-r16) OPTIONAL,

-- R1 59-2-1-3-3-2: Parameter combinations 7-8 for extended Rel-16 eType-II codebook for up to 128 ports

eType2ExtPC7-8-r19 ENUMERATED {supported} OPTIONAL,

-- R1 59-2-1-3-3: Rank 3,4 for extended Rel-16 eType-II codebook for up to 128 ports

eType2R3R4Ext-r19 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER

(0..maxNrofCSI-RS-ResourcesAlt-1-r16) OPTIONAL

}

CodebookParametersfeType2Ext-r19 ::= SEQUENCE {

-- R1 59-2-1-4: Extended Rel-17 FeType-II codebook with 64 Tx ports

feType2-64PortExt-r19 SEQUENCE {

supportedCSI-RS-ResourceExtList-r19 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER

(0..maxNrofCSI-RS-ResourcesAlt-1-r16),

processingCapability-r19 ENUMERATED {cap1, cap2},

maxNumberResource-r19 ENUMERATED {n2, n4},

supportedCSI-RS-ResourceListPerCC-r19 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER

(0..maxNrofCSI-RS-ResourcesAlt-1-r16)

},

-- R1 59-2-1-4a: Extended Rel-17 FeType-II codebook with 48 Tx ports

feType2-48PortExt-r19 SEQUENCE {

supportedCSI-RS-ResourceExtList-r19 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER

(0..maxNrofCSI-RS-ResourcesAlt-1-r16),

processingCapability-r19 ENUMERATED {cap1, cap2},

maxNumberResource-r19 ENUMERATED {n2,n3},

supportedCSI-RS-ResourceListPerCC-r19 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER

(0..maxNrofCSI-RS-ResourcesAlt-1-r16)

} OPTIONAL,

-- R1 59-2-1-4b: M=2 and R=1 for extended Rel-17 FeType-II PS (port selection) codebook for up to 64 ports

feType2-M2R1Ext-r19 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER

(0..maxNrofCSI-RS-ResourcesAlt-1-r16) OPTIONAL,

--R1 59-2-1-4c: M=2 and R=2 for extended Rel-17 FeType-II PS (port selection) codebook for up to 64 ports

feType2-M2R2Ext-r19 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER

(0..maxNrofCSI-RS-ResourcesAlt-1-r16) OPTIONAL,

-- R1 59-2-1-4d: Rank 3,4 for extended Rel-17 FeType-II PS (port selection) codebook for up to 64ports

feType2-R3R4Ext-r19 ENUMERATED {supported} OPTIONAL

}

CodebookParameterseType2DopplerExt-r19 ::= SEQUENCE {

-- R1 59-2-1-5: Extended Rel-18 eType-II Doppler codebook for 64 Tx ports

eType2Doppler-64PortExt-r19 SEQUENCE {

supportedCSI-RS-ResourceExtList-r19 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER

(0..maxNrofCSI-RS-ResourcesAlt-1-r16),

processingCapability-r19 ENUMERATED {cap1, cap2},

valueY-P-SP-CSI-RS-r19 INTEGER (1..3),

valueY-A-CSI-RS-r19 INTEGER (1..3),

scalingfactor-r19 ENUMERATED {n1, n2, n4},

maxNumberResource-r19 ENUMERATED {n2, n4},

supportedCSI-RS-ResourceListPerCC-r19 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER

(0..maxNrofCSI-RS-ResourcesAlt-1-r16)

},

-- R1 59-2-1-5a: Extended Rel-18 eType-II Doppler codebook for 48 Tx ports

eType2Doppler-48PortExt-r19 SEQUENCE {

supportedCSI-RS-ResourceExtList-r19 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER

(0..maxNrofCSI-RS-ResourcesAlt-1-r16),

processingCapability-r19 ENUMERATED {cap1, cap2},

valueY-P-SP-CSI-RS-r19 INTEGER (1..3),

valueY-A-CSI-RS-r19 INTEGER (1..3),

scalingfactor-r19 ENUMERATED {n1, n2, n4},

maxNumberResource-r19 ENUMERATED {n2,n3},

supportedCSI-RS-ResourceListPerCC-r19 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER

(0..maxNrofCSI-RS-ResourcesAlt-1-r16)

} OPTIONAL,

-- R1 59-2-1-5b: Extended Rel-18 eType-II Doppler codebook for 128 Tx ports

eType2Doppler-128PortExt-r19 SEQUENCE {

supportedCSI-RS-ResourceExtList-r19 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER

(0..maxNrofCSI-RS-ResourcesAlt-1-r16),

processingCapability-r19 ENUMERATED {cap1, cap2},

valueY-P-SP-CSI-RS-r19 INTEGER (1..3),

valueY-A-CSI-RS-r19 INTEGER (1..3),

scalingfactor-r19 ENUMERATED {n1, n2, n4},

supportedCSI-RS-ResourceListPerCC-r19 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER

(0..maxNrofCSI-RS-ResourcesAlt-1-r16)

} OPTIONAL,

-- R1 59-2-1-5c: N4>1 for extended Rel-18 Type-II Doppler codebook for up to 128 ports

eType2DopplerN4Ext-r19 SEQUENCE {

supportedCSI-RS-ReportSettingList1-r19 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF

SupportedCSI-RS-ReportSettingExt-r19,

supportedCSI-RS-ReportSettingList2-r19 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF

SupportedCSI-RS-ReportSettingExt-r19

} OPTIONAL,

-- R1 59-2-1-5d: DD unit size d=1 when A-CSI-RS is configured for CMR N4>1 for extended Rel-18 Type-II Doppler codebook for up to 128 ports

ddUnitSize-A-CSI-RS-CMR-Ext-r19 ENUMERATED {supported} OPTIONAL,

-- R1 59-2-1-5e: Maximum number of aperiodic CSI-RS resources groups that can be configured in the same CSI report setting for extended

-- Rel-18 Type-II Doppler codebook for up to 128 ports

maxNumberAperiodicCSI-RS-ResourceExt-r19 ENUMERATED {n4, n8, n12} OPTIONAL,

-- R1 59-2-1-5f: PMI subband R=2 for extended Rel-18 Type-II Doppler codebook for up to 128 ports

eType2DopplerR2Ext-r19 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER (0..maxNrofCSI-RS-ResourcesAlt-1-r16)

OPTIONAL,

-- R1 59-2-1-5g: X=1 based on first and last slot of WCSI for extended Rel-18 Type-II Doppler codebook for up to 128 ports

eType2DopplerX1Ext-r19 ENUMERATED {supported} OPTIONAL,

-- R1 59-2-1-5h: X=2 CQI based on 2 slots for extended Rel-18 Type-II Doppler codebook for up to 128 ports

eType2DopplerX2Ext-r19 ENUMERATED {supported} OPTIONAL,

--R1 59-2-1-5i: l = (n – nCSI,ref ) for CSI reference slot for extended Rel-18 Type-II Doppler codebook for up to 128 ports

eType2DopplerL-N4D1Ext-r19 ENUMERATED {supported} OPTIONAL,

-- R1 59-2-1-5j: L=6 for CSI reference slot for extended Rel-18 Type-II Doppler codebook for up to 128 ports

eType2DopplerL6Ext-r19 ENUMERATED {supported} OPTIONAL,

-- R1 59-2-1-5k: Rank 3 and 4 for CSI reference slot for extended Rel-18 Type-II Doppler codebook for up to 128 ports

eType2DopplerR3R4Ext-r19 ENUMERATED {supported} OPTIONAL,

-- R1 59-2-1-5l: Processing timeline for CSI reference slot for extended Rel-18 Type-II Doppler codebook for up to 128 ports

eType2DopplerProcessingTimelineExt-r19 SEQUENCE {

valueW-r19 SEQUENCE{

scs-15kHz ENUMERATED {value1, value2} OPTIONAL,

scs-30kHz ENUMERATED {value1, value2} OPTIONAL,

scs-60kHz ENUMERATED {value1, value2} OPTIONAL,

scs-120kHz ENUMERATED {value1, value2} OPTIONAL

},

timeRelaxation-r19 ENUMERATED {cap1, cap2}

} OPTIONAL,

-- R1 59-2-1-5m: Maximum periodicity of CMR when configured as periodic CSI-Rs for extended Rel-18 Type-II Doppler codebook for up to 128 ports

eType2MaxPeriodicityCMR-r19 ENUMERATED {sl4, sl5, sl8, sl10, sl20} OPTIONAL

}

-- R1 59-2-2-1: Hybrid BF (CRI-based) with Rel-15 Type-I SP codebook

CodebookParametersHybridBF-Type1SP-r19 ::= SEQUENCE {

maxNumberCRI-Report-r19 INTEGER (1..4),

supportedCSI-RS-ResourceHybridList-r19 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER

(0..maxNrofCSI-RS-ResourcesAlt-1-r16),

maxValueKs-r19 INTEGER (2..8)

}

-- R1 59-2-2-2: Hybrid BF (CRI-based) with Rel-16 eType-II codebook

CodebookParametersHybridBF-eType2-r19 ::= SEQUENCE {

maxNumberCRI-Report-r19 INTEGER (1..2),

supportedCSI-RS-ResourceHybridList-r19 SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesExt-r16)) OF INTEGER

(0..maxNrofCSI-RS-ResourcesAlt-1-r16),

maxValueKs-r19 INTEGER (2..8)

}

CodebookVariantsList-r16 ::= SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesAlt-r16)) OF SupportedCSI-RS-Resource

CodebookVariantsListExt-r19 ::= SEQUENCE (SIZE (1.. maxNrofCSI-RS-ResourcesAlt-r16)) OF SupportedCSI-RS-ResourceExt-r19

CodebookVariantsListAggregate-r19 ::= SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesAlt-r16)) OF SupportedCSI-RS-ResourceAggregate-r19

CodebookVariantsListHybrid-r19 ::= SEQUENCE (SIZE (1..maxNrofCSI-RS-ResourcesAlt-r16)) OF SupportedCSI-RS-ResourceHybrid-r19

SupportedCSI-RS-Resource ::= SEQUENCE {

maxNumberTxPortsPerResource ENUMERATED {p2, p4, p8, p12, p16, p24, p32},

maxNumberResourcesPerBand INTEGER (1..64),

totalNumberTxPortsPerBand INTEGER (2..256)

}

SupportedCSI-RS-ReportSetting-r18 ::= SEQUENCE {

maxN4-r18 ENUMERATED {n1, n2, n4, n8},

maxNumberTxPortsPerResource-r18 ENUMERATED {p2, p4, p8, p12, p16, p24, p32},

maxNumberResourcesPerBand-r18 INTEGER (1..64),

totalNumberTxPortsPerBand-r18 INTEGER (2..256)

}

SupportedCSI-RS-ResourceExt-r19 ::= SEQUENCE {

maxNumberResourcesPerBand-r19 INTEGER (1..256),

totalNumberTxPortsPerBand-r19 INTEGER (64..1024)

}

SupportedCSI-RS-ResourceAggregate-r19 ::= SEQUENCE {

maxNumberTxPortsPerAggregatedResource-r19 ENUMERATED {p48, p64, p128},

maxNumberAggregatedResources-r19 INTEGER (1..64),

totalNumberTxPorts-r19 INTEGER (48..1024)

}

SupportedCSI-RS-ReportSettingExt-r19 ::= SEQUENCE {

maxN4-r19 ENUMERATED {n1, n2, n4, n8},

maxNumberTxPortsPerAggregatedResource-r19 ENUMERATED {p48, p64, p128},

maxNumberAggregatedResources-r19 INTEGER (2..64),

totalNumberTxPorts-r19 INTEGER (64..1024)

}

SupportedCSI-RS-ResourceHybrid-r19 ::= SEQUENCE {

maxNumberTxPortsPerResource-r19 ENUMERATED {p2, p4, p8, p12, p16, p24, p32},

maxNumberResources-r19 INTEGER (1..256),

totalNumberTxPorts-r19 INTEGER (64..1024)

}

-- TAG-CODEBOOKPARAMETERS-STOP

-- ASN1STOP

|  |
| --- |
| *CodebookParameters* field descriptions |
| ***supportedCSI-RS-ResourceListAlt***  This field indicates the alternative list of *SupportedCSI-RS-Resource* supported for each codebook type. The supported CSI-RS resource is indicated by an integer value which pinpoints *SupportedCSI-RS-Resource* defined in *CodebookVariantsList*. The value 0 corresponds to the first entry of *CodebookVariantsList*. The value 1 corresponds to the second entry of *CodebookVariantsList*, and so on. For each codebook type, the field shall be included in both *codebookParametersPerBC* (but optional for single CC) and *codebookParametersPerBand*. |
| ***supportedCSI-RS-ResourceExtList-r19, supportedCSI-RS-ResourceListPerCC-r19***  This field indicates the alternative list of *SupportedCSI-RS-ResourceExt* supported for each codebook type. The supported CSI-RS resource is indicated by an integer value which pinpoints *SupportedCSI-RS-ResourceExt* defined in *CodebookVariantsListExt*. The value 0 corresponds to the first entry of *CodebookVariantsListExt*. The value 1 corresponds to the second entry of *CodebookVariantsListExt*, and so on. For each codebook type, the field shall be included in both *codebookParametersPerBC* (but optional for single CC) and *codebookParametersPerBand*. |
| ***supportedCSI-RS-ResourceHybridList-r19***  This field indicates the alternative list of *SupportedCSI-RS-ResourceHybrid* supported for each codebook type. The supported CSI-RS resource is indicated by an integer value which pinpoints *SupportedCSI-RS- ResourceHybrid* defined in *CodebookVariantsListHybrid*. The value 0 corresponds to the first entry of *CodebookVariantsListHybrid*. The value 1 corresponds to the second entry of *CodebookVariantsListHybrid*, and so on. For each codebook type, the field shall be included in both *codebookParametersPerBC* (but optional for single CC) and *codebookParametersPerBand*. |

#### – *DL-PRS-MeasurementWithRxFH-RRC-Connected*

The IE *DL-PRS-MeasurementWithRxFH-RRC-Connected* is used to convey the capabilities supported by the UE for PRS measurement with Rx frequency hopping within a measurement gap and measurement reporting in RRC\_CONNECTED for RedCap UEs.

*DL-PRS-MeasurementWithRxFH-RRC-Connected information element*

-- ASN1START

-- TAG-DL-PRS-MEASUREMENTWITHRXFH-RRC-CONNECTED-START

DL-PRS-MeasurementWithRxFH-RRC-Connected-r18 ::= SEQUENCE {

maximumPRS-BandwidthAcrossAllHopsFR1-r18 ENUMERATED {mhz40, mhz50, mhz80, mhz100} OPTIONAL,

maximumPRS-BandwidthAcrossAllHopsFR2-r18 ENUMERATED {mhz100, mhz200, mhz400} OPTIONAL,

maximumFH-Hops-r18 ENUMERATED {n2, n3, n4, n5, n6} OPTIONAL,

processingDuration-r18 SEQUENCE {

processingPRS-SymbolsDurationN3-r18 ENUMERATED {msDot125, msDot25, msDot5, ms1, ms2, ms4, ms6, ms8, ms12,

ms16, ms20, ms25, ms30, ms32, ms35, ms40, ms45, ms50},

processingDurationT3-r18 ENUMERATED {ms8, ms16, ms20, ms30, ms40, ms80, ms160, ms320, ms640, ms1280}

} OPTIONAL,

rf-RxRetuneTimeFR1-r18 ENUMERATED {n70, n140, n210} OPTIONAL,

rf-RxRetuneTimeFR2-r18 ENUMERATED {n35, n70, n140} OPTIONAL,

numOfOverlappingPRB-r18 ENUMERATED {n0, n1, n2, n4} OPTIONAL,

...

}

-- TAG-DL-PRS-MEASUREMENTWITHRXFH-RRC-CONNECTED-STOP

-- ASN1STOP

#### – *ERedCapParameters*

The IE *ERedCapParameters* is used to indicate the UE capabilities supported by eRedCap UEs.

*ERedCapParameters* information element

-- ASN1START

-- TAG-EREDCAPPARAMETERS-START

ERedCapParameters-r18::= SEQUENCE {

-- R1 48-1: eRedCap UE with reduced peak data rate and reduced baseband bandwidth in FR1

supportOfERedCap-r18 ENUMERATED {supported},

-- R1 48-2: eRedCap UE with reduced peak data rate without reduced baseband bandwidth in FR1

eRedCapNotReducedBB-BW-r18 ENUMERATED {supported} OPTIONAL,

eRedCapIgnoreCapabilityFiltering-r18 ENUMERATED {supported} OPTIONAL

}

-- TAG-EREDCAPPARAMETERS-STOP

-- ASN1STOP

#### – *FeatureSetCombination*

The IE *FeatureSetCombination* is a two-dimensional matrix of *FeatureSet* entries.

Each *FeatureSetsPerBand* contains a list of feature sets applicable to the carrier(s) of one band entry of the associated band combination. Across the associated bands, the UE shall support the combination of *FeatureSets* at the same position in the *FeatureSetsPerBand*. All *FeatureSetsPerBand* in one *FeatureSetCombination* must have the same number of entries.

The number of *FeatureSetsPerBand* in the *FeatureSetCombination* must be equal to the number of band entries in an associated band combination. The first *FeatureSetPerBand* applies to the first band entry of the band combination, and so on.

Each *FeatureSet* contains either a pair of NR or E-UTRA feature set IDs for UL and DL.

In case of NR, the actual feature sets for UL and DL are defined in the *FeatureSets* IE and referred to from here by their ID, i.e., their position in the *featureSetsUplink* / *featureSetsDownlink* list in the FeatureSet IE.

In case of E-UTRA, the feature sets referred to from this list are defined in TS 36.331 [10] and conveyed as part of the *UE-EUTRA-Capability* container.

The *FeatureSetUplink* and *FeatureSetDownlink* referred to from the *FeatureSet* comprise, among other information, a set of *FeatureSetUplinkPerCC-Ids* and *FeatureSetDownlinkPerCC-Ids*. The number of these per-CC IDs determines the number of carriers that the UE is able to aggregate contiguously in frequency domain in the corresponding band. The number of carriers supported by the UE is also restricted by the bandwidth class indicated in the associated *BandCombination*, if present.

In feature set combinations the UE shall exclude entries with same or lower capabilities, since the network may anyway assume that the UE supports those.

NOTE 1: The UE may advertise fallback band-combinations in which it supports additional functionality explicitly in two ways: Either by setting FeatureSet IDs to zero (inter-band and intra-band non-contiguous fallback) and by reducing the number of FeatureSet-PerCC Ids in a Feature Set (intra-band contiguous fallback). Or by separate *BandCombination* entries with associated *FeatureSetCombinations*.

NOTE 2: The UE may advertise a *FeatureSetCombination* containing only fallback band combinations. That means, in a *FeatureSetCombination,* each group of *FeatureSets* across the bands may contain at least one pair of *FeatureSetUplinkId* and *FeatureSetDownlinkId* which is set to 0/0.

NOTE 3: The Network configures serving cell(s) and BWP(s) configuration to comply with capabilities derived from the combination of FeatureSets at the same position in the FeatureSetsPerBand, regardless of activated/deactivated serving cell(s) and BWP(s).

*FeatureSetCombination* information element

-- ASN1START

-- TAG-FEATURESETCOMBINATION-START

FeatureSetCombination ::= SEQUENCE (SIZE (1..maxSimultaneousBands)) OF FeatureSetsPerBand

FeatureSetsPerBand ::= SEQUENCE (SIZE (1..maxFeatureSetsPerBand)) OF FeatureSet

FeatureSet ::= CHOICE {

eutra SEQUENCE {

downlinkSetEUTRA FeatureSetEUTRA-DownlinkId,

uplinkSetEUTRA FeatureSetEUTRA-UplinkId

},

nr SEQUENCE {

downlinkSetNR FeatureSetDownlinkId,

uplinkSetNR FeatureSetUplinkId

}

}

-- TAG-FEATURESETCOMBINATION-STOP

-- ASN1STOP

#### – *FeatureSetCombinationId*

The IE *FeatureSetCombinationId* identifies a *FeatureSetCombination*. The *FeatureSetCombinationId* of a *FeatureSetCombination* is the position of the *FeatureSetCombination* in the featureSetCombinations list (in *UE-NR-Capability* or *UE-MRDC-Capability*). The *FeatureSetCombinationId* = 0 refers to the first entry in the *featureSetCombinations* list (in *UE-NR-Capability* or *UE-MRDC-Capability*).

NOTE: The *FeatureSetCombinationId* = 1024 is not used due to the maximum entry number of *featureSetCombinations*.

*FeatureSetCombinationId* information element

-- ASN1START

-- TAG-FEATURESETCOMBINATIONID-START

FeatureSetCombinationId ::= INTEGER (0.. maxFeatureSetCombinations)

-- TAG-FEATURESETCOMBINATIONID-STOP

-- ASN1STOP

#### – *FeatureSetDownlink*

The IE *FeatureSetDownlink* indicates a set of features that the UE supports on the carriers corresponding to one band entry in a band combination.

*FeatureSetDownlink* information element

-- ASN1START

-- TAG-FEATURESETDOWNLINK-START

FeatureSetDownlink ::= SEQUENCE {

featureSetListPerDownlinkCC SEQUENCE (SIZE (1..maxNrofServingCells)) OF FeatureSetDownlinkPerCC-Id,

intraBandFreqSeparationDL FreqSeparationClass OPTIONAL,

scalingFactor ENUMERATED {f0p4, f0p75, f0p8} OPTIONAL,

dummy8 ENUMERATED {supported} OPTIONAL,

scellWithoutSSB ENUMERATED {supported} OPTIONAL,

csi-RS-MeasSCellWithoutSSB ENUMERATED {supported} OPTIONAL,

dummy1 ENUMERATED {supported} OPTIONAL,

type1-3-CSS ENUMERATED {supported} OPTIONAL,

pdcch-MonitoringAnyOccasions ENUMERATED {withoutDCI-Gap, withDCI-Gap} OPTIONAL,

dummy2 ENUMERATED {supported} OPTIONAL,

ue-SpecificUL-DL-Assignment ENUMERATED {supported} OPTIONAL,

searchSpaceSharingCA-DL ENUMERATED {supported} OPTIONAL,

timeDurationForQCL SEQUENCE {

scs-60kHz ENUMERATED {s7, s14, s28} OPTIONAL,

scs-120kHz ENUMERATED {s14, s28} OPTIONAL

} OPTIONAL,

pdsch-ProcessingType1-DifferentTB-PerSlot SEQUENCE {

scs-15kHz ENUMERATED {upto2, upto4, upto7} OPTIONAL,

scs-30kHz ENUMERATED {upto2, upto4, upto7} OPTIONAL,

scs-60kHz ENUMERATED {upto2, upto4, upto7} OPTIONAL,

scs-120kHz ENUMERATED {upto2, upto4, upto7} OPTIONAL

} OPTIONAL,

dummy3 DummyA OPTIONAL,

dummy4 SEQUENCE (SIZE (1.. maxNrofCodebooks)) OF DummyB OPTIONAL,

dummy5 SEQUENCE (SIZE (1.. maxNrofCodebooks)) OF DummyC OPTIONAL,

dummy6 SEQUENCE (SIZE (1.. maxNrofCodebooks)) OF DummyD OPTIONAL,

dummy7 SEQUENCE (SIZE (1.. maxNrofCodebooks)) OF DummyE OPTIONAL

}

FeatureSetDownlink-v1540 ::= SEQUENCE {

oneFL-DMRS-TwoAdditionalDMRS-DL ENUMERATED {supported} OPTIONAL,

additionalDMRS-DL-Alt ENUMERATED {supported} OPTIONAL,

twoFL-DMRS-TwoAdditionalDMRS-DL ENUMERATED {supported} OPTIONAL,

oneFL-DMRS-ThreeAdditionalDMRS-DL ENUMERATED {supported} OPTIONAL,

pdcch-MonitoringAnyOccasionsWithSpanGap SEQUENCE {

scs-15kHz ENUMERATED {set1, set2, set3} OPTIONAL,

scs-30kHz ENUMERATED {set1, set2, set3} OPTIONAL,

scs-60kHz ENUMERATED {set1, set2, set3} OPTIONAL,

scs-120kHz ENUMERATED {set1, set2, set3} OPTIONAL

} OPTIONAL,

pdsch-SeparationWithGap ENUMERATED {supported} OPTIONAL,

pdsch-ProcessingType2 SEQUENCE {

scs-15kHz ProcessingParameters OPTIONAL,

scs-30kHz ProcessingParameters OPTIONAL,

scs-60kHz ProcessingParameters OPTIONAL

} OPTIONAL,

pdsch-ProcessingType2-Limited SEQUENCE {

differentTB-PerSlot-SCS-30kHz ENUMERATED {upto1, upto2, upto4, upto7}

} OPTIONAL,

dl-MCS-TableAlt-DynamicIndication ENUMERATED {supported} OPTIONAL

}

FeatureSetDownlink-v15a0 ::= SEQUENCE {

supportedSRS-Resources SRS-Resources OPTIONAL

}

FeatureSetDownlink-v15t0 ::= SEQUENCE {

zeroSlotOffsetAperiodicSRS ENUMERATED {supported} OPTIONAL

}

FeatureSetDownlink-v1610 ::= SEQUENCE {

-- R1 22-4e/4f/4g/4h: CBG based reception for DL with unicast PDSCH(s) per slot per CC with UE processing time Capability 1

cbgPDSCH-ProcessingType1-DifferentTB-PerSlot-r16 SEQUENCE {

scs-15kHz-r16 ENUMERATED {one, upto2, upto4, upto7} OPTIONAL,

scs-30kHz-r16 ENUMERATED {one, upto2, upto4, upto7} OPTIONAL,

scs-60kHz-r16 ENUMERATED {one, upto2, upto4, upto7} OPTIONAL,

scs-120kHz-r16 ENUMERATED {one, upto2, upto4, upto7} OPTIONAL

} OPTIONAL,

-- R1 22-3e/3f/3g/3h: CBG based reception for DL with unicast PDSCH(s) per slot per CC with UE processing time Capability 2

cbgPDSCH-ProcessingType2-DifferentTB-PerSlot-r16 SEQUENCE {

scs-15kHz-r16 ENUMERATED {one, upto2, upto4, upto7} OPTIONAL,

scs-30kHz-r16 ENUMERATED {one, upto2, upto4, upto7} OPTIONAL,

scs-60kHz-r16 ENUMERATED {one, upto2, upto4, upto7} OPTIONAL,

scs-120kHz-r16 ENUMERATED {one, upto2, upto4, upto7} OPTIONAL

} OPTIONAL,

intraFreqDAPS-r16 SEQUENCE {

intraFreqDiffSCS-DAPS-r16 ENUMERATED {supported} OPTIONAL,

intraFreqAsyncDAPS-r16 ENUMERATED {supported} OPTIONAL

} OPTIONAL,

intraBandFreqSeparationDL-v1620 FreqSeparationClassDL-v1620 OPTIONAL,

intraBandFreqSeparationDL-Only-r16 FreqSeparationClassDL-Only-r16 OPTIONAL,

-- R1 11-2: Rel-16 PDCCH monitoring capability

pdcch-Monitoring-r16 SEQUENCE {

pdsch-ProcessingType1-r16 SEQUENCE {

scs-15kHz-r16 PDCCH-MonitoringOccasions-r16 OPTIONAL,

scs-30kHz-r16 PDCCH-MonitoringOccasions-r16 OPTIONAL

} OPTIONAL,

pdsch-ProcessingType2-r16 SEQUENCE {

scs-15kHz-r16 PDCCH-MonitoringOccasions-r16 OPTIONAL,

scs-30kHz-r16 PDCCH-MonitoringOccasions-r16 OPTIONAL

} OPTIONAL

} OPTIONAL,

-- R1 11-2b: Mix of Rel. 16 PDCCH monitoring capability and Rel. 15 PDCCH monitoring capability on different carriers

pdcch-MonitoringMixed-r16 ENUMERATED {supported} OPTIONAL,

-- R1 18-5c: Processing up to X unicast DCI scheduling for DL per scheduled CC

crossCarrierSchedulingProcessing-DiffSCS-r16 SEQUENCE {

scs-15kHz-120kHz-r16 ENUMERATED {n1,n2,n4} OPTIONAL,

scs-15kHz-60kHz-r16 ENUMERATED {n1,n2,n4} OPTIONAL,

scs-30kHz-120kHz-r16 ENUMERATED {n1,n2,n4} OPTIONAL,

scs-15kHz-30kHz-r16 ENUMERATED {n2} OPTIONAL,

scs-30kHz-60kHz-r16 ENUMERATED {n2} OPTIONAL,

scs-60kHz-120kHz-r16 ENUMERATED {n2} OPTIONAL

} OPTIONAL,

-- R1 16-2b-1: Support of single-DCI based SDM scheme

singleDCI-SDM-scheme-r16 ENUMERATED {supported} OPTIONAL

}

FeatureSetDownlink-v16k0 ::= SEQUENCE {

-- R1 22-8: For SRS for CB PUSCH and antenna switching on FR1 with symbol level offset for aperiodic SRS transmission

offsetSRS-CB-PUSCH-Ant-Switch-fr1-r16 ENUMERATED {supported} OPTIONAL,

-- R1 22-8a: PDCCH monitoring on any span of up to 3 consecutive OFDM symbols of a slot and constrained timeline for SRS for CB

-- PUSCH and antenna switching on FR1

offsetSRS-CB-PUSCH-PDCCH-MonitorSingleOcc-fr1-r16 ENUMERATED {supported} OPTIONAL,

-- R1 22-8b: For type 1 CSS with dedicated RRC configuration, type 3 CSS, and UE-SS, monitoring occasion can be any OFDM symbol(s)

-- of a slot for Case 2 and constrained timeline for SRS for CB PUSCH and antenna switching on FR1

offsetSRS-CB-PUSCH-PDCCH-MonitorAnyOccWithoutGap-fr1-r16 ENUMERATED {supported} OPTIONAL,

-- R1 22-8c: For type 1 CSS with dedicated RRC configuration, type 3 CSS, and UE-SS, monitoring occasion can be any OFDM symbol(s)

-- of a slot for Case 2 with a DCI gap and constrained timeline for SRS for CB PUSCH and antenna switching on FR1

offsetSRS-CB-PUSCH-PDCCH-MonitorAnyOccWithGap-fr1-r16 ENUMERATED {supported} OPTIONAL,

-- R1 22-8d: All PDCCH monitoring occasion can be any OFDM symbol(s) of a slot for Case 2 with a span gap and constrained timeline

-- for SRS for CB PUSCH and antenna switching on FR1

offsetSRS-CB-PUSCH-PDCCH-MonitorAnyOccWithSpanGap-fr1-r16 SEQUENCE {

scs-15kHz-r16 ENUMERATED {set1, set2, set3} OPTIONAL,

scs-30kHz-r16 ENUMERATED {set1, set2, set3} OPTIONAL,

scs-60kHz-r16 ENUMERATED {set1, set2, set3} OPTIONAL

} OPTIONAL

}

FeatureSetDownlink-v1700 ::= SEQUENCE {

-- R1 36-2: Scaling factor to be applied to 1024QAM for FR1

scalingFactor-1024QAM-FR1-r17 ENUMERATED {f0p4, f0p75, f0p8} OPTIONAL,

-- R1 24 feature for existing UE cap to include new SCS

timeDurationForQCL-v1710 SEQUENCE {

scs-480kHz ENUMERATED {s56, s112} OPTIONAL,

scs-960kHz ENUMERATED {s112, s224} OPTIONAL

} OPTIONAL,

-- R1 23-6-1 SFN scheme A (scheme 1) for PDSCH and PDCCH

sfn-SchemeA-r17 ENUMERATED {supported} OPTIONAL,

-- R1 23-6-1-1 SFN scheme A (scheme 1) for PDCCH only

sfn-SchemeA-PDCCH-only-r17 ENUMERATED {supported} OPTIONAL,

-- R1 23-6-1a Dynamic switching - scheme A

sfn-SchemeA-DynamicSwitching-r17 ENUMERATED {supported} OPTIONAL,

-- R1 23-6-1b SFN scheme A (scheme 1) for PDSCH only

sfn-SchemeA-PDSCH-only-r17 ENUMERATED {supported} OPTIONAL,

-- R1 23-6-2 SFN scheme B (TRP based pre-compensation) for PDSCH and PDCCH

sfn-SchemeB-r17 ENUMERATED {supported} OPTIONAL,

-- R1 23-6-2a Dynamic switching - scheme B

sfn-SchemeB-DynamicSwitching-r17 ENUMERATED {supported} OPTIONAL,

-- R1 23-6-2b SFN scheme B (TRP based pre-compensation) for PDSCH only

sfn-SchemeB-PDSCH-only-r17 ENUMERATED {supported} OPTIONAL,

-- R1 23-2-1d PDCCH repetition for Case 2 PDCCH monitoring with a span gap

mTRP-PDCCH-Case2-1SpanGap-r17 SEQUENCE {

scs-15kHz-r17 PDCCH-RepetitionParameters-r17 OPTIONAL,

scs-30kHz-r17 PDCCH-RepetitionParameters-r17 OPTIONAL,

scs-60kHz-r17 PDCCH-RepetitionParameters-r17 OPTIONAL,

scs-120kHz-r17 PDCCH-RepetitionParameters-r17 OPTIONAL

} OPTIONAL,

-- R1 23-2-1e PDCCH repetition for Rel-16 PDCCH monitoring

mTRP-PDCCH-legacyMonitoring-r17 SEQUENCE {

scs-15kHz-r17 PDCCH-RepetitionParameters-r17 OPTIONAL,

scs-30kHz-r17 PDCCH-RepetitionParameters-r17 OPTIONAL

} OPTIONAL,

-- R1 23-2-4 Simultaneous configuration of PDCCH repetition and multi-DCI based multi-TRP

mTRP-PDCCH-multiDCI-multiTRP-r17 ENUMERATED {supported} OPTIONAL,

-- R1 33-2: Dynamic scheduling for multicast for PCell

dynamicMulticastPCell-r17 ENUMERATED {supported} OPTIONAL,

-- R1 23-2-1 PDCCH repetition

mTRP-PDCCH-Repetition-r17 SEQUENCE {

numBD-twoPDCCH-r17 INTEGER (2..3),

maxNumOverlaps-r17 ENUMERATED {n1,n2,n3,n5,n10,n20,n40}

} OPTIONAL

}

FeatureSetDownlink-v1720 ::= SEQUENCE {

-- R1 25-19: RTT-based Propagation delay compensation based on CSI-RS for tracking and SRS

rtt-BasedPDC-CSI-RS-ForTracking-r17 ENUMERATED {supported} OPTIONAL,

-- R1 25-19a: RTT-based Propagation delay compensation based on DL PRS for RTT-based PDC and SRS

rtt-BasedPDC-PRS-r17 SEQUENCE {

maxNumberPRS-Resource-r17 ENUMERATED {n1, n2, n4, n8, n16, n32, n64},

maxNumberPRS-ResourceProcessedPerSlot-r17 SEQUENCE {

scs-15kHz-r17 ENUMERATED {n1, n2, n4, n6, n8, n12, n16, n24, n32, n48, n64} OPTIONAL,

scs-30kHz-r17 ENUMERATED {n1, n2, n4, n6, n8, n12, n16, n24, n32, n48, n64} OPTIONAL,

scs-60kHz-r17 ENUMERATED {n1, n2, n4, n6, n8, n12, n16, n24, n32, n48, n64} OPTIONAL,

scs-120kHz-r17 ENUMERATED {n1, n2, n4, n6, n8, n12, n16, n24, n32, n48, n64} OPTIONAL

}

} OPTIONAL,

-- R1 33-5-1: SPS group-common PDSCH for multicast on PCell

sps-Multicast-r17 ENUMERATED {supported} OPTIONAL

}

FeatureSetDownlink-v1730 ::= SEQUENCE {

-- R1 25-19b: Support of PRS as spatial relation RS for SRS

prs-AsSpatialRelationRS-For-SRS-r17 ENUMERATED {supported} OPTIONAL

}

FeatureSetDownlink-v17d0 ::= SEQUENCE {

-- R1 23-8-4 Maximum 2 SP and 1 periodic SRS sets for antenna switching

srs-AntennaSwitching2SP-1Periodic-r17 ENUMERATED {supported} OPTIONAL,

-- R1 23-8-9 Extension of aperiodic SRS configuration for 1T4R, 1T2R and 2T4R

srs-ExtensionAperiodicSRS-r17 ENUMERATED {supported} OPTIONAL,

-- R1 23-8-10 1 aperiodic SRS resource set for 1T4R

srs-OneAP-SRS-r17 ENUMERATED {supported} OPTIONAL

}

FeatureSetDownlink-v1800 ::= SEQUENCE {

-- R1 40-1-14a: Dynamic switching - scheme A

dynamicSwitchingA-r18 ENUMERATED {supported} OPTIONAL,

-- R1 40-1-14b: Dynamic switching - scheme B

dynamicSwitchingB-r18 ENUMERATED {supported} OPTIONAL,

-- R1 40-3-2-11: Aperiodic CSI report timing relaxation for doppler codebook based on Type-II codebook

aperiodicCSI-TimeRelaxation-r18 SEQUENCE {

valueW-r18 SEQUENCE{

scs-15kHz ENUMERATED {value1, value2} OPTIONAL,

scs-30kHz ENUMERATED {value1, value2} OPTIONAL,

scs-60kHz ENUMERATED {value1, value2} OPTIONAL,

scs-120kHz ENUMERATED {value1, value2} OPTIONAL

},

timeRelaxation-r18 ENUMERATED {cap1, cap2}

} OPTIONAL,

-- R1 40-4-1: Basic feature of Rel.18 enhanced DMRS ports for PDSCH for scheduling of mapping type A

pdsch-TypeA-DMRS-r18 ENUMERATED {supported} OPTIONAL,

-- R1 40-4-1a: Basic feature of Rel.18 enhanced DMRS ports for PDSCH for scheduling of mapping type B

pdsch-TypeB-DMRS-r18 ENUMERATED {supported} OPTIONAL,

-- R1 40-4-1b: 1 symbol FL DMRS and 2 additional DMRS symbols for more than one port for Rel.18 enhanced DMRS ports for PDSCH

pdsch-1SymbolFL-DMRS-Addition2Symbol-r18 ENUMERATED {supported} OPTIONAL,

-- R1 40-4-1c: Alternative additional DMRS position for co-existence with LTE CRS for Rel.18 enhanced DMRS ports for PDSCH

pdsch-AlternativeDMRS-Coexistence-r18 ENUMERATED {supported} OPTIONAL,

-- R1 40-4-1d: 2 symbols FL-DMRS for Rel.18 enhanced DMRS ports for PDSCH

pdsch-2SymbolFL-DMRS-r18 ENUMERATED {supported} OPTIONAL,

-- R1 40-4-1e: 2-symbol FL DMRS + one additional 2-symbols DMRS for Rel.18 enhanced DMRS ports for PDSCH

pdsch-2SymbolFL-DMRS-Addition2Symbol-r18 ENUMERATED {supported} OPTIONAL,

-- R1 40-4-1f: 1 symbol FL DMRS and 3 additional DMRS symbols for Rel.18 enhanced DMRS ports for PDSCH

pdsch-1SymbolFL-DMRS-Addition3Symbol-r18 ENUMERATED {supported} OPTIONAL,

-- R1 40-4-1g: DMRS type for Rel.18 enhanced DMRS ports for PDSCH

pdsch-DMRS-Type-r18 ENUMERATED {etype1, etype1And2} OPTIONAL,

-- R1 40-4-1h: 1 port DL PTRS for Rel.18 enhanced DMRS ports for PDSCH with rank 1-8

pdsch-1PortDL-PTRS-r18 ENUMERATED {supported} OPTIONAL,

-- R1 40-4-1i: 2 port DL PTRS for Rel.18 enhanced DMRS ports for PDSCH with rank 1-8

pdsch-2PortDL-PTRS-r18 ENUMERATED {supported} OPTIONAL,

-- R1 40-4-1j: Support 1 symbol FL DMRS and 2 additional DMRS symbols for one port for scheduling of mapping type A

mappingTypeA-1SymbolFL-DMRS-Addition2Symbol-r18 ENUMERATED {supported} OPTIONAL,

-- R1 40-4-2: Capability on the maximum number of configured DMRS types for PDSCH across all DL DCI formats per cell

maxNumberDMRS-AcrossAllDL-DCI-r18 INTEGER (2..4) OPTIONAL,

-- R1 40-4-4: Reception of PDSCH without the scheduling restriction for Rel.18 eType1 DMRS ports

pdsch-ReceptionWithoutSchedulingRestriction-r18 ENUMERATED {supported} OPTIONAL,

-- R1 40-4-4a: Reception of PDSCH without the scheduling restriction for Rel.18 eType1 DMRS ports for PDSCH with fdmSchemeA

pdsch-ReceptionSchemeA-r18 ENUMERATED {supported} OPTIONAL,

-- R1 40-4-4b: Reception of PDSCH without the scheduling restriction for Rel.18 eType1 DMRS ports for PDSCH with fdmSchemeB

pdsch-ReceptionSchemeB-r18 ENUMERATED {supported} OPTIONAL,

-- R1 40-4-5: Rel-18 DL DMRS with single DCI based M-TRP

dmrs-MultiTRP-SingleDCI-r18 ENUMERATED {supported} OPTIONAL,

-- R1 40-4-5a: Additional row(s) for antenna ports (0,2,3) for Rel.18 DL DMRS ports for single-DCI based M-TRP

dmrs-MultiTRP-AdditionRows-r18 ENUMERATED {supported} OPTIONAL,

-- R1 40-4-7: Rel-18 DL DMRS with M-DCI based M-TRP

dmrs-MultiTRP-MultiDCI-r18 ENUMERATED {supported} OPTIONAL,

-- R1 40-4-12: Support of Rel-18 DMRS and PDSCH processing capability 2 simultaneously

simulDMRS-PDSCH-r18 SEQUENCE {

scs-15kHz-r18 INTEGER (0..4) OPTIONAL,

scs-30kHz-r18 INTEGER (0..5) OPTIONAL,

scs-60kHz-r18 INTEGER (0..7) OPTIONAL

} OPTIONAL,

-- R1 53-1: Support RLM/BM/BFD and gapless L3 intra-frequency measurements based on CD-SSB outside active BWP without interruptions

bwpOperationMeasWithoutInterrupt-r18 ENUMERATED {supported} OPTIONAL,

-- R1 55-6: (2, 2) span-based PDCCH monitoring with additional restriction(s)

pdcch-MonitoringSpan2-2-r18 SEQUENCE{

pdsch-ProcessingType1-r18 SEQUENCE{

scs-15kHz-r18 ENUMERATED {supported} OPTIONAL,

scs-30kHz-r18 ENUMERATED {supported} OPTIONAL

},

pdsch-ProcessingType2-r18 SEQUENCE{

scs-15kHz-r18 ENUMERATED {supported} OPTIONAL,

scs-30kHz-r18 ENUMERATED {supported} OPTIONAL

}

} OPTIONAL,

-- R1 55-6b: Mix of Rel-16 PDCCH monitoring capability and Rel. 15 PDCCH monitoring capability on different carriers

pdcch-MonitoringMixed-r18 ENUMERATED {supported} OPTIONAL,

-- R1 55-6h: PDCCH repetition for Rel-16 PDCCH monitoring

mTRP-PDCCH-legacyMonitoring-r18 SEQUENCE {

scs-15kHz-r18 PDCCH-RepetitionParameters-r17 OPTIONAL,

scs-30kHz-r18 PDCCH-RepetitionParameters-r17 OPTIONAL

} OPTIONAL,

-- R4 42-1: Support of SCell without SS/PBCH block for inter-band CA

scellWithoutSSB-InterBandCA-r18 CHOICE {

supportOfSingleGroup ENUMERATED {referenceBand, scellWithoutSSB, both},

supportOfMultipleGroups ENUMERATED {referenceBand1, scellWithoutSSB1, referenceBand2, scellWithoutSSB2}

} OPTIONAL,

dummy SEQUENCE (SIZE (1..maxBandsMRDC)) OF Dummy-PDCCH-RACH-DL-Info-r18 OPTIONAL

}

FeatureSetDownlink-v1830 ::= SEQUENCE {

-- R4 39-4: Interruption on DL slot(s) due to PDCCH- ordered RACH transmission

pdcch-RACH-AffectedBands-TargetBandList-r18 SEQUENCE (SIZE (1..maxBandsMRDC)) OF ENUMERATED {noInterruption, interruption}

OPTIONAL,

-- R4 39-4a: Interruption due to RF retuning for PDCCH- ordered RACH

pdcch-RACH-SwitchingTime-TargetBandList-r18 SEQUENCE (SIZE (1..maxBandsMRDC)) OF ENUMERATED {ms0, ms0dot25, ms0dot5, ms1, ms2, notSupported}

OPTIONAL,

-- R4 39-5: the RF/BB preparation time for PDCCH ordered RACH of which the resources are not fully contained

-- in any of UE's configured UL BWP(s) of active serving cells

pdcch-RACH-PrepTime-TargetBandList-r18 SEQUENCE (SIZE (1..maxBandsMRDC)) OF ENUMERATED {ms1, ms3, ms5, ms10, notSupported}

OPTIONAL

}

FeatureSetDownlink-v1860 ::= SEQUENCE {

-- R1 40-5-5: Maximum 2 SP and 1 periodic SRS sets for 8T8R antenna switching

srs-AntennaSwitching8T8R2SP-1Periodic-r18 ENUMERATED {supported} OPTIONAL

}

FeatureSetDownlink-v1900 ::= SEQUENCE {

-- R1 59-4-4a: Support two TAs enhancement for intra-cell beam management

twoTA-IntraCellBM-r19 ENUMERATED {supported} OPTIONAL,

-- R1 59-4-4b: Support two TAs enhancement for inter-cell beam management operation

twoTA-InterCellBM-r19 ENUMERATED {supported} OPTIONAL,

-- R1 59-4-4d: PDCCH ordered sent by one TRP triggers RACH procedure towards a different TRP based on CRFA for inter-cell

-- without CORESETPoolIndex

interCellCRFA-r19 ENUMERATED {supported} OPTIONAL,

-- R1 59-3-3-1: Maximum 2 SP and 1 periodic SRS sets for 3T6R antenna switching

srs-AntennaSwitching3T6R2SP-1Periodic-r19 ENUMERATED {supported} OPTIONAL,

-- R1 59-3-3a-1: Maximum 2 SP and 1 periodic SRS sets for 3T3R antenna switching

srs-AntennaSwitching3T3R2SP-1Periodic-r19 ENUMERATED {supported} OPTIONAL

}

PDCCH-MonitoringOccasions-r16 ::= SEQUENCE {

period7span3-r16 ENUMERATED {supported} OPTIONAL,

period4span3-r16 ENUMERATED {supported} OPTIONAL,

period2span2-r16 ENUMERATED {supported} OPTIONAL

}

PDCCH-RepetitionParameters-r17 ::= SEQUENCE {

supportedMode-r17 ENUMERATED {intra-span, inter-span, both},

limitX-PerCC-r17 ENUMERATED {n4, n8, n16, n32, n44, n64, nolimit} OPTIONAL,

limitX-AcrossCC-r17 ENUMERATED {n4, n8, n16, n32, n44, n64, n128, n256, n512, nolimit} OPTIONAL

}

DummyA ::= SEQUENCE {

maxNumberNZP-CSI-RS-PerCC INTEGER (1..32),

maxNumberPortsAcrossNZP-CSI-RS-PerCC ENUMERATED {p2, p4, p8, p12, p16, p24, p32, p40, p48, p56, p64, p72, p80,

p88, p96, p104, p112, p120, p128, p136, p144, p152, p160, p168,

p176, p184, p192, p200, p208, p216, p224, p232, p240, p248, p256},

maxNumberCS-IM-PerCC ENUMERATED {n1, n2, n4, n8, n16, n32},

maxNumberSimultaneousCSI-RS-ActBWP-AllCC ENUMERATED {n5, n6, n7, n8, n9, n10, n12, n14, n16, n18, n20, n22, n24, n26,

n28, n30, n32, n34, n36, n38, n40, n42, n44, n46, n48, n50, n52,

n54, n56, n58, n60, n62, n64},

totalNumberPortsSimultaneousCSI-RS-ActBWP-AllCC ENUMERATED {p8, p12, p16, p24, p32, p40, p48, p56, p64, p72, p80,

p88, p96, p104, p112, p120, p128, p136, p144, p152, p160, p168,

p176, p184, p192, p200, p208, p216, p224, p232, p240, p248, p256}

}

DummyB ::= SEQUENCE {

maxNumberTxPortsPerResource ENUMERATED {p2, p4, p8, p12, p16, p24, p32},

maxNumberResources INTEGER (1..64),

totalNumberTxPorts INTEGER (2..256),

supportedCodebookMode ENUMERATED {mode1, mode1AndMode2},

maxNumberCSI-RS-PerResourceSet INTEGER (1..8)

}

DummyC ::= SEQUENCE {

maxNumberTxPortsPerResource ENUMERATED {p8, p16, p32},

maxNumberResources INTEGER (1..64),

totalNumberTxPorts INTEGER (2..256),

supportedCodebookMode ENUMERATED {mode1, mode2, both},

supportedNumberPanels ENUMERATED {n2, n4},

maxNumberCSI-RS-PerResourceSet INTEGER (1..8)

}

DummyD ::= SEQUENCE {

maxNumberTxPortsPerResource ENUMERATED {p4, p8, p12, p16, p24, p32},

maxNumberResources INTEGER (1..64),

totalNumberTxPorts INTEGER (2..256),

parameterLx INTEGER (2..4),

amplitudeScalingType ENUMERATED {wideband, widebandAndSubband},

amplitudeSubsetRestriction ENUMERATED {supported} OPTIONAL,

maxNumberCSI-RS-PerResourceSet INTEGER (1..8)

}

DummyE ::= SEQUENCE {

maxNumberTxPortsPerResource ENUMERATED {p4, p8, p12, p16, p24, p32},

maxNumberResources INTEGER (1..64),

totalNumberTxPorts INTEGER (2..256),

parameterLx INTEGER (2..4),

amplitudeScalingType ENUMERATED {wideband, widebandAndSubband},

maxNumberCSI-RS-PerResourceSet INTEGER (1..8)

}

Dummy-PDCCH-RACH-DL-Info-r18 ::= CHOICE {

notSupported NULL,

supported SEQUENCE {

-- R4 39-4: Interruption on DL slot(s) due to PDCCH- ordered RACH transmission

pdcch-RACH-AffectedBands-r18 ENUMERATED {noIntrruption, interruption},

-- R4 39-4a: Interruption on DL slot(s) due to PDCCH- ordered RACH transmission

pdcch-RACH-SwitchingTimeList-r18 ENUMERATED {ms0, ms0dot25, ms0dot5 , ms1, ms2} OPTIONAL,

-- R4 39-5: the RF/BB preparation time for PDCCH ordered RACH of which the resources are not fully contained

-- in any of UE's configured UL BWP(s) of active serving cells

pdcch-RACH-PrepTime-r18 ENUMERATED {ms1, ms3, ms5, ms10} OPTIONAL

}

}

-- TAG-FEATURESETDOWNLINK-STOP

-- ASN1STOP

|  |
| --- |
| *FeatureSetDownlink* field descriptions |
| ***featureSetListPerDownlinkCC***  Indicates which features the UE supports on the individual DL carriers of the feature set (and hence of a band entry that refer to the feature set). The UE shall hence include at least as many *FeatureSetDownlinkPerCC-Id* in this list as the number of carriers it supports according to the *ca-BandwidthClassDL*, except if indicating additional functionality by reducing the number of *FeatureSetDownlinkPerCC-Id* in the feature set (see NOTE 1 in *FeatureSetCombination* IE description). The order of the elements in this list is not relevant, i.e., the network may configure any of the carriers in accordance with any of the *FeatureSetDownlinkPerCC-Id* in this list. |
| ***supportedSRS-Resources***  Indicates supported SRS resources for SRS carrier switching to the band associated with this *FeatureSetDownlink*. The UE is only allowed to set this field for a band with associated *FeatureSetUplinkId* set to 0. |

#### – *FeatureSetDownlinkId*

The IE *FeatureSetDownlinkId* identifies a downlink feature set. The *FeatureSetDownlinkId* of a *FeatureSetDownlink* is the index position of the *FeatureSetDownlink* in the *featureSetsDownlink* list in the *FeatureSets* IE. The first element in that list is referred to by *FeatureSetDownlinkId* = 1. The *FeatureSetDownlinkId=0* is not used by an actual *FeatureSetDownlink* but means that the UE does not support a carrier in this band of a band combination.

*FeatureSetDownlinkId* information element

-- ASN1START

-- TAG-FEATURESETDOWNLINKID-START

FeatureSetDownlinkId ::= INTEGER (0..maxDownlinkFeatureSets)

-- TAG-FEATURESETDOWNLINKID-STOP

-- ASN1STOP

#### – *FeatureSetDownlinkPerCC*

The IE *FeatureSetDownlinkPerCC* indicates a set of features that the UE supports on the corresponding carrier of one band entry of a band combination.

*FeatureSetDownlinkPerCC* information element

-- ASN1START

-- TAG-FEATURESETDOWNLINKPERCC-START

FeatureSetDownlinkPerCC ::= SEQUENCE {

supportedSubcarrierSpacingDL SubcarrierSpacing,

supportedBandwidthDL SupportedBandwidth,

channelBW-90mhz ENUMERATED {supported} OPTIONAL,

maxNumberMIMO-LayersPDSCH MIMO-LayersDL OPTIONAL,

supportedModulationOrderDL ModulationOrder OPTIONAL

}

FeatureSetDownlinkPerCC-v1620 ::= SEQUENCE {

-- R1 16-2a: Mulit-DCI based multi-TRP

multiDCI-MultiTRP-r16 MultiDCI-MultiTRP-r16 OPTIONAL,

-- R1 16-2b-3: Support of single-DCI based FDMSchemeB

supportFDM-SchemeB-r16 ENUMERATED {supported} OPTIONAL

}

FeatureSetDownlinkPerCC-v1700 ::= SEQUENCE {

supportedMinBandwidthDL-r17 SupportedBandwidth-v1700 OPTIONAL,

broadcastSCell-r17 ENUMERATED {supported} OPTIONAL,

-- R1 33-2g: MIMO layers for multicast PDSCH

maxNumberMIMO-LayersMulticastPDSCH-r17 ENUMERATED {n2, n4, n8} OPTIONAL,

-- R1 33-2h: Dynamic scheduling for multicast for SCell

dynamicMulticastSCell-r17 ENUMERATED {supported} OPTIONAL,

supportedBandwidthDL-v1710 SupportedBandwidth-v1700 OPTIONAL,

-- R4 24-1/24-2/24-3/24-4/24-5

supportedCRS-InterfMitigation-r17 CRS-InterfMitigation-r17 OPTIONAL

}

FeatureSetDownlinkPerCC-v1720 ::= SEQUENCE {

-- R1 33-2j: Supported maximum modulation order used for maximum data rate calculation for multicast PDSCH

maxModulationOrderForMulticastDataRateCalculation-r17 ENUMERATED {qam64, qam256, qam1024} OPTIONAL,

-- R1 33-1-2: FDM-ed unicast PDSCH and group-common PDSCH for broadcast

fdm-BroadcastUnicast-r17 ENUMERATED {supported} OPTIONAL,

-- R1 33-3-2: FDM-ed unicast PDSCH and one group-common PDSCH for multicast

fdm-MulticastUnicast-r17 ENUMERATED {supported} OPTIONAL

}

FeatureSetDownlinkPerCC-v1730 ::= SEQUENCE {

-- R1 33-3-3: Intra-slot TDM-ed unicast PDSCH and group-common PDSCH

intraSlotTDM-UnicastGroupCommonPDSCH-r17 ENUMERATED {yes, no} OPTIONAL,

-- R1 33-5-3: One SPS group-common PDSCH configuration for multicast for SCell

sps-MulticastSCell-r17 ENUMERATED {supported} OPTIONAL,

-- R1 33-5-4: Up to 8 SPS group-common PDSCH configurations per CFR for multicast for SCell

sps-MulticastSCellMultiConfig-r17 INTEGER (1..8) OPTIONAL,

-- R1 33-1-1: Dynamic slot-level repetition for broadcast MTCH

dci-BroadcastWith16Repetitions-r17 ENUMERATED {supported} OPTIONAL

}

FeatureSetDownlinkPerCC-v1780 ::= SEQUENCE {

supportedBandwidthDL-v1780 SupportedBandwidth-v1700 OPTIONAL

}

FeatureSetDownlinkPerCC-v1800 ::= SEQUENCE {

-- R1 40-2-1: Basic feature for multi-DCI based intra-cell Multi-TRP operation with two TA enhancement

multiDCI-IntraCellMultiTRP-TwoTA-r18 ENUMERATED {supported} OPTIONAL,

-- R1 40-2-2: Basic feature for multi-DCI based inter-cell Multi-TRP operation with two TA enhancement

multiDCI-InterCellMultiTRP-TwoTA-r18 INTEGER (1..2) OPTIONAL,

-- R1 40-2-6: Rx timing difference larger than CP length

rxTimingDiff-r18 ENUMERATED {supported} OPTIONAL,

-- R1 55-7: Two QCL TypeD for CORESET monitoring in multi-DCI based multi-TRP

multiDCI-MultiTRP-CORESET-Monitoring-r18 ENUMERATED {supported} OPTIONAL,

broadcastNonServingCell-r18 ENUMERATED {supported} OPTIONAL,

-- R4 30-1: Supports scheduling restriction relaxation and measurement restriction relaxation

schedulingMeasurementRelaxation-r18 ENUMERATED {supported} OPTIONAL

}

FeatureSetDownlinkPerCC-v1840 ::= SEQUENCE {

supportedBandwidthDL-v1840 SupportedBandwidth-v1840 OPTIONAL,

supportedMinBandwidthDL-v1840 SupportedBandwidth-v1840 OPTIONAL

}

FeatureSetDownlinkPerCC-v1900 ::= SEQUENCE {

-- R1 67-1: 32 DL HARQ processes for TN in FR1 and FR2-1

support32-DL-HARQ-ProcessTN-r19 ENUMERATED {supported} OPTIONAL

}

MultiDCI-MultiTRP-r16 ::= SEQUENCE {

maxNumberCORESET-r16 ENUMERATED {n2, n3, n4, n5},

maxNumberCORESETPerPoolIndex-r16 INTEGER (1..3),

maxNumberUnicastPDSCH-PerPool-r16 ENUMERATED {n1, n2, n3, n4, n7}

}

CRS-InterfMitigation-r17 ::= SEQUENCE {

-- R4 24-1 CRS-IM (Interference Mitigation) in DSS scenario

crs-IM-DSS-15kHzSCS-r17 ENUMERATED {supported} OPTIONAL,

-- R4 24-2 CRS-IM in non-DSS and 15 kHz NR SCS scenario, without the assistance of network signaling on LTE channel bandwidth

crs-IM-nonDSS-15kHzSCS-r17 ENUMERATED {supported} OPTIONAL,

-- R4 24-3 CRS-IM in non-DSS and 15 kHz NR SCS scenario, with the assistance of network signaling on LTE channel bandwidth

crs-IM-nonDSS-NWA-15kHzSCS-r17 ENUMERATED {supported} OPTIONAL,

-- R4 24-4 CRS-IM in non-DSS and 30 kHz NR SCS scenario, without the assistance of network signaling on LTE channel bandwidth

crs-IM-nonDSS-30kHzSCS-r17 ENUMERATED {supported} OPTIONAL,

-- R4 24-5 CRS-IM in non-DSS and 30 kHz NR SCS scenario, with the assistance of network signaling on LTE channel bandwidth

crs-IM-nonDSS-NWA-30kHzSCS-r17 ENUMERATED {supported} OPTIONAL

}

-- TAG-FEATURESETDOWNLINKPERCC-STOP

-- ASN1STOP

#### – *FeatureSetDownlinkPerCC-Id*

The IE *FeatureSetDownlinkPerCC-Id* identifies a set of features applicable to one carrier of a feature set. The *FeatureSetDownlinkPerCC-Id* of a *FeatureSetDownlinkPerCC* is the index position of the *FeatureSetDownlinkPerCC* in the *featureSetsDownlinkPerCC*. The first element in the list is referred to by *FeatureSetDownlinkPerCC-Id* = 1, and so on.

*FeatureSetDownlinkPerCC-Id* information element

-- ASN1START

-- TAG-FEATURESETDOWNLINKPERCC-ID-START

FeatureSetDownlinkPerCC-Id ::= INTEGER (1..maxPerCC-FeatureSets)

-- TAG-FEATURESETDOWNLINKPERCC-ID-STOP

-- ASN1STOP

#### – *FeatureSetEUTRA-DownlinkId*

The IE *FeatureSetEUTRA-DownlinkId* identifies a downlink feature set in E-UTRA list (see TS 36.331 [10]. The first element in that list is referred to by *FeatureSetEUTRA-DownlinkId* = 1. The *FeatureSetEUTRA-DownlinkId=0* is used when the UE does not support a carrier in this band of a band combination.

*FeatureSetEUTRA-DownlinkId* information element

-- ASN1START

-- TAG-FEATURESETEUTRADOWNLINKID-START

FeatureSetEUTRA-DownlinkId ::= INTEGER (0..maxEUTRA-DL-FeatureSets)

-- TAG-FEATURESETEUTRADOWNLINKID-STOP

-- ASN1STOP

#### – *FeatureSetEUTRA-UplinkId*

The IE *FeatureSetEUTRA-UplinkId* identifies an uplink feature set in E-UTRA list (see TS 36.331 [10]. The first element in that list is referred to by *FeatureSetEUTRA-UplinkId* = 1. The *FeatureSetEUTRA-UplinkId* *=0* is used when the UE does not support a carrier in this band of a band combination.

*FeatureSetEUTRA-UplinkId* information element

-- ASN1START

-- TAG-FEATURESETEUTRAUPLINKID-START

FeatureSetEUTRA-UplinkId ::= INTEGER (0..maxEUTRA-UL-FeatureSets)

-- TAG-FEATURESETEUTRAUPLINKID-STOP

-- ASN1STOP

#### – *FeatureSets*

The IE *FeatureSets* is used to provide pools of downlink and uplink features sets. A *FeatureSetCombination* refers to the IDs of the feature set(s) that the UE supports in that *FeatureSetCombination*. The *BandCombination* entries in the *BandCombinationList* then indicate the ID of the *FeatureSetCombination* that the UE supports for that band combination.

The entries in the lists in this IE are identified by their index position. For example, the *FeatureSetUplinkPerCC-Id* = 4 identifies the 4th element in the *featureSetsUplinkPerCC* list.

NOTE: When feature sets (per CC) IEs require extension in future versions of the specification, new versions of the *FeatureSetDownlink*, *FeatureSetUplink*, *FeatureSets*, *FeatureSetDownlinkPerCC* and/or *FeatureSetUplinkPerCC* will be created and instantiated in corresponding new lists in the *FeatureSets* IE. For example, if new capability bits are to be added to the *FeatureSetDownlink*, they will instead be defined in a new *FeatureSetDownlink-rxy* which will be instantiated in a new *featureSetDownlinkList-rxy* list. If a UE indicates in a *FeatureSetCombination* that it supports the *FeatureSetDownlink* with ID #5, it implies that it supports both the features in *FeatureSetDownlink* #5 and *FeatureSetDownlink-rxy* #5 (if present). The number of entries in the new list(s) shall be the same as in the original list(s).

*FeatureSets* information element

-- ASN1START

-- TAG-FEATURESETS-START

FeatureSets ::= SEQUENCE {

featureSetsDownlink SEQUENCE (SIZE (1..maxDownlinkFeatureSets)) OF FeatureSetDownlink OPTIONAL,

featureSetsDownlinkPerCC SEQUENCE (SIZE (1..maxPerCC-FeatureSets)) OF FeatureSetDownlinkPerCC OPTIONAL,

featureSetsUplink SEQUENCE (SIZE (1..maxUplinkFeatureSets)) OF FeatureSetUplink OPTIONAL,

featureSetsUplinkPerCC SEQUENCE (SIZE (1..maxPerCC-FeatureSets)) OF FeatureSetUplinkPerCC OPTIONAL,

...,

[[

featureSetsDownlink-v1540 SEQUENCE (SIZE (1..maxDownlinkFeatureSets)) OF FeatureSetDownlink-v1540 OPTIONAL,

featureSetsUplink-v1540 SEQUENCE (SIZE (1..maxUplinkFeatureSets)) OF FeatureSetUplink-v1540 OPTIONAL,

featureSetsUplinkPerCC-v1540 SEQUENCE (SIZE (1..maxPerCC-FeatureSets)) OF FeatureSetUplinkPerCC-v1540 OPTIONAL

]],

[[

featureSetsDownlink-v15a0 SEQUENCE (SIZE (1..maxDownlinkFeatureSets)) OF FeatureSetDownlink-v15a0 OPTIONAL

]],

[[

featureSetsDownlink-v1610 SEQUENCE (SIZE (1..maxDownlinkFeatureSets)) OF FeatureSetDownlink-v1610 OPTIONAL,

featureSetsUplink-v1610 SEQUENCE (SIZE (1..maxUplinkFeatureSets)) OF FeatureSetUplink-v1610 OPTIONAL,

featureSetDownlinkPerCC-v1620 SEQUENCE (SIZE (1..maxPerCC-FeatureSets)) OF FeatureSetDownlinkPerCC-v1620 OPTIONAL

]],

[[

featureSetsUplink-v1630 SEQUENCE (SIZE (1..maxUplinkFeatureSets)) OF FeatureSetUplink-v1630 OPTIONAL

]],

[[

featureSetsUplink-v1640 SEQUENCE (SIZE (1..maxUplinkFeatureSets)) OF FeatureSetUplink-v1640 OPTIONAL

]],

[[

featureSetsDownlink-v1700 SEQUENCE (SIZE (1..maxDownlinkFeatureSets)) OF FeatureSetDownlink-v1700 OPTIONAL,

featureSetsDownlinkPerCC-v1700 SEQUENCE (SIZE (1..maxPerCC-FeatureSets)) OF FeatureSetDownlinkPerCC-v1700 OPTIONAL,

featureSetsUplink-v1710 SEQUENCE (SIZE (1..maxUplinkFeatureSets)) OF FeatureSetUplink-v1710 OPTIONAL,

featureSetsUplinkPerCC-v1700 SEQUENCE (SIZE (1..maxPerCC-FeatureSets)) OF FeatureSetUplinkPerCC-v1700 OPTIONAL

]],

[[

featureSetsDownlink-v1720 SEQUENCE (SIZE (1..maxDownlinkFeatureSets)) OF FeatureSetDownlink-v1720 OPTIONAL,

featureSetsDownlinkPerCC-v1720 SEQUENCE (SIZE (1..maxPerCC-FeatureSets)) OF FeatureSetDownlinkPerCC-v1720 OPTIONAL,

featureSetsUplink-v1720 SEQUENCE (SIZE (1..maxUplinkFeatureSets)) OF FeatureSetUplink-v1720 OPTIONAL

]],

[[

featureSetsDownlink-v1730 SEQUENCE (SIZE (1..maxDownlinkFeatureSets)) OF FeatureSetDownlink-v1730 OPTIONAL,

featureSetsDownlinkPerCC-v1730 SEQUENCE (SIZE (1..maxPerCC-FeatureSets)) OF FeatureSetDownlinkPerCC-v1730 OPTIONAL

]],

[[

featureSetsDownlinkPerCC-v1780 SEQUENCE (SIZE (1..maxPerCC-FeatureSets)) OF FeatureSetDownlinkPerCC-v1780 OPTIONAL,

featureSetsUplinkPerCC-v1780 SEQUENCE (SIZE (1..maxPerCC-FeatureSets)) OF FeatureSetUplinkPerCC-v1780 OPTIONAL

]],

[[

featureSetsDownlink-v1800 SEQUENCE (SIZE (1..maxDownlinkFeatureSets)) OF FeatureSetDownlink-v1800 OPTIONAL,

featureSetsDownlinkPerCC-v1800 SEQUENCE (SIZE (1..maxPerCC-FeatureSets)) OF FeatureSetDownlinkPerCC-v1800 OPTIONAL,

featureSetsUplink-v1800 SEQUENCE (SIZE (1..maxUplinkFeatureSets)) OF FeatureSetUplink-v1800 OPTIONAL,

featureSetsUplinkPerCC-v1800 SEQUENCE (SIZE (1..maxPerCC-FeatureSets)) OF FeatureSetUplinkPerCC-v1800 OPTIONAL

]],

[[

featureSetsDownlink-v1830 SEQUENCE (SIZE (1..maxDownlinkFeatureSets)) OF FeatureSetDownlink-v1830 OPTIONAL

]],

[[

featureSetsDownlinkPerCC-v1840 SEQUENCE (SIZE (1..maxPerCC-FeatureSets)) OF FeatureSetDownlinkPerCC-v1840 OPTIONAL,

featureSetsUplinkPerCC-v1840 SEQUENCE (SIZE (1..maxPerCC-FeatureSets)) OF FeatureSetUplinkPerCC-v1840 OPTIONAL

]],

[[

featureSetsUplink-v1850 SEQUENCE (SIZE (1..maxUplinkFeatureSets)) OF FeatureSetUplink-v1850 OPTIONAL,

featureSetsUplinkPerCC-v1850 SEQUENCE (SIZE (1..maxPerCC-FeatureSets)) OF FeatureSetUplinkPerCC-v1850 OPTIONAL

]],

[[

featureSetsDownlink-v1860 SEQUENCE (SIZE (1..maxDownlinkFeatureSets)) OF FeatureSetDownlink-v1860 OPTIONAL

]],

[[

featureSetsDownlink-v1900 SEQUENCE (SIZE (1..maxDownlinkFeatureSets)) OF FeatureSetDownlink-v1900 OPTIONAL,

featureSetsDownlinkPerCC-v1900 SEQUENCE (SIZE (1..maxPerCC-FeatureSets)) OF FeatureSetDownlinkPerCC-v1900 OPTIONAL,

featureSetsUplink-v1900 SEQUENCE (SIZE (1..maxUplinkFeatureSets)) OF FeatureSetUplink-v1900 OPTIONAL,

featureSetsUplinkPerCC-v1900 SEQUENCE (SIZE (1..maxPerCC-FeatureSets)) OF FeatureSetUplinkPerCC-v1900 OPTIONAL

]]

}

FeatureSets-v15t0 ::= SEQUENCE {

featureSetsDownlink-v15t0 SEQUENCE (SIZE (1..maxDownlinkFeatureSets)) OF FeatureSetDownlink-v15t0 OPTIONAL

}

FeatureSets-v16d0 ::= SEQUENCE {

featureSetsUplink-v16d0 SEQUENCE (SIZE (1..maxUplinkFeatureSets)) OF FeatureSetUplink-v16d0 OPTIONAL

}

FeatureSets-v16k0 ::= SEQUENCE {

featureSetsDownlink-v16k0 SEQUENCE (SIZE (1..maxDownlinkFeatureSets)) OF FeatureSetDownlink-v16k0 OPTIONAL

}

FeatureSets-v17d0 ::= SEQUENCE {

featureSetsDownlink-v17d0 SEQUENCE (SIZE (1..maxDownlinkFeatureSets)) OF FeatureSetDownlink-v17d0 OPTIONAL

}

-- TAG-FEATURESETS-STOP

-- ASN1STOP

#### – *FeatureSetUplink*

The IE *FeatureSetUplink* is used to indicate the features that the UE supports on the carriers corresponding to one band entry in a band combination.

*FeatureSetUplink* information element

-- ASN1START

-- TAG-FEATURESETUPLINK-START

FeatureSetUplink ::= SEQUENCE {

featureSetListPerUplinkCC SEQUENCE (SIZE (1.. maxNrofServingCells)) OF FeatureSetUplinkPerCC-Id,

scalingFactor ENUMERATED {f0p4, f0p75, f0p8} OPTIONAL,

dummy3 ENUMERATED {supported} OPTIONAL,

intraBandFreqSeparationUL FreqSeparationClass OPTIONAL,

searchSpaceSharingCA-UL ENUMERATED {supported} OPTIONAL,

dummy1 DummyI OPTIONAL,

supportedSRS-Resources SRS-Resources OPTIONAL,

twoPUCCH-Group ENUMERATED {supported} OPTIONAL,

dynamicSwitchSUL ENUMERATED {supported} OPTIONAL,

simultaneousTxSUL-NonSUL ENUMERATED {supported} OPTIONAL,

pusch-ProcessingType1-DifferentTB-PerSlot SEQUENCE {

scs-15kHz ENUMERATED {upto2, upto4, upto7} OPTIONAL,

scs-30kHz ENUMERATED {upto2, upto4, upto7} OPTIONAL,

scs-60kHz ENUMERATED {upto2, upto4, upto7} OPTIONAL,

scs-120kHz ENUMERATED {upto2, upto4, upto7} OPTIONAL

} OPTIONAL,

dummy2 DummyF OPTIONAL

}

FeatureSetUplink-v1540 ::= SEQUENCE {

zeroSlotOffsetAperiodicSRS ENUMERATED {supported} OPTIONAL,

pa-PhaseDiscontinuityImpacts ENUMERATED {supported} OPTIONAL,

pusch-SeparationWithGap ENUMERATED {supported} OPTIONAL,

pusch-ProcessingType2 SEQUENCE {

scs-15kHz ProcessingParameters OPTIONAL,

scs-30kHz ProcessingParameters OPTIONAL,

scs-60kHz ProcessingParameters OPTIONAL

} OPTIONAL,

ul-MCS-TableAlt-DynamicIndication ENUMERATED {supported} OPTIONAL

}

FeatureSetUplink-v1610 ::= SEQUENCE {

-- R1 11-5: PUsCH repetition Type B

pusch-RepetitionTypeB-r16 SEQUENCE {

maxNumberPUSCH-Tx-r16 ENUMERATED {n2, n3, n4, n7, n8, n12},

hoppingScheme-r16 ENUMERATED {interSlotHopping, interRepetitionHopping, both}

} OPTIONAL,

-- R1 11-7: UL cancelation scheme for self-carrier

ul-CancellationSelfCarrier-r16 ENUMERATED {supported} OPTIONAL,

-- R1 11-7a: UL cancelation scheme for cross-carrier

ul-CancellationCrossCarrier-r16 ENUMERATED {supported} OPTIONAL,

-- R1 16-5c: The maximum number of SRS resources in one SRS resource set with usage set to 'codebook' for Mode 2

ul-FullPwrMode2-MaxSRS-ResInSet-r16 ENUMERATED {n1, n2, n4} OPTIONAL,

-- R1 22-4a/4b/4c/4d: CBG based transmission for UL with unicast PUSCH(s) per slot per CC with UE processing time Capability 1

cbgPUSCH-ProcessingType1-DifferentTB-PerSlot-r16 SEQUENCE {

scs-15kHz-r16 ENUMERATED {one-pusch, upto2, upto4, upto7} OPTIONAL,

scs-30kHz-r16 ENUMERATED {one-pusch, upto2, upto4, upto7} OPTIONAL,

scs-60kHz-r16 ENUMERATED {one-pusch, upto2, upto4, upto7} OPTIONAL,

scs-120kHz-r16 ENUMERATED {one-pusch, upto2, upto4, upto7} OPTIONAL

} OPTIONAL,

-- R1 22-3a/3b/3c/3d: CBG based transmission for UL with unicast PUSCH(s) per slot per CC with UE processing time Capability 2

cbgPUSCH-ProcessingType2-DifferentTB-PerSlot-r16 SEQUENCE {

scs-15kHz-r16 ENUMERATED {one-pusch, upto2, upto4, upto7} OPTIONAL,

scs-30kHz-r16 ENUMERATED {one-pusch, upto2, upto4, upto7} OPTIONAL,

scs-60kHz-r16 ENUMERATED {one-pusch, upto2, upto4, upto7} OPTIONAL,

scs-120kHz-r16 ENUMERATED {one-pusch, upto2, upto4, upto7} OPTIONAL

} OPTIONAL,

supportedSRS-PosResources-r16 SRS-AllPosResources-r16 OPTIONAL,

intraFreqDAPS-UL-r16 SEQUENCE {

dummy ENUMERATED {supported} OPTIONAL,

intraFreqTwoTAGs-DAPS-r16 ENUMERATED {supported} OPTIONAL,

dummy1 ENUMERATED {supported} OPTIONAL,

dummy2 ENUMERATED {supported} OPTIONAL,

dummy3 ENUMERATED {short, long} OPTIONAL

} OPTIONAL,

intraBandFreqSeparationUL-v1620 FreqSeparationClassUL-v1620 OPTIONAL,

-- R1 11-3: More than one PUCCH for HARQ-ACK transmission within a slot

multiPUCCH-r16 SEQUENCE {

sub-SlotConfig-NCP-r16 ENUMERATED {set1, set2} OPTIONAL,

sub-SlotConfig-ECP-r16 ENUMERATED {set1, set2} OPTIONAL

} OPTIONAL,

-- R1 11-3c: 2 PUCCH of format 0 or 2 for a single 7\*2-symbol subslot based HARQ-ACK codebook

twoPUCCH-Type1-r16 ENUMERATED {supported} OPTIONAL,

-- R1 11-3d: 2 PUCCH of format 0 or 2 for a single 2\*7-symbol subslot based HARQ-ACK codebook

twoPUCCH-Type2-r16 ENUMERATED {supported} OPTIONAL,

-- R1 11-3e: 1 PUCCH format 0 or 2 and 1 PUCCH format 1, 3 or 4 in the same subslot for a single 2\*7-symbol HARQ-ACK codebooks

twoPUCCH-Type3-r16 ENUMERATED {supported} OPTIONAL,

-- R1 11-3f: 2 PUCCH transmissions in the same subslot for a single 2\*7-symbol HARQ-ACK codebooks which are not covered by 11-3d and

-- 11-3e

twoPUCCH-Type4-r16 ENUMERATED {supported} OPTIONAL,

-- R1 11-3g: SR/HARQ-ACK multiplexing once per subslot using a PUCCH (or HARQ-ACK piggybacked on a PUSCH) when SR/HARQ-ACK

-- are supposed to be sent with different starting symbols in a subslot

mux-SR-HARQ-ACK-r16 ENUMERATED {supported} OPTIONAL,

dummy1 ENUMERATED {supported} OPTIONAL,

dummy2 ENUMERATED {supported} OPTIONAL,

-- R1 11-4c: 2 PUCCH of format 0 or 2 for two HARQ-ACK codebooks with one 7\*2-symbol sub-slot based HARQ-ACK codebook

twoPUCCH-Type5-r16 ENUMERATED {supported} OPTIONAL,

-- R1 11-4d: 2 PUCCH of format 0 or 2 in consecutive symbols for two HARQ-ACK codebooks with one 2\*7-symbol sub-slot based HARQ-ACK

-- codebook

twoPUCCH-Type6-r16 ENUMERATED {supported} OPTIONAL,

-- R1 11-4e: 2 PUCCH of format 0 or 2 for two subslot based HARQ-ACK codebooks

twoPUCCH-Type7-r16 ENUMERATED {supported} OPTIONAL,

-- R1 11-4f: 1 PUCCH format 0 or 2 and 1 PUCCH format 1, 3 or 4 in the same subslot for HARQ-ACK codebooks with one 2\*7-symbol

-- subslot based HARQ-ACK codebook

twoPUCCH-Type8-r16 ENUMERATED {supported} OPTIONAL,

-- R1 11-4g: 1 PUCCH format 0 or 2 and 1 PUCCH format 1, 3 or 4 in the same subslot for two subslot based HARQ-ACK codebooks

twoPUCCH-Type9-r16 ENUMERATED {supported} OPTIONAL,

-- R1 11-4h: 2 PUCCH transmissions in the same subslot for two HARQ-ACK codebooks with one 2\*7-symbol subslot which are not covered

-- by 11-4c and 11-4e

twoPUCCH-Type10-r16 ENUMERATED {supported} OPTIONAL,

-- R1 11-4i: 2 PUCCH transmissions in the same subslot for two subslot based HARQ-ACK codebooks which are not covered by 11-4d and

-- 11-4f

twoPUCCH-Type11-r16 ENUMERATED {supported} OPTIONAL,

-- R1 12-1: UL intra-UE multiplexing/prioritization of overlapping channel/signals with two priority levels in physical layer

ul-IntraUE-Mux-r16 SEQUENCE {

pusch-PreparationLowPriority-r16 ENUMERATED {sym0, sym1, sym2},

pusch-PreparationHighPriority-r16 ENUMERATED {sym0, sym1, sym2}

} OPTIONAL,

-- R1 16-5a: Supported UL full power transmission mode of fullpower

ul-FullPwrMode-r16 ENUMERATED {supported} OPTIONAL,

-- R1 18-5d: Processing up to X unicast DCI scheduling for UL per scheduled CC

crossCarrierSchedulingProcessing-DiffSCS-r16 SEQUENCE {

scs-15kHz-120kHz-r16 ENUMERATED {n1,n2,n4} OPTIONAL,

scs-15kHz-60kHz-r16 ENUMERATED {n1,n2,n4} OPTIONAL,

scs-30kHz-120kHz-r16 ENUMERATED {n1,n2,n4} OPTIONAL,

scs-15kHz-30kHz-r16 ENUMERATED {n2} OPTIONAL,

scs-30kHz-60kHz-r16 ENUMERATED {n2} OPTIONAL,

scs-60kHz-120kHz-r16 ENUMERATED {n2} OPTIONAL

} OPTIONAL,

-- R1 16-5b: Supported UL full power transmission mode of fullpowerMode1

ul-FullPwrMode1-r16 ENUMERATED {supported} OPTIONAL,

-- R1 16-5c-2: Ports configuration for Mode 2

ul-FullPwrMode2-SRSConfig-diffNumSRSPorts-r16 ENUMERATED {p1-2, p1-4, p1-2-4} OPTIONAL,

-- R1 16-5c-3: TPMI group for Mode 2

ul-FullPwrMode2-TPMIGroup-r16 SEQUENCE {

twoPorts-r16 BIT STRING(SIZE(2)) OPTIONAL,

fourPortsNonCoherent-r16 ENUMERATED{g0, g1, g2, g3} OPTIONAL,

fourPortsPartialCoherent-r16 ENUMERATED{g0, g1, g2, g3, g4, g5, g6} OPTIONAL

} OPTIONAL

}

FeatureSetUplink-v1630 ::= SEQUENCE {

-- R1 22-8: For SRS for CB PUSCH and antenna switching on FR1 with symbol level offset for aperiodic SRS transmission

offsetSRS-CB-PUSCH-Ant-Switch-fr1-r16 ENUMERATED {supported} OPTIONAL,

-- R1 22-8a: PDCCH monitoring on any span of up to 3 consecutive OFDM symbols of a slot and constrained timeline for SRS for CB

-- PUSCH and antenna switching on FR1

offsetSRS-CB-PUSCH-PDCCH-MonitorSingleOcc-fr1-r16 ENUMERATED {supported} OPTIONAL,

-- R1 22-8b: For type 1 CSS with dedicated RRC configuration, type 3 CSS, and UE-SS, monitoring occasion can be any OFDM symbol(s)

-- of a slot for Case 2 and constrained timeline for SRS for CB PUSCH and antenna switching on FR1

offsetSRS-CB-PUSCH-PDCCH-MonitorAnyOccWithoutGap-fr1-r16 ENUMERATED {supported} OPTIONAL,

-- R1 22-8c: For type 1 CSS with dedicated RRC configuration, type 3 CSS, and UE-SS, monitoring occasion can be any OFDM symbol(s)

-- of a slot for Case 2 with a DCI gap and constrained timeline for SRS for CB PUSCH and antenna switching on FR1

offsetSRS-CB-PUSCH-PDCCH-MonitorAnyOccWithGap-fr1-r16 ENUMERATED {supported} OPTIONAL,

dummy ENUMERATED {supported} OPTIONAL,

-- R1 22-9: Cancellation of PUCCH, PUSCH or PRACH with a DCI scheduling a PDSCH or CSI-RS or a DCI format 2\_0 for SFI

partialCancellationPUCCH-PUSCH-PRACH-TX-r16 ENUMERATED {supported} OPTIONAL

}

FeatureSetUplink-v1640 ::= SEQUENCE {

-- R1 11-4: Two HARQ-ACK codebooks with up to one sub-slot based HARQ-ACK codebook (i.e. slot-based + slot-based, or slot-based +

-- sub-slot based) simultaneously constructed for supporting HARQ-ACK codebooks with different priorities at a UE

twoHARQ-ACK-Codebook-type1-r16 SubSlot-Config-r16 OPTIONAL,

-- R1 11-4a: Two sub-slot based HARQ-ACK codebooks simultaneously constructed for supporting HARQ-ACK codebooks with different

-- priorities at a UE

twoHARQ-ACK-Codebook-type2-r16 SubSlot-Config-r16 OPTIONAL,

-- R1 22-8d: All PDCCH monitoring occasion can be any OFDM symbol(s) of a slot for Case 2 with a span gap and constrained timeline

-- for SRS for CB PUSCH and antenna switching on FR1

offsetSRS-CB-PUSCH-PDCCH-MonitorAnyOccWithSpanGap-fr1-r16 SEQUENCE {

scs-15kHz-r16 ENUMERATED {set1, set2, set3} OPTIONAL,

scs-30kHz-r16 ENUMERATED {set1, set2, set3} OPTIONAL,

scs-60kHz-r16 ENUMERATED {set1, set2, set3} OPTIONAL

} OPTIONAL

}

FeatureSetUplink-v16d0 ::= SEQUENCE {

pusch-RepetitionTypeB-v16d0 SEQUENCE {

maxNumberPUSCH-Tx-Cap1-r16 ENUMERATED {n2, n3, n4, n7, n8, n12},

maxNumberPUSCH-Tx-Cap2-r16 ENUMERATED {n2, n3, n4, n7, n8, n12}

} OPTIONAL

}

FeatureSetUplink-v1710 ::= SEQUENCE {

-- R1 23-3-1 Multi-TRP PUSCH repetition (type A) -codebook based

mTRP-PUSCH-TypeA-CB-r17 ENUMERATED {n1,n2,n4} OPTIONAL,

-- R1 23-3-1-2 Multi-TRP PUSCH repetition (type A) - non-codebook based

mTRP-PUSCH-RepetitionTypeA-r17 ENUMERATED {n1,n2,n3,n4} OPTIONAL,

-- R1 23-3-3 Multi-TRP PUCCH repetition-intra-slot

mTRP-PUCCH-IntraSlot-r17 ENUMERATED {pf0-2, pf1-3-4, pf0-4} OPTIONAL,

-- R1 23-8-4 Maximum 2 SP and 1 periodic SRS sets for antenna switching

srs-AntennaSwitching2SP-1Periodic-r17 ENUMERATED {supported} OPTIONAL,

-- R1 23-8-9 Extension of aperiodic SRS configuration for 1T4R, 1T2R and 2T4R

srs-ExtensionAperiodicSRS-r17 ENUMERATED {supported} OPTIONAL,

-- R1 23-8-10 1 aperiodic SRS resource set for 1T4R

srs-OneAP-SRS-r17 ENUMERATED {supported} OPTIONAL,

-- R4 16-8 UE power class per band per band combination

ue-PowerClassPerBandPerBC-r17 ENUMERATED {pc1dot5, pc2, pc3} OPTIONAL,

-- R4 17-8 UL transmission in FR2 bands within an UL gap when the UL gap is activated

tx-Support-UL-GapFR2-r17 ENUMERATED {supported} OPTIONAL

}

FeatureSetUplink-v1720 ::= SEQUENCE {

-- R1 25-3: Repetitions for PUCCH format 0, 1, 2, 3 and 4 over multiple PUCCH subslots with configured K = 2, 4, 8

pucch-Repetition-F0-1-2-3-4-RRC-Config-r17 ENUMERATED {supported} OPTIONAL,

-- R1 25-3a: Repetitions for PUCCH format 0, 1, 2, 3 and 4 over multiple PUCCH subslots using dynamic repetition indication

pucch-Repetition-F0-1-2-3-4-DynamicIndication-r17 ENUMERATED {supported} OPTIONAL,

-- R1 25-3b: Inter-subslot frequency hopping for PUCCH repetitions

interSubslotFreqHopping-PUCCH-r17 ENUMERATED {supported} OPTIONAL,

-- R1 25-8: Semi-static HARQ-ACK codebook for sub-slot PUCCH

semiStaticHARQ-ACK-CodebookSub-SlotPUCCH-r17 ENUMERATED {supported} OPTIONAL,

-- R1 25-14: PHY prioritization of overlapping low-priority DG-PUSCH and high-priority CG-PUSCH

phy-PrioritizationLowPriorityDG-HighPriorityCG-r17 INTEGER(1..16) OPTIONAL,

-- R1 25-15: PHY prioritization of overlapping high-priority DG-PUSCH and low-priority CG-PUSCH

phy-PrioritizationHighPriorityDG-LowPriorityCG-r17 SEQUENCE {

pusch-PreparationLowPriority-r17 ENUMERATED{sym0, sym1, sym2},

additionalCancellationTime-r17 SEQUENCE {

scs-15kHz-r17 ENUMERATED{sym0, sym1, sym2} OPTIONAL,

scs-30kHz-r17 ENUMERATED{sym0, sym1, sym2, sym3, sym4} OPTIONAL,

scs-60kHz-r17 ENUMERATED{sym0, sym1, sym2, sym3, sym4, sym5, sym6, sym7, sym8} OPTIONAL,

scs-120kHz-r17 ENUMERATED{sym0, sym1, sym2, sym3, sym4, sym5, sym6, sym7, sym8, sym9,

sym10, sym11, sym12, sym13, sym14, sym15, sym16} OPTIONAL

},

maxNumberCarriers-r17 INTEGER(1..16)

} OPTIONAL,

-- R4 17-5 Support of UL DC location(s) report

extendedDC-LocationReport-r17 ENUMERATED {supported} OPTIONAL

}

FeatureSetUplink-v1800 ::= SEQUENCE {

-- R1 40-3-3-1a: Supported maximum delay value larger than D\_basic

maxDelayValueBeyondD-Basic-r18 ENUMERATED {sl2,sl3,sl4,sl5,sl6,sl10} OPTIONAL,

-- R1 40-3-3-2: Number of delay values

tdcp-NumberDelayValue-r18 INTEGER (2..4) OPTIONAL,

-- R1 40-3-3-4: Phase report

phaseReportMoreThanOne-r18 ENUMERATED {supported} OPTIONAL,

-- R1 40-3-3-6: Maximum number of TRS resource sets in a report configuration

maxNumberTRS-ResourceSet-r18 INTEGER (2..3) OPTIONAL,

-- R1 40-3-3-7: Maximum number of TDCP report settings per-BWP

maxNumberTDCP-PerBWP-r18 INTEGER (1..4) OPTIONAL,

-- R1 40-4-6c: DMRS type for Rel.18 enhanced DMRS ports for PUSCH

pusch-DMRS-TypeEnh-r18 SEQUENCE {

dmrs-Type-r18 ENUMERATED {etype1, both},

pusch-TypeA-DMRS-r18 SEQUENCE {

-- R1 40-4-6: Basic feature of Rel.18 enhanced DMRS ports for PUSCH for scheduling mapping of type A for Rel.18 enhanced

-- DMRS ports

dmrs-TypeA-r18 ENUMERATED {supported},

-- R1 40-4-6d: 2 symbols front-loaded DMRS (uplink) for Rel.18 enhanced DMRS ports for PUSCH

pusch-2SymbolFL-DMRS-r18 ENUMERATED {supported} OPTIONAL,

-- R1 40-4-6e: 2-symbol FL DMRS + one additional 2-symbols DMRS for Rel.18 enhanced DMRS ports for PUSCH

pusch-2SymbolFL-DMRS-Addition2Symbol-r18 ENUMERATED {supported} OPTIONAL,

-- R1 40-4-6f: 1 symbol FL DMRS and 3 additional DMRS symbols for Rel.18 enhanced DMRS ports for PUSCH

pusch-1SymbolFL-DMRS-Addition3Symbol-r18 ENUMERATED {supported} OPTIONAL,

-- R1 40-4-6k: 1 symbol FL DMRS and 2 additional DMRS symbols for more than one port for Rel.18 enhanced DMRS ports for

-- PUSCH

pusch-1SymbolFL-DMRS-BeyondOnePort-r18 ENUMERATED {supported} OPTIONAL

} OPTIONAL,

-- R1 40-4-10: DMRS port configuration for PUSCH with 8Tx

dummy ENUMERATED {rel15, both} OPTIONAL,

-- R1 40-4-6a: Basic feature of Rel.18 enhanced DMRS ports for PUSCH for scheduling type B for Rel.18 enhanced DMRS ports

pusch-TypeB-DMRS-r18 ENUMERATED {supported} OPTIONAL,

-- R1 40-4-6g: 1 port UL PTRS for Rel.18 enhanced DMRS ports for PUSCH with rank 1-4

pusch-rank-1-4-1Port-r18 ENUMERATED {supported} OPTIONAL,

-- R1 40-4-6h: 1 port UL PTRS for Rel.18 enhanced DMRS ports for PUSCH with rank 5-8

pusch-rank-5-8-1Port-r18 ENUMERATED {supported} OPTIONAL,

-- R1 40-4-6i: 2 port UL PTRS for Rel.18 enhanced DMRS ports for PUSCH with rank 1-4

pusch-rank-1-4-2Port-r18 ENUMERATED {supported} OPTIONAL,

-- R1 40-4-6j: 2 port UL PTRS for Rel.18 enhanced DMRS ports for PUSCH with rank 5-8

pusch-rank-5-8-2Port-r18 ENUMERATED {supported} OPTIONAL

} OPTIONAL,

-- R1 40-4-13: Support Rel-18 UL DMRS with single-DCI based M-TRP

ul-DMRS-SingleDCI-M-TRP-r18 ENUMERATED {supported} OPTIONAL,

-- R1 40-4-14: Support Rel-18 UL DMRS with M-DCI based M-TRP

ul-DMRS-M-DCI-M-TRP-r18 ENUMERATED {supported} OPTIONAL,

-- R1 40-5-5: Maximum 2 SP and 1 periodic SRS sets for 8T8R antenna switching

srs-AntennaSwitching8T8R2SP-1Periodic-r18 ENUMERATED {supported} OPTIONAL,

-- R1 40-6-4: Single-DCI based STx2P SFN scheme for PUCCH

pucch-SingleDCI-STx2P-SFN-r18 ENUMERATED {pf0-2, pf1-3-4, pf0-4} OPTIONAL,

-- R1 41-4-6: Positioning SRS bandwidth aggregation in RRC\_CONNECTED

posSRS-BWA-RRC-Connected-r18 PosSRS-BWA-RRC-Connected-r18 OPTIONAL,

-- R1 41-4-7: Positioning SRS bandwidth aggregation independent from UL communication CA in RRC\_CONNECTED

posSRS-BWA-IndependentCA-RRC-Connected-r18 PosSRS-BWA-IndependentCA-RRC-Connected-r18 OPTIONAL,

-- R1 41-4-9: Indicate which other bands in the band combination are affected due to the need of a guard period

posSRS-BWA-AffectedBandList-r18 SEQUENCE (SIZE (1..maxBands)) OF FreqBandIndicatorNR OPTIONAL,

-- R1 45-5a: RACH-based early TA acquisition with simultaneous transmission

rach-EarlyTA-BandList-r18 SEQUENCE (SIZE (1..maxBandsMRDC)) OF BOOLEAN OPTIONAL,

-- R1 49-6: Two HARQ-ACK codebooks with up to one sub-slot based HARQ-ACK codebook simultaneously constructed for supporting

-- HARQ-ACK codebooks with different priorities by DCI format 1\_3

simultaneous-2-1-HARQ-ACK-CB-r18 SubSlot-Config-r16 OPTIONAL,

-- R1 49-6a: Two HARQ-ACK codebooks with two sub-slot based HARQ-ACK codebook simultaneously constructed for supporting

-- HARQ-ACK codebooks with different priorities by DCI format 1\_3

simultaneous-2-2-HARQ-ACK-CB-r18 SubSlot-Config-r16 OPTIONAL,

-- R1 49-7: UL intra-UE multiplexing/prioritization of overlapping channel/signals with two priority levels in physical

-- layer for DCI format 1\_3/0\_3

ul-IntraUE-MuxEnh-r18 SEQUENCE {

pusch-PreparationLowPriority-r18 ENUMERATED {sym0, sym1, sym2},

pusch-PreparationHighPriority-r18 ENUMERATED {sym0, sym1, sym2}

} OPTIONAL,

-- R4 27-1 TxDiversity for 4Tx

txDiversity4Tx-r18 ENUMERATED {supported} OPTIONAL,

-- R4 41-2: Power boosting for DFT-s-OFDM pi/2 BPSK and QPSK transmissions without modified spectrum flatness requirement

powerBoosting-pi2BPSK-QPSK-r18 ENUMERATED {supported} OPTIONAL,

-- R4 41-3: Power boosting for DFT-s-OFDM pi/2 BPSK and QPSK transmissions with modified spectrum flatness requirement shaping

powerBoosting-pi2BPSK-QPSK-Modified-r18 ENUMERATED {supported} OPTIONAL,

-- R4 44-1 TxDiversity for 2Tx

txDiversity2Tx-r18 ENUMERATED {supported} OPTIONAL,

ue-PowerClassPerBandPerBC-v1820 ENUMERATED {pc5} OPTIONAL

}

FeatureSetUplink-v1850 ::= SEQUENCE {

-- R1 40-4-10: DMRS port configuration for PUSCH with 8Tx

pusch-DMRS8Tx-r18 ENUMERATED {rel15, both} OPTIONAL,

-- R1 40-7-1h: UE 8Tx PUSCH processing capability for codebook

additionalTime-CB-8TxPUSCH-r18 SEQUENCE {

scs-15kHz-r18 ENUMERATED {sym1, sym2, sym4} OPTIONAL,

scs-30kHz-r18 ENUMERATED {sym1, sym2, sym4, sym8} OPTIONAL,

scs-60kHz-r18 ENUMERATED {sym2, sym4, sym8, sym16} OPTIONAL,

scs-120kHz-r18 ENUMERATED {sym4, sym8, sym16, sym32} OPTIONAL,

scs-480kHz-r18 ENUMERATED {sym16, sym32, sym64, sym128} OPTIONAL,

scs-960kHz-r18 ENUMERATED {sym32, sym64, sym128, sym256} OPTIONAL

} OPTIONAL,

-- R1 40-7-2b: UE 8Tx PUSCH processing capability for non-codebook

additionalTime-NonCB-8TxPUSCH-r18 SEQUENCE {

scs-15kHz-r18 ENUMERATED {sym1, sym2, sym4} OPTIONAL,

scs-30kHz-r18 ENUMERATED {sym1, sym2, sym4, sym8} OPTIONAL,

scs-60kHz-r18 ENUMERATED {sym2, sym4, sym8, sym16} OPTIONAL,

scs-120kHz-r18 ENUMERATED {sym4, sym8, sym16, sym32} OPTIONAL,

scs-480kHz-r18 ENUMERATED {sym16, sym32, sym64, sym128} OPTIONAL,

scs-960kHz-r18 ENUMERATED {sym32, sym64, sym128, sym256} OPTIONAL

} OPTIONAL

}

FeatureSetUplink-v1900 ::= SEQUENCE {

-- R1 59-2-1-8: SRS Port Grouping

srs-PortGrouping-r19 ENUMERATED {xt8r, xt6r, both} OPTIONAL,

-- R1 59-2-4: Association up to 128 CSI-RS ports and SRS for non-codebook-based PUSCH

nonCodebook-CSI-RS-SRS-Enh-r19 ENUMERATED {supported} OPTIONAL,

-- R1 59-3-3-1: Maximum 2 SP and 1 periodic SRS sets for 3T6R antenna switching

srs-AntennaSwitching3T6R2SP-1Periodic-r19 ENUMERATED {supported} OPTIONAL,

-- R1 59-3-3a-1: Maximum 2 SP and 1 periodic SRS sets for 3T3R antenna switching

srs-AntennaSwitching3T3R2SP-1Periodic-r19 ENUMERATED {supported} OPTIONAL,

-- R1 59-3-4: M-TRP PUSCH repetition (type A) of 3-antenna-port PUSCH transmission – codebook based

mTRP-PUSCH-TypeA-CB-3Port-r19 INTEGER (1..2) OPTIONAL,

-- R1 59-3-4a: M-TRP PUSCH repetition (type A) of 3-antenna-port PUSCH transmission – codebook based

mTRP-PUSCH-RepetitionTypeA-3Port-r19 INTEGER (1..3) OPTIONAL,

-- R1 59-3-6: PTRS of 3-antenna-port PUSCH transmission

threePortsPTRS-PUSCH-r19 INTEGER (1..2) OPTIONAL,

-- R1 59-3-7: UL full power transmission mode of fullpower

ul-FullPwrMode-3Port-r19 ENUMERATED {supported} OPTIONAL

}

SubSlot-Config-r16 ::= SEQUENCE {

sub-SlotConfig-NCP-r16 ENUMERATED {n4,n5,n6,n7} OPTIONAL,

sub-SlotConfig-ECP-r16 ENUMERATED {n4,n5,n6} OPTIONAL

}

SRS-AllPosResources-r16 ::= SEQUENCE {

srs-PosResources-r16 SRS-PosResources-r16,

srs-PosResourceAP-r16 SRS-PosResourceAP-r16 OPTIONAL,

srs-PosResourceSP-r16 SRS-PosResourceSP-r16 OPTIONAL

}

SRS-PosResources-r16 ::= SEQUENCE {

maxNumberSRS-PosResourceSetPerBWP-r16 ENUMERATED {n1, n2, n4, n8, n12, n16},

maxNumberSRS-PosResourcesPerBWP-r16 ENUMERATED {n1, n2, n4, n8, n16, n32, n64},

maxNumberSRS-ResourcesPerBWP-PerSlot-r16 ENUMERATED {n1, n2, n3, n4, n5, n6, n8, n10, n12, n14},

maxNumberPeriodicSRS-PosResourcesPerBWP-r16 ENUMERATED {n1, n2, n4, n8, n16, n32, n64},

maxNumberPeriodicSRS-PosResourcesPerBWP-PerSlot-r16 ENUMERATED {n1, n2, n3, n4, n5, n6, n8, n10, n12, n14}

}

SRS-PosResourceAP-r16 ::= SEQUENCE {

maxNumberAP-SRS-PosResourcesPerBWP-r16 ENUMERATED {n1, n2, n4, n8, n16, n32, n64},

maxNumberAP-SRS-PosResourcesPerBWP-PerSlot-r16 ENUMERATED {n1, n2, n3, n4, n5, n6, n8, n10, n12, n14}

}

SRS-PosResourceSP-r16 ::= SEQUENCE {

maxNumberSP-SRS-PosResourcesPerBWP-r16 ENUMERATED {n1, n2, n4, n8, n16, n32, n64},

maxNumberSP-SRS-PosResourcesPerBWP-PerSlot-r16 ENUMERATED {n1, n2, n3, n4, n5, n6, n8, n10, n12, n14}

}

SRS-Resources ::= SEQUENCE {

maxNumberAperiodicSRS-PerBWP ENUMERATED {n1, n2, n4, n8, n16},

maxNumberAperiodicSRS-PerBWP-PerSlot INTEGER (1..6),

maxNumberPeriodicSRS-PerBWP ENUMERATED {n1, n2, n4, n8, n16},

maxNumberPeriodicSRS-PerBWP-PerSlot INTEGER (1..6),

maxNumberSemiPersistentSRS-PerBWP ENUMERATED {n1, n2, n4, n8, n16},

maxNumberSemiPersistentSRS-PerBWP-PerSlot INTEGER (1..6),

maxNumberSRS-Ports-PerResource ENUMERATED {n1, n2, n4}

}

DummyF ::= SEQUENCE {

maxNumberPeriodicCSI-ReportPerBWP INTEGER (1..4),

maxNumberAperiodicCSI-ReportPerBWP INTEGER (1..4),

maxNumberSemiPersistentCSI-ReportPerBWP INTEGER (0..4),

simultaneousCSI-ReportsAllCC INTEGER (5..32)

}

PosSRS-BWA-RRC-Connected-r18 ::= SEQUENCE {

numOfCarriersIntraBandContiguous-r18 ENUMERATED {two, three, twoandthree},

maximumAggregatedBW-TwoCarriersFR1-r18 ENUMERATED {mhz20, mhz40, mhz50, mhz80, mhz100,

mhz160, mhz180, mhz190, mhz200} OPTIONAL,

maximumAggregatedBW-TwoCarriersFR2-r18 ENUMERATED {mhz50, mhz100, mhz200, mhz400, mhz600, mhz800} OPTIONAL,

maximumAggregatedBW-ThreeCarriersFR1-r18 ENUMERATED {mhz80, mhz100, mhz160, mhz200, mhz240, mhz300} OPTIONAL,

maximumAggregatedBW-ThreeCarriersFR2-r18 ENUMERATED {mhz50, mhz100, mhz200, mhz300, mhz400,

mhz600, mhz800, mhz1000, mhz1200}

OPTIONAL,

maximumAggregatedResourceSet-r18 ENUMERATED {n1, n2, n4, n8, n12, n16},

maximumAggregatedResourcePeriodic-r18 ENUMERATED {n1, n2, n4, n8, n16, n32, n64},

maximumAggregatedResourceAperiodic-r18 ENUMERATED {n0, n1, n2, n4, n8, n16, n32, n64},

maximumAggregatedResourceSemi-r18 ENUMERATED {n0, n1, n2, n4, n8, n16, n32, n64},

maximumAggregatedResourcePeriodicPerSlot-r18 ENUMERATED {n1, n2, n3, n4, n5, n6, n8, n10, n12, n14},

maximumAggregatedResourceAperiodicPerSlot-r18 ENUMERATED {n0, n1, n2, n3, n4, n5, n6, n8, n10, n12, n14},

maximumAggregatedResourceSemiPerSlot-r18 ENUMERATED {n0, n1, n2, n3, n4, n5, n6, n8, n10, n12, n14},

...

}

PosSRS-BWA-IndependentCA-RRC-Connected-r18 ::= SEQUENCE {

numOfCarriersIntraBandContiguous-r18 ENUMERATED {two, three, twoandthree},

maximumAggregatedBW-TwoCarriersFR1-r18 ENUMERATED {mhz20, mhz40, mhz50, mhz80, mhz100,

mhz160, mhz180, mhz190, mhz200} OPTIONAL,

maximumAggregatedBW-TwoCarriersFR2-r18 ENUMERATED {mhz50, mhz100, mhz200, mhz400, mhz600, mhz800} OPTIONAL,

maximumAggregatedBW-ThreeCarriersFR1-r18 ENUMERATED {mhz80, mhz100, mhz160, mhz200, mhz240, mhz300} OPTIONAL,

maximumAggregatedBW-ThreeCarriersFR2-r18 ENUMERATED {mhz50, mhz100, mhz200, mhz300, mhz400,

mhz600, mhz800, mhz1000, mhz1200}

OPTIONAL,

maximumAggregatedResourceSet-r18 ENUMERATED {n1, n2, n4, n8, n12, n16},

maximumAggregatedResourcePeriodic-r18 ENUMERATED {n1, n2, n4, n8, n16, n32, n64},

maximumAggregatedResourceAperiodic-r18 ENUMERATED {n0, n1, n2, n4, n8, n16, n32, n64},

maximumAggregatedResourceSemi-r18 ENUMERATED {n0, n1, n2, n4, n8, n16, n32, n64},

maximumAggregatedResourcePeriodicPerSlot-r18 ENUMERATED {n1, n2, n3, n4, n5, n6, n8, n10, n12, n14},

maximumAggregatedResourceAperiodicPerSlot-r18 ENUMERATED {n0, n1, n2, n3, n4, n5, n6, n8, n10, n12, n14},

maximumAggregatedResourceSemiPerSlot-r18 ENUMERATED {n0, n1, n2, n3, n4, n5, n6, n8, n10, n12, n14},

guardPeriod-r18 ENUMERATED {n0, n30, n100, n140, n200},

powerClassForTwoAggregatedCarriers-r18 ENUMERATED {pc2, pc3} OPTIONAL,

powerClassForThreeAggregatedCarriers-r18 ENUMERATED {pc2, pc3} OPTIONAL,

...

}

-- TAG-FEATURESETUPLINK-STOP

-- ASN1STOP

|  |
| --- |
| *FeatureSetUplink* field descriptions |
| ***featureSetListPerUplinkCC***  Indicates which features the UE supports on the individual UL carriers of the feature set (and hence of a band entry that refers to the feature set). The UE shall hence include at least as many *FeatureSetUplinkPerCC-Id* in this list as the number of carriers it supports according to the *ca-BandwidthClassUL*, except if indicating additional functionality by reducing the number of *FeatureSetUplinkPerCC-Id* in the feature set (see NOTE 1 in *FeatureSetCombination* IE description). The order of the elements in this list is not relevant, i.e., the network may configure any of the carriers in accordance with any of the *FeatureSetUplinkPerCC-Id* in this list. |

#### – *FeatureSetUplinkId*

The IE *FeatureSetUplinkId* identifies an uplink feature set. The *FeatureSetUplinkId* of a *FeatureSetUplink* is the index position of the *FeatureSetUplink* in the *featureSetsUplink* list in the *FeatureSets* IE. The first element in the list is referred to by *FeatureSetUplinkId* = 1, and so on. The *FeatureSetUplinkId =0* is not used by an actual *FeatureSetUplink* but means that the UE does not support a carrier in this band of a band combination.

*FeatureSetUplinkId* information element

-- ASN1START

-- TAG-FEATURESETUPLINKID-START

FeatureSetUplinkId ::= INTEGER (0..maxUplinkFeatureSets)

-- TAG-FEATURESETUPLINKID-STOP

-- ASN1STOP

#### – *FeatureSetUplinkPerCC*

The IE *FeatureSetUplinkPerCC* indicates a set of features that the UE supports on the corresponding carrier of one band entry of a band combination.

*FeatureSetUplinkPerCC* information element

-- ASN1START

-- TAG-FEATURESETUPLINKPERCC-START

FeatureSetUplinkPerCC ::= SEQUENCE {

supportedSubcarrierSpacingUL SubcarrierSpacing,

supportedBandwidthUL SupportedBandwidth,

channelBW-90mhz ENUMERATED {supported} OPTIONAL,

mimo-CB-PUSCH SEQUENCE {

maxNumberMIMO-LayersCB-PUSCH MIMO-LayersUL OPTIONAL,

maxNumberSRS-ResourcePerSet INTEGER (1..2)

} OPTIONAL,

maxNumberMIMO-LayersNonCB-PUSCH MIMO-LayersUL OPTIONAL,

supportedModulationOrderUL ModulationOrder OPTIONAL

}

FeatureSetUplinkPerCC-v1540 ::= SEQUENCE {

mimo-NonCB-PUSCH SEQUENCE {

maxNumberSRS-ResourcePerSet INTEGER (1..4),

maxNumberSimultaneousSRS-ResourceTx INTEGER (1..4)

} OPTIONAL

}

FeatureSetUplinkPerCC-v1700 ::= SEQUENCE {

supportedMinBandwidthUL-r17 SupportedBandwidth-v1700 OPTIONAL,

-- R1 23-3-1-3 FeMIMO: Multi-TRP PUSCH repetition (type B) - non-codebook based

mTRP-PUSCH-RepetitionTypeB-r17 ENUMERATED {n1,n2,n3,n4} OPTIONAL,

-- R1 23-3-1-1 -codebook based Multi-TRP PUSCH repetition (type B)

mTRP-PUSCH-TypeB-CB-r17 ENUMERATED {n1,n2,n4} OPTIONAL,

supportedBandwidthUL-v1710 SupportedBandwidth-v1700 OPTIONAL

}

FeatureSetUplinkPerCC-v1780 ::= SEQUENCE {

supportedBandwidthUL-v1780 SupportedBandwidth-v1700 OPTIONAL

}

FeatureSetUplinkPerCC-v1800 ::= SEQUENCE {

-- R1 40-2-7: Two TAs for multi-DCI STxMP PUSCH+PUSCH

twoPUSCH-MultiDCI-STx2P-TwoTA-r18 ENUMERATED {supported} OPTIONAL,

-- R1 40-6-1: Single-DCI based STx2P SDM scheme for PUSCH-codebook

pusch-CB-SingleDCI-STx2P-SDM-r18 SEQUENCE {

maxNumberSRS-ResourcePerSet-r18 ENUMERATED {n1,n2,n4},

maxNumberLayerPerPanel-r18 INTEGER (1..2),

maxNumberNZP-PUSCH-PortsPerSet-r18 ENUMERATED {n1,n2,n4},

maxNumberSRS-AntennaPortsPerSet-r18 ENUMERATED {n1,n2,n4}

} OPTIONAL,

-- R1 40-6-1a: Single-DCI based STx2P SDM scheme for PUSCH-noncodebook

pusch-NonCB-SingleDCI-STx2P-SDM-r18 SEQUENCE {

maxNumberSRS-ResourcePerSet-r18 INTEGER (1..4),

maxNumberLayerPerPanel-r18 INTEGER (1..2),

maxNumberSimulSRS-OneResourcePerSet-r18 INTEGER (1..4),

maxNumberSimulSRS-TwoResourcePerSet-r18 INTEGER (1..8)

} OPTIONAL,

-- R1 40-6-2: Single-DCI based STx2P SFN scheme for PUSCH-codebook

pusch-CB-SingleDCI-STx2P-SFN-r18 SEQUENCE {

maxNumberSRS-ResourcePerSet-r18 ENUMERATED {n1,n2,n4},

maxNumberLayerPerSet-r18 INTEGER (1..2),

maxNumberSRS-AntennaPortsPerSet-r18 ENUMERATED {n1,n2,n4},

maxNumberNZP-PUSCH-PortsPerSet-r18 ENUMERATED {n1,n2,n4}

} OPTIONAL,

-- R1 40-6-2a: Single-DCI based STx2P SFN scheme for PUSCH-noncodebook

pusch-NonCB-SingleDCI-STx2P-SFN-r18 SEQUENCE {

maxNumberSRS-ResourcePerSet-r18 INTEGER (1..4),

maxNumberLayerPerSet-r18 INTEGER (1..2),

maxNumberSimulSRS-OneResourcePerSet-r18 INTEGER (1..4),

maxNumberSimulSRS-TwoResourcePerSet-r18 INTEGER (1..8)

} OPTIONAL,

-- R1 40-6-3a: codebook multi-DCI based STx2P PUSCH+PUSCH for DG+DG

twoPUSCH-CB-MultiDCI-STx2P-DG-DG-r18 SEQUENCE {

maxNumberSRS-ResourcePerSet-r18 ENUMERATED {n1, n2, n4},

maxNumberLayerOverlapping-r18 INTEGER (1..2),

maxNumberNZP-PUSCH-Overlapping-r18 ENUMERATED {n1, n2, n4},

maxNumberPUSCH-PerCORESET-PerSlot-r18 SEQUENCE {

scs-60kHz-r18 ENUMERATED {n1,n2,n3,n4,n7} OPTIONAL,

scs-120kHz-r18 ENUMERATED {n1,n2,n3,n4,n7} OPTIONAL

} OPTIONAL,

maxNumberTotalLayerOverlapping-r18 INTEGER (2..4),

maxNumberSRS-AntennaPortsPerSet-r18 ENUMERATED {n1,n2,n4}

} OPTIONAL,

-- R1 40-6-3b: Noncodebook multi-DCI based STx2P PUSCH+PUSCH for DG+DG

twoPUSCH-NonCB-MultiDCI-STx2P-DG-DG-r18 SEQUENCE {

maxNumberSRS-ResourcePerSet-r18 INTEGER (1..4),

maxNumberLayerOverlapping-r18 INTEGER (1..2),

maxNumberSimulSRS-ResourcePerSet-r18 INTEGER (1..4),

maxNumberPUSCH-PerCORESET-PerSlot-r18 SEQUENCE {

scs-60kHz-r18 ENUMERATED {n1,n2,n3,n4,n7} OPTIONAL,

scs-120kHz-r18 ENUMERATED {n1,n2,n3,n4,n7} OPTIONAL

} OPTIONAL,

maxNumberTotalLayerOverlapping-r18 INTEGER (2..4)

} OPTIONAL,

-- R1 40-6-6: Out-of-order operation for multi-DCI based STx2P PUSCH+PUSCH

twoPUSCH-MultiDCI-STx2P-OutOfOrder-r18 ENUMERATED {supported} OPTIONAL,

codebookParameter8TxPUSCH-r18 SEQUENCE {

-- R1 40-7-1: Basic features for Codebook-based 8Tx PUSCH

codebook-8TxBasic-r18 SEQUENCE {

maxNumberPUSCH-MIMO-Layer-r18 INTEGER (1..8),

maxNumberSRS-Resource-r18 INTEGER (1..2),

srs-8TxPorts-r18 ENUMERATED {noTDM, both}

},

-- R1 40-7-1a: Codebook-based 8Tx PUSCH-codebook1

codebook1-8TxPUSCH-r18 SEQUENCE {

codebookN1N4-r18 ENUMERATED {ng1n4n1,ng1n2n2,both} OPTIONAL,

srs-8TxPorts-r18 ENUMERATED {noTDM, both}

},

-- R1 40-7-1b: Codebook-based 8Tx PUSCH-codebook2

codebook2-8TxPUSCH-r18 ENUMERATED {supported} OPTIONAL,

-- R1 40-7-1c: Codebook-based 8Tx PUSCH-codebook3

codebook3-8TxPUSCH-r18 ENUMERATED {supported} OPTIONAL,

-- R1 40-7-1d: Codebook-based 8Tx PUSCH-codebook4

codebook4-8TxPUSCH-r18 ENUMERATED {supported} OPTIONAL,

-- R1 40-7-1e: UL full power transmission mode 0

ul-FullPwrTransMode0-r18 ENUMERATED {supported} OPTIONAL,

-- R1 40-7-1f: UL full power transmission mode 1

ul-FullPwrTransMode1-r18 ENUMERATED {supported} OPTIONAL,

-- R1 40-7-1g: UL full power transmission mode 2 with 1/2/4 resources

ul-FullPwrTransMode2-r18 ENUMERATED {n1,n2,n4} OPTIONAL,

-- R1 40-7-1g-1: SRS resources for UL full power transmission mode 2

ul-SRS-TransMode2-r18 BIT STRING (SIZE(3)) OPTIONAL,

-- R1 40-7-1g-2: TPMI group(s) which delivers full power for codebook2

tpmi-FullPwrCodebook2-r18 ENUMERATED {first, second} OPTIONAL

} OPTIONAL,

-- R1 40-7-2: Basic features for Non-Codebook-based 8Tx PUSCH

nonCodebook-8TxPUSCH-r18 SEQUENCE {

maxNumberPUSCH-MIMO-Layer-r18 INTEGER (1..8),

maxNumberSRS-Resource-r18 INTEGER (1..8),

maxNumberSimultaneousSRS-r18 INTEGER (1..8)

} OPTIONAL,

-- R1 40-7-2a: Association between CSI-RS and SRS for non-codebook case

nonCodebook-CSI-RS-SRS-r18 ENUMERATED {supported} OPTIONAL,

-- R1 40-7-3: CBG based 2 CWs PUSCH with rank >4

cgb-2CW-PUSCH-r18 ENUMERATED {supported} OPTIONAL

}

FeatureSetUplinkPerCC-v1840 ::= SEQUENCE {

supportedBandwidthUL-v1840 SupportedBandwidth-v1840 OPTIONAL,

supportedMinBandwidthUL-v1840 SupportedBandwidth-v1840 OPTIONAL

}

FeatureSetUplinkPerCC-v1850 ::= SEQUENCE {

-- R1 40-6-3a-1: UE STxMP processing capability for codebook

twoPUSCH-CB-MultiDCI-STx2P-AdditionalTime-r18 CHOICE {

scs-60kHz-r18 ENUMERATED {sym1, sym4, sym8, sym16},

scs-120kHz-r18 ENUMERATED {sym4, sym8, sym16, sym32},

scs-480kHz-r18 ENUMERATED {sym16, sym32, sym64, sym128},

scs-960kHz-r18 ENUMERATED {sym32, sym64, sym128,sym256}

} OPTIONAL,

-- R1 40-6-3b-2: UE STxMP processing capability for non-codebook

twoPUSCH-NonCB-MultiDCI-STx2P-AdditionalTime-r18 CHOICE {

scs-60kHz-r18 ENUMERATED {sym1, sym4, sym8, sym16},

scs-120kHz-r18 ENUMERATED {sym4, sym8, sym16, sym32},

scs-480kHz-r18 ENUMERATED {sym16, sym32, sym64, sym128},

scs-960kHz-r18 ENUMERATED {sym32, sym64, sym128,sym256}

} OPTIONAL

}

FeatureSetUplinkPerCC-v1900 ::= SEQUENCE {

-- R1 67-1a: 32 UL HARQ processes for TN in FR1 and FR2-1

support32-UL-HARQ-ProcessTN-r19 ENUMERATED {supported} OPTIONAL,

-- R1 59-3-1: Non-codebook based PUSCH transmission for 3TX for single TRP

nonCodebook-3TxPUSCH-SingleTRP-r19 SEQUENCE {

maxNumberLayer-r19 INTEGER (1..3),

maxNumberSRS-Resource-r19 INTEGER (1..3),

maxNumberSimultaneousSRS-r19 INTEGER (1..3)

} OPTIONAL,

-- R1 59-3-2: Codebook based PUSCH transmission for 3TX for single TRP

codebook-3TxPUSCH-SingleTRP-r19 SEQUENCE {

maxNumberPUSCH-MIMO-Layer-r19 INTEGER (1..3),

maxNumberSRS-Resource-r19 INTEGER (1..2)

} OPTIONAL,

-- R1 59-3-5: M-TRP PUSCH repetition (type B) of 3-antenna-port PUSCH transmission – codebook based

codebook-3PortPUSCH-TypeB-r19 INTEGER (1..2) OPTIONAL,

-- R1 59-3-5a: M-TRP PUSCH repetition (type B) of 3-antenna-port PUSCH transmission – non-codebook based

mTRP-PUSCH-RepetitionTypeB-3Port-r19 INTEGER (1..3) OPTIONAL

}

-- TAG-FEATURESETUPLINKPERCC-STOP

-- ASN1STOP

#### – *FeatureSetUplinkPerCC-Id*

The IE *FeatureSetUplinkPerCC-Id* identifies a set of features applicable to one carrier of a feature set. The *FeatureSetUplinkPerCC-Id* of a *FeatureSetUplinkPerCC* is the index position of the *FeatureSetUplinkPerCC* in the *featureSetsUplinkPerCC*. The first element in the list is referred to by *FeatureSetUplinkPerCC-Id* = 1, and so on.

*FeatureSetUplinkPerCC-Id* information element

-- ASN1START

-- TAG-FEATURESETUPLINKPERCC-ID-START

FeatureSetUplinkPerCC-Id ::= INTEGER (1..maxPerCC-FeatureSets)

-- TAG-FEATURESETUPLINKPERCC-ID-STOP

-- ASN1STOP

#### – *FreqBandIndicatorEUTRA*

-- ASN1START

-- TAG-FREQBANDINDICATOREUTRA-START

FreqBandIndicatorEUTRA ::= INTEGER (1..maxBandsEUTRA)

-- TAG-FREQBANDINDICATOREUTRA-STOP

-- ASN1STOP

#### – *FreqBandList*

The IE *FreqBandList* is used by the network to request NR CA, NR non-CA and/or MR-DC band combinations for specific NR and/or E-UTRA frequency bands and/or up to a specific number of carriers and/or up to specific aggregated bandwidth. This is also used to request feature sets (for NR) and feature set combinations (for NR and MR-DC). For NR sidelink communication, this is used by the initiating UE to request sidelink UE radio access capabilities from the peer UE. This is also used to request lower MSD capability for specific NR frequency bands for the UE supporting lower MSD.

*FreqBandList* information element

-- ASN1START

-- TAG-FREQBANDLIST-START

FreqBandList ::= SEQUENCE (SIZE (1..maxBandsMRDC)) OF FreqBandInformation

FreqBandInformation ::= CHOICE {

bandInformationEUTRA FreqBandInformationEUTRA,

bandInformationNR FreqBandInformationNR

}

FreqBandInformationEUTRA ::= SEQUENCE {

bandEUTRA FreqBandIndicatorEUTRA,

ca-BandwidthClassDL-EUTRA CA-BandwidthClassEUTRA OPTIONAL, -- Need N

ca-BandwidthClassUL-EUTRA CA-BandwidthClassEUTRA OPTIONAL -- Need N

}

FreqBandInformationNR ::= SEQUENCE {

bandNR FreqBandIndicatorNR,

maxBandwidthRequestedDL AggregatedBandwidth OPTIONAL, -- Need N

maxBandwidthRequestedUL AggregatedBandwidth OPTIONAL, -- Need N

maxCarriersRequestedDL INTEGER (1..maxNrofServingCells) OPTIONAL, -- Need N

maxCarriersRequestedUL INTEGER (1..maxNrofServingCells) OPTIONAL -- Need N

}

AggregatedBandwidth ::= ENUMERATED {mhz50, mhz100, mhz150, mhz200, mhz250, mhz300, mhz350,

mhz400, mhz450, mhz500, mhz550, mhz600, mhz650, mhz700, mhz750, mhz800}

-- TAG-FREQBANDLIST-STOP

-- ASN1STOP

#### – *FreqSeparationClass*

The IE *FreqSeparationClas*s is used for an intra-band non-contiguous CA band combination to indicate frequency separation between lower edge of lowest CC and upper edge of highest CC in a frequency band.

*FreqSeparationClass* information element

-- ASN1START

-- TAG-FREQSEPARATIONCLASS-START

FreqSeparationClass ::= ENUMERATED { mhz800, mhz1200, mhz1400, ..., mhz400-v1650, mhz600-v1650}

FreqSeparationClassDL-v1620 ::= ENUMERATED {mhz1000, mhz1600, mhz1800, mhz2000, mhz2200, mhz2400}

FreqSeparationClassUL-v1620 ::= ENUMERATED {mhz1000}

-- TAG-FREQSEPARATIONCLASS-STOP

-- ASN1STOP

#### *– FreqSeparationClassDL-Only*

The IE *FreqSeparationClassDL-Only* is used to indicate the frequency separation between lower edge of lowest CC and upper edge of highest CC of DL only frequency spectrum in a frequency band.

*FreqSeparationClassDL-Only* information element

-- ASN1START

-- TAG-FREQSEPARATIONCLASSDL-Only-START

FreqSeparationClassDL-Only-r16 ::= ENUMERATED {mhz200, mhz400, mhz600, mhz800, mhz1000, mhz1200}

-- TAG-FREQSEPARATIONCLASSDL-Only-STOP

-- ASN1STOP

#### – *FR2-2-AccessParamsPerBand*

The IE *FR2-2-AccessParamsPerBand* is used to convey FR2-2 related parameters specific for a certain frequency band (not per feature set or band combination).

FR2-2-AccessParamsPerBand information element

-- ASN1START

-- TAG-FR2-2-ACCESSPARAMSPERBAND-START

FR2-2-AccessParamsPerBand-r17 ::= SEQUENCE {

-- R1 24-1: Basic FR2-2 DL support

dl-FR2-2-SCS-120kHz-r17 ENUMERATED {supported} OPTIONAL,

-- R1 24-1a: Basic FR2-2 UL support

ul-FR2-2-SCS-120kHz-r17 ENUMERATED {supported} OPTIONAL,

-- R1 24-2: 120KHz SSB support for initial access in FR2-2

initialAccessSSB-120kHz-r17 ENUMERATED {supported} OPTIONAL,

-- R1 24-1b: Wideband PRACH for 120 kHz in FR2-2

widebandPRACH-SCS-120kHz-r17 ENUMERATED {supported} OPTIONAL,

-- R1 24-1c: Multi-RB support PUCCH format 0/1/4 for 120 kHz in FR2-2

multiRB-PUCCH-SCS-120kHz-r17 ENUMERATED {supported} OPTIONAL,

-- R1 24-1d: Multiple PDSCH scheduling by single DCI for 120kHz in FR2-2

multiPDSCH-SingleDCI-FR2-2-SCS-120kHz-r17 ENUMERATED {supported} OPTIONAL,

-- R1 24-1e: Multiple PUSCH scheduling by single DCI for 120kHz in FR2-2

multiPUSCH-SingleDCI-FR2-2-SCS-120kHz-r17 ENUMERATED {supported} OPTIONAL,

-- R1 24-4: 480KHz SCS support for DL

dl-FR2-2-SCS-480kHz-r17 ENUMERATED {supported} OPTIONAL,

-- R1 24-4a: 480KHz SCS support for UL

ul-FR2-2-SCS-480kHz-r17 ENUMERATED {supported} OPTIONAL,

-- R1 24-3: 480KHz SSB support for initial access in FR2-2

initialAccessSSB-480kHz-r17 ENUMERATED {supported} OPTIONAL,

-- R1 24-4b: Wideband PRACH for 480 kHz in FR2-2

widebandPRACH-SCS-480kHz-r17 ENUMERATED {supported} OPTIONAL,

-- R1 24-4c: Multi-RB support PUCCH format 0/1/4 for 480 kHz in FR2-2

multiRB-PUCCH-SCS-480kHz-r17 ENUMERATED {supported} OPTIONAL,

-- R1 24-4f: Enhanced PDCCH monitoring for 480KHz in FR2-2

enhancedPDCCH-monitoringSCS-480kHz-r17 ENUMERATED {supported} OPTIONAL,

-- R1 24-5: 960KHz SCS support for DL

dl-FR2-2-SCS-960kHz-r17 ENUMERATED {supported} OPTIONAL,

-- R1 24-5a: 960KHz SCS support for UL

ul-FR2-2-SCS-960kHz-r17 ENUMERATED {supported} OPTIONAL,

-- R1 24-5c: Multi-RB support PUCCH format 0/1/4 for 960 kHz in FR2-2

multiRB-PUCCH-SCS-960kHz-r17 ENUMERATED {supported} OPTIONAL,

-- R1 24-5f: Enhanced PDCCH monitoring for 960KHz in FR2-2

enhancedPDCCH-monitoringSCS-960kHz-r17 SEQUENCE {

pdcch-monitoring4-1-r17 ENUMERATED {supported} OPTIONAL,

pdcch-monitoring4-2-r17 ENUMERATED {supported} OPTIONAL,

pdcch-monitoring8-4-r17 ENUMERATED {supported} OPTIONAL

} OPTIONAL,

-- R1 24-6: Type 1 channel access procedure in uplink for FR2-2 with shared spectrum channel access

type1-ChannelAccess-FR2-2-r17 ENUMERATED {supported} OPTIONAL,

-- R1 24-7: Type 2 channel access procedure in uplink for FR2-2 with shared spectrum channel access

type2-ChannelAccess-FR2-2-r17 ENUMERATED {supported} OPTIONAL,

-- R1 24-10: Reduced beam switching time delay

reduced-BeamSwitchTiming-FR2-2-r17 ENUMERATED {supported} OPTIONAL,

-- R1 24-8: 32 DL HARQ processes for FR 2-2

support32-DL-HARQ-ProcessPerSCS-r17 SEQUENCE {

scs-120kHz-r17 ENUMERATED {supported} OPTIONAL,

scs-480kHz-r17 ENUMERATED {supported} OPTIONAL,

scs-960kHz-r17 ENUMERATED {supported} OPTIONAL

} OPTIONAL,

-- R1 24-9: 32 UL HARQ processes for FR 2-2

support32-UL-HARQ-ProcessPerSCS-r17 SEQUENCE {

scs-120kHz-r17 ENUMERATED {supported} OPTIONAL,

scs-480kHz-r17 ENUMERATED {supported} OPTIONAL,

scs-960kHz-r17 ENUMERATED {supported} OPTIONAL

} OPTIONAL,

...,

[[

-- R4 15-1: 64QAM for PUSCH for FR2-2

modulation64-QAM-PUSCH-FR2-2-r17 ENUMERATED {supported} OPTIONAL

]]

}

-- TAG-FR2-2-ACCESSPARAMSPERBAND-STOP

-- ASN1STOP

#### – *HighSpeedParameters*

The IE *HighSpeedParameters* is used to convey capabilities related to high speed scenarios.

*HighSpeedParameters* information element

-- ASN1START

-- TAG-HIGHSPEEDPARAMETERS-START

HighSpeedParameters-r16 ::= SEQUENCE {

measurementEnhancement-r16 ENUMERATED {supported} OPTIONAL,

demodulationEnhancement-r16 ENUMERATED {supported} OPTIONAL

}

HighSpeedParameters-v1650 ::= CHOICE {

intraNR-MeasurementEnhancement-r16 ENUMERATED {supported},

interRAT-MeasurementEnhancement-r16 ENUMERATED {supported}

}

HighSpeedParameters-v1700 ::= SEQUENCE {

-- R4 18-1: Enhanced RRM requirements specified for CA for FR1 HST

measurementEnhancementCA-r17 ENUMERATED {supported} OPTIONAL,

-- R4 18-2: Enhanced RRM requirements specified for inter-frequency measurement in connected mode for FR1 HST

measurementEnhancementInterFreq-r17 ENUMERATED {supported} OPTIONAL

}

-- TAG-HIGHSPEEDPARAMETERS-STOP

-- ASN1STOP

#### – *IMS-Parameters*

The IE *IMS-Parameters* is used to convey capabilities related to IMS.

*IMS-Parameters* information element

-- ASN1START

-- TAG-IMS-PARAMETERS-START

IMS-Parameters ::= SEQUENCE {

ims-ParametersCommon IMS-ParametersCommon OPTIONAL,

ims-ParametersFRX-Diff IMS-ParametersFRX-Diff OPTIONAL,

...

}

IMS-Parameters-v1700 ::= SEQUENCE {

ims-ParametersFR2-2-r17 IMS-ParametersFR2-2-r17 OPTIONAL

}

IMS-ParametersCommon ::= SEQUENCE {

voiceOverEUTRA-5GC ENUMERATED {supported} OPTIONAL,

...,

[[

voiceOverSCG-BearerEUTRA-5GC ENUMERATED {supported} OPTIONAL

]],

[[

voiceFallbackIndicationEPS-r16 ENUMERATED {supported} OPTIONAL

]]

}

IMS-ParametersFRX-Diff ::= SEQUENCE {

voiceOverNR ENUMERATED {supported} OPTIONAL,

...

}

IMS-ParametersFR2-2-r17 ::= SEQUENCE {

voiceOverNR-r17 ENUMERATED {supported} OPTIONAL,

...

}

-- TAG-IMS-PARAMETERS-STOP

-- ASN1STOP

#### – *InterRAT-Parameters*

The IE *InterRAT-Parameters* is used convey UE capabilities related to the other RATs.

*InterRAT-Parameters* information element

-- ASN1START

-- TAG-INTERRAT-PARAMETERS-START

InterRAT-Parameters ::= SEQUENCE {

eutra EUTRA-Parameters OPTIONAL,

...,

[[

utra-FDD-r16 UTRA-FDD-Parameters-r16 OPTIONAL

]]

}

EUTRA-Parameters ::= SEQUENCE {

supportedBandListEUTRA SEQUENCE (SIZE (1..maxBandsEUTRA)) OF FreqBandIndicatorEUTRA,

eutra-ParametersCommon EUTRA-ParametersCommon OPTIONAL,

eutra-ParametersXDD-Diff EUTRA-ParametersXDD-Diff OPTIONAL,

...

}

EUTRA-ParametersCommon ::= SEQUENCE {

mfbi-EUTRA ENUMERATED {supported} OPTIONAL,

modifiedMPR-BehaviorEUTRA BIT STRING (SIZE (32)) OPTIONAL,

multiNS-Pmax-EUTRA ENUMERATED {supported} OPTIONAL,

rs-SINR-MeasEUTRA ENUMERATED {supported} OPTIONAL,

...,

[[

ne-DC ENUMERATED {supported} OPTIONAL

]],

[[

nr-HO-ToEN-DC-r16 ENUMERATED {supported} OPTIONAL

]]

}

EUTRA-ParametersXDD-Diff ::= SEQUENCE {

rsrqMeasWidebandEUTRA ENUMERATED {supported} OPTIONAL,

...

}

UTRA-FDD-Parameters-r16 ::= SEQUENCE {

supportedBandListUTRA-FDD-r16 SEQUENCE (SIZE (1..maxBandsUTRA-FDD-r16)) OF SupportedBandUTRA-FDD-r16,

...

}

SupportedBandUTRA-FDD-r16 ::= ENUMERATED {

bandI, bandII, bandIII, bandIV, bandV, bandVI,

bandVII, bandVIII, bandIX, bandX, bandXI,

bandXII, bandXIII, bandXIV, bandXV, bandXVI,

bandXVII, bandXVIII, bandXIX, bandXX,

bandXXI, bandXXII, bandXXIII, bandXXIV,

bandXXV, bandXXVI, bandXXVII, bandXXVIII,

bandXXIX, bandXXX, bandXXXI, bandXXXII}

-- TAG-INTERRAT-PARAMETERS-STOP

-- ASN1STOP

#### – *MAC-Parameters*

The IE *MAC-Parameters* is used to convey capabilities related to MAC.

*MAC-Parameters* information element

-- ASN1START

-- TAG-MAC-PARAMETERS-START

MAC-Parameters ::= SEQUENCE {

mac-ParametersCommon MAC-ParametersCommon OPTIONAL,

mac-ParametersXDD-Diff MAC-ParametersXDD-Diff OPTIONAL

}

MAC-Parameters-v1610 ::= SEQUENCE {

mac-ParametersFRX-Diff-r16 MAC-ParametersFRX-Diff-r16 OPTIONAL

}

MAC-Parameters-v1700 ::= SEQUENCE {

mac-ParametersFR2-2-r17 MAC-ParametersFR2-2-r17 OPTIONAL

}

MAC-Parameters-v17b0 ::= SEQUENCE {

mTRP-PUSCH-PHR-Type1-Reporting-r17 ENUMERATED {supported} OPTIONAL

}

MAC-Parameters-v17c0 ::= SEQUENCE {

directSCellActivationWithTCI-r17 ENUMERATED {supported} OPTIONAL

}

MAC-ParametersCommon ::= SEQUENCE {

lcp-Restriction ENUMERATED {supported} OPTIONAL,

dummy ENUMERATED {supported} OPTIONAL,

lch-ToSCellRestriction ENUMERATED {supported} OPTIONAL,

...,

[[

recommendedBitRate ENUMERATED {supported} OPTIONAL,

recommendedBitRateQuery ENUMERATED {supported} OPTIONAL

]],

[[

recommendedBitRateMultiplier-r16 ENUMERATED {supported} OPTIONAL,

preEmptiveBSR-r16 ENUMERATED {supported} OPTIONAL,

autonomousTransmission-r16 ENUMERATED {supported} OPTIONAL,

lch-PriorityBasedPrioritization-r16 ENUMERATED {supported} OPTIONAL,

lch-ToConfiguredGrantMapping-r16 ENUMERATED {supported} OPTIONAL,

lch-ToGrantPriorityRestriction-r16 ENUMERATED {supported} OPTIONAL,

singlePHR-P-r16 ENUMERATED {supported} OPTIONAL,

ul-LBT-FailureDetectionRecovery-r16 ENUMERATED {supported} OPTIONAL,

-- R4 8-1: MPE

tdd-MPE-P-MPR-Reporting-r16 ENUMERATED {supported} OPTIONAL,

lcid-ExtensionIAB-r16 ENUMERATED {supported} OPTIONAL

]],

[[

spCell-BFR-CBRA-r16 ENUMERATED {supported} OPTIONAL

]],

[[

srs-ResourceId-Ext-r16 ENUMERATED {supported} OPTIONAL

]],

[[

enhancedUuDRX-forSidelink-r17 ENUMERATED {supported} OPTIONAL,

--27-10: Support of UL MAC CE based MG activation request for PRS measurements

mg-ActivationRequestPRS-Meas-r17 ENUMERATED {supported} OPTIONAL,

--27-11: Support of DL MAC CE based MG activation request for PRS measurements

mg-ActivationCommPRS-Meas-r17 ENUMERATED {supported} OPTIONAL,

intraCG-Prioritization-r17 ENUMERATED {supported} OPTIONAL,

jointPrioritizationCG-Retx-Timer-r17 ENUMERATED {supported} OPTIONAL,

survivalTime-r17 ENUMERATED {supported} OPTIONAL,

lcg-ExtensionIAB-r17 ENUMERATED {supported} OPTIONAL,

harq-FeedbackDisabled-r17 ENUMERATED {supported} OPTIONAL,

uplink-Harq-ModeB-r17 ENUMERATED {supported} OPTIONAL,

sr-TriggeredBy-TA-Report-r17 ENUMERATED {supported} OPTIONAL,

extendedDRX-CycleInactive-r17 ENUMERATED {supported} OPTIONAL,

simultaneousSR-PUSCH-DiffPUCCH-groups-r17 ENUMERATED {supported} OPTIONAL,

lastTransmissionUL-r17 ENUMERATED {supported} OPTIONAL

]],

[[

harq-RTT-TimerDL-ForNTN-MulticastMBS-r17 ENUMERATED {supported} OPTIONAL

]],

[[

sr-TriggeredByTA-ReportATG-r18 ENUMERATED {supported} OPTIONAL,

extendedDRX-CycleInactive-r18 ENUMERATED {supported} OPTIONAL,

additionalBS-Table-r18 ENUMERATED {supported} OPTIONAL,

delayStatusReport-r18 ENUMERATED {supported} OPTIONAL,

cg-RetransmissionMonitoringDisabling-r18 ENUMERATED {supported} OPTIONAL,

non-IntegerDRX-r18 ENUMERATED {supported} OPTIONAL

]],

[[

multipleEntryDelayStatusReport-r19 ENUMERATED {supported} OPTIONAL,

lcp-PriorityAdjustment-r19 ENUMERATED {supported} OPTIONAL,

ul-RateControl-r19 ENUMERATED {supported} OPTIONAL,

ul-RateQuery-r19 ENUMERATED {supported} OPTIONAL,

delayStatusReportNonDelayReportingData-r19 ENUMERATED {supported} OPTIONAL

]]

}

MAC-ParametersFRX-Diff-r16 ::= SEQUENCE {

directMCG-SCellActivation-r16 ENUMERATED {supported} OPTIONAL,

directMCG-SCellActivationResume-r16 ENUMERATED {supported} OPTIONAL,

directSCG-SCellActivation-r16 ENUMERATED {supported} OPTIONAL,

directSCG-SCellActivationResume-r16 ENUMERATED {supported} OPTIONAL,

-- R1 19-1: DRX Adaptation

drx-Adaptation-r16 SEQUENCE {

non-SharedSpectrumChAccess-r16 MinTimeGap-r16 OPTIONAL,

sharedSpectrumChAccess-r16 MinTimeGap-r16 OPTIONAL

} OPTIONAL,

...

}

MAC-ParametersFR2-2-r17 ::= SEQUENCE {

directMCG-SCellActivation-r17 ENUMERATED {supported} OPTIONAL,

directMCG-SCellActivationResume-r17 ENUMERATED {supported} OPTIONAL,

directSCG-SCellActivation-r17 ENUMERATED {supported} OPTIONAL,

directSCG-SCellActivationResume-r17 ENUMERATED {supported} OPTIONAL,

drx-Adaptation-r17 SEQUENCE {

non-SharedSpectrumChAccess-r17 MinTimeGapFR2-2-r17 OPTIONAL,

sharedSpectrumChAccess-r17 MinTimeGapFR2-2-r17 OPTIONAL

} OPTIONAL,

...

}

MAC-ParametersXDD-Diff ::= SEQUENCE {

skipUplinkTxDynamic ENUMERATED {supported} OPTIONAL,

logicalChannelSR-DelayTimer ENUMERATED {supported} OPTIONAL,

longDRX-Cycle ENUMERATED {supported} OPTIONAL,

shortDRX-Cycle ENUMERATED {supported} OPTIONAL,

multipleSR-Configurations ENUMERATED {supported} OPTIONAL,

multipleConfiguredGrants ENUMERATED {supported} OPTIONAL,

...,

[[

secondaryDRX-Group-r16 ENUMERATED {supported} OPTIONAL

]],

[[

enhancedSkipUplinkTxDynamic-r16 ENUMERATED {supported} OPTIONAL,

enhancedSkipUplinkTxConfigured-r16 ENUMERATED {supported} OPTIONAL

]],

[[

dummy1 ENUMERATED {supported} OPTIONAL,

dummy2 ENUMERATED {supported} OPTIONAL

]]

}

MinTimeGap-r16 ::= SEQUENCE {

scs-15kHz-r16 ENUMERATED {sl1, sl3} OPTIONAL,

scs-30kHz-r16 ENUMERATED {sl1, sl6} OPTIONAL,

scs-60kHz-r16 ENUMERATED {sl1, sl12} OPTIONAL,

scs-120kHz-r16 ENUMERATED {sl2, sl24} OPTIONAL

}

MinTimeGapFR2-2-r17 ::= SEQUENCE {

scs-120kHz-r17 ENUMERATED {sl2, sl24} OPTIONAL,

scs-480kHz-r17 ENUMERATED {sl8, sl96} OPTIONAL,

scs-960kHz-r17 ENUMERATED {sl16, sl192} OPTIONAL

}

MAC-ParametersPerBand-r18 ::= SEQUENCE {

ptm-Retransmission-r18 ENUMERATED {supported} OPTIONAL,

ptm-RetransmissionInactive-r18 ENUMERATED {supported} OPTIONAL,

...

}

-- TAG-MAC-PARAMETERS-STOP

-- ASN1STOP

#### – *MeasAndMobParameters*

The IE *MeasAndMobParameters* is used to convey UE capabilities related to measurements for radio resource management (RRM), radio link monitoring (RLM) and mobility (e.g. handover).

*MeasAndMobParameters* information element

-- ASN1START

-- TAG-MEASANDMOBPARAMETERS-START

MeasAndMobParameters ::= SEQUENCE {

measAndMobParametersCommon MeasAndMobParametersCommon OPTIONAL,

measAndMobParametersXDD-Diff MeasAndMobParametersXDD-Diff OPTIONAL,

measAndMobParametersFRX-Diff MeasAndMobParametersFRX-Diff OPTIONAL

}

MeasAndMobParameters-v15t0 ::= SEQUENCE {

measAndMobParametersCommon-v15t0 MeasAndMobParametersCommon-v15t0 OPTIONAL

}

MeasAndMobParameters-v1700 ::= SEQUENCE {

measAndMobParametersFR2-2-r17 MeasAndMobParametersFR2-2-r17 OPTIONAL

}

MeasAndMobParametersCommon ::= SEQUENCE {

supportedGapPattern BIT STRING (SIZE (22)) OPTIONAL,

ssb-RLM ENUMERATED {supported} OPTIONAL,

ssb-AndCSI-RS-RLM ENUMERATED {supported} OPTIONAL,

...,

[[

eventB-MeasAndReport ENUMERATED {supported} OPTIONAL,

handoverFDD-TDD ENUMERATED {supported} OPTIONAL,

eutra-CGI-Reporting ENUMERATED {supported} OPTIONAL,

nr-CGI-Reporting ENUMERATED {supported} OPTIONAL

]],

[[

independentGapConfig ENUMERATED {supported} OPTIONAL,

periodicEUTRA-MeasAndReport ENUMERATED {supported} OPTIONAL,

handoverFR1-FR2 ENUMERATED {supported} OPTIONAL,

maxNumberCSI-RS-RRM-RS-SINR ENUMERATED {n4, n8, n16, n32, n64, n96} OPTIONAL

]],

[[

nr-CGI-Reporting-ENDC ENUMERATED {supported} OPTIONAL

]],

[[

eutra-CGI-Reporting-NEDC ENUMERATED {supported} OPTIONAL,

eutra-CGI-Reporting-NRDC ENUMERATED {supported} OPTIONAL,

nr-CGI-Reporting-NEDC ENUMERATED {supported} OPTIONAL,

nr-CGI-Reporting-NRDC ENUMERATED {supported} OPTIONAL

]],

[[

reportAddNeighMeasForPeriodic-r16 ENUMERATED {supported} OPTIONAL,

condHandoverParametersCommon-r16 SEQUENCE {

condHandoverFDD-TDD-r16 ENUMERATED {supported} OPTIONAL,

condHandoverFR1-FR2-r16 ENUMERATED {supported} OPTIONAL

} OPTIONAL,

nr-NeedForGap-Reporting-r16 ENUMERATED {supported} OPTIONAL,

supportedGapPattern-NRonly-r16 BIT STRING (SIZE (10)) OPTIONAL,

supportedGapPattern-NRonly-NEDC-r16 ENUMERATED {supported} OPTIONAL,

maxNumberCLI-RSSI-r16 ENUMERATED {n8, n16, n32, n64} OPTIONAL,

maxNumberCLI-SRS-RSRP-r16 ENUMERATED {n4, n8, n16, n32} OPTIONAL,

maxNumberPerSlotCLI-SRS-RSRP-r16 ENUMERATED {n2, n4, n8} OPTIONAL,

mfbi-IAB-r16 ENUMERATED {supported} OPTIONAL,

dummy ENUMERATED {supported} OPTIONAL,

nr-CGI-Reporting-NPN-r16 ENUMERATED {supported} OPTIONAL,

idleInactiveEUTRA-MeasReport-r16 ENUMERATED {supported} OPTIONAL,

idleInactive-ValidityArea-r16 ENUMERATED {supported} OPTIONAL,

eutra-AutonomousGaps-r16 ENUMERATED {supported} OPTIONAL,

eutra-AutonomousGaps-NEDC-r16 ENUMERATED {supported} OPTIONAL,

eutra-AutonomousGaps-NRDC-r16 ENUMERATED {supported} OPTIONAL,

pcellT312-r16 ENUMERATED {supported} OPTIONAL,

supportedGapPattern-r16 BIT STRING (SIZE (2)) OPTIONAL

]],

[[

-- R4 19-2 Concurrent measurement gaps

concurrentMeasGap-r17 CHOICE {

concurrentPerUE-OnlyMeasGap-r17 ENUMERATED {supported},

concurrentPerUE-PerFRCombMeasGap-r17 ENUMERATED {supported}

} OPTIONAL,

-- R4 19-1 Network controlled small gap (NCSG)

nr-NeedForGapNCSG-Reporting-r17 ENUMERATED {supported} OPTIONAL,

eutra-NeedForGapNCSG-Reporting-r17 ENUMERATED {supported} OPTIONAL,

-- R4 19-1-1 per FR Network controlled small gap (NCSG)

ncsg-MeasGapPerFR-r17 ENUMERATED {supported} OPTIONAL,

-- R4 19-1-2 Network controlled small gap (NCSG) supported patterns

ncsg-MeasGapPatterns-r17 BIT STRING (SIZE(24)) OPTIONAL,

-- R4 19-1-3 Network controlled small gap (NCSG) supported NR-only patterns

ncsg-MeasGapNR-Patterns-r17 BIT STRING (SIZE(24)) OPTIONAL,

-- R4 19-3-2 pre-configured measurement gap

preconfiguredUE-AutonomousMeasGap-r17 ENUMERATED {supported} OPTIONAL,

-- R4 19-3-1 pre-configured measurement gap

preconfiguredNW-ControlledMeasGap-r17 ENUMERATED {supported} OPTIONAL,

handoverFR1-FR2-2-r17 ENUMERATED {supported} OPTIONAL,

handoverFR2-1-FR2-2-r17 ENUMERATED {supported} OPTIONAL,

-- RAN4 14-1: per-FR MG for PRS measurement

independentGapConfigPRS-r17 ENUMERATED {supported} OPTIONAL,

rrm-RelaxationRRC-ConnectedRedCap-r17 ENUMERATED {supported} OPTIONAL,

-- R4 25-3: Parallel measurements with multiple measurement gaps

parallelMeasurementGap-r17 ENUMERATED {n2} OPTIONAL,

condHandoverWithSCG-NRDC-r17 ENUMERATED {supported} OPTIONAL,

gNB-ID-LengthReporting-r17 ENUMERATED {supported} OPTIONAL,

gNB-ID-LengthReporting-ENDC-r17 ENUMERATED {supported} OPTIONAL,

gNB-ID-LengthReporting-NEDC-r17 ENUMERATED {supported} OPTIONAL,

gNB-ID-LengthReporting-NRDC-r17 ENUMERATED {supported} OPTIONAL,

gNB-ID-LengthReporting-NPN-r17 ENUMERATED {supported} OPTIONAL

]],

[[

-- R4 25-1: Parallel measurements on multiple SMTC-s for a single frequency carrier

parallelSMTC-r17 ENUMERATED {n4} OPTIONAL,

-- R4 19-2-1 Concurrent measurement gaps for EUTRA

concurrentMeasGapEUTRA-r17 ENUMERATED {supported} OPTIONAL,

serviceLinkPropDelayDiffReporting-r17 ENUMERATED {supported} OPTIONAL,

-- R4 19-1-4 Network controlled small gap (NCSG) performing measurement based on flag deriveSSB-IndexFromCellInter

ncsg-SymbolLevelScheduleRestrictionInter-r17 ENUMERATED {supported} OPTIONAL

]],

[[

eventD1-MeasReportTrigger-r17 ENUMERATED {supported} OPTIONAL,

independentGapConfig-maxCC-r17 SEQUENCE {

fr1-Only-r17 INTEGER (1..32) OPTIONAL,

fr2-Only-r17 INTEGER (1..32) OPTIONAL,

fr1-AndFR2-r17 INTEGER (1..32) OPTIONAL

} OPTIONAL

]],

[[

interSatMeas-r17 ENUMERATED {supported} OPTIONAL,

deriveSSB-IndexFromCellInterNon-NCSG-r17 ENUMERATED {supported} OPTIONAL

]],

[[

-- R4 31-1 Enhanced L3 measurement reporting for unknown SCell activation if the valid L3 measurement results are available

l3-MeasUnknownSCellActivation-r18 ENUMERATED {supported} OPTIONAL,

-- R4 31-3 Shorter measurement interval for unknown SCell activation

shortMeasInterval-r18 ENUMERATED {supported} OPTIONAL,

nr-NeedForInterruptionReport-r18 ENUMERATED {supported} OPTIONAL,

measSequenceConfig-r18 ENUMERATED {supported} OPTIONAL,

cellIndividualOffsetPerMeasEvent-r18 ENUMERATED {supported} OPTIONAL,

eventD2-MeasReportTrigger-r18 ENUMERATED {supported} OPTIONAL,

-- R4 32-1: Concurrent gaps with Pre-MG in a FR

concurrentMeasGapsPreMG-r18 ENUMERATED {supported} OPTIONAL,

-- R4 32-2: Support for dynamic collisions

dynamicCollision-r18 ENUMERATED {supported} OPTIONAL,

-- R4 32-3: Concurrent gaps with NCSG in a FR

concurrentMeasGapsNCSG-r18 ENUMERATED {supported} OPTIONAL,

-- R4 32-4: Inter-RAT EUTRAN measurements without gap and outside active DL BWP

eutra-NoGapMeasurementOutsideBWP-r18 ENUMERATED {supported} OPTIONAL,

-- R4 32-5: Inter-RAT EUTRAN measurement without gap and within active DL BWP

eutra-NoGapMeasurementInsideBWP-r18 ENUMERATED {supported} OPTIONAL,

-- R4 32-6: Effective measurement window for inter-RAT EUTRAN measurements

eutra-MeasEMW-r18 BIT STRING (SIZE(6)) OPTIONAL,

-- R4 32-7: Simultaneous reception of NR data and EUTRAN CRS with different numerology

concurrentMeasCRS-InsideBWP-EUTRA-r18 ENUMERATED {supported} OPTIONAL,

-- R4 39-2a: SSB based inter-frequency L1-RSRP measurements with measurement gaps

ltm-InterFreqMeasGap-r18 ENUMERATED {supported} OPTIONAL,

dummy-ltm-FastUE-Processing-r18 SEQUENCE {

fr1-r18 ENUMERATED {ms10, ms15},

fr2-r18 ENUMERATED {ms10, ms15},

fr1-AndFR2-r18 ENUMERATED {ms20, ms30}

} OPTIONAL,

rach-LessHandoverInterFreq-r18 ENUMERATED {supported} OPTIONAL,

enterAndLeaveCellReport-r18 ENUMERATED {supported} OPTIONAL,

bestCellChangeReport-r18 ENUMERATED {supported} OPTIONAL,

secondBestCellChangeReport-r18 ENUMERATED {supported} OPTIONAL

]],

[[

ltm-InterFreq-r18 ENUMERATED {supported} OPTIONAL,

ltm-MCG-NRDC-r18 ENUMERATED {supported} OPTIONAL,

ltm-RACH-LessDG-r18 ENUMERATED {supported} OPTIONAL,

ltm-RACH-LessCG-r18 ENUMERATED {supported} OPTIONAL,

ltm-Recovery-r18 ENUMERATED {supported} OPTIONAL,

ltm-ReferenceConfig-r18 ENUMERATED {supported} OPTIONAL,

ltm-MCG-NRDC-Release-r18 ENUMERATED {supported} OPTIONAL,

-- R4 39-7: Faster UE processing time during cell switch

ltm-FastUE-Processing-r18 SEQUENCE {

fr1-r18 ENUMERATED {ms10, ms15} OPTIONAL,

fr2-r18 ENUMERATED {ms10, ms15} OPTIONAL,

fr1-AndFR2-r18 ENUMERATED {ms20, ms30} OPTIONAL

} OPTIONAL,

ntn-NeighbourCellInfoSupport-r18 ENUMERATED {supported} OPTIONAL

]],

[[

ltm-interFreqL1-OnlyInBC-r18 ENUMERATED {supported} OPTIONAL

]],

[[

ltm-KeyUpdateMCG-r19 ENUMERATED {supported} OPTIONAL,

ltm-KeyUpdateSCG-r19 ENUMERATED {supported} OPTIONAL,

cltm-EarlyTA-Indication-r19 INTEGER (1..8) OPTIONAL,

cltm-ExecutionConditionL1-r19 ENUMERATED {supported} OPTIONAL,

cltm-ExecutionConditionL3-r19 INTEGER (1..2) OPTIONAL,

ltm-EventMeasAndReport-r19 ENUMERATED {supported} OPTIONAL,

ltm-RecoveryWithKeyUpdate-r19 ENUMERATED {supported} OPTIONAL,

-- R4 49-1: Simultaneous L3 measurement on three carriers for measurements without measurement gap under CA/DC operation

threeCarrierMeasWithoutGap-r19 SEQUENCE {

fr1-CA-NR-DC-r19 ENUMERATED {supported} OPTIONAL,

fr1-FR2-CA-r19 ENUMERATED {supported} OPTIONAL,

fr1-FR2-NR-DC-r19 ENUMERATED {supported} OPTIONAL

} OPTIONAL,

-- R4 49-3: L3 serving cell and neighbor cells measurement and report on one serving carrier per-band for

-- intra-frequency measurements without measurement gap

multiCarrierSingleReportWithoutGap-r19 ENUMERATED {supported} OPTIONAL,

-- R4 52-3: Skip SSB based L1-RSRP measurement for candidate cell CSI-RS-based L1-RSRP measurement

skipSSB-L1-RSRP-Meas-r19 ENUMERATED {neighbour, both} OPTIONAL,

gapOccasionCancelRatioReport-r19 ENUMERATED {supported} OPTIONAL,

twoSMTC-Periodicities-r19 ENUMERATED {supported} OPTIONAL,

reportClosestReferenceLocations-r19 ENUMERATED {supported} OPTIONAL

]]

}

MeasAndMobParametersCommon-v15t0 ::= SEQUENCE {

intraF-NeighMeasForSCellWithoutSSB ENUMERATED{supported} OPTIONAL

}

MeasAndMobParametersXDD-Diff ::= SEQUENCE {

intraAndInterF-MeasAndReport ENUMERATED {supported} OPTIONAL,

eventA-MeasAndReport ENUMERATED {supported} OPTIONAL,

...,

[[

handoverInterF ENUMERATED {supported} OPTIONAL,

handoverLTE-EPC ENUMERATED {supported} OPTIONAL,

handoverLTE-5GC ENUMERATED {supported} OPTIONAL

]],

[[

sftd-MeasNR-Neigh ENUMERATED {supported} OPTIONAL,

sftd-MeasNR-Neigh-DRX ENUMERATED {supported} OPTIONAL

]],

[[

dummy ENUMERATED {supported} OPTIONAL

]]

}

MeasAndMobParametersFRX-Diff ::= SEQUENCE {

ss-SINR-Meas ENUMERATED {supported} OPTIONAL,

csi-RSRP-AndRSRQ-MeasWithSSB ENUMERATED {supported} OPTIONAL,

csi-RSRP-AndRSRQ-MeasWithoutSSB ENUMERATED {supported} OPTIONAL,

csi-SINR-Meas ENUMERATED {supported} OPTIONAL,

csi-RS-RLM ENUMERATED {supported} OPTIONAL,

...,

[[

handoverInterF ENUMERATED {supported} OPTIONAL,

handoverLTE-EPC ENUMERATED {supported} OPTIONAL,

handoverLTE-5GC ENUMERATED {supported} OPTIONAL

]],

[[

maxNumberResource-CSI-RS-RLM ENUMERATED {n2, n4, n6, n8} OPTIONAL

]],

[[

simultaneousRxDataSSB-DiffNumerology ENUMERATED {supported} OPTIONAL

]],

[[

nr-AutonomousGaps-r16 ENUMERATED {supported} OPTIONAL,

nr-AutonomousGaps-ENDC-r16 ENUMERATED {supported} OPTIONAL,

nr-AutonomousGaps-NEDC-r16 ENUMERATED {supported} OPTIONAL,

nr-AutonomousGaps-NRDC-r16 ENUMERATED {supported} OPTIONAL,

dummy ENUMERATED {supported} OPTIONAL,

cli-RSSI-Meas-r16 ENUMERATED {supported} OPTIONAL,

cli-SRS-RSRP-Meas-r16 ENUMERATED {supported} OPTIONAL,

interFrequencyMeas-NoGap-r16 ENUMERATED {supported} OPTIONAL,

simultaneousRxDataSSB-DiffNumerology-Inter-r16 ENUMERATED {supported} OPTIONAL,

idleInactiveNR-MeasReport-r16 ENUMERATED {supported} OPTIONAL,

-- R4 6-2: Support of beam level Early Measurement Reporting

idleInactiveNR-MeasBeamReport-r16 ENUMERATED {supported} OPTIONAL

]],

[[

increasedNumberofCSIRSPerMO-r16 ENUMERATED {supported} OPTIONAL

]]

}

MeasAndMobParametersFR2-2-r17 ::= SEQUENCE {

handoverInterF-r17 ENUMERATED {supported} OPTIONAL,

handoverLTE-EPC-r17 ENUMERATED {supported} OPTIONAL,

handoverLTE-5GC-r17 ENUMERATED {supported} OPTIONAL,

idleInactiveNR-MeasReport-r17 ENUMERATED {supported} OPTIONAL,

...

}

-- TAG-MEASANDMOBPARAMETERS-STOP

-- ASN1STOP

#### – *MeasAndMobParametersMRDC*

The IE *MeasAndMobParametersMRDC* is used to convey capability parameters related to RRM measurements and RRC mobility.

*MeasAndMobParametersMRDC* information element

-- ASN1START

-- TAG-MEASANDMOBPARAMETERSMRDC-START

MeasAndMobParametersMRDC ::= SEQUENCE {

measAndMobParametersMRDC-Common MeasAndMobParametersMRDC-Common OPTIONAL,

measAndMobParametersMRDC-XDD-Diff MeasAndMobParametersMRDC-XDD-Diff OPTIONAL,

measAndMobParametersMRDC-FRX-Diff MeasAndMobParametersMRDC-FRX-Diff OPTIONAL

}

MeasAndMobParametersMRDC-v1560 ::= SEQUENCE {

measAndMobParametersMRDC-XDD-Diff-v1560 MeasAndMobParametersMRDC-XDD-Diff-v1560 OPTIONAL

}

MeasAndMobParametersMRDC-v1610 ::= SEQUENCE {

measAndMobParametersMRDC-Common-v1610 MeasAndMobParametersMRDC-Common-v1610 OPTIONAL,

interNR-MeasEUTRA-IAB-r16 ENUMERATED {supported} OPTIONAL

}

MeasAndMobParametersMRDC-v1700 ::= SEQUENCE {

measAndMobParametersMRDC-Common-v1700 MeasAndMobParametersMRDC-Common-v1700 OPTIONAL

}

MeasAndMobParametersMRDC-v1730 ::= SEQUENCE {

measAndMobParametersMRDC-Common-v1730 MeasAndMobParametersMRDC-Common-v1730 OPTIONAL

}

MeasAndMobParametersMRDC-v1810 ::= SEQUENCE {

measAndMobParametersMRDC-Common-v1810 MeasAndMobParametersMRDC-Common-v1810 OPTIONAL

}

MeasAndMobParametersMRDC-v1900 ::= SEQUENCE {

measAndMobParametersMRDC-Common-v1900 MeasAndMobParametersMRDC-Common-v1900 OPTIONAL

}

MeasAndMobParametersMRDC-Common ::= SEQUENCE {

independentGapConfig ENUMERATED {supported} OPTIONAL

}

MeasAndMobParametersMRDC-Common-v1610 ::= SEQUENCE {

condPSCellChangeParametersCommon-r16 SEQUENCE {

condPSCellChangeFDD-TDD-r16 ENUMERATED {supported} OPTIONAL,

condPSCellChangeFR1-FR2-r16 ENUMERATED {supported} OPTIONAL

} OPTIONAL,

pscellT312-r16 ENUMERATED {supported} OPTIONAL

}

MeasAndMobParametersMRDC-Common-v1700 ::= SEQUENCE {

condPSCellChangeParameters-r17 SEQUENCE {

inter-SN-condPSCellChangeFDD-TDD-NRDC-r17 ENUMERATED {supported} OPTIONAL,

inter-SN-condPSCellChangeFR1-FR2-NRDC-r17 ENUMERATED {supported} OPTIONAL,

inter-SN-condPSCellChangeFDD-TDD-ENDC-r17 ENUMERATED {supported} OPTIONAL,

inter-SN-condPSCellChangeFR1-FR2-ENDC-r17 ENUMERATED {supported} OPTIONAL,

mn-InitiatedCondPSCellChange-FR1FDD-ENDC-r17 ENUMERATED {supported} OPTIONAL,

mn-InitiatedCondPSCellChange-FR1TDD-ENDC-r17 ENUMERATED {supported} OPTIONAL,

mn-InitiatedCondPSCellChange-FR2TDD-ENDC-r17 ENUMERATED {supported} OPTIONAL,

sn-InitiatedCondPSCellChange-FR1FDD-ENDC-r17 ENUMERATED {supported} OPTIONAL,

sn-InitiatedCondPSCellChange-FR1TDD-ENDC-r17 ENUMERATED {supported} OPTIONAL,

sn-InitiatedCondPSCellChange-FR2TDD-ENDC-r17 ENUMERATED {supported} OPTIONAL

} OPTIONAL,

condHandoverWithSCG-ENDC-r17 ENUMERATED {supported} OPTIONAL,

condHandoverWithSCG-NEDC-r17 ENUMERATED {supported} OPTIONAL

}

MeasAndMobParametersMRDC-Common-v1730 ::= SEQUENCE {

independentGapConfig-maxCC-r17 SEQUENCE {

fr1-Only-r17 INTEGER (1..32) OPTIONAL,

fr2-Only-r17 INTEGER (1..32) OPTIONAL,

fr1-AndFR2-r17 INTEGER (1..32) OPTIONAL

}

}

MeasAndMobParametersMRDC-Common-v1810 ::= SEQUENCE {

mn-ConfiguredMN-TriggerSCPAC-r18 ENUMERATED {supported} OPTIONAL,

mn-ConfiguredSN-TriggerSCPAC-r18 ENUMERATED {supported} OPTIONAL,

sn-ConfiguredSCPAC-r18 ENUMERATED {supported} OPTIONAL,

mn-ConfiguredMN-TriggerSCPAC-afterSCG-release-r18 ENUMERATED {supported} OPTIONAL,

mn-ConfiguredReferenceConfigSCPAC-r18 ENUMERATED {supported} OPTIONAL,

sn-ConfiguredReferenceConfigSCPAC-r18 ENUMERATED {supported} OPTIONAL,

condHandoverWithCandSCG-Addition-r18 ENUMERATED {supported} OPTIONAL,

condHandoverWithCandSCG-FR1-FR2-Change-r18 ENUMERATED {supported} OPTIONAL,

condHandoverWithCandSCG-FDD-TDD-Change-r18 ENUMERATED {supported} OPTIONAL

}

MeasAndMobParametersMRDC-Common-v1900 ::= SEQUENCE {

-- R4 49-1: Simultaneous L3 measurement on three carriers for measurements without measurement gap under CA/DC operation

threeCarrierMeasWithoutGap-r19 ENUMERATED {supported} OPTIONAL

}

MeasAndMobParametersMRDC-XDD-Diff ::= SEQUENCE {

sftd-MeasPSCell ENUMERATED {supported} OPTIONAL,

sftd-MeasNR-Cell ENUMERATED {supported} OPTIONAL

}

MeasAndMobParametersMRDC-XDD-Diff-v1560 ::= SEQUENCE {

sftd-MeasPSCell-NEDC ENUMERATED {supported} OPTIONAL

}

MeasAndMobParametersMRDC-FRX-Diff ::= SEQUENCE {

simultaneousRxDataSSB-DiffNumerology ENUMERATED {supported} OPTIONAL

}

-- TAG-MEASANDMOBPARAMETERSMRDC-STOP

-- ASN1STOP

#### – *MIMO-Layers*

The IE *MIMO-Layers* is used to convey the number of supported MIMO layers.

*MIMO-Layers* information element

-- ASN1START

-- TAG-MIMO-LAYERS-START

MIMO-LayersDL ::= ENUMERATED {twoLayers, fourLayers, eightLayers}

MIMO-LayersUL ::= ENUMERATED {oneLayer, twoLayers, fourLayers}

-- TAG-MIMO-LAYERS-STOP

-- ASN1STOP

#### – *MIMO-ParametersPerBand*

The IE *MIMO-ParametersPerBand* is used to convey MIMO related parameters specific for a certain band (not per feature set or band combination).

*MIMO-ParametersPerBand* information element

-- ASN1START

-- TAG-MIMO-PARAMETERSPERBAND-START

MIMO-ParametersPerBand ::= SEQUENCE {

tci-StatePDSCH SEQUENCE {

maxNumberConfiguredTCI-StatesPerCC ENUMERATED {n4, n8, n16, n32, n64, n128} OPTIONAL,

maxNumberActiveTCI-PerBWP ENUMERATED {n1, n2, n4, n8} OPTIONAL

} OPTIONAL,

additionalActiveTCI-StatePDCCH ENUMERATED {supported} OPTIONAL,

pusch-TransCoherence ENUMERATED {nonCoherent, partialCoherent, fullCoherent} OPTIONAL,

beamCorrespondenceWithoutUL-BeamSweeping ENUMERATED {supported} OPTIONAL,

periodicBeamReport ENUMERATED {supported} OPTIONAL,

aperiodicBeamReport ENUMERATED {supported} OPTIONAL,

sp-BeamReportPUCCH ENUMERATED {supported} OPTIONAL,

sp-BeamReportPUSCH ENUMERATED {supported} OPTIONAL,

dummy1 DummyG OPTIONAL,

maxNumberRxBeam INTEGER (2..8) OPTIONAL,

maxNumberRxTxBeamSwitchDL SEQUENCE {

scs-15kHz ENUMERATED {n4, n7, n14} OPTIONAL,

scs-30kHz ENUMERATED {n4, n7, n14} OPTIONAL,

scs-60kHz ENUMERATED {n4, n7, n14} OPTIONAL,

scs-120kHz ENUMERATED {n4, n7, n14} OPTIONAL,

scs-240kHz ENUMERATED {n4, n7, n14} OPTIONAL

} OPTIONAL,

maxNumberNonGroupBeamReporting ENUMERATED {n1, n2, n4} OPTIONAL,

groupBeamReporting ENUMERATED {supported} OPTIONAL,

uplinkBeamManagement SEQUENCE {

maxNumberSRS-ResourcePerSet-BM ENUMERATED {n2, n4, n8, n16},

maxNumberSRS-ResourceSet INTEGER (1..8)

} OPTIONAL,

maxNumberCSI-RS-BFD INTEGER (1..64) OPTIONAL,

maxNumberSSB-BFD INTEGER (1..64) OPTIONAL,

maxNumberCSI-RS-SSB-CBD INTEGER (1..256) OPTIONAL,

dummy2 ENUMERATED {supported} OPTIONAL,

twoPortsPTRS-UL ENUMERATED {supported} OPTIONAL,

dummy5 SRS-Resources OPTIONAL,

dummy3 INTEGER (1..4) OPTIONAL,

beamReportTiming SEQUENCE {

scs-15kHz ENUMERATED {sym2, sym4, sym8} OPTIONAL,

scs-30kHz ENUMERATED {sym4, sym8, sym14, sym28} OPTIONAL,

scs-60kHz ENUMERATED {sym8, sym14, sym28} OPTIONAL,

scs-120kHz ENUMERATED {sym14, sym28, sym56} OPTIONAL

} OPTIONAL,

ptrs-DensityRecommendationSetDL SEQUENCE {

scs-15kHz PTRS-DensityRecommendationDL OPTIONAL,

scs-30kHz PTRS-DensityRecommendationDL OPTIONAL,

scs-60kHz PTRS-DensityRecommendationDL OPTIONAL,

scs-120kHz PTRS-DensityRecommendationDL OPTIONAL

} OPTIONAL,

ptrs-DensityRecommendationSetUL SEQUENCE {

scs-15kHz PTRS-DensityRecommendationUL OPTIONAL,

scs-30kHz PTRS-DensityRecommendationUL OPTIONAL,

scs-60kHz PTRS-DensityRecommendationUL OPTIONAL,

scs-120kHz PTRS-DensityRecommendationUL OPTIONAL

} OPTIONAL,

dummy4 DummyH OPTIONAL,

aperiodicTRS ENUMERATED {supported} OPTIONAL,

...,

[[

dummy6 ENUMERATED {true} OPTIONAL,

beamManagementSSB-CSI-RS BeamManagementSSB-CSI-RS OPTIONAL,

beamSwitchTiming SEQUENCE {

scs-60kHz ENUMERATED {sym14, sym28, sym48, sym224, sym336} OPTIONAL,

scs-120kHz ENUMERATED {sym14, sym28, sym48, sym224, sym336} OPTIONAL

} OPTIONAL,

codebookParameters CodebookParameters OPTIONAL,

csi-RS-IM-ReceptionForFeedback CSI-RS-IM-ReceptionForFeedback OPTIONAL,

csi-RS-ProcFrameworkForSRS CSI-RS-ProcFrameworkForSRS OPTIONAL,

csi-ReportFramework CSI-ReportFramework OPTIONAL,

csi-RS-ForTracking CSI-RS-ForTracking OPTIONAL,

srs-AssocCSI-RS SEQUENCE (SIZE (1.. maxNrofCSI-RS-Resources)) OF SupportedCSI-RS-Resource OPTIONAL,

spatialRelations SpatialRelations OPTIONAL

]],

[[

-- R1 16-2b-0: Support of default QCL assumption with two TCI states

defaultQCL-TwoTCI-r16 ENUMERATED {supported} OPTIONAL,

codebookParametersPerBand-r16 CodebookParameters-v1610 OPTIONAL,

-- R1 16-1b-3: Support of PUCCH resource groups per BWP for simultaneous spatial relation update

simul-SpatialRelationUpdatePUCCHResGroup-r16 ENUMERATED {supported} OPTIONAL,

-- R1 16-1f: Maximum number of SCells configured for SCell beam failure recovery simultaneously

maxNumberSCellBFR-r16 ENUMERATED {n1,n2,n4,n8} OPTIONAL,

-- R1 16-2c: Supports simultaneous reception with different Type-D for FR2 only

simultaneousReceptionDiffTypeD-r16 ENUMERATED {supported} OPTIONAL,

-- R1 16-1a-1: SSB/CSI-RS for L1-SINR measurement

ssb-csirs-SINR-measurement-r16 SEQUENCE {

maxNumberSSB-CSIRS-OneTx-CMR-r16 ENUMERATED {n8, n16, n32, n64},

maxNumberCSI-IM-NZP-IMR-res-r16 ENUMERATED {n8, n16, n32, n64},

maxNumberCSIRS-2Tx-res-r16 ENUMERATED {n0, n4, n8, n16, n32, n64},

maxNumberSSB-CSIRS-res-r16 ENUMERATED {n8, n16, n32, n64, n128},

maxNumberCSI-IM-NZP-IMR-res-mem-r16 ENUMERATED {n8, n16, n32, n64, n128},

supportedCSI-RS-Density-CMR-r16 ENUMERATED {one, three, oneAndThree},

maxNumberAperiodicCSI-RS-Res-r16 ENUMERATED {n2, n4, n8, n16, n32, n64},

supportedSINR-meas-r16 ENUMERATED {ssbWithCSI-IM, ssbWithNZP-IMR, csirsWithNZP-IMR, csi-RSWithoutIMR} OPTIONAL

} OPTIONAL,

-- R1 16-1a-2: Non-group based L1-SINR reporting

nonGroupSINR-reporting-r16 ENUMERATED {n1, n2, n4} OPTIONAL,

-- R1 16-1a-3: Non-group based L1-SINR reporting

groupSINR-reporting-r16 ENUMERATED {supported} OPTIONAL,

multiDCI-multiTRP-Parameters-r16 SEQUENCE {

-- R1 16-2a-0: Overlapping PDSCHs in time and fully overlapping in frequency and time

overlapPDSCHsFullyFreqTime-r16 INTEGER (1..2) OPTIONAL,

-- R1 16-2a-1: Overlapping PDSCHs in time and partially overlapping in frequency and time

overlapPDSCHsInTimePartiallyFreq-r16 ENUMERATED {supported} OPTIONAL,

-- R1 16-2a-2: Out of order operation for DL

outOfOrderOperationDL-r16 SEQUENCE {

supportPDCCH-ToPDSCH-r16 ENUMERATED {supported} OPTIONAL,

supportPDSCH-ToHARQ-ACK-r16 ENUMERATED {supported} OPTIONAL

} OPTIONAL,

-- R1 16-2a-3: Out of order operation for UL

outOfOrderOperationUL-r16 ENUMERATED {supported} OPTIONAL,

-- R1 16-2a-5: Separate CRS rate matching

separateCRS-RateMatching-r16 ENUMERATED {supported} OPTIONAL,

-- R1 16-2a-6: Default QCL enhancement for multi-DCI based multi-TRP

defaultQCL-PerCORESETPoolIndex-r16 ENUMERATED {supported} OPTIONAL,

-- R1 16-2a-7: Maximum number of activated TCI states

maxNumberActivatedTCI-States-r16 SEQUENCE {

maxNumberPerCORESET-Pool-r16 ENUMERATED {n1, n2, n4, n8},

maxTotalNumberAcrossCORESET-Pool-r16 ENUMERATED {n2, n4, n8, n16}

} OPTIONAL

} OPTIONAL,

singleDCI-SDM-scheme-Parameters-r16 SEQUENCE {

-- R1 16-2b-1b: Single-DCI based SDM scheme - Support of new DMRS port entry

supportNewDMRS-Port-r16 ENUMERATED {supported1, supported2, supported3} OPTIONAL,

-- R1 16-2b-1a: Support of s-port DL PTRS

supportTwoPortDL-PTRS-r16 ENUMERATED {supported} OPTIONAL

} OPTIONAL,

-- R1 16-2b-2: Support of single-DCI based FDMSchemeA

supportFDM-SchemeA-r16 ENUMERATED {supported} OPTIONAL,

-- R1 16-2b-3a: Single-DCI based FDMSchemeB CW soft combining

supportCodeWordSoftCombining-r16 ENUMERATED {supported} OPTIONAL,

-- R1 16-2b-4: Single-DCI based TDMSchemeA

supportTDM-SchemeA-r16 ENUMERATED {kb3, kb5, kb10, kb20, noRestriction} OPTIONAL,

-- R1 16-2b-5: Single-DCI based inter-slot TDM

supportInter-slotTDM-r16 SEQUENCE {

supportRepNumPDSCH-TDRA-r16 ENUMERATED {n2, n3, n4, n5, n6, n7, n8, n16},

maxTBS-Size-r16 ENUMERATED {kb3, kb5, kb10, kb20, noRestriction},

maxNumberTCI-states-r16 INTEGER (1..2)

} OPTIONAL,

-- R1 16-4: Low PAPR DMRS for PDSCH

lowPAPR-DMRS-PDSCH-r16 ENUMERATED {supported} OPTIONAL,

-- R1 16-6a: Low PAPR DMRS for PUSCH without transform precoding

lowPAPR-DMRS-PUSCHwithoutPrecoding-r16 ENUMERATED {supported} OPTIONAL,

-- R1 16-6b: Low PAPR DMRS for PUCCH

lowPAPR-DMRS-PUCCH-r16 ENUMERATED {supported} OPTIONAL,

-- R1 16-6c: Low PAPR DMRS for PUSCH with transform precoding & pi/2 BPSK

lowPAPR-DMRS-PUSCHwithPrecoding-r16 ENUMERATED {supported} OPTIONAL,

-- R1 16-7: Extension of the maximum number of configured aperiodic CSI report settings

csi-ReportFrameworkExt-r16 CSI-ReportFrameworkExt-r16 OPTIONAL,

-- R1 16-3a, 16-3a-1, 16-3b, 16-3b-1, 16-8: Individual new codebook types

codebookParametersAddition-r16 CodebookParametersAddition-r16 OPTIONAL,

-- R1 16-8: Mixed codebook types

codebookComboParametersAddition-r16 CodebookComboParametersAddition-r16 OPTIONAL,

-- R4 8-2: SSB based beam correspondence

beamCorrespondenceSSB-based-r16 ENUMERATED {supported} OPTIONAL,

-- R4 8-3: CSI-RS based beam correspondence

beamCorrespondenceCSI-RS-based-r16 ENUMERATED {supported} OPTIONAL,

beamSwitchTiming-r16 SEQUENCE {

scs-60kHz-r16 ENUMERATED {sym224, sym336} OPTIONAL,

scs-120kHz-r16 ENUMERATED {sym224, sym336} OPTIONAL

} OPTIONAL

]],

[[

-- R1 16-1a-4: Semi-persistent L1-SINR report on PUCCH

semi-PersistentL1-SINR-Report-PUCCH-r16 SEQUENCE {

supportReportFormat1-2OFDM-syms-r16 ENUMERATED {supported} OPTIONAL,

supportReportFormat4-14OFDM-syms-r16 ENUMERATED {supported} OPTIONAL

} OPTIONAL,

-- R1 16-1a-5: Semi-persistent L1-SINR report on PUSCH

semi-PersistentL1-SINR-Report-PUSCH-r16 ENUMERATED {supported} OPTIONAL

]],

[[

-- R1 16-1h: Support of 64 configured PUCCH spatial relations

spatialRelations-v1640 SEQUENCE {

maxNumberConfiguredSpatialRelations-v1640 ENUMERATED {n96, n128, n160, n192, n224, n256, n288, n320}

} OPTIONAL,

-- R1 16-1i: Support of 64 configured candidate beam RSs for BFR

support64CandidateBeamRS-BFR-r16 ENUMERATED {supported} OPTIONAL

]],

[[

-- R1 16-2a-9: Interpretation of maxNumberMIMO-LayersPDSCH for multi-DCI based mTRP

maxMIMO-LayersForMulti-DCI-mTRP-r16 ENUMERATED {supported} OPTIONAL

]],

[[

supportedSINR-meas-v1670 BIT STRING (SIZE (4)) OPTIONAL

]],

[[

-- R1 23-8-5 Increased repetition for SRS

srs-increasedRepetition-r17 ENUMERATED {supported} OPTIONAL,

-- R1 23-8-6 Partial frequency sounding of SRS

srs-partialFrequencySounding-r17 ENUMERATED {supported} OPTIONAL,

-- R1 23-8-7 Start RB location hopping for partial frequency SRS

srs-startRB-locationHoppingPartial-r17 ENUMERATED {supported} OPTIONAL,

-- R1 23-8-8 Comb-8 SRS

srs-combEight-r17 ENUMERATED {supported} OPTIONAL,

-- R1 23-9-1 Basic Features of Further Enhanced Port-Selection Type II Codebook (FeType-II) per band information

codebookParametersfetype2-r17 CodebookParametersfetype2-r17 OPTIONAL,

-- R1 23-3-1-2a Two associated CSI-RS resources

mTRP-PUSCH-twoCSI-RS-r17 ENUMERATED {supported} OPTIONAL,

-- R1 23-3-2 Multi-TRP PUCCH repetition scheme 1 (inter-slot)

mTRP-PUCCH-InterSlot-r17 ENUMERATED {pf0-2, pf1-3-4, pf0-4} OPTIONAL,

-- R1 23-3-2b Cyclic mapping for multi-TRP PUCCH repetition

mTRP-PUCCH-CyclicMapping-r17 ENUMERATED {supported} OPTIONAL,

-- R1 23-3-2c Second TPC field for multi-TRP PUCCH repetition

mTRP-PUCCH-SecondTPC-r17 ENUMERATED {supported} OPTIONAL,

-- R1 23-5-2 MTRP BFR based on two BFD-RS set

mTRP-BFR-twoBFD-RS-Set-r17 SEQUENCE {

maxBFD-RS-resourcesPerSetPerBWP-r17 ENUMERATED {n1, n2},

maxBFR-r17 INTEGER (1..9),

maxBFD-RS-resourcesAcrossSetsPerBWP-r17 ENUMERATED {n2, n3, n4}

} OPTIONAL,

-- R1 23-5-2a PUCCH-SR resources for MTRP BFRQ - Max number of PUCCH-SR resources for MTRP BFRQ per cell group

mTRP-BFR-PUCCH-SR-perCG-r17 ENUMERATED{n1, n2} OPTIONAL,

-- R1 23-5-2b Association between a BFD-RS resource set on SpCell and a PUCCH SR resource

mTRP-BFR-association-PUCCH-SR-r17 ENUMERATED {supported} OPTIONAL,

-- R1 23-6-3 Simultaneous activation of two TCI states for PDCCH across multiple CCs (HST/URLLC)

sfn-SimulTwoTCI-AcrossMultiCC-r17 ENUMERATED {supported} OPTIONAL,

-- R1 23-6-4 Default DL beam setup for SFN

sfn-DefaultDL-BeamSetup-r17 ENUMERATED {supported} OPTIONAL,

-- R1 23-6-4a Default UL beam setup for SFN PDCCH(FR2 only)

sfn-DefaultUL-BeamSetup-r17 ENUMERATED {supported} OPTIONAL,

-- R1 23-8-1 SRS triggering offset enhancement

srs-TriggeringOffset-r17 ENUMERATED {n1, n2, n4} OPTIONAL,

-- R1 23-8-2 Triggering SRS only in DCI 0\_1/0\_2

srs-TriggeringDCI-r17 ENUMERATED {supported} OPTIONAL,

-- R1 23-9-5 Active CSI-RS resources and ports for mixed codebook types in any slot per band information

codebookComboParameterMixedType-r17 CodebookComboParameterMixedType-r17 OPTIONAL,

-- R1 23-1-1 Unified TCI [with joint DL/UL TCI update] for intra-cell beam management

unifiedJointTCI-r17 SEQUENCE{

maxConfiguredJointTCI-r17 ENUMERATED {n8, n12, n16, n24, n32, n48, n64, n128},

maxActivatedTCIAcrossCC-r17 ENUMERATED {n1, n2, n4, n8, n16}

} OPTIONAL,

-- R1 23-1-1b Unified TCI with joint DL/UL TCI update for intra- and inter-cell beam management with more than one MAC-CE

unifiedJointTCI-multiMAC-CE-r17 SEQUENCE{

minBeamApplicationTime-r17 ENUMERATED {n1, n2, n4, n7, n14, n28, n42, n56, n70, n84, n98, n112, n224, n336}

OPTIONAL,

maxNumMAC-CE-PerCC ENUMERATED {n2, n3, n4, n5, n6, n7, n8}

} OPTIONAL,

-- R1 23-1-1d Per BWP TCI state pool configuration for CA mode

unifiedJointTCI-perBWP-CA-r17 ENUMERATED {supported} OPTIONAL,

-- R1 23-1-1e TCI state pool configuration with TCI pool sharing for CA mode

unifiedJointTCI-ListSharingCA-r17 ENUMERATED {n1,n2,n4,n8} OPTIONAL,

-- R1 23-1-1f Common multi-CC TCI state ID update and activation

unifiedJointTCI-commonMultiCC-r17 ENUMERATED {supported} OPTIONAL,

-- R1 23-1-1g Beam misalignment between the DL source RS in the TCI state

unifiedJointTCI-BeamAlignDLRS-r17 ENUMERATED {supported} OPTIONAL,

-- R1 23-1-1h Association between TCI state and UL PC settings for PUCCH, PUSCH, and SRS

unifiedJointTCI-PC-association-r17 ENUMERATED {supported} OPTIONAL,

-- R1 23-1-1i Indication/configuration of R17 TCI states for aperiodic CSI-RS, PDCCH, PDSCH

unifiedJointTCI-Legacy-r17 ENUMERATED {supported} OPTIONAL,

-- 23-1-1m Indication/configuration of R17 TCI states for SRS

unifiedJointTCI-Legacy-SRS-r17 ENUMERATED {supported} OPTIONAL,

-- R1 23-1-1j Indication/configuration of R17 TCI states for CORESET #0

unifiedJointTCI-Legacy-CORESET0-r17 ENUMERATED {supported} OPTIONAL,

-- R1 23-1-1c SCell BFR with unified TCI framework (NOTE; pre-requisite is empty)

unifiedJointTCI-SCellBFR-r17 ENUMERATED {supported} OPTIONAL,

-- R1 23-1-1a Unified TCI with joint DL/UL TCI update for inter-cell beam management

unifiedJointTCI-InterCell-r17 SEQUENCE{

additionalMAC-CE-PerCC-r17 ENUMERATED {n0, n1, n2, n4},

additionalMAC-CE-AcrossCC-r17 ENUMERATED {n0, n1, n2, n4}

} OPTIONAL,

-- R1 23-10-1 Unified TCI with separate DL/UL TCI update for intra-cell beam management

unifiedSeparateTCI-r17 SEQUENCE{

maxConfiguredDL-TCI-r17 ENUMERATED {n4, n8, n12, n16, n24, n32, n48, n64, n128},

maxConfiguredUL-TCI-r17 ENUMERATED {n4, n8, n12, n16, n24, n32, n48, n64},

maxActivatedDL-TCIAcrossCC-r17 ENUMERATED {n1, n2, n4, n8, n16},

maxActivatedUL-TCIAcrossCC-r17 ENUMERATED {n1, n2, n4, n8, n16}

} OPTIONAL,

-- R1 23-10-1b Unified TCI with separate DL/UL TCI update for intra-cell beam management with more than one MAC-CE

unifiedSeparateTCI-multiMAC-CE-r17 SEQUENCE{

minBeamApplicationTime-r17 ENUMERATED {n1, n2, n4, n7, n14, n28, n42, n56, n70, n84, n98, n112, n224, n336},

maxActivatedDL-TCIPerCC-r17 INTEGER (2..8),

maxActivatedUL-TCIPerCC-r17 INTEGER (2..8)

} OPTIONAL,

-- R1 23-10-1d Per BWP DL/UL-TCI state pool configuration for CA mode

unifiedSeparateTCI-perBWP-CA-r17 ENUMERATED {supported} OPTIONAL,

-- R1 23-10-1e TCI state pool configuration with DL/UL-TCI pool sharing for CA mode

unifiedSeparateTCI-ListSharingCA-r17 SEQUENCE {

maxNumListDL-TCI-r17 ENUMERATED {n1,n2,n4,n8} OPTIONAL,

maxNumListUL-TCI-r17 ENUMERATED {n1,n2,n4,n8} OPTIONAL

} OPTIONAL,

-- R1 23-10-1f Common multi-CC DL/UL-TCI state ID update and activation with separate DL/UL TCI update

unifiedSeparateTCI-commonMultiCC-r17 ENUMERATED {supported} OPTIONAL,

-- 23-10-1m Unified TCI with separate DL/UL TCI update for inter-cell beam management with more than one MAC-CE

unifiedSeparateTCI-InterCell-r17 SEQUENCE {

k-DL-PerCC-r17 ENUMERATED {n0, n1, n2, n4},

k-UL-PerCC-r17 ENUMERATED {n0, n1, n2, n4},

k-DL-AcrossCC-r17 ENUMERATED {n0, n1, n2, n4},

k-UL-AcrossCC-r17 ENUMERATED {n0, n1, n2, n4}

} OPTIONAL,

-- R1 23-1-2 Inter-cell beam measurement and reporting (for inter-cell BM and mTRP)

unifiedJointTCI-mTRP-InterCell-BM-r17 SEQUENCE {

maxNumAdditionalPCI-L1-RSRP-r17 INTEGER (1..7),

maxNumSSB-ResourceL1-RSRP-AcrossCC-r17 ENUMERATED {n1,n2,n4,n8}

} OPTIONAL,

-- R1 23-1-3 MPE mitigation

mpe-Mitigation-r17 SEQUENCE {

maxNumP-MPR-RI-pairs-r17 INTEGER (1..4),

maxNumConfRS-r17 ENUMERATED {n1, n2, n4, n8, n12, n16, n28, n32, n48, n64}

} OPTIONAL,

-- R1 23-1-4 UE capability value reporting

srs-PortReport-r17 SEQUENCE {

capVal1-r17 ENUMERATED {n1, n2, n4} OPTIONAL,

capVal2-r17 ENUMERATED {n1, n2, n4} OPTIONAL,

capVal3-r17 ENUMERATED {n1, n2, n4} OPTIONAL,

capVal4-r17 ENUMERATED {n1, n2, n4} OPTIONAL

} OPTIONAL,

-- R1 23-2-1a Monitoring of individual candidates

mTRP-PDCCH-individual-r17 ENUMERATED {supported} OPTIONAL,

-- R1 23-2-1b PDCCH repetition with PDCCH monitoring on any span of up to 3 consecutive OFDM symbols of a slot

mTRP-PDCCH-anySpan-3Symbols-r17 ENUMERATED {supported} OPTIONAL,

-- R1 23-2-2 Two QCL TypeD for CORESET monitoring in PDCCH repetition

mTRP-PDCCH-TwoQCL-TypeD-r17 ENUMERATED {supported} OPTIONAL,

-- R1 23-3-1-2b CSI-RS processing framework for SRS with two associated CSI-RS resources

mTRP-PUSCH-CSI-RS-r17 SEQUENCE {

maxNumPeriodicSRS-r17 INTEGER (1..8),

maxNumAperiodicSRS-r17 INTEGER (1..8),

maxNumSP-SRS-r17 INTEGER (0..8),

numSRS-ResourcePerCC-r17 INTEGER (1..16),

numSRS-ResourceNonCodebook-r17 INTEGER (1..2)

} OPTIONAL,

-- R1 23-3-1a Cyclic mapping for Multi-TRP PUSCH repetition

mTRP-PUSCH-cyclicMapping-r17 ENUMERATED {typeA,typeB,both} OPTIONAL,

-- R1 23-3-1b Second TPC field for Multi-TRP PUSCH repetition

mTRP-PUSCH-secondTPC-r17 ENUMERATED {supported} OPTIONAL,

-- R1 23-3-1c Two PHR reporting

mTRP-PUSCH-twoPHR-Reporting-r17 ENUMERATED {supported} OPTIONAL,

-- R1 23-3-1e A-CSI report

mTRP-PUSCH-A-CSI-r17 ENUMERATED {supported} OPTIONAL,

-- R1 23-3-1f SP-CSI report

mTRP-PUSCH-SP-CSI-r17 ENUMERATED {supported} OPTIONAL,

-- R1 23-3-1g CG PUSCH transmission

mTRP-PUSCH-CG-r17 ENUMERATED {supported} OPTIONAL,

-- R1 23-3-2d Updating two Spatial relation or two sets of power control parameters for PUCCH group

mTRP-PUCCH-MAC-CE-r17 ENUMERATED {supported} OPTIONAL,

-- R1 23-3-2e Maximum number of power control parameter sets configured for multi-TRP PUCCH repetition in FR1

mTRP-PUCCH-maxNum-PC-FR1-r17 INTEGER (3..8) OPTIONAL,

-- R1 23-4 IntCell-mTRP

mTRP-inter-Cell-r17 SEQUENCE {

maxNumAdditionalPCI-Case1-r17 INTEGER (1..7),

maxNumAdditionalPCI-Case2-r17 INTEGER (0..7)

} OPTIONAL,

-- R1 23-5-1 Group based L1-RSRP reporting enhancements

mTRP-GroupBasedL1-RSRP-r17 SEQUENCE {

maxNumBeamGroups-r17 INTEGER (1..4),

maxNumRS-WithinSlot-r17 ENUMERATED {n2,n3,n4,n8,n16,n32,n64},

maxNumRS-AcrossSlot-r17 ENUMERATED {n8, n16, n32, n64, n128}

} OPTIONAL,

-- R1 23-5-2c MAC-CE based update of explicit BFD-RS mTRP-PUCCH-IntraSlot-r17 => per band

mTRP-BFD-RS-MAC-CE-r17 ENUMERATED {n4, n8, n12, n16, n32, n48, n64 } OPTIONAL,

-- R1 23-7-1 Basic Features of CSI Enhancement for Multi-TRP

mTRP-CSI-EnhancementPerBand-r17 SEQUENCE {

maxNumNZP-CSI-RS-r17 INTEGER (2..8),

cSI-Report-mode-r17 ENUMERATED {mode1, mode2, both},

supportedComboAcrossCCs-r17 SEQUENCE (SIZE (1..16)) OF CSI-MultiTRP-SupportedCombinations-r17,

codebookModeNCJT-r17 ENUMERATED{mode1,mode1And2}

} OPTIONAL,

-- R1 23-7-1b Active CSI-RS resources and ports in the presence of multi-TRP CSI

codebookComboParameterMultiTRP-r17 CodebookComboParameterMultiTRP-r17 OPTIONAL,

-- R1 23-7-1a Additional CSI report mode 1

mTRP-CSI-additionalCSI-r17 ENUMERATED{x1,x2} OPTIONAL,

-- R1 23-7-4 Support of Nmax=2 for Multi-TRP CSI

mTRP-CSI-N-Max2-r17 ENUMERATED {supported} OPTIONAL,

-- R1 23-7-5 CMR sharing

mTRP-CSI-CMR-r17 ENUMERATED {supported} OPTIONAL,

-- R1 23-8-11 Partial frequency sounding of SRS for non-frequency hopping case

srs-partialFreqSounding-r17 ENUMERATED {supported} OPTIONAL,

-- R1-24 feature: Extend beamSwitchTiming for FR2-2

beamSwitchTiming-v1710 SEQUENCE {

scs-480kHz ENUMERATED {sym56, sym112, sym192, sym896, sym1344} OPTIONAL,

scs-960kHz ENUMERATED {sym112, sym224, sym384, sym1792, sym2688} OPTIONAL

} OPTIONAL,

-- R1-24 feature: Extend beamSwitchTiming-r16 for FR2-2

beamSwitchTiming-r17 SEQUENCE {

scs-480kHz-r17 ENUMERATED {sym896, sym1344} OPTIONAL,

scs-960kHz-r17 ENUMERATED {sym1792, sym2688} OPTIONAL

} OPTIONAL,

-- R1-24 feature: Extend beamReportTiming for FR2-2

beamReportTiming-v1710 SEQUENCE {

scs-480kHz-r17 ENUMERATED {sym56, sym112, sym224} OPTIONAL,

scs-960kHz-r17 ENUMERATED {sym112, sym224, sym448} OPTIONAL

} OPTIONAL,

-- R1-24 feature: Extend maximum number of RX/TX beam switch DL for FR2-2

maxNumberRxTxBeamSwitchDL-v1710 SEQUENCE {

scs-480kHz-r17 ENUMERATED {n2, n4, n7} OPTIONAL,

scs-960kHz-r17 ENUMERATED {n1, n2, n4, n7} OPTIONAL

} OPTIONAL

]],

[[

-- R1-23-1-4a: Semi-persistent/aperiodic capability value report

srs-PortReportSP-AP-r17 ENUMERATED {supported} OPTIONAL,

maxNumberRxBeam-v1720 INTEGER (9..12) OPTIONAL,

-- R1-23-6-5 Support implicit configuration of RS(s) with two TCI states for beam failure detection

sfn-ImplicitRS-twoTCI-r17 ENUMERATED {supported} OPTIONAL,

-- R1-23-6-6 QCL-TypeD collision handling with CORESET with 2 TCI states

sfn-QCL-TypeD-Collision-twoTCI-r17 ENUMERATED {supported} OPTIONAL,

-- R1-23-7-1c Basic Features of CSI Enhancement for Multi-TRP - number of CPUs

mTRP-CSI-numCPU-r17 ENUMERATED {n2, n3, n4} OPTIONAL

]],

[[

supportRepNumPDSCH-TDRA-DCI-1-2-r17 ENUMERATED {n2, n3, n4, n5, n6, n7, n8, n16} OPTIONAL

]],

[[

codebookParametersetype2DopplerCSI-r18 CodebookParametersetype2DopplerCSI-r18 OPTIONAL,

codebookParametersfetype2DopplerCSI-r18 CodebookParametersfetype2DopplerCSI-r18 OPTIONAL,

codebookParametersetype2CJT-r18 CodebookParametersetype2CJT-r18 OPTIONAL,

codebookParametersfetype2CJT-r18 CodebookParametersfetype2CJT-r18 OPTIONAL,

codebookComboParametersCJT-r18 CodebookComboParametersCJT-r18 OPTIONAL,

codebookParametersHARQ-ACK-PUSCH-r18 CodebookParametersHARQ-ACK-PUSCH-r18 OPTIONAL,

-- R1 40-1-1: Unified TCI with joint DL/UL TCI update for single-DCI based intra-cell multi-TRP with single activated TCI

-- codepoint per CC

tci-JointTCI-UpdateSingleActiveTCI-PerCC-r18 SEQUENCE {

maxNumberConfigJointTCIPerCC-PerBWP-r18 ENUMERATED {n8,n12,n16,n24,n32,n48,n64,n128},

maxNumberActiveJointTCI-AcrossCC-r18 ENUMERATED {n2,n4,n6,n8,n16,n32}

} OPTIONAL,

-- R1 40-1-1a: Unified TCI with joint DL/UL TCI update for single-DCI based intra-cell multi-TRP with multiple activated TCI

-- codepoints per CC

tci-JointTCI-UpdateMultiActiveTCI-PerCC-r18 SEQUENCE {

tci-StateInd-r18 ENUMERATED {withAssignment, withoutAssignment},

maxNumberActiveJointTCI-PerCC-r18 INTEGER (2..8)

} OPTIONAL,

-- R1 40-1-1c: DCI format 1\_1 and if supported 1\_2 configured with TCI selection field

tci-SelectionDCI-r18 ENUMERATED {supported} OPTIONAL,

-- R1 40-1-2: Unified TCI with separate DL/UL TCI update for single-DCI based intra-cell multi-TRP with single activated TCI

-- codepoint per CC

tci-SeparateTCI-UpdateSingleActiveTCI-PerCC-r18 SEQUENCE {

maxNumConfigDL-TCI-PerCC-PerBWP-r18 ENUMERATED {n4, n8, n12, n16, n24, n32, n48, n64, n128},

maxNumConfigUL-TCI-PerCC-PerBWP-r18 ENUMERATED {n4, n8, n12, n16, n24, n32, n48, n64},

maxNumActiveDL-TCI-AcrossCC-r18 ENUMERATED {n2, n4, n8, n16},

maxNumActiveUL-TCI-AcrossCC-r18 ENUMERATED {n2, n4, n8, n16}

} OPTIONAL,

-- R1 40-1-2a: Unified TCI with separate DL/UL TCI update for single-DCI based intra-cell multi-TRP with multiple

-- activated TCI codepoints per CC

tci-SeparateTCI-UpdateMultiActiveTCI-PerCC-r18 SEQUENCE {

maxNumActiveDL-TCI-AcrossCC-r18 ENUMERATED {n2, n4, n8, n16},

maxNumActiveUL-TCI-AcrossCC-r18 ENUMERATED {n2, n4, n8, n16}

} OPTIONAL,

-- R1 40-1-3: Per aperiodic CSI-RS resource/resource set configuration for TCI selection in S-DCI based MTRP

tci-SelectionAperiodicCSI-RS-r18 ENUMERATED {perResource, perResourceSet, both} OPTIONAL,

-- R1 40-1-3a: Per aperiodic CSI-RS resource/resource set configuration for TCI selection in M-DCI based MTRP

tci-SelectionAperiodicCSI-RS-M-DCI-r18 ENUMERATED {perResource, perResourceSet, both} OPTIONAL,

-- R1 40-1-4: Two TCI states for CJT Tx scheme for PDSCH

twoTCI-StatePDSCH-CJT-TxScheme-r18 ENUMERATED {cjtSchemeA, cjtSchemeB, both} OPTIONAL,

-- R1 40-1-7: Unified TCI with joint DL/UL TCI update for multi-DCI based multi-TRP with single activated TCI

-- codepoint per CORESETPoolIndex per CC

tci-JointTCI-UpdateSingleActiveTCI-PerCC-PerCORESET-r18 SEQUENCE {

mTRP-Operation-r18 ENUMERATED {intraCell, intraCellAndInterCell},

maxNumberConfigJointTCIPerCC-PerBWP-r18 ENUMERATED {n8,n12,n16,n24,n32,n48,n64,n128},

maxNumberActiveJointTCIAcrossCC-PerCORESET-r18 ENUMERATED {n1,n2,n4,n8,n16}

} OPTIONAL,

-- R1 40-1-7a: Unified TCI with joint DL/UL TCI update for multi-DCI based multi-TRP with multiple activated TCI

-- codepoints per CORESETPoolIndex per CC

tci-JointTCI-UpdateMultiActiveTCI-PerCC-PerCORESET-r18 INTEGER (2..8) OPTIONAL,

-- R1 40-1-8: TRP-specific BFR with unified TCI framework with Unified TCI

tci-TRP-BFR-r18 ENUMERATED {supported} OPTIONAL,

-- R1 40-1-9: Unified TCI with separate DL/UL TCI update for multi-DCI based multi-TRP with single activated TCI

-- codepoint per CORESETPoolIndex per CC

tci-SeparateTCI-UpdateSingleActiveTCI-PerCC-PerCORESET-r18 SEQUENCE {

mTRP-Operation-r18 ENUMERATED {intraCell, intraCellAndInterCell},

maxNumConfigDL-TCI-PerCC-PerBWP-r18 ENUMERATED {n8, n12, n16, n24, n32, n48, n64, n128},

maxNumConfigUL-TCI-PerCC-PerBWP-r18 ENUMERATED {n8, n12, n16, n24, n32, n48, n64},

maxNumActiveDL-TCI-AcrossCC-r18 ENUMERATED {n1, n2, n4, n8, n16},

maxNumActiveUL-TCI-AcrossCC-r18 ENUMERATED {n1, n2, n4, n8, n16}

} OPTIONAL,

-- R1 40-1-9a: Unified TCI with separate DL/UL TCI update for multi-DCI based multi-TRP with multiple activated TCI

-- codepoints per CORESETPoolIndex per CC

tci-SeparateTCI-UpdateMultiActiveTCI-PerCC-PerCORESET-r18 SEQUENCE {

maxNumConfigDL-TCI-PerCC-PerBWP-r18 INTEGER (1..8),

maxNumConfigUL-TCI-PerCC-PerBWP-r18 INTEGER (1..8)

} OPTIONAL,

-- R1 40-1-12: Common multi-CC TCI state ID update and activation for single-DCI based multi-TRP

commonTCI-SingleDCI-r18 INTEGER (1..4) OPTIONAL,

-- R1 40-1-13: Common multi-CC TCI state ID update and activation for multi-DCI based multi-TRP

commonTCI-MultiDCI-r18 INTEGER (1..4) OPTIONAL,

-- R1 40-1-14: Two PHR reporting for STx2P

twoPHR-Reporting-r18 ENUMERATED {supported} OPTIONAL,

-- R1 40-2-3: TAG ID indication via absolute TA command MAC CE

spCell-TAG-Ind-r18 ENUMERATED {supported} OPTIONAL,

-- R1 40-2-4: PDCCH order sent by one TRP triggers RACH procedure (specifically PRACH) towards a different TRP based on CFRA for

-- inter-cell

interCellCrossTRP-PDCCH-OrderCFRA-r18 ENUMERATED {supported} OPTIONAL,

-- R1 40-2-4a: PDCCH order sent by one TRP triggers RACH procedure (specifically PRACH) towards a different TRP based on CFRA for

-- intra-cell

intraCellCrossTRP-PDCCH-OrderCFRA-r18 ENUMERATED {supported} OPTIONAL,

-- R1 40-2-9: Overlapping UL transmission reduction

overlapUL-TransReduction-r18 ENUMERATED {supported} OPTIONAL,

-- R1 40-3-2-12: Supported maximum periodicity of CMR when configured as periodic CSI-RS

maxPeriodicityCMR-r18 ENUMERATED {sl4, sl5, sl8, sl10, sl20} OPTIONAL,

-- R1 40-3-3-1: TDCP (Time Domain Channel Properties) report

tdcp-Report-r18 SEQUENCE {

valueX-r18 INTEGER (1..2),

maxNumberActiveResource-r18 INTEGER (2..32)

} OPTIONAL,

-- R1 40-3-3-5: Number of CSI-RS resources for TDCP

tdcp-Resource-r18 SEQUENCE {

maxNumberConfigPerCC-r18 ENUMERATED {n2,n4,n6,n8,n10,n12},

maxNumberConfigAcrossCC-r18 INTEGER (1..32),

maxNumberSimultaneousPerCC-r18 ENUMERATED {n2, n4, n6, n8, n12, n16, n20, n24, n28, n32}

} OPTIONAL,

-- R1 40-3-1-24: Timeline for regular eType-II-CJT CSI, or for port selection FeType-II-CJT CSI

timelineRelax-CJT-CSI-r18 ENUMERATED {n0,n2} OPTIONAL,

-- R1 40-4-11: Joint configuration of Rel.18 DMRS ports and Rel.18 dynamic switching between DFT-S-OFDM and CP-OFDM for PUSCH

jointConfigDMRSPortDynamicSwitching-r18 ENUMERATED {supported} OPTIONAL,

-- R1 40-5-1: SRS comb offset hopping

srs-combOffsetHopping-r18 ENUMERATED {supported} OPTIONAL,

-- R1 40-5-1a: Comb offset hopping time-domain behavior when repetition factor R>1

srs-combOffsetInTime-r18 ENUMERATED {srs, rsrs, both} OPTIONAL,

-- R1 40-5-1b: SRS comb offset hopping combined with group/sequence hopping

srs-combOffsetCombinedGroupSequence-r18 ENUMERATED {supported} OPTIONAL,

-- R1 40-5-1c: Comb offset hopping within a subset

srs-combOffsetHoppingWithinSubset-r18 ENUMERATED {supported} OPTIONAL,

-- R1 40-5-2: SRS cyclic shift hopping

srs-cyclicShiftHopping-r18 ENUMERATED {supported} OPTIONAL,

-- R1 40-5-2a: Smaller cyclic shift granularity for cyclic shift hopping

srs-cyclicShiftHoppingSmallGranularity-r18 ENUMERATED {supported} OPTIONAL,

-- R1 40-5-2b: SRS cyclic shift hopping combined with group/sequence hopping

srs-cyclicShiftCombinedGroupSequence-r18 ENUMERATED {supported} OPTIONAL,

-- R1 40-5-2c: Cyclic shift hopping within a subset

cyclicShiftHoppingWithinSubset-r18 ENUMERATED {supported} OPTIONAL,

-- R1 40-5-3: SRS cyclic shift hopping combined with SRS comb offset hopping

srs-cyclicShiftCombinedCombOffset-r18 ENUMERATED {supported} OPTIONAL,

-- R1 40-6-1-1: 2 PTRS ports for single-DCI based STx2P SDM scheme for PUSCH-codebook

pusch-CB-2PTRS-SingleDCI-STx2P-SDM-r18 ENUMERATED {supported} OPTIONAL,

-- R1 40-6-1a-1: 2 PTRS ports for single-DCI based STx2P SDM scheme for PUSCH-noncodebook

pusch-NonCB-2PTRS-SingleDCI-STx2P-SDM-r18 ENUMERATED {supported} OPTIONAL,

-- R1 40-6-1b: Association between CSI-RS and SRS for noncodebook single-DCI based STx2P SDM scheme for PUSCH

pusch-NonCB-SingleDCI-STx2P-SDM-CSI-RS-SRS-r18 SEQUENCE {

maxNumberPeriodicSRS-Resource-PerBWP-r18 INTEGER (1..8),

maxNumberAperiodicSRS-Resource-PerBWP-r18 INTEGER (1..8),

maxNumberSemiPersistentSRS-ResourcePerBWP-r18 INTEGER (0..8),

valueY-SRS-ResourceAssociate-r18 INTEGER (1..16),

valueX-CSI-RS-ResourceAssociate-r18 INTEGER (1..2)

} OPTIONAL,

-- R1 40-6-3b-1: Associated CSI-RS resources for noncodebook multi-DCI based STx2P PUSCH+PUSCH

twoPUSCH-NonCB-Multi-DCI-STx2P-CSI-RS-Resource-r18 SEQUENCE {

maxNumberPeriodicSRS-r18 INTEGER (1..8),

maxNumberAperiodicSRS-r18 INTEGER (1..8),

maxNumberSemiPersistentSRS-r18 INTEGER (0..8),

simultaneousSRS-PerCC-r18 INTEGER (1..16),

simultaneousCSI-RS-NonCB-r18 INTEGER (1..2)

} OPTIONAL,

-- R1 40-6-1-2: New UL DMRS port entry for single-DCI based SDM scheme for Rel-15 DMRS port and/or Rel-18 DMRS port

dmrs-PortEntrySingleDCI-SDM-r18 ENUMERATED {supported} OPTIONAL,

-- R1 40-6-2-1: 2 PTRS ports for single-DCI based STx2P SFN scheme for PUSCH-codebook

pusch-CB-2PTRS-SingleDCI-STx2P-SFN-r18 ENUMERATED {supported} OPTIONAL,

-- R1 40-6-2a-1: 2 PTRS ports for single-DCI based STx2P SFN scheme for PUSCH-codebook

pusch-NonCB-2PTRS-SingleDCI-STx2P-SFN-r18 ENUMERATED {supported} OPTIONAL,

-- R1 40-6-2b: Association between CSI-RS and SRS for noncodebook single-DCI based STx2P SFN scheme for PUSCH

pusch-NonCB-SingleDCI-STx2P-SFN-CSI-RS-SRS-r18 SEQUENCE {

maxNumberPeriodicSRS-Resource-PerBWP-r18 INTEGER (1..8),

maxNumberAperiodicSRS-Resource-PerBWP-r18 INTEGER (1..8),

maxNumberSemiPersistentSRS-ResourcePerBWP-r18 INTEGER (0..8),

valueY-SRS-ResourceAssociate-r18 INTEGER (1..16),

valueX-CSI-RS-ResourceAssociate-r18 INTEGER (1..2)

} OPTIONAL,

-- R1 40-6-3c: Codebook multi-DCI based STx2P PUSCH+PUSCH - Fully overlapping PUSCHs in time and fully overlapping in frequency

twoPUSCH-CB-MultiDCI-STx2P-FullTimeFullFreqOverlap-r18 ENUMERATED {supported} OPTIONAL,

-- R1 40-6-3d: Codebook multi-DCI based STx2P PUSCH+PUSCH - Fully overlapping PUSCHs in time and partially overlapping in frequency

twoPUSCH-CB-MultiDCI-STx2P-FullTimePartialFreqOverlap-r18 ENUMERATED {supported} OPTIONAL,

-- R1 40-6-3e: Codebook multi-DCI based STx2P PUSCH+PUSCH - Partially overlapping PUSCHs in time and fully overlapping in frequency

twoPUSCH-CB-MultiDCI-STx2P-PartialTimeFullFreqOverlap-r18 ENUMERATED {supported} OPTIONAL,

-- R1 40-6-3f: Codebook multi-DCI based STx2P PUSCH+PUSCH - Partially overlapping PUSCHs in time, partially overlapping in frequency

twoPUSCH-CB-MultiDCI-STx2P-PartialTimePartialFreqOverlap-r18 ENUMERATED {supported} OPTIONAL,

-- R1 40-6-3g: Codebook multi-DCI based STx2P PUSCH+PUSCH - Partially overlapping PUSCHs in time, partially or non-overlapping

-- in frequency

twoPUSCH-CB-MultiDCI-STx2P-PartialTimeNonFreqOverlap-r18 ENUMERATED {supported} OPTIONAL,

-- R1 40-6-3h: Codebook multi-DCI based STx2P PUSCH+PUSCH for CG+CG

twoPUSCH-CB-MultiDCI-STx2P-CG-CG-r18 ENUMERATED {supported} OPTIONAL,

-- R1 40-6-3i: Codebook multi-DCI based STx2P PUSCH+PUSCH for DG+CG

twoPUSCH-CB-MultiDCI-STx2P-CG-DG-r18 ENUMERATED {supported} OPTIONAL,

-- R1 40-6-3j: Noncodebook multi-DCI based STx2P PUSCH+PUSCH - Fully overlapping PUSCHs in time and fully overlapping in frequency

twoPUSCH-NonCB-MultiDCI-STx2P-FullTimeFullFreqOverlap-r18 ENUMERATED {supported} OPTIONAL,

-- R1 40-6-3k: Noncodebook multi-DCI based STx2P PUSCH+PUSCH - Fully overlapping PUSCHs in time and partially overlapping in

-- frequency

twoPUSCH-NonCB-MultiDCI-STx2P-FullTimePartialFreqOverlap-r18 ENUMERATED {supported} OPTIONAL,

-- R1 40-6-3l: Noncodebook multi-DCI based STx2P PUSCH+PUSCH - Partially overlapping PUSCHs in time and fully overlapping in

-- frequency

twoPUSCH-NonCB-MultiDCI-STx2P-PartialTimeFullFreqOverlap-r18 ENUMERATED {supported} OPTIONAL,

-- R1 40-6-3m: Noncodebook multi-DCI based STx2P PUSCH+PUSCH - Partially overlapping PUSCHs in time, partially overlapping in

-- frequency

twoPUSCH-NonCB-MultiDCI-STx2P-PartialTimePartialFreqOverlap-r18 ENUMERATED {supported} OPTIONAL,

-- R1 40-6-3n: Noncodebook multi-DCI based STx2P PUSCH+PUSCH - Partially overlapping PUSCHs in time, non-overlapping in frequency

twoPUSCH-NonCB-MultiDCI-STx2P-PartialTimeNonFreqOverlap-r18 ENUMERATED {supported} OPTIONAL,

-- R1 40-6-3o: Noncodebook multi-DCI based STx2P PUSCH+PUSCH for CG+CG

twoPUSCH-NonCB-MultiDCI-STx2P-CG-CG-r18 ENUMERATED {supported} OPTIONAL,

-- R1 40-6-3p: Noncodebook multi-DCI based STx2P PUSCH+PUSCH for DG+CG

twoPUSCH-NonCB-MultiDCI-STx2P-CG-DG-r18 ENUMERATED {supported} OPTIONAL,

-- R1 40-6-4a: Dynamic indication of repetition number for SFN scheme for PUCCH

pucch-RepetitionDynamicIndicationSFN-r18 ENUMERATED {supported} OPTIONAL,

-- R1 40-6-5: Support grouped-based beam reporting for STx2P

groupBeamReporting-STx2P-r18 SEQUENCE {

groupL1-RSRP-Reporting-r18 ENUMERATED {jointULandDL, ulOnly, both},

maxNumberBeamGroups-r18 INTEGER (1..4),

maxNumberResWithinSlotAcrossCC-r18 ENUMERATED {n2,n3,n4,n8,n16,n32,n64},

maxNumberResAcrossCC-r18 ENUMERATED {n8,n16,n32,n64,n128}

} OPTIONAL

]],

[[

-- R1 40-4-1k: Simultaneous Configuration of Rel-18 DL DMRS and DCI format 1\_3

simulConfigDMRS-DCI-1-3-r18 ENUMERATED {supported} OPTIONAL

]],

[[

codebookParametersType1SP-SchemeA-r19 CodebookParametersType1SP-SchemeA-r19 OPTIONAL,

codebookParametersType1SP-SchemeB-r19 CodebookParametersType1SP-SchemeB-r19 OPTIONAL,

codebookParametersType1MP-r19 CodebookParametersType1MP-r19 OPTIONAL,

codebookParameterseType2Ext-r19 CodebookParameterseType2Ext-r19 OPTIONAL,

codebookParametersfeType2Ext-r19 CodebookParametersfeType2Ext-r19 OPTIONAL,

codebookParameterseType2DopplerExt-r19 CodebookParameterseType2DopplerExt-r19 OPTIONAL,

codebookParametersHybridBF-Type1SP-r19 CodebookParametersHybridBF-Type1SP-r19 OPTIONAL,

codebookParametersHybridBF-eType2-r19 CodebookParametersHybridBF-eType2-r19 OPTIONAL,

-- R1 58-3-1: CSI prediction for UE-sided inference when N4=1

aiml-CSI-Prediction-r19 ENUMERATED {supported} OPTIONAL,

-- R1 59-1-1: UE-initiated/event-driven beam management for Event-2 based measurement and report for Mode A

uei-ModeA-Event2-r19 INTEGER (1..64) OPTIONAL,

-- R1 59-1-2: UE-initiated/event-driven beam management Mode B

uei-ModeB-r19 SEQUENCE {

scs15kHz-r19 ENUMERATED {n0, n1, n2, n4, n8, n16} OPTIONAL,

scs30kHz-r19 ENUMERATED {n0, n2, n4, n8, n16, n32} OPTIONAL,

scs60kHz-r19 ENUMERATED {n0, n4, n8, n32, n64} OPTIONAL,

scs120kHz-r19 ENUMERATED {n0, n8, n16, n32, n64, n128} OPTIONAL,

scs480kHz-r19 ENUMERATED {n0, n32, n64, n128, n256, n512} OPTIONAL,

scs960kHz-r19 ENUMERATED {n0, n64, n128, n256, n512} OPTIONAL

} OPTIONAL,

-- R1 59-1-3: Triggering event determination via detecting ≥ M event instances for at least one new beam within a time window.

uei-TriggerEventDetermination-r19 INTEGER (1..64) OPTIONAL,

-- R1 59-1-4: UE-initiated/event-driven beam management for Event-1 based measurement and report for Mode A

uei-ModeA-Event1-r19 ENUMERATED {supported} OPTIONAL,

-- R1 59-1-5: UE-initiated/event-driven beam management for Event-7 based measurement and report for Mode A

uei-ModeA-Event7-r19 BIT STRING (SIZE (8)) OPTIONAL,

-- R1 59-1-7: 1-bit condition met indication in RSRP report format for each report of CRI/SSBRI for Event-2 and Event-7

event2ConditionIndication-r19 ENUMERATED {supported} OPTIONAL,

-- R1 59-2-1-6: CSI-RS resource time domain restriction for Type-I and Type II codebook enhancement for up to 128 ports

timeRestriction128Port-r19 ENUMERATED {supported} OPTIONAL,

-- R1 59-2-1-7: Group-specific 3-bit scaling factors for up to 128 ports

groupScalingFactor-r19 ENUMERATED {rank1, rank1and2} OPTIONAL,

-- R1 59-2-2-3a: Configuration of MR always-reported resources with Rel-15 Type-I SP codebook

mr-AlwaysReportedType1SP-r19 ENUMERATED {supported} OPTIONAL,

-- R1 59-2-2-3b: Configuration of MR always-reported resources with Rel-16 eType-II codebook with R=1

mr-AlwaysReported-eType2-r19 ENUMERATED {supported} OPTIONAL,

-- R1 59-2-3-1: CJTC Dd report

cjtc-DdReport-r19 SEQUENCE {

minRangeDdInCyclicPrefix-r19 ENUMERATED {half, full},

maxResolutionDd-r19 ENUMERATED {n32,n64,n128,n256},

scalingFactor-r19 INTEGER (1..2)

} OPTIONAL,

-- R1 59-2-3-1a: CJTC Dd report processing

cjtc-DdReportProcessing-r19 SEQUENCE {

maxNumberTRS-Resource-r19 ENUMERATED {n2,n4,n6,n8,n10,n12},

maxNumberTRS-ResourceAcrossCC-r19 ENUMERATED {n2,n4,n6,n8,n12,n64},

maxNumberCSI-RS-ResourcePerCC-r19 ENUMERATED {n2,n4,n6,n8,n12,n16,n20,n24,n28,n32},

maxNumberCSI-RS-ResourceAcrossCC-r19 ENUMERATED {n2,n4,n6,n8,n12,n16,n20,n24,n28,n32,n64},

valueX-r19 INTEGER (1..2)

} OPTIONAL,

-- R1 59-2-3-2: CJTC FO report

cjtc-FO-Report-r19 SEQUENCE {

minRangeFO-r19 ENUMERATED {ppmDot1, ppmDot2},

maxResolutionFO-r19 ENUMERATED {n16,n32,n256},

scalingFactor-r19 INTEGER (1..2)

} OPTIONAL,

-- R1 59-2-3-2a: CJTC FO report processing

cjtc-FO-ReportProcessing-r19 SEQUENCE {

maxNumberTRS-Resource-r19 ENUMERATED {n2,n4,n6,n8,n10,n12},

maxNumberTRS-ResourceAcrossCC-r19 ENUMERATED {n2,n4,n6,n8,n12,n64},

maxNumberCSI-RS-ResourcePerCC-r19 ENUMERATED {n2,n4,n6,n8,n12,n16,n20,n24,n28,n32},

maxNumberCSI-RS-ResourceAcrossCC-r19 ENUMERATED {n2,n4,n6,n8,n12,n16,n20,n24,n28,n32,n64},

valueX-r19 INTEGER (1..2)

} OPTIONAL,

-- R1 59-2-3-3: CJTC wideband PO report

cjtc-PO-ReportWideband-r19 SEQUENCE {

maxResolution-r19 ENUMERATED {n16, n32},

scalingFactor-r19 INTEGER (1..2),

maxSlotDuration-r19 INTEGER (1..2)

} OPTIONAL,

-- R1 59-2-3-3a: CJTC wideband PO report processing

cjtc-PO-ReportWidebandProcessing-r19 SEQUENCE {

maxNumberCSI-RS-Configured-r19 ENUMERATED {n2,n4,n6,n8,n10,n12},

maxNumberCSI-RS-ConfiguredAcrossCC-r19 ENUMERATED {n2,n4,n6,n8,n12,n64},

maxNumberCSI-RS-ResourcePerCC-r19 ENUMERATED {n2,n4,n6,n8,n12,n16,n20,n24,n28,n32},

maxNumberCSI-RS-ResourceAcrossCC-r19 ENUMERATED {n2,n4,n6,n8,n12,n16,n20,n24,n28,n32,n64},

valueX-r19 INTEGER (1..2)

} OPTIONAL,

-- R1 59-2-3-4: CJTC subband PO report

cjtc-PO-ReportSubband-r19 SEQUENCE {

maxResolution-r19 ENUMERATED {n16, n32},

minSubbandSize-r19 ENUMERATED {n1,n2,n4,n8,n16},

scalingFactor-r19 INTEGER (1..2),

maxSlotDuration-r19 INTEGER (1..2)

} OPTIONAL,

-- R1 59-2-3-5: CJTC Dd+FO report

cjtc-DdFO-Report-r19 SEQUENCE {

minRangeDdInCyclicPrefix-r19 ENUMERATED {half, full},

maxResolutionDd-r19 ENUMERATED {n32,n64,n128,n256},

minRangeFO-r19 ENUMERATED {ppmDot1, ppmDot2},

maxResolutionFO-r19 ENUMERATED {n16,n32,n256},

scalingFactor-r19 INTEGER (1..2)

} OPTIONAL,

-- R1 59-2-3-5a: CJTC Dd+FO report processing

cjtc-DdFO-ReportProcessing-r19 SEQUENCE {

maxNumberTRS-Resource-r19 ENUMERATED {n2,n4,n6,n8,n10,n12},

maxNumberTRS-ResourceAcrossCC-r19 ENUMERATED {n2,n4,n6,n8,n12,n64},

maxNumberCSI-RS-ResourcePerCC-r19 ENUMERATED {n2,n4,n6,n8,n12,n16,n20,n24,n28,n32},

maxNumberCSI-RS-ResourceAcrossCC-r19 ENUMERATED {n2,n4,n6,n8,n12,n16,n20,n24,n28,n32,n64},

valueX-r19 INTEGER (1..2)

} OPTIONAL,

-- R1 59-2-3-6a: New CJT QCL assumptions for PDSCH pre-compensation for Scheme-C

cjt-QCL-PDSCH-SchemeC-r19 ENUMERATED {supported} OPTIONAL,

-- R1 59-2-3-6b: New CJT QCL assumptions for PDSCH pre-compensation for Scheme-D

cjt-QCL-PDSCH-SchemeD-r19 ENUMERATED {supported} OPTIONAL,

-- R1 59-2-3-6c: New CJT QCL assumptions for PDSCH pre-compensation for Scheme-E

cjt-QCL-PDSCH-SchemeE-r19 ENUMERATED {supported} OPTIONAL,

-- R1 59-2-3-7: Linkage of CJTC Dd and Rel-18 eType-II CJT with joint triggering

linked-CJTC-Dd-eType2CJT-Joint-r19 ENUMERATED {supported} OPTIONAL,

-- R1 59-2-3-7a: Linkage of CJTC Dd and Rel-18 eType-II CJT with joint triggering

linked-CJTC-Dd-eType2CJT-Separate-r19 ENUMERATED {supported} OPTIONAL,

-- R1 59-2-3-8: Separate triggering with configuration of 1-bit indicator per CSI trigger state

linked-CJTC-Dd-eType2CJT-SeparatePerState-r19 ENUMERATED {supported} OPTIONAL,

-- R1 59-2-3-10: Relaxed timeline for joint triggering of CJTC Dd and Rel-18 eType-II CJT

timelineRelax-CJTC-Dd-eType2CJT-r19 SEQUENCE {

scs15kHz-r19 ENUMERATED {n2,n4,n8} OPTIONAL,

scs30kHz-r19 ENUMERATED {n4,n8,n14,n28} OPTIONAL,

scs60kHz-r19 ENUMERATED {n8,n14,n28} OPTIONAL,

scs120kHz-r19 ENUMERATED {n14,n28,n56} OPTIONAL,

scs480kHz-r19 ENUMERATED {n56,n112,n224} OPTIONAL,

scs960kHz-r19 ENUMERATED {n112,n224,n448} OPTIONAL

} OPTIONAL,

-- R1 59-3-1a: Association between CSI-RS and SRS for non-codebook-based 3Tx PUSCH transmission for single TRP

nonCodebook-CSI-RS-SRS-3TxPUSCH-r19 SEQUENCE (SIZE (1.. maxNrofCSI-RS-Resources))

OF SupportedCSI-RS-Resource OPTIONAL,

-- R1 59-4-1a: PL offset for PUCCH/PUSCH/SRS power control for joint DL/UL TCI state(s)

pathlossOffsetPUCCH-PUSCH-SRS-JointTCI-r19 ENUMERATED {supported} OPTIONAL,

-- R1 59-4-1b: PL offset for PUCCH/PUSCH/SRS power control for separate DL/UL TCI state(s)

pathlossOffsetPUCCH-PUSCH-SRS-SeparateTCI-r19 ENUMERATED {supported} OPTIONAL,

-- R1 59-4-2a: Path Loss offset on PDCCH-order PRACH for joint DL/UL TCI state(s)

pathlossOffsetPRACH-JointTCI-r19 ENUMERATED {supported} OPTIONAL,

-- R1 59-4-2b: Path Loss offset on PDCCH-order PRACH for separate DL/UL TCI state(s)

pathlossOffsetPRACH-SeparateTCI-r19 ENUMERATED {supported} OPTIONAL,

-- R1 59-4-7a: Extended value range of starting bit of block in DCI format 2\_3

extendedStartBitDCI-2-3-r19 ENUMERATED {supported} OPTIONAL,

-- R1 59-4-3: Two SRS closed-loop power control adjustment states separate from PUSCH

twoSRS-PwrControlAdjust-r19 ENUMERATED {supported} OPTIONAL,

-- R1 59-4-5: Overlapping UL transmission reduction

overlapUL-TransReductionEnh-r19 ENUMERATED {supported} OPTIONAL,

-- R1 59-4-6: MAC-CE update of PL offset value(s)

pathlossOffsetUpdate-r19 ENUMERATED {supported} OPTIONAL,

-- R1 59-4-7b: DCI format 2\_3 to indicate TPC for one of two separate SRS closed loop indexes

twoSRS-TPC-DCI-2-3-r19 ENUMERATED {supported} OPTIONAL,

-- R1 59-4-8: DCI format 1\_1 to indicate TPC command for SRS associated with a separate SRS CLPC adjustment state

srs-TPC-CLPC-AdjustmentState-r19 ENUMERATED {supported} OPTIONAL,

-- R1 59-4-9a: DCI format 1\_1 to indicate one of two separate SRS closed loop indexes under separate DL/UL TCI state mode

twoSRS-DCI-1-1-Separate-r19 ENUMERATED {supported} OPTIONAL,

-- R1 59-4-9b: DCI format 1\_1 to indicate one of two separate SRS closed loop indexes under joint TCI state mode

twoSRS-DCI-1-1-Joint-r19 ENUMERATED {supported} OPTIONAL,

-- R1 59-4-11: Support of including PL offset in the calculation of Type 1 PHR based on actual PUSCH transmission

-- and Type 1 PHR based on reference PUSCH

pathlossOffsetPHR-r19 ENUMERATED {supported} OPTIONAL

]]

}

MIMO-ParametersPerBand-v17b0 ::= SEQUENCE {

-- R1 23-1-1b Unified TCI with joint DL/UL TCI update for intra- and inter-cell beam management with more than one MAC-CE

unifiedJointTCI-multiMAC-CE-v17b0 SEQUENCE{

minBeamApplicationTimeJointTCI-v17b0 CHOICE {

fr1-v17b0 SEQUENCE {

scs-15kHz-v17b0 ENUMERATED {sym1, sym2, sym4, sym7, sym14, sym28, sym42, sym56, sym70} OPTIONAL,

scs-30kHz-v17b0 ENUMERATED {sym1, sym2, sym4, sym7, sym14, sym28, sym42, sym56, sym70} OPTIONAL,

scs-60kHz-v17b0 ENUMERATED {sym1, sym2, sym4, sym7, sym14, sym28, sym42, sym56, sym70} OPTIONAL

},

fr2-v17b0 SEQUENCE {

scs-60kHz-v17b0 ENUMERATED {sym1, sym2, sym4, sym7, sym14, sym28, sym42, sym56, sym70,

sym84, sym98, sym112, sym224, sym336} OPTIONAL,

scs-120kHz-v17b0 ENUMERATED {sym1, sym2, sym4, sym7, sym14, sym28, sym42, sym56, sym70,

sym84, sym98, sym112, sym224, sym336} OPTIONAL

}

},

maxNumMAC-CE-PerCC-v17b0 ENUMERATED {n2, n3, n4, n5, n6, n7, n8}

} OPTIONAL,

-- R1 23-10-1b Unified TCI with separate DL/UL TCI update for intra-cell beam management with more than one MAC-CE

unifiedSeparateTCI-multiMAC-CE-v17b0 SEQUENCE{

minBeamApplicationTimeSeparateTCI-v17b0 CHOICE {

fr1-v17b0 SEQUENCE {

scs-15kHz-v17b0 ENUMERATED {sym1, sym2, sym4, sym7, sym14, sym28, sym42, sym56, sym70} OPTIONAL,

scs-30kHz-v17b0 ENUMERATED {sym1, sym2, sym4, sym7, sym14, sym28, sym42, sym56, sym70} OPTIONAL,

scs-60kHz-v17b0 ENUMERATED {sym1, sym2, sym4, sym7, sym14, sym28, sym42, sym56, sym70} OPTIONAL

},

fr2-v17b0 SEQUENCE {

scs-60kHz-v17b0 ENUMERATED {sym1, sym2, sym4, sym7, sym14, sym28, sym42, sym56, sym70,

sym84, sym98, sym112, sym224, sym336} OPTIONAL,

scs-120kHz-v17b0 ENUMERATED {sym1, sym2, sym4, sym7, sym14, sym28, sym42, sym56, sym70,

sym84, sym98, sym112, sym224, sym336} OPTIONAL

}

},

maxActivatedDL-TCIPerCC-v17b0 INTEGER (2..8),

maxActivatedUL-TCIPerCC-v17b0 INTEGER (2..8)

} OPTIONAL

}

DummyG ::= SEQUENCE {

maxNumberSSB-CSI-RS-ResourceOneTx ENUMERATED {n8, n16, n32, n64},

maxNumberSSB-CSI-RS-ResourceTwoTx ENUMERATED {n0, n4, n8, n16, n32, n64},

supportedCSI-RS-Density ENUMERATED {one, three, oneAndThree}

}

BeamManagementSSB-CSI-RS ::= SEQUENCE {

maxNumberSSB-CSI-RS-ResourceOneTx ENUMERATED {n0, n8, n16, n32, n64},

maxNumberCSI-RS-Resource ENUMERATED {n0, n4, n8, n16, n32, n64},

maxNumberCSI-RS-ResourceTwoTx ENUMERATED {n0, n4, n8, n16, n32, n64},

supportedCSI-RS-Density ENUMERATED {one, three, oneAndThree} OPTIONAL,

maxNumberAperiodicCSI-RS-Resource ENUMERATED {n0, n1, n4, n8, n16, n32, n64}

}

DummyH ::= SEQUENCE {

burstLength INTEGER (1..2),

maxSimultaneousResourceSetsPerCC INTEGER (1..8),

maxConfiguredResourceSetsPerCC INTEGER (1..64),

maxConfiguredResourceSetsAllCC INTEGER (1..128)

}

CSI-RS-ForTracking ::= SEQUENCE {

maxBurstLength INTEGER (1..2),

maxSimultaneousResourceSetsPerCC INTEGER (1..8),

maxConfiguredResourceSetsPerCC INTEGER (1..64),

maxConfiguredResourceSetsAllCC INTEGER (1..256)

}

CSI-RS-IM-ReceptionForFeedback ::= SEQUENCE {

maxConfigNumberNZP-CSI-RS-PerCC INTEGER (1..64),

maxConfigNumberPortsAcrossNZP-CSI-RS-PerCC INTEGER (2..256),

maxConfigNumberCSI-IM-PerCC ENUMERATED {n1, n2, n4, n8, n16, n32},

maxNumberSimultaneousNZP-CSI-RS-PerCC INTEGER (1..64),

totalNumberPortsSimultaneousNZP-CSI-RS-PerCC INTEGER (2..256)

}

CSI-RS-ProcFrameworkForSRS ::= SEQUENCE {

maxNumberPeriodicSRS-AssocCSI-RS-PerBWP INTEGER (1..4),

maxNumberAperiodicSRS-AssocCSI-RS-PerBWP INTEGER (1..4),

maxNumberSP-SRS-AssocCSI-RS-PerBWP INTEGER (0..4),

simultaneousSRS-AssocCSI-RS-PerCC INTEGER (1..8)

}

CSI-ReportFramework ::= SEQUENCE {

maxNumberPeriodicCSI-PerBWP-ForCSI-Report INTEGER (1..4),

maxNumberAperiodicCSI-PerBWP-ForCSI-Report INTEGER (1..4),

maxNumberSemiPersistentCSI-PerBWP-ForCSI-Report INTEGER (0..4),

maxNumberPeriodicCSI-PerBWP-ForBeamReport INTEGER (1..4),

maxNumberAperiodicCSI-PerBWP-ForBeamReport INTEGER (1..4),

maxNumberAperiodicCSI-triggeringStatePerCC ENUMERATED {n3, n7, n15, n31, n63, n128},

maxNumberSemiPersistentCSI-PerBWP-ForBeamReport INTEGER (0..4),

simultaneousCSI-ReportsPerCC INTEGER (1..8)

}

CSI-ReportFrameworkExt-r16 ::= SEQUENCE {

maxNumberAperiodicCSI-PerBWP-ForCSI-ReportExt-r16 INTEGER (5..8)

}

PTRS-DensityRecommendationDL ::= SEQUENCE {

frequencyDensity1 INTEGER (1..276),

frequencyDensity2 INTEGER (1..276),

timeDensity1 INTEGER (0..29),

timeDensity2 INTEGER (0..29),

timeDensity3 INTEGER (0..29)

}

PTRS-DensityRecommendationUL ::= SEQUENCE {

frequencyDensity1 INTEGER (1..276),

frequencyDensity2 INTEGER (1..276),

timeDensity1 INTEGER (0..29),

timeDensity2 INTEGER (0..29),

timeDensity3 INTEGER (0..29),

sampleDensity1 INTEGER (1..276),

sampleDensity2 INTEGER (1..276),

sampleDensity3 INTEGER (1..276),

sampleDensity4 INTEGER (1..276),

sampleDensity5 INTEGER (1..276)

}

SpatialRelations ::= SEQUENCE {

maxNumberConfiguredSpatialRelations ENUMERATED {n4, n8, n16, n32, n64, n96},

maxNumberActiveSpatialRelations ENUMERATED {n1, n2, n4, n8, n14},

additionalActiveSpatialRelationPUCCH ENUMERATED {supported} OPTIONAL,

maxNumberDL-RS-QCL-TypeD ENUMERATED {n1, n2, n4, n8, n14}

}

DummyI ::= SEQUENCE {

supportedSRS-TxPortSwitch ENUMERATED {t1r2, t1r4, t2r4, t1r4-t2r4, tr-equal},

txSwitchImpactToRx ENUMERATED {true} OPTIONAL

}

CSI-MultiTRP-SupportedCombinations-r17 ::= SEQUENCE {

maxNumTx-Ports-r17 ENUMERATED {n2, n4, n8, n12, n16, n24, n32},

maxTotalNumCMR-r17 INTEGER (2..64),

maxTotalNumTx-PortsNZP-CSI-RS-r17 INTEGER (2..256)

}

-- TAG-MIMO-PARAMETERSPERBAND-STOP

-- ASN1STOP

|  |
| --- |
| *MIMO-ParametersPerBand* field descriptions |
| ***codebookParametersPerBand***  For a given frequency band, this field this field indicates the alternative list of *SupportedCSI-RS-Resource* supported for each codebook type. The supported CSI-RS resources indicated by this field are referred by *codebookParametersperBC* in *CA-ParametersNR* to indicate the supported CSI-RS resource per band combination. |
| ***csi-RS-IM-ReceptionForFeedback/ csi-RS-ProcFrameworkForSRS/ csi-ReportFramework***  CSI related capabilities which the UE supports on each of the carriers operated on this band. If the network configures the UE with serving cells on both FR1 and FR2 bands these values may be further limited by the corresponding fields in *fr1-fr2-Add-UE-NR-Capabilities*. |
| ***supportNewDMRS-Port***  Presence of this field set to *supported1*, *supported2* or *supported3* indicates that the UE supports the new DMRS port entry {0,2,3}. |

#### – *ModulationOrder*

The IE *ModulationOrder* is used to convey the maximum supported modulation order.

*ModulationOrder* information element

-- ASN1START

-- TAG-MODULATIONORDER-START

ModulationOrder ::= ENUMERATED {bpsk-halfpi, bpsk, qpsk, qam16, qam64, qam256}

-- TAG-MODULATIONORDER-STOP

-- ASN1STOP

#### – *MRDC-Parameters*

The IE *MRDC-Parameters* contains the band combination parameters specific to MR-DC for a given MR-DC band combination.

*MRDC-Parameters* information element

-- ASN1START

-- TAG-MRDC-PARAMETERS-START

MRDC-Parameters ::= SEQUENCE {

singleUL-Transmission ENUMERATED {supported} OPTIONAL,

dynamicPowerSharingENDC ENUMERATED {supported} OPTIONAL,

tdm-Pattern ENUMERATED {supported} OPTIONAL,

ul-SharingEUTRA-NR ENUMERATED {tdm, fdm, both} OPTIONAL,

ul-SwitchingTimeEUTRA-NR ENUMERATED {type1, type2} OPTIONAL,

simultaneousRxTxInterBandENDC ENUMERATED {supported} OPTIONAL,

asyncIntraBandENDC ENUMERATED {supported} OPTIONAL,

...,

[[

dualPA-Architecture ENUMERATED {supported} OPTIONAL,

intraBandENDC-Support ENUMERATED {non-contiguous, both} OPTIONAL,

ul-TimingAlignmentEUTRA-NR ENUMERATED {required} OPTIONAL

]]

}

MRDC-Parameters-v1580 ::= SEQUENCE {

dynamicPowerSharingNEDC ENUMERATED {supported} OPTIONAL

}

MRDC-Parameters-v1590 ::= SEQUENCE {

interBandContiguousMRDC ENUMERATED {supported} OPTIONAL

}

MRDC-Parameters-v15g0 ::= SEQUENCE {

simultaneousRxTxInterBandENDCPerBandPair SimultaneousRxTxPerBandPair OPTIONAL

}

MRDC-Parameters-v15n0 ::= SEQUENCE {

intraBandENDC-Support-UL ENUMERATED {non-contiguous, both} OPTIONAL

}

MRDC-Parameters-v1620 ::= SEQUENCE {

maxUplinkDutyCycle-interBandENDC-TDD-PC2-r16 SEQUENCE{

eutra-TDD-Config0-r16 ENUMERATED {n20, n40, n50, n60, n70, n80, n90, n100} OPTIONAL,

eutra-TDD-Config1-r16 ENUMERATED {n20, n40, n50, n60, n70, n80, n90, n100} OPTIONAL,

eutra-TDD-Config2-r16 ENUMERATED {n20, n40, n50, n60, n70, n80, n90, n100} OPTIONAL,

eutra-TDD-Config3-r16 ENUMERATED {n20, n40, n50, n60, n70, n80, n90, n100} OPTIONAL,

eutra-TDD-Config4-r16 ENUMERATED {n20, n40, n50, n60, n70, n80, n90, n100} OPTIONAL,

eutra-TDD-Config5-r16 ENUMERATED {n20, n40, n50, n60, n70, n80, n90, n100} OPTIONAL,

eutra-TDD-Config6-r16 ENUMERATED {n20, n40, n50, n60, n70, n80, n90, n100} OPTIONAL

} OPTIONAL,

-- R1 18-2 Single UL TX operation for TDD PCell in EN-DC

tdm-restrictionTDD-endc-r16 ENUMERATED {supported} OPTIONAL,

-- R1 18-2a Single UL TX operation for FDD PCell in EN-DC

tdm-restrictionFDD-endc-r16 ENUMERATED {supported} OPTIONAL,

-- R1 18-2b Support of HARQ-offset for SUO case1 in EN-DC with LTE TDD PCell for type 1 UE

singleUL-HARQ-offsetTDD-PCell-r16 ENUMERATED {supported} OPTIONAL,

-- R1 18-3 Dual Tx transmission for EN-DC with FDD PCell(TDM pattern for dual Tx UE)

tdm-restrictionDualTX-FDD-endc-r16 ENUMERATED {supported} OPTIONAL

}

MRDC-Parameters-v1630 ::= SEQUENCE {

-- R4 2-20 Maximum uplink duty cycle for FDD+TDD EN-DC power class 2

maxUplinkDutyCycle-interBandENDC-FDD-TDD-PC2-r16 SEQUENCE {

maxUplinkDutyCycle-FDD-TDD-EN-DC1-r16 ENUMERATED {n30, n40, n50, n60, n70, n80, n90, n100} OPTIONAL,

maxUplinkDutyCycle-FDD-TDD-EN-DC2-r16 ENUMERATED {n30, n40, n50, n60, n70, n80, n90, n100} OPTIONAL

} OPTIONAL,

-- R4 2-19 FDD-FDD or TDD-TDD inter-band MR-DC with overlapping or partially overlapping DL spectrum

interBandMRDC-WithOverlapDL-Bands-r16 ENUMERATED {supported} OPTIONAL

}

MRDC-Parameters-v1700 ::= SEQUENCE {

condPSCellAdditionENDC-r17 ENUMERATED {supported} OPTIONAL,

scg-ActivationDeactivationENDC-r17 ENUMERATED {supported} OPTIONAL,

scg-ActivationDeactivationResumeENDC-r17 ENUMERATED {supported} OPTIONAL

}

MRDC-Parameters-v1770 ::= SEQUENCE {

-- R4 26-1: Higher Power Limit CA DC

higherPowerLimitMRDC-r17 ENUMERATED {supported} OPTIONAL

}

MRDC-Parameters-v1790 ::= SEQUENCE {

intraBandENDC-Support-v1790 ENUMERATED {non-contiguous, both} OPTIONAL,

intraBandENDC-Support-UL-v1790 ENUMERATED {non-contiguous, both} OPTIONAL

}

MRDC-Parameters-v1840 ::= SEQUENCE {

intraBandENDC-NominalSpacing-r18 ENUMERATED {supported} OPTIONAL

}

MRDC-Parameters-v1900 ::= SEQUENCE {

-- R4 47-2: Support network control of requirement for UE supporting interBandMRDC-WithOverlapDL-Bands-r19

interBandMRDC-WithOverlapDL-Bands-r19 ENUMERATED {supported} OPTIONAL

}

-- TAG-MRDC-PARAMETERS-STOP

-- ASN1STOP

#### – *NCR-Parameters*

The IE *NCR-Parameters* is used to indicate the UE capabilities supported by NCR-MT.

*NCR-Parameters* information element

-- ASN1START

-- TAG-NCR-PARAMETERS-START

NCR-Parameters-r18::= SEQUENCE {

inactiveStateNCR-r18 ENUMERATED {supported} OPTIONAL,

supportedNumberOfDRBs-NCR-r18 ENUMERATED {n1,n16} OPTIONAL,

dummy ENUMERATED {supported} OPTIONAL

}

-- TAG-NCR-PARAMETERS-STOP

-- ASN1STOP

|  |
| --- |
| *NCR-Parameters* field descriptions |
| ***dummy***  The field is not used in the specification and the network ignores the received value. |

#### – *NRDC-Parameters*

The IE *NRDC-Parameters* contains parameters specific to NR-DC, i.e., which are not applicable to NR SA.

*NRDC-Parameters* information element

-- ASN1START

-- TAG-NRDC-PARAMETERS-START

NRDC-Parameters ::= SEQUENCE {

measAndMobParametersNRDC MeasAndMobParametersMRDC OPTIONAL,

generalParametersNRDC GeneralParametersMRDC-XDD-Diff OPTIONAL,

fdd-Add-UE-NRDC-Capabilities UE-MRDC-CapabilityAddXDD-Mode OPTIONAL,

tdd-Add-UE-NRDC-Capabilities UE-MRDC-CapabilityAddXDD-Mode OPTIONAL,

fr1-Add-UE-NRDC-Capabilities UE-MRDC-CapabilityAddFRX-Mode OPTIONAL,

fr2-Add-UE-NRDC-Capabilities UE-MRDC-CapabilityAddFRX-Mode OPTIONAL,

dummy2 OCTET STRING OPTIONAL,

dummy SEQUENCE {} OPTIONAL

}

NRDC-Parameters-v1570 ::= SEQUENCE {

sfn-SyncNRDC ENUMERATED {supported} OPTIONAL

}

NRDC-Parameters-v15c0 ::= SEQUENCE {

pdcp-DuplicationSplitSRB ENUMERATED {supported} OPTIONAL,

pdcp-DuplicationSplitDRB ENUMERATED {supported} OPTIONAL

}

NRDC-Parameters-v1610 ::= SEQUENCE {

measAndMobParametersNRDC-v1610 MeasAndMobParametersMRDC-v1610 OPTIONAL

}

NRDC-Parameters-v1700 ::= SEQUENCE {

f1c-OverNR-RRC-r17 ENUMERATED {supported} OPTIONAL,

measAndMobParametersNRDC-v1700 MeasAndMobParametersMRDC-v1700

}

-- TAG-NRDC-PARAMETERS-STOP

-- ASN1STOP

#### – *NTN-Parameters*

The IE *NTN-Parameters* is used to convey the subset of UE Radio Access Capability Parameters that apply to NTN access when there is a difference compared to TN access.

*NTN-Parameters* information element

-- ASN1START

-- TAG-NTN-PARAMETERS-START

NTN-Parameters-r17 ::= SEQUENCE {

inactiveStateNTN-r17 ENUMERATED {supported} OPTIONAL,

ra-SDT-NTN-r17 ENUMERATED {supported} OPTIONAL,

srb-SDT-NTN-r17 ENUMERATED {supported} OPTIONAL,

measAndMobParametersNTN-r17 MeasAndMobParameters OPTIONAL,

mac-ParametersNTN-r17 MAC-Parameters OPTIONAL,

phy-ParametersNTN-r17 Phy-Parameters OPTIONAL,

fdd-Add-UE-NR-CapabilitiesNTN-r17 UE-NR-CapabilityAddXDD-Mode OPTIONAL,

fr1-Add-UE-NR-CapabilitiesNTN-r17 UE-NR-CapabilityAddFRX-Mode OPTIONAL,

ue-BasedPerfMeas-ParametersNTN-r17 UE-BasedPerfMeas-Parameters-r16 OPTIONAL,

son-ParametersNTN-r17 SON-Parameters-r16 OPTIONAL

}

NTN-Parameters-v1820 ::= SEQUENCE {

fr2-Add-UE-NR-CapabilitiesNTN-r18 UE-NR-CapabilityAddFRX-Mode OPTIONAL

}

-- TAG-NTN-PARAMETERS-STOP

-- ASN1STOP

|  |
| --- |
| *NTN-Parameters* field descriptions |
| ***fdd-Add-UE-NR-CapabilitiesNTN***  NTN related capabilities which the UE supports in NTN differently than in TN. If absent, *fdd-Add-UE-NR-Capabilities* applies to NTN. |
| ***fr1-Add-UE-NR-CapabilitiesNTN***  NTN related capabilities which the UE supports in NTN differently than in TN. If absent, *fr1-Add-UE-NR-Capabilities* applies to NTN. |
| ***fr2-Add-UE-NR-CapabilitiesNTN***  NTN related capabilities which the UE supports in NTN differently than in TN. If absent, *fr2-Add-UE-NR-Capabilities* applies to NTN. This field is not used in this release of specification. |
| ***mac-ParametersNTN***  NTN related capabilities which the UE supports in NTN differently than in TN. If absent, *mac-Parameters* applies to NTN. |
| ***measAndMobParametersNTN***  NTN related capabilities which the UE supports in NTN differently than in TN. If absent, *measAndMobParameters* applies to NTN. |
| ***phy-ParametersNTN***  NTN related capabilities which the UE supports in NTN differently than in TN. If absent, *phy-Parameters* applies to NTN. |
| ***son-ParametersNTN***  NTN related capabilities which the UE supports in NTN differently than in TN. If absent, *son-Parameters-r16* applies to NTN. |
| ***ue-BasedPerfMeas-ParametersNTN***  NTN related capabilities which the UE supports in NTN differently than in TN. If absent, *ue-BasedPerfMeas-Parameters-r16* applies to NTN. |

#### – *OLPC-SRS-Pos*

The IE *OLPC-SRS-Pos* is used to convey OLPC SRS positioning related parameters specific for a certain band.

*OLPC-SRS-Pos* information element

-- ASN1START

-- TAG-OLPC-SRS-POS-START

OLPC-SRS-Pos-r16 ::= SEQUENCE {

olpc-SRS-PosBasedOnPRS-Serving-r16 ENUMERATED {supported} OPTIONAL,

olpc-SRS-PosBasedOnSSB-Neigh-r16 ENUMERATED {supported} OPTIONAL,

olpc-SRS-PosBasedOnPRS-Neigh-r16 ENUMERATED {supported} OPTIONAL,

maxNumberPathLossEstimatePerServing-r16 ENUMERATED {n1, n4, n8, n16} OPTIONAL

}

--TAG-OLPC-SRS-POS-STOP

-- ASN1STOP

#### – *PDCP-Parameters*

The IE *PDCP-Parameters* is used to convey capabilities related to PDCP.

*PDCP-Parameters* information element

-- ASN1START

-- TAG-PDCP-PARAMETERS-START

PDCP-Parameters ::= SEQUENCE {

supportedROHC-Profiles SEQUENCE {

profile0x0000 BOOLEAN,

profile0x0001 BOOLEAN,

profile0x0002 BOOLEAN,

profile0x0003 BOOLEAN,

profile0x0004 BOOLEAN,

profile0x0006 BOOLEAN,

profile0x0101 BOOLEAN,

profile0x0102 BOOLEAN,

profile0x0103 BOOLEAN,

profile0x0104 BOOLEAN

},

maxNumberROHC-ContextSessions ENUMERATED {cs2, cs4, cs8, cs12, cs16, cs24, cs32, cs48, cs64,

cs128, cs256, cs512, cs1024, cs16384, spare2, spare1},

uplinkOnlyROHC-Profiles ENUMERATED {supported} OPTIONAL,

continueROHC-Context ENUMERATED {supported} OPTIONAL,

outOfOrderDelivery ENUMERATED {supported} OPTIONAL,

shortSN ENUMERATED {supported} OPTIONAL,

pdcp-DuplicationSRB ENUMERATED {supported} OPTIONAL,

pdcp-DuplicationMCG-OrSCG-DRB ENUMERATED {supported} OPTIONAL,

...,

[[

drb-IAB-r16 ENUMERATED {supported} OPTIONAL,

non-DRB-IAB-r16 ENUMERATED {supported} OPTIONAL,

extendedDiscardTimer-r16 ENUMERATED {supported} OPTIONAL,

continueEHC-Context-r16 ENUMERATED {supported} OPTIONAL,

ehc-r16 ENUMERATED {supported} OPTIONAL,

maxNumberEHC-Contexts-r16 ENUMERATED {cs2, cs4, cs8, cs16, cs32, cs64, cs128, cs256, cs512,

cs1024, cs2048, cs4096, cs8192, cs16384, cs32768, cs65536} OPTIONAL,

jointEHC-ROHC-Config-r16 ENUMERATED {supported} OPTIONAL,

pdcp-DuplicationMoreThanTwoRLC-r16 ENUMERATED {supported} OPTIONAL

]],

[[

longSN-RedCap-r17 ENUMERATED {supported} OPTIONAL,

udc-r17 SEQUENCE {

standardDictionary-r17 ENUMERATED {supported} OPTIONAL,

operatorDictionary-r17 SEQUENCE {

versionOfDictionary-r17 INTEGER (0..15),

associatedPLMN-ID-r17 PLMN-Identity

} OPTIONAL,

continueUDC-r17 ENUMERATED {supported} OPTIONAL,

supportOfBufferSize-r17 ENUMERATED {kbyte4, kbyte8} OPTIONAL

} OPTIONAL

]],

[[

longSN-NCR-r18 ENUMERATED {supported} OPTIONAL,

supportOfPDU-SetDiscard-r18 ENUMERATED {supported} OPTIONAL,

psi-BasedDiscard-r18 ENUMERATED {supported} OPTIONAL,

supportOfSN-GapReport-r18 ENUMERATED {supported} OPTIONAL

]]

}

-- TAG-PDCP-PARAMETERS-STOP

-- ASN1STOP

#### – *PDCP-ParametersMRDC*

The IE *PDCP-ParametersMRDC* is used to convey PDCP related capabilities for MR-DC.

*PDCP-ParametersMRDC* information element

-- ASN1START

-- TAG-PDCP-PARAMETERSMRDC-START

PDCP-ParametersMRDC ::= SEQUENCE {

pdcp-DuplicationSplitSRB ENUMERATED {supported} OPTIONAL,

pdcp-DuplicationSplitDRB ENUMERATED {supported} OPTIONAL

}

PDCP-ParametersMRDC-v1610 ::= SEQUENCE {

scg-DRB-NR-IAB-r16 ENUMERATED {supported} OPTIONAL

}

-- TAG-PDCP-PARAMETERSMRDC-STOP

-- ASN1STOP

#### – *Phy-Parameters*

The IE *Phy-Parameters* is used to convey the physical layer capabilities.

*Phy-Parameters* information element

-- ASN1START

-- TAG-PHY-PARAMETERS-START

Phy-Parameters ::= SEQUENCE {

phy-ParametersCommon Phy-ParametersCommon OPTIONAL,

phy-ParametersXDD-Diff Phy-ParametersXDD-Diff OPTIONAL,

phy-ParametersFRX-Diff Phy-ParametersFRX-Diff OPTIONAL,

phy-ParametersFR1 Phy-ParametersFR1 OPTIONAL,

phy-ParametersFR2 Phy-ParametersFR2 OPTIONAL

}

Phy-Parameters-v16a0 ::= SEQUENCE {

phy-ParametersCommon-v16a0 Phy-ParametersCommon-v16a0 OPTIONAL

}

Phy-ParametersCommon ::= SEQUENCE {

csi-RS-CFRA-ForHO ENUMERATED {supported} OPTIONAL,

dynamicPRB-BundlingDL ENUMERATED {supported} OPTIONAL,

sp-CSI-ReportPUCCH ENUMERATED {supported} OPTIONAL,

sp-CSI-ReportPUSCH ENUMERATED {supported} OPTIONAL,

nzp-CSI-RS-IntefMgmt ENUMERATED {supported} OPTIONAL,

type2-SP-CSI-Feedback-LongPUCCH ENUMERATED {supported} OPTIONAL,

precoderGranularityCORESET ENUMERATED {supported} OPTIONAL,

dynamicHARQ-ACK-Codebook ENUMERATED {supported} OPTIONAL,

semiStaticHARQ-ACK-Codebook ENUMERATED {supported} OPTIONAL,

spatialBundlingHARQ-ACK ENUMERATED {supported} OPTIONAL,

dynamicBetaOffsetInd-HARQ-ACK-CSI ENUMERATED {supported} OPTIONAL,

pucch-Repetition-F1-3-4 ENUMERATED {supported} OPTIONAL,

ra-Type0-PUSCH ENUMERATED {supported} OPTIONAL,

dynamicSwitchRA-Type0-1-PDSCH ENUMERATED {supported} OPTIONAL,

dynamicSwitchRA-Type0-1-PUSCH ENUMERATED {supported} OPTIONAL,

pdsch-MappingTypeA ENUMERATED {supported} OPTIONAL,

pdsch-MappingTypeB ENUMERATED {supported} OPTIONAL,

interleavingVRB-ToPRB-PDSCH ENUMERATED {supported} OPTIONAL,

interSlotFreqHopping-PUSCH ENUMERATED {supported} OPTIONAL,

type1-PUSCH-RepetitionMultiSlots ENUMERATED {supported} OPTIONAL,

type2-PUSCH-RepetitionMultiSlots ENUMERATED {supported} OPTIONAL,

pusch-RepetitionMultiSlots ENUMERATED {supported} OPTIONAL,

pdsch-RepetitionMultiSlots ENUMERATED {supported} OPTIONAL,

downlinkSPS ENUMERATED {supported} OPTIONAL,

configuredUL-GrantType1 ENUMERATED {supported} OPTIONAL,

configuredUL-GrantType2 ENUMERATED {supported} OPTIONAL,

pre-EmptIndication-DL ENUMERATED {supported} OPTIONAL,

cbg-TransIndication-DL ENUMERATED {supported} OPTIONAL,

cbg-TransIndication-UL ENUMERATED {supported} OPTIONAL,

cbg-FlushIndication-DL ENUMERATED {supported} OPTIONAL,

dynamicHARQ-ACK-CodeB-CBG-Retx-DL ENUMERATED {supported} OPTIONAL,

rateMatchingResrcSetSemi-Static ENUMERATED {supported} OPTIONAL,

rateMatchingResrcSetDynamic ENUMERATED {supported} OPTIONAL,

bwp-SwitchingDelay ENUMERATED {type1, type2} OPTIONAL,

...,

[[

dummy ENUMERATED {supported} OPTIONAL

]],

[[

maxNumberSearchSpaces ENUMERATED {n10} OPTIONAL,

rateMatchingCtrlResrcSetDynamic ENUMERATED {supported} OPTIONAL,

maxLayersMIMO-Indication ENUMERATED {supported} OPTIONAL

]],

[[

spCellPlacement CarrierAggregationVariant OPTIONAL

]],

[[

-- R1 9-1: Basic channel structure and procedure of 2-step RACH

twoStepRACH-r16 ENUMERATED {supported} OPTIONAL,

-- R1 11-1: Monitoring DCI format 1\_2 and DCI format 0\_2

dci-Format1-2And0-2-r16 ENUMERATED {supported} OPTIONAL,

-- R1 11-1a: Monitoring both DCI format 0\_1/1\_1 and DCI format 0\_2/1\_2 in the same search space

monitoringDCI-SameSearchSpace-r16 ENUMERATED {supported} OPTIONAL,

-- R1 11-10: Type 2 configured grant release by DCI format 0\_1

type2-CG-ReleaseDCI-0-1-r16 ENUMERATED {supported} OPTIONAL,

-- R1 11-11: Type 2 configured grant release by DCI format 0\_2

type2-CG-ReleaseDCI-0-2-r16 ENUMERATED {supported} OPTIONAL,

-- R1 12-3: SPS release by DCI format 1\_1

sps-ReleaseDCI-1-1-r16 ENUMERATED {supported} OPTIONAL,

-- R1 12-3a: SPS release by DCI format 1\_2

sps-ReleaseDCI-1-2-r16 ENUMERATED {supported} OPTIONAL,

-- R1 14-8: CSI trigger states containing non-active BWP

csi-TriggerStateNon-ActiveBWP-r16 ENUMERATED {supported} OPTIONAL,

-- R1 20-2: Support up to 4 SMTCs configured for an IAB node MT per frequency location, including IAB-specific SMTC window periodicities

separateSMTC-InterIAB-Support-r16 ENUMERATED {supported} OPTIONAL,

-- R1 20-3: Support RACH configuration separately from the RACH configuration for UE access, including new IAB-specific offset and scaling factors

separateRACH-IAB-Support-r16 ENUMERATED {supported} OPTIONAL,

-- R1 20-5a: Support semi-static configuration/indication of UL-Flexible-DL slot formats for IAB-MT resources

ul-flexibleDL-SlotFormatSemiStatic-IAB-r16 ENUMERATED {supported} OPTIONAL,

-- R1 20-5b: Support dynamic indication of UL-Flexible-DL slot formats for IAB-MT resources

ul-flexibleDL-SlotFormatDynamics-IAB-r16 ENUMERATED {supported} OPTIONAL,

dft-S-OFDM-WaveformUL-IAB-r16 ENUMERATED {supported} OPTIONAL,

-- R1 20-6: Support DCI Format 2\_5 based indication of soft resource availability to an IAB node

dci-25-AI-RNTI-Support-IAB-r16 ENUMERATED {supported} OPTIONAL,

-- R1 20-7: Support T\_delta reception.

t-DeltaReceptionSupport-IAB-r16 ENUMERATED {supported} OPTIONAL,

-- R1 20-8: Support of Desired guard symbol reporting and provided guard symbok reception.

guardSymbolReportReception-IAB-r16 ENUMERATED {supported} OPTIONAL,

-- R1 18-8 HARQ-ACK codebook type and spatial bundling per PUCCH group

harqACK-CB-SpatialBundlingPUCCH-Group-r16 ENUMERATED {supported} OPTIONAL,

-- R1 19-2: Cross Slot Scheduling

crossSlotScheduling-r16 SEQUENCE {

non-SharedSpectrumChAccess-r16 ENUMERATED {supported} OPTIONAL,

sharedSpectrumChAccess-r16 ENUMERATED {supported} OPTIONAL

} OPTIONAL,

maxNumberSRS-PosPathLossEstimateAllServingCells-r16 ENUMERATED {n1, n4, n8, n16} OPTIONAL,

extendedCG-Periodicities-r16 ENUMERATED {supported} OPTIONAL,

extendedSPS-Periodicities-r16 ENUMERATED {supported} OPTIONAL,

codebookVariantsList-r16 CodebookVariantsList-r16 OPTIONAL,

-- R1 11-6: PUSCH repetition Type A

pusch-RepetitionTypeA-r16 SEQUENCE {

sharedSpectrumChAccess-r16 ENUMERATED {supported} OPTIONAL,

non-SharedSpectrumChAccess-r16 ENUMERATED {supported} OPTIONAL

} OPTIONAL,

-- R1 11-4b: DL priority indication in DCI with mixed DCI formats

dci-DL-PriorityIndicator-r16 ENUMERATED {supported} OPTIONAL,

-- R1 12-1a: UL priority indication in DCI with mixed DCI formats

dci-UL-PriorityIndicator-r16 ENUMERATED {supported} OPTIONAL,

-- R1 16-1e: Maximum number of configured pathloss reference RSs for PUSCH/PUCCH/SRS by RRC for MAC-CE based pathloss reference RS update

maxNumberPathlossRS-Update-r16 ENUMERATED {n4, n8, n16, n32, n64} OPTIONAL,

-- R1 18-9: Usage of the PDSCH starting time for HARQ-ACK type 2 codebook

type2-HARQ-ACK-Codebook-r16 ENUMERATED {supported} OPTIONAL,

-- R1 16-1g-1: Resources for beam management, pathloss measurement, BFD, RLM and new beam identification across frequency ranges

maxTotalResourcesForAcrossFreqRanges-r16 SEQUENCE {

maxNumberResWithinSlotAcrossCC-AcrossFR-r16 ENUMERATED {n2, n4, n8, n12, n16, n32, n64, n128} OPTIONAL,

maxNumberResAcrossCC-AcrossFR-r16 ENUMERATED {n2, n4, n8, n12, n16, n32, n40, n48, n64, n72, n80, n96, n128, n256}

OPTIONAL

} OPTIONAL,

-- R1 16-2a-4: HARQ-ACK for multi-DCI based multi-TRP - separate

harqACK-separateMultiDCI-MultiTRP-r16 SEQUENCE {

maxNumberLongPUCCHs-r16 ENUMERATED {longAndLong, longAndShort, shortAndShort} OPTIONAL

} OPTIONAL,

-- R1 16-2a-4: HARQ-ACK for multi-DCI based multi-TRP - joint

harqACK-jointMultiDCI-MultiTRP-r16 ENUMERATED {supported} OPTIONAL,

-- R4 9-1: BWP switching on multiple CCs RRM requirements

bwp-SwitchingMultiCCs-r16 CHOICE {

type1-r16 ENUMERATED {us100, us200},

type2-r16 ENUMERATED {us200, us400, us800, us1000}

} OPTIONAL

]],

[[

targetSMTC-SCG-r16 ENUMERATED {supported} OPTIONAL,

supportRepetitionZeroOffsetRV-r16 ENUMERATED {supported} OPTIONAL,

-- R1 11-12: in-order CBG-based re-transmission

cbg-TransInOrderPUSCH-UL-r16 ENUMERATED {supported} OPTIONAL

]],

[[

-- R4 6-3: Dormant BWP switching on multiple CCs RRM requirements

bwp-SwitchingMultiDormancyCCs-r16 CHOICE {

type1-r16 ENUMERATED {us100, us200},

type2-r16 ENUMERATED {us200, us400, us800, us1000}

} OPTIONAL,

-- R1 16-2a-8: Indicates that retransmission scheduled by a different CORESETPoolIndex for multi-DCI multi-TRP is not supported.

supportRetx-Diff-CoresetPool-Multi-DCI-TRP-r16 ENUMERATED {notSupported} OPTIONAL,

-- R1 22-10: Support of pdcch-MonitoringAnyOccasionsWithSpanGap in case of cross-carrier scheduling with different SCSs

pdcch-MonitoringAnyOccasionsWithSpanGapCrossCarrierSch-r16 ENUMERATED {mode2, mode3} OPTIONAL

]],

[[

-- R1 16-1j-1: Support of 2 port CSI-RS for new beam identification

newBeamIdentifications2PortCSI-RS-r16 ENUMERATED {supported} OPTIONAL,

-- R1 16-1j-2: Support of 2 port CSI-RS for pathloss estimation

pathlossEstimation2PortCSI-RS-r16 ENUMERATED {supported} OPTIONAL

]],

[[

mux-HARQ-ACK-withoutPUCCH-onPUSCH-r16 ENUMERATED {supported} OPTIONAL

]],

[[

-- R1 31-1: Support of Desired Guard Symbol reporting and provided guard symbol reception.

guardSymbolReportReception-IAB-r17 ENUMERATED {supported} OPTIONAL,

-- R1 31-2: support of restricted IAB-DU beam reception

restricted-IAB-DU-BeamReception-r17 ENUMERATED {supported} OPTIONAL,

-- R1 31-3: support of recommended IAB-MT beam transmission for DL and UL beam

recommended-IAB-MT-BeamTransmission-r17 ENUMERATED {supported} OPTIONAL,

-- R1 31-4: support of case 6 timing alignment indication reception

case6-TimingAlignmentReception-IAB-r17 ENUMERATED {supported} OPTIONAL,

-- R1 31-5: support of case 7 timing offset indication reception and case 7 timing at parent-node indication reception

case7-TimingAlignmentReception-IAB-r17 ENUMERATED {supported} OPTIONAL,

-- R1 31-6: support of desired DL Tx power adjustment reporting and DL Tx power adjustment reception

dl-tx-PowerAdjustment-IAB-r17 ENUMERATED {supported} OPTIONAL,

-- R1 31-7: support of desired IAB-MT PSD range reporting

desired-ul-tx-PowerAdjustment-r17 ENUMERATED {supported} OPTIONAL,

-- R1 31-8: support of monitoring DCI Format 2\_5 scrambled by AI-RNTI for indication of FDM soft resource availability to an IAB node

fdm-SoftResourceAvailability-DynamicIndication-r17 ENUMERATED{supported} OPTIONAL,

-- R1 31-10: Support of updated T\_delta range reception

updated-T-DeltaRangeReception-r17 ENUMERATED{supported} OPTIONAL,

-- R1 30-5: Support slot based dynamic PUCCH repetition indication for PUCCH formats 0/1/2/3/4

slotBasedDynamicPUCCH-Rep-r17 ENUMERATED {supported} OPTIONAL,

-- R1 25-1: Support of HARQ-ACK deferral in case of TDD collision

sps-HARQ-ACK-Deferral-r17 SEQUENCE {

non-SharedSpectrumChAccess-r17 ENUMERATED {supported} OPTIONAL,

sharedSpectrumChAccess-r17 ENUMERATED {supported} OPTIONAL

} OPTIONAL,

-- R1 23-1-1k Maximum number of configured CC lists (per UE)

unifiedJointTCI-commonUpdate-r17 INTEGER (1..4) OPTIONAL,

-- R1 23-2-1c PDCCH repetition with a single span of three contiguous OFDM symbols that is within the first four OFDM symbols in a slot

mTRP-PDCCH-singleSpan-r17 ENUMERATED {supported} OPTIONAL,

-- R1 27-23: Support of more than one activated PRS processing windows across all active DL BWPs

supportedActivatedPRS-ProcessingWindow-r17 ENUMERATED {n2, n3, n4} OPTIONAL,

cg-TimeDomainAllocationExtension-r17 ENUMERATED {supported} OPTIONAL

]],

[[

-- R1 25-20: Propagation delay compensation based on Rel-15 TA procedure for TN and licensed

ta-BasedPDC-TN-NonSharedSpectrumChAccess-r17 ENUMERATED {supported} OPTIONAL,

-- R1 31-11: Directional Collision Handling in DC operation

directionalCollisionDC-IAB-r17 ENUMERATED {supported} OPTIONAL

]],

[[

dummy1 ENUMERATED {supported} OPTIONAL,

dummy2 ENUMERATED {supported} OPTIONAL,

dummy3 ENUMERATED {supported} OPTIONAL,

dummy4 ENUMERATED {supported} OPTIONAL,

srs-AdditionalRepetition-r17 ENUMERATED {supported} OPTIONAL,

pusch-Repetition-CG-SDT-r17 ENUMERATED {supported} OPTIONAL

]],

[[

multiPDSCH-PerSlotType1-CB-Support-r17 ENUMERATED {supported} OPTIONAL

]],

[[

-- R1 42-6: Joint operation of power domain and spatial domain adaptation

jointPowerSpatialAdaptation-r18 ENUMERATED {supported} OPTIONAL,

-- R1 43-3: Aperiodic beam indication for access link

ncr-AperiodicBeamInd-AccessLink-r18 SEQUENCE {

scs-15kHz-r18 INTEGER (0..1) OPTIONAL,

scs-30kHz-r18 INTEGER (0..1) OPTIONAL,

scs-60kHz-r18 INTEGER (0..2) OPTIONAL,

scs-120kHz-r18 INTEGER (0..2) OPTIONAL

} OPTIONAL,

-- R1 43-4: Semi-persistent beam indication for access link

ncr-Semi-PersistentBeamInd-AccessLink-r18 ENUMERATED {supported} OPTIONAL,

-- R1 43-5: Simulatenous UL transmission of backhaul link and C-Link

ncr-SimultaneousUL-BackhaulAndC-Link-r18 ENUMERATED {supported} OPTIONAL,

-- R1 43-6: Dedicated signalling for backhaul link beam indication

ncr-BackhaulBeamInd-r18 ENUMERATED {nonUnifiedTCI, unifiedTCI, both} OPTIONAL,

-- R1 43-8: Adaptive beam for NCR backhaul link/C-link

ncr-AdaptiveBeamBackhaulAndC-Link-r18 ENUMERATED {nonUnifiedTCI, unifiedTCI, both} OPTIONAL,

-- R1 49-4a: Nominal RBG size of Configuration 3 for FDRA type 0 for DCI format 1\_3

nominalRBG-SizeOfConfig-3-FDRA-Type-0-DCI-1-3-r18 ENUMERATED {supported} OPTIONAL,

-- R1 49-4b: Nominal RBG size of Configuration 3 for FDRA type 0 for DCI format 0\_3

nominalRBG-SizeOfConfig-3-FDRA-Type-0-DCI-0-3-r18 ENUMERATED {supported} OPTIONAL,

-- R1 49-4c: Configurable Type-1A fields for DCI format 0\_3/1\_3

configurableType-1A-FieldsForDCI-0-3-And-1-3-r18 ENUMERATED {supported} OPTIONAL,

-- R1 49-4d: FDRA Type 1 granularity of 2, 4, 8, or 16 consecutive RBs based RIV for DCI format 1\_3/0\_3

fdra-Type-1-Gty-2-4-8-16-RBs-RIV-DCI-1-3-And-0-3-r18 ENUMERATED {supported} OPTIONAL,

-- R1 49-6b: DL priority indication in DCI with mixed DCI formats including DCI format 1\_3

priorityIndicationDL-r18 ENUMERATED {supported} OPTIONAL,

-- R1 49-7a: UL priority indication in DCI with mixed DCI formats including DCI format 0\_3

priorityIndicationUL-r18 ENUMERATED {supported} OPTIONAL,

-- R1 49-10: Dynamic indication of applicable minimum scheduling restriction by DCI format 0\_3/1\_3

dynamicIndicationSchedulingRestriction-r18 ENUMERATED {supported} OPTIONAL,

-- R1 49-11: PHY priority indication for one-shot HARQ-ACK feedback triggered by DCI format 1\_3

priorityIndicationOneSlotHARQ-r18 ENUMERATED {supported} OPTIONAL,

-- R1 50-1c: Multi-PUSCHs Type 2 configured grant release by DCI format 0\_1

multiPUSCH-DCI-0-1-r18 ENUMERATED {supported} OPTIONAL,

-- R1 50-1d: Multi-PUSCHs Type 2 configured grant release by DCI format 0\_2

multiPUSCH-DCI-0-2-r18 ENUMERATED {supported} OPTIONAL,

-- R1 55-1: Additional SR periodicities

additionalSR-Periodicities-r18 SEQUENCE {

scs-30kHz-r18 ENUMERATED {supported} OPTIONAL,

scs-120kHz-r18 ENUMERATED {supported} OPTIONAL

} OPTIONAL,

-- R1 55-5: Enable MAC CE based pathloss RS updates for Type 1 CG-PUSCH

pathlossRS-UpdateForType1CG-PUSCH-r18 ENUMERATED {supported} OPTIONAL,

-- R4 38-9: Dormant BWP switching on multiple CCs RRM requirements with DCI 0-3/1-3

bwp-SwitchingMultiDormancyCC-DCI-0-3-And-1-3-r18 CHOICE {

type1-r18 ENUMERATED {us100, us200},

type2-r18 ENUMERATED {us200, us400, us800, us1000}

} OPTIONAL

]],

[[

ncr-dft-S-OFDM-WaveformUL-r18 ENUMERATED {supported} OPTIONAL

]],

[[

codebookVariantsListExt-r19 CodebookVariantsListExt-r19 OPTIONAL,

codebookVariantsListAggregate-r19 CodebookVariantsListAggregate-r19 OPTIONAL,

codebookVariantsListHybrid-r19 CodebookVariantsListHybrid-r19 OPTIONAL,

-- R1 58-1-2: UE-side beam prediction for BM Case1 for inference

aiml-BM-Case1-r19 ENUMERATED {supported} OPTIONAL,

-- R1 58-1-4: UE-side beam prediction for BM Case2 for inferenc

aiml-BM-Case2-r19 ENUMERATED {supported} OPTIONAL,

-- R1 64-1: Enabling TX/RX during measurement gap scheduling restriction

enableTx-RxDuringMeasGap-r19 SEQUENCE {

additionalDCI-r19 BIT STRING (SIZE (3)),

indicationField-r19 ENUMERATED {option1,option2},

minimumTimeOffset-r19 ENUMERATED {ms5,ms3}

} OPTIONAL

]]

}

Phy-ParametersCommon-v16a0 ::= SEQUENCE {

srs-PeriodicityAndOffsetExt-r16 ENUMERATED {supported} OPTIONAL

}

Phy-ParametersXDD-Diff ::= SEQUENCE {

dynamicSFI ENUMERATED {supported} OPTIONAL,

twoPUCCH-F0-2-ConsecSymbols ENUMERATED {supported} OPTIONAL,

twoDifferentTPC-Loop-PUSCH ENUMERATED {supported} OPTIONAL,

twoDifferentTPC-Loop-PUCCH ENUMERATED {supported} OPTIONAL,

...,

[[

dl-SchedulingOffset-PDSCH-TypeA ENUMERATED {supported} OPTIONAL,

dl-SchedulingOffset-PDSCH-TypeB ENUMERATED {supported} OPTIONAL,

ul-SchedulingOffset ENUMERATED {supported} OPTIONAL

]]

}

Phy-ParametersFRX-Diff ::= SEQUENCE {

dynamicSFI ENUMERATED {supported} OPTIONAL,

dummy1 BIT STRING (SIZE (2)) OPTIONAL,

twoFL-DMRS BIT STRING (SIZE (2)) OPTIONAL,

dummy2 BIT STRING (SIZE (2)) OPTIONAL,

dummy3 BIT STRING (SIZE (2)) OPTIONAL,

supportedDMRS-TypeDL ENUMERATED {type1, type1And2} OPTIONAL,

supportedDMRS-TypeUL ENUMERATED {type1, type1And2} OPTIONAL,

semiOpenLoopCSI ENUMERATED {supported} OPTIONAL,

csi-ReportWithoutPMI ENUMERATED {supported} OPTIONAL,

csi-ReportWithoutCQI ENUMERATED {supported} OPTIONAL,

onePortsPTRS BIT STRING (SIZE (2)) OPTIONAL,

twoPUCCH-F0-2-ConsecSymbols ENUMERATED {supported} OPTIONAL,

pucch-F2-WithFH ENUMERATED {supported} OPTIONAL,

pucch-F3-WithFH ENUMERATED {supported} OPTIONAL,

pucch-F4-WithFH ENUMERATED {supported} OPTIONAL,

pucch-F0-2WithoutFH ENUMERATED {notSupported} OPTIONAL,

pucch-F1-3-4WithoutFH ENUMERATED {notSupported} OPTIONAL,

mux-SR-HARQ-ACK-CSI-PUCCH-MultiPerSlot ENUMERATED {supported} OPTIONAL,

uci-CodeBlockSegmentation ENUMERATED {supported} OPTIONAL,

onePUCCH-LongAndShortFormat ENUMERATED {supported} OPTIONAL,

twoPUCCH-AnyOthersInSlot ENUMERATED {supported} OPTIONAL,

intraSlotFreqHopping-PUSCH ENUMERATED {supported} OPTIONAL,

pusch-LBRM ENUMERATED {supported} OPTIONAL,

pdcch-BlindDetectionCA INTEGER (4..16) OPTIONAL,

tpc-PUSCH-RNTI ENUMERATED {supported} OPTIONAL,

tpc-PUCCH-RNTI ENUMERATED {supported} OPTIONAL,

tpc-SRS-RNTI ENUMERATED {supported} OPTIONAL,

absoluteTPC-Command ENUMERATED {supported} OPTIONAL,

twoDifferentTPC-Loop-PUSCH ENUMERATED {supported} OPTIONAL,

twoDifferentTPC-Loop-PUCCH ENUMERATED {supported} OPTIONAL,

pusch-HalfPi-BPSK ENUMERATED {supported} OPTIONAL,

pucch-F3-4-HalfPi-BPSK ENUMERATED {supported} OPTIONAL,

almostContiguousCP-OFDM-UL ENUMERATED {supported} OPTIONAL,

sp-CSI-RS ENUMERATED {supported} OPTIONAL,

sp-CSI-IM ENUMERATED {supported} OPTIONAL,

tdd-MultiDL-UL-SwitchPerSlot ENUMERATED {supported} OPTIONAL,

multipleCORESET ENUMERATED {supported} OPTIONAL,

...,

[[

csi-RS-IM-ReceptionForFeedback CSI-RS-IM-ReceptionForFeedback OPTIONAL,

csi-RS-ProcFrameworkForSRS CSI-RS-ProcFrameworkForSRS OPTIONAL,

csi-ReportFramework CSI-ReportFramework OPTIONAL,

mux-SR-HARQ-ACK-CSI-PUCCH-OncePerSlot SEQUENCE {

sameSymbol ENUMERATED {supported} OPTIONAL,

diffSymbol ENUMERATED {supported} OPTIONAL

} OPTIONAL,

mux-SR-HARQ-ACK-PUCCH ENUMERATED {supported} OPTIONAL,

mux-MultipleGroupCtrlCH-Overlap ENUMERATED {supported} OPTIONAL,

dl-SchedulingOffset-PDSCH-TypeA ENUMERATED {supported} OPTIONAL,

dl-SchedulingOffset-PDSCH-TypeB ENUMERATED {supported} OPTIONAL,

ul-SchedulingOffset ENUMERATED {supported} OPTIONAL,

dl-64QAM-MCS-TableAlt ENUMERATED {supported} OPTIONAL,

ul-64QAM-MCS-TableAlt ENUMERATED {supported} OPTIONAL,

cqi-TableAlt ENUMERATED {supported} OPTIONAL,

oneFL-DMRS-TwoAdditionalDMRS-UL ENUMERATED {supported} OPTIONAL,

twoFL-DMRS-TwoAdditionalDMRS-UL ENUMERATED {supported} OPTIONAL,

oneFL-DMRS-ThreeAdditionalDMRS-UL ENUMERATED {supported} OPTIONAL

]],

[[

pdcch-BlindDetectionNRDC SEQUENCE {

pdcch-BlindDetectionMCG-UE INTEGER (1..15),

pdcch-BlindDetectionSCG-UE INTEGER (1..15)

} OPTIONAL,

mux-HARQ-ACK-PUSCH-DiffSymbol ENUMERATED {supported} OPTIONAL

]],

[[

-- R1 11-1b: Type 1 HARQ-ACK codebook support for relative TDRA for DL

type1-HARQ-ACK-Codebook-r16 ENUMERATED {supported} OPTIONAL,

-- R1 11-8: Enhanced UL power control scheme

enhancedPowerControl-r16 ENUMERATED {supported} OPTIONAL,

-- R1 16-1b-1: TCI state activation across multiple CCs

simultaneousTCI-ActMultipleCC-r16 ENUMERATED {supported} OPTIONAL,

-- R1 16-1b-2: Spatial relation update across multiple CCs

simultaneousSpatialRelationMultipleCC-r16 ENUMERATED {supported} OPTIONAL,

cli-RSSI-FDM-DL-r16 ENUMERATED {supported} OPTIONAL,

cli-SRS-RSRP-FDM-DL-r16 ENUMERATED {supported} OPTIONAL,

-- R1 19-3: Maximum MIMO Layer Adaptation

maxLayersMIMO-Adaptation-r16 ENUMERATED {supported} OPTIONAL,

-- R1 12-5: Configuration of aggregation factor per SPS configuration

aggregationFactorSPS-DL-r16 ENUMERATED {supported} OPTIONAL,

-- R1 16-1g: Resources for beam management, pathloss measurement, BFD, RLM and new beam identification

maxTotalResourcesForOneFreqRange-r16 SEQUENCE {

maxNumberResWithinSlotAcrossCC-OneFR-r16 ENUMERATED {n2, n4, n8, n12, n16, n32, n64, n128} OPTIONAL,

maxNumberResAcrossCC-OneFR-r16 ENUMERATED {n2, n4, n8, n12, n16, n32, n40, n48, n64, n72, n80, n96, n128, n256}

OPTIONAL

} OPTIONAL,

-- R1 16-7: Extension of the maximum number of configured aperiodic CSI report settings

csi-ReportFrameworkExt-r16 CSI-ReportFrameworkExt-r16 OPTIONAL

]],

[[

twoTCI-Act-servingCellInCC-List-r16 ENUMERATED {supported} OPTIONAL

]],

[[

-- R1 22-11: Support of 'cri-RI-CQI' report without non-PMI-PortIndication

cri-RI-CQI-WithoutNon-PMI-PortInd-r16 ENUMERATED {supported} OPTIONAL

]],

[[

-- R1 25-11: 4-bits subband CQI for TN and licensed

cqi-4-BitsSubbandTN-NonSharedSpectrumChAccess-r17 ENUMERATED {supported} OPTIONAL

]],

[[

multipleCORESET-RedCap-r17 ENUMERATED {supported} OPTIONAL

]]

}

Phy-ParametersFR1 ::= SEQUENCE {

pdcch-MonitoringSingleOccasion ENUMERATED {supported} OPTIONAL,

scs-60kHz ENUMERATED {supported} OPTIONAL,

pdsch-256QAM-FR1 ENUMERATED {supported} OPTIONAL,

pdsch-RE-MappingFR1-PerSymbol ENUMERATED {n10, n20} OPTIONAL,

...,

[[

pdsch-RE-MappingFR1-PerSlot ENUMERATED {n16, n32, n48, n64, n80, n96, n112, n128,

n144, n160, n176, n192, n208, n224, n240, n256} OPTIONAL

]],

[[

-- R1 22-12: PDCCH monitoring with a single span of three contiguous OFDM symbols that is within the first four OFDM symbols in a

-- slot

pdcch-MonitoringSingleSpanFirst4Sym-r16 ENUMERATED {supported} OPTIONAL

]],

[[

-- R1 56-4: K1 range extension defined for ATG as well

k1-RangeExtensionATG-r18 ENUMERATED {supported} OPTIONAL,

-- R1 56-3: Increasing the number of HARQ processes defined for ATG as well

maxHARQ-ProcessNumberATG-r18 ENUMERATED {u16d32, u32d16, u32d32} OPTIONAL,

-- R1 56-1: Uplink Time and Frequency pre-compensation and timing relationship enhancements defined for ATG as well

uplinkPreCompensationATG-r18 ENUMERATED {supported} OPTIONAL,

-- R1 56-2: UE reporting of TA information

uplinkTA-ReportingATG-r18 ENUMERATED {supported} OPTIONAL,

-- R4 36-1: MU-MIMO Interference Mitigation advanced receiver

advReceiver-MU-MIMO-r18 ENUMERATED {supported} OPTIONAL,

-- R4 41-1: Support of delta PPowerClass reporting mechanism

deltaPowerClassReporting-r18 ENUMERATED {type1, type2} OPTIONAL,

-- R1 51-2b: Support 12 PRB CORESET0 with an associated SS/PBCH block located at GSCN 41637

support12PRB-CORESET0-GSCN-41637-r18 ENUMERATED {supported} OPTIONAL,

-- R1 51-3: Support 5 MHz channel bandwidth with 20 PRB CORESET0

support5MHz-ChannelBW-20PRB-CORESET0-r18 ENUMERATED {supported} OPTIONAL

]]

}

Phy-ParametersFR2 ::= SEQUENCE {

dummy ENUMERATED {supported} OPTIONAL,

pdsch-RE-MappingFR2-PerSymbol ENUMERATED {n6, n20} OPTIONAL,

...,

[[

pCell-FR2 ENUMERATED {supported} OPTIONAL,

pdsch-RE-MappingFR2-PerSlot ENUMERATED {n16, n32, n48, n64, n80, n96, n112, n128,

n144, n160, n176, n192, n208, n224, n240, n256} OPTIONAL

]],

[[

-- R1 16-1c: Support of default spatial relation and pathloss reference RS for dedicated-PUCCH/SRS and PUSCH

defaultSpatialRelationPathlossRS-r16 ENUMERATED {supported} OPTIONAL,

-- R1 16-1d: Support of spatial relation update for AP-SRS via MAC CE

spatialRelationUpdateAP-SRS-r16 ENUMERATED {supported} OPTIONAL,

maxNumberSRS-PosSpatialRelationsAllServingCells-r16 ENUMERATED {n0, n1, n2, n4, n8, n16} OPTIONAL

]],

[[

-- R4 30-3: Supports Indication of multi-Rx operation preference

multiRxPreferenceIndication-r18 ENUMERATED {supported} OPTIONAL

]]

}

-- TAG-PHY-PARAMETERS-STOP

-- ASN1STOP

|  |
| --- |
| *Phy-ParametersFRX-Diff* field descriptions |
| ***csi-RS-IM-ReceptionForFeedback/ csi-RS-ProcFrameworkForSRS/ csi-ReportFramework***  These fields are optionally present in *fr1-fr2-Add-UE-NR-Capabilities* in *UE-NR-Capability*. They shall not be set in any other instance of the IE *Phy-ParametersFRX-Diff*. If the network configures the UE with serving cells on both FR1 and FR2 bands, these parameters, if present, limit the corresponding parameters in *MIMO-ParametersPerBand*. |

#### – *Phy-ParametersMRDC*

The IE *Phy-ParametersMRDC* is used to convey physical layer capabilities for MR-DC.

*Phy-ParametersMRDC* information element

-- ASN1START

-- TAG-PHY-PARAMETERSMRDC-START

Phy-ParametersMRDC ::= SEQUENCE {

naics-Capability-List SEQUENCE (SIZE (1..maxNrofNAICS-Entries)) OF NAICS-Capability-Entry OPTIONAL,

...,

[[

spCellPlacement CarrierAggregationVariant OPTIONAL

]],

[[

-- R1 18-3b: Semi-statically configured LTE UL transmissions in all UL subframes not limited to tdm-pattern in case of TDD PCell

tdd-PCellUL-TX-AllUL-Subframe-r16 ENUMERATED {supported} OPTIONAL,

-- R1 18-3a: Semi-statically configured LTE UL transmissions in all UL subframes not limited to tdm-pattern in case of FDD PCell

fdd-PCellUL-TX-AllUL-Subframe-r16 ENUMERATED {supported} OPTIONAL

]]

}

NAICS-Capability-Entry ::= SEQUENCE {

numberOfNAICS-CapableCC INTEGER(1..5),

numberOfAggregatedPRB ENUMERATED {n50, n75, n100, n125, n150, n175, n200, n225,

n250, n275, n300, n350, n400, n450, n500, spare},

...

}

-- TAG-PHY-PARAMETERSMRDC-STOP

-- ASN1STOP

|  |
| --- |
| *PHY-ParametersMRDC* field descriptions |
| ***naics-Capability-List***  Indicates that UE in MR-DC supports NAICS as defined in TS 36.331 [10]. |

#### – *Phy-ParametersSharedSpectrumChAccess*

The IE *Phy-ParametersSharedSpectrumChAccess* is used to convey the physical layer capabilities specific for shared spectrum channel access.

*Phy-ParametersSharedSpectrumChAccess* information element

-- ASN1START

-- TAG-PHY-PARAMETERSSHAREDSPECTRUMCHACCESS-START

Phy-ParametersSharedSpectrumChAccess-r16 ::= SEQUENCE {

-- 10-32 (1-2): SS block based SINR measurement (SS-SINR) for unlicensed spectrum

ss-SINR-Meas-r16 ENUMERATED {supported} OPTIONAL,

-- 10-33 (2-32a): Semi-persistent CSI report on PUCCH for unlicensed spectrum

sp-CSI-ReportPUCCH-r16 ENUMERATED {supported} OPTIONAL,

-- 10-33a (2-32b): Semi-persistent CSI report on PUSCH for unlicensed spectrum

sp-CSI-ReportPUSCH-r16 ENUMERATED {supported} OPTIONAL,

-- 10-34 (3-6): Dynamic SFI monitoring for unlicensed spectrum

dynamicSFI-r16 ENUMERATED {supported} OPTIONAL,

-- 10-35c (4-19c): SR/HARQ-ACK/CSI multiplexing once per slot using a PUCCH (or HARQ-ACK/CSI piggybacked on a PUSCH) when SR/HARQ-

-- ACK/CSI are supposed to be sent with different starting symbols in a slot for unlicensed spectrum

-- 10-35 (4-19): SR/HARQ-ACK/CSI multiplexing once per slot using a PUCCH (or HARQ-ACK/CSI piggybacked on a PUSCH) when SR/HARQ-

-- ACK/CSI are supposed to be sent with the same starting symbol on the PUCCH resources in a slot for unlicensed spectrum

mux-SR-HARQ-ACK-CSI-PUCCH-OncePerSlot-r16 SEQUENCE {

sameSymbol-r16 ENUMERATED {supported} OPTIONAL,

diffSymbol-r16 ENUMERATED {supported} OPTIONAL

} OPTIONAL,

-- 10-35a (4-19a): Overlapping PUCCH resources have different starting symbols in a slot for unlicensed spectrum

mux-SR-HARQ-ACK-PUCCH-r16 ENUMERATED {supported} OPTIONAL,

-- 10-35b (4-19b): SR/HARQ-ACK/CSI multiplexing more than once per slot using a PUCCH (or HARQ-ACK/CSI piggybacked on a PUSCH) when

-- SR/HARQ ACK/CSI are supposed to be sent with the same or different starting symbol in a slot for unlicensed spectrum

mux-SR-HARQ-ACK-CSI-PUCCH-MultiPerSlot-r16 ENUMERATED {supported} OPTIONAL,

-- 10-36 (4-28): HARQ-ACK multiplexing on PUSCH with different PUCCH/PUSCH starting OFDM symbols for unlicensed spectrum

mux-HARQ-ACK-PUSCH-DiffSymbol-r16 ENUMERATED {supported} OPTIONAL,

-- 10-37 (4-23): Repetitions for PUCCH format 1, 3, and 4 over multiple slots with K = 2, 4, 8 for unlicensed spectrum

pucch-Repetition-F1-3-4-r16 ENUMERATED {supported} OPTIONAL,

-- 10-38 (5-14): Type 1 configured PUSCH repetitions over multiple slots for unlicensed spectrum

type1-PUSCH-RepetitionMultiSlots-r16 ENUMERATED {supported} OPTIONAL,

-- 10-39 (5-16): Type 2 configured PUSCH repetitions over multiple slots for unlicensed spectrum

type2-PUSCH-RepetitionMultiSlots-r16 ENUMERATED {supported} OPTIONAL,

-- 10-40 (5-17): PUSCH repetitions over multiple slots for unlicensed spectrum

pusch-RepetitionMultiSlots-r16 ENUMERATED {supported} OPTIONAL,

-- 10-40a (5-17a): PDSCH repetitions over multiple slots for unlicensed spectrum

pdsch-RepetitionMultiSlots-r16 ENUMERATED {supported} OPTIONAL,

-- 10-41 (5-18): DL SPS

downlinkSPS-r16 ENUMERATED {supported} OPTIONAL,

-- 10-42 (5-19): Type 1 Configured UL grant

configuredUL-GrantType1-r16 ENUMERATED {supported} OPTIONAL,

-- 10-43 (5-20): Type 2 Configured UL grant

configuredUL-GrantType2-r16 ENUMERATED {supported} OPTIONAL,

-- 10-44 (5-21): Pre-emption indication for DL

pre-EmptIndication-DL-r16 ENUMERATED {supported} OPTIONAL,

...

}

-- TAG-PHY-PARAMETERSSHAREDSPECTRUMCHACCESS-STOP

-- ASN1STOP

#### – *PosSRS-BWA-RRC-Inactive*

The IE *PosSRS-BWA-RRC-Inactive* is used to convey the capabilities supported by the UE for support of positioning SRS bandwidth aggregation in RRC\_INACTIVE

*PosSRS-BWA-RRC-Inactive* information element

-- ASN1START

-- TAG-POSSRS-BWA-RRC-INACTIVE-START

PosSRS-BWA-RRC-Inactive-r18 ::= SEQUENCE {

numOfCarriersIntraBandContiguous-r18 ENUMERATED {two, three, twoandthree},

maximumAggregatedBW-TwoCarriersFR1-r18 ENUMERATED { mhz20, mhz40, mhz50, mhz80, mhz100, mhz160,

mhz180, mhz190, mhz200} OPTIONAL,

maximumAggregatedBW-TwoCarriersFR2-r18 ENUMERATED {mhz50, mhz100, mhz200, mhz400, mhz600, mhz800} OPTIONAL,

maximumAggregatedBW-ThreeCarriersFR1-r18 ENUMERATED {mhz80, mhz100, mhz160, mhz200, mhz240, mhz300} OPTIONAL,

maximumAggregatedBW-ThreeCarriersFR2-r18 ENUMERATED {mhz50, mhz100, mhz200, mhz300, mhz400, mhz600,

mhz800, mhz1000, mhz1200} OPTIONAL,

maximumAggregatedResourceSet-r18 ENUMERATED {n1, n2, n4, n8, n12, n16},

maximumAggregatedResourcePeriodic-r18 ENUMERATED {n1, n2, n4, n8, n16, n32, n64},

maximumAggregatedResourceSemi-r18 ENUMERATED {n0, n1, n2, n4, n8, n16, n32, n64},

maximumAggregatedResourcePeriodicPerSlot-r18 ENUMERATED {n1, n2, n3, n4, n5, n6, n8, n10, n12, n14},

maximumAggregatedResourceSemiPerSlot-r18 ENUMERATED {n0, n1, n2, n3, n4, n5, n6, n8, n10, n12, n14},

guardPeriod-r18 ENUMERATED {n0, n30, n100, n140, n200},

powerClassForTwoAggregatedCarriers-r18 ENUMERATED {pc2, pc3} OPTIONAL,

powerClassForThreeAggregatedCarriers-r18 ENUMERATED {pc2, pc3} OPTIONAL,

...

}

-- TAG-POSSRS-BWA-RRC-INACTIVE-STOP

-- ASN1STOP

#### – *PosSRS-RRC-Inactive-OutsideInitialUL-BWP*

The IE *PosSRS-RRC-Inactive-OutsideInitialUL-BWP* is used to convey the capabilities supported by the UE for SRS for Positioning transmission in RRC\_INACTIVE state configured outside initial UL BWP.

*PosSRS-RRC-Inactive-OutsideInitialUL-BWP* information element

-- ASN1START

-- TAG-POSSRS-RRC-INACTIVE-OUTSIDEINITIALUL-BWP-START

PosSRS-RRC-Inactive-OutsideInitialUL-BWP-r17::= SEQUENCE {

-- R1 27-15b: Positioning SRS transmission in RRC\_INACTIVE state configured outside initial UL BWP

maxSRSposBandwidthForEachSCS-withinCC-FR1-r17 ENUMERATED {mhz5, mhz10, mhz15, mhz20, mhz25, mhz30, mhz35, mhz40,

mhz45, mhz50, mhz60, mhz70, mhz80, mhz90, mhz100} OPTIONAL,

maxSRSposBandwidthForEachSCS-withinCC-FR2-r17 ENUMERATED {mhz50, mhz100, mhz200, mhz400} OPTIONAL,

maxNumOfSRSposResourceSets-r17 ENUMERATED {n1, n2, n4, n8, n12, n16} OPTIONAL,

maxNumOfPeriodicSRSposResources-r17 ENUMERATED {n1, n2, n4, n8, n16, n32, n64} OPTIONAL,

maxNumOfPeriodicSRSposResourcesPerSlot-r17 ENUMERATED {n1, n2, n3, n4, n5, n6, n8, n10, n12, n14} OPTIONAL,

differentNumerologyBetweenSRSposAndInitialBWP-r17 ENUMERATED {supported} OPTIONAL,

srsPosWithoutRestrictionOnBWP-r17 ENUMERATED {supported} OPTIONAL,

maxNumOfPeriodicAndSemipersistentSRSposResources-r17 ENUMERATED {n1, n2, n4, n8, n16, n32, n64} OPTIONAL,

maxNumOfPeriodicAndSemipersistentSRSposResourcesPerSlot-r17 ENUMERATED {n1, n2, n3, n4, n5, n6, n8, n10, n12, n14} OPTIONAL,

differentCenterFreqBetweenSRSposAndInitialBWP-r17 ENUMERATED {supported} OPTIONAL,

switchingTimeSRS-TX-OtherTX-r17 ENUMERATED {us100, us140, us200, us300, us500} OPTIONAL,

-- R1 27-15c: Support of positioning SRS transmission in RRC\_INACTIVE state outside initial BWP with semi-persistent SRS

maxNumOfSemiPersistentSRSposResources-r17 ENUMERATED {n1, n2, n4, n8, n16, n32, n64} OPTIONAL,

maxNumOfSemiPersistentSRSposResourcesPerSlot-r17 ENUMERATED {n1, n2, n3, n4, n5, n6, n8, n10, n12, n14} OPTIONAL,

...

}

-- TAG-POSSRS-RRC-INACTIVE-OUTSIDEINITIALUL-BWP-STOP

-- ASN1STOP

#### – *PosSRS-TxFrequencyHoppingRRC-Connected*

The IE *PosSRS-TxFrequencyHoppingRRC-Connected* is used to convey the capabilities supported by the RRC\_CONNECTED UE for support of positioning SRS with Tx frequency hopping for RedCap UEs.

*PosSRS-TxFrequencyHoppingRRC-Connected* information element

-- ASN1START

-- TAG-POSSRS-TXFREQUENCYHOPPINGRRCCONNECTED-START

PosSRS-TxFrequencyHoppingRRC-Connected-r18 ::= SEQUENCE {

maximumSRS-BandwidthAcrossAllHopsFR1-r18 ENUMERATED {mhz40, mhz50, mhz80, mhz100} OPTIONAL,

maximumSRS-BandwidthAcrossAllHopsFR2-r18 ENUMERATED {mhz100, mhz200, mhz400} OPTIONAL,

maximumTxFH-Hops-r18 ENUMERATED {n2, n3, n4, n5, n6} OPTIONAL,

rf-TxRetuneTimeFR1-r18 ENUMERATED {n70, n140, n210} OPTIONAL,

rf-TxRetuneTimeFR2-r18 ENUMERATED {n35, n70, n140} OPTIONAL,

switchTimeBetweenActiveBWP-FrequencyHop-r18 ENUMERATED {n100, n140, n200, n300, n500} OPTIONAL,

numOfOverlappingPRB-r18 ENUMERATED {n0, n1, n2, n4} OPTIONAL,

maximumSRS-ResourcePeriodic-r18 ENUMERATED {n1, n2, n4, n8, n16, n32, n64} OPTIONAL,

maximumSRS-ResourceAperiodic-r18 ENUMERATED {n0,n1, n2, n4, n8, n16, n32, n64} OPTIONAL,

maximumSRS-ResourceSemipersistent-r18 ENUMERATED {n0,n1, n2, n4, n8, n16, n32, n64} OPTIONAL,

...

}

-- TAG-POSSRS-TXFREQUENCYHOPPINGRRCCONNECTED-STOP

-- ASN1STOP

#### – *PosSRS-TxFrequencyHoppingRRC-ConnectedNonRedCap*

The IE *PosSRS-TxFrequencyHoppingRRC-ConnectedNonRedCap* is used to convey the capabilities supported by the RRC\_CONNECTED UE for support of positioning SRS with Tx frequency hopping for non-RedCap UEs.

*PosSRS-TxFrequencyHoppingRRC-ConnectedNonRedCap information element*

-- ASN1START

-- TAG-POSSRS-TXFREQUENCYHOPPINGRRCCONNECTEDNONREDCAP-START

PosSRS-TxFrequencyHoppingRRC-ConnectedNonRedCap-r19 ::= SEQUENCE {

maximumSRS-BandwidthAcrossAllHopsFR1-r19 ENUMERATED {mhz40, mhz50, mhz80, mhz100} OPTIONAL,

maximumSRS-BandwidthAcrossAllHopsFR2-r19 ENUMERATED {mhz100, mhz200, mhz400} OPTIONAL,

maximumTxFH-Hops-r19 ENUMERATED {n2, n3, n4, n5, n6} OPTIONAL,

rf-TxRetuneTimeFR1-r19 ENUMERATED {us0, us70, us140, us210} OPTIONAL,

rf-TxRetuneTimeFR2-r19 ENUMERATED {us0, us35, us70, us140} OPTIONAL,

switchTimeBetweenActiveBWP-FrequencyHop-r19 ENUMERATED {us0, us100, us140, us200, us300, us500} OPTIONAL,

numOfOverlappingPRB-r19 ENUMERATED {n0, n1, n2, n4} OPTIONAL,

maximumSRS-ResourcePeriodic-r19 ENUMERATED {n1, n2, n4, n8, n16, n32, n64} OPTIONAL,

maximumSRS-ResourceAperiodic-r19 ENUMERATED {n0, n1, n2, n4, n8, n16, n32, n64} OPTIONAL,

maximumSRS-ResourceSemipersistent-r19 ENUMERATED {n0, n1, n2, n4, n8, n16, n32, n64} OPTIONAL,

...

}

-- TAG-POSSRS- TXFREQUENCYHOPPINGRRCCONNECTEDNONREDCAP-STOP

-- ASN1STOP

#### – *PosSRS-TxFrequencyHoppingRRC-Inactive*

The IE *PosSRS-TxFrequencyHoppingRRC-Inactive* is used to convey the capabilities supported by the RRC\_INACTIVE UE for support of positioning SRS with Tx frequency hopping for RedCap UEs.

*PosSRS-TxFrequencyHoppingRRC-Inactive* information element

-- ASN1START

-- TAG-POSSRS-TXFREQUENCYHOPPINGRRCINACTIVE-START

PosSRS-TxFrequencyHoppingRRC-Inactive-r18 ::= SEQUENCE {

maximumSRS-BandwidthAcrossAllHopsFR1-r18 ENUMERATED {mhz40, mhz50, mhz80, mhz100} OPTIONAL,

maximumSRS-BandwidthAcrossAllHopsFR2-r18 ENUMERATED {mhz100, mhz200, mhz400} OPTIONAL,

maximumTxFH-Hops-r18 ENUMERATED {n2, n3, n4, n5, n6} OPTIONAL,

rf-TxRetuneTimeFR1-r18 ENUMERATED {n70, n140, n210} OPTIONAL,

rf-TxRetuneTimeFR2-r18 ENUMERATED {n35, n70, n140} OPTIONAL,

switchTimeBetweenActiveBWP-FrequencyHop-r18 ENUMERATED {n100, n140, n200, n300, n500} OPTIONAL,

numOfOverlappingPRB-r18 ENUMERATED {n0, n1, n2, n4} OPTIONAL,

maximumSRS-Resource-Periodic-r18 ENUMERATED {n1, n2, n4, n8, n16, n32, n64} OPTIONAL,

maximumSRS-Resource-Semipersistent-r18 ENUMERATED {n0, n1, n2, n4, n8, n16, n32, n64} OPTIONAL,

...

}

-- TAG-POSSRS-TXFREQUENCYHOPPINGRRCINACTIVE-STOP

-- ASN1STOP

#### – *PosSRS-TxFrequencyHoppingRRC-InactiveNonRedCap*

The IE *PosSRS-TxFrequencyHoppingRRC-InactiveNonRedCap* is used to convey the capabilities supported by the RRC\_INACTIVE UE for support of positioning SRS with Tx frequency hopping for non-RedCap UEs.

*PosSRS-TxFrequencyHoppingRRC-InactiveNonRedCap information element*

-- ASN1START

-- TAG-POSSRS-TXFREQUENCYHOPPINGRRCINACTIVENONREDCAP-START

PosSRS-TxFrequencyHoppingRRC-InactiveNonRedCap-r19 ::= SEQUENCE {

maximumSRS-BandwidthAcrossAllHops-FR1-r19 ENUMERATED {mhz40, mhz50, mhz80, mhz100} OPTIONAL,

maximumSRS-BandwidthAcrossAllHops-FR2-r19 ENUMERATED {mhz100, mhz200, mhz400} OPTIONAL,

maximumTxFH-Hops-r19 ENUMERATED {n2, n3, n4, n5, n6} OPTIONAL,

rf-TxRetuneTimeFR1-r19 ENUMERATED {us0, us70, us140, us210} OPTIONAL,

rf-TxRetuneTimeFR2-r19 ENUMERATED {us0, us35, us70, us140} OPTIONAL,

switchTimeBetweenActiveBWP-FrequencyHop-r19 ENUMERATED {us0, us100, us140, us200, us300, us500} OPTIONAL,

numOfOverlappingPRB-r19 ENUMERATED {n0, n1, n2, n4} OPTIONAL,

maximumSRS-Resource-Periodic-r19 ENUMERATED {n1, n2, n4, n8, n16, n32, n64} OPTIONAL,

maximumSRS-Resource-Semipersistent-r19 ENUMERATED {n0, n1, n2, n4, n8, n16, n32, n64} OPTIONAL,

...

}

-- TAG-POSSRS-TXFREQUENCYHOPPINGRRCCINACTIVENONREDCAP-STOP

-- ASN1STOP

#### *– PowSav-Parameters*

The IE *PowSav-Parameters* is used to convey the capabilities supported by the UE for the power saving preferences.

*PowSav-Parameters* information element

-- ASN1START

-- TAG-POWSAV-PARAMETERS-START

PowSav-Parameters-r16 ::= SEQUENCE {

powSav-ParametersCommon-r16 PowSav-ParametersCommon-r16 OPTIONAL,

powSav-ParametersFRX-Diff-r16 PowSav-ParametersFRX-Diff-r16 OPTIONAL,

...

}

PowSav-Parameters-v1700 ::= SEQUENCE {

powSav-ParametersFR2-2-r17 PowSav-ParametersFR2-2-r17 OPTIONAL,

...

}

PowSav-ParametersCommon-r16 ::= SEQUENCE {

drx-Preference-r16 ENUMERATED {supported} OPTIONAL,

maxCC-Preference-r16 ENUMERATED {supported} OPTIONAL,

releasePreference-r16 ENUMERATED {supported} OPTIONAL,

-- R1 19-4a: UE assistance information

minSchedulingOffsetPreference-r16 ENUMERATED {supported} OPTIONAL,

...

}

PowSav-ParametersFRX-Diff-r16 ::= SEQUENCE {

maxBW-Preference-r16 ENUMERATED {supported} OPTIONAL,

maxMIMO-LayerPreference-r16 ENUMERATED {supported} OPTIONAL,

...

}

PowSav-ParametersFR2-2-r17 ::= SEQUENCE {

maxBW-Preference-r17 ENUMERATED {supported} OPTIONAL,

maxMIMO-LayerPreference-r17 ENUMERATED {supported} OPTIONAL,

...

}

-- TAG-POWSAV-PARAMETERS-STOP

-- ASN1STOP

#### – *ProcessingParameters*

The IE *ProcessingParameters* is used to indicate PDSCH/PUSCH processing capabilities supported by the UE.

*ProcessingParameters* information element

-- ASN1START

-- TAG-PROCESSINGPARAMETERS-START

ProcessingParameters ::= SEQUENCE {

fallback ENUMERATED {sc, cap1-only},

differentTB-PerSlot SEQUENCE {

upto1 NumberOfCarriers OPTIONAL,

upto2 NumberOfCarriers OPTIONAL,

upto4 NumberOfCarriers OPTIONAL,

upto7 NumberOfCarriers OPTIONAL

} OPTIONAL

}

NumberOfCarriers ::= INTEGER (1..16)

-- TAG-PROCESSINGPARAMETERS-STOP

-- ASN1STOP

#### – *PRS-ProcessingCapabilityOutsideMGinPPWperType*

The IE *PRS-ProcessingCapabilityOutsideMGinPPWperType* is used to indicate DL PRS Processing Capability outside MG capabilities supported by the UE.

*PRS-ProcessingCapabilityOutsideMGinPPWperType* information element

-- ASN1START

-- TAG-PRS-PROCESSINGCAPABILITYOUTSIDEMGINPPWPERType-START

PRS-ProcessingCapabilityOutsideMGinPPWperType-r17 ::= SEQUENCE {

prsProcessingType-r17 ENUMERATED {type1A, type1B, type2},

ppw-dl-PRS-BufferType-r17 ENUMERATED {type1, type2, ...},

ppw-durationOfPRS-Processing-r17 CHOICE {

ppw-durationOfPRS-Processing1-r17 SEQUENCE {

ppw-durationOfPRS-ProcessingSymbolsN-r17 ENUMERATED {msDot125, msDot25, msDot5, ms1, ms2, ms4, ms6, ms8, ms12,

ms16, ms20, ms25, ms30, ms32, ms35, ms40, ms45, ms50},

ppw-durationOfPRS-ProcessingSymbolsT-r17 ENUMERATED {ms1, ms2, ms4, ms8, ms16, ms20, ms30, ms40, ms80,

ms160, ms320, ms640, ms1280}

},

ppw-durationOfPRS-Processing2-r17 SEQUENCE {

ppw-durationOfPRS-ProcessingSymbolsN2-r17 ENUMERATED {msDot125, msDot25, msDot5, ms1, ms2, ms3, ms4, ms5,

ms6, ms8, ms12},

ppw-durationOfPRS-ProcessingSymbolsT2-r17 ENUMERATED {ms4, ms5, ms6, ms8}

}

} OPTIONAL,

ppw-maxNumOfDL-PRS-ResProcessedPerSlot-r17 SEQUENCE {

scs15-r17 ENUMERATED {n1, n2, n4, n6, n8, n12, n16, n24, n32, n48, n64} OPTIONAL,

scs30-r17 ENUMERATED {n1, n2, n4, n6, n8, n12, n16, n24, n32, n48, n64} OPTIONAL,

scs60-r17 ENUMERATED {n1, n2, n4, n6, n8, n12, n16, n24, n32, n48, n64} OPTIONAL,

scs120-r17 ENUMERATED {n1, n2, n4, n6, n8, n12, n16, n24, n32, n48, n64} OPTIONAL,

...

},

ppw-maxNumOfDL-Bandwidth-r17 CHOICE {

fr1-r17 ENUMERATED {mhz5, mhz10, mhz20, mhz40, mhz50, mhz80, mhz100},

fr2-r17 ENUMERATED {mhz50, mhz100, mhz200, mhz400}

} OPTIONAL

}

-- TAG-PRS-PROCESSINGCAPABILITYOUTSIDEMGINPPWPERType-STOP

-- ASN1STOP

#### – *RAT-Type*

The IE *RAT-Type* is used to indicate the radio access technology (RAT), including NR, of the requested/transferred UE capabilities.

*RAT-Type* information element

-- ASN1START

-- TAG-RAT-TYPE-START

RAT-Type ::= ENUMERATED {nr, eutra-nr, eutra, utra-fdd-v1610, ...}

-- TAG-RAT-TYPE-STOP

-- ASN1STOP

#### – *RedCapParameters*

The IE *RedCapParameters* is used to indicate the UE capabilities supported by RedCap UEs.

*RedCapParameters* information element

-- ASN1START

-- TAG-REDCAPPARAMETERS-START

RedCapParameters-r17::= SEQUENCE {

-- R1 28-1: RedCap UE

supportOfRedCap-r17 ENUMERATED {supported} OPTIONAL,

supportOf16DRB-RedCap-r17 ENUMERATED {supported} OPTIONAL

}

RedCapParameters-v1740::= SEQUENCE {

ncd-SSB-ForRedCapInitialBWP-SDT-r17 ENUMERATED {supported} OPTIONAL

}

-- TAG-REDCAPPARAMETERS-STOP

-- ASN1STOP

#### – *RF-Parameters*

The IE *RF-Parameters* is used to convey RF-related capabilities for NR operation.

*RF-Parameters* information element

-- ASN1START

-- TAG-RF-PARAMETERS-START

RF-Parameters ::= SEQUENCE {

supportedBandListNR SEQUENCE (SIZE (1..maxBands)) OF BandNR,

supportedBandCombinationList BandCombinationList OPTIONAL,

appliedFreqBandListFilter FreqBandList OPTIONAL,

...,

[[

supportedBandCombinationList-v1540 BandCombinationList-v1540 OPTIONAL,

srs-SwitchingTimeRequested ENUMERATED {true} OPTIONAL

]],

[[

supportedBandCombinationList-v1550 BandCombinationList-v1550 OPTIONAL

]],

[[

supportedBandCombinationList-v1560 BandCombinationList-v1560 OPTIONAL

]],

[[

supportedBandCombinationList-v1610 BandCombinationList-v1610 OPTIONAL,

supportedBandCombinationListSidelinkEUTRA-NR-r16 BandCombinationListSidelinkEUTRA-NR-r16 OPTIONAL,

supportedBandCombinationList-UplinkTxSwitch-r16 BandCombinationList-UplinkTxSwitch-r16 OPTIONAL

]],

[[

supportedBandCombinationList-v1630 BandCombinationList-v1630 OPTIONAL,

supportedBandCombinationListSidelinkEUTRA-NR-v1630 BandCombinationListSidelinkEUTRA-NR-v1630 OPTIONAL,

supportedBandCombinationList-UplinkTxSwitch-v1630 BandCombinationList-UplinkTxSwitch-v1630 OPTIONAL

]],

[[

supportedBandCombinationList-v1640 BandCombinationList-v1640 OPTIONAL,

supportedBandCombinationList-UplinkTxSwitch-v1640 BandCombinationList-UplinkTxSwitch-v1640 OPTIONAL

]],

[[

supportedBandCombinationList-v1650 BandCombinationList-v1650 OPTIONAL,

supportedBandCombinationList-UplinkTxSwitch-v1650 BandCombinationList-UplinkTxSwitch-v1650 OPTIONAL

]],

[[

extendedBand-n77-r16 ENUMERATED {supported} OPTIONAL

]],

[[

supportedBandCombinationList-UplinkTxSwitch-v1670 BandCombinationList-UplinkTxSwitch-v1670 OPTIONAL

]],

[[

supportedBandCombinationList-v1680 BandCombinationList-v1680 OPTIONAL

]],

[[

supportedBandCombinationList-v1690 BandCombinationList-v1690 OPTIONAL,

supportedBandCombinationList-UplinkTxSwitch-v1690 BandCombinationList-UplinkTxSwitch-v1690 OPTIONAL

]],

[[

supportedBandCombinationList-v1700 BandCombinationList-v1700 OPTIONAL,

supportedBandCombinationList-UplinkTxSwitch-v1700 BandCombinationList-UplinkTxSwitch-v1700 OPTIONAL,

supportedBandCombinationListSL-RelayDiscovery-r17 OCTET STRING OPTIONAL, -- Contains PC5 BandCombinationListSidelinkNR-r16

supportedBandCombinationListSL-NonRelayDiscovery-r17 OCTET STRING OPTIONAL, -- Contains PC5 BandCombinationListSidelinkNR-r16

supportedBandCombinationListSidelinkEUTRA-NR-v1710 BandCombinationListSidelinkEUTRA-NR-v1710 OPTIONAL,

sidelinkRequested-r17 ENUMERATED {true} OPTIONAL,

extendedBand-n77-2-r17 ENUMERATED {supported} OPTIONAL

]],

[[

supportedBandCombinationList-v1720 BandCombinationList-v1720 OPTIONAL,

supportedBandCombinationList-UplinkTxSwitch-v1720 BandCombinationList-UplinkTxSwitch-v1720 OPTIONAL

]],

[[

supportedBandCombinationList-v1730 BandCombinationList-v1730 OPTIONAL,

supportedBandCombinationList-UplinkTxSwitch-v1730 BandCombinationList-UplinkTxSwitch-v1730 OPTIONAL,

supportedBandCombinationListSL-RelayDiscovery-v1730 BandCombinationListSL-Discovery-r17 OPTIONAL,

supportedBandCombinationListSL-NonRelayDiscovery-v1730 BandCombinationListSL-Discovery-r17 OPTIONAL

]],

[[

supportedBandCombinationList-v1740 BandCombinationList-v1740 OPTIONAL,

supportedBandCombinationList-UplinkTxSwitch-v1740 BandCombinationList-UplinkTxSwitch-v1740 OPTIONAL

]],

[[

supportedBandCombinationList-v1760 BandCombinationList-v1760 OPTIONAL,

supportedBandCombinationList-UplinkTxSwitch-v1760 BandCombinationList-UplinkTxSwitch-v1760 OPTIONAL

]],

[[

dummy1 BandCombinationList-v1770 OPTIONAL,

dummy2 BandCombinationList-UplinkTxSwitch-v1770 OPTIONAL

]],

[[

supportedBandCombinationList-v1780 BandCombinationList-v1780 OPTIONAL,

supportedBandCombinationList-UplinkTxSwitch-v1780 BandCombinationList-UplinkTxSwitch-v1780 OPTIONAL

]],

[[

supportedBandCombinationList-v1800 BandCombinationList-v1800 OPTIONAL,

supportedBandCombinationList-UplinkTxSwitch-v1800 BandCombinationList-UplinkTxSwitch-v1800 OPTIONAL,

supportedBandCombinationListSL-U2U-Relay-r18 SEQUENCE {

supportedBandCombinationListSL-U2U-RelayDiscovery-r18 OCTET STRING OPTIONAL, -- Contains PC5

-- BandCombinationListSidelinkNR-r16

supportedBandCombinationListSL-U2U-DiscoveryExt BandCombinationListSL-Discovery-r17 OPTIONAL

} OPTIONAL

]],

[[

supportedBandCombinationList-v1830 BandCombinationList-v1830 OPTIONAL,

supportedBandCombinationList-UplinkTxSwitch-v1830 BandCombinationList-UplinkTxSwitch-v1830 OPTIONAL

]],

[[

supportedBandCombinationList-v1840 BandCombinationList-v1840 OPTIONAL,

supportedBandCombinationList-UplinkTxSwitch-v1840 BandCombinationList-UplinkTxSwitch-v1840 OPTIONAL

]],

[[

supportedBandCombinationList-v1860 BandCombinationList-v1860 OPTIONAL,

supportedBandCombinationList-UplinkTxSwitch-v1860 BandCombinationList-UplinkTxSwitch-v1860 OPTIONAL

]],

[[

supportedBandCombinationList-v1900 BandCombinationList-v1900 OPTIONAL,

supportedBandCombinationList-UplinkTxSwitch-v1900 BandCombinationList-UplinkTxSwitch-v1900 OPTIONAL

]]

}

RF-Parameters-v15g0 ::= SEQUENCE {

supportedBandCombinationList-v15g0 BandCombinationList-v15g0 OPTIONAL

}

RF-Parameters-v16a0 ::= SEQUENCE {

supportedBandCombinationList-v16a0 BandCombinationList-v16a0 OPTIONAL,

supportedBandCombinationList-UplinkTxSwitch-v16a0 BandCombinationList-UplinkTxSwitch-v16a0 OPTIONAL

}

RF-Parameters-v16c0 ::= SEQUENCE {

supportedBandListNR-v16c0 SEQUENCE (SIZE (1..maxBands)) OF BandNR-v16c0

}

RF-Parameters-v16j0 ::= SEQUENCE {

supportedBandCombinationList-v16j0 BandCombinationList-v16j0 OPTIONAL,

supportedBandCombinationList-UplinkTxSwitch-v16j0 BandCombinationList-UplinkTxSwitch-v16j0 OPTIONAL

}

RF-Parameters-v17b0 ::= SEQUENCE {

supportedBandListNR-v17b0 SEQUENCE (SIZE (1..maxBands)) OF BandNR-v17b0 OPTIONAL,

supportedBandCombinationList-v17b0 BandCombinationList-v17b0 OPTIONAL,

supportedBandCombinationList-UplinkTxSwitch-v17b0 BandCombinationList-UplinkTxSwitch-v17b0 OPTIONAL

}

BandNR ::= SEQUENCE {

bandNR FreqBandIndicatorNR,

modifiedMPR-Behaviour BIT STRING (SIZE (8)) OPTIONAL,

mimo-ParametersPerBand MIMO-ParametersPerBand OPTIONAL,

extendedCP ENUMERATED {supported} OPTIONAL,

multipleTCI ENUMERATED {supported} OPTIONAL,

bwp-WithoutRestriction ENUMERATED {supported} OPTIONAL,

bwp-SameNumerology ENUMERATED {upto2, upto4} OPTIONAL,

bwp-DiffNumerology ENUMERATED {upto4} OPTIONAL,

crossCarrierScheduling-SameSCS ENUMERATED {supported} OPTIONAL,

pdsch-256QAM-FR2 ENUMERATED {supported} OPTIONAL,

pusch-256QAM ENUMERATED {supported} OPTIONAL,

ue-PowerClass ENUMERATED {pc1, pc2, pc3, pc4} OPTIONAL,

rateMatchingLTE-CRS ENUMERATED {supported} OPTIONAL,

channelBWs-DL CHOICE {

fr1 SEQUENCE {

scs-15kHz BIT STRING (SIZE (10)) OPTIONAL,

scs-30kHz BIT STRING (SIZE (10)) OPTIONAL,

scs-60kHz BIT STRING (SIZE (10)) OPTIONAL

},

fr2 SEQUENCE {

scs-60kHz BIT STRING (SIZE (3)) OPTIONAL,

scs-120kHz BIT STRING (SIZE (3)) OPTIONAL

}

} OPTIONAL,

channelBWs-UL CHOICE {

fr1 SEQUENCE {

scs-15kHz BIT STRING (SIZE (10)) OPTIONAL,

scs-30kHz BIT STRING (SIZE (10)) OPTIONAL,

scs-60kHz BIT STRING (SIZE (10)) OPTIONAL

},

fr2 SEQUENCE {

scs-60kHz BIT STRING (SIZE (3)) OPTIONAL,

scs-120kHz BIT STRING (SIZE (3)) OPTIONAL

}

} OPTIONAL,

...,

[[

maxUplinkDutyCycle-PC2-FR1 ENUMERATED {n60, n70, n80, n90, n100} OPTIONAL

]],

[[

pucch-SpatialRelInfoMAC-CE ENUMERATED {supported} OPTIONAL,

powerBoosting-pi2BPSK ENUMERATED {supported} OPTIONAL

]],

[[

maxUplinkDutyCycle-FR2 ENUMERATED {n15, n20, n25, n30, n40, n50, n60, n70, n80, n90, n100} OPTIONAL

]],

[[

channelBWs-DL-v1590 CHOICE {

fr1 SEQUENCE {

scs-15kHz BIT STRING (SIZE (16)) OPTIONAL,

scs-30kHz BIT STRING (SIZE (16)) OPTIONAL,

scs-60kHz BIT STRING (SIZE (16)) OPTIONAL

},

fr2 SEQUENCE {

scs-60kHz BIT STRING (SIZE (8)) OPTIONAL,

scs-120kHz BIT STRING (SIZE (8)) OPTIONAL

}

} OPTIONAL,

channelBWs-UL-v1590 CHOICE {

fr1 SEQUENCE {

scs-15kHz BIT STRING (SIZE (16)) OPTIONAL,

scs-30kHz BIT STRING (SIZE (16)) OPTIONAL,

scs-60kHz BIT STRING (SIZE (16)) OPTIONAL

},

fr2 SEQUENCE {

scs-60kHz BIT STRING (SIZE (8)) OPTIONAL,

scs-120kHz BIT STRING (SIZE (8)) OPTIONAL

}

} OPTIONAL

]],

[[

asymmetricBandwidthCombinationSet BIT STRING (SIZE (1..32)) OPTIONAL

]],

[[

-- R1 10: NR-unlicensed

sharedSpectrumChAccessParamsPerBand-r16 SharedSpectrumChAccessParamsPerBand-r16 OPTIONAL,

-- R1 11-7b: Independent cancellation of the overlapping PUSCHs in an intra-band UL CA

cancelOverlappingPUSCH-r16 ENUMERATED {supported} OPTIONAL,

-- R1 14-1: Multiple LTE-CRS rate matching patterns

multipleRateMatchingEUTRA-CRS-r16 SEQUENCE {

maxNumberPatterns-r16 INTEGER (2..6),

maxNumberNon-OverlapPatterns-r16 INTEGER (1..3)

} OPTIONAL,

-- R1 14-1a: Two LTE-CRS overlapping rate matching patterns within a part of NR carrier using 15 kHz overlapping with a LTE carrier

overlapRateMatchingEUTRA-CRS-r16 ENUMERATED {supported} OPTIONAL,

-- R1 14-2: PDSCH Type B mapping of length 9 and 10 OFDM symbols

pdsch-MappingTypeB-Alt-r16 ENUMERATED {supported} OPTIONAL,

-- R1 14-3: One slot periodic TRS configuration for FR1

oneSlotPeriodicTRS-r16 ENUMERATED {supported} OPTIONAL,

olpc-SRS-Pos-r16 OLPC-SRS-Pos-r16 OPTIONAL,

spatialRelationsSRS-Pos-r16 SpatialRelationsSRS-Pos-r16 OPTIONAL,

simulSRS-MIMO-TransWithinBand-r16 ENUMERATED {n2} OPTIONAL,

channelBW-DL-IAB-r16 CHOICE {

fr1-100mhz SEQUENCE {

scs-15kHz ENUMERATED {supported} OPTIONAL,

scs-30kHz ENUMERATED {supported} OPTIONAL,

scs-60kHz ENUMERATED {supported} OPTIONAL

},

fr2-200mhz SEQUENCE {

scs-60kHz ENUMERATED {supported} OPTIONAL,

scs-120kHz ENUMERATED {supported} OPTIONAL

}

} OPTIONAL,

channelBW-UL-IAB-r16 CHOICE {

fr1-100mhz SEQUENCE {

scs-15kHz ENUMERATED {supported} OPTIONAL,

scs-30kHz ENUMERATED {supported} OPTIONAL,

scs-60kHz ENUMERATED {supported} OPTIONAL

},

fr2-200mhz SEQUENCE {

scs-60kHz ENUMERATED {supported} OPTIONAL,

scs-120kHz ENUMERATED {supported} OPTIONAL

}

} OPTIONAL,

rasterShift7dot5-IAB-r16 ENUMERATED {supported} OPTIONAL,

ue-PowerClass-v1610 ENUMERATED {pc1dot5} OPTIONAL,

condHandover-r16 ENUMERATED {supported} OPTIONAL,

condHandoverFailure-r16 ENUMERATED {supported} OPTIONAL,

condHandoverTwoTriggerEvents-r16 ENUMERATED {supported} OPTIONAL,

condPSCellChange-r16 ENUMERATED {supported} OPTIONAL,

condPSCellChangeTwoTriggerEvents-r16 ENUMERATED {supported} OPTIONAL,

mpr-PowerBoost-FR2-r16 ENUMERATED {supported} OPTIONAL,

-- R1 11-9: Multiple active configured grant configurations for a BWP of a serving cell

activeConfiguredGrant-r16 SEQUENCE {

maxNumberConfigsPerBWP-r16 ENUMERATED {n1, n2, n4, n8, n12},

maxNumberConfigsAllCC-r16 INTEGER (2..32)

} OPTIONAL,

-- R1 11-9a: Joint release in a DCI for two or more configured grant Type 2 configurations for a given BWP of a serving cell

jointReleaseConfiguredGrantType2-r16 ENUMERATED {supported} OPTIONAL,

-- R1 12-2: Multiple SPS configurations

sps-r16 SEQUENCE {

maxNumberConfigsPerBWP-r16 INTEGER (1..8),

maxNumberConfigsAllCC-r16 INTEGER (2..32)

} OPTIONAL,

-- R1 12-2a: Joint release in a DCI for two or more SPS configurations for a given BWP of a serving cell

jointReleaseSPS-r16 ENUMERATED {supported} OPTIONAL,

-- R1 13-19: Simultaneous positioning SRS and MIMO SRS transmission within a band across multiple CCs

simulSRS-TransWithinBand-r16 ENUMERATED {n2} OPTIONAL,

trs-AdditionalBandwidth-r16 ENUMERATED {trs-AddBW-Set1, trs-AddBW-Set2} OPTIONAL,

handoverIntraF-IAB-r16 ENUMERATED {supported} OPTIONAL

]],

[[

-- R1 22-5a: Simultaneous transmission of SRS for antenna switching and SRS for CB/NCB /BM for intra-band UL CA

-- R1 22-5c: Simultaneous transmission of SRS for antenna switching and SRS for antenna switching for intra-band UL CA

simulTX-SRS-AntSwitchingIntraBandUL-CA-r16 SimulSRS-ForAntennaSwitching-r16 OPTIONAL,

-- R1 10: NR-unlicensed

sharedSpectrumChAccessParamsPerBand-v1630 SharedSpectrumChAccessParamsPerBand-v1630 OPTIONAL

]],

[[

handoverUTRA-FDD-r16 ENUMERATED {supported} OPTIONAL,

-- R4 7-4: Report the shorter transient capability supported by the UE: 2, 4 or 7us

enhancedUL-TransientPeriod-r16 ENUMERATED {us2, us4, us7} OPTIONAL,

sharedSpectrumChAccessParamsPerBand-v1640 SharedSpectrumChAccessParamsPerBand-v1640 OPTIONAL

]],

[[

type1-PUSCH-RepetitionMultiSlots-v1650 ENUMERATED {supported} OPTIONAL,

type2-PUSCH-RepetitionMultiSlots-v1650 ENUMERATED {supported} OPTIONAL,

pusch-RepetitionMultiSlots-v1650 ENUMERATED {supported} OPTIONAL,

configuredUL-GrantType1-v1650 ENUMERATED {supported} OPTIONAL,

configuredUL-GrantType2-v1650 ENUMERATED {supported} OPTIONAL,

sharedSpectrumChAccessParamsPerBand-v1650 SharedSpectrumChAccessParamsPerBand-v1650 OPTIONAL

]],

[[

enhancedSkipUplinkTxConfigured-v1660 ENUMERATED {supported} OPTIONAL,

enhancedSkipUplinkTxDynamic-v1660 ENUMERATED {supported} OPTIONAL

]],

[[

maxUplinkDutyCycle-PC1dot5-MPE-FR1-r16 ENUMERATED {n10, n15, n20, n25, n30, n40, n50, n60, n70, n80, n90, n100} OPTIONAL,

txDiversity-r16 ENUMERATED {supported} OPTIONAL

]],

[[

-- R1 36-1: Support of 1024QAM for PDSCH for FR1

pdsch-1024QAM-FR1-r17 ENUMERATED {supported} OPTIONAL,

-- R4 22-1 support of FR2 HST operation

ue-PowerClass-v1700 ENUMERATED {pc5, pc6, pc7} OPTIONAL,

-- R1 24: NR extension to 71GHz (FR2-2)

fr2-2-AccessParamsPerBand-r17 FR2-2-AccessParamsPerBand-r17 OPTIONAL,

rlm-Relaxation-r17 ENUMERATED {supported} OPTIONAL,

bfd-Relaxation-r17 ENUMERATED {supported} OPTIONAL,

cg-SDT-r17 ENUMERATED {supported} OPTIONAL,

locationBasedCondHandover-r17 ENUMERATED {supported} OPTIONAL,

timeBasedCondHandover-r17 ENUMERATED {supported} OPTIONAL,

eventA4BasedCondHandover-r17 ENUMERATED {supported} OPTIONAL,

mn-InitiatedCondPSCellChangeNRDC-r17 ENUMERATED {supported} OPTIONAL,

sn-InitiatedCondPSCellChangeNRDC-r17 ENUMERATED {supported} OPTIONAL,

-- R1 29-3a: PDCCH skipping

pdcch-SkippingWithoutSSSG-r17 ENUMERATED {supported} OPTIONAL,

-- R1 29-3b: 2 search space sets group switching

sssg-Switching-1BitInd-r17 ENUMERATED {supported} OPTIONAL,

-- R1 29-3c: 3 search space sets group switching

sssg-Switching-2BitInd-r17 ENUMERATED {supported} OPTIONAL,

-- R1 29-3d: 2 search space sets group switching with PDCCH skipping

pdcch-SkippingWithSSSG-r17 ENUMERATED {supported} OPTIONAL,

-- R1 29-3e: Support Search space set group switching capability 2 for FR1

searchSpaceSetGrp-switchCap2-r17 ENUMERATED {supported} OPTIONAL,

-- R1 26-1: Uplink Time and Frequency pre-compensation and timing relationship enhancements

uplinkPreCompensation-r17 ENUMERATED {supported} OPTIONAL,

-- R1 26-4: UE reporting of information related to TA pre-compensation

uplink-TA-Reporting-r17 ENUMERATED {supported} OPTIONAL,

-- R1 26-5: Increasing the number of HARQ processes

max-HARQ-ProcessNumber-r17 ENUMERATED {u16d32, u32d16, u32d32} OPTIONAL,

-- R1 26-6: Type-2 HARQ codebook enhancement

type2-HARQ-Codebook-r17 ENUMERATED {supported} OPTIONAL,

-- R1 26-6a: Type-1 HARQ codebook enhancement

type1-HARQ-Codebook-r17 ENUMERATED {supported} OPTIONAL,

-- R1 26-6b: Type-3 HARQ codebook enhancement

type3-HARQ-Codebook-r17 ENUMERATED {supported} OPTIONAL,

-- R1 26-9: UE-specific K\_offset

ue-specific-K-Offset-r17 ENUMERATED {supported} OPTIONAL,

-- R1 24-1f: Multiple PDSCH scheduling by single DCI for 120kHz in FR2-1

multiPDSCH-SingleDCI-FR2-1-SCS-120kHz-r17 ENUMERATED {supported} OPTIONAL,

-- R1 24-1g: Multiple PUSCH scheduling by single DCI for 120kHz in FR2-1

multiPUSCH-SingleDCI-FR2-1-SCS-120kHz-r17 ENUMERATED {supported} OPTIONAL,

-- R4 14-4: Parallel PRS measurements in RRC\_INACTIVE state, FR1/FR2 diff

parallelPRS-MeasRRC-Inactive-r17 ENUMERATED {supported} OPTIONAL,

-- R1 27-1-2: Support of UE-TxTEGs for UL TDOA

nr-UE-TxTEG-ID-MaxSupport-r17 ENUMERATED {n1, n2, n3, n4, n6, n8} OPTIONAL,

-- R1 27-17: PRS processing in RRC\_INACTIVE

prs-ProcessingRRC-Inactive-r17 ENUMERATED {supported} OPTIONAL,

-- R1 27-3-2: DL PRS measurement outside MG and in a PRS processing window

prs-ProcessingWindowType1A-r17 ENUMERATED {option1, option2, option3} OPTIONAL,

prs-ProcessingWindowType1B-r17 ENUMERATED {option1, option2, option3} OPTIONAL,

prs-ProcessingWindowType2-r17 ENUMERATED {option1, option2, option3} OPTIONAL,

-- R1 27-15: Positioning SRS transmission in RRC\_INACTIVE state for initial UL BWP

srs-AllPosResourcesRRC-Inactive-r17 SRS-AllPosResourcesRRC-Inactive-r17 OPTIONAL,

-- R1 27-16: OLPC for positioning SRS in RRC\_INACTIVE state - gNB

olpc-SRS-PosRRC-Inactive-r17 OLPC-SRS-Pos-r16 OPTIONAL,

-- R1 27-19: Spatial relation for positioning SRS in RRC\_INACTIVE state - gNB

spatialRelationsSRS-PosRRC-Inactive-r17 SpatialRelationsSRS-Pos-r16 OPTIONAL,

-- R1 30-1: Increased maximum number of PUSCH Type A repetitions

maxNumberPUSCH-TypeA-Repetition-r17 ENUMERATED {supported} OPTIONAL,

-- R1 30-2: PUSCH Type A repetitions based on available slots

puschTypeA-RepetitionsAvailSlot-r17 ENUMERATED {supported} OPTIONAL,

-- R1 30-3: TB processing over multi-slot PUSCH

tb-ProcessingMultiSlotPUSCH-r17 ENUMERATED {supported} OPTIONAL,

-- R1 30-3a: Repetition of TB processing over multi-slot PUSCH

tb-ProcessingRepMultiSlotPUSCH-r17 ENUMERATED {supported} OPTIONAL,

-- R1 30-4: The maximum duration for DM-RS bundling

maxDurationDMRS-Bundling-r17 SEQUENCE {

fdd-r17 ENUMERATED {n4, n8, n16, n32} OPTIONAL,

tdd-r17 ENUMERATED {n2, n4, n8, n16} OPTIONAL

} OPTIONAL,

-- R1 30-6: Repetition of PUSCH transmission scheduled by RAR UL grant and DCI format 0\_0 with CRC scrambled by TC-RNTI

pusch-RepetitionMsg3-r17 ENUMERATED {supported} OPTIONAL,

sharedSpectrumChAccessParamsPerBand-v1710 SharedSpectrumChAccessParamsPerBand-v1710 OPTIONAL,

-- R4 25-2: Parallel measurements on cells belonging to a different NGSO satellite than a serving satellite without scheduling restrictions

-- on normal operations with the serving cell

parallelMeasurementWithoutRestriction-r17 ENUMERATED {supported} OPTIONAL,

-- R4 25-5: Parallel measurements on multiple NGSO satellites within a SMTC

maxNumber-NGSO-SatellitesWithinOneSMTC-r17 ENUMERATED {n1, n2, n3, n4} OPTIONAL,

-- R1 26-10: K1 range extension

k1-RangeExtension-r17 ENUMERATED {supported} OPTIONAL,

-- R1 35-1: Aperiodic CSI-RS for tracking for fast SCell activation

aperiodicCSI-RS-FastScellActivation-r17 SEQUENCE {

maxNumberAperiodicCSI-RS-PerCC-r17 ENUMERATED {n8, n16, n32, n48, n64, n128, n255},

maxNumberAperiodicCSI-RS-AcrossCCs-r17 ENUMERATED {n8, n16, n32, n64, n128, n256, n512, n1024}

} OPTIONAL,

-- R1 35-2: Aperiodic CSI-RS bandwidth for tracking for fast SCell activation for 10MHz UE channel bandwidth

aperiodicCSI-RS-AdditionalBandwidth-r17 ENUMERATED {addBW-Set1, addBW-Set2} OPTIONAL,

-- R1 28-1a: RRC-configured DL BWP without CD-SSB or NCD-SSB

bwp-WithoutCD-SSB-OrNCD-SSB-RedCap-r17 ENUMERATED {supported} OPTIONAL,

-- R1 28-3: Half-duplex FDD operation type A for (e)RedCap UE

halfDuplexFDD-TypeA-RedCap-r17 ENUMERATED {supported} OPTIONAL,

-- R1 27-15b: Positioning SRS transmission in RRC\_INACTIVE state configured outside initial UL BWP

posSRS-RRC-Inactive-OutsideInitialUL-BWP-r17 PosSRS-RRC-Inactive-OutsideInitialUL-BWP-r17 OPTIONAL,

-- R4 15-3 UE support of CBW for 480kHz SCS

channelBWs-DL-SCS-480kHz-FR2-2-r17 BIT STRING (SIZE (8)) OPTIONAL,

channelBWs-UL-SCS-480kHz-FR2-2-r17 BIT STRING (SIZE (8)) OPTIONAL,

-- R4 15-4 UE support of CBW for 960kHz SCS

channelBWs-DL-SCS-960kHz-FR2-2-r17 BIT STRING (SIZE (8)) OPTIONAL,

channelBWs-UL-SCS-960kHz-FR2-2-r17 BIT STRING (SIZE (8)) OPTIONAL,

-- R4 17-1 UL gap for Tx power management

ul-GapFR2-r17 ENUMERATED {supported} OPTIONAL,

-- R1 25-4: One-shot HARQ ACK feedback triggered by DCI format 1\_2

oneShotHARQ-feedbackTriggeredByDCI-1-2-r17 ENUMERATED {supported} OPTIONAL,

-- R1 25-5: PHY priority handling for one-shot HARQ ACK feedback

oneShotHARQ-feedbackPhy-Priority-r17 ENUMERATED {supported} OPTIONAL,

-- R1 25-6: Enhanced type 3 HARQ-ACK codebook feedback

enhancedType3-HARQ-CodebookFeedback-r17 SEQUENCE {

enhancedType3-HARQ-Codebooks-r17 ENUMERATED {n1, n2, n4, n8},

maxNumberPUCCH-Transmissions-r17 ENUMERATED {n1, n2, n3, n4, n5, n6, n7}

} OPTIONAL,

-- R1 25-7: Triggered HARQ-ACK codebook re-transmission

triggeredHARQ-CodebookRetx-r17 SEQUENCE {

minHARQ-Retx-Offset-r17 ENUMERATED {n-7, n-5, n-3, n-1, n1},

maxHARQ-Retx-Offset-r17 ENUMERATED {n4, n6, n8, n10, n12, n14, n16, n18, n20, n22, n24}

} OPTIONAL

]],

[[

-- R4 22-2 support of one shot large UL timing adjustment

ue-OneShotUL-TimingAdj-r17 ENUMERATED {supported} OPTIONAL,

-- R1 25-2: Repetitions for PUCCH format 0, and 2 over multiple slots with K = 2, 4, 8

pucch-Repetition-F0-2-r17 ENUMERATED {supported} OPTIONAL,

-- R1 25-11a: 4-bits subband CQI for NTN and unlicensed

cqi-4-BitsSubbandNTN-SharedSpectrumChAccess-r17 ENUMERATED {supported} OPTIONAL,

-- R1 25-16: HARQ-ACK with different priorities multiplexing on a PUCCH/PUSCH

mux-HARQ-ACK-DiffPriorities-r17 ENUMERATED {supported} OPTIONAL,

-- R1 25-20a: Propagation delay compensation based on Rel-15 TA procedure for NTN and unlicensed

ta-BasedPDC-NTN-SharedSpectrumChAccess-r17 ENUMERATED {supported} OPTIONAL,

-- R1 33-2b: DCI-based enabling/disabling ACK/NACK-based feedback for dynamic scheduling for multicast

ack-NACK-FeedbackForMulticastWithDCI-Enabler-r17 ENUMERATED {supported} OPTIONAL,

-- R1 33-2e: Multiple G-RNTIs for group-common PDSCHs

maxNumberG-RNTI-r17 INTEGER (2..8) OPTIONAL,

-- R1 33-2f: Dynamic multicast with DCI format 4\_2

dynamicMulticastDCI-Format4-2-r17 ENUMERATED {supported} OPTIONAL,

-- R1 33-2i: Supported maximal modulation order for multicast PDSCH

maxModulationOrderForMulticast-r17 CHOICE {

fr1-r17 ENUMERATED {qam256, qam1024},

fr2-r17 ENUMERATED {qam64, qam256}

} OPTIONAL,

-- R1 33-3-1: Dynamic Slot-level repetition for group-common PDSCH for TN and licensed

dynamicSlotRepetitionMulticastTN-NonSharedSpectrumChAccess-r17 ENUMERATED {n8, n16} OPTIONAL,

-- R1 33-3-1a: Dynamic Slot-level repetition for group-common PDSCH for NTN and unlicensed

dynamicSlotRepetitionMulticastNTN-SharedSpectrumChAccess-r17 ENUMERATED {n8, n16} OPTIONAL,

-- R1 33-4-1: DCI-based enabling/disabling NACK-only based feedback for dynamic scheduling for multicast

nack-OnlyFeedbackForMulticastWithDCI-Enabler-r17 ENUMERATED {supported} OPTIONAL,

-- R1 33-5-1b: DCI-based enabling/disabling ACK/NACK-based feedback for dynamic scheduling for multicast

ack-NACK-FeedbackForSPS-MulticastWithDCI-Enabler-r17 ENUMERATED {supported} OPTIONAL,

-- R1 33-5-1h: Multiple G-CS-RNTIs for SPS group-common PDSCHs

maxNumberG-CS-RNTI-r17 INTEGER (2..8) OPTIONAL,

-- R1 33-10: Support group-common PDSCH RE-level rate matching for multicast

re-LevelRateMatchingForMulticast-r17 ENUMERATED {supported} OPTIONAL,

-- R1 36-1a: Support of 1024QAM for PDSCH with maximum 2 MIMO layers for FR1

pdsch-1024QAM-2MIMO-FR1-r17 ENUMERATED {supported} OPTIONAL,

-- R4 14-3 PRS measurement without MG

prs-MeasurementWithoutMG-r17 ENUMERATED {cpLength, quarterSymbol, halfSymbol, halfSlot} OPTIONAL,

-- R4 25-7: The number of target NGSO satellites the UE can monitor per carrier

maxNumber-NGSO-SatellitesPerCarrier-r17 INTEGER (3..4) OPTIONAL,

-- R1 27-3-3 DL PRS Processing Capability outside MG - buffering capability

prs-ProcessingCapabilityOutsideMGinPPW-r17 SEQUENCE (SIZE(1..3)) OF PRS-ProcessingCapabilityOutsideMGinPPWperType-r17 OPTIONAL,

-- R1 27-15a: Positioning SRS transmission in RRC\_INACTIVE state for initial UL BWP with semi-persistent SRS

srs-SemiPersistent-PosResourcesRRC-Inactive-r17 SEQUENCE {

maxNumOfSemiPersistentSRSposResources-r17 ENUMERATED {n1, n2, n4, n8, n16, n32, n64},

maxNumOfSemiPersistentSRSposResourcesPerSlot-r17 ENUMERATED {n1, n2, n3, n4, n5, n6, n8, n10, n12, n14}

} OPTIONAL,

-- R2: UE support of CBW for 120kHz SCS

channelBWs-DL-SCS-120kHz-FR2-2-r17 BIT STRING (SIZE (8)) OPTIONAL,

channelBWs-UL-SCS-120kHz-FR2-2-r17 BIT STRING (SIZE (8)) OPTIONAL

]],

[[

-- R1 30-4a: DM-RS bundling for PUSCH repetition type A

dmrs-BundlingPUSCH-RepTypeA-r17 ENUMERATED {supported} OPTIONAL,

-- R1 30-4b: DM-RS bundling for PUSCH repetition type B

dmrs-BundlingPUSCH-RepTypeB-r17 ENUMERATED {supported} OPTIONAL,

-- R1 30-4c: DM-RS bundling for TB processing over multi-slot PUSCH

dmrs-BundlingPUSCH-multiSlot-r17 ENUMERATED {supported} OPTIONAL,

-- R1 30-4d: DMRS bundling for PUCCH repetitions

dmrs-BundlingPUCCH-Rep-r17 ENUMERATED {supported} OPTIONAL,

-- R1 30-4e: Enhanced inter-slot frequency hopping with inter-slot bundling for PUSCH

interSlotFreqHopInterSlotBundlingPUSCH-r17 ENUMERATED {supported} OPTIONAL,

-- R1 30-4f: Enhanced inter-slot frequency hopping for PUCCH repetitions with DMRS bundling

interSlotFreqHopPUCCH-r17 ENUMERATED {supported} OPTIONAL,

-- R1 30-4g: Restart DM-RS bundling

dmrs-BundlingRestart-r17 ENUMERATED {supported} OPTIONAL,

-- R1 30-4h: DM-RS bundling for non-back-to-back transmission

dmrs-BundlingNonBackToBackTX-r17 ENUMERATED {supported} OPTIONAL

]],

[[

-- R1 33-5-1e: Dynamic Slot-level repetition for SPS group-common PDSCH for multicast

maxDynamicSlotRepetitionForSPS-Multicast-r17 ENUMERATED {n8, n16} OPTIONAL,

-- R1 33-5-1g: DCI-based enabling/disabling NACK-only based feedback for SPS group-common PDSCH for multicast

nack-OnlyFeedbackForSPS-MulticastWithDCI-Enabler-r17 ENUMERATED {supported} OPTIONAL,

-- R1 33-5-1i: Multicast SPS scheduling with DCI format 4\_2

sps-MulticastDCI-Format4-2-r17 ENUMERATED {supported} OPTIONAL,

-- R1 33-5-2: Multiple SPS group-common PDSCH configuration on PCell

sps-MulticastMultiConfig-r17 INTEGER (1..8) OPTIONAL,

-- R1 33-6-1: DL priority indication for multicast in DCI

priorityIndicatorInDCI-Multicast-r17 ENUMERATED {supported} OPTIONAL,

-- R1 33-6-1a: DL priority configuration for SPS multicast

priorityIndicatorInDCI-SPS-Multicast-r17 ENUMERATED {supported} OPTIONAL,

-- R1 33-6-2: Two HARQ-ACK codebooks simultaneously constructed for supporting HARQ-ACK codebooks with different priorities

-- for unicast and multicast at a UE

twoHARQ-ACK-CodebookForUnicastAndMulticast-r17 ENUMERATED {supported} OPTIONAL,

-- R1 33-6-3: More than one PUCCH for HARQ-ACK transmission for multicast or for unicast and multicast within a slot

multiPUCCH-HARQ-ACK-ForMulticastUnicast-r17 ENUMERATED {supported} OPTIONAL,

-- R1 33-9: Supporting unicast PDCCH to release SPS group-common PDSCH

releaseSPS-MulticastWithCS-RNTI-r17 ENUMERATED {supported} OPTIONAL

]],

[[

-- R1 41-3-1a UE automomous TA adjustment when cell-reselection happens

posUE-TA-AutoAdjustment-r18 ENUMERATED {supported} OPTIONAL,

-- R1 41-3-1: SRS for positioning configuration in multiple cells for UEs in RRC\_INACTIVE state for initial UL BWP

posSRS-ValidityAreaRRC-InactiveInitialUL-BWP-r18 ENUMERATED {supported} OPTIONAL,

-- R1 41-3-2: SRS for positioning configuration in multiple cells for UEs in RRC\_INACTIVE state for configured outside

-- initial UL BWP

posSRS-ValidityAreaRRC-InactiveOutsideInitialUL-BWP-r18 ENUMERATED {supported} OPTIONAL,

-- R1 41-5-1:PRS measurement with Rx frequency hopping within a MG and measurement reporting RRC\_CONNECTED for RedCap UEs

dl-PRS-MeasurementWithRxFH-RRC-ConnectedForRedCap-r18 DL-PRS-MeasurementWithRxFH-RRC-Connected-r18 OPTIONAL,

-- R1 41-5-2: Support of positioning SRS with Tx frequency hopping in RRC\_CONNECTED for RedCap UEs

posSRS-TxFH-RRC-ConnectedForRedCap-r18 PosSRS-TxFrequencyHoppingRRC-Connected-r18 OPTIONAL,

-- R1 41-5-2a: Support of positioning SRS with Tx frequency hopping in RRC\_INACTIVE for RedCap UEs

posSRS-TxFH-RRC-InactiveForRedCap-r18 PosSRS-TxFrequencyHoppingRRC-Inactive-r18 OPTIONAL,

-- R1 41-4-8: Support of Positioning SRS bandwidth aggregation in RRC\_INACTIVE

posSRS-BWA-RRC-Inactive-r18 PosSRS-BWA-RRC-Inactive-r18 OPTIONAL,

-- R1 41-4-6a support a Rel-17 single DCI scheduling positioning SRS resource sets across the linked carriers

-- for SRS bandwidth aggregation in RRC\_CONNECTED state

posJointTriggerBySingleDCI-RRC-Connected-r18 ENUMERATED {supported} OPTIONAL,

-- R1 41-5-1a PRS measurement with Rx frequency hopping in RRC\_INACTIVE for RedCap UEs

dl-PRS-MeasurementWithRxFH-RRC-InactiveforRedCap-r18 ENUMERATED {supported} OPTIONAL,

-- R1 41-5-1b PRS measurement with Rx frequency hopping in RRC\_IDLE for RedCap UEs

dl-PRS-MeasurementWithRxFH-RRC-IdleforRedCap-r18 ENUMERATED {supported} OPTIONAL,

-- R1 42-1: Spatial domain adaptation with CSI feedback based on CSI report sub-configuration(s) for periodic CSI reporting

spatialAdaptation-CSI-Feedback-r18 SEQUENCE {

csiFeedbackType-r18 ENUMERATED {sdType1, sdType2, both},

maxNumberLmax-r18 INTEGER (2..4),

maxNumberCSI-ResourcePerCC-r18 SEQUENCE {

sdType1-Resource-r18 INTEGER (1..32),

sdType2-Resource-r18 INTEGER (1..32)

},

maxNumberTotalCSI-ResourcePerCC-r18 SEQUENCE {

sdType1-Resource-r18 ENUMERATED {n8, n16, n24, n32, n64, n128},

sdType2-Resource-r18 ENUMERATED {n8, n16, n24, n32, n64, n128}

},

totalNumberCSI-Reporting-r18 INTEGER (2..4)

} OPTIONAL,

-- R1 42-1a: Spatial domain adaptation with CSI feedback based on CSI report sub-configuration(s) for periodic CSI

-- reporting on PUSCH

spatialAdaptation-CSI-FeedbackPUSCH-r18 SEQUENCE {

csiFeedbackType-r18 ENUMERATED {sdType1, sdType2, both},

maxNumberLmax-r18 INTEGER (2..8),

subReportCSI-r18 INTEGER (2..4),

maxNumberCSI-ResourcePerCC-r18 INTEGER (1..32),

maxNumberTotalCSI-ResourcePerCC-r18 ENUMERATED {n8, n16, n24, n32, n64, n128},

totalNumberCSI-Reporting-r18 INTEGER (2..12)

} OPTIONAL,

-- R1 42-1b: Spatial domain adaptation with CSI feedback based on CSI report sub-configuration(s) for aperiodic CSI reporting

spatialAdaptation-CSI-FeedbackAperiodic-r18 SEQUENCE {

csiFeedbackType-r18 ENUMERATED {sdType1, sdType2, both},

maxNumberLmax-r18 INTEGER (2..8),

subReportCSI-r18 INTEGER (2..4),

maxNumberCSI-ResourcePerCC-r18 SEQUENCE {

sdType1-Resource-r18 INTEGER (1..32),

sdType2-Resource-r18 INTEGER (1..32)

},

maxNumberTotalCSI-ResourcePerCC-r18 SEQUENCE {

sdType1-Resource-r18 ENUMERATED {n8, n16, n24, n32, n64, n128},

sdType2-Resource-r18 ENUMERATED {n8, n16, n24, n32, n64, n128}

},

totalNumberCSI-Reporting-r18 INTEGER (2..12)

} OPTIONAL,

-- R1 42-1c: Spatial domain adaptation with CSI feedback based on CSI report sub-configuration(s) for semi-persistent

-- CSI reporting on PUCCH

spatialAdaptation-CSI-FeedbackPUCCH-r18 SEQUENCE {

csiFeedbackType-r18 ENUMERATED {sdType1, sdType2, both},

maxNumberLmax-r18 INTEGER (2..4),

subReportCSI-r18 INTEGER (2..4),

maxNumberCSI-ResourcePerCC-r18 INTEGER (1..32),

maxNumberTotalCSI-ResourcePerCC-r18 ENUMERATED {n8, n16, n24, n32, n64, n128},

totalNumberCSI-Reporting-r18 INTEGER (2..4)

} OPTIONAL,

-- R1 42-2: Power domain adaptation with CSI feedback based on CSI report sub-configuration(s) for periodic CSI reporting

powerAdaptation-CSI-Feedback-r18 SEQUENCE {

maxNumberLmax-r18 INTEGER (2..4),

maxNumberCSI-ResourcePerCC-r18 INTEGER (1..32),

maxNumberTotalCSI-ResourcePerCC-r18 ENUMERATED {n8, n16, n24, n32, n64, n128},

totalNumberCSI-Reporting-r18 INTEGER (2..4)

} OPTIONAL,

-- R1 42-2a: Power domain adaptation with CSI feedback based on CSI report sub-configuration(s) for semi-persistent CSI

-- reporting on PUSCH

powerAdaptation-CSI-FeedbackPUSCH-r18 SEQUENCE {

maxNumberLmax-r18 INTEGER (2..8),

subReportCSI-r18 INTEGER (2..4),

maxNumberCSI-ResourcePerCC-r18 INTEGER (1..32),

maxNumberTotalCSI-ResourcePerCC-r18 ENUMERATED {n8, n16, n24, n32, n64, n128},

totalNumberCSI-Reporting-r18 INTEGER (2..12)

} OPTIONAL,

-- R1 42-2b: Power domain adaptation with CSI feedback based on CSI report sub-configuration(s) for aperiodic CSI reporting

powerAdaptation-CSI-FeedbackAperiodic-r18 SEQUENCE {

maxNumberLmax-r18 INTEGER (2..8),

subReportCSI-r18 INTEGER (2..4),

maxNumberCSI-ResourcePerCC-r18 INTEGER (1..32),

maxNumberTotalCSI-ResourcePerCC-r18 ENUMERATED {n8, n16, n24, n32, n64, n128},

totalNumberCSI-Reporting-r18 INTEGER (2..12)

} OPTIONAL,

-- R1 42-2c: Power domain adaptation with CSI feedback based on CSI report sub-configuration(s) for semi-persistent CSI

-- reporting on PUCCH

powerAdaptation-CSI-FeedbackPUCCH-r18 SEQUENCE {

maxNumberLmax-r18 INTEGER (2..4),

subReportCSI-r18 INTEGER (2..4),

maxNumberCSI-ResourcePerCC-r18 INTEGER (1..32),

maxNumberTotalCSI-ResourcePerCC-r18 ENUMERATED {n8, n16, n24, n32, n64, n128},

totalNumberCSI-Reporting-r18 INTEGER (2..4)

} OPTIONAL,

-- R1 42-4: Cell DTX and/or DRX operation based on RRC configuration

nes-CellDTX-DRX-r18 ENUMERATED {cellDTXonly, cellDRXonly, both} OPTIONAL,

-- R1 42-5: Cell DTX/DRX operation triggered by DCI format 2\_9

nes-CellDTX-DRX-DCI2-9-r18 ENUMERATED {supported} OPTIONAL,

-- R1 42-7: Mixed codebook combination for spatial domain adaptation with CSI feedback based on CSI report sub-configuration(s),

-- each containing one port subset configuration

mixCodeBookSpatialAdaptation-r18 ENUMERATED {supported} OPTIONAL,

-- R1 42-8: the number of CSI report(s) for which the UE can measure and process reference signals simultaneously in a CC of the

-- band for which this capability is provided.

simultaneousCSI-SubReportsPerCC-r18 INTEGER (1..8) OPTIONAL,

-- R1 44-2: NTN DMRS bundling enhancement for PUSCH in NGSO scenarios

ntn-DMRS-BundlingNGSO-r18 ENUMERATED {n4, n8, n16, n32} OPTIONAL,

-- R1 45-3: Beam indication with joint DL/UL LTM TCI states

ltm-BeamIndicationJointTCI-r18 SEQUENCE {

maxNumberJointTCI-PerCell-r18 ENUMERATED {n8,n12,n16,n24,n32,n48,n64,n128},

qcl-Resource-r18 ENUMERATED {ssb, trs, both},

maxNumberJointTCI-AcrossCells-r18 INTEGER (1..128),

maxNumberCells-r18 INTEGER (1..8)

} OPTIONAL,

dummy-ltm-MAC-CE-JointTCI-r18 SEQUENCE {

qcl-Resource-r18 ENUMERATED {ssb, trs, both},

maxNumberJointTCI-PerCell-r18 INTEGER (1..16),

maxNumberJointTCI-AcrossCells-r18 ENUMERATED {n1,n2,n3,n4,n8,n16,n32}

} OPTIONAL,

-- R1 45-4: Beam indication with separate DL/UL LTM TCI states

ltm-BeamIndicationSeparateTCI-r18 SEQUENCE {

maxNumberDL-TCI-PerCell-r18 ENUMERATED {n4,n8,n12,n16,n24,n32,n48,n64,n128},

maxNumberUL-TCI-PerCell-r18 ENUMERATED {n4,n8,n12,n16,n24,n32,n48,n64},

qcl-Resource-r18 ENUMERATED {ssb, trs, both},

maxNumberDL-TCI-AcrossCells-r18 INTEGER (1..128),

maxNumberUL-TCI-AcrossCells-r18 INTEGER (1..64),

maxNumberCells-r18 INTEGER (1..8)

} OPTIONAL,

dummy-ltm-MAC-CE-SeparateTCI-r18 SEQUENCE {

qcl-Resource-r18 ENUMERATED {ssb, trs, both},

maxNumberDL-TCI-PerCell-r18 INTEGER (1..8),

maxNumberUL-TCI-PerCell-r18 INTEGER (1..8),

maxNumberDL-TCI-AcrossCells-r18 ENUMERATED {n1,n2,n4,n8,n16},

maxNumberUL-TCI-AcrossCells-r18 ENUMERATED {n1,n2,n4,n8,n16}

} OPTIONAL,

-- R1 45-5: RACH-based early TA acquisition

rach-EarlyTA-Measurement-r18 INTEGER (1..8) OPTIONAL,

-- R1 45-6: UE-based TA measurement

ue-TA-Measurement-r18 INTEGER (1..8) OPTIONAL,

-- R1 45-7: TA indication in cell switch command

ta-IndicationCellSwitch-r18 ENUMERATED {supported} OPTIONAL,

-- R1 49-8: Triggered HARQ-ACK codebook re-transmission for DCI format 1\_3

triggeredHARQ-CodebookRetxDCI-1-3-r18 SEQUENCE {

minHARQ-Retx-Offset-r18 ENUMERATED {n-7, n-5, n-3, n-1, n1},

maxHARQ-Retx-Offset-r18 ENUMERATED {n4, n6, n8, n10, n12, n14, n16, n18, n20, n22, n24}

} OPTIONAL,

-- R1 49-12: Unified TCI with joint DL/UL TCI update by DCI format 1\_3 for intra-cell and inter-cell beam management with more than

-- one MAC-CE activated joint TCI state per CC

unifiedJointTCI-MultiMAC-CE-DCI-1-3-r18 SEQUENCE {

minBeamApplicationTime-r18 CHOICE {

fr1-r18 SEQUENCE {

scs-15kHz-r18 ENUMERATED {sym1, sym2, sym4, sym7, sym14, sym28, sym42, sym56, sym70} OPTIONAL,

scs-30kHz-r18 ENUMERATED {sym1, sym2, sym4, sym7, sym14, sym28, sym42, sym56, sym70} OPTIONAL,

scs-60kHz-r18 ENUMERATED {sym1, sym2, sym4, sym7, sym14, sym28, sym42, sym56, sym70} OPTIONAL

},

fr2-r18 SEQUENCE {

scs-60kHz-r18 ENUMERATED {sym1, sym2, sym4, sym7, sym14, sym28, sym42, sym56, sym70,

sym84, sym98, sym112, sym224, sym336} OPTIONAL,

scs-120kHz-r18 ENUMERATED {sym1, sym2, sym4, sym7, sym14, sym28, sym42, sym56, sym70,

sym84, sym98, sym112, sym224, sym336} OPTIONAL

}

},

maxActivatedTCI-PerCC-r18 INTEGER (2..8) OPTIONAL

} OPTIONAL,

-- R1 49-12a: Unified TCI with separate DL/UL TCI update by DCI format 1\_3 for intra-cell beam management with more than

-- one MAC-CE activated separate TCI state per CC

unifiedSeparateTCI-MultiMAC-CE-IntraCell-r18 SEQUENCE {

minBeamApplicationTime-r18 CHOICE {

fr1-r18 SEQUENCE {

scs-15kHz-r18 ENUMERATED {sym1, sym2, sym4, sym7, sym14, sym28, sym42, sym56, sym70,

sym84, sym98, sym112, sym224, sym336} OPTIONAL,

scs-30kHz-r18 ENUMERATED {sym1, sym2, sym4, sym7, sym14, sym28, sym42, sym56, sym70,

sym84, sym98, sym112, sym224, sym336} OPTIONAL,

scs-60kHz-r18 ENUMERATED {sym1, sym2, sym4, sym7, sym14, sym28, sym42, sym56, sym70,

sym84, sym98, sym112, sym224, sym336} OPTIONAL

},

fr2-r18 SEQUENCE {

scs-60kHz-r18 ENUMERATED {sym1, sym2, sym4, sym7, sym14, sym28, sym42, sym56, sym70,

sym84, sym98, sym112, sym224, sym336} OPTIONAL,

scs-120kHz-r18 ENUMERATED {sym1, sym2, sym4, sym7, sym14, sym28, sym42, sym56, sym70,

sym84, sym98, sym112, sym224, sym336} OPTIONAL

}

},

maxActivatedDL-TCI-PerCC-r18 INTEGER (2..8) OPTIONAL,

maxActivatedUL-TCI-PerCC-r18 INTEGER (2..8) OPTIONAL

} OPTIONAL,

-- R1 50-1: Multi-PUSCHs for Configured Grant

multiPUSCH-CG-r18 ENUMERATED {n16, n32} OPTIONAL,

-- R1 50-1a: Multiple active multi-PUSCHs configured grant configurations for a BWP of a serving cell

multiPUSCH-ActiveConfiguredGrant-r18 SEQUENCE {

maxNumberConfigsPerBWP ENUMERATED {n1, n2, n4, n8, n12},

maxNumberConfigsAllCC-FR1 INTEGER (2..32),

maxNumberConfigsAllCC-FR2 INTEGER (2..32)

} OPTIONAL,

-- R1 50-1b: Joint release in a DCI for two or more configured grant Type 2 configurations, including multi-PUSCH CG

-- configuration(s), for a given BWP of a serving cell

jointReleaseDCI-r18 ENUMERATED {supported} OPTIONAL,

-- R1 50-2: UCI indication of unused CG-PUSCH transmission occasions

cg-PUSCH-UTO-UCI-Ind-r18 ENUMERATED {supported} OPTIONAL,

-- R1 50-3: PDCCH monitoring resumption after UL NACK

pdcch-MonitoringResumptionAfterUL-NACK-r18 ENUMERATED {supported} OPTIONAL,

-- R1 51-1: Support for 3 MHz symmetric channel bandwidth in DL and UL

support3MHz-ChannelBW-Symmetric-r18 ENUMERATED {supported} OPTIONAL,

-- R1 51-1a: Support for 3 MHz channel bandwidth in uplink with larger than 3 MHz channel BW in DL

support3MHz-ChannelBW-Asymmetric-r18 ENUMERATED {supported} OPTIONAL,

-- R1 51-2a: support 12 PRB CORESET0

support12PRB-CORESET0-r18 ENUMERATED {supported} OPTIONAL,

-- R1 52-1: Reception of NR PDCCH candidates overlapping with LTE CRS REs

nr-PDCCH-OverlapLTE-CRS-RE-r18 SEQUENCE {

overlapInRE-r18 ENUMERATED {oneSymbolNoOverlap, someOrAllSymOverlap},

overlapInSymbol-r18 ENUMERATED {symbol2,symbol1And2}

} OPTIONAL,

-- R1 52-1a: Reception of NR PDCCH candidates overlapping with LTE CRS REs with multiple non-overlapping CRS rate matching patterns

nr-PDCCH-OverlapLTE-CRS-RE-MultiPatterns-r18 ENUMERATED {supported} OPTIONAL,

-- R1 52-1b: NR PDCCH reception that overlaps with LTE CRS within a single span of 3 consecutive OFDM symbols that is within the

-- first 4 OFDM symbols in a slot

nr-PDCCH-OverlapLTE-CRS-RE-Span-3-4-r18 ENUMERATED {supported} OPTIONAL,

-- R1 52-2: Two LTE-CRS overlapping rate matching patterns within NR 15 kHz carrier overlapping with LTE carrier (regardless of

-- support or configuration of multi-TRP)

twoRateMatchingEUTRA-CRS-patterns-3-4-r18 SEQUENCE {

maxNumberPatterns-r18 INTEGER (2..6),

maxNumberNon-OverlapPatterns-r18 INTEGER (1..3)

} OPTIONAL,

-- R1 52-2a: Two LTE-CRS overlapping rate matching patterns with two different values of coresetPoolIndex within NR 15 kHz carrier

-- overlapping with LTE carrier

overlapRateMatchingEUTRA-CRS-Patterns-3-4-Diff-CS-Pool-r18 ENUMERATED {supported} OPTIONAL,

-- R1 53-3: Support RLM/BM/BFD measurements based on NCD-SSB within active BWP

ncd-SSB-BWP-Wor-r18 ENUMERATED {supported} OPTIONAL,

-- R1 53-4: Support Support RLM/BM/BFD measurements based on CSI-RS when CD-SSB is outside active BWP

rlm-BM-BFD-CSI-RS-OutsideActiveBWP-r18 ENUMERATED {supported} OPTIONAL,

-- R1 54-1: PRACH coverage enhancements

prach-CoverageEnh-r18 ENUMERATED {supported} OPTIONAL,

-- R1 54-1a: PRACH repetitions with less than N symbols gap

prach-Repetition-r18 ENUMERATED {supported} OPTIONAL,

-- R1 54-3: Dynamic waveform switching

dynamicWaveformSwitch-r18 ENUMERATED {supported} OPTIONAL,

-- R1 54-3a: PHR enhancement for dynamic waveform switching

dynamicWaveformSwitchPHR-r18 ENUMERATED {supported} OPTIONAL,

-- R1 54-3b: Dynamic waveform switching for intra-band UL CA

dynamicWaveformSwitchIntraCA-r18 INTEGER (2..8) OPTIONAL,

-- R1 55-3: Multiple PUSCHs scheduling by single DCI for non-consecutive slots in FR1

multiPUSCH-SingleDCI-NonConsSlots-r18 ENUMERATED {supported} OPTIONAL,

-- R1 55-2d: single-symbol DL-PRS used in RTT-based Propagation delay compensation

pdc-maxNumberPRS-ResourceProcessedPerSlot-r18 SEQUENCE {

fr1-r18 SEQUENCE {

scs-15kHz-r18 ENUMERATED {n1, n2, n4, n6, n8, n12, n16, n24, n32, n48, n64} OPTIONAL,

scs-30kHz-r18 ENUMERATED {n1, n2, n4, n6, n8, n12, n16, n24, n32, n48, n64} OPTIONAL,

scs-60kHz-r18 ENUMERATED {n1, n2, n4, n6, n8, n12, n16, n24, n32, n48, n64} OPTIONAL

},

fr2-r18 SEQUENCE {

scs-60kHz-r18 ENUMERATED {n1, n2, n4, n6, n8, n12, n16, n24, n32, n48, n64} OPTIONAL,

scs-120kHz-r18 ENUMERATED {n1, n2, n4, n6, n8, n12, n16, n24, n32, n48, n64} OPTIONAL

}

} OPTIONAL,

-- R1 57-2: Intra-slot TDM-ed unicast PDSCH and group-common PDSCH for multicast in RRC\_INACTIVE state

intraSlot-PDSCH-MulticastInactive-r18 BOOLEAN OPTIONAL,

-- R1 57-1: Dynamic scheduling for multicast in RRC\_INACTIVE state

multicastInactive-r18 ENUMERATED {supported} OPTIONAL,

thresholdBasedMulticastResume-r18 ENUMERATED {supported} OPTIONAL,

-- R4 27-2: LowerMSD for inter-band NR CA and EN-DC

lowerMSD-r18 SEQUENCE (SIZE (1..maxLowerMSD-r18)) OF LowerMSD-r18 OPTIONAL,

lowerMSD-ENDC-r18 SEQUENCE (SIZE (1..maxLowerMSD-r18)) OF LowerMSD-r18 OPTIONAL,

-- R4 28-1: Enhanced channel raster

enhancedChannelRaster-r18 ENUMERATED {supported} OPTIONAL,

-- R4 30-2: Fast beam sweeping for layer-1 measurement when the UE is in multi-Rx operation

fastBeamSweepingMultiRx-r18 ENUMERATED {n2,n4,n6} OPTIONAL,

-- R4 31-2 Beam sweeping factor reduction for FR2 unknown SCell activation

beamSweepingFactorReduction-r18 SEQUENCE {

reduceForCellDetection ENUMERATED {n1, n2, n4, n6},

reduceForSSB-L1-RSRP-Meas INTEGER (0..7)

} OPTIONAL,

-- R4 34-1: Support of NR FR2 HST with simultaneous DL reception with two different QCL TypeD RSs

simultaneousReceptionTwoQCL-r18 ENUMERATED {supported} OPTIONAL,

-- R4 34-2: Enhanced FR2 HST RRM requirements for intra-band CA and inter-frequency measurements in connected mode

measEnhCAInterFreqFR2-r18 ENUMERATED {supported} OPTIONAL,

-- R4 34-4: Support of enhanced MAC CE for TCI state switch indication for FR2 HST

tci-StateSwitchInd-r18 ENUMERATED {supported} OPTIONAL,

-- R4 35-2: the requirements defined for ATG UE with antenna array or omni-direction antenna requirements.

antennaArrayType-r18 ENUMERATED {supported} OPTIONAL,

locationBasedCondHandoverATG-r18 ENUMERATED {supported} OPTIONAL,

-- R4 35-3: rated maximum output power value range from 23dBm to 40dBm with 1dB as granularity at maximum modulation order and full

-- PRB configurations.

maxOutputPowerATG-r18 INTEGER (1..18) OPTIONAL,

-- R4 39-6: Fast processing of LTM candidate cell RRC configuration

ltm-FastProcessingConfig-r18 SEQUENCE {

maxNumberStoredConfigCells-r18 ENUMERATED {n2,n3,n4,n5,n6,n7,n8,n9,n10,n11,n12,n16},

maxNumberConfigs-r18 INTEGER (1..4)

} OPTIONAL,

-- R4 39-8: Measurement validation based on EMR measurement during connection setup/resume

measValidationReportEMR-r18 ENUMERATED {supported} OPTIONAL,

-- R4 39-9: Measurement validation based on reselection measurement during connection setup/resume

measValidationReportReselectionMeasurements-r18 ENUMERATED {supported} OPTIONAL,

eventA4BasedCondHandoverNES-r18 ENUMERATED {supported} OPTIONAL,

nesBasedCondHandoverWithDCI-r18 ENUMERATED {supported} OPTIONAL,

rach-LessHandoverCG-r18 ENUMERATED {supported} OPTIONAL,

rach-LessHandoverDG-r18 ENUMERATED {supported} OPTIONAL,

locationBasedCondHandoverEMC-r18 ENUMERATED {supported} OPTIONAL,

mt-CG-SDT-r18 ENUMERATED {supported} OPTIONAL,

posSRS-PreconfigureRRC-InactiveInitialUL-BWP-r18 ENUMERATED {supported} OPTIONAL,

posSRS-PreconfigureRRC-InactiveOutsideInitialUL-BWP-r18 ENUMERATED {supported} OPTIONAL,

cg-SDT-PeriodicityExt-r18 ENUMERATED {supported} OPTIONAL,

-- R2: 2Rx XR UEs

supportOf2RxXR-r18 ENUMERATED {supported} OPTIONAL,

condHandoverWithCandSCG-change-r18 ENUMERATED {supported} OPTIONAL

]],

[[

mac-ParametersPerBand-r18 MAC-ParametersPerBand-r18 OPTIONAL,

channelBW-DL-NCR-r18 CHOICE {

fr1-100mhz SEQUENCE {

scs-15kHz ENUMERATED {supported} OPTIONAL,

scs-30kHz ENUMERATED {supported} OPTIONAL,

scs-60kHz ENUMERATED {supported} OPTIONAL

},

fr2-200mhz SEQUENCE {

scs-60kHz ENUMERATED {supported} OPTIONAL,

scs-120kHz ENUMERATED {supported} OPTIONAL

}

} OPTIONAL,

channelBW-UL-NCR-r18 CHOICE {

fr1-100mhz SEQUENCE {

scs-15kHz ENUMERATED {supported} OPTIONAL,

scs-30kHz ENUMERATED {supported} OPTIONAL,

scs-60kHz ENUMERATED {supported} OPTIONAL

},

fr2-200mhz SEQUENCE {

scs-60kHz ENUMERATED {supported} OPTIONAL,

scs-120kHz ENUMERATED {supported} OPTIONAL

}

} OPTIONAL,

ncr-PDSCH-64QAM-FR2-r18 ENUMERATED {supported} OPTIONAL,

ltm-MCG-IntraFreq-r18 ENUMERATED {supported} OPTIONAL,

ltm-SCG-IntraFreq-r18 ENUMERATED {supported} OPTIONAL

]],

[[

-- R1 45-3a: MAC-CE activated joint LTM TCI states

ltm-MAC-CE-JointTCI-r18 SEQUENCE {

qcl-Resource-r18 ENUMERATED {ssb, trs, both},

maxNumberJointTCI-PerCell-r18 INTEGER (1..16),

maxNumberJointTCI-AcrossCells-r18 INTEGER (1..32)

} OPTIONAL,

-- R1 45-4a: MAC-CE activated DL/UL LTM TCI states

ltm-MAC-CE-SeparateTCI-r18 SEQUENCE {

qcl-Resource-r18 ENUMERATED {ssb, trs, both},

maxNumberDL-TCI-PerCell-r18 INTEGER (1..8),

maxNumberUL-TCI-PerCell-r18 INTEGER (1..8),

maxNumberDL-TCI-AcrossCells-r18 INTEGER (1..32),

maxNumberUL-TCI-AcrossCells-r18 INTEGER (1..32)

} OPTIONAL

]],

[[  
 -- R1 60-7: UL resource muting for CP-OFDM waveform

ul-ResourceMutingCP-OFDM-r19 ENUMERATED {supported} OPTIONAL,

-- R1 60-7a: UL resource muting for DFTS-OFDM waveform

ul-ResourceMutingDFTS-OFDM-r19 ENUMERATED {supported} OPTIONAL,

-- R1 61-1: On-demand SSB SCell operation indicated by RRC based signaling in Case #1

od-SSB-NoAlwaysOn-RRC-r19 ENUMERATED {supported} OPTIONAL,

-- R1 61-1a: On-demand SSB SCell operation indicated to be activated by RRC based signaling and indicated to be adapted

-- and deactivated by MAC CE signalling in Case #1

od-SSB-NoAlwaysOn-RRC-MAC-CE-r19 ENUMERATED {supported} OPTIONAL,

-- R1 61-2: On-demand SSB SCell operation indicated by RRC based signaling in Case #2 for same center frequency

od-SSB-AlwaysOn-RRC-r19 ENUMERATED {timec1,timec1nc2} OPTIONAL,

-- R1 61-2a: On-demand SSB SCell operation indicated by RRC based signaling in Case #2 for different center frequency

od-SSB-AlwaysOn-RRC-Diff-r19 ENUMERATED {supported} OPTIONAL,

-- R1 61-2b: On-demand SSB SCell operation indicated to be activated by RRC based signaling and indicated to be adapted

-- and deactivated by MAC CE signalling in Case #2 for same center frequency

od-SSB-AlwaysOn-RRC-MAC-CE-r19 ENUMERATED {supported} OPTIONAL,

-- R1 61-2c: On-demand SSB SCell operation indicated to be activated by RRC based signaling and indicated to be adapted

-- and deactivated by MAC CE signalling in Case #2 for different center frequencies

od-SSB-AlwaysOn-RRC-MAC-CE-Diff-r19 ENUMERATED {supported} OPTIONAL,

-- R1 61-3: On-demand SSB SCell operation indicated via MAC CE in Case #1

od-SSB-NoAlwaysOn-MAC-CE-r19 ENUMERATED {explicit, both} OPTIONAL,

-- R1 61-4: On-demand SSB SCell operation indicated via MAC CE in Case #2 for same center frequency

od-SSB-AlwaysOn-MAC-CE-r19 SEQUENCE {

timeRelation-r19 ENUMERATED {timec1,timec1nc2},

deactivationScheme-r19 ENUMERATED {explicit, both}

} OPTIONAL,

-- R1 61-4a: On-demand SSB SCell operation indicated via MAC CE in Case #2 for different center frequencies

od-SSB-AlwaysOn-MAC-CE-Diff-r19 ENUMERATED {explicit, both} OPTIONAL,

-- R1 61-6: SSB burst periodicity adaptation for SCell operation

ssb-BurstPeriodicityAdaptation-r19 ENUMERATED {supported} OPTIONAL,

-- R1 61-7: Adaptation of RACH in time domain based on additional RACH resources

rach-AdaptationTimeDomain-r19 ENUMERATED {supported} OPTIONAL,

-- R1 63-3: CSI-RS as Type-D QCL source RS in the indicated joint LTM TCI state

ltm-BeamIndicationJointTCI-CSI-RS-r19 ENUMERATED {supported} OPTIONAL,

-- R1 63-3a: CSI-RS as Type-D QCL source RS for MAC-CE activated joint LTM TCI states

ltm-MAC-CE-JointTCI-CSI-RS-r19 ENUMERATED {supported} OPTIONAL,

-- R1 63-4: CSI-RS as Type-D QCL source RS in the indicated separate DL/UL LTM TCI states

ltm-BeamIndicationSeparateTCI-CSI-RS-r19 ENUMERATED {supported} OPTIONAL,

-- R1 63-4a: CSI-RS as Type-D QCL source RS for MAC-CE activated separate DL/UL LTM TCI states

ltm-MAC-CE-SeparateTCI-CSI-RS-r19 ENUMERATED {supported} OPTIONAL,

-- R1 67-2: Support of positioning SRS with Tx frequency hopping in RRC\_CONNECTED for non-RedCap UEs

posSRS-TxFH-RRC-ConnectedForNonRedCap-r19 PosSRS-TxFrequencyHoppingRRC-ConnectedNonRedCap-r19 OPTIONAL,

-- R1 67-2a: Support of positioning SRS with Tx frequency hopping in RRC\_INACTIVE for non-RedCap UEs

posSRS-TxFH-RRC-InactiveForNonRedCap-r19 PosSRS-TxFrequencyHoppingRRC-InactiveNonRedCap-r19 OPTIONAL,

-- R1 67-3: Fallback to a SSSG with designated index after a PUCCH carrying an SR is transmitted

sr-TriggeredSSSG-Switching-r19 ENUMERATED {supported} OPTIONAL,

-- R4 46-4: MPR reduction for single carrier with single value

mpr-SingleCC-SingleValue-r19[RIL]: O002, UECap ENUMERATED {supported} OPTIONAL,

-- R4 46-5: MPR reduction for single carrier with multiple values

mpr-SingleCC-MultipleValue-r19 ENUMERATED {supported} OPTIONAL,

-- R4 49-2: Fast Rx beam sweeping factor for FR2-1 L3 measurement delay reduction

fastRx-BSF-MeasDelayReduction-r19 ENUMERATED {n2,n4,n6} OPTIONAL,

-- R4-50-2: Additional processing time for OD-SSB activation and parameter update

od-SSB-AdditionalProcessingTime-r19 ENUMERATED {supported} OPTIONAL,

-- R4 61-1: Tx output power enhancement for NR-NTN UE

ntn-PowerBoosting-ERedCap-r19 ENUMERATED {supported} OPTIONAL

]]

}

BandNR-v16c0 ::= SEQUENCE {

pusch-RepetitionTypeA-v16c0 ENUMERATED {supported} OPTIONAL,

...

}

BandNR-v17b0 ::= SEQUENCE {

mimo-ParametersPerBand-v17b0 MIMO-ParametersPerBand-v17b0 OPTIONAL,

...

}

LowerMSD-r18 ::= SEQUENCE {

aggressorband1-r18 CHOICE {

nr FreqBandIndicatorNR,

eutra FreqBandIndicatorEUTRA

},

aggressorband2-r18 FreqBandIndicatorNR OPTIONAL,

msd-Information-r18 SEQUENCE (SIZE (1..maxLowerMSDInfo-r18)) OF MSD-Information-r18

}

MSD-Information-r18 ::= SEQUENCE {

msd-Type-r18 ENUMERATED {harmonic, harmonicMixing, crossBandIsolation, imd2, imd3, imd4, imd5, all, spare8, spare7,

spare6, spare5,spare4, spare3, spare2, spare1},

msd-PowerClass-r18 ENUMERATED {pc1dot5, pc2, pc3},

msd-Class-r18 ENUMERATED {classI, classII, classIII, classIV, classV, classVI, classVII, classVIII }

}

-- TAG-RF-PARAMETERS-STOP

-- ASN1STOP

|  |
| --- |
| *RF-Parameters* field descriptions |
| ***appliedFreqBandListFilter***  In this field the UE mirrors the *FreqBandList* that the NW provided in the capability enquiry, if any, as described in clause 5.6.1.4. The UE filtered the band combinations in the *supportedBandCombinationList* in accordance with this *appliedFreqBandListFilter*. The UE does not include this field if the UE capability is requested by E-UTRAN and the network request includes the field *eutra-nr-only* [10]. |
| ***dummy1, dummy2, dummy-ltm-MAC-CE-JointTCI-r18, dummy-ltm-MAC-CE-SeparateTCI-r18***  The fields are not used in the specification and the network ignores the received values. |
| ***supportedBandCombinationList***  A list of band combinations that the UE supports for NR (and NR-DC, if requested). The *FeatureSetCombinationId*:s in this list refer to the *FeatureSetCombination* entries in the *featureSetCombinations* list in the *UE-NR-Capability* IE. The UE does not include this field if the UE capability is requested by E-UTRAN and the network request includes the field *eutra-nr-only* [10]. |
| ***supportedBandCombinationListSidelinkEUTRA-NR***  A list of band combinations that the UE supports for NR sidelink communication only, for joint NR sidelink communication and V2X sidelink communication, or for V2X sidelink communication only. The UE does not include this field if the UE capability is requested by E-UTRAN (see TS 36.331[10]) and the network request includes the field *eutra-nr-only*. |
| ***supportedBandCombinationListSL-NonRelayDiscovery***  A list of band combinations that the UE supports for NR sidelink non-relay discovery. The encoding is defined in PC5 *BandCombinationListSidelinkNR-r16.* |
| ***supportedBandCombinationListSL-RelayDiscovery***  A list of band combinations that the UE supports for NR sidelink relay discovery. The encoding is defined in PC5 *BandCombinationListSidelinkNR-r16.* |
| ***supportedBandCombinationListSL-U2U-DiscoveryExt***  This field indicates the band parameter in *BandCombinationListSL-Discovery-r17* that the UE supports for NR U2U sidelink relay discovery in a band included in *supportedBandCombinationListSL-U2U-RelayDiscovery*. |
| ***supportedBandCombinationListSL-U2U-RelayDiscovery***  A list of band combinations that the UE supports for NR U2U sidelink relay discovery. The encoding is defined in PC5 *BandCombinationListSidelinkNR-r16.* |
| ***supportedBandCombinationList-UplinkTxSwitch***  A list of band combinations that the UE supports dynamic uplink Tx switching for NR UL CA and SUL. The *FeatureSetCombinationId*:s in this list refer to the *FeatureSetCombination* entries in the *featureSetCombinations* list in the *UE-NR-Capability* IE. The UE does not include this field if the UE capability is requested by E-UTRAN and the network request includes the field *eutra-nr-only* [10]. |
| ***supportedBandListNR***  A list of NR bands supported by the UE. If *supportedBandListNR-v16c0* is included, the UE shall include the same number of entries, and listed in the same order, as in *supportedBandListNR* (without suffix). |

#### – *RF-ParametersMRDC*

The IE *RF-ParametersMRDC* is used to convey RF related capabilities for MR-DC.

*RF-ParametersMRDC* information element

-- ASN1START

-- TAG-RF-PARAMETERSMRDC-START

RF-ParametersMRDC ::= SEQUENCE {

supportedBandCombinationList BandCombinationList OPTIONAL,

appliedFreqBandListFilter FreqBandList OPTIONAL,

...,

[[

srs-SwitchingTimeRequested ENUMERATED {true} OPTIONAL,

supportedBandCombinationList-v1540 BandCombinationList-v1540 OPTIONAL

]],

[[

supportedBandCombinationList-v1550 BandCombinationList-v1550 OPTIONAL

]],

[[

supportedBandCombinationList-v1560 BandCombinationList-v1560 OPTIONAL,

supportedBandCombinationListNEDC-Only BandCombinationList OPTIONAL

]],

[[

supportedBandCombinationList-v1570 BandCombinationList-v1570 OPTIONAL

]],

[[

supportedBandCombinationList-v1580 BandCombinationList-v1580 OPTIONAL

]],

[[

supportedBandCombinationList-v1590 BandCombinationList-v1590 OPTIONAL

]],

[[

supportedBandCombinationListNEDC-Only-v15a0 SEQUENCE {

supportedBandCombinationList-v1540 BandCombinationList-v1540 OPTIONAL,

supportedBandCombinationList-v1560 BandCombinationList-v1560 OPTIONAL,

supportedBandCombinationList-v1570 BandCombinationList-v1570 OPTIONAL,

supportedBandCombinationList-v1580 BandCombinationList-v1580 OPTIONAL,

supportedBandCombinationList-v1590 BandCombinationList-v1590 OPTIONAL

} OPTIONAL

]],

[[

supportedBandCombinationList-v1610 BandCombinationList-v1610 OPTIONAL,

supportedBandCombinationListNEDC-Only-v1610 BandCombinationList-v1610 OPTIONAL,

supportedBandCombinationList-UplinkTxSwitch-r16 BandCombinationList-UplinkTxSwitch-r16 OPTIONAL

]],

[[

supportedBandCombinationList-v1630 BandCombinationList-v1630 OPTIONAL,

supportedBandCombinationListNEDC-Only-v1630 BandCombinationList-v1630 OPTIONAL,

supportedBandCombinationList-UplinkTxSwitch-v1630 BandCombinationList-UplinkTxSwitch-v1630 OPTIONAL

]],

[[

supportedBandCombinationList-v1640 BandCombinationList-v1640 OPTIONAL,

supportedBandCombinationListNEDC-Only-v1640 BandCombinationList-v1640 OPTIONAL,

supportedBandCombinationList-UplinkTxSwitch-v1640 BandCombinationList-UplinkTxSwitch-v1640 OPTIONAL

]],

[[

supportedBandCombinationList-UplinkTxSwitch-v1670 BandCombinationList-UplinkTxSwitch-v1670 OPTIONAL

]],

[[

supportedBandCombinationList-v1700 BandCombinationList-v1700 OPTIONAL,

supportedBandCombinationList-UplinkTxSwitch-v1700 BandCombinationList-UplinkTxSwitch-v1700 OPTIONAL

]],

[[

supportedBandCombinationList-v1720 BandCombinationList-v1720 OPTIONAL,

supportedBandCombinationListNEDC-Only-v1720 SEQUENCE {

supportedBandCombinationList-v1700 BandCombinationList-v1700 OPTIONAL,

supportedBandCombinationList-v1720 BandCombinationList-v1720 OPTIONAL

} OPTIONAL,

supportedBandCombinationList-UplinkTxSwitch-v1720 BandCombinationList-UplinkTxSwitch-v1720 OPTIONAL

]],

[[

supportedBandCombinationList-v1730 BandCombinationList-v1730 OPTIONAL,

supportedBandCombinationListNEDC-Only-v1730 BandCombinationList-v1730 OPTIONAL,

supportedBandCombinationList-UplinkTxSwitch-v1730 BandCombinationList-UplinkTxSwitch-v1730 OPTIONAL

]],

[[

supportedBandCombinationList-v1740 BandCombinationList-v1740 OPTIONAL,

supportedBandCombinationListNEDC-Only-v1740 BandCombinationList-v1740 OPTIONAL,

supportedBandCombinationList-UplinkTxSwitch-v1740 BandCombinationList-UplinkTxSwitch-v1740 OPTIONAL

]],

[[

dummy1 BandCombinationList-v1770 OPTIONAL,

dummy2 BandCombinationList-UplinkTxSwitch-v1770 OPTIONAL

]],

[[

supportedBandCombinationList-v1780 BandCombinationList-v1780 OPTIONAL,

supportedBandCombinationListNEDC-Only-v1780 BandCombinationList-v1780 OPTIONAL,

supportedBandCombinationList-UplinkTxSwitch-v1780 BandCombinationList-UplinkTxSwitch-v1780 OPTIONAL

]],

[[

supportedBandCombinationList-v1790 BandCombinationList-v1790 OPTIONAL,

supportedBandCombinationList-UplinkTxSwitch-v1790 BandCombinationList-UplinkTxSwitch-v1790 OPTIONAL

]],

[[

supportedBandCombinationList-v1800 BandCombinationList-v1800 OPTIONAL,

supportedBandCombinationList-UplinkTxSwitch-v1800 BandCombinationList-UplinkTxSwitch-v1800 OPTIONAL

]],

[[

supportedBandCombinationList-v1830 BandCombinationList-v1830 OPTIONAL,

supportedBandCombinationList-UplinkTxSwitch-v1830 BandCombinationList-UplinkTxSwitch-v1830 OPTIONAL

]],

[[

supportedBandCombinationList-v1840 BandCombinationList-v1840 OPTIONAL,

supportedBandCombinationList-UplinkTxSwitch-v1840 BandCombinationList-UplinkTxSwitch-v1840 OPTIONAL

]],

[[

supportedBandCombinationList-v1860 BandCombinationList-v1860 OPTIONAL,

supportedBandCombinationList-UplinkTxSwitch-v1860 BandCombinationList-UplinkTxSwitch-v1860 OPTIONAL

]],

[[

supportedBandCombinationList-v1900 BandCombinationList-v1900 OPTIONAL,

supportedBandCombinationList-UplinkTxSwitch-v1900 BandCombinationList-UplinkTxSwitch-v1900 OPTIONAL

]]

}

RF-ParametersMRDC-v15g0 ::= SEQUENCE {

supportedBandCombinationList-v15g0 BandCombinationList-v15g0 OPTIONAL,

supportedBandCombinationListNEDC-Only-v15g0 BandCombinationList-v15g0 OPTIONAL

}

RF-ParametersMRDC-v15n0 ::= SEQUENCE {

supportedBandCombinationList-v15n0 BandCombinationList-v15n0 OPTIONAL

}

RF-ParametersMRDC-v16e0 ::= SEQUENCE {

supportedBandCombinationList-UplinkTxSwitch-v16e0 BandCombinationList-UplinkTxSwitch-v16e0 OPTIONAL

}

-- TAG-RF-PARAMETERSMRDC-STOP

-- ASN1STOP

|  |
| --- |
| *RF-ParametersMRDC* field descriptions |
| ***appliedFreqBandListFilter***  In this field the UE mirrors the *FreqBandList* that the NW provided in the capability enquiry, if any. The UE filtered the band combinations in the *supportedBandCombinationList* in accordance with this *appliedFreqBandListFilter*. |
| ***dummy1, dummy2***  The fields are not used in the specification and the network ignores the received values. |
| ***supportedBandCombinationList***  A list of band combinations that the UE supports for (NG)EN-DC, or both (NG)EN-DC and NE-DC. The *FeatureSetCombinationId*:s in this list refer to the *FeatureSetCombination* entries in the *featureSetCombinations* list in the *UE-MRDC-Capability* IE. |
| ***supportedBandCombinationListNEDC-Only, supportedBandCombinationListNEDC-Only-v1610, supportedBandCombinationListNEDC-Only-v1780***  A list of band combinations that the UE supports only for NE-DC. The *FeatureSetCombinationId*:s in this list refer to the *FeatureSetCombination* entries in the *featureSetCombinations* list in the *UE-MRDC-Capability* IE. |
| ***supportedBandCombinationList-UplinkTxSwitch***  A list of band combinations that the UE supports dynamic UL Tx switching for (NG)EN-DC. The *FeatureSetCombinationId*:s in this list refer to the *FeatureSetCombination* entries in the *featureSetCombinations* list in the *UE-MRDC-Capability* IE. |

#### – *RLC-Parameters*

The IE *RLC-Parameters* is used to convey capabilities related to RLC.

*RLC-Parameters* information element

-- ASN1START

-- TAG-RLC-PARAMETERS-START

RLC-Parameters ::= SEQUENCE {

am-WithShortSN ENUMERATED {supported} OPTIONAL,

um-WithShortSN ENUMERATED {supported} OPTIONAL,

um-WithLongSN ENUMERATED {supported} OPTIONAL,

...,

[[

extendedT-PollRetransmit-r16 ENUMERATED {supported} OPTIONAL,

extendedT-StatusProhibit-r16 ENUMERATED {supported} OPTIONAL

]],

[[

am-WithLongSN-RedCap-r17 ENUMERATED {supported} OPTIONAL

]],

[[

am-WithLongSN-NCR-r18 ENUMERATED {supported} OPTIONAL

]],

[[

remainingTimeBasedRetransmission-r19 ENUMERATED {supported} OPTIONAL,

remainingTimeBasedPolling-r19 ENUMERATED {supported} OPTIONAL,

rxRLC-Discard-r19 ENUMERATED {supported} OPTIONAL,

txRLC-StopReTxDiscardedSDU-r19 ENUMERATED {supported} OPTIONAL

]]

}

-- TAG-RLC-PARAMETERS-STOP

-- ASN1STOP

#### – *SDAP-Parameters*

The IE *SDAP-Parameters* is used to convey capabilities related to SDAP.

*SDAP-Parameters* information element

-- ASN1START

-- TAG-SDAP-PARAMETERS-START

SDAP-Parameters ::= SEQUENCE {

as-ReflectiveQoS ENUMERATED {true} OPTIONAL,

...,

[[

sdap-QOS-IAB-r16 ENUMERATED {supported} OPTIONAL,

sdapHeaderIAB-r16 ENUMERATED {supported} OPTIONAL

]],

[[

sdap-QOS-NCR-r18 ENUMERATED {supported} OPTIONAL,

sdap-HeaderNCR-r18 ENUMERATED {supported} OPTIONAL

]]

}

-- TAG-SDAP-PARAMETERS-STOP

-- ASN1STOP

#### – *SharedSpectrumChAccessParamsPerBand*

The IE *SharedSpectrumChAccessParamsPerBand* is used to convey shared channel access related parameters specific for a certain frequency band (not per feature set or band combination).

*SharedSpectrumChAccessParamsPerBand* information element

-- ASN1START

-- TAG-SHAREDSPECTRUMCHACCESSPARAMSPERBAND-START

SharedSpectrumChAccessParamsPerBand-r16 ::= SEQUENCE {

-- R1 10-1: UL channel access for dynamic channel access mode

ul-DynamicChAccess-r16 ENUMERATED {supported} OPTIONAL,

-- R1 10-1a: UL channel access for semi-static channel access mode

ul-Semi-StaticChAccess-r16 ENUMERATED {supported} OPTIONAL,

-- R1 10-2: SSB-based RRM for dynamic channel access mode

ssb-RRM-DynamicChAccess-r16 ENUMERATED {supported} OPTIONAL,

-- R1 10-2a: SSB-based RRM for semi-static channel access mode

ssb-RRM-Semi-StaticChAccess-r16 ENUMERATED {supported} OPTIONAL,

-- R1 10-2b: MIB reading on unlicensed cell

mib-Acquisition-r16 ENUMERATED {supported} OPTIONAL,

-- R1 10-2c: SSB-based RLM for dynamic channel access mode

ssb-RLM-DynamicChAccess-r16 ENUMERATED {supported} OPTIONAL,

-- R1 10-2d: SSB-based RLM for semi-static channel access mode

ssb-RLM-Semi-StaticChAccess-r16 ENUMERATED {supported} OPTIONAL,

-- R1 10-2e: SIB1 reception on unlicensed cell

sib1-Acquisition-r16 ENUMERATED {supported} OPTIONAL,

-- R1 10-2f: Support monitoring of extended RAR window

extRA-ResponseWindow-r16 ENUMERATED {supported} OPTIONAL,

-- R1 10-2g: SSB-based BFD/CBD for dynamic channel access mode

ssb-BFD-CBD-dynamicChannelAccess-r16 ENUMERATED {supported} OPTIONAL,

-- R1 10-2h: SSB-based BFD/CBD for semi-static channel access mode

ssb-BFD-CBD-semi-staticChannelAccess-r16 ENUMERATED {supported} OPTIONAL,

-- R1 10-2i: CSI-RS-based BFD/CBD for NR-U

csi-RS-BFD-CBD-r16 ENUMERATED {supported} OPTIONAL,

-- R1 10-7: UL channel access for 10 MHz SCell

ul-ChannelBW-SCell-10mhz-r16 ENUMERATED {supported} OPTIONAL,

-- R1 10-10: RSSI and channel occupancy measurement and reporting

rssi-ChannelOccupancyReporting-r16 ENUMERATED {supported} OPTIONAL,

-- R1 10-11:SRS starting position at any OFDM symbol in a slot

srs-StartAnyOFDM-Symbol-r16 ENUMERATED {supported} OPTIONAL,

-- R1 10-20: Support search space set configuration with freqMonitorLocation-r16

searchSpaceFreqMonitorLocation-r16 INTEGER (1..5) OPTIONAL,

-- R1 10-20a: Support coreset configuration with rb-Offset

coreset-RB-Offset-r16 ENUMERATED {supported} OPTIONAL,

-- R1 10-23:CGI reading on unlicensed cell for ANR functionality

cgi-Acquisition-r16 ENUMERATED {supported} OPTIONAL,

-- R1 10-25: Enable configured UL transmissions when DCI 2\_0 is configured but not detected

configuredUL-Tx-r16 ENUMERATED {supported} OPTIONAL,

-- R1 10-27: Wideband PRACH

prach-Wideband-r16 ENUMERATED {supported} OPTIONAL,

-- R1 10-29: Support available RB set indicator field in DCI 2\_0

dci-AvailableRB-Set-r16 ENUMERATED {supported} OPTIONAL,

-- R1 10-30: Support channel occupancy duration indicator field in DCI 2\_0

dci-ChOccupancyDuration-r16 ENUMERATED {supported} OPTIONAL,

-- R1 10-8: Type B PDSCH length {3, 5, 6, 8, 9, 10, 11, 12, 13} without DMRS shift due to CRS collision

typeB-PDSCH-length-r16 ENUMERATED {supported} OPTIONAL,

-- R1 10-9: Search space set group switching with explicit DCI 2\_0 bit field trigger or with implicit PDCCH decoding with DCI 2\_0 monitoring

searchSpaceSwitchWithDCI-r16 ENUMERATED {supported} OPTIONAL,

-- R1 10-9b: Search space set group switching with implicit PDCCH decoding without DCI 2\_0 monitoring

searchSpaceSwitchWithoutDCI-r16 ENUMERATED {supported} OPTIONAL,

-- R1 10-9d: Support Search space set group switching capability 2

searchSpaceSwitchCapability2-r16 ENUMERATED {supported} OPTIONAL,

-- R1 10-14: Non-numerical PDSCH to HARQ-ACK timing

non-numericalPDSCH-HARQ-timing-r16 ENUMERATED {supported} OPTIONAL,

-- R1 10-15: Enhanced dynamic HARQ codebook

enhancedDynamicHARQ-codebook-r16 ENUMERATED {supported} OPTIONAL,

-- R1 10-16: One-shot HARQ ACK feedback

oneShotHARQ-feedback-r16 ENUMERATED {supported} OPTIONAL,

-- R1 10-17: Multi-PUSCH UL grant

multiPUSCH-UL-grant-r16 ENUMERATED {supported} OPTIONAL,

-- R1 10-26: CSI-RS based RLM for NR-U

csi-RS-RLM-r16 ENUMERATED {supported} OPTIONAL,

dummy ENUMERATED {supported} OPTIONAL,

-- R1 10-31: Support of P/SP-CSI-RS reception with CSI-RS-ValidationWith-DCI-r16 configured

periodicAndSemi-PersistentCSI-RS-r16 ENUMERATED {supported} OPTIONAL,

-- R1 10-3: PRB interlace mapping for PUSCH

pusch-PRB-interlace-r16 ENUMERATED {supported} OPTIONAL,

-- R1 10-3a: PRB interlace mapping for PUCCH

pucch-F0-F1-PRB-Interlace-r16 ENUMERATED {supported} OPTIONAL,

-- R1 10-12: OCC for PRB interlace mapping for PF2 and PF3

occ-PRB-PF2-PF3-r16 ENUMERATED {supported} OPTIONAL,

-- R1 10-13a: Extended CP range of more than one symbol for CG-PUSCH

extCP-rangeCG-PUSCH-r16 ENUMERATED {supported} OPTIONAL,

-- R1 10-18: Configured grant with retransmission in CG resources

configuredGrantWithReTx-r16 ENUMERATED {supported} OPTIONAL,

-- R1 10-21a: Support using ED threshold given by gNB for UL to DL COT sharing

ed-Threshold-r16 ENUMERATED {supported} OPTIONAL,

-- R1 10-21b: Support UL to DL COT sharing

ul-DL-COT-Sharing-r16 ENUMERATED {supported} OPTIONAL,

-- R1 10-24: CG-UCI multiplexing with HARQ ACK

mux-CG-UCI-HARQ-ACK-r16 ENUMERATED {supported} OPTIONAL,

-- R1 10-28: Configured grant with Rel-16 enhanced resource configuration

cg-resourceConfig-r16 ENUMERATED {supported} OPTIONAL

}

SharedSpectrumChAccessParamsPerBand-v1630 ::= SEQUENCE {

-- R4 4-1: DL reception in intra-carrier guardband

dl-ReceptionIntraCellGuardband-r16 ENUMERATED {supported} OPTIONAL,

-- R4 4-2: DL reception when gNB does not transmit on all RB sets of a carrier as a result of LBT

dl-ReceptionLBT-subsetRB-r16 ENUMERATED {supported} OPTIONAL

}

SharedSpectrumChAccessParamsPerBand-v1640 ::= SEQUENCE {

-- 10-26b(1-4): CSI-RS based RRM measurement with associated SS-block

csi-RSRP-AndRSRQ-MeasWithSSB-r16 ENUMERATED {supported} OPTIONAL,

-- 10-26c(1-5): CSI-RS based RRM measurement without associated SS-block

csi-RSRP-AndRSRQ-MeasWithoutSSB-r16 ENUMERATED {supported} OPTIONAL,

-- 10-26d(1-6): CSI-RS based RS-SINR measurement

csi-SINR-Meas-r16 ENUMERATED {supported} OPTIONAL,

-- 10-26e(1-8): RLM based on a mix of SS block and CSI-RS signals within active BWP

ssb-AndCSI-RS-RLM-r16 ENUMERATED {supported} OPTIONAL,

-- 10-26f(1-9): CSI-RS based contention free RA for HO

csi-RS-CFRA-ForHO-r16 ENUMERATED {supported} OPTIONAL

}

SharedSpectrumChAccessParamsPerBand-v1650 ::= SEQUENCE {

-- Extension of R1 10-9 capability to configure up to 16 instead of 4 cells or cell groups, respectively

extendedSearchSpaceSwitchWithDCI-r16 ENUMERATED {supported} OPTIONAL

}

SharedSpectrumChAccessParamsPerBand-v1710 ::= SEQUENCE {

-- R1 25-12: UE initiated semi-static channel occupancy with dependent configurations

ul-Semi-StaticChAccessDependentConfig-r17 ENUMERATED {supported} OPTIONAL,

-- R1 25-13: UE initiated semi-static channel occupancy with independent configurations

ul-Semi-StaticChAccessIndependentConfig-r17 ENUMERATED {supported} OPTIONAL

}

-- TAG-SHAREDSPECTRUMCHACCESSPARAMSPERBAND-STOP

-- ASN1STOP

#### – S*haredSpectrumChAccessParamsSidelinkPerBand*

The IE *SharedSpectrumChAccessParamsSidelinkPerBand* is used to convey shared channel access related parameters related to NR sidelink communication, specific for a certain frequency band (not per feature set or band combination).

*SharedSpectrumChAccessParamsSidelinkPerBand* information element

-- ASN1START

-- TAG-SHAREDSPECTRUMCHACCESSPARAMSSIDELINKPERBAND-START

SharedSpectrumChAccessParamsSidelinkPerBand-r18 ::= SEQUENCE {

-- R1 47-k1: SL channel access for dynamic channel access mode

sl-DynamicChannelAccess-r18 ENUMERATED {supported} OPTIONAL,

-- R1 47-k2: SL multi-channel access for dynamic channel access mode

sl-DynamicMultiChannelAccess-r18 INTEGER (2..5) OPTIONAL,

-- R1 47-k6: Type1 LBT blocking Option 1

sl-LBT-Option1-r18 ENUMERATED {supported} OPTIONAL,

-- R1 47-k7: Type1 LBT blocking Option 2

sl-LBT-Option2-r18 ENUMERATED {supported} OPTIONAL,

-- R1 47-k9: Sidelink mode 1 resource allocation in shared spectrum

sl-ResourceAllocMode1-r18 ENUMERATED {supported} OPTIONAL,

-- R1 47-m1: Interlace RB-based SL transmission/reception

sl-Interlace-RB-TxRx-r18 ENUMERATED {supported} OPTIONAL,

-- R1 47-m5: Multiple PSFCH occasions per PSCCH/PSSCH

sl-PSFCH-MultiOccasion-r18 INTEGER (1..4) OPTIONAL,

-- R1 47-m10: Contiguous RB-based PSCCH/PSSCH transmission/reception

sl-ContiguousRB-TxRx-r18 ENUMERATED {supported} OPTIONAL,

-- R1 47-m11: PSFCH transmissions in multiple contiguous RB sets

sl-PSFCH-MultiContiguousRB-r18 ENUMERATED {supported} OPTIONAL,

-- R1 47-m11a: PSFCH transmissions in multiple non-contiguous RB sets

sl-PSFCH-MultiNonContiguousRB-r18 ENUMERATED {supported} OPTIONAL,

-- R1 47-m13: Transmissions/receptions of multiple dedicated PRBs in common interlace-based PSFCH

sl-MultiplePRB-CommonInterlacePSFCH-r18 SEQUENCE {

tx-TotalPRB-PSFCH-r18 ENUMERATED {n4, n5, n8, n15, n16, n20},

rx-TotalPRB-PSFCH-r18 ENUMERATED {n5, n6, n15, n16, n25, n26, n32, n35, n45, n46, n50, n64, n65}

} OPTIONAL,

-- R1 47-m13a: Transmissions/receptions of multiple interlaces in dedicated interlace-based PSFCH

sl-MultiplePRB-DedicatedInterlacePSFCH-r18 SEQUENCE {

tx-TotalPRB-PSFCH-r18 INTEGER (1..3),

rx-TotalPRB-PSFCH-r18 INTEGER (1..5)

} OPTIONAL

}

-- TAG-SHAREDSPECTRUMCHACCESSPARAMSSIDELINKPERBAND-STOP

-- ASN1STOP

#### – *SidelinkParameters*

The IE *SidelinkParameters* is used to convey capabilities related to NR and V2X sidelink communications/positioning.

*SidelinkParameters* information element

-- ASN1START

-- TAG-SIDELINKPARAMETERS-START

SidelinkParameters-r16 ::= SEQUENCE {

sidelinkParametersNR-r16 SidelinkParametersNR-r16 OPTIONAL,

sidelinkParametersEUTRA-r16 SidelinkParametersEUTRA-r16 OPTIONAL

}

SidelinkParametersNR-r16 ::= SEQUENCE {

rlc-ParametersSidelink-r16 RLC-ParametersSidelink-r16 OPTIONAL,

mac-ParametersSidelink-r16 MAC-ParametersSidelink-r16 OPTIONAL,

fdd-Add-UE-Sidelink-Capabilities-r16 UE-SidelinkCapabilityAddXDD-Mode-r16 OPTIONAL,

tdd-Add-UE-Sidelink-Capabilities-r16 UE-SidelinkCapabilityAddXDD-Mode-r16 OPTIONAL,

supportedBandListSidelink-r16 SEQUENCE (SIZE (1..maxBands)) OF BandSidelink-r16 OPTIONAL,

...,

[[

relayParameters-r17 RelayParameters-r17 OPTIONAL

]],

[[

-- R1 32-x: Use of new P0 parameters for open loop power control

p0-OLPC-Sidelink-r17 ENUMERATED {supported} OPTIONAL

]],

[[

pdcp-ParametersSidelink-r18 PDCP-ParametersSidelink-r18 OPTIONAL,

--R1 41-1-1a: Common SL-PRS processing capability

sl-PRS-CommonProcCapabilityPerUE-r18 SEQUENCE {

maxNumOfActiveSL-PRS-Resources-r18 SEQUENCE {

fr1-r18 ENUMERATED {n1, n2, n4, n6, n8, n12, n16, n24} OPTIONAL,

fr2-r18 ENUMERATED {n1, n2, n4, n6, n8, n12, n16, n24, n32, n48, n64, n128} OPTIONAL

},

maxNumOfSlotswithActiveSL-PRS-Resources-r18 SEQUENCE {

fr1-r18 ENUMERATED {n1, n2, n3, n4, n6, n8} OPTIONAL,

fr2-r18 ENUMERATED {n1, n2, n4, n8, n12, n16, n24, n32, n48, n64} OPTIONAL

}

} OPTIONAL

]]

}

SidelinkParametersEUTRA-r16 ::= SEQUENCE {

sl-ParametersEUTRA1-r16 OCTET STRING OPTIONAL,

sl-ParametersEUTRA2-r16 OCTET STRING OPTIONAL,

sl-ParametersEUTRA3-r16 OCTET STRING OPTIONAL,

supportedBandListSidelinkEUTRA-r16 SEQUENCE (SIZE (1..maxBandsEUTRA)) OF BandSidelinkEUTRA-r16 OPTIONAL,

...

}

RLC-ParametersSidelink-r16 ::= SEQUENCE {

am-WithLongSN-Sidelink-r16 ENUMERATED {supported} OPTIONAL,

um-WithLongSN-Sidelink-r16 ENUMERATED {supported} OPTIONAL,

...

}

MAC-ParametersSidelink-r16 ::= SEQUENCE {

mac-ParametersSidelinkCommon-r16 MAC-ParametersSidelinkCommon-r16 OPTIONAL,

mac-ParametersSidelinkXDD-Diff-r16 MAC-ParametersSidelinkXDD-Diff-r16 OPTIONAL,

...

}

UE-SidelinkCapabilityAddXDD-Mode-r16 ::= SEQUENCE {

mac-ParametersSidelinkXDD-Diff-r16 MAC-ParametersSidelinkXDD-Diff-r16 OPTIONAL

}

MAC-ParametersSidelinkCommon-r16 ::= SEQUENCE {

lcp-RestrictionSidelink-r16 ENUMERATED {supported} OPTIONAL,

multipleConfiguredGrantsSidelink-r16 ENUMERATED {supported} OPTIONAL,

...,

[[

drx-OnSidelink-r17 ENUMERATED {supported} OPTIONAL

]],

[[

sl-LBT-FailureDectectionRecovery-r18 ENUMERATED {supported} OPTIONAL

]]

}

MAC-ParametersSidelinkXDD-Diff-r16 ::= SEQUENCE {

multipleSR-ConfigurationsSidelink-r16 ENUMERATED {supported} OPTIONAL,

logicalChannelSR-DelayTimerSidelink-r16 ENUMERATED {supported} OPTIONAL,

...

}

BandSidelinkEUTRA-r16 ::= SEQUENCE {

freqBandSidelinkEUTRA-r16 FreqBandIndicatorEUTRA,

-- R1 15-7: Transmitting LTE sidelink mode 3 scheduled by NR Uu

gnb-ScheduledMode3SidelinkEUTRA-r16 SEQUENCE {

gnb-ScheduledMode3DelaySidelinkEUTRA-r16 ENUMERATED {ms0, ms0dot25, ms0dot5, ms0dot625, ms0dot75, ms1,

ms1dot25, ms1dot5, ms1dot75, ms2, ms2dot5, ms3, ms4,

ms5, ms6, ms8, ms10, ms20}

} OPTIONAL,

-- R1 15-9: Transmitting LTE sidelink mode 4 configured by NR Uu

gnb-ScheduledMode4SidelinkEUTRA-r16 ENUMERATED {supported} OPTIONAL

}

BandSidelink-r16 ::= SEQUENCE {

freqBandSidelink-r16 FreqBandIndicatorNR,

--15-1

sl-Reception-r16 SEQUENCE {

harq-RxProcessSidelink-r16 ENUMERATED {n16, n24, n32, n48, n64},

pscch-RxSidelink-r16 ENUMERATED {value1, value2},

scs-CP-PatternRxSidelink-r16 CHOICE {

fr1-r16 SEQUENCE {

scs-15kHz-r16 BIT STRING (SIZE (16)) OPTIONAL,

scs-30kHz-r16 BIT STRING (SIZE (16)) OPTIONAL,

scs-60kHz-r16 BIT STRING (SIZE (16)) OPTIONAL

},

fr2-r16 SEQUENCE {

scs-60kHz-r16 BIT STRING (SIZE (16)) OPTIONAL,

scs-120kHz-r16 BIT STRING (SIZE (16)) OPTIONAL

}

} OPTIONAL,

extendedCP-RxSidelink-r16 ENUMERATED {supported} OPTIONAL

} OPTIONAL,

--15-2

sl-TransmissionMode1-r16 SEQUENCE {

harq-TxProcessModeOneSidelink-r16 ENUMERATED {n8, n16},

scs-CP-PatternTxSidelinkModeOne-r16 CHOICE {

fr1-r16 SEQUENCE {

scs-15kHz-r16 BIT STRING (SIZE (16)) OPTIONAL,

scs-30kHz-r16 BIT STRING (SIZE (16)) OPTIONAL,

scs-60kHz-r16 BIT STRING (SIZE (16)) OPTIONAL

},

fr2-r16 SEQUENCE {

scs-60kHz-r16 BIT STRING (SIZE (16)) OPTIONAL,

scs-120kHz-r16 BIT STRING (SIZE (16)) OPTIONAL

}

},

extendedCP-TxSidelink-r16 ENUMERATED {supported} OPTIONAL,

harq-ReportOnPUCCH-r16 ENUMERATED {supported} OPTIONAL

} OPTIONAL,

--15-4

sync-Sidelink-r16 SEQUENCE {

gNB-Sync-r16 ENUMERATED {supported} OPTIONAL,

gNB-GNSS-UE-SyncWithPriorityOnGNB-ENB-r16 ENUMERATED {supported} OPTIONAL,

gNB-GNSS-UE-SyncWithPriorityOnGNSS-r16 ENUMERATED {supported} OPTIONAL

} OPTIONAL,

--15-10

sl-Tx-256QAM-r16 ENUMERATED {supported} OPTIONAL,

--15-11

psfch-FormatZeroSidelink-r16 SEQUENCE {

psfch-RxNumber ENUMERATED {n5, n15, n25, n32, n35, n45, n50, n64},

psfch-TxNumber ENUMERATED {n4, n8, n16}

} OPTIONAL,

--15-12

lowSE-64QAM-MCS-TableSidelink-r16 ENUMERATED {supported} OPTIONAL,

--15-15

enb-sync-Sidelink-r16 ENUMERATED {supported} OPTIONAL,

...,

[[

--15-3

sl-TransmissionMode2-r16 SEQUENCE {

harq-TxProcessModeTwoSidelink-r16 ENUMERATED {n8, n16},

scs-CP-PatternTxSidelinkModeTwo-r16 ENUMERATED {supported} OPTIONAL,

dl-openLoopPC-Sidelink-r16 ENUMERATED {supported} OPTIONAL

} OPTIONAL,

--15-5

congestionControlSidelink-r16 SEQUENCE {

cbr-ReportSidelink-r16 ENUMERATED {supported} OPTIONAL,

cbr-CR-TimeLimitSidelink-r16 ENUMERATED {time1, time2}

} OPTIONAL,

--15-22

fewerSymbolSlotSidelink-r16 ENUMERATED {supported} OPTIONAL,

--15-23

sl-openLoopPC-RSRP-ReportSidelink-r16 ENUMERATED {supported} OPTIONAL,

--13-1

sl-Rx-256QAM-r16 ENUMERATED {supported} OPTIONAL

]],

[[

ue-PowerClassSidelink-r16 ENUMERATED {pc2, pc3, pc5-v1820, spare5, spare4, spare3, spare2, spare1}

OPTIONAL

]],

[[

--32-4a

sl-TransmissionMode2-RandomResourceSelection-r17 SEQUENCE {

harq-TxProcessModeTwoSidelink-r17 ENUMERATED {n8, n16},

scs-CP-PatternTxSidelinkModeTwo-r17 CHOICE {

fr1-r17 SEQUENCE {

scs-15kHz-r17 BIT STRING (SIZE (16)) OPTIONAL,

scs-30kHz-r17 BIT STRING (SIZE (16)) OPTIONAL,

scs-60kHz-r17 BIT STRING (SIZE (16)) OPTIONAL

},

fr2-r17 SEQUENCE {

scs-60kHz-r17 BIT STRING (SIZE (16)) OPTIONAL,

scs-120kHz-r17 BIT STRING (SIZE (16)) OPTIONAL

}

} OPTIONAL,

extendedCP-Mode2Random-r17 ENUMERATED {supported} OPTIONAL,

dl-openLoopPC-Sidelink-r17 ENUMERATED {supported} OPTIONAL

} OPTIONAL,

--32-4b

sync-Sidelink-v1710 SEQUENCE {

sync-GNSS-r17 ENUMERATED {supported} OPTIONAL,

gNB-Sync-r17 ENUMERATED {supported} OPTIONAL,

gNB-GNSS-UE-SyncWithPriorityOnGNB-ENB-r17 ENUMERATED {supported} OPTIONAL,

gNB-GNSS-UE-SyncWithPriorityOnGNSS-r17 ENUMERATED {supported} OPTIONAL

} OPTIONAL,

--32-4c

enb-sync-Sidelink-v1710 ENUMERATED {supported} OPTIONAL,

--32-5a-2

rx-IUC-Scheme1-PreferredMode2Sidelink-r17 ENUMERATED {supported} OPTIONAL,

--32-5a-3

rx-IUC-Scheme1-NonPreferredMode2Sidelink-r17 ENUMERATED {supported} OPTIONAL,

--32-5b-2

rx-IUC-Scheme2-Mode2Sidelink-r17 ENUMERATED {n5, n15, n25, n32, n35, n45, n50, n64} OPTIONAL,

--32-6-1

rx-IUC-Scheme1-SCI-r17 ENUMERATED {supported} OPTIONAL,

--32-6-2

rx-IUC-Scheme1-SCI-ExplicitReq-r17 ENUMERATED {supported} OPTIONAL

]],

[[

sharedSpectrumChAccessParamsSidelinkPerBand-r18 SharedSpectrumChAccessParamsSidelinkPerBand-r18 OPTIONAL,

--R1 41-1-1 Common SL-PRS processing capability in a SL BWP

sl-PRS-CommonProcCapabilityPerBand-r18 SEQUENCE {

maxSL-PRS-Bandwidth-r18 CHOICE {

fr1-r18 ENUMERATED {mhz5, mhz10, mhz20, mhz40, mhz50, mhz80, mhz100},

fr2-r18 ENUMERATED {mhz50, mhz100, mhz200, mhz400}

},

maxNumOfActiveSL-PRS-ResourcesInOneSlot-r18 CHOICE {

fr1-r18 ENUMERATED {n1, n2, n4, n6, n8, n12, n16, n24},

fr2-r18 ENUMERATED {n1, n2, n4, n6, n8, n12, n16, n24, n32, n48, n64, n128}

},

maxNumOfSlotsWithActiveSL-PRS-Resources-r18 CHOICE {

fr1-r18 ENUMERATED {n1, n2, n3, n4, n6, n8},

fr2-r18 ENUMERATED {n1, n2, n4, n8, n12, n16, n24, n32, n48, n64}

},

minTimeAfterEndofSlotCarryActiveSL-PRS-Resources-r18 ENUMERATED {ms20, ms30, ms40, ms50, ms80, ms100, ms160}

} OPTIONAL,

-- R1 41-1-2: Receiving SL-PRS in a shared resource pool

sl-PRS-RxInSharedResourcePool-r18 ENUMERATED {supported} OPTIONAL,

-- R1 41-1-3: Receiving SL-PRS in a dedicated resource pool

sl-PRS-RxInDedicatedResourcePool-r18 SEQUENCE {

numOfSupportedRxPSCCH-PerSlot-r18 ENUMERATED {value1, value2},

supportedCP-TypeFor60kHzSCS-r18 ENUMERATED {ncp, ncpAndECP}

} OPTIONAL,

-- R1 41-1-4a: Transmitting SL-PRS in a shared resource pool

sl-PRS-TxInSharedResourcePool-r18 ENUMERATED {supported} OPTIONAL,

-- R1 41-1-4b: Transmitting SL-PRS scheme 1 in a dedicated resource pool

sl-PRS-TxScheme1InDedicatedResourcePool-r18 ENUMERATED {supported} OPTIONAL,

-- R1 41-1-4c: Transmitting SL-PRS mode 2 in a dedicated resource pool

sl-PRS-TxScheme2InDedicatedResourcePool-r18 ENUMERATED {supported} OPTIONAL,

-- R1 41-1-5: SL-PRS congestion control in a dedicated resource pool

sl-PRS-CongestionCtrl-r18 ENUMERATED {cpt1, cpt2, cpt3} OPTIONAL,

-- R1 41-1-8: Support of random selection in a dedicated resource pool

sl-PRS-TxRandomSelection-r18 ENUMERATED {supported} OPTIONAL,

-- R1 41-1-10: Support of full sensing in a dedicated resource pool

sl-PRS-TxUsingFullSensing-r18 ENUMERATED {value1, value2} OPTIONAL,

-- R1 41-1-20: Supports SL PRS Rx for a band configured with SL CA

sl-PRS-RxForBandWithSL-CA-r18 ENUMERATED {supported} OPTIONAL,

-- R1 41-1-21: Supports SL PRS Tx for a band configured with SL CA

sl-PRS-TxForBandWithSL-CA-r18 ENUMERATED {supported} OPTIONAL,

-- R1 47-s1: Transmission/Reception using dynamic resource pool sharing

sl-DynamicSharingTxRx-r18 ENUMERATED {supported} OPTIONAL,

-- R1 47-v1: NR SL communication with SL CA

sl-CA-Communication-r18 SEQUENCE {

numberOfCarriers-r18 INTEGER (2..8),

numberOfPSCCH-DecodeValueZ-r18 INTEGER (1..2),

totalBandwidth-r18 ENUMERATED {mhz20,mhz30,mhz40,mhz50,mhz60,mhz70}

} OPTIONAL,

-- R1 47-v2: Synchronization for SL CA

sl-CA-Synchronization-r18 ENUMERATED {supported} OPTIONAL,

-- R1 47-v3: PSFCH for SL CA

sl-CA-PSFCH-r18 SEQUENCE {

rx-PSFCH-Resource-r18 ENUMERATED {n5,n15,n25,n32,n35,n45,n50,n64,n100},

tx-PSFCH-Resource-r18 ENUMERATED {n4,n8,n16,n24}

} OPTIONAL,

-- R4 45-2: SL reception in intra-carrier guard band

sl-ReceptionIntraCarrierGuardBand-r18 ENUMERATED {supported} OPTIONAL

]],

[[

-- R1 41-1-17: Open loop SL pathloss based power control for SL-PRS and associated PSCCH and SL RSRP report for dedicated

-- resource pool

sl-PathlossBasedOLPC-SL-RSRP-Report-r18 ENUMERATED {supported} OPTIONAL

]]

}

RelayParameters-r17 ::= SEQUENCE {

relayUE-Operation-L2-r17 ENUMERATED {supported} OPTIONAL,

remoteUE-Operation-L2-r17 ENUMERATED {supported} OPTIONAL,

remoteUE-PathSwitchToIdleInactiveRelay-r17 ENUMERATED {supported} OPTIONAL,

...,

[[

relayUE-U2U-OperationL2-r18 ENUMERATED {supported} OPTIONAL,

remoteUE-U2U-OperationL2-r18 ENUMERATED {supported} OPTIONAL,

remoteUE-U2N-PathSwitchOperationL2-r18 ENUMERATED {supported} OPTIONAL,

multipathRemoteUE-PC5L2-r18 ENUMERATED {supported} OPTIONAL,

multipathRelayUE-N3C-r18 ENUMERATED {supported} OPTIONAL,

multipathRemoteUE-N3C-r18 ENUMERATED {supported} OPTIONAL,

remoteUE-IndirectPathAddChangeToIdleInactiveRelay-r18 ENUMERATED {supported} OPTIONAL,

pdcp-DuplicationMoreThanOneUuRLC-r18 ENUMERATED {supported} OPTIONAL,

pdcp-CADuplicationDirectpath-DRB-r18 ENUMERATED {supported} OPTIONAL,

pdcp-CADuplicationDirectpath-SRB-r18 ENUMERATED {supported} OPTIONAL,

pdcp-DuplicationMP-SplitDRB-r18 ENUMERATED {supported} OPTIONAL,

pdcp-DuplicationMP-SplitSRB-r18 ENUMERATED {supported} OPTIONAL,

directpathRLF-RecoveryViaSRB1-r18 ENUMERATED {supported} OPTIONAL,

splitDRB-WithUL-BothDirectIndirect-r18 ENUMERATED {supported} OPTIONAL

]],

[[

relayUE-MH-OperationL2-r19 ENUMERATED {supported} OPTIONAL,

remoteUE-MH-OperationL2-r19 ENUMERATED {supported} OPTIONAL

]]

}

PDCP-ParametersSidelink-r18 ::= SEQUENCE {

pdcp-DuplicationSRB-sidelink-r18 ENUMERATED {supported} OPTIONAL,

pdcp-DuplicationDRB-sidelink-r18 ENUMERATED {supported} OPTIONAL,

...

}

-- TAG-SIDELINKPARAMETERS-STOP

-- ASN1STOP

|  |
| --- |
| *SidelinkParametersEUTRA* field descriptions |
| ***sl-ParametersEUTRA1, sl-ParametersEUTRA2, sl-ParametersEUTRA3***  This field includes IE of *SL-Parameters-v1430* (where *v2x-eNB-Scheduled-r14* and *V2X-SupportedBandCombination-r14* shall not be included), *SL-Parameters-v1530* (where *V2X-SupportedBandCombination-r1530* shall not be included) and *SL-Parameters-v1540* respectively defined in 36.331 [10]. It is used for reporting the per-UE capability for V2X sidelink communication. |

#### – *SimultaneousRxTxPerBandPair*

The IE *SimultaneousRxTxPerBandPair* contains the simultaneous Rx/Tx UE capability for each band pair in a band combination.

***SimultaneousRxTxPerBandPair* information element**

-- ASN1START

-- TAG-SIMULTANEOUSRXTXPERBANDPAIR-START

SimultaneousRxTxPerBandPair ::= BIT STRING (SIZE (3..496))

-- TAG-SIMULTANEOUSRXTXPERBANDPAIR-STOP

-- ASN1STOP

#### – *SON-Parameters*

The IE *SON-Parameters* contains SON related parameters.

*SON-Parameters* information element

-- ASN1START

-- TAG-SON-PARAMETERS-START

SON-Parameters-r16 ::= SEQUENCE {

rach-Report-r16 ENUMERATED {supported} OPTIONAL,

...,

[[

rlfReportCHO-r17 ENUMERATED {supported} OPTIONAL,

rlfReportDAPS-r17 ENUMERATED {supported} OPTIONAL,

success-HO-Report-r17 ENUMERATED {supported} OPTIONAL,

twoStepRACH-Report-r17 ENUMERATED {supported} OPTIONAL,

pscell-MHI-Report-r17 ENUMERATED {supported} OPTIONAL,

onDemandSI-Report-r17 ENUMERATED {supported} OPTIONAL

]],

[[

cef-ReportRedCap-r17 ENUMERATED {supported} OPTIONAL,

rlf-ReportRedCap-r17 ENUMERATED {supported} OPTIONAL

]],

[[

spr-Report-r18 ENUMERATED {supported} OPTIONAL,

successIRAT-HO-Report-r18 ENUMERATED {supported} OPTIONAL

]],

[[

rlfReport-LTM-r19 ENUMERATED {supported} OPTIONAL,

rlfReportCondHandoverWithCandSCG-r19 ENUMERATED {supported} OPTIONAL

]]

}

-- TAG-SON-PARAMETERS-STOP

-- ASN1STOP

#### – *SpatialRelationsSRS-Pos*

The IE *SpatialRelationsSRS-Pos* is used to convey spatial relation for SRS for positioning related parameters.

*SpatialRelationsSRS-Pos* information element

-- ASN1START

-- TAG-SPATIALRELATIONSSRS-POS-START

SpatialRelationsSRS-Pos-r16 ::= SEQUENCE {

spatialRelation-SRS-PosBasedOnSSB-Serving-r16 ENUMERATED {supported} OPTIONAL,

spatialRelation-SRS-PosBasedOnCSI-RS-Serving-r16 ENUMERATED {supported} OPTIONAL,

spatialRelation-SRS-PosBasedOnPRS-Serving-r16 ENUMERATED {supported} OPTIONAL,

spatialRelation-SRS-PosBasedOnSRS-r16 ENUMERATED {supported} OPTIONAL,

spatialRelation-SRS-PosBasedOnSSB-Neigh-r16 ENUMERATED {supported} OPTIONAL,

spatialRelation-SRS-PosBasedOnPRS-Neigh-r16 ENUMERATED {supported} OPTIONAL

}

--TAG-SPATIALRELATIONSSRS-POS-STOP

-- ASN1STOP

#### – *SRS-AllPosResourcesRRC-Inactive*

The IE *SRS-AllPosResourcesRRC-Inactive* is used to convey SRS positioning related parameters specific for a certain band.

*SRS-AllPosResourcesRRC-Inactive* information element

-- ASN1START

-- TAG-SRS-ALLPOSRESOURCESRRC-INACTIVE-START

SRS-AllPosResourcesRRC-Inactive-r17 ::= SEQUENCE {

srs-PosResourcesRRC-Inactive-r17 SEQUENCE {

-- R1 27-15: Positioning SRS transmission in RRC\_INACTIVE state for initial UL BWP

maxNumberSRS-PosResourceSetPerBWP-r17 ENUMERATED {n1, n2, n4, n8, n12, n16},

maxNumberSRS-PosResourcesPerBWP-r17 ENUMERATED {n1, n2, n4, n8, n16, n32, n64},

maxNumberSRS-ResourcesPerBWP-PerSlot-r17 ENUMERATED {n1, n2, n3, n4, n5, n6, n8, n10, n12, n14},

maxNumberPeriodicSRS-PosResourcesPerBWP-r17 ENUMERATED {n1, n2, n4, n8, n16, n32, n64},

maxNumberPeriodicSRS-PosResourcesPerBWP-PerSlot-r17 ENUMERATED {n1, n2, n3, n4, n5, n6, n8, n10, n12, n14},

dummy1 ENUMERATED {n1, n2, n4, n8, n16, n32, n64 },

dummy2 ENUMERATED {n1, n2, n3, n4, n5, n6, n8, n10, n12, n14}

}

}

-- TAG-SRS-ALLPOSRESOURCESRRC-INACTIVE-STOP

-- ASN1STOP

|  |
| --- |
| *SRS-AllPosResourcesRRC-Inactive* field descriptions |
| ***dummy1, dummy2***  The fields are not used in the specification and the network ignores the received values. |

#### – *SRS-SwitchingTimeNR*

The IE *SRS-SwitchingTimeNR* is used to indicate the SRS carrier switching time supported by the UE for one NR band pair.

*SRS-SwitchingTimeNR information element*

-- ASN1START

-- TAG-SRS-SWITCHINGTIMENR-START

SRS-SwitchingTimeNR ::= SEQUENCE {

switchingTimeDL ENUMERATED {n0us, n30us, n100us, n140us, n200us, n300us, n500us, n900us} OPTIONAL,

switchingTimeUL ENUMERATED {n0us, n30us, n100us, n140us, n200us, n300us, n500us, n900us} OPTIONAL

}

-- TAG-SRS-SWITCHINGTIMENR-STOP

-- ASN1STOP

#### – *SRS-SwitchingTimeEUTRA*

The IE *SRS-SwitchingTimeEUTRA* is used to indicate the SRS carrier switching time supported by the UE for one E-UTRA band pair.

*SRS-SwitchingTimeEUTRA information element*

-- ASN1START

-- TAG-SRS-SWITCHINGTIMEEUTRA-START

SRS-SwitchingTimeEUTRA ::= SEQUENCE {

switchingTimeDL ENUMERATED {n0, n0dot5, n1, n1dot5, n2, n2dot5, n3, n3dot5, n4, n4dot5, n5, n5dot5, n6, n6dot5, n7}

OPTIONAL,

switchingTimeUL ENUMERATED {n0, n0dot5, n1, n1dot5, n2, n2dot5, n3, n3dot5, n4, n4dot5, n5, n5dot5, n6, n6dot5, n7}

OPTIONAL

}

-- TAG-SRS-SWITCHINGTIMEEUTRA-STOP

-- ASN1STOP

#### – *SupportedAggBandwidth*

The IE *SupportedAggBandwidth* is used to indicate the aggregated bandwidth supported by the UE.

*SupportedAggBandwidth* information element

-- ASN1START

-- TAG-SUPPORTEDAGGBANDWIDTH-START

SupportedAggBandwidth-r17 ::= CHOICE {

fr1-r17 ENUMERATED {mhz20, mhz30, mhz35, mhz40, mhz50, mhz60, mhz70, mhz80, mhz90, mhz100, mhz110, mhz120, mhz130, mhz140,

mhz150, mhz160, mhz180, mhz200, mhz220, mhz230, mhz250, mhz280, mhz290, mhz300, mhz350, mhz400, mhz450,

mhz500, mhz600, mhz700, mhz800, spare1},

fr2-r17 ENUMERATED {mhz200, mhz300, mhz400, mhz500, mhz600, mhz700, mhz800, mhz900, mhz1000, mhz1100, mhz1200, mhz1300, mhz1400,

mhz1500, mhz1600, mhz1700, mhz1800, mhz1900, mhz2000, mhz2100, mhz2200, mhz2300, mhz2400, spare9, spare8,

spare7, spare6, spare5, spare4, spare3, spare2, spare1}

}

-- TAG-SUPPORTEDAGGBANDWIDTH-STOP

-- ASN1STOP

#### – *SupportedBandwidth*

The IE *SupportedBandwidth* is used to indicate the channel bandwidth supported by the UE on one carrier of a band of a band combination.

*SupportedBandwidth* information element

-- ASN1START

-- TAG-SUPPORTEDBANDWIDTH-START

SupportedBandwidth ::= CHOICE {

fr1 ENUMERATED {mhz5, mhz10, mhz15, mhz20, mhz25, mhz30, mhz40, mhz50, mhz60, mhz80, mhz100},

fr2 ENUMERATED {mhz50, mhz100, mhz200, mhz400}

}

SupportedBandwidth-v1700 ::= CHOICE {

fr1-r17 ENUMERATED {mhz5, mhz10, mhz15, mhz20, mhz25, mhz30, mhz35, mhz40, mhz45, mhz50, mhz60, mhz70, mhz80, mhz90, mhz100},

fr2-r17 ENUMERATED {mhz50, mhz100, mhz200, mhz400, mhz800, mhz1600, mhz2000}

}

SupportedBandwidth-v1840 ::= ENUMERATED {mhz3}

-- TAG-SUPPORTEDBANDWIDTH-STOP

-- ASN1STOP

#### – *UE-BasedPerfMeas-Parameters*

The IE *UE-BasedPerfMeas-Parameters* contains UE-based performance measurement parameters.

*UE-BasedPerfMeas-Parameters* information element

-- ASN1START

-- TAG-UE-BASEDPERFMEAS-PARAMETERS-START

UE-BasedPerfMeas-Parameters-r16 ::= SEQUENCE {

barometerMeasReport-r16 ENUMERATED {supported} OPTIONAL,

immMeasBT-r16 ENUMERATED {supported} OPTIONAL,

immMeasWLAN-r16 ENUMERATED {supported} OPTIONAL,

loggedMeasBT-r16 ENUMERATED {supported} OPTIONAL,

loggedMeasurements-r16 ENUMERATED {supported} OPTIONAL,

loggedMeasWLAN-r16 ENUMERATED {supported} OPTIONAL,

orientationMeasReport-r16 ENUMERATED {supported} OPTIONAL,

speedMeasReport-r16 ENUMERATED {supported} OPTIONAL,

gnss-Location-r16 ENUMERATED {supported} OPTIONAL,

ulPDCP-Delay-r16 ENUMERATED {supported} OPTIONAL,

...,

[[

sigBasedLogMDT-OverrideProtect-r17 ENUMERATED {supported} OPTIONAL,

multipleCEF-Report-r17 ENUMERATED {supported} OPTIONAL,

excessPacketDelay-r17 ENUMERATED {supported} OPTIONAL,

earlyMeasLog-r17 ENUMERATED {supported} OPTIONAL

]],

[[

loggedMDT-PNI-NPN-r18 ENUMERATED {supported} OPTIONAL,

loggedMDT-SNPN-r18 ENUMERATED {supported} OPTIONAL

]],

[[

geoAreaScopeChecking-r19 ENUMERATED {supported} OPTIONAL

]]

}

-- TAG-UE-BASEDPERFMEAS-PARAMETERS-STOP

-- ASN1STOP

#### – *UE-CapabilityRAT-ContainerList*

The IE *UE-CapabilityRAT-ContainerList* contains a list of radio access technology specific capability containers.

*UE-CapabilityRAT-ContainerList* information element

-- ASN1START

-- TAG-UE-CAPABILITYRAT-CONTAINERLIST-START

UE-CapabilityRAT-ContainerList ::= SEQUENCE (SIZE (0..maxRAT-CapabilityContainers)) OF UE-CapabilityRAT-Container

UE-CapabilityRAT-Container ::= SEQUENCE {

rat-Type RAT-Type,

ue-CapabilityRAT-Container OCTET STRING

}

-- TAG-UE-CAPABILITYRAT-CONTAINERLIST-STOP

-- ASN1STOP

|  |
| --- |
| *UE-CapabilityRAT-ContainerList* field descriptions |
| ***ue-CapabilityRAT-Container***  Container for the UE capabilities of the indicated RAT. The encoding is defined in the specification of each RAT:  For *rat-Type* set to *nr*: the encoding of UE capabilities is defined in *UE-NR-Capability*.  For *rat-Type* set to *eutra-nr*: the encoding of UE capabilities is defined in *UE-MRDC-Capability*.  For *rat-Type* set to *eutra*: the encoding of UE capabilities is defined in *UE-EUTRA-Capability* specified in TS 36.331 [10].  For *rat-Type* set to *utra-fdd*: the octet string contains the INTER RAT HANDOVER INFO message defined in TS 25.331 [45]. |

#### – *UE-CapabilityRAT-RequestList*

The IE *UE-CapabilityRAT-RequestList* is used to request UE capabilities for one or more RATs from the UE.

*UE-CapabilityRAT-RequestList* information element

-- ASN1START

-- TAG-UE-CAPABILITYRAT-REQUESTLIST-START

UE-CapabilityRAT-RequestList ::= SEQUENCE (SIZE (1..maxRAT-CapabilityContainers)) OF UE-CapabilityRAT-Request

UE-CapabilityRAT-Request ::= SEQUENCE {

rat-Type RAT-Type,

capabilityRequestFilter OCTET STRING OPTIONAL, -- Need N

...

}

-- TAG-UE-CAPABILITYRAT-REQUESTLIST-STOP

-- ASN1STOP

|  |
| --- |
| *UE-CapabilityRAT-Request* field descriptions |
| ***capabilityRequestFilter***  Information by which the network requests the UE to filter the UE capabilities.  For *rat-Type* set to *nr* or *eutra-nr*: the encoding of the *capabilityRequestFilter* is defined in *UE-CapabilityRequestFilterNR*.  For *rat-Type* set to *eutra*: the encoding of the *capabilityRequestFilter* is defined by *UECapabilityEnquiry* message defined in TS36.331 [10], in which *RAT-Type* in *UE-CapabilityRequest* includes only '*eutra'*. |
| ***rat-Type***  The RAT type for which the NW requests UE capabilities. |

#### – *UE-CapabilityRequestFilterNR*

The IE *UE-CapabilityRequestFilterNR* is used to request filtered UE capabilities.

*UE-CapabilityRequestFilterNR* information element

-- ASN1START

-- TAG-UE-CAPABILITYREQUESTFILTERNR-START

UE-CapabilityRequestFilterNR ::= SEQUENCE {

frequencyBandListFilter FreqBandList OPTIONAL, -- Need N

nonCriticalExtension UE-CapabilityRequestFilterNR-v1540 OPTIONAL

}

UE-CapabilityRequestFilterNR-v1540 ::= SEQUENCE {

srs-SwitchingTimeRequest ENUMERATED {true} OPTIONAL, -- Need N

nonCriticalExtension UE-CapabilityRequestFilterNR-v1710 OPTIONAL

}

UE-CapabilityRequestFilterNR-v1710 ::= SEQUENCE {

sidelinkRequest-r17 ENUMERATED {true} OPTIONAL, -- Need N

nonCriticalExtension SEQUENCE {} OPTIONAL

}

-- TAG-UE-CAPABILITYREQUESTFILTERNR-STOP

-- ASN1STOP

#### – *UE-CapabilityRequestFilterCommon*

The IE *UE-CapabilityRequestFilterCommon* is used to request filtered UE capabilities. The filter is common for all capability containers that are requested.

*UE-CapabilityRequestFilterCommon* information element

-- ASN1START

-- TAG-UE-CAPABILITYREQUESTFILTERCOMMON-START

UE-CapabilityRequestFilterCommon ::= SEQUENCE {

mrdc-Request SEQUENCE {

omitEN-DC ENUMERATED {true} OPTIONAL, -- Need N

includeNR-DC ENUMERATED {true} OPTIONAL, -- Need N

includeNE-DC ENUMERATED {true} OPTIONAL -- Need N

} OPTIONAL, -- Need N

...,

[[

codebookTypeRequest-r16 SEQUENCE {

type1-SinglePanel-r16 ENUMERATED {true} OPTIONAL, -- Need N

type1-MultiPanel-r16 ENUMERATED {true} OPTIONAL, -- Need N

type2-r16 ENUMERATED {true} OPTIONAL, -- Need N

type2-PortSelection-r16 ENUMERATED {true} OPTIONAL -- Need N

} OPTIONAL, -- Need N

uplinkTxSwitchRequest-r16 ENUMERATED {true} OPTIONAL -- Need N

]],

[[

requestedCellGrouping-r16 SEQUENCE (SIZE (1..maxCellGroupings-r16)) OF CellGrouping-r16 OPTIONAL -- Cond NRDC

]],

[[

fallbackGroupFiveRequest-r17 ENUMERATED {true} OPTIONAL -- Need N

]],

[[

lowerMSDRequest-r18 SEQUENCE {

pc1dot5-r18 ENUMERATED {true} OPTIONAL, -- Need N

pc2-r18 ENUMERATED {true} OPTIONAL, -- Need N

pc3-r18 ENUMERATED {true} OPTIONAL -- Need N

} OPTIONAL -- Need N

]]

}

CellGrouping-r16 ::= SEQUENCE {

mcg-r16 SEQUENCE (SIZE (1..maxBands)) OF FreqBandIndicatorNR,

scg-r16 SEQUENCE (SIZE (1..maxBands)) OF FreqBandIndicatorNR,

mode-r16 ENUMERATED {sync, async}

}

-- TAG-UE-CAPABILITYREQUESTFILTERCOMMON-STOP

-- ASN1STOP

|  |
| --- |
| *UE-CapabilityRequestFilterCommon field descriptions* |
| ***codebookTypeRequest***  Only if this field is present, the UE includes *SupportedCSI-RS-Resource* supported for the codebook type(s) requested within this field (i.e. type I single/multi-panel, type II and type II port selection) into *codebookVariantsList*, *codebookParametersPerBand* and *codebookParametersPerBC*. If this field is present and none of the codebook types is requested within this field (i.e. empty field), the UE includes *SupportedCSI-RS-Resource* supported for all codebook types into *codebookVariantsList*, *codebookParametersPerBand* and *codebookParametersPerBC*. |
| ***fallbackGroupFiveRequest***  Only if this field is present, the UE supporting FR2 CA bandwidth class from fallback group 5 shall include band combinations with FR2 CA bandwidth class from fallback group 5, and shall omit band combinations with FR2 CA bandwidth class from fallback group 2 or 3 (see TS 38.101-2 [39]) with same or lower capabilities. |
| ***includeNE-DC***  Only if this field is present, the UE supporting NE-DC shall indicate support for NE-DC in band combinations and include feature set combinations which are applicable to NE-DC. Band combinations supporting both NE-DC and (NG)EN-DC shall be included in *supportedBandCombinationList*, band combinations supporting only NE-DC shall be included in *supportedBandCombinationListNEDC-Only*. |
| ***includeNR-DC***  Only if this field is present, the UE supporting NR-DC shall indicate support for NR-DC in band combinations and include feature set combinations which are applicable to NR-DC. |
| ***lowerMSDRequest***  Only if this field is present, the UE supporting lower MSD shall indicate the lower MSD capability for the requested power class if supported. If no power class is explicitly requested, the UE supporting lower MSD shall indicate the lower MSD capability for the highest supported power class of the band combination consisting of victim band and aggressor band(s). |
| ***mode***  The mode of NR-DC operation that the NW is interested in for this cell grouping. The value *sync* means that the UE only indicates NR-DC support for band combinations for which it supports synchronous NR-DC with the requested cell grouping. The value *async* means that the UE only indicates NR-DC support for band combinations for which it supports asynchronous NR-DC with the requested cell grouping. |
| ***omitEN-DC***  Only if this field is present, the UE shall omit band combinations and feature set combinations which are only applicable to (NG)EN-DC. |
| ***requestedCellGrouping***  The NR-DC cell groupings that the NW is interested in, i.e., the bands that it might use in an MCG and the bands that it might use in an SCG. Only if this field is present, the UE indicates NR-DC support for band combinations for which it supports the requested cell grouping, i.e., in which it supports at least one of the *mcg* bands on MCG and at least one of the *scg* bands on the SCG. In its *supportedBandCombinationList*, the UE indicates which of its NR-DC band combinations supports which of the requested cell groupings. The first element in this list is referred to by ID#0, the second by ID#1 and so on. If this field is absent, the UE only includes band combinations for which it supports NR-DC with only FR1 bands in MCG and only FR2 bands in SCG.  Example 1: *requestedCellGrouping* is set to *mcg*=[n1, n7, n41, n66] and *scg*=[n78, n261]. This assumes that the NW would always use CA among n1, n7, n41 and n66 (depending on which are deployed on a given site) whereas with n78 and/or n261 the NW may need to use DC. With this filter a UE may report a band combination n1A-n7A-n78A for NR-DC only if it supports that serving cells for n1 and n7 are in the MCG and a serving cell for n78 is in the SCG. The UE may also report a band combination n41C-n261M for NR-DC provided that it supports a serving cell for n41 in the MCG and a serving cell for n261 in the SCG.  Example 2: One *requestedCellGrouping* is set to *mcg*=[n1, n7, n41, n66] and s*cg*=[n78, n261] and another *requestedCellGrouping* is set to *mcg*=[n1, n7, n66] and s*cg*=[ n41, n78, n261]. This assumes that the NW uses sometimes CA among n1, n7, n41 and n66 (as in example 1) and sometimes CA among n1, n7 and n66 but DC towards one or several of n41, n78, n261. If a UE supports n1A-n41A-n78A only if n41A and n78A are in the same cell group, this UE may only indicate cell grouping ID#1 (not #0) in its BC. |
| ***uplinkTxSwitchRequest***  Only if this field is present, the UE supporting dynamic UL Tx switching shall indicate support for UL Tx switching in band combinations which are applicable to inter-band UL CA, SUL and (NG)EN-DC. |

|  |  |
| --- | --- |
| Conditional Presence | Explanation |
| *NRDC* | The field is optionally present, Need N, if *includeNR-DC* is included. It is absent otherwise. |

#### – *UE-MRDC-Capability*

The IE *UE-MRDC-Capability* is used to convey the UE Radio Access Capability Parameters for MR-DC, see TS 38.306 [26].

*UE-MRDC-Capability* information element

-- ASN1START

-- TAG-UE-MRDC-CAPABILITY-START

UE-MRDC-Capability ::= SEQUENCE {

measAndMobParametersMRDC MeasAndMobParametersMRDC OPTIONAL,

phy-ParametersMRDC-v1530 Phy-ParametersMRDC OPTIONAL,

rf-ParametersMRDC RF-ParametersMRDC,

generalParametersMRDC GeneralParametersMRDC-XDD-Diff OPTIONAL,

fdd-Add-UE-MRDC-Capabilities UE-MRDC-CapabilityAddXDD-Mode OPTIONAL,

tdd-Add-UE-MRDC-Capabilities UE-MRDC-CapabilityAddXDD-Mode OPTIONAL,

fr1-Add-UE-MRDC-Capabilities UE-MRDC-CapabilityAddFRX-Mode OPTIONAL,

fr2-Add-UE-MRDC-Capabilities UE-MRDC-CapabilityAddFRX-Mode OPTIONAL,

featureSetCombinations SEQUENCE (SIZE (1..maxFeatureSetCombinations)) OF FeatureSetCombination OPTIONAL,

pdcp-ParametersMRDC-v1530 PDCP-ParametersMRDC OPTIONAL,

lateNonCriticalExtension OCTET STRING (CONTAINING UE-MRDC-Capability-v15g0) OPTIONAL,

nonCriticalExtension UE-MRDC-Capability-v1560 OPTIONAL

}

-- Regular non-critical extensions:

UE-MRDC-Capability-v1560 ::= SEQUENCE {

receivedFilters OCTET STRING (CONTAINING UECapabilityEnquiry-v1560-IEs) OPTIONAL,

measAndMobParametersMRDC-v1560 MeasAndMobParametersMRDC-v1560 OPTIONAL,

fdd-Add-UE-MRDC-Capabilities-v1560 UE-MRDC-CapabilityAddXDD-Mode-v1560 OPTIONAL,

tdd-Add-UE-MRDC-Capabilities-v1560 UE-MRDC-CapabilityAddXDD-Mode-v1560 OPTIONAL,

nonCriticalExtension UE-MRDC-Capability-v1610 OPTIONAL

}

UE-MRDC-Capability-v1610 ::= SEQUENCE {

measAndMobParametersMRDC-v1610 MeasAndMobParametersMRDC-v1610 OPTIONAL,

generalParametersMRDC-v1610 GeneralParametersMRDC-v1610 OPTIONAL,

pdcp-ParametersMRDC-v1610 PDCP-ParametersMRDC-v1610 OPTIONAL,

nonCriticalExtension UE-MRDC-Capability-v1700 OPTIONAL

}

UE-MRDC-Capability-v1700 ::= SEQUENCE {

measAndMobParametersMRDC-v1700 MeasAndMobParametersMRDC-v1700,

nonCriticalExtension UE-MRDC-Capability-v1730 OPTIONAL

}

UE-MRDC-Capability-v1730 ::= SEQUENCE {

measAndMobParametersMRDC-v1730 MeasAndMobParametersMRDC-v1730 OPTIONAL,

nonCriticalExtension UE-MRDC-Capability-v1800 OPTIONAL

}

UE-MRDC-Capability-v1800 ::= SEQUENCE {

-- R4 33-2: Support network control of requirementnetwork applicability for UE supporting interBandMRDC-WithOverlapDL-Bands-r16

requirementTypeIndication-r18 ENUMERATED {supported} OPTIONAL,

measAndMobParametersMRDC-v1810 MeasAndMobParametersMRDC-v1810 OPTIONAL,

nonCriticalExtension UE-MRDC-Capability-v1900 OPTIONAL

}

UE-MRDC-Capability-v1900 ::= SEQUENCE {

measAndMobParametersMRDC-v1900 MeasAndMobParametersMRDC-v1900 OPTIONAL,

nonCriticalExtension SEQUENCE {} OPTIONAL

}

-- Late non-critical extensions:

UE-MRDC-Capability-v15g0 ::= SEQUENCE {

rf-ParametersMRDC-v15g0 RF-ParametersMRDC-v15g0 OPTIONAL,

nonCriticalExtension UE-MRDC-Capability-v15n0 OPTIONAL

}

UE-MRDC-Capability-v15n0 ::= SEQUENCE {

rf-ParametersMRDC-v15n0 RF-ParametersMRDC-v15n0 OPTIONAL,

-- Following field is only for REL-15 late non-critical extensions

lateNonCriticalExtension OCTET STRING OPTIONAL,

nonCriticalExtension UE-MRDC-Capability-v16e0 OPTIONAL

}

UE-MRDC-Capability-v16e0 ::= SEQUENCE {

rf-ParametersMRDC-v16e0 RF-ParametersMRDC-v16e0 OPTIONAL,

nonCriticalExtension SEQUENCE {} OPTIONAL

}

UE-MRDC-CapabilityAddXDD-Mode ::= SEQUENCE {

measAndMobParametersMRDC-XDD-Diff MeasAndMobParametersMRDC-XDD-Diff OPTIONAL,

generalParametersMRDC-XDD-Diff GeneralParametersMRDC-XDD-Diff OPTIONAL

}

UE-MRDC-CapabilityAddXDD-Mode-v1560 ::= SEQUENCE {

measAndMobParametersMRDC-XDD-Diff-v1560 MeasAndMobParametersMRDC-XDD-Diff-v1560 OPTIONAL

}

UE-MRDC-CapabilityAddFRX-Mode ::= SEQUENCE {

measAndMobParametersMRDC-FRX-Diff MeasAndMobParametersMRDC-FRX-Diff

}

GeneralParametersMRDC-XDD-Diff ::= SEQUENCE {

splitSRB-WithOneUL-Path ENUMERATED {supported} OPTIONAL,

splitDRB-withUL-Both-MCG-SCG ENUMERATED {supported} OPTIONAL,

srb3 ENUMERATED {supported} OPTIONAL,

dummy ENUMERATED {supported} OPTIONAL,

...

}

GeneralParametersMRDC-v1610 ::= SEQUENCE {

f1c-OverEUTRA-r16 ENUMERATED {supported} OPTIONAL

}

-- TAG-UE-MRDC-CAPABILITY-STOP

-- ASN1STOP

|  |
| --- |
| *UE-MRDC-Capability* field descriptions |
| ***featureSetCombinations***  A list of *FeatureSetCombination*:s for *supportedBandCombinationList* and *supportedBandCombinationListNEDC-Only* in *UE-MRDC-Capability*. The *FeatureSetDownlink*:s and *FeatureSetUplink*:s referred to from these *FeatureSetCombination*:s are defined in the *featureSets* list in *UE-NR-Capability*. |

#### – *UE-NR-Capability*

The IE *UE-NR-Capability* is used to convey the NR UE Radio Access Capability Parameters, see TS 38.306 [26].

*UE-NR-Capability* information element

-- ASN1START

-- TAG-UE-NR-CAPABILITY-START

UE-NR-Capability ::= SEQUENCE {

accessStratumRelease AccessStratumRelease,

pdcp-Parameters PDCP-Parameters,

rlc-Parameters RLC-Parameters OPTIONAL,

mac-Parameters MAC-Parameters OPTIONAL,

phy-Parameters Phy-Parameters,

rf-Parameters RF-Parameters,

measAndMobParameters MeasAndMobParameters OPTIONAL,

fdd-Add-UE-NR-Capabilities UE-NR-CapabilityAddXDD-Mode OPTIONAL,

tdd-Add-UE-NR-Capabilities UE-NR-CapabilityAddXDD-Mode OPTIONAL,

fr1-Add-UE-NR-Capabilities UE-NR-CapabilityAddFRX-Mode OPTIONAL,

fr2-Add-UE-NR-Capabilities UE-NR-CapabilityAddFRX-Mode OPTIONAL,

featureSets FeatureSets OPTIONAL,

featureSetCombinations SEQUENCE (SIZE (1..maxFeatureSetCombinations)) OF FeatureSetCombination OPTIONAL,

lateNonCriticalExtension OCTET STRING (CONTAINING UE-NR-Capability-v15c0) OPTIONAL,

nonCriticalExtension UE-NR-Capability-v1530 OPTIONAL

}

-- Regular non-critical Rel-15 extensions:

UE-NR-Capability-v1530 ::= SEQUENCE {

fdd-Add-UE-NR-Capabilities-v1530 UE-NR-CapabilityAddXDD-Mode-v1530 OPTIONAL,

tdd-Add-UE-NR-Capabilities-v1530 UE-NR-CapabilityAddXDD-Mode-v1530 OPTIONAL,

dummy ENUMERATED {supported} OPTIONAL,

interRAT-Parameters InterRAT-Parameters OPTIONAL,

inactiveState ENUMERATED {supported} OPTIONAL,

delayBudgetReporting ENUMERATED {supported} OPTIONAL,

nonCriticalExtension UE-NR-Capability-v1540 OPTIONAL

}

UE-NR-Capability-v1540 ::= SEQUENCE {

sdap-Parameters SDAP-Parameters OPTIONAL,

overheatingInd ENUMERATED {supported} OPTIONAL,

ims-Parameters IMS-Parameters OPTIONAL,

fr1-Add-UE-NR-Capabilities-v1540 UE-NR-CapabilityAddFRX-Mode-v1540 OPTIONAL,

fr2-Add-UE-NR-Capabilities-v1540 UE-NR-CapabilityAddFRX-Mode-v1540 OPTIONAL,

fr1-fr2-Add-UE-NR-Capabilities UE-NR-CapabilityAddFRX-Mode OPTIONAL,

nonCriticalExtension UE-NR-Capability-v1550 OPTIONAL

}

UE-NR-Capability-v1550 ::= SEQUENCE {

reducedCP-Latency ENUMERATED {supported} OPTIONAL,

nonCriticalExtension UE-NR-Capability-v1560 OPTIONAL

}

UE-NR-Capability-v1560 ::= SEQUENCE {

nrdc-Parameters NRDC-Parameters OPTIONAL,

receivedFilters OCTET STRING (CONTAINING UECapabilityEnquiry-v1560-IEs) OPTIONAL,

nonCriticalExtension UE-NR-Capability-v1570 OPTIONAL

}

UE-NR-Capability-v1570 ::= SEQUENCE {

nrdc-Parameters-v1570 NRDC-Parameters-v1570 OPTIONAL,

nonCriticalExtension UE-NR-Capability-v1610 OPTIONAL

}

-- Late non-critical Rel-15 extensions:

UE-NR-Capability-v15c0 ::= SEQUENCE {

nrdc-Parameters-v15c0 NRDC-Parameters-v15c0 OPTIONAL,

partialFR2-FallbackRX-Req ENUMERATED {true} OPTIONAL,

nonCriticalExtension UE-NR-Capability-v15g0 OPTIONAL

}

UE-NR-Capability-v15g0 ::= SEQUENCE {

rf-Parameters-v15g0 RF-Parameters-v15g0 OPTIONAL,

nonCriticalExtension UE-NR-Capability-v15j0 OPTIONAL

}

UE-NR-Capability-v15j0 ::= SEQUENCE {

-- Following field is only for REL-15 late non-critical extensions

lateNonCriticalExtension OCTET STRING (CONTAINING UE-NR-Capability-v15t0) OPTIONAL,

nonCriticalExtension UE-NR-Capability-v16a0 OPTIONAL

}

UE-NR-Capability-v15t0 ::= SEQUENCE {

featureSets-v15t0 FeatureSets-v15t0 OPTIONAL,

measAndMobParameters-v15t0 MeasAndMobParameters-v15t0 OPTIONAL,

nonCriticalExtension SEQUENCE {} OPTIONAL

}

-- Regular non-critical Rel-16 extensions:

UE-NR-Capability-v1610 ::= SEQUENCE {

inDeviceCoexInd-r16 ENUMERATED {supported} OPTIONAL,

dl-DedicatedMessageSegmentation-r16 ENUMERATED {supported} OPTIONAL,

nrdc-Parameters-v1610 NRDC-Parameters-v1610 OPTIONAL,

powSav-Parameters-r16 PowSav-Parameters-r16 OPTIONAL,

fr1-Add-UE-NR-Capabilities-v1610 UE-NR-CapabilityAddFRX-Mode-v1610 OPTIONAL,

fr2-Add-UE-NR-Capabilities-v1610 UE-NR-CapabilityAddFRX-Mode-v1610 OPTIONAL,

bh-RLF-Indication-r16 ENUMERATED {supported} OPTIONAL,

directSN-AdditionFirstRRC-IAB-r16 ENUMERATED {supported} OPTIONAL,

bap-Parameters-r16 BAP-Parameters-r16 OPTIONAL,

referenceTimeProvision-r16 ENUMERATED {supported} OPTIONAL,

sidelinkParameters-r16 SidelinkParameters-r16 OPTIONAL,

highSpeedParameters-r16 HighSpeedParameters-r16 OPTIONAL,

mac-Parameters-v1610 MAC-Parameters-v1610 OPTIONAL,

mcgRLF-RecoveryViaSCG-r16 ENUMERATED {supported} OPTIONAL,

resumeWithStoredMCg-SCells-r16 ENUMERATED {supported} OPTIONAL,

resumeWithStoredSCG-r16 ENUMERATED {supported} OPTIONAL,

resumeWithSCG-Config-r16 ENUMERATED {supported} OPTIONAL,

ue-BasedPerfMeas-Parameters-r16 UE-BasedPerfMeas-Parameters-r16 OPTIONAL,

son-Parameters-r16 SON-Parameters-r16 OPTIONAL,

onDemandSIB-Connected-r16 ENUMERATED {supported} OPTIONAL,

nonCriticalExtension UE-NR-Capability-v1640 OPTIONAL

}

UE-NR-Capability-v1640 ::= SEQUENCE {

redirectAtResumeByNAS-r16 ENUMERATED {supported} OPTIONAL,

phy-ParametersSharedSpectrumChAccess-r16 Phy-ParametersSharedSpectrumChAccess-r16 OPTIONAL,

nonCriticalExtension UE-NR-Capability-v1650 OPTIONAL

}

UE-NR-Capability-v1650 ::= SEQUENCE {

mpsPriorityIndication-r16 ENUMERATED {supported} OPTIONAL,

highSpeedParameters-v1650 HighSpeedParameters-v1650 OPTIONAL,

nonCriticalExtension UE-NR-Capability-v1690 OPTIONAL

}

UE-NR-Capability-v1690 ::= SEQUENCE {

ul-RRC-Segmentation-r16 ENUMERATED {supported} OPTIONAL,

nonCriticalExtension UE-NR-Capability-v1700 OPTIONAL

}

-- Late non-critical extensions from Rel-16 onwards:

UE-NR-Capability-v16a0 ::= SEQUENCE {

phy-Parameters-v16a0 Phy-Parameters-v16a0 OPTIONAL,

rf-Parameters-v16a0 RF-Parameters-v16a0 OPTIONAL,

nonCriticalExtension UE-NR-Capability-v16c0 OPTIONAL

}

UE-NR-Capability-v16c0 ::= SEQUENCE {

rf-Parameters-v16c0 RF-Parameters-v16c0 OPTIONAL,

nonCriticalExtension UE-NR-Capability-v16d0 OPTIONAL

}

UE-NR-Capability-v16d0 ::= SEQUENCE {

featureSets-v16d0 FeatureSets-v16d0 OPTIONAL,

nonCriticalExtension UE-NR-Capability-v16j0 OPTIONAL

}

UE-NR-Capability-v16j0 ::= SEQUENCE {

rf-Parameters-v16j0 RF-Parameters-v16j0 OPTIONAL,

-- Following field is only for REL-16 late non-critical extensions

lateNonCriticalExtension OCTET STRING (CONTAINING UE-NR-Capability-v16k0) OPTIONAL,

nonCriticalExtension UE-NR-Capability-v17b0 OPTIONAL

}

UE-NR-Capability-v16k0 ::= SEQUENCE {

featureSets-v16k0 FeatureSets-v16k0 OPTIONAL,

nonCriticalExtension SEQUENCE {} OPTIONAL

}

-- Regular non-critical Rel-17 extensions:

UE-NR-Capability-v1700 ::= SEQUENCE {

inactiveStatePO-Determination-r17 ENUMERATED {supported} OPTIONAL,

highSpeedParameters-v1700 HighSpeedParameters-v1700 OPTIONAL,

powSav-Parameters-v1700 PowSav-Parameters-v1700 OPTIONAL,

mac-Parameters-v1700 MAC-Parameters-v1700 OPTIONAL,

ims-Parameters-v1700 IMS-Parameters-v1700 OPTIONAL,

measAndMobParameters-v1700 MeasAndMobParameters-v1700,

appLayerMeasParameters-r17 AppLayerMeasParameters-r17 OPTIONAL,

redCapParameters-r17 RedCapParameters-r17 OPTIONAL,

ra-SDT-r17 ENUMERATED {supported} OPTIONAL,

srb-SDT-r17 ENUMERATED {supported} OPTIONAL,

gNB-SideRTT-BasedPDC-r17 ENUMERATED {supported} OPTIONAL,

bh-RLF-DetectionRecovery-Indication-r17 ENUMERATED {supported} OPTIONAL,

nrdc-Parameters-v1700 NRDC-Parameters-v1700 OPTIONAL,

bap-Parameters-v1700 BAP-Parameters-v1700 OPTIONAL,

musim-GapPreference-r17 ENUMERATED {supported} OPTIONAL,

musimLeaveConnected-r17 ENUMERATED {supported} OPTIONAL,

mbs-Parameters-r17 MBS-Parameters-r17,

nonTerrestrialNetwork-r17 ENUMERATED {supported} OPTIONAL,

ntn-ScenarioSupport-r17 ENUMERATED {gso, ngso} OPTIONAL,

sliceInfoforCellReselection-r17 ENUMERATED {supported} OPTIONAL,

ue-RadioPagingInfo-r17 UE-RadioPagingInfo-r17 OPTIONAL,

-- R4 17-2 UL gap pattern for Tx power management

ul-GapFR2-Pattern-r17 BIT STRING (SIZE (4)) OPTIONAL,

ntn-Parameters-r17 NTN-Parameters-r17 OPTIONAL,

nonCriticalExtension UE-NR-Capability-v1740 OPTIONAL

}

UE-NR-Capability-v1740 ::= SEQUENCE {

redCapParameters-v1740 RedCapParameters-v1740,

nonCriticalExtension UE-NR-Capability-v1750 OPTIONAL

}

UE-NR-Capability-v1750 ::= SEQUENCE {

crossCarrierSchedulingConfigurationRelease-r17 ENUMERATED {supported} OPTIONAL,

nonCriticalExtension UE-NR-Capability-v1800 OPTIONAL

}

-- Late non-critical extensions from Rel-17 onwards:

UE-NR-Capability-v17b0 ::= SEQUENCE {

mac-Parameters-v17b0 MAC-Parameters-v17b0 OPTIONAL,

rf-Parameters-v17b0 RF-Parameters-v17b0 OPTIONAL,

ul-RRC-MaxCapaSegments-r17 ENUMERATED {supported} OPTIONAL,

nonCriticalExtension UE-NR-Capability-v17c0 OPTIONAL

}

UE-NR-Capability-v17c0 ::= SEQUENCE {

mac-Parameters-v17c0 MAC-Parameters-v17c0 OPTIONAL,

nonCriticalExtension UE-NR-Capability-v17d0 OPTIONAL

}

UE-NR-Capability-v17d0 ::= SEQUENCE {

featureSets-v17d0 FeatureSets-v17d0 OPTIONAL,

nonCriticalExtension SEQUENCE {} OPTIONAL

}

-- Regular non-critical Rel-18 extensions:

UE-NR-Capability-v1800 ::= SEQUENCE {

airToGroundNetwork-r18 ENUMERATED {supported} OPTIONAL,

eRedCapParameters-r18 ERedCapParameters-r18 OPTIONAL,

ncr-Parameters-r18 NCR-Parameters-r18 OPTIONAL,

softSatelliteSwitchResyncNTN-r18 ENUMERATED {supported} OPTIONAL,

hardSatelliteSwitchResyncNTN-r18 ENUMERATED {supported} OPTIONAL,

mt-SDT-r18 ENUMERATED {supported} OPTIONAL,

mt-SDT-NTN-r18 ENUMERATED {supported} OPTIONAL,

inDeviceCoexIndAutonomousDenial-r18 ENUMERATED {supported} OPTIONAL,

inDeviceCoexIndFDM-r18 ENUMERATED {supported} OPTIONAL,

inDeviceCoexIndTDM-r18 ENUMERATED {supported} OPTIONAL,

musim-GapPriorityPreference-r18 ENUMERATED {supported} OPTIONAL,

musim-CapabilityRestriction-r18 ENUMERATED {supported} OPTIONAL,

dummy ENUMERATED {supported} OPTIONAL,

ra-InsteadCG-SDT-r18 ENUMERATED {supported} OPTIONAL,

resumeAfterSDT-Release-r18 ENUMERATED {supported} OPTIONAL,

ul-TrafficInfo-r18 ENUMERATED {supported} OPTIONAL,

aerialParameters-r18 AerialParameters-r18 OPTIONAL,

--R4 40-2: beam steering

ntn-VSAT-AntennaType-r18 ENUMERATED {electronic, mechanical} OPTIONAL,

--R4 40-1: VSAT UE type in NTN

ntn-VSAT-MobilityType-r18 ENUMERATED {fixed, mobile} OPTIONAL,

ntn-Parameters-v1820 NTN-Parameters-v1820 OPTIONAL,

nonCriticalExtension UE-NR-Capability-v1830 OPTIONAL

}

UE-NR-Capability-v1830 ::= SEQUENCE {

sib19-Support-r18 ENUMERATED {supported} OPTIONAL,

nonCriticalExtension UE-NR-Capability-v1860 OPTIONAL

}

UE-NR-Capability-v1860 ::= SEQUENCE {

ntn-CHO-OnlyLocationTimeTrigger-r18 ENUMERATED {supported} OPTIONAL,

nonCriticalExtension UE-NR-Capability-v1900 OPTIONAL

}

UE-NR-Capability-v1900 ::= SEQUENCE {

aiml-Parameters-r19 AIML-Parameters-r19 OPTIONAL,

ue-RadioPagingInfo-r19 OCTET STRING (CONTAINING UE-RadioPagingInfo-r19) OPTIONAL,

-- R4 61-2: Support of (e)RedCap UE with FR1-NTN

ntn-ERedCap-FR1-r19 ENUMERATED {supported} OPTIONAL,

onDemandSIB1-r19 ENUMERATED {supported} OPTIONAL,

nonCriticalExtension SEQUENCE{} OPTIONAL

}

UE-NR-CapabilityAddXDD-Mode ::= SEQUENCE {

phy-ParametersXDD-Diff Phy-ParametersXDD-Diff OPTIONAL,

mac-ParametersXDD-Diff MAC-ParametersXDD-Diff OPTIONAL,

measAndMobParametersXDD-Diff MeasAndMobParametersXDD-Diff OPTIONAL

}

UE-NR-CapabilityAddXDD-Mode-v1530 ::= SEQUENCE {

eutra-ParametersXDD-Diff EUTRA-ParametersXDD-Diff

}

UE-NR-CapabilityAddFRX-Mode ::= SEQUENCE {

phy-ParametersFRX-Diff Phy-ParametersFRX-Diff OPTIONAL,

measAndMobParametersFRX-Diff MeasAndMobParametersFRX-Diff OPTIONAL

}

UE-NR-CapabilityAddFRX-Mode-v1540 ::= SEQUENCE {

ims-ParametersFRX-Diff IMS-ParametersFRX-Diff OPTIONAL

}

UE-NR-CapabilityAddFRX-Mode-v1610 ::= SEQUENCE {

powSav-ParametersFRX-Diff-r16 PowSav-ParametersFRX-Diff-r16 OPTIONAL,

mac-ParametersFRX-Diff-r16 MAC-ParametersFRX-Diff-r16 OPTIONAL

}

BAP-Parameters-r16 ::= SEQUENCE {

flowControlBH-RLC-ChannelBased-r16 ENUMERATED {supported} OPTIONAL,

flowControlRouting-ID-Based-r16 ENUMERATED {supported} OPTIONAL

}

BAP-Parameters-v1700 ::= SEQUENCE {

bapHeaderRewriting-Rerouting-r17 ENUMERATED {supported} OPTIONAL,

bapHeaderRewriting-Routing-r17 ENUMERATED {supported} OPTIONAL

}

MBS-Parameters-r17 ::= SEQUENCE {

maxMRB-Add-r17 INTEGER (1..16) OPTIONAL

}

-- TAG-UE-NR-CAPABILITY-STOP

-- ASN1STOP

|  |
| --- |
| *UE-NR-Capability* field descriptions |
| ***featureSetCombinations***  A list of *FeatureSetCombination:s* for *supportedBandCombinationList* in *UE-NR-Capability*. The *FeatureSetDownlink:s* and *FeatureSetUplink:s* referred to from these *FeatureSetCombination:s* are defined in the *featureSets* list in *UE-NR-Capability*. |

|  |
| --- |
| *UE-NR-Capability-v1540 field descriptions* |
| ***fr1-fr2-Add-UE-NR-Capabilities***  This instance of *UE-NR-CapabilityAddFRX-Mode* does not include any other fields than *csi-RS-IM-ReceptionForFeedback*/ *csi-RS-ProcFrameworkForSRS*/ *csi-ReportFramework*. |

#### – *UE-RadioPagingInfo*

The IE *UE-RadioPagingInfo* contains UE capability information needed for paging.

*UE-RadioPagingInfo* information element

-- ASN1START

-- TAG-UE-RADIOPAGINGINFO-START

UE-RadioPagingInfo-r17 ::= SEQUENCE {

-- R1 29-1: Paging enhancement

pei-SubgroupingSupportBandList-r17 SEQUENCE (SIZE (1..maxBands)) OF FreqBandIndicatorNR OPTIONAL,

...

}

UE-RadioPagingInfo-r19 ::= SEQUENCE {

lpwus-SupportedBandList-r19 SEQUENCE (SIZE (1..maxBands)) OF LPWUS-SupportedBandInfo-r19 OPTIONAL,

pagingAdaptation-r19 ENUMERATED {supported} OPTIONAL,

pagingAdaptionPEI-SupportBandList-r19 SEQUENCE (SIZE (1..maxBands)) OF FreqBandIndicatorNR OPTIONAL,

...

}

LPWUS-SupportedBandInfo-r19 ::= SEQUENCE {

supportedBandIndicator-r19 FreqBandIndicatorNR,

-- R1 62-1: LP-WUS operation in IDLE/INACTIVE mode based on OOK signal

lpwus-OOK-r19 ENUMERATED {supported} OPTIONAL,

-- R1 62-1a: LP-WUS operation in IDLE/INACTIVE mode based on OFDM overlaid sequence

lpwus-OFDM-r19 ENUMERATED {supported} OPTIONAL,

-- R1 62-1b: LP-SS based RRM measurement in IDLE/INACTIVE mode when LP-SS overlaid sequence is configured

lpwus-LP-SS-r19 ENUMERATED {supported} OPTIONAL,

minimumTimeGap-r19 [RIL]: E038, LPWUS SEQUENCE {

wakeUpDelay-SSB-Periodicity-LessThan20ms-r19 ENUMERATED {ms70, ms500, ms900} OPTIONAL,

wakeUpDelay-SSB-Periodicity-40ms-r19 ENUMERATED {ms130, ms600, ms1000} OPTIONAL,

wakeUpDelay-SSB-Periodicity-80ms-r19 ENUMERATED {ms250, ms800, ms1200} OPTIONAL,

wakeUpDelay-SSB-Periodicity-160ms-r19 ENUMERATED {ms490, ms1200, ms1600} OPTIONAL

}

}

-- TAG-UE-RADIOPAGINGINFO-STOP

-- ASN1STOP

NEXT CHANGE

# 11 Radio information related interactions between network nodes

## 11.1 General

This clause specifies RRC messages that are transferred between network nodes. These RRC messages may be transferred to or from the UE via another Radio Access Technology. Consequently, these messages have similar characteristics as the RRC messages that are transferred across the NR radio interface, i.e. the same transfer syntax and protocol extension mechanisms apply.

## 11.2 Inter-node RRC messages

### 11.2.1 General

This clause specifies RRC messages that are sent either across the X2-, Xn- or the NG-interface, either to or from the gNB, i.e. a single 'logical channel' is used for all RRC messages transferred across network nodes. The information could originate from or be destined for another RAT.

-- ASN1START

-- TAG-NR-INTER-NODE-DEFINITIONS-START

NR-InterNodeDefinitions DEFINITIONS AUTOMATIC TAGS ::=

BEGIN

IMPORTS

AffectedCarrierFreqCombList-r16,

AffectedCarrierFreqRangeCombList-r18,

ARFCN-ValueNR,

ARFCN-ValueEUTRA,

CandidateServingFreqListNR-r16,

CandidateServingFreqRangeListNR-r18,

CellIdentity,

CGI-InfoEUTRA,

CGI-InfoNR,

CondReconfigExecCondSCG-r17,

CSI-RS-Index,

CSI-RS-CellMobility,

DRX-Config,

EUTRA-PhysCellId,

FeatureSetDownlinkPerCC-Id,

FeatureSetUplinkPerCC-Id,

FlightPathInfoReport-r18,

FreqBandIndicatorNR,

GapConfig,

IDC-TDM-Assistance-r18,

maxBandComb,

maxBands,

maxBandsEUTRA,

maxCandidateBandIndex-r18,

maxCellSFTD,

maxFeatureSetsPerBand,

maxFreq,

maxFreqIDC-MRDC,

maxNrofCombIDC,

maxNrofCondCells-r16,

maxNrofCondCells-1-r17,

maxNrofPhysicalResourceBlocks,

maxNrofSCells,

maxNrofServingCells,

maxNrofServingCells-1,

maxNrofServingCellsEUTRA,

maxNrofIndexesToReport,

maxNrofLTM-Configs-r18,

maxSimultaneousBands,

MBSInterestIndication-r17,

MeasQuantityResults,

MeasResultCellListSFTD-EUTRA,

MeasResultCellListSFTD-NR,

MeasResultList2NR,

MeasResultSCG-Failure,

MeasResultServFreqListEUTRA-SCG,

MUSIM-CandidateBandList-r18,

MUSIM-CapRestriction-r18,

MUSIM-GapConfig-r17,

NeedForGapsInfoNR-r16,

NeedForGapNCSG-InfoNR-r17,

NeedForGapNCSG-InfoEUTRA-r17,

NeedForInterruptionInfoNR-r18,

OverheatingAssistance,

OverheatingAssistance-r17,

P-Max,

PhysCellId,

RadioBearerConfig,

RAN-NotificationAreaInfo,

ReferenceConfiguration-r18,

ReportConfigNR,

RRCReconfiguration,

ServCellIndex,

SetupRelease,

SSB-Index,

SSB-MTC,

SSB-ToMeasure,

SS-RSSI-Measurement,

ShortMAC-I,

SubcarrierSpacing,

UEAssistanceInformation,

UE-CapabilityRAT-ContainerList,

maxNrofCLI-RSSI-Resources-r16,

maxNrofCLI-SRS-Resources-r16,

RSSI-ResourceId-r16,

SDT-Config-r17,

SidelinkUEInformationNR-r16,

SRS-PosRRC-InactiveValidityAreaPreConfigList-r18,

SRS-ResourceId,

SuccessPSCell-Config-r18,

SupportedAggBandwidth-r17,

UE-RadioPagingInfo-r17,

UE-RadioPagingInfo-r19

FROM NR-RRC-Definitions;

-- TAG-NR-INTER-NODE-DEFINITIONS-STOP

-- ASN1STOP

### 11.2.2 Message definitions

#### – *UERadioPagingInformation*

This message is used to transfer radio paging information, covering both upload to and download from the 5GC, and between gNBs.

Direction: gNB to/ from 5GC and gNB to/from gNB

*UERadioPagingInformation* message

-- ASN1START

-- TAG-UE-RADIO-PAGING-INFORMATION-START

UERadioPagingInformation ::= SEQUENCE {

criticalExtensions CHOICE {

c1 CHOICE{

ueRadioPagingInformation UERadioPagingInformation-IEs,

spare7 NULL,

spare6 NULL, spare5 NULL, spare4 NULL,

spare3 NULL, spare2 NULL, spare1 NULL

},

criticalExtensionsFuture SEQUENCE {}

}

}

UERadioPagingInformation-IEs ::= SEQUENCE {

supportedBandListNRForPaging SEQUENCE (SIZE (1..maxBands)) OF FreqBandIndicatorNR OPTIONAL,

nonCriticalExtension UERadioPagingInformation-v15e0-IEs OPTIONAL

}

UERadioPagingInformation-v15e0-IEs ::= SEQUENCE {

dl-SchedulingOffset-PDSCH-TypeA-FDD-FR1 ENUMERATED {supported} OPTIONAL,

dl-SchedulingOffset-PDSCH-TypeA-TDD-FR1 ENUMERATED {supported} OPTIONAL,

dl-SchedulingOffset-PDSCH-TypeA-TDD-FR2 ENUMERATED {supported} OPTIONAL,

dl-SchedulingOffset-PDSCH-TypeB-FDD-FR1 ENUMERATED {supported} OPTIONAL,

dl-SchedulingOffset-PDSCH-TypeB-TDD-FR1 ENUMERATED {supported} OPTIONAL,

dl-SchedulingOffset-PDSCH-TypeB-TDD-FR2 ENUMERATED {supported} OPTIONAL,

nonCriticalExtension UERadioPagingInformation-v1700-IEs OPTIONAL

}

UERadioPagingInformation-v1700-IEs ::= SEQUENCE {

ue-RadioPagingInfo-r17 OCTET STRING (CONTAINING UE-RadioPagingInfo-r17) OPTIONAL,

inactiveStatePO-Determination-r17 ENUMERATED {supported} OPTIONAL,

numberOfRxRedCap-r17 ENUMERATED {one, two} OPTIONAL,

halfDuplexFDD-TypeA-RedCap-r17 SEQUENCE (SIZE (1..maxBands)) OF FreqBandIndicatorNR OPTIONAL,

nonCriticalExtension UERadioPagingInformation-v1800-IEs OPTIONAL

}

UERadioPagingInformation-v1800-IEs ::= SEQUENCE {

numberOfRxERedCap-r18 ENUMERATED {one, two} OPTIONAL,

supportOf2RxXR-r18 ENUMERATED {supported} OPTIONAL,

nonCriticalExtension UERadioPagingInformation-v1840-IEs OPTIONAL

}

UERadioPagingInformation-v1840-IEs ::= SEQUENCE {

dl-SchedulingOffset-PDSCH-TypeA-FDD-FR2-NTN-r18 ENUMERATED {supported} OPTIONAL,

dl-SchedulingOffset-PDSCH-TypeB-FDD-FR2-NTN-r18 ENUMERATED {supported} OPTIONAL,

nonCriticalExtension UERadioPagingInformation-v1900-IEs OPTIONAL

}

UERadioPagingInformation-v1900-IEs ::= SEQUENCE {

ue-RadioPagingInfo-r19 OCTET STRING (CONTAINING UE-RadioPagingInfo-r19) OPTIONAL,

nonCriticalExtension SEQUENCE {} OPTIONAL

}

-- TAG-UE-RADIO-PAGING-INFORMATION-STOP

-- ASN1STOP

| *UERadioPagingInformation* field descriptions |
| --- |
| ***supportedBandListNRForPaging***  Indicates the UE supported NR frequency bands which are derived by the gNB from *UE-NR-Capability*. |
| ***dl-SchedulingOffset-PDSCH-TypeA-FDD-FR1***  Indicates whether the UE supports DL scheduling slot offset (K0) greater than 0 for PDSCH mapping type A in FDD FR1. |
| ***dl-SchedulingOffset-PDSCH-TypeA-FDD-FR2-NTN***  Indicates whether the UE supports DL scheduling slot offset (K0) greater than 0 for PDSCH mapping type A in FDD FR2-NTN. |
| ***dl-SchedulingOffset-PDSCH-TypeA-TDD-FR1***  Indicates whether the UE supports DL scheduling slot offset (K0) greater than 0 for PDSCH mapping type A in TDD FR1. |
| ***dl-SchedulingOffset-PDSCH-TypeA-TDD-FR2***  Indicates whether the UE supports DL scheduling slot offset (K0) greater than 0 for PDSCH mapping type A in TDD FR2. |
| ***dl-SchedulingOffset-PDSCH-TypeB-FDD-FR1***  Indicates whether the UE supports DL scheduling slot offset (K0) greater than 0 for PDSCH mapping type B in FDD FR1. |
| ***dl-SchedulingOffset-PDSCH-TypeB-FDD-FR2-NTN***  Indicates whether the UE supports DL scheduling slot offset (K0) greater than 0 for PDSCH mapping type B in FDD FR2-NTN. |
| ***dl-SchedulingOffset-PDSCH-TypeB-TDD-FR1***  Indicates whether the UE supports DL scheduling slot offset (K0) greater than 0 for PDSCH mapping type B in TDD FR1. |
| ***dl-SchedulingOffset-PDSCH-TypeB-TDD-FR2***  Indicates whether the UE supports DL scheduling slot offset (K0) greater than 0 for PDSCH mapping type B in TDD FR2. |
| ***halfDuplexFDD-TypeA-RedCap***  Indicates whether the (e)RedCap UE only supports half-duplex operation for FDD in the indicated band(s). |
| ***inactiveStatePO-Determination***  Indicates whether the UE supports to use the same i\_s to determine PO in RRC\_INACTIVE state as in RRC\_IDLE state. |
| ***numberOfRxERedCap***  Indicates the number of Rx branches supported by an eRedCap UE. |
| ***numberOfRxRedCap***  Indicates the number of Rx branches supported by a RedCap UE. |
| ***supportOf2RxXR***  Indicates whether the UE is a 2Rx XR UE. |
| ***ue-RadioPagingInfo***  The field is used to transfer UE capability information used for paging. The gNB generates the ue-RadioPagingInfo-r17 and the contained UE capability information is absent when not supported by the UE. The content of *ue-RadioPagingInfo-r19* is generated by the UE. |

#### – *UERadioAccessCapabilityInformation*

This message is used to transfer UE radio access capability information, covering both upload to and download from the 5GC.

Direction: ng-eNB or gNB to/ from 5GC

*UERadioAccessCapabilityInformation* message

-- ASN1START

-- TAG-UE-RADIO-ACCESS-CAPABILITY-INFORMATION-START

UERadioAccessCapabilityInformation ::= SEQUENCE {

criticalExtensions CHOICE {

c1 CHOICE{

ueRadioAccessCapabilityInformation UERadioAccessCapabilityInformation-IEs,

spare7 NULL,

spare6 NULL, spare5 NULL, spare4 NULL,

spare3 NULL, spare2 NULL, spare1 NULL

},

criticalExtensionsFuture SEQUENCE {}

}

}

UERadioAccessCapabilityInformation-IEs ::= SEQUENCE {

ue-RadioAccessCapabilityInfo OCTET STRING (CONTAINING UE-CapabilityRAT-ContainerList),

nonCriticalExtension SEQUENCE {} OPTIONAL

}

-- TAG-UE-RADIO-ACCESS-CAPABILITY-INFORMATION-STOP

-- ASN1STOP

|  |
| --- |
| *UERadioAccessCapabilityInformation-IEs* field descriptions |
| ***ue-RadioAccessCapabilityInfo***  Including NR, MR-DC, E-UTRA radio access capabilities. A gNB that retrieves MRDC related capability containers ensures that the set of included MRDC containers is consistent w.r.t. the feature set related information. |

END OF CHANGE