3GPP TSG-RAN WG2 Meeting #116-e draftR2-2111396

**Electronic Meeting, Nov 1st - 12th 2021**

**Source: Document Rapporteur (Ericsson)**

**Title: RAN2 agreements for Rel-17 NB-IoT and LTE-MTC**

**Agenda Item: 9.1.1**

**Document for: Endorsement**

# 1 Introduction

This document lists RAN2 agreements made for Rel-17 “Additional enhancements for NB-IoT and LTE-M” work item (WI code NB\_IOTenh4\_LTE\_eMTC6; WID in [RP-201306](http://3gpp.org/ftp/tsg_ran/TSG_RAN/TSGR_88e/Docs/RP-201306.zip)), until and including the RAN2#116-e, November 1st – 12th 2021.

NOTE: Email agreements for CRs/specific topics are not listed in this document.

# 2 Additional enhancements for NB-IoT and LTE-MTC

## 2.1 Organizational

|  |
| --- |
| RAN2#111-e agreements:   * Will maintain a document similar to the one used in R16 for capturing agreements. * The endorsed report can be provided in R2-2008309. * [Post111-e][350][NBIOT/eMTC R17] Capture the agreements (Ericsson)   + - Scope: Capture the agreements.     - Intended outcome: endorsed report in R2-2008309     - Deadline: Friday, 2020-09-04 13:00 UTC   RAN2#112-e agreements: None (except for this document, see clause 5)  RAN2#113-e agreements: None (except for this document, see clause 5)  RAN2#113bis-e agreements: None (except for this document, see clause 5)  RAN2#114-e agreements: None (except for this document, see clause 5)  RAN2#115-e agreements: None (except for this document, see clause 5)  RAN2#116-e agreements: None (except for this document, see clause 5) |

## 2.2 NB-IoT neighbour cell measurements and corresponding measurement triggering before RLF

|  |
| --- |
| RAN2#111-e agreements:   * Study current RLF procedure to understand the time taken to select the cell for access. Start and end points FFS. * Support neighbour cell measurements in RRC\_CONNECTED, at least for intra-frequency.   + - FFS inter-frequency     - FFS whether measurements are done on the anchor carrier     - FFS how neighbour cell measurement is triggered     - FFS how to perform neighbour cell measurements * Working assumption: Neighbour cell measurement results are not reported to the network in RRC\_CONNECTED.   + - FFS whether and when other information can be sent   RAN2#112-e agreements:   * Enhancements to the random-access procedure are not considered. * The solution includes reduction of the time between declaration of RLF and the start of the random-access procedure (points C and D) * FFS whether the solution includes reduction of the time between out-of-sync detection and declaration of RLF (points B and C)   RAN2#113-e agreements:   * Neighbour cells measurement (detection and measurements) are performed only on the anchor carrier. * The solution is optional   [R2-2102165](http://ftp.3gpp.org/tsg_ran/WG2_RL2/TSGR2_113-e/Docs/R2-2102165.zip) LS on neighbour cell measurement in NB-IoT RRC\_CONNECTED state LS out Rel-17 To: RAN4. NB\_IOTenh4\_LTE\_eMTC6-Core  RAN2#113bis-e agreements: None  RAN2#114-e agreements:   * The criteria to start measurements is based on a combination of serving cell quality threshold (option b) and variance of the serving cell quality (option c) * Configuration of the criteria to start the measurements is supported.   + - FFS whether any further information needs to be provided by NW * FFS whether any assistance information from UE is needed. * FFS if/how to support ‘early’ RLF.   RAN2#115-e agreements:   * The configuration of the criteria for starting the measurements include a serving cell NRSRP threshold. FFS how to address variance (as agreed last meeting) * It is useful to have a shorter T310 timer for UEs supporting this enhancement, but FFS whether this is best achieved with the existing dedicated signalling or based on a new condition * Prioritisation of carriers/cells to measure is left to the UE implementation. * FFS: whether to provide a separate criteria for inter-frequency measurements (i.e., needing re-tuning) considering that they will take longer and should start earlier. * Legacy relaxed monitoring criteria is reused to address the variance part of the criteria to start the measurements.   + - FFS: Whether it is enabled by the provision of separate SSearchDeltaP and TSearchDeltaP parameters from RRC\_IDLE. * The conditions where the UE is required to perform measurements are specified. No requirement on when to stop measurements is needed. * The configuration of the criteria for starting the measurements is provided via broadcast signalling. * Provision of information regarding which cells/carriers to be considered is not supported. It is up to UE implementation to choose and prioritize carrier/cell list for measurement. * Report of the cells measured in RRC\_IDLE to assist measurement configuration is not supported. * Report of information about connected measurements during the RRC Connection re-establishment procedure for network optimisation is not supported. * There is no need to specify which subframes can be used for measurements beyond them not being needed for PDCCH monitoring or data transmission / reception. * Support for connected mode measurement is optional with capability signalling. * FFS: Whether to support an indication from the UE that it starts/ stops performing measurement   RAN2#116-e agreements:   * NW signals two separate thresholds for intra- and inter-frequency measurements. * The values of s-SearchDeltaP and TSearchDeltaP may be different in RRC\_CONNECTED and RRC\_IDLE, they are signalled in a separate set of parameters. * s-SearchDeltaP has the same value range as the existing RRC\_IDLE parameter * [FFS] An indication that the UE starts measurement is not introduced. * No enhancement is introduced to have a shorter T310 timer for mobile UEs supporting connected mode measurement. * For RRC\_CONNECTED state, TSearchDeltaP is configured via SIB. * Working assumption: For RRC\_CONNECTED state, TSearchDeltaP range is 10 – 60 seconds. * For RRC\_CONNECTED state, no default value for TSearchDeltaP. * No limit for how long UE can remain in relaxed neighbour cell monitoring state whilst it is in RRC\_CONNECTED state. * For RRC\_CONNECTED state, the RRC\_IDLE state SSearchDeltaP is not used if the RRC\_CONNECTED state SSearchDeltaP is not provided. * Relaxed neighbour cell monitoring is enabled in RRC\_CONNECTED state if TSearchDeltaP and SSearchDeltaP for RRC\_CONNECTED state are provided. |

## 2.3 NB-IoT carrier selection based on the coverage level, and associated carrier specific configuration

|  |
| --- |
| RAN2#111-e agreements:   * Paging carrier selection Improvements based on CE level is considered * Paging carrier selection Improvements based on DRX cycle may be considered   + - whether DRX cycle is considered as part of CE level (Rmax) or can be also considered separately * Enhancements for NPRACH Carrier selection carrier may be considered * Paging carrier selection Improvements solely based on WUS or GWUS is not considered * FFS service based   RAN2#112-e agreements: None  RAN2#113-e agreements:   * Select between one of the options:   + - Option 1: UE selects a paging carrier based on a rule configured by the network     - Option 2: NW configures a specific paging carrier * Working assumption: For both options, when coverage changes, mechanism that requires UE to report the update of coverage is not introduced.   RAN2#113bis-e agreements: None  RAN2#114-e agreements:   * Rel-17 paging carriers and the legacy paging carriers should be exclusive. * RAN2 assumes S1AP/NGAP update is not needed. * Carrier selection criteria does not include power boosting or service * FFS: For option 1, whether DRX can be part of the carrier selection criteria * Rel-17 paging carrier configuration is provided in broadcast signalling. * Select between the following sub-options:   + - Option 1c: Network enables UE to select a Rel-17 paging carrier by providing the coverage information (CEL/Rmax) for the carrier selection to the UE in dedicated signalling     - Option 2a: NW indicates the carrier to use explicitly via dedicated signalling based on information determined within the NW.     - FFS for both options whether there is a report from the UE to suggest a carrier or provide a metric report * Working assumption: UE metric for determining carrier suitability and selection is based on measured NRSRP. FFS whether to use a hysteresis/longer averaging/timer * For option 1, upon cell change, FFS:   + - Alt 1: based on previously determined CEL and broadcasted paging carrier configuration in the new cell.     - Alt 2: UE needs to perform fallback mechanism. * For option 2, upon cell change, UE needs to perform fallback mechanism. * Whenever the R17 coverage-based carrier criteria is met, UE uses the R17 coverage based carrier, otherwise UE should use the fallback mechanism * For both options, fall back carrier is legacy paging carrier based on UE\_ID   RAN2#115-e agreements:   * Support coverage or carrier specific DRX configurations, FFS details. * UE capability for Rel-17 paging carrier selection should be introduced * UE metric for determining carrier suitability and selection is based on NRSRP. * Use a hysteresis/longer averaging/timer for UE metric based on NRSRP. * FFS whether to introduce new UE report and/or whether to mandate support of existing Msg5 reporting.   RAN2#116-e agreements:   * DRX is not used a criterion that needs to be explicitly considered for paging carrier selection. * Option 1c with Alt2 (fallback when cell change) is supported |

## 2.4 Other

### NB-IoT 16-QAM for unicast in UL and DL

|  |
| --- |
| RAN2#113bis-e agreements:   * Working assumption: For the UE supporting 16-QAM, the L2 buffer size is 12000 bytes. * Working assumption: Support of 16-QAM has separate UE capabilities for DL and UL   RAN2#114-e agreements: None  RAN2#115-e agreements:   * Confirm the working assumption: The support of 16-QAM uses separate UE capabilities for DL and UL. * 16QAM is configured via dedicated signaling separately for UL and DL. * A NPUSCH 16QAM activation indication is needed in PUR configuration.   RAN2#116-e agreements:   * Confirm the working assumption of 12000 bytes for DL 16QAM for NB-IoT |

### LTE-MTC 14 HARQ processes in DL for HD-FDD Cat M1 UEs

|  |
| --- |
| RAN2#113bis-e agreements:   * 14 HARQ activation is configured by dedicated RRC signalling. * Working assumption: No change to current L2 buffer size requirement   RAN2#114-e agreements: None  RAN2#115-e agreements:   * Confirm the working assumption: No change to current L2 buffer size requirement for HD-FDD Cat M1 UEs supporting 14 HARQ processes in DL. |

### LTE-MTC Max DL TBS of 1736 bits for HD-FDD Cat. M1 UEs in CE mode A only

|  |
| --- |
| RAN2#113bis-e agreements:   * DL TBS of 1736 bits is configured by dedicated RRC signalling. * FFS: Whether to update L2 buffer size requirement   RAN2#114-e agreements: None  RAN2#115-e agreements:   * The table 4.1A-1 in TS 36.306 for DL Category M1 needs to be updated to indicate 1736 bits TBS and 43008 soft channel bits. * Max DL TBS of 1736 bits can be supported for PUR. * FFS EDT support.   RAN2#116-e agreements:   * No change to existing L2 buffer requirements for supporting 1736bits TBS for eMTC. |

# 3 References: List of approved outgoing Rel-17 LSs

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Tdoc** | **Meeting** | **Title** | **WI** | **To** | **Cc** |
| R2-2102165 | RAN2#113-e | LS on neighbour cell measurement in NB-IoT RRC\_CONNECTED state | NB\_IOTenh4\_LTE\_eMTC6-Core | RAN4 |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |

# 4 References: Reports from the breakout session

|  |  |  |  |
| --- | --- | --- | --- |
| **Meeting** | **Date** | **Title** | **Tdoc** |
| RAN2#111-e, Online | 17-28 August 2020 | Report NB-IoT breakout session | R2-2008127 |
| RAN2#112-e, Online | 2-13 November 2020 | Report NB-IoT breakout session | R2-2010707 |
| RAN2#113-e, Online | Jan 25 - Feb 5 2021 | Report NB-IoT breakout session | R2-2101957 |
| RAN2#113bis-e, Online | 12 - 20 April 2021 | Report NB-IoT breakout session | R2-2104307 |
| RAN2#114-e, Online | 19 – 27 May 2021 | Report NB-IoT breakout session | R2-2106477 |
| RAN2#115-e, Online | 9 - 27 August 2021 | Report NB-IoT breakout session | R2-2108837 |
| RAN2#116-e, Online | 1 – 12 November 2021 | Report NB-IoT breakout session | R2-2111297 |

# 5 Change history

|  |  |  |
| --- | --- | --- |
| **Tdoc** | **Title** | **Comment** |
| R2-2008309 | RAN2 agreements for Rel-17 additional enhancements for NB-IoT & LTE-MTC | Post RAN2#111-e |
| R2-2010911 | RAN2 agreements for Rel-17 additional enhancements for NB-IoT & LTE-MTC | Post RAN2#112-e |
| R2-2102164 | RAN2 agreements for Rel-17 additional enhancements for NB-IoT & LTE-MTC | Post RAN2#113-e |
| R2-2104451 | RAN2 agreements for Rel-17 additional enhancements for NB-IoT & LTE-MTC | Post RAN2#113bis-e |
| R2-2106602 | RAN2 agreements for Rel-17 additional enhancements for NB-IoT & LTE-MTC | Post RAN2#114-e |
| R2-2108974 | RAN2 agreements for Rel-17 additional enhancements for NB-IoT & LTE-MTC | Post RAN2#115-e |
| R2-2111396 | RAN2 agreements for Rel-17 additional enhancements for NB-IoT & LTE-MTC | Post RAN2#116-e |