**3GPP TSG-RAN WG2 Meeting #117-e *DRAFT* R2-2203699**

**Online, 21 Feb – 03 Mar, 2022**

|  |
| --- |
| *CR-Form-v12.1* |
| **CHANGE REQUEST** |
|  |
|  | **36.300** | **CR** | **1360** | **rev** | **-** | **Current version:** | **16.7.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network | **X** | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  | Introduction of new bands and bandwidth allocation for LTE-based 5G terrestrial broadcast |
|  |  |
| ***Source to WG:*** | Qualcomm Inc. |
| ***Source to TSG:*** | R2 |
|  |  |
| ***Work item code:*** | LTE\_terr\_bcast\_bands\_part1-Core |  | ***Date:*** | 2022-03-xx |
|  |  |  |  |  |
| ***Category:*** | B |  | ***Release:*** | Rel-17 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-15 (Release 15)Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)* |
|  |  |
| ***Reason for change:*** | RAN1 CRs for the WI were approved by RAN#94e in RP-212975. RAN2 CR for RRC configuration was agreed in R2-2203633.RAN1 sent LS to RAN2 in R2-2204128/R1-2202825 requesting updates to stage 2.This CR is to introduce the stage 2 description to the specification. |
|  |  |
| ***Summary of change:*** |  Following changes are introduced: 1. Introduce the stage 2 description as requested by RAN1.
 |
|  |  |
| ***Consequences if not approved:*** | New bands and bandwidth allocation for LTE-based 5G terrestrial broadcast cannot be supported. RAN2 specification remains incomplete and misaligned with RAN1 specifications. |
|  |  |
| ***Clauses affected:*** | 5.1.1 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** | **X** |  |  Other core specifications  | TS 36.306 CR 1836TS 36.331 CR 4780 |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

**First Change**

### 5.1.1 Basic transmission scheme based on OFDM

The downlink transmission scheme is based on conventional OFDM using a cyclic prefix. The OFDM sub-carrier spacing is *Δf* = 15 kHz. 12 consecutive sub-carriers during one slot correspond to one downlink *resource block*. In the frequency domain, the number of resource blocks, NRB, can range from NRB-min = 6 to NRB-max = 110 per CC or per Cell in case of CA or DC.

In addition, there are also four reduced sub-carrier spacings, *Δflow* = 7.5 kHz, *Δflow1* = 2.5 kHz, *Δflow2* = 1.25 kHz and *Δflow3* ≈ 0.37 kHz for both MBMS-dedicated cell and MBMS/Unicast-mixed cell.

In case of 15 kHz sub-carrier spacing there are two cyclic-prefix lengths, corresponding to seven and six OFDM symbols per slot respectively.

- Normal cyclic prefix: TCP = 160×Ts (OFDM symbol #0) , TCP = 144×Ts (OFDM symbol #1 to #6)

- Extended cyclic prefix: TCP-e = 512×Ts (OFDM symbol #0 to OFDM symbol #5)

where Ts = 1/ (2048 × Δf)

In case of 7.5 kHz sub-carrier spacing, there is only a single cyclic prefix length TCP-low = 1024×Ts, corresponding to 3 OFDM symbols per slot.

In case of 2.5 kHz sub-carrier spacing, there is only a single cyclic prefix length TCP-low1 = 3072×Ts, corresponding to 1 OFDM symbol per slot.

In case of 1.25 kHz sub-carrier spacing, there is only a single cyclic prefix length TCP-low2 = 6144×Ts, corresponding to 1 OFDM symbol per subframe.

In case of 0.37 kHz sub-carrier spacing, there is only a single cyclic prefix length TCP-low3 = 9216×Ts, corresponding to 1 OFDM symbol per 3 ms slot as defined in TS 36.211 [4], clause 4.1.

For MBMS-dedicated cells, the PMCH bandwidth can be indicated to be larger than the carrier bandwidth. In particular, a PMCH bandwidth of 30, 35 or 40 PRBs (corresponding to 6/ 7/ 8MHz) can be indicated when the carrier bandwidth is 15 or 25 PRBs (corresponding to 3/ 5 MHz).

In case of FDD, operation with half duplex from UE point of view is supported.

**End of Changes**