3GPP RAN WG2 Meeting #118-e R2-22xxxxx

eMeeting May 9th – 20th, 2022

Agenda Item: 6.10.3.1.1

Source: ZTE corporation,Sanechips

Title: Report of [POST118-e][111][NTN] 38.304 CR (ZTE)

Document for: Discussion, Decision

# Introduction

This document is intended address a subset of remaining idle mode open issues as per the following email discussion guidelines:

* [POST118-e][111][NTN] 38.304 CR (ZTE)

Scope: Update the 38.304 CR, reflecting the meeting agreements

Intended outcome: Agreeable 38.304 CR in R2-2206500

Deadline (for companies' feedback): **Thursday 2022-05-26 20:00 UTC**

Deadline (for final CR): Friday 2022-05-27 10:00 UTC

# Discussion

## Two options on capturing the cellBarredNTN

Two options have been provided on how to capture the usage of *cellBarredNTN* in 38.304:

### **Option 1**

Option 1-Start of change

5.3.1 Cell status and cell reservations

Cell status and cell reservations are indicated in the *MIB or SIB1* message as specified in TS 38.331 [3] by means of following fields:

- *cellBarred* (IE type: "barred" or "not barred")   
Indicated in *MIB* message. In case of multiple PLMNs or NPNs indicated in *SIB1*, this field is common for all PLMNs and NPNs.

- *cellBarred-NTN* (IE type: "barred" or "not barred")  
Indicated in SIB1 message. In case of multiple PLMNs or NPNs indicated in *SIB1*, this field is common for all PLMNs and NPNs. This field is only applicable to NTN-capable UEs.

- *cellBarredRedCap1Rx* (IE type: "barred" or "not barred")  
Indicated in *SIB1* message. In case of multiple PLMNs or NPNs indicated in *SIB1*, this field is common for all PLMNs and NPNs. This field is only applicable to RedCap UEs.

- *cellBarredRedCap2Rx* (IE type: "barred" or "not barred")  
Indicated in *SIB1* message. In case of multiple PLMNs or NPNs indicated in *SIB1*, this field is common for all PLMNs and NPNs. This field is only applicable to RedCap UEs.

- *cellReservedForOperatorUse* (IE type: "reserved" or "not reserved")   
Indicated in *SIB1* message*.* In case of multiple PLMNs or NPNs indicated in *SIB1*, this field is specified per PLMN or per SNPN.

- *cellReservedForOtherUse* (IE type: "true")   
Indicated in *SIB1* message. In case of multiple PLMNs indicated in *SIB1*, this field is common for all PLMNs.

*- cellReservedForFutureUse* (IE type: "true")   
Indicated in *SIB1* message. In case of multiple PLMNs or NPNs indicated in *SIB1*, this field is common for all PLMNs and NPNs.

NOTE 0: IAB-MT ignores the *cellBarred*, *cellReservedForOperatorUse, cellReservedForFutureUse,* and *intraFreqReselection* (i.e. treats *intraFreqReselection* as if it was set to *allowed*) as defined in TS 38.331 [3]. IAB-MT also ignores *cellReservedForOtherUse* for cell barring determination (i.e. NPN capable IAB-MT considers *cellReservedForOtherUse* for determination of an NPN-only cell) as defined in TS 38.331 [3].

- *iab-Support* (IE type: "true")  
Indicated in *SIB1* message. In case of multiple PLMNs or NPNs indicated in *SIB1*, this field is specified per PLMN or per SNPN.

Editor's note: Working assumption: A new bit, e.g. cellBarred-NTN, is introduced in SIB1 for NR-NTN. FFS on the expected UE behaviour upon reception of the new bit and the existing cellBarred.

When cell status is indicated as "not barred" and "not reserved" for operator use and not "true" for other use and not "true" for future use,

- UEs shall treat this cell as candidate during the cell selection and cell reselection procedures.

When cell broadcasts any CAG-IDs or NIDs and the cell status is indicated as "not barred" and "not reserved" for operator use and "true" for other use, and not "true" for future use:

- All NPN-capable UEs shall treat this cell as candidate during the cell selection and cell reselection procedures, other UEs shall treat this cell as if cell status is "barred".

When cell status is indicated as "true" for other use, and either cell does not broadcast any CAG-IDs or NIDs or does not broadcast any CAG-IDs and the UE is not operating in SNPN Access Mode,

- The UE shall treat this cell as if cell status is "barred".

When cell status is indicated as "true" for future use,

- The UE shall treat this cell as if cell status is "barred".

When cell status is indicated as "not barred" and "reserved" for operator use for any PLMN/SNPN and not "true" for other use and not "true" for future use,

- UEs assigned to Access Identity 11 or 15 operating in their HPLMN/EHPLMN shall treat this cell as candidate during the cell selection and reselection procedures if the field *cellReservedForOperatorUse* for that PLMN set to "reserved".

- UEs assigned to Access Identity 11 or 15 shall treat this cell as candidate during the cell selection and reselection procedures if the field *cellReservedForOperatorUse* for selected/registered SNPN is set to "reserved".

- UEs assigned to an Access Identity 0, 1, 2 and 12 to 14 shall behave as if the cell status is "barred" in case the cell is "reserved for operator use" for the registered PLMN/SNPN or the selected PLMN/SNPN.

- UEs assigned to Access Identity 3 shall behave as if the cell status is "barred" in case the cell is "reserved for operator use" for the registered PLMN or the selected PLMN.

NOTE 1: Access Identities 11, 15 are only valid for use in the HPLMN/ EHPLMN; Access Identities 12, 13, 14 are only valid for use in the home country as specified in TS 22.261 [12].

NOTE 1a: Access Identity 3 is only valid for PLMNs that indicate to potential Disaster Inbound Roamers that the UEs can access the PLMN as specified in TS 22.261 [12].

When cell status "barred" is indicated or to be treated as if the cell status is "barred",

- The UE is not permitted to select/reselect this cell for TN access, not even for emergency calls.

- The UE shall select another cell according to the following rule:

- If the cell is to be treated as if the cell status is "barred" due to being unable to acquire the *MIB*:

- the UE may exclude the barred cell as a candidate for cell selection/reselection for up to 300 seconds.

- the UE may select another cell on the same frequency if the selection criteria are fulfilled.

- else:

- If the UE is a RedCap UE, the UE shall acquire SIB1 and, in the remainder of this procedure, consider '*intraFreqReselection* in MIB' to be '*intraFreqReselectionRedCap* in SIB1', if available*.*

- If the field *intraFreqReselection* in *MIB* message is set to "allowed":

- the UE may select another cell on the same frequency if re-selection criteria are fulfilled;

- If the cell is to be treated as if the cell status is "barred" due to being unable to acquire the *SIB1*:

- the UE may exclude the barred cell as a candidate for cell selection/reselection for up to 300 seconds;

- else:

- the UE shall exclude the barred cell as a candidate for cell selection/reselection for 300 seconds.

- If the field *intraFreqReselection* in *MIB* message is set to "not allowed":

- If the cell is to be treated as if the cell status is "barred" due to being unable to acquire the *SIB1*:

- the UE may exclude the barred cell as a candidate for cell selection/reselection for up to 300 seconds;

- If the cell operates in licensed spectrum:

- the UE shall not re-select to another cell on the same frequency as the barred cell and exclude such cell(s) as candidate(s) for cell selection/reselection for 300 seconds;

- else:

- the UE may select to another cell on the same frequency if the reselection criteria are fulfilled.

- else:

- If the cell operates in licensed spectrum, or if this cell belongs to a PLMN which is indicated as being equivalent to the registered PLMN or the selected PLMN of the UE, or if this cell belongs to the registered SNPN or the selected SNPN of the UE:

- the UE shall not re-select to another cell on the same frequency as the barred cell and exclude such cell(s) as candidate(s) for cell selection/reselection for 300 seconds;

- else:

- the UE may select to another cell on the same frequency if the reselection criteria are fulfilled.

- the UE shall exclude the barred cell as a candidate for cell selection/reselection for 300 seconds.

When cell status "barred" is indicated for RedCap UEs with 1Rx/2Rx or to be treated as if the cell status is "barred",

- The UE is not permitted to select/reselect this cell, not even for emergency calls.

- The UE shall select another cell according to the following rule:

- If the cell is to be treated as if the cell status is "barred" due to not supporting RedCap UEs:

- the UE may exclude the barred cell as a candidate for cell selection/reselection for up to 300 seconds.

- the UE may select another cell on the same frequency if the selection criteria are fulfilled.

- else:

- If the field *intraFreqReselectionRedCap* in *SIB1* message is set to "allowed":

- the UE shall exclude the barred cell as a candidate for cell selection/reselection for 300 seconds.

- the UE may select another cell on the same frequency if re-selection criteria are fulfilled.

- If the field *intraFreqReselectionRedCap* in *SIB1* message is set to "not allowed":

- If the cell operates in licensed spectrum, or if this cell belongs to a PLMN which is indicated as being equivalent to the registered PLMN or the selected PLMN of the UE, or if this cell belongs to the registered SNPN or the selected SNPN of the UE:

- the UE shall not re-select to another cell on the same frequency as the barred cell and exclude such cell(s) as candidate(s) for cell selection/reselection for 300 seconds.

- else:

- the UE may select to another cell on the same frequency if the reselection criteria are fulfilled.

- the UE shall exclude the barred cell as a candidate for cell selection/reselection for 300 seconds.

When *cellBarredNTN* is indicated as “barred” for NTN UEs,

- The NTN UE is not permitted to select/reselect this cell for NTN access, not even for emergency calls.

- The NTN UE shall select another cell for NTN access according to the following rule:

- If the field *intraFreqReselection* in *MIB* message is set to "allowed":

- the UE may select another cell on the same frequency if re-selection criteria are fulfilled;

- the UE shall exclude the barred cell as a candidate for cell selection/reselection for 300 seconds.

- If the field *intraFreqReselection* in *MIB* message is set to "not allowed":

- If the cell operates in licensed spectrum, or if this cell belongs to a PLMN which is indicated as being equivalent to the registered PLMN or the selected PLMN of the UE, or if this cell belongs to the registered SNPN or the selected SNPN of the UE:

- the UE shall not re-select to another cell on the same frequency as the barred cell and exclude such cell(s) as candidate(s) for cell selection/reselection for 300 seconds;

- else:

- the UE may select to another cell on the same frequency if the reselection criteria are fulfilled.

- the UE shall exclude the barred cell as a candidate for cell selection/reselection for 300 seconds.

When *cellBarredNTN* is not broadcast for NTN UEs,

- The NTN UE is not permitted to select/reselect this cell for NTN access, not even for emergency calls.

- The NTN UE shall select another cell for NTN access according to the following rule:

- If the field *intraFreqReselection* in *MIB* message is set to "allowed":

- the UE may select another cell on the same frequency if re-selection criteria are fulfilled;

- If the field *intraFreqReselection* in *MIB* message is set to "not allowed":

- If the cell operates in licensed spectrum, or if this cell belongs to a PLMN which is indicated as being equivalent to the registered PLMN or the selected PLMN of the UE, or if this cell belongs to the registered SNPN or the selected SNPN of the UE:

- the UE shall not re-select to another cell on the same frequency as the barred cell;

- else:

- the UE may select to another cell on the same frequency if the reselection criteria are fulfilled.

The cell selection of another cell may also include a change of RAT.

NOTE 2: If barring of a cell is triggered by the condition of *trackingAreaCode* and *trackingAreaList* not being provided, as specified in TS 38.331 [3], the barring only applies to this PLMN and the UE can re-evaluate the barring condition again due to selection of another PLMN.

Option 1-End of change

### **Option 2**

Option 2-Start of change

5.3.1 Cell status and cell reservations

Cell status and cell reservations are indicated in the *MIB or SIB1* message as specified in TS 38.331 [3] by means of following fields:

- *cellBarred* (IE type: "barred" or "not barred")   
Indicated in *MIB* message. In case of multiple PLMNs or NPNs indicated in *SIB1*, this field is common for all PLMNs and NPNs.

- *cellBarred-NTN* (IE type: "barred" or "not barred")  
Indicated in SIB1 message. In case of multiple PLMNs or NPNs indicated in *SIB1*, this field is common for all PLMNs and NPNs. This field is only applicable to NTN-capable UEs.

- *cellBarredRedCap1Rx* (IE type: "barred" or "not barred")  
Indicated in *SIB1* message. In case of multiple PLMNs or NPNs indicated in *SIB1*, this field is common for all PLMNs and NPNs. This field is only applicable to RedCap UEs.

- *cellBarredRedCap2Rx* (IE type: "barred" or "not barred")  
Indicated in *SIB1* message. In case of multiple PLMNs or NPNs indicated in *SIB1*, this field is common for all PLMNs and NPNs. This field is only applicable to RedCap UEs.

- *cellReservedForOperatorUse* (IE type: "reserved" or "not reserved")   
Indicated in *SIB1* message*.* In case of multiple PLMNs or NPNs indicated in *SIB1*, this field is specified per PLMN or per SNPN.

- *cellReservedForOtherUse* (IE type: "true")   
Indicated in *SIB1* message. In case of multiple PLMNs indicated in *SIB1*, this field is common for all PLMNs.

*- cellReservedForFutureUse* (IE type: "true")   
Indicated in *SIB1* message. In case of multiple PLMNs or NPNs indicated in *SIB1*, this field is common for all PLMNs and NPNs.

NOTE 0: IAB-MT ignores the *cellBarred*, *cellReservedForOperatorUse, cellReservedForFutureUse,* and *intraFreqReselection* (i.e. treats *intraFreqReselection* as if it was set to *allowed*) as defined in TS 38.331 [3]. IAB-MT also ignores *cellReservedForOtherUse* for cell barring determination (i.e. NPN capable IAB-MT considers *cellReservedForOtherUse* for determination of an NPN-only cell) as defined in TS 38.331 [3].

- *iab-Support* (IE type: "true")  
Indicated in *SIB1* message. In case of multiple PLMNs or NPNs indicated in *SIB1*, this field is specified per PLMN or per SNPN.

Editor's note: Working assumption: A new bit, e.g. cellBarred-NTN, is introduced in SIB1 for NR-NTN. FFS on the expected UE behaviour upon reception of the new bit and the existing cellBarred.

When cell status is indicated as "not barred" and "not reserved" for operator use and not "true" for other use and not "true" for future use,

- UEs shall treat this cell as candidate during the cell selection and cell reselection procedures.

When cell broadcasts any CAG-IDs or NIDs and the cell status is indicated as "not barred" and "not reserved" for operator use and "true" for other use, and not "true" for future use:

- All NPN-capable UEs shall treat this cell as candidate during the cell selection and cell reselection procedures, other UEs shall treat this cell as if cell status is "barred".

When cell status is indicated as "true" for other use, and either cell does not broadcast any CAG-IDs or NIDs or does not broadcast any CAG-IDs and the UE is not operating in SNPN Access Mode,

- The UE shall treat this cell as if cell status is "barred".

When cell status is indicated as "true" for future use,

- The UE shall treat this cell as if cell status is "barred".

When cell status is indicated as "not barred" and "reserved" for operator use for any PLMN/SNPN and not "true" for other use and not "true" for future use,

- UEs assigned to Access Identity 11 or 15 operating in their HPLMN/EHPLMN shall treat this cell as candidate during the cell selection and reselection procedures if the field *cellReservedForOperatorUse* for that PLMN set to "reserved".

- UEs assigned to Access Identity 11 or 15 shall treat this cell as candidate during the cell selection and reselection procedures if the field *cellReservedForOperatorUse* for selected/registered SNPN is set to "reserved".

- UEs assigned to an Access Identity 0, 1, 2 and 12 to 14 shall behave as if the cell status is "barred" in case the cell is "reserved for operator use" for the registered PLMN/SNPN or the selected PLMN/SNPN.

- UEs assigned to Access Identity 3 shall behave as if the cell status is "barred" in case the cell is "reserved for operator use" for the registered PLMN or the selected PLMN.

NOTE 1: Access Identities 11, 15 are only valid for use in the HPLMN/ EHPLMN; Access Identities 12, 13, 14 are only valid for use in the home country as specified in TS 22.261 [12].

NOTE 1a: Access Identity 3 is only valid for PLMNs that indicate to potential Disaster Inbound Roamers that the UEs can access the PLMN as specified in TS 22.261 [12].

When cell status "barred" is indicated or to be treated as if the cell status is "barred",

- The UE is not permitted to select/reselect this cell, not even for emergency calls.

- The UE shall select another cell according to the following rule:

- If the cell is to be treated as if the cell status is "barred" due to being unable to acquire the *MIB*:

- the UE may exclude the barred cell as a candidate for cell selection/reselection for up to 300 seconds.

- the UE may select another cell on the same frequency if the selection criteria are fulfilled.

- else:

- If the UE is a RedCap UE, the UE shall acquire SIB1 and, in the remainder of this procedure, consider '*intraFreqReselection* in MIB' to be '*intraFreqReselectionRedCap* in SIB1', if available*.*

- If the field *intraFreqReselection* in *MIB* message is set to "allowed":

- the UE may select another cell on the same frequency if re-selection criteria are fulfilled;

- If the cell is to be treated as if the cell status is "barred" due to being unable to acquire the *SIB1*:

- the UE may exclude the barred cell as a candidate for cell selection/reselection for up to 300 seconds;

- else:

- the UE shall exclude the barred cell as a candidate for cell selection/reselection for 300 seconds.

- If the field *intraFreqReselection* in *MIB* message is set to "not allowed":

- If the cell is to be treated as if the cell status is "barred" due to being unable to acquire the *SIB1*:

- the UE may exclude the barred cell as a candidate for cell selection/reselection for up to 300 seconds;

- If the cell operates in licensed spectrum:

- the UE shall not re-select to another cell on the same frequency as the barred cell and exclude such cell(s) as candidate(s) for cell selection/reselection for 300 seconds;

- else:

- the UE may select to another cell on the same frequency if the reselection criteria are fulfilled.

- else:

- If the cell operates in licensed spectrum, or if this cell belongs to a PLMN which is indicated as being equivalent to the registered PLMN or the selected PLMN of the UE, or if this cell belongs to the registered SNPN or the selected SNPN of the UE:

- the UE shall not re-select to another cell on the same frequency as the barred cell and exclude such cell(s) as candidate(s) for cell selection/reselection for 300 seconds;

- else:

- the UE may select to another cell on the same frequency if the reselection criteria are fulfilled.

- the UE shall exclude the barred cell as a candidate for cell selection/reselection for 300 seconds.

When cell status "barred" is indicated for RedCap UEs with 1Rx/2Rx or to be treated as if the cell status is "barred",

- The UE is not permitted to select/reselect this cell, not even for emergency calls.

- The UE shall select another cell according to the following rule:

- If the cell is to be treated as if the cell status is "barred" due to not supporting RedCap UEs:

- the UE may exclude the barred cell as a candidate for cell selection/reselection for up to 300 seconds.

- the UE may select another cell on the same frequency if the selection criteria are fulfilled.

- else:

- If the field *intraFreqReselectionRedCap* in *SIB1* message is set to "allowed":

- the UE shall exclude the barred cell as a candidate for cell selection/reselection for 300 seconds.

- the UE may select another cell on the same frequency if re-selection criteria are fulfilled.

- If the field *intraFreqReselectionRedCap* in *SIB1* message is set to "not allowed":

- If the cell operates in licensed spectrum, or if this cell belongs to a PLMN which is indicated as being equivalent to the registered PLMN or the selected PLMN of the UE, or if this cell belongs to the registered SNPN or the selected SNPN of the UE:

- the UE shall not re-select to another cell on the same frequency as the barred cell and exclude such cell(s) as candidate(s) for cell selection/reselection for 300 seconds.

- else:

- the UE may select to another cell on the same frequency if the reselection criteria are fulfilled.

- the UE shall exclude the barred cell as a candidate for cell selection/reselection for 300 seconds.

The cell selection of another cell may also include a change of RAT.

NOTE 2: If barring of a cell is triggered by the condition of *trackingAreaCode* and *trackingAreaList* not being provided, as specified in TS 38.331 [3], the barring only applies to this PLMN and the UE can re-evaluate the barring condition again due to selection of another PLMN.

Option 2-End of change

**Question 1) On how to capture the usage of cellBarredNTN, which option do companies prefer? Option 1/2/other?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Option 1/2/other** | **Comments** |
| Samsung | Option 1 with comment | We prefer Option 1 that it would be better to specify cell barring procedure for NTN UE separately, similar to redcap UE.  However, “*This field is only applicable to NTN-capable UEs.*” => We think it should be changed into “This field is only applicable for NTN access” since NTN-capable UEs can access either TN access or NTN access, for TN access, NTN UE follows cellBarred, and only for NTN access, NTN UE follows cellBarredNTN. |
| Qualcomm | Option 2 with comments | See above, it says “When cell status "barred" is indicated or to be treated as if the cell status is "barred",  This should be true whether be it for cellBarred or cellBarredNTN. So additional text specific to NTN in option 1 is not necessary.  However, following part of the option 1 is ok. It helps a lot to clarify.  When *cellBarredNTN* is not broadcast in the cell,  - The NTN UE is not permitted to select/reselect this cell for NTN access, not even for emergency calls.  - The NTN UE shall select another cell for NTN access: |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

**For option 1, it has been raised during [AT118-e][111][NTN] Idle mode (ZTE) - 38.304 CR discussion that we need to consider whether to introduce *intraFreqReselectionNTN* in SIB1 for NTN UEs as we did for RedCap UEs and follow the similar handling.**

**If we introduce this new bit, the text would be updated as follows:**

When *cellBarredNTN* is indicated as “barred” for NTN UEs,

- The NTN UE is not permitted to select/reselect this cell for NTN access, not even for emergency calls.

- The NTN UE shall select another cell for NTN access according to the following rule:

- If the field *intraFreqReselectionNTN* in *SIB1* message is set to "allowed":

- the UE may select another cell on the same frequency if re-selection criteria are fulfilled;

- the UE shall exclude the barred cell as a candidate for cell selection/reselection for 300 seconds.

- If the field *intraFreqReselectionNTN* in *SIB1* message is set to "not allowed":

- If the cell operates in licensed spectrum, or if this cell belongs to a PLMN which is indicated as being equivalent to the registered PLMN or the selected PLMN of the UE, or if this cell belongs to the registered SNPN or the selected SNPN of the UE:

- the UE shall not re-select to another cell on the same frequency as the barred cell and exclude such cell(s) as candidate(s) for cell selection/reselection for 300 seconds;

- else:

- the UE may select to another cell on the same frequency if the reselection criteria are fulfilled.

- the UE shall exclude the barred cell as a candidate for cell selection/reselection for 300 seconds.

When *cellBarredNTN* is not broadcast for NTN UEs,

- The NTN UE is not permitted to select/reselect this cell for NTN access, not even for emergency calls.

- The NTN UE shall select another cell for NTN access according to the following rule:

- If the field *intraFreqReselectionNTN* in *SIB1* message is set to "allowed":

- the UE may select another cell on the same frequency if re-selection criteria are fulfilled;

- If the field *intraFreqReselectionNTN* in *SIB1* message is set to "not allowed":

- If the cell operates in licensed spectrum, or if this cell belongs to a PLMN which is indicated as being equivalent to the registered PLMN or the selected PLMN of the UE, or if this cell belongs to the registered SNPN or the selected SNPN of the UE:

- the UE shall not re-select to another cell on the same frequency as the barred cell;

- else:

- the UE may select to another cell on the same frequency if the reselection criteria are fulfilled.

**Question 2.1) For option 1, do companies support to introduce *intraFreqReselectionNTN* in SIB1 for NTN UEs, and NTN UE intended for NTN access would follow such indication in cell reselection？**

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes/No** | **Comments** |
| Samsung | Yes | We support introducing intraFreqReselectionNTN in SIB1 for NTN UEs, similar as intraFreqReselectionRedCap introduced for Redcap UEs, so that a complete independent cell barring procedure can be specified for NTN UEs. |
| Qualcomm | Yes | When legacy or TN UEs comes to select this cell (frequency can be overlapped or adjacent to the TN) and sees cell barred in TN, they should follow the intraFreqReselection in MIB. However, network may need to set intraFreqReselection differently for NTN access. |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

**Question 2.2) If the answer to Q2.1 is “Yes”, do companies agree with the changes above on introduction of the *intraFreqReselectionNTN* in SIB1?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes/No** | **Comments** |
| Samsung | Yes with comments | We support introducing intraFreqReselectionNTN in SIB1.  However, we think there is no different UE behavior required for two cases (cellBarredNTN is indicated as “barred” and cellBarredNTN is not broadcast so it is implicitly considered as barred), so it would be good to combine two cases into a same graph.”. Note in the current draft, it seems “the UE shall exclude the barred cell as a candidate for cell selection/reselection for 300 seconds.” is only applied to the case (cellBarredNTN is indicated as “barred”), but it not applied to the case (cellBarredNTN is not broadcast so it is implicitly considered as barred”, we don’t understand why there should be difference. |
| Qualcomm | No | For redcap UE, following is specified. We can do the same for NTN.  - If the UE is a RedCap UE, the UE shall acquire SIB1 and, in the remainder of this procedure, consider '*intraFreqReselection* in MIB' to be '*intraFreqReselectionRedCap* in SIB1', if available*.* |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

# Conclusions

<To be generated based on company input>

# References

1. R2-22xxxxx\_NTN corrections to 38.304\_v08\_Rapporteur