**3GPP TSG-RAN2 Meeting #118-e *R2-2206706***

**Electronic meeting, 9th - 20th May, 2022**

|  |
| --- |
| *CR-Form-v12.2* |
| **CHANGE REQUEST** |
|  |
|  | **38.304** | **CR** | **0252** | **rev** | **1** | **Current version:** | **17.0.0** |  |
|  |
| *For* [***HELP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network | **X** | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  | Miscellaneous corrections for RedCap WI  |
|  |  |
| ***Source to WG:*** | Samsung |
| ***Source to TSG:*** | R2 |
|  |  |
| ***Work item code:*** | NR\_redcap-Core |  | ***Date:*** | 2022-05-20 |
|  |  |  |  |  |
| ***Category:*** | **F** |  | ***Release:*** | Rel-17 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)Rel-19 (Release 19)* |
|  |  |
| ***Reason for change:*** | 1. To address class 0 issues for RedCap WI
2. To apply result of [AT118-e][115][RedCap] 38.304 CR (Samsung) (Phase 2)
3. To apply an agreement in RAN2#118e: Agreed as: Adopt proposed TP2 in R2-2206213, on top of changes in R2-2206023
4. To update [TBD]
 |
|  |  |
| ***Summary of change:*** | 1. Class 0 issues are corrected.
2. Corrections on [AT118-e][115][RedCap] 38.304 CR (Samsung) (Phase 2) are updated.
3. Proposed TP2 in R2-2206213
4. Update [TBD] based on endorsed RAN4 CR (i.e., R4-2211038)
 |
|  |  |
| ***Consequences if not approved:*** | 1. Class 0 issues are not addressed.
2. Corrections on [AT118-e][115][RedCap] 38.304 CR (Samsung) (Phase 2) are not updated
3. Agreement in RAN2#118e is not included
4. The text [TBD] remains in specification
 |
|  |  |
| ***Clauses affected:*** | 5.2.4.9.0, 5.3.1, 7.1 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  |   |
| ***affected:*** |  |  |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  |  |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

##### 5.2.4.9.0 Relaxed measurement rules

When the UE is required to perform measurements of intra-frequency cells or NR inter-frequency cells or inter-RAT frequency cells according to the measurement rules in clause 5.2.4.2:

- if *lowMobilityEvaluation* is configured and *cellEdgeEvaluation* is not configured; and

- if the UE has performed normal intra-frequency, NR inter-frequency, or inter-RAT frequency measurements for at least TSearchDeltaP after (re-)selecting a new cell; and

- if the relaxed measurement criterion in clause 5.2.4.9.1 is fulfilled for a period of TSearchDeltaP:

- the UE may choose to perform relaxed measurements for intra-frequency cells according to relaxation methods in clauses 4.2.2.9 in TS 38.133 [8];

- if the serving cell fulfils Srxlev > SnonIntraSearchP and Squal > SnonIntraSearchQ:

- for any NR inter-frequency or inter-RAT frequency of higher priority, if less than 1 hour has passed since measurements of corresponding frequency cell(s) for cell reselection were last performed; and,

- if *highPriorityMeasRelax* is configured with value *true*:

- the UE may choose not to perform measurement on this frequency cell(s);

- else (i.e. the serving cell fulfils Srxlev ≤ SnonIntraSearchP or Squal ≤ SnonIntraSearchQ):

- the UE may choose to perform relaxed measurements for NR inter-frequency cells or inter-RAT frequency cells according to relaxation methods in clauses 4.2.2.10, and 4.2.2.11 in TS 38.133 [8];

- if *cellEdgeEvaluation* is configured and *lowMobilityEvaluation* is not configured; and

- if the relaxed measurement criterion in clause 5.2.4.9.2 is fulfilled:

- the UE may choose to perform relaxed measurements for intra-frequency cells according to relaxation methods in clauses 4.2.2.9 in TS 38.133 [8];

- if the serving cell fulfils Srxlev ≤ SnonIntraSearchP or Squal ≤ SnonIntraSearchQ:

- the UE may choose to perform relaxed measurements for NR inter-frequency cells or inter-RAT frequency cells according to relaxation methods in clauses 4.2.2.10, and 4.2.2.11 in TS 38.133 [8];

- if both *lowMobilityEvaluation* and *cellEdgeEvaluation* are configured:

- if the UE has performed normal intra-frequency, NR inter-frequency, or inter-RAT frequency measurements for at least TSearchDeltaP after (re-)selecting a new cell; and

- if the relaxed measurement criterion in clause 5.2.4.9.1 is fulfilled for a period of TSearchDeltaP; and

- if the relaxed measurement criterion in clause 5.2.4.9.2 is fulfilled:

- for any intra-frequency, NR inter-frequency, or inter-RAT frequency, if less than 1 hour has passed since measurements of corresponding frequency cell(s) for cell reselection were last performed:

- the UE may choose not to perform measurement for measurements on this frequency cell(s);

- else:

- if the UE has performed normal intra-frequency, NR inter-frequency, or inter-RAT frequency measurements for at least TSearchDeltaP after (re-)selecting a new cell, and the relaxed measurement criterion in clause 5.2.4.9.1 is fulfilled for a period of TSearchDeltaP; or,

- if the relaxed measurement criterion in clause 5.2.4.9.2 is fulfilled:

- if *combineRelaxedMeasCondition* is not configured:

- the UE may choose to perform relaxed measurements for intra-frequency cells, NR inter-frequency cells of equal or lower priority, or inter-RAT frequency cells of lower priority according to relaxation methods in clauses 4.2.2.9, 4.2.2.10, and 4.2.2.11 in TS 38.133 [8];

- if the serving cell fulfils Srxlev ≤ SnonIntraSearchP or Squal ≤ SnonIntraSearchQ:

- the UE may choose to perform relaxed measurement for NR inter-frequency cells of higher priority, or inter-RAT frequency cells of higher priority according to relaxation methods in clauses 4.2.2.10, and 4.2.2.11 in TS 38.133 [8];

- if the UE is a RedCap UE; and

- if *stationaryMobilityEvaluation* is configured and *cellEdgeEvaluationWhileStationary* is not configured; and

- if the UE has performed normal intra-frequency, NR inter-frequency, or inter-RAT frequency measurements for at least TSearchDeltaP-Stationary after (re-)selecting a new cell; and

- if the relaxed measurement criterion in clause 5.2.4.9.3 is fulfilled for a period of TSearchDeltaP-Stationary:

- the UE may choose to perform relaxed measurements for intra-frequency cells, NR inter-frequency cells, or inter-RAT frequency cells according to relaxation methods in clauses 4.2B.2.9, 4.2B.2.10, and 4.2B.2.11 in TS 38.133 [8];

- if both *stationaryMobilityEvaluation* and *cellEdgeEvaluationWhileStationary* are configured:

- if the UE has performed normal intra-frequency, NR inter-frequency, or inter-RAT frequency measurements for at least TSearchDeltaP-Stationary after (re-)selecting a new cell; and

- if the relaxed measurement criterion in clause 5.2.4.9.4 is fulfilled:

- the UE may choose to perform relaxed measurements for intra-frequency cells, NR inter-frequency cells, or inter-RAT frequency cells according to relaxation methods in clauses 4.2B.2.9, 4.2B.2.10, and 4.2B.2.11 in TS 38.133 [8];

- else:

- if *combineRelaxedMeasCondition2* is not configured:

- if the UE has performed normal intra-frequency, NR inter-frequency, or inter-RAT frequency measurements for at least TSearchDeltaP-Stationary after (re-)selecting a new cell; and

- if the relaxed measurement criterion in clause 5.2.4.9.3 is fulfilled for a period of TSearchDeltaP-Stationary:

- the UE may choose to perform relaxed measurements for intra-frequency cells, NR inter-frequency cells, or inter-RAT frequency cells according to relaxation methods in clauses 4.2B.2.9, 4.2B.2.10, and 4.2B.2.11 in TS 38.133 [8];

NOTE 1: It is up to UE implementation when to start performing relaxed measurements in RRC Idle/Inactive if multiple methods are configured.

NOTE 2: It is up to UE implementation which relaxation method to perform based on the "allowed" cases as specified in TS 38.133 [8] for RRC Idle/Inactive if multiple methods are configured.

The above relaxed measurements and no measurement are not applicable for frequencies that are included in *VarMeasIdleConfig*, if configured and for which the UE supports dual connectivity or carrier aggregation between those frequencies and the frequency of the current serving cell.

### 5.3.1 Cell status and cell reservations

Cell status and cell reservations are indicated in the *MIB or SIB1* message as specified in TS 38.331 [3] by means of following fields:

- *cellBarred* (IE type: "barred" or "not barred")
Indicated in *MIB* message. In case of multiple PLMNs or NPNs indicated in *SIB1*, this field is common for all PLMNs and NPNs.

- *cellBarredRedCap1Rx* (IE type: "barred" or "not barred")
Indicated in *SIB1* message. In case of multiple PLMNs or NPNs indicated in *SIB1*, this field is common for all PLMNs and NPNs. This field is only applicable to RedCap UEs.

- *cellBarredRedCap2Rx* (IE type: "barred" or "not barred")
Indicated in *SIB1* message. In case of multiple PLMNs or NPNs indicated in *SIB1*, this field is common for all PLMNs and NPNs. This field is only applicable to RedCap UEs.

- *cellReservedForOperatorUse* (IE type: "reserved" or "not reserved")
Indicated in *SIB1* message*.* In case of multiple PLMNs or NPNs indicated in *SIB1*, this field is specified per PLMN or per SNPN.

- *cellReservedForOtherUse* (IE type: "true")
Indicated in *SIB1* message. In case of multiple PLMNs indicated in *SIB1*, this field is common for all PLMNs.

*- cellReservedForFutureUse* (IE type: "true")
Indicated in *SIB1* message. In case of multiple PLMNs or NPNs indicated in *SIB1*, this field is common for all PLMNs and NPNs.

NOTE 0: IAB-MT ignores the *cellBarred*, *cellReservedForOperatorUse, cellReservedForFutureUse,* and *intraFreqReselection* (i.e. treats *intraFreqReselection* as if it was set to *allowed*) as defined in TS 38.331 [3]. IAB-MT also ignores *cellReservedForOtherUse* for cell barring determination (i.e. NPN capable IAB-MT considers *cellReservedForOtherUse* for determination of an NPN-only cell) as defined in TS 38.331 [3].

- *iab-Support* (IE type: "true")
Indicated in *SIB1* message. In case of multiple PLMNs or NPNs indicated in *SIB1*, this field is specified per PLMN or per SNPN.

Editor's note: Working assumption: A new bit, e.g. cellBarred-NTN, is introduced in SIB1 for NR-NTN. FFS on the expected UE behaviour upon reception of the new bit and the existing cellBarred.

When cell status is indicated as "not barred" and "not reserved" for operator use and not "true" for other use and not "true" for future use,

- UEs shall treat this cell as candidate during the cell selection and cell reselection procedures.

When cell broadcasts any CAG-IDs or NIDs and the cell status is indicated as "not barred" and "not reserved" for operator use and "true" for other use, and not "true" for future use:

- All NPN-capable UEs shall treat this cell as candidate during the cell selection and cell reselection procedures, other UEs shall treat this cell as if cell status is "barred".

When cell status is indicated as "true" for other use, and either cell does not broadcast any CAG-IDs or NIDs or does not broadcast any CAG-IDs and the UE is not operating in SNPN Access Mode,

- The UE shall treat this cell as if cell status is "barred".

When cell status is indicated as "true" for future use,

- The UE shall treat this cell as if cell status is "barred".

When cell status is indicated as "not barred" and "reserved" for operator use for any PLMN/SNPN and not "true" for other use and not "true" for future use,

- UEs assigned to Access Identity 11 or 15 operating in their HPLMN/EHPLMN shall treat this cell as candidate during the cell selection and reselection procedures if the field *cellReservedForOperatorUse* for that PLMN set to "reserved".

- UEs assigned to Access Identity 11 or 15 shall treat this cell as candidate during the cell selection and reselection procedures if the field *cellReservedForOperatorUse* for selected/registered SNPN is set to "reserved".

- UEs assigned to an Access Identity 0, 1, 2 and 12 to 14 shall behave as if the cell status is "barred" in case the cell is "reserved for operator use" for the registered PLMN/SNPN or the selected PLMN/SNPN.

- UEs assigned to Access Identity 3 shall behave as if the cell status is "barred" in case the cell is "reserved for operator use" for the registered PLMN or the selected PLMN.

NOTE 1: Access Identities 11, 15 are only valid for use in the HPLMN/ EHPLMN; Access Identities 12, 13, 14 are only valid for use in the home country as specified in TS 22.261 [12].

NOTE 1a: Access Identity 3 is only valid for PLMNs that indicate to potential Disaster Inbound Roamers that the UEs can access the PLMN as specified in TS 22.261 [12].

When cell status "barred" is indicated or to be treated as if the cell status is "barred",

- The UE is not permitted to select/reselect this cell, not even for emergency calls.

- The UE shall select another cell according to the following rule:

- If the cell is to be treated as if the cell status is "barred" due to being unable to acquire the *MIB*:

- the UE may exclude the barred cell as a candidate for cell selection/reselection for up to 300 seconds.

- the UE may select another cell on the same frequency if the selection criteria are fulfilled.

- else:

- If the UE is a RedCap UE, the UE shall acquire SIB1 and, in the remainder of this procedure, consider '*intraFreqReselection* in MIB' to be '*intraFreqReselectionRedCap* in SIB1', if available*.*

- If the UE is a not a RedCap UE, or the UE is a RedCap UE and *intraFreqReselectionRedCap* in SIB1 is available:

- If the field *intraFreqReselection* in *MIB* message is set to "allowed":

- the UE may select another cell on the same frequency if re-selection criteria are fulfilled;

- If the cell is to be treated as if the cell status is "barred" due to being unable to acquire the *SIB1*:

- the UE may exclude the barred cell as a candidate for cell selection/reselection for up to 300 seconds;

- else:

- the UE shall exclude the barred cell as a candidate for cell selection/reselection for 300 seconds.

- If the field *intraFreqReselection* in *MIB* message is set to "not allowed":

- If the cell is to be treated as if the cell status is "barred" due to being unable to acquire the *SIB1*:

- the UE may exclude the barred cell as a candidate for cell selection/reselection for up to 300 seconds;

- If the cell operates in licensed spectrum:

- the UE shall not re-select to another cell on the same frequency as the barred cell and exclude such cell(s) as candidate(s) for cell selection/reselection for 300 seconds;

- else:

- the UE may select to another cell on the same frequency if the reselection criteria are fulfilled.

- else:

- If the cell operates in licensed spectrum, or if this cell belongs to a PLMN which is indicated as being equivalent to the registered PLMN or the selected PLMN of the UE, or if this cell belongs to the registered SNPN or the selected SNPN of the UE:

- the UE shall not re-select to another cell on the same frequency as the barred cell and exclude such cell(s) as candidate(s) for cell selection/reselection for 300 seconds;

- else:

- the UE may select to another cell on the same frequency if the reselection criteria are fulfilled.

- the UE shall exclude the barred cell as a candidate for cell selection/reselection for 300 seconds.

When cell status "barred" is indicated for RedCap UEs with 1Rx/2Rx or to be treated as if the cell status is "barred",

- The UE is not permitted to select/reselect this cell, not even for emergency calls.

- The UE shall select another cell according to the following rule:

- If the cell is to be treated as if the cell status is "barred" due to being unable to acquire the *SIB1*:

- the UE may exclude the barred cell as a candidate for cell selection/reselection for up to 300 seconds.

- the UE may select another cell on the same frequency if the selection criteria are fulfilled.

- else:

- If the field *intraFreqReselectionRedCap* in *SIB1* message is set to "allowed"; or

- If the cell is to be treated as if the cell status is “barred” due to not supporting RedCap UEs:

- the UE shall exclude the barred cell as a candidate for cell selection/reselection for 300 seconds.

- the UE may select another cell on the same frequency if re-selection criteria are fulfilled.

- If the field *intraFreqReselectionRedCap* in *SIB1* message is set to "not allowed":

- If the cell operates in licensed spectrum, or if this cell belongs to a PLMN which is indicated as being equivalent to the registered PLMN or the selected PLMN of the UE, or if this cell belongs to the registered SNPN or the selected SNPN of the UE:

- the UE shall not re-select to another cell on the same frequency as the barred cell and exclude such cell(s) as candidate(s) for cell selection/reselection for 300 seconds.

- else:

- the UE may select to another cell on the same frequency if the reselection criteria are fulfilled.

- the UE shall exclude the barred cell as a candidate for cell selection/reselection for 300 seconds.

The cell selection of another cell may also include a change of RAT.

NOTE 2: If barring of a cell is triggered by the condition of *trackingAreaCode* and *trackingAreaList* not being provided, as specified in TS 38.331 [3], the barring only applies to this PLMN and the UE can re-evaluate the barring condition again due to selection of another PLMN.

## 7.1 Discontinuous Reception for paging

The UE may use Discontinuous Reception (DRX) in RRC\_IDLE and RRC\_INACTIVE state in order to reduce power consumption. The UE monitors one paging occasion (PO) per DRX cycle. A PO is a set of PDCCH monitoring occasions and can consist of multiple time slots (e.g. subframe or OFDM symbol) where paging DCI can be sent (TS 38.213 [4]). One Paging Frame (PF) is one Radio Frame and may contain one or multiple PO(s) or starting point of a PO.

In multi-beam operations, the UE assumes that the same paging message and the same Short Message are repeated in all transmitted beams and thus the selection of the beam(s) for the reception of the paging message and Short Message is up to UE implementation. The paging message is same for both RAN initiated paging and CN initiated paging.

The UE initiates RRC Connection Resume procedure upon receiving RAN initiated paging. If the UE receives a CN initiated paging in RRC\_INACTIVE state, the UE moves to RRC\_IDLE and informs NAS. However, if a L2 U2N Relay UE in RRC\_INACTIVE state receives a CN initiated paging for a L2 U2N Remote UE, the L2 U2N Relay UE does not move to RRC\_IDLE state.

NOTE: The L2 U2N Remote UE does not need to monitor the PO in order to receive the paging message.

The PF and PO for paging are determined by the following formulae:

SFN for the PF is determined by:

(SFN + PF\_offset) mod T = (T div N)\*(UE\_ID mod N)

Index (i\_s), indicating the index of the PO is determined by:

i\_s = floor (UE\_ID/N) mod Ns

The PDCCH monitoring occasions for paging are determined according to *pagingSearchSpace* as specified in TS 38.213 [4] and *firstPDCCH-MonitoringOccasionOfPO* and *nrofPDCCH-MonitoringOccasionPerSSB-InPO* ifconfigured as specified in TS 38.331 [3]. When *SearchSpaceId* = 0 is configured for *pagingSearchSpace*, the PDCCH monitoring occasions for paging are same as for RMSI as defined in clause 13 in TS 38.213 [4].

When *SearchSpaceId* = 0 is configured for *pagingSearchSpace*, Ns is either 1 or 2. For Ns = 1, there is only one PO which starts from the first PDCCH monitoring occasion for paging in the PF. For Ns = 2, PO is either in the first half frame (i\_s = 0) or the second half frame (i\_s = 1) of the PF.

When *SearchSpaceId* other than 0 is configured for *pagingSearchSpace,* the UE monitors the (i\_s + 1)th PO. A PO is a set of 'S\*X ' consecutive PDCCH monitoring occasions where 'S' is the number of actual transmitted SSBs determined according to *ssb-PositionsInBurst* in *SIB1* and X is the *nrofPDCCH-MonitoringOccasionPerSSB-InPO* if configured or is equal to 1 otherwise. The [x\*S+K]th PDCCH monitoring occasion for paging in the PO corresponds to the Kth transmitted SSB, where x=0,1,…,X-1, K=1,2,…,S. The PDCCH monitoring occasions for paging which do not overlap with UL symbols (determined according to *tdd-UL-DL-ConfigurationCommon*) are sequentially numbered from zero starting from the first PDCCH monitoring occasion for paging in the PF. When *firstPDCCH-MonitoringOccasionOfPO* is present, the starting PDCCH monitoring occasion number of (i\_s + 1)th PO is the (i\_s + 1)th value of the *firstPDCCH-MonitoringOccasionOfPO* parameter; otherwise, it is equal to i\_s \* S\*X. If X > 1, when the UE detects a PDCCH transmission addressed to P-RNTI within its PO, the UE is not required to monitor the subsequent PDCCH monitoring occasions for this PO.

NOTE 1: A PO associated with a PF may start in the PF or after the PF.

NOTE 2: The PDCCH monitoring occasions for a PO can span multiple radio frames. When *SearchSpaceId* other than 0 is configured for *paging-SearchSpace* the PDCCH monitoring occasions for a PO can span multiple periods of the paging search space.

The following parameters are used for the calculation of PF and i\_s above:

T: DRX cycle of the UE.

If eDRX is not configured as defined in clause 7.4:

- T is determined by the shortest of the UE specific DRX value(s), if configured by RRC and/or upper layers, and a default DRX value broadcast in system information. In RRC\_IDLE state, if UE specific DRX is not configured by upper layers, the default value is applied.

In RRC\_IDLE state, if eDRX is configured by upper layers, i.e., TeDRX, CN, according to clause 7.4:

- If TeDRX, CN is no longer than 1024 radio frames:

- T = TeDRX, CN;

- else:

- During CN configured PTW, T is determined by the shortest of UE specific DRX value, if configured by upper layers, and the default DRX value broadcast in system information.

In RRC\_INACTIVE state, if eDRX is configured by RRC, i.e., TeDRX, RAN , and/or upper layers, i.e., TeDRX, CN, as defined in clause 7.4:

- If both TeDRX, CN and TeDRX, RAN are no longer than 1024 radio frames, T = min{TeDRX, RAN, TeDRX, CN}.

- If TeDRX, CN is no longer than 1024 radio frames and no TeDRX, RAN is configured, T is determined by the shortest of UE specific DRX value configured by RRC, and TeDRX, CN.

- If TeDRX, CN is longer than 1024 radio frames:

- If TeDRX, RAN is not configured:

- During CN configured PTW, T is determined by the shortest of the UE specific DRX value (s), if configured by RRC and/or upper layers, and a default DRX value broadcast in system information. Outside the CN configured PTW, T is determined by the UE specific DRX value configured by RRC;

- else if TeDRX, RAN is no longer than 1024 radio frames:

- During CN configured PTW, T is determined by the shortest of the UE specific DRX value, if configured by upper layers and TeDRX, RAN, and a default DRX value broadcast in system information. Outside the CN configured PTW, T is determined by TeDRX, RAN.

N: number of total paging frames in T

Ns: number of paging occasions for a PF

PF\_offset: offset used for PF determination

UE\_ID:

If an eDRX cycle is configured by RRC or upper layers and *eDRX-Allowed* is signalled in SIB1:

- 5G-S-TMSI mod 4096

else:

- 5G-S-TMSI mod 1024

Parameters *Ns*, *nAndPagingFrameOffset*, *nrofPDCCH-MonitoringOccasionPerSSB-InPO*, and the length of default DRX Cycle are signaled in *SIB1*. The values of N and PF\_offset are derived from the parameter *nAndPagingFrameOffset* as defined in TS 38.331 [3]. The parameter *first-PDCCH-MonitoringOccasionOfPO* is signalled in *SIB1* for paging in initial DL BWP.For paging in a DL BWP other than the initial DL BWP, the parameter *first-PDCCH-MonitoringOccasionOfPO* is signaled in the corresponding BWP configuration.

If the UE has no 5G-S-TMSI, for instance when the UE has not yet registered onto the network, the UE shall use as default identity UE\_ID = 0 in the PF and i\_s formulas above.

5G-S-TMSI is a 48 bit long bit string as defined in TS 23.501 [10]. 5G-S-TMSI shall in the formulae above be interpreted as a binary number where the left most bit represents the most significant bit.

In RRC\_INACTIVE state, if the UE supports *inactiveStatePO-Determination* and the network broadcasts *ranPagingInIdlePO* with value "true", the UE shall use the same i\_s as for RRC\_IDLE state. Otherwise, the UE determines the i\_s based on the parameters and formula above.

In RRC\_INACTIVE state, if eDRX value configured by upper layers is no longer than 1024 radio frames, the UE shall use the same i\_s as for RRC\_IDLE state.

In RRC\_INACTIVE state, if eDRX value configured by upper layers is longer than 1024 radio frames, during CN PTW, the UE shall use the same i\_s as for RRC\_IDLE state.