3GPP TSG-RAN2 Meeting #119-e R2-220xxxx

eMeeting, 17-26 August 2022

Agenda Item: 8.5.1

Source: Qualcomm

Title: Summary of [Post119-e][261][XR] Reply LS to SA2 on UE power savings for XRM services

Document for: Discussion and Decision

# **Introduction**

This report provides a summary of the following post-meeting email discussion:

* [Post119-e][261][XR] LS to SA2 on XR power saving (Qualcomm)

 Scope: Answer SA2 LS on UE power saving (in [R2-2206966](https://www.3gpp.org/ftp/TSG_RAN/WG2_RL2/TSGR2_119-e/Docs/R2-2206966.zip)) according to RAN2 agreements.

 Intended outcome: Approved LS.

 Deadline: Short

The deadlines for this discussion are the following:

* **August 31th 1200 UTC:** deadline forcompanies’ feedback;
* **August 31th 1800** **UTC**: the rapporteur will provide a summary and a draft LS for review;
* **September 1st 2400 UTC**: deadline for companies’ feedback on the draft LS.

# **Contact information**

|  |  |  |
| --- | --- | --- |
| Company | Name | Email |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

# **Discussion**

## Background

In its LS [1], SA2 requested RAN1 and RAN2 to reply which type of information should be provided to RAN for UE power saving enhancements for XRM services:

|  |
| --- |
| **Overall Description:**TR38.838 evaluates the impact of power saving schemes on the performance of XR applications and identify potential enhancements under RAN2 responsibility. Specifically, the following power saving features have been identified:- CDRX enhancements - PDCCH monitoring enhancements It understood that these enhancements require assistance information from the network whose specification falls under SA2 responsibility.In 3GPP SA WG2 Meeting #S2-149E, new key issue was agreed for TR 23*.700-60* to study potential enhancements for power consumption considering traffic pattern of media services in the scope of FS\_XRM. It was agreed as follows:* Which information (e.g., XR/media traffic characteristics, traffic pattern and statistics), if any, is needed by the RAN from the CN and/or the UE to enhance power management (i.e., CDRX)? If needed, how such information is collected?

NOTE: This Key issue requires collaboration with RAN WGs.SA2 wants to request RAN1, RAN2 which type of information will be useful for the RAN for power saving enhancements for XR applications.**ACTION:** SA2 kindly asks RAN1, RAN2 to take the above information into account and clarify which type of information should be provided to the RAN for power saving enhancements for XR applications. |

RAN1 provided the following information in their reply LS [2]:

|  |
| --- |
| RAN1’s understanding is that RAN2 will also discuss the XR-awareness and decide what information from core network to RAN is helpful for XR-specific traffic handling. This reply LS is only from RAN1 perspective, and RAN1 expects SA2 to take into account response from both RAN1 and RAN2. In context of SA2 LS, RAN1 discussed what type of information from the core network to RAN could be helpful for the enhancement of XR-specific UE power management, if feasible, and identified following possible candidates for each XR application flow: * PDU set periodicity and start time of the first PDU of a PDU set: this can be helpful for e.g., configuring the periodicity and start time of CDRX or PDCCH monitoring to match with traffic period.
* PDU set end indication or indication of the last PDU in a PDU set: this can be helpful for gNB, e.g., to indicate the UE to dynamically skip PDCCH monitoring once the last PDU of the PDU set is delivered.
* PDU set level QoS parameters including priority and [air interface] delay budget of a PDU set: this can help the gNB to select suitable CDRX parameters (e.g., periodicities) that enable fulfilling the delay requirements for a given flow. It also helps with UE power saving, e.g., by reducing retransmission or by early dropping of a PDU that exceeds the delay deadline. Additionally, it can also be helpful for efficient radio resource management by gNB for capacity improvement.
* PDU set size (number of bits) or number of PDUs in a PDU set: RAN1’s understanding is that in comparison to the statistical information, real-time or dynamic information provided to gNB, if possible, can help scheduler make more efficient scheduling decision to enable UE power saving.
* PDU set identity and relationship information among PDUs within the same PDU set: gNB can use this information for early PDU dropping as mentioned above.
* Jitter information such as the range of the jitter (minimum and maximum value): Here jitter refers to packet arrival time variation at gNB for DL direction. gNB could use this information to configure parameters of UE power saving schemes, e.g., CDRX OnDuration and Active Time or PDCCH monitoring duration for handling of the jitter.
 |

In this email discussion, we discuss **from RAN2’s perspective** what type of information should be provided to RAN for UE power savings.

## Summary of submitted proposals

Several companies have submitted proposals on what information should be included in the reply LS to SA2. They are summarized in Table 1.

Table 1. Types of information proposed by companies

|  |  |  |
| --- | --- | --- |
| Type of information for RAN | Media unit | Proponents |
| Traffic pattern (e.g. periodicity, start time of media unit) | Burst | [3] |
| PDU set | [4], [6], [8], [10] |
| Unspecified | [5] |
| Jitter information of media unit (e.g. range, mean, variance of jitter in the start time of a media unit)  | Burst | [3] |
| PDU set | [4], [6], [7] , [8], [10] |
| Unspecified  | [5] |
| Size information of media unit (e.g. avg and max size) | Burst | [3] |
| PDU set | [4], [5], [8], [10] |
| Unspecified |  |
| Boundary indication of media unit (e.g. end of burst, last PDU in a PDU set) | Burst | [3], [7] |
| PDU set | [4], [6] |
| Information for identifying a media unit (e.g. sequence number) | Burst | [3] |
| PDU set | [4], [10] |
| QoS requirements for media units (e.g. priority, PSDB, PSER) | PDU set | [4], [5], [6], [7], [8], [10] |
| Relationship information of media unit (e.g. dependency among PDUs within a PDU Set or between PDU sets) | PDU set | [4], [6] |
| Explicit indication and conditions for delivery vs discard of a media unit | PDU | [9] |

## Discussion

The rapporteur observes that most companies are aligned in what type of information is useful to RAN, e.g. traffic pattern, jitter statistics, size information, boundary indicators, etc. However, companies have different views on which type of media unit that such information should be defined for, e.g. whether the information is for a PDU Set or a Data Burst.

To facilitate the discussion, the definition of these two different media units are copied from [11] below:

* **PDU Set**: A PDU Set is composed of one or more PDUs carrying the payload of one unit of information generated at the application level (e.g. a frame or video slice for XRM Services, as used in TR 26.926 [27]).
* **Data Burst**: A set of datamultiple PDUs generated and sent by the application in a short period of time. (NOTE: A Data Burst can be composed by one or multiple PDU Sets).

With the above definitions, the rapporteur’s understanding is that XR traffic periodicity is defined based on the number of UL/DL periodic bursts per second.

Based on the above observations, the rapporteur suggests that we organize our discussion in the following way:

* We first discuss whether a type of information (e.g. traffic pattern, jitter statistics, etc) is useful to RAN. The list of possible types of information selected based on those summarized in Table 1.
* For each type of information, we select which type of media unit (e.g. PDU Set vs Data Burst) this information is defined for. Moreover, how often this type of information should be signalled to RAN, e.g. whether it is static (e.g. defined in specs), semi-static (e.g. network configuration) or dynamic (e.g. via user-plane signaling).
* When companies comment, please do indicate which parameter(s) of that information they prefer (e.g. for traffic pattern, a parameter can be periodicity) and justifications for your preference. (e.g. useful for configuring DRX). A parameter without proper justification will be deprioritized.

**Q1. Do you think traffic pattern is useful to RAN for UE power savings?**

If you do, which type of media unit do you think should be used to define traffic pattern?

* Option 1. PDU Set;
* Option 2. Data Burst.

In your comment, please indicate which traffic pattern parameters you prefer (e.g. periodicity, start time, etc of your preferred media unot) and justification for your preference.

|  |  |  |
| --- | --- | --- |
| **Your preference**(No/Op1/Op2) | **How traffic pattern info should be signalled?**(static/semi-static/dynamic) | **Comments**(Any specific traffic pattern parameter(s) you prefer and justification for your preference) |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

**Q2. Do you think jitter information is useful to RAN for UE power savings?**

If you do, which type of media unit do you think should be used to define traffic pattern?

* Option 1. PDU;
* Option 2. PDU Set;
* Option 3. Data Burst.

In your comment, please indicate which jitter parameter(s) you prefer (e.g. range, mean, variance of start time of your preferred media unit) and justification for your preference.

|  |  |  |
| --- | --- | --- |
| **Your preference**(Op1/Op2/Op3/No) | **How jitter info should be signalled?**(static/semi-static/dynamic) | **Comments**(Any specific jitter parameter(s) you prefer and justification for your preference) |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

**Q3. Do you think size information (e.g. number of PDUs in a PDU set or number of PDU Sets in a Data Burst) is useful to RAN for UE power savings?**

If you do, which type of media unit do you think this size information should be for?

* Option 1. PDU Set;
* Option 2. Data Burst.

In your comment, please indicate which parameter(s) of size information you prefer (e.g. number of PDUs in a PDU Set or a Data Burst) and justifications for your preference.

|  |  |  |
| --- | --- | --- |
| **Your preference**(Op1/Op2/No) | **How size info should be signalled?**(static/semi-static/dynamic) | **Comments**(Any specific parameter(s) of size information you prefer and justification for your preference) |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

**Q4. Do you think boundary indication for a media unit (e.g. indication for end of a PDU Set or a Data Burst) is useful to RAN for UE power savings?**

If you do, which type of media unit do you think this size information should be for?

* Option 1. PDU Set;
* Option 2. Data Burst.

In your comment, please indicate what type of boundary indication you prefer (e.g. end of a PDU Set or a Data Burst) and justifications for your preference.

For this question, the rapporteur’s understanding is that it is not possible to signal boundary information to RAN in a static or semi-static manner. Please indicate in your comments if you have a different view.

|  |  |
| --- | --- |
| **Your preference**(Op1/Op2/No) | **Comments**(Any specific type of boundary indication you prefer and justification for your preference) |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |

**Q5. Do you think information for identifying a media unit (e.g. sequence number for PDU Sets or Data Bursts) is useful to RAN for UE power savings?**

If you do, which type of media unit do you think this size information should be for?

* Option 1. PDU;
* Option 2. PDU Set;
* Option 3. Data Burst.

In your comment, please indicate what type of information you think is useful in identifying a media unit (e.g. sequence number of PDUs in a PDU Set or sequence number of PDU Sets in a Data Burst) and justifications for your preference.

For this question, the rapporteur’s understanding is that it is not possible to signal information for identifying a media unit to RAN in a static or semi-static manner. Please indicate in your comments if you have a different view.

|  |  |
| --- | --- |
| **Your preference**(Op1/Op2/Op3/No) | **Comments**(which type of information for identifying a media unit you prefer and justification for your preference) |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |

**Q6. Do you think QoS requirements for media units (e.g. PDSB, PSER) are useful to RAN for UE power savings?**

If you do, which type of media unit do you think this size information should be for?

* Option 1. PDU;
* Option 2. PDU set.

In your comment, please indicate what type(s) of QoS requirements you think is useful (e.g. PSDB and/or PSER for PDU Set) and justifications for your preference.

For this question, as QoS requirements are defined by SA2, the rapporteur’s view is that we do not need to discuss how they should be defined/configured/signaled. Please indicate in your comments if you have a different view.

|  |  |
| --- | --- |
| **Your preference**(Op1/Op2/No) | **Comments**(Any specific QoS requirements you prefer and justification for your preference) |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |

**Q7. Do you think relationship information between media units (e.g. between PDUs within a PDU Set or between PDU Sets) is useful to RAN for UE power savings?**

In your comment, please indicate what type(s) of relationship information (e.g. between PDUs within a PDU Set, or between PDU Sets) between media units you think is useful and justifications for your preference.

For this question, the rapporteur’s understanding is that it is not possible to signal relationship information between media units in a static or semi-static manner. Please indicate in your comments if you have a different view.

|  |  |
| --- | --- |
| **Your preference**(Yes/No) | **Comments**(which type of relationship information between media units you prefer and justification for your preference) |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |

**Q8. Do you think any explicit indication and/or conditions for RAN to decide on delivery vs discard of a media unit would be useful for UE power savings?**

If you do, which type of media unit do you think such type of indications and/or conditions should be for?

* Option 1. PDU;
* Option 2. PDU Set.

In your comment, please indicate what type(s) of indication and/or conditions you prefer and justifications for your preference.

|  |  |  |
| --- | --- | --- |
| **Your preference**(No/Op1/Op2) | **How such indications or conditions should be signalled?**(static/semi-static/dynamic) | **Comments**(Any specific type(s) of indication and/or conditions you prefer and justification for your preference) |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

In [3], it is stated that for XR traffic flows not based on PDU Sets, information including traffic periodicity, start offset of PDUs and range of jitter can be useful to RAN in DRX configurations, and the information can be semi-statically provided to RAN (e.g., at PDU/QoS flow establishment or modification).

**Q9. For XR traffic flows not based on PDU Sets, do you think it is useful to provide RAN with their periodicity, start offset of PDUs and range of jitter for UE power savings?**

|  |  |
| --- | --- |
| **Yes/No** | **Comments**(Please provide you preferred parameters if they are not mentioned in Q9) |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |

**Q10. Any additional information that you think is important for RAN but is not included in any of the questions above?**

|  |  |  |
| --- | --- | --- |
| **Your preferred information** | **How should the information be signalled?**(static/semi-static/dynamic) | **Justifications for your preferred information**  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

# **Conclusions**

(To be added later)

# References

1. R2-2204523, LS on UE Power Saving for XR and Media Services (S2-2203418; contact: Nokia).
2. R2-2206923, Reply LS on UE Power Saving for XR and Media Services (R1-2205531; contact: Qualcomm).
3. R2-2207042, Draft reply LS on UE power savings for XR and media services, Qualcomm Incorporated.
4. R2-2207117, XR awareness: RAN2 areas of interest, assumptions, and inputs to SA2 LS, Intel Corporation.
5. R2-2207509, Consideration on power saving for XR service, CATT.
6. R2-2207757, Discussion on XR-specific power saving, vivo.
7. R2-2207888, Discussion on XR-specific power saving techniques, Huawei, HiSilicon.
8. R2-2208020, XR Power Saving enhancements, Nokia, Nokia Shanghai Bell.
9. R2-3308316, Discussion of SA2 LS on UE Power Saving for XR and Media Services, Meta.
10. R2-2208680, Discussion on power saving enhancements for XR, Ericsson.
11. TR 23.700-60 v0.3.0, Study on XR (Extended Reality) and media services (Rel-18).