**3GPP TSG-RAN WG2 Meeting #122 *R2-230xxxx***

**Incheon, South Korea, May 22 – 26, 2023**

|  |
| --- |
| *CR-Form-v12.2* |
| **CHANGE REQUEST** |
|  |
|  | **38.331** | **CR** | **4117** | **rev** | **1** | **Current version:** | **17.4.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network | **X** | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  | Miscellaneous non-controversial corrections Set XVIII |
|  |  |
| ***Source to WG:*** | Ericsson |
| ***Source to TSG:*** | R2 |
|  |  |
| ***Work item code:*** | TEI17 |  | ***Date:*** | 2023-05-29 |
|  |  |  |  |  |
| ***Category:*** | F |  | ***Release:*** | Rel-17 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)Rel-19 (Release 19)* |
|  |  |
| ***Reason for change:*** | Correction of miscellaneous non-controversial errors (typos etc). |
|  |  |
| ***Summary of change:*** | 1. 6.1.2 Need codes and conditions for optional fieldsBased on discussion at #121bis-e of R2-2303282 Clarification on drb-ContinueROHC, added an optional field with Need N in ASN.1 example.
2. BWP-UplinkDedicated field descriptions

Changed typo BPW to BWP.**CRs agreed at #121bis-e to be merged:**1. R2-2304536 Clarifications on CG Parameters in NR-UIn field description for cg-StartingFullBW-InsideCOT in CG-StartingOffsets, added reference to TS 38.211.
2. R2-2303127 General MBS CR to 38.331Changed message name Paging to use italics.
3. R2-2304170 Editorial modification to TS 38.331 on NR MBSFor mcch-ModificationPeriod-r17 in SIB20, changed the value ‘r2048’ to ‘rf2048’.

**CRs agreed at #122 to be merged:**1. R2-2306890 Miscellaneous corrections on NR QoE
	1. Clause 5.3.5.13d, 5.3.8.3: In NOTE 1 and in the action when the UE receives RRCRelease message with suspendConfig the term “application layer measurement reports” has been corrected to “application layer measurement report containers”.
	2. *MeasurementReportAppLayer* message: The ASN.1 values of appLayerSessionStatus have been corrected to “start” and “stop”.
	3. Clause 6.3.4, AppLayerMeasConfig field descriptions
		1. In the description of rrc-SegAllowed the word “allowed” has been replaced by “enabled” to be aligned with ASN.1.
		2. The description of transmissionOfSessionStartStop has been improved.
		3. In the description of ran-VisiblePeriodicity the missing word "measurements" has been added in “RAN visible application layer reporting”.
		4. In the description of serviceType a minor editorial issue has been fixed.
2. R2-2306354 Clarification on scellActiationRS-ConfigToAddModList field descriptionCorrected reference number in the field description of scellActivationRS-ConfigToAddModList.
3. R2-2305489 Corrections on the general description of UL information transfer
	1. 5.7.2.1 General (UL information transfer)Added the description “in RRC\_CONNECTED or in RRC\_INACTIVE during SDT” similar to the description in 5.7.1.1 for DL information transfer.
	2. Figure 5.7.4.1-1: UE Assistance InformationChanged “*RRCReconfiguration”* to “RRC Reconfiguration” to indicate the procedure name, not message name.
4. R2-2305135 Miscellaneous corrections for Rel-17 RRC
	1. In the description of field *monitoringSlotPeriodicityAndOffset* and condition *Setup4* the references to *monitoringSlotPeriodicityAndOffset-r17* have been replaced by *monitoringSlotPeriodicityAndOffset-v1710*.
	2. Some other editorial issues are corrected.

**Impact analysis**Impacted 5G architecture options: NR SA, (NG)EN-DC, NE-DC, NR-DCImpacted functionality:MiscellaneousInter-operability:There are no interoperability issues. |
|  |  |
| ***Consequences if not approved:*** | Typos and minor errors remain in the RRC specification. |
|  |  |
| ***Clauses affected:*** | 5.3.2.2, 5.3.5.13d, 5.3.8.3, 5.7.2.1, 5.7.4.1, 6.1.2, 6.2.2, 6.3.1, 6.3.2, 6.3.3, 6.3.4 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

#### 5.3.2.2 Initiation

The network initiates the paging procedure by transmitting the *Paging* message at the UE's paging occasion as specified in TS 38.304 [20]. The network may address multiple UEs within a *Paging* message by including one *PagingRecord* for each UE. The network may also include one or multiple TMGI(s) in the *Paging* message to page UEs for specific MBS multicast session(s).

*Next change*

#### 5.3.5.13d Application layer measurement configuration

The UE shall:

1> if *measConfigAppLayerToReleaseList* is included in *appLayerMeasConfig* within *RRCReconfiguration* or *RRCResume*:

2> for each *measConfigAppLayerId* value included in the *measConfigAppLayerToReleaseList*:

3> forward the *measConfigAppLayerId* and inform upper layers about the release of the application layer measurement configuration including any RAN visible application layer measurement configuration;

3> discard any application layer measurement report received from upper layers;

3> consider itself not to be configured to send application layer measurement report for the *measConfigAppLayerId*.

1> if *measConfigAppLayerToAddModList* is included in *appLayerMeasConfig* within *RRCReconfiguration* or *RRCResume*:

2> for each *measConfigAppLayerId* value included in the *measConfigAppLayerToAddModList*:

3> if *measConfigAppLayerContainer* is included for the corresponding *MeasConfigAppLayer* configuration:

4> forward the *measConfigAppLayerContainer*, the *measConfigAppLayerId* and the *serviceType* to upper layers considering the *serviceType*;

3> consider itself to be configured to send application layer measurement report for the *measConfigAppLayerId* in accordance with 5.7.16;

3> forward the *transmissionOfSessionStartStop*, if configured, and *measConfigAppLayerId* to upper layers considering the *serviceType*;

3> if *ran-VisibleParameters* is set to setup and the parameters have been received:

4> forward the *measConfigAppLayerId,* the *ran-VisiblePeriodicity*, if configured, the *numberOfBufferLevelEntries*, if configured, and the *reportPlayoutDelayForMediaStartup*, if configured, to upper layers considering the *serviceType*;

3> else if *ran-VisibleParameters* is set to release:

4> forward the *measConfigAppLayerId* and inform upper layers about the release of the RAN visible application layer measurement configuration;

3> if *pauseReporting* is set to *true*:

4> if at least one segment, but not all segments, of a segmented *MeasurementReportAppLayer* message containing an application layer measurement report associated with the *measConfigAppLayerId* has been submitted to lower layers for transmission:

5> submit the remaining segments of the *MeasurementReportAppLayer* message to lower layers for transmission;

4> suspend submitting application layer measurement report containers to lower layers for the application layer measurement configuration associated with the *measConfigAppLayerId*;

4> store any previously or subsequently received application layer measurement report containers associated with the *measConfigAppLayerId* for which no segment, or full message, has been submitted to lower layers for transmission;

3> else if *pauseReporting* is set to *false* and if transmission of application layer measurement report containers has previously been suspended for the application layer measurement configuration associated with the *measConfigAppLayerId*:

4> submit stored application layer measurement report containers to lower layers, if any, for the application layer measurements configuration associated with the *measConfigAppLayerId;*

4> resume submitting application layer measurement report containers to lower layers for the application layer measurement configuration associated with the *measConfigAppLayerId*;

NOTE 1: The UE may discard reports when the memory reserved for storing application layer measurement report containers become full.

NOTE 2: The transmission of RAN visible application layer measurement reports and *appLayerSessionStatus* is not paused when *pauseReporting* is set to *true*.

*Next change*

#### 5.3.8.3 Reception of the *RRCRelease* by the UE

The UE shall:

1> delay the following actions defined in this clause 60 ms from the moment the *RRCRelease* message was received or optionally when lower layers indicate that the receipt of the *RRCRelease* message has been successfully acknowledged, whichever is earlier;

1> stop timer T380, if running;

1> stop timer T320, if running;

1> if timer T316 is running;

2> stop timer T316;

2> clear the information included in *VarRLF-Report,* if any;

1> stop timer T350, if running;

1> stop timer T346g, if running;

1> if theAS security is not activated:

2> ignore any field included in *RRCRelease* message except *waitTime*;

2> perform the actions upon going to RRC\_IDLE as specified in 5.3.11 with the release cause 'other' upon which the procedure ends;

1> if the *RRCRelease* message includes *redirectedCarrierInfo* indicating redirection to *eutra*:

2> if *cnType* is included:

3> after the cell selection, indicate the available CN Type(s) and the received *cnType* to upper layers;

NOTE 1: Handling the case if the E-UTRA cell selected after the redirection does not support the core network type specified by the *cnType,* is up to UE implementation.

2> if *voiceFallbackIndication* is included:

3> consider the RRC connection release was for EPS fallback for IMS voice (see TS 23.502 [43]);

1> if the *RRCRelease* message includes the *cellReselectionPriorities*:

2> store the cell reselection priority information provided by the *cellReselectionPriorities*;

2> if the *t320* is included:

3> start timer T320, with the timer value set according to the value of *t320*;

1> else:

2> apply the cell reselection priority information broadcast in the system information;

1> if *deprioritisationReq* is included and the UE supports RRC connection release with deprioritisation:

2> start or restart timer T325 with the timer value set to the *deprioritisationTimer* signalled;

2> store the *deprioritisationReq* until T325 expiry;

NOTE 1a: The UE stores the deprioritisation request irrespective of any cell reselection absolute priority assignments (by dedicated or common signalling) and regardless of RRC connections in NR or other RATs unless specified otherwise.

1> if the *RRCRelease* includes the *measIdleConfig*:

2> if T331 is running:

3> stop timer T331;

3> perform the actions as specified in 5.7.8.3;

2> if the *measIdleConfig* is set to *setup*:

3> store the received *measIdleDuration* in *VarMeasIdleConfig*;

3> start timer T331 with the value set to *measIdleDuration*;

3> if the *measIdleConfig* contains *measIdleCarrierListNR*:

4> store the received *measIdleCarrierListNR* in *VarMeasIdleConfig*;

3> if the *measIdleConfig* contains *measIdleCarrierListEUTRA*:

4> store the received *measIdleCarrierListEUTRA* in *VarMeasIdleConfig*;

3> if the *measIdleConfig* contains *validityAreaList*:

4> store the received *validityAreaList* in *VarMeasIdleConfig*;

1> if the *RRCRelease* includes *suspendConfig*:

2> reset MAC and release the default MAC Cell Group configuration, if any;

2> apply the received *suspendConfig* except the received *nextHopChainingCount*;

2> if the *sdt-Config* is configured:

3> for each of the DRB in the *sdt-DRB-List*:

4> consider the DRB to be configured for SDT;

3> if *sdt-SRB2-Indication* is configured:

4> consider the SRB2 to be configured for SDT;

3> for each RLC bearer (except those associated with broadcast MRBs) that is not suspended:

4> re-establish the RLC entity as specified in TS 38.322 [4];

3> for SRB2 (if it is resumed) and for SRB1:

4> trigger the PDCP entity to perform SDU discard as specified in TS 38.323 [5];

3> if *sdt-MAC-PHY-CG-Config* is configured:

4> configure the PCell with the configured grant resources for SDT and instruct the MAC entity to start the *cg-SDT-TimeAlignmentTimer*;

2> if *srs-PosRRC-Inactive* is configured:

3> apply the configuration and instruct MAC to start the *inactivePosSRS-TimeAlignmentTimer*;

NOTE 1b: The Network should provide full configuration to UE for SRS for Positioning in RRC\_INACTIVE.

2> remove all the entries within the MCG and the SCG *VarConditionalReconfig*, if any;

2> for each *measId* of the MCG *measConfig* and for each *measId* of the SCG *measConfig*, if configured, if the associated *reportConfig* has a *reportType* set to *condTriggerConfig*:

3> for the associated *reportConfigId*:

4> remove the entry with the matching *reportConfigId* from the *reportConfigList* within the *VarMeasConfig*;

3> if the associated *measObjectId* is only associated to a *reportConfig* with *reportType* set to *condTriggerConfig*:

4> remove the entry with the matching *measObjectId* from the *measObjectList* within the *VarMeasConfig*;

3> remove the entry with the matching *measId* from the *measIdList* within the *VarMeasConfig*;

2> if the UE is acting as L2 U2N Remote UE:

3> if the PC5-RRC connection with the U2N Relay UE is determined to be released:

4> indicate upper layers to trigger PC5 unicast link release;

3> else (i.e., maintain the PC5 RRC connection):

4> establish or re-establish (e.g. via release and add) SL RLC entity for SRB1;

2> else:

3> re-establish RLC entities for SRB1;

2> if the *RRCRelease* message with *suspendConfig* was received in response to an *RRCResumeRequest* or an *RRCResumeRequest1*:

3> stop the timer T319 if running;

3> in the stored UE Inactive AS context:

4> replace the KgNB and KRRCint keys with the current KgNB and KRRCint keys;

4> replace the *nextHopChainingCount* with the value of *nextHopChainingCount* received in the *RRCRelease* message*;*

4> replace the *cellIdentity* with the *cellIdentity* of the cell the UE has received the *RRCRelease* message;

4> if the *suspendConfig* contains the *sl-UEIdentityRemote* (i.e. the UE is a L2 U2N Remote UE):

5> replace the C-RNTI with the value of the *sl-UEIdentityRemote*;

5> replace the physical cell identitywith the value of the *sl-PhysCellId* in *sl-ServingCellInfo* contained in the discovery message received from the connected L2 U2N Relay UE;

4> else:

5> replace the C-RNTI with the C-RNTI used in the cell (see TS 38.321 [3]) the UE has received the *RRCRelease* message;

5> replace the physical cell identitywith the physical cell identity of the cell the UE has received the *RRCRelease* message;

3> replace the *nextHopChainingCount* with the value associated with the current KgNB;

3> stop the timer T319a if running and consider SDT procedure is not ongoing;

2> else:

3> store in the UE Inactive AS Context the *nextHopChainingCount* received in the *RRCRelease* message*,* the current KgNB and KRRCint keys, the ROHC state, the EHC context(s), the UDC state, the stored QoS flow to DRB mapping rules, the application layer measurement configuration, the C-RNTI used in the source PCell, the *cellIdentity* and the physical cell identity of the source PCell, the *spCellConfigCommon* within *ReconfigurationWithSync* of the NR PSCell (if configured) and all other parameters configured except for:

- parameters within *ReconfigurationWithSync* of the PCell;

- parameters within *ReconfigurationWithSync* of the NR PSCell, if configured;

- parameters within *MobilityControlInfoSCG* of the E-UTRA PSCell, if configured;

- *servingCellConfigCommonSIB*;

- *sl-L2RelayUE-Config*, if configured;

- *sl-L2RemoteUE-Config*, if configured;

NOTE 1c: *suspendConfig* is not stored as part of UE Inactive AS Context, except for the fields explicitly specified.

3> store any previously or subsequently received application layer measurement report containers for which no segment, or full message, has been submitted to lower layers for transmission;

NOTE 2: NR sidelink communication/discovery related configurations and logged measurement configuration are not stored as UE Inactive AS Context, when UE enters RRC\_INACTIVE.

2> suspend all SRB(s) and DRB(s) and multicast MRB(s), except SRB0 and broadcast MRBs;

2> indicate PDCP suspend to lower layers of all DRBs and multicast MRBs;

2> release the SRAP entity, if configured;

2> if the *t380* is included:

3> start timer T380, with the timer value set to *t380*;

2> if the *RRCRelease* message is including the *waitTime*:

3> start timer T302 with the value set to the *waitTime*;

3> inform upper layers that access barring is applicable for all access categories except categories '0' and '2';

2> if T390 is running:

3> stop timer T390 for all access categories;

3> perform the actions as specified in 5.3.14.4;

2> indicate the suspension of the RRC connection to upper layers;

2> if the UE is capable of L2 U2N Remote UE:

3> enter RRC\_INACTIVE, and perform either cell selection as specified in TS 38.304 [20], or relay selection as specified in clause 5.8.15.3, or both;

2> else:

3> enter RRC\_INACTIVE and perform cell selection as specified in TS 38.304 [20];

1> else:

2> perform the actions upon going to RRC\_IDLE as specified in 5.3.11, with the release cause 'other'.

NOTE 3: Whether to release the PC5 unicast link is left to L2 U2N Remote UE's implementation.

NOTE 4: It is left to UE implementation whether to stop T430, if running, when going to RRC\_INACTIVE.

### 5.7.2 UL information transfer

#### 5.7.2.1 General



Figure 5.7.2.1-1: UL information transfer

The purpose of this procedure is to transfer NAS dedicated information from the UE to the network in RRC\_CONNECTED or in RRC\_INACTIVE during SDT, or to transfer F1-C related information from IAB-DU to IAB Donor-CU via the collocated IAB-MT in RRC\_CONNECTED.

### 5.7.4 UE Assistance Information

#### 5.7.4.1 General



Figure 5.7.4.1-1: UE Assistance Information

The purpose of this procedure is for the UE to inform the network of:

- its delay budget report carrying desired increment/decrement in the connected mode DRX cycle length, or;

- its overheating assistance information, or;

- its IDC assistance information, or;

- its preference on DRX parameters for power saving, or;

- its preference on the maximum aggregated bandwidth for power saving, or;

- its preference on the maximum number of secondary component carriers for power saving, or;

- its preference on the maximum number of MIMO layers for power saving, or;

- its preference on the minimum scheduling offset for cross-slot scheduling for power saving, or;

- its preference on the RRC state, or;

- configured grant assistance information for NR sidelink communication, or;

- its preference in being provisioned with reference time information, or;

- its preference for FR2 UL gap, or;

- its preference to transition out of RRC\_CONNECTED state for MUSIM operation, or;

- its preference on the MUSIM gaps, or;

- its relaxation state for RLM measurements, or;

- its relaxation state for BFD measurements, or;

- availability of data and/or signalling mapped to radio bearers which are not configured for SDT, or;

- its preference for the SCG to be deactivated, or;

- indicate that the UE has uplink data to transmit for a DRB for which there is no MCG RLC bearer while the SCG is deactivated, or;

- change of its fulfilment status for RRM measurement relaxation criterion, or;

- service link (specified in TS 38.300 [2]) propagation delay difference between serving cell and neighbour cell(s).

*Next change*

###

### 6.1.2 Need codes and conditions for optional fields

The need for fields to be present in a message or an abstract type, i.e., the ASN.1 fields that are specified as OPTIONAL in the abstract notation (ASN.1), is specified by means of comment text tags attached to the OPTIONAL statement in the abstract syntax. All comment text tags are available for use in the downlink direction for RRC message and in the sidelink for PC5 RRC message. The meaning of each tag is specified in table 6.1.2-1.

If conditions are used, a conditional presence table is provided for the message or information element specifying the need of the field for each condition case. The table also specifies whether UE maintains or releases the value in case the field is absent. The conditions clarify what the UE may expect regarding the setting of the message by the network for the RRC message or by the peer UE in the sidelink RRC message. Violation of conditions is regarded as invalid network behaviour when transmitting downlink RRC message or invalid UE behavior when transmitting PC5 RRC message, which the UE is not required to cope with. Hence the general error handling defined in 10.4 does not apply in case a field is absent although it is mandatory according to the CondC or CondM condition.

For guidelines on the use of need codes and conditions, see Annex A.6 and A.7.

Table 6.1.2-1: Meaning of abbreviations used to specify the need for fields to be present

| Abbreviation | Meaning |
| --- | --- |
| Cond conditionTag | Conditionally presentPresence of the field is specified in a tabular form following the ASN.1 segment. |
| CondC conditionTag | Configuration conditionPresence of the field is conditional to other configuration settings. |
| CondM conditionTag | Message conditionPresence of the field is conditional to other fields included in the message. |
| Need S | *Specified*Used for (configuration) fields, whose field description or procedure **specifies** the UE behavior performed upon receiving a message with the field absent (and not if field description or procedure specifies the UE behavior when field is not configured). |
| Need M | *Maintain*Used for (configuration) fields that are stored by the UE i.e. not one-shot. Upon receiving a message with the field absent, the UE maintains the current value. |
| Need N | *No action* (one-shot configuration that is not maintained)Used for (configuration) fields that are not stored and whose presence causes a one-time action by the UE. Upon receiving message with the field absent, the UE takes no action. |
| Need R | *Release*Used for (configuration) fields that are stored by the UE i.e. not one-shot. Upon receiving a message with the field absent, the UE releases the current value. |

NOTE: In this version of the specification, the condition tags CondC and CondM are not used.

Any field with Need M or Need N in system information shall be interpreted as Need R.

The need code used within a CondX definition only applies for the case (part of the condition) where it is defined: A condition may have different need codes for different parts of the condition. In particular, the CondX definition may contain the following "otherwise the field is absent" parts:

- "Otherwise, the field is absent": The field is not relevant or should not be configured when this part of the condition applies. In particular, the UE behaviour is not defined when the field is configured via another part of the condition and is reconfigured to this part of the condition. A need code is not provided when the transition from another part of the condition to this part of the condition is not supported, when the field clearly is a one-shot or there is no difference whether UE maintains or releases the value (e.g., in case the field is mandatory present according to the other part of the condition).

- "Otherwise, the field is absent, Need R": The field is released if absent when this part of the condition applies. This handles UE behaviour in case the field is configured via another part of the condition and this part of the condition applies (which means that network when transmitting downlink RRC message or peer UE transmitting PC5 RRC message can assume UE releases the field if this part of the condition is valid).

- "Otherwise, the field is absent, Need M": The UE retains the field if it was already configured when this part of the condition applies. This means the network when transmitting downlink RRC message or the peer UE when transmitting PC5 RRC message cannot release the field, but UE retains the previously configured value.

Use of different Need codes in different parts of a condition should be avoided.

For downlink RRC message and sidelink PC5 RRC messages, the need codes, conditions and ASN.1 defaults specified for a particular (child) field only apply in case the (parent) field including the particular field is present. Thus, if the parent is absent the UE shall not release the field unless the absence of the parent field implies that.

For (parent) fields without need codes in downlink RRC messages or sidelink PC5 RRC message, if the parent field is absent, UE shall follow the need codes of the child fields. Thus, if parent field is absent, the need code of each child field is followed (i.e. Need R child fields are released, Need M child fields are not modified and the actions for Need S child fields depend on the specified conditions of each field). Examples of (parent) fields in downlink RRC messages and sidelink PC5 RRC message without need codes where this rule applies are:

- *nonCriticalExtension* fields at the end of a message using empty SEQUENCE extension mechanism,

- groups of non-critical extensions using double brackets (referred to as extension groups), and

- non-critical extensions at the end of a message or at the end of a structure, contained in a BIT STRING or OCTET STRING (referred to as parent extension fields).

The handling of need codes as specified in the previous is illustrated by means of an example, as shown in the following ASN.1.

-- /example/ ASN1START

RRCMessage-IEs ::= SEQUENCE {

 field1 InformationElement1 OPTIONAL, -- Need M

 field2 InformationElement2 OPTIONAL, -- Need R

 nonCriticalExtension RRCMessage-v1570-IEs OPTIONAL

}

RRCMessage-1570-IEs ::= SEQUENCE {

 field3 InformationElement3 OPTIONAL, -- Need M

 nonCriticalExtension RRCMessage-v1640-IEs OPTIONAL

}

RRCMessage-v1640-IEs ::= SEQUENCE {

 field4 InformationElement4 OPTIONAL, -- Need R

 nonCriticalExtension SEQUENCE {} OPTIONAL

}

InformationElement1 ::= SEQUENCE {

 field10 InformationElement10 OPTIONAL, -- Need N

 field11 InformationElement11 OPTIONAL, -- Need M

 field12 InformationElement12 OPTIONAL, -- Need R

 ...,

 [[

 field13 InformationElement13 OPTIONAL, -- Need R

 field14 InformationElement14 OPTIONAL -- Need M

 ]]

}

InformationElement2 ::= SEQUENCE {

 field21 InformationElement11 OPTIONAL, -- Need M

 ...

}

-- ASN1STOP

The handling of need codes as specified in the previous implies that:

- if *field1* in *RRCMessage-IEs* is absent, UE does not modify or take action on any child fields configured within *field1* (regardless of their need codes);

- if *field2* in *RRCMessage-IEs* is absent, UE releases the *field2* (and also its child field *field21*);

- if *field1* or *field2* in *RRCMessage-IEs* is present, UE retains or releases their child fields according to the child field presence conditions;

- if *field1* in *RRCMessage-IEs* is present but the extension group containing *field13* and *field14* is absent, the UE releases *field13* but does not modify *field14*;

- if *nonCriticalExtension* defined by IE *RRCMessage-v1570-IEs* is absent, the UE does not modify *field3* but releases *field4*;

*Next change*

### 6.2.2 Message definitions

<Text omitted>

– *MeasurementReportAppLayer*

The *MeasurementReportAppLayer* message is used for sending application layer measurement report.

Signalling radio bearer: SRB4

RLC-SAP: AM

Logical channel: DCCH

Direction: UE to Network

***MeasurementReportAppLayer message***

-- ASN1START

-- TAG-MEASUREMENTREPORTAPPLAYER-START

MeasurementReportAppLayer-r17 ::= SEQUENCE {

 criticalExtensions CHOICE {

 measurementReportAppLayer-r17 MeasurementReportAppLayer-r17-IEs,

 criticalExtensionsFuture SEQUENCE {}

 }

}

MeasurementReportAppLayer-r17-IEs ::= SEQUENCE {

 measurementReportAppLayerList-r17 MeasurementReportAppLayerList-r17,

 lateNonCriticalExtension OCTET STRING OPTIONAL,

 nonCriticalExtension SEQUENCE{} OPTIONAL

}

MeasurementReportAppLayerList-r17 ::= SEQUENCE (SIZE (1..maxNrofAppLayerMeas-r17)) OF MeasReportAppLayer-r17

MeasReportAppLayer-r17 ::= SEQUENCE {

 measConfigAppLayerId-r17 MeasConfigAppLayerId-r17,

 measReportAppLayerContainer-r17 OCTET STRING OPTIONAL,

 appLayerSessionStatus-r17 ENUMERATED {start, stop} OPTIONAL,

 ran-VisibleMeasurements-r17 RAN-VisibleMeasurements-r17 OPTIONAL

}

RAN-VisibleMeasurements-r17 ::= SEQUENCE {

 appLayerBufferLevelList-r17 SEQUENCE (SIZE (1..8)) OF AppLayerBufferLevel-r17 OPTIONAL,

 playoutDelayForMediaStartup-r17 INTEGER (0..30000) OPTIONAL,

 pdu-SessionIdList-r17 SEQUENCE (SIZE (1..maxNrofPDU-Sessions-r17)) OF PDU-SessionID OPTIONAL,

 ...

}

AppLayerBufferLevel-r17 ::= INTEGER (0..30000)

-- TAG-MEASUREMENTREPORTAPPLAYER-STOP

-- ASN1STOP

|  |
| --- |
| ***MeasReportAppLayer* field descriptions** |
| ***appLayerSessionStatus***Indicates that an application layer measurement session in the application layer starts or ends. |
| ***measReportAppLayerContainer***The field contains the application layer measurement report container, see Annex L (normative) in TS 26.247 [68], clause 16.5 in TS 26.114 [69] and TS 26.118 [70]. |
| ***ran-VisibleMeasurements***The field contains the RAN visible application layer measurement report. |

|  |
| --- |
| ***RAN-VisibleMeasurements* field descriptions** |
| ***appLayerBufferLevelList***The field indicates a list of application layer buffer levels, and each *AppLayerBufferLevel* indicates the application layer buffer level in ms. Value 0 corresponds to 0ms, value 1 corresponds to 10ms, value 2 corresponds to 20 ms and so on. If the buffer level is larger than the maximum value of 30000 (5 minutes), the UE reports 30000. |
| ***playoutDelayForMediaStartup***Indicates the application layer playout delay for media start-up in ms. Value 0 corresponds to 0ms, value 1 corresponds to 1ms, value 2 corresponds to 2 ms and so on. If the playout delay for media start-up is larger than the maximum value of 30000ms, the UE reports 30000. |
| ***pdu-SessionIdList***Contains the identity of the PDU session, or the identities of the PDU sessions, used for application data flows subject to the RAN visible application layer measurements. |

*Next change*

### 6.3.1 System information blocks

<cut>

#### – *SIB20*

*SIB20* contains the information required to acquire the MCCH/MTCH configuration for MBS broadcast.

*SIB20* information element

-- ASN1START

-- TAG-SIB20-START

SIB20-r17 ::= SEQUENCE {

 mcch-Config-r17 MCCH-Config-r17,

 cfr-ConfigMCCH-MTCH-r17 CFR-ConfigMCCH-MTCH-r17 OPTIONAL, -- Need S

 lateNonCriticalExtension OCTET STRING OPTIONAL,

 ...

}

MCCH-Config-r17 ::= SEQUENCE {

 mcch-RepetitionPeriodAndOffset-r17 MCCH-RepetitionPeriodAndOffset-r17,

 mcch-WindowStartSlot-r17 INTEGER (0..79),

 mcch-WindowDuration-r17 ENUMERATED {sl2, sl4, sl8, sl10, sl20, sl40,sl80, sl160} OPTIONAL, -- Need S

 mcch-ModificationPeriod-r17 ENUMERATED {rf2, rf4, rf8, rf16, rf32, rf64, rf128, rf256,

 rf512, rf1024, rf2048, rf4096, rf8192, rf16384, rf32768, rf65536}

}

MCCH-RepetitionPeriodAndOffset-r17 ::= CHOICE {

 rf1-r17 INTEGER(0),

 rf2-r17 INTEGER(0..1),

 rf4-r17 INTEGER(0..3),

 rf8-r17 INTEGER(0..7),

 rf16-r17 INTEGER(0..15),

 rf32-r17 INTEGER(0..31),

 rf64-r17 INTEGER(0..63),

 rf128-r17 INTEGER(0..127),

 rf256-r17 INTEGER(0..255)

}

-- TAG-SIB20-STOP

-- ASN1STOP

| *SIB20* field descriptions |
| --- |
| ***cfr-ConfigMCCH-MTCH***Common frequency resource used for MCCH and MTCH reception. If the field is absent, the CFR for broadcast has the same location and size as CORESET#0 and PDSCH configuration of MCCH is the same as PDSCH configuration provided in *initialDownlinkBWP* in *SIB1*. |
| ***mcch-WindowDuration***Indicates, starting from the slot indicated by *mcch-WindowStartSlot*, the duration in slots during which MCCH may be scheduled. Absence of this field means that MCCH is only scheduled in the slot indicated by *mcch-WindowStartSlot*. The network always configures *mcch-WindowDuration* to be shorter or equal to the length of MCCH repetition period. |
| ***mcch-ModificationPeriod***Defines periodically appearing boundaries, i.e. radio frames for which SFN mod *mcch-ModificationPeriod* = 0. The contents of different transmissions of MCCH information can only be different if there is at least one such boundary in-between them. Value rf2 corresponds to two radio frames, value rf4 corresponds to four radio frames and so on. |
| ***mcch-RepetitionPeriodAndOffset***Defines the length and the offset of the MCCH repetition period. rf1 corresponds to a repetition period length of one radio frame, rf2 corresponds to a repetition period length of two radio frames and so on. The corresponding integer value indicates the offset of the repetition period in the number of radio frames. MCCH is scheduled in the MCCH transmission window starting from each radio frame for which: SFN mod repetition period length = offset of the repetition period. |
| ***mcch-WindowStartSlot***Indicates the slot in which MCCH transmission window starts. |

### 6.3.2 Radio resource control information elements

<cut>

#### – *BWP-UplinkDedicated*

The IE *BWP-UplinkDedicated* is used to configure the dedicated (UE specific) parameters of an uplink BWP.

*BWP-UplinkDedicated* information element

-- ASN1START

-- TAG-BWP-UPLINKDEDICATED-START

BWP-UplinkDedicated ::= SEQUENCE {

 pucch-Config SetupRelease { PUCCH-Config } OPTIONAL, -- Need M

 pusch-Config SetupRelease { PUSCH-Config } OPTIONAL, -- Need M

 configuredGrantConfig SetupRelease { ConfiguredGrantConfig } OPTIONAL, -- Need M

 srs-Config SetupRelease { SRS-Config } OPTIONAL, -- Need M

 beamFailureRecoveryConfig SetupRelease { BeamFailureRecoveryConfig } OPTIONAL, -- Cond SpCellOnly

 ...,

 [[

 sl-PUCCH-Config-r16 SetupRelease { PUCCH-Config } OPTIONAL, -- Need M

 cp-ExtensionC2-r16 INTEGER (1..28) OPTIONAL, -- Need R

 cp-ExtensionC3-r16 INTEGER (1..28) OPTIONAL, -- Need R

 useInterlacePUCCH-PUSCH-r16 ENUMERATED {enabled} OPTIONAL, -- Need R

 pucch-ConfigurationList-r16 SetupRelease { PUCCH-ConfigurationList-r16 } OPTIONAL, -- Need M

 lbt-FailureRecoveryConfig-r16 SetupRelease { LBT-FailureRecoveryConfig-r16 } OPTIONAL, -- Need M

 configuredGrantConfigToAddModList-r16 ConfiguredGrantConfigToAddModList-r16 OPTIONAL, -- Need N

 configuredGrantConfigToReleaseList-r16 ConfiguredGrantConfigToReleaseList-r16 OPTIONAL, -- Need N

 configuredGrantConfigType2DeactivationStateList-r16 ConfiguredGrantConfigType2DeactivationStateList-r16 OPTIONAL -- Need R

 ]],

 [[

 ul-TCI-StateList-r17 CHOICE {

 explicitlist SEQUENCE {

 ul-TCI-ToAddModList-r17 SEQUENCE (SIZE (1..maxUL-TCI-r17)) OF TCI-UL-State-r17 OPTIONAL, -- Need N

 ul-TCI-ToReleaseList-r17 SEQUENCE (SIZE (1..maxUL-TCI-r17)) OF TCI-UL-StateId-r17 OPTIONAL -- Need N

 },

 unifiedTCI-StateRef-r17 ServingCellAndBWP-Id-r17

 } OPTIONAL, -- Need R

 ul-powerControl-r17 Uplink-powerControlId-r17 OPTIONAL, -- Cond NoTCI-PC

 pucch-ConfigurationListMulticast1-r17 SetupRelease { PUCCH-ConfigurationList-r16 } OPTIONAL, -- Need M

 pucch-ConfigurationListMulticast2-r17 SetupRelease { PUCCH-ConfigurationList-r16 } OPTIONAL -- Need M

 ]],

 [[

 pucch-ConfigMulticast1-r17 SetupRelease { PUCCH-Config } OPTIONAL, -- Need M

 pucch-ConfigMulticast2-r17 SetupRelease { PUCCH-Config } OPTIONAL -- Need M

 ]],

 [[

 pathlossReferenceRSToAddModList-r17 SEQUENCE (SIZE (1..maxNrofPathlossReferenceRSs-r17)) OF PathlossReferenceRS-r17

 OPTIONAL, -- Need N

 pathlossReferenceRSToReleaseList-r17 SEQUENCE (SIZE (1..maxNrofPathlossReferenceRSs-r17)) OF PathlossReferenceRS-Id-r17

 OPTIONAL -- Need N

 ]]

}

ConfiguredGrantConfigToAddModList-r16 ::= SEQUENCE (SIZE (1..maxNrofConfiguredGrantConfig-r16)) OF ConfiguredGrantConfig

ConfiguredGrantConfigToReleaseList-r16 ::= SEQUENCE (SIZE (1..maxNrofConfiguredGrantConfig-r16)) OF ConfiguredGrantConfigIndex-r16

ConfiguredGrantConfigType2DeactivationState-r16 ::= SEQUENCE (SIZE (1..maxNrofConfiguredGrantConfig-r16)) OF ConfiguredGrantConfigIndex-r16

ConfiguredGrantConfigType2DeactivationStateList-r16 ::=

 SEQUENCE (SIZE (1..maxNrofCG-Type2DeactivationState)) OF ConfiguredGrantConfigType2DeactivationState-r16

-- TAG-BWP-UPLINKDEDICATED-STOP

-- ASN1STOP

|  |
| --- |
| *BWP-UplinkDedicated* field descriptions |
| ***beamFailureRecoveryConfig***Configuration of beam failure recovery. If *supplementaryUplink* is present, the field is present only in one of the uplink carriers, either UL or SUL. |
| ***configuredGrantConfig***A *Configured-Grant* of *type1* or *type2*. It may be configured for UL or SUL but in case of *type1* not for both at a time. Except for reconfiguration with sync, the NW does not reconfigure *configuredGrantConfig* when there is an active configured uplink grant Type 2 (see TS 38.321 [3]). However, the NW may release the *configuredGrantConfig* at any time. Network can only configure configured grant in one BWP using either this field or *configuredGrantConfigToAddModList.* |
| ***configuredGrantConfigToAddModList***Indicates a list of one or more configured grant configurations to be added or modified for one BWP. Except for reconfiguration with sync, the NW does not reconfigure a Type 2 configured grant configuration when it is active (see TS 38.321 [3]). The network configures multiple CG configurations for one BWP with either all configurations or no configuration configured with *cg-RetransmissionTimer-r16*. |
| ***configuredGrantConfigToReleaseList***Indicates a list of one or more UL Configured Grant configurations to be released. The NW may release a configured grant configuration at any time. |
| ***configuredGrantConfigType2DeactivationStateList***Indicates a list of the deactivation states in which each state can be mapped to a single or multiple Configured Grant type 2 configurations to be deactivated when the corresponding deactivation DCI is received, see clause 7.3.1 in TS 38.212 [17] and clause 10.2 in TS 38.213 [13]. |
| ***cp-ExtensionC2, cp-ExtensionC3***Configures the cyclic prefix (CP) extension (see TS 38.211 [16], clause 5.3.1). For 15 kHz SCS, {1..28} are valid for both *cp-ExtensionC2* and *cp-ExtensionC3*. For 30 kHz SCS, {1..28} are valid for *cp-ExtensionC2* and {2..28} are valid for *cp-ExtensionC3.* For 60 kHz SCS, {2..28} are valid for *cp-ExtensionC2* and {3..28} are valid for *cp-ExtensionC3*. |
| ***lbt-FailureRecoveryConfig***Configures parameters used for detection of consistent uplink LBT failures for operationwith shared spectrum channel access, as specified in TS 38.321 [3]. |
| ***pathlossReferenceRSToAddModList***A list of Reference Signals (e.g. a CSI-RS config or a SS block) to be used for path loss estimation for PUSCH, PUCCH and SRS for unified TCI state operation. If *unifiedTCI-StateType* is not configured for the serving cell, no element in this list is configured. |
| ***pucch-Config***PUCCH configuration for one BWP of the normal UL or SUL of a serving cell. If the UE is configured with SUL, the network configures PUCCH only on the BWPs of one of the uplinks (normal UL or SUL). The network configures *PUCCH-Config* at least on non-initial BWP(s) for SpCell and on all BWP(s) for PUCCH SCell. If supported by the UE, the network may configure at most one additional SCell of a cell group with *PUCCH-Config* (i.e. PUCCH SCell). If PUCCH cell switching is supported by the UE, the network may configure two TDD serving cells with *PUCCH-Config* within each PUCCH group. For supporting PUCCH cell switching in the PUCCH group with the SpCell, the TDD SpCell and one TDD SCell shall have *PUCCH-Config* on their normal UL. For supporting PUCCH cell switching in the PUCCH group with only SCells, two TDD SCells shall have *PUCCH-Config* on their normal UL.In (NG)EN-DC and NE-DC, the NW configures at most one serving cell per frequency range with PUCCH. In (NG)EN-DC and NE-DC, if two PUCCH groups are configured, the serving cells of the NR PUCCH group in FR2 use the same numerology. For NR-DC, the maximum number of PUCCH groups in each cell group is one, and only the same numerology is supported for the cell group with carriers only in FR2.The NW may configure PUCCH for a BWP when setting up the BWP. The network may also add/remove the *pucch-Config* in an *RRCReconfiguration* with *reconfigurationWithSync* (for SpCell or PUCCH SCell) or with SCell release and add (for PUCCH SCell) to move the PUCCH between the UL and SUL carrier of one serving cell. In other cases, only modifications of a previously configured *pucch-Config* are allowed.If one (S)UL BWP of a serving cell is configured with PUCCH, all other (S)UL BWPs must be configured with PUCCH, too. |
| ***pucch-ConfigurationList***PUCCH configurations for two simultaneously constructed HARQ-ACK codebooks (see TS 38.213 [13], clause 9.1). Different PUCCH Resource IDs are configured in different *PUCCH-Config* within the *pucch-ConfigurationList* if configured. |
| ***pucch-ConfigurationListMulticast1***PUCCH configurations for two simultaneously constructed HARQ-ACK codebooks for MBS multicast (see TS 38.213, clause 9). |
| ***pucch-ConfigurationListMulticast2***PUCCH configurations for two simultaneously constructed NACK-only feedback for MBS multicast (see TS 38.213, clause 9). |
| ***pusch-Config***PUSCH configuration for one BWP of the normal UL or SUL of a serving cell. If the UE is configured with SUL and if it has a *PUSCH-Config* for both UL and SUL, an UL/SUL indicator field in DCI indicates which of the two to use. See TS 38.212 [17], clause 7.3.1. |
| ***pucch-ConfigMulticast1***PUCCH configuration for the HARQ-ACK codebook for MBS multicast when multicast feedback is not configured with a priority value (see TS 38.213 [13], clause 9). If the field is not configured, *pucch-Config* applies. |
| ***pucch-ConfigMulticast2***PUCCH configuration for the NACK-only feedback for MBS multicast when multicast feedback is not configured with a priority value (see TS 38.213 [13], clause 9). If the field is not configured, *pucch-Config* applies. |
| ***sl-PUCCH-Config***Indicates the UE specific PUCCH configurations used for the HARQ-ACK feedback reporting for NR sidelink communication. |
| ***srs-Config***Uplink sounding reference signal configuration. |
| ***ul-powerControl***Configures power control parameters for PUCCH, PUSCH and SRS when UE is configured with *unifiedTCI-StateType* for this serving cell. For each serving cell, *ul-powerControl* is either configured in all *BWP-UplinkDedicated* or it is not configured in any *BWP-UplinkDedicated*. When *unifiedTCI-StateRef* in the *BWP-UplinkDedicated* of a serving cell refers to another serving cell, *ul-powerControl* is either configured in all *BWP-UplinkDedicated* of these two serving cells or it is not configured in any *BWP-UplinkDedicated* of these two serving cells. |
| ***ul-TCI-StateList***Indicates the applicable UL TCI states for PUCCH, PUSCH and SRS. |
| ***ul-TCI-ToAddModList***Indicates a list of UL TCI states. |
| ***unifiedTCI-StateRef***Provides the serving cell and UL BWP where UL TCI states applicable to this UL BWP are defined. |
| ***useInterlacePUCCH-PUSCH***If the field is present, the UE uses uplink frequency domain resource allocation Type 2 for PUSCH (see TS 38.213 [13], clause 8.3 and TS 38.214 [19], clause 6.1.2.2) and uses interlaced PUCCH Format 0, 1, 2, and 3 for PUCCH (see TS 38.213 [13], clause 9.2.1). |

|  |  |
| --- | --- |
| Conditional Presence | Explanation |
| *NoTCI-PC* | The field is optionally present, Need R, if *unifiedTCI-StateType* is configured for this serving cell and *ul-powerControl* is not configured for any UL TCI state or joint TCI state of this serving cell. Otherwise it is absent, Need R |
| *SpCellOnly* | The field is optionally present, Need M, in the *BWP-UplinkDedicated* of an SpCell. It is absent otherwise.  |

NOTE 1: In case of *RRCReconfiguration* with *reconfigurationWithSync*, the UE performs a MAC reset, which involves releasing the PUCCH-CSI/SRS/SR configuration in accordance with clause 5.3.12 and TS 38.321 [3], clauses 5.12 and 5.2. Hence, for these parts of the dedicated radio resource configuration, delta signalling is not supported in the message when *reconfigurationWithSync* is included.

#### – *ConfiguredGrantConfig*

The IE *ConfiguredGrantConfig* is used to configure uplink transmission without dynamic grant according to two possible schemes. The actual uplink grant may either be configured via RRC (*type1*) or provided via the PDCCH (addressed to CS-RNTI) (*type2*). Multiple Configured Grant configurations may be configured in one BWP of a serving cell.

*ConfiguredGrantConfig* information element

-- ASN1START

-- TAG-CONFIGUREDGRANTCONFIG-START

ConfiguredGrantConfig ::= SEQUENCE {

 frequencyHopping ENUMERATED {intraSlot, interSlot} OPTIONAL, -- Need S

 cg-DMRS-Configuration DMRS-UplinkConfig,

 mcs-Table ENUMERATED {qam256, qam64LowSE} OPTIONAL, -- Need S

 mcs-TableTransformPrecoder ENUMERATED {qam256, qam64LowSE} OPTIONAL, -- Need S

 uci-OnPUSCH SetupRelease { CG-UCI-OnPUSCH } OPTIONAL, -- Need M

 resourceAllocation ENUMERATED { resourceAllocationType0, resourceAllocationType1, dynamicSwitch },

 rbg-Size ENUMERATED {config2} OPTIONAL, -- Need S

 powerControlLoopToUse ENUMERATED {n0, n1},

 p0-PUSCH-Alpha P0-PUSCH-AlphaSetId,

 transformPrecoder ENUMERATED {enabled, disabled} OPTIONAL, -- Need S

 nrofHARQ-Processes INTEGER(1..16),

 repK ENUMERATED {n1, n2, n4, n8},

 repK-RV ENUMERATED {s1-0231, s2-0303, s3-0000} OPTIONAL, -- Need R

 periodicity ENUMERATED {

 sym2, sym7, sym1x14, sym2x14, sym4x14, sym5x14, sym8x14, sym10x14, sym16x14, sym20x14,

 sym32x14, sym40x14, sym64x14, sym80x14, sym128x14, sym160x14, sym256x14, sym320x14, sym512x14,

 sym640x14, sym1024x14, sym1280x14, sym2560x14, sym5120x14,

 sym6, sym1x12, sym2x12, sym4x12, sym5x12, sym8x12, sym10x12, sym16x12, sym20x12, sym32x12,

 sym40x12, sym64x12, sym80x12, sym128x12, sym160x12, sym256x12, sym320x12, sym512x12, sym640x12,

 sym1280x12, sym2560x12

 },

 configuredGrantTimer INTEGER (1..64) OPTIONAL, -- Need R

 rrc-ConfiguredUplinkGrant SEQUENCE {

 timeDomainOffset INTEGER (0..5119),

 timeDomainAllocation INTEGER (0..15),

 frequencyDomainAllocation BIT STRING (SIZE(18)),

 antennaPort INTEGER (0..31),

 dmrs-SeqInitialization INTEGER (0..1) OPTIONAL, -- Need R

 precodingAndNumberOfLayers INTEGER (0..63),

 srs-ResourceIndicator INTEGER (0..15) OPTIONAL, -- Need R

 mcsAndTBS INTEGER (0..31),

 frequencyHoppingOffset INTEGER (1.. maxNrofPhysicalResourceBlocks-1) OPTIONAL, -- Need R

 pathlossReferenceIndex INTEGER (0..maxNrofPUSCH-PathlossReferenceRSs-1),

 ...,

 [[

 pusch-RepTypeIndicator-r16 ENUMERATED {pusch-RepTypeA,pusch-RepTypeB} OPTIONAL, -- Need M

 frequencyHoppingPUSCH-RepTypeB-r16 ENUMERATED {interRepetition, interSlot} OPTIONAL, -- Cond RepTypeB

 timeReferenceSFN-r16 ENUMERATED {sfn512} OPTIONAL -- Need S

 ]],

 [[

 pathlossReferenceIndex2-r17 INTEGER (0..maxNrofPUSCH-PathlossReferenceRSs-1) OPTIONAL, -- Need R

 srs-ResourceIndicator2-r17 INTEGER (0..15) OPTIONAL, -- Need R

 precodingAndNumberOfLayers2-r17 INTEGER (0..63) OPTIONAL, -- Need R

 timeDomainAllocation-v1710 INTEGER (16..63) OPTIONAL, -- Need M

 timeDomainOffset-r17 INTEGER (0..40959) OPTIONAL, -- Need R

 cg-SDT-Configuration-r17 CG-SDT-Configuration-r17 OPTIONAL -- Need M

 ]]

 } OPTIONAL, -- Need R

 ...,

 [[

 cg-RetransmissionTimer-r16 INTEGER (1..64) OPTIONAL, -- Need R

 cg-minDFI-Delay-r16 ENUMERATED

 {sym7, sym1x14, sym2x14, sym3x14, sym4x14, sym5x14, sym6x14, sym7x14, sym8x14,

 sym9x14, sym10x14, sym11x14, sym12x14, sym13x14, sym14x14,sym15x14, sym16x14

 } OPTIONAL, -- Need R

 cg-nrofPUSCH-InSlot-r16 INTEGER (1..7) OPTIONAL, -- Need R

 cg-nrofSlots-r16 INTEGER (1..40) OPTIONAL, -- Need R

 cg-StartingOffsets-r16 CG-StartingOffsets-r16 OPTIONAL, -- Need R

 cg-UCI-Multiplexing-r16 ENUMERATED {enabled} OPTIONAL, -- Need R

 cg-COT-SharingOffset-r16 INTEGER (1..39) OPTIONAL, -- Need R

 betaOffsetCG-UCI-r16 INTEGER (0..31) OPTIONAL, -- Need R

 cg-COT-SharingList-r16 SEQUENCE (SIZE (1..1709)) OF CG-COT-Sharing-r16 OPTIONAL, -- Need R

 harq-ProcID-Offset-r16 INTEGER (0..15) OPTIONAL, -- Need M

 harq-ProcID-Offset2-r16 INTEGER (0..15) OPTIONAL, -- Need M

 configuredGrantConfigIndex-r16 ConfiguredGrantConfigIndex-r16 OPTIONAL, -- Cond CG-List

 configuredGrantConfigIndexMAC-r16 ConfiguredGrantConfigIndexMAC-r16 OPTIONAL, -- Cond CG-IndexMAC

 periodicityExt-r16 INTEGER (1..5120) OPTIONAL, -- Need R

 startingFromRV0-r16 ENUMERATED {on, off} OPTIONAL, -- Need R

 phy-PriorityIndex-r16 ENUMERATED {p0, p1} OPTIONAL, -- Need R

 autonomousTx-r16 ENUMERATED {enabled} OPTIONAL -- Cond LCH-BasedPrioritization

 ]],

 [[

 cg-betaOffsetsCrossPri0-r17 SetupRelease { BetaOffsetsCrossPriSelCG-r17 } OPTIONAL, -- Need M

 cg-betaOffsetsCrossPri1-r17 SetupRelease { BetaOffsetsCrossPriSelCG-r17 } OPTIONAL, -- Need M

 mappingPattern-r17 ENUMERATED {cyclicMapping, sequentialMapping} OPTIONAL, -- Cond SRSsets

 sequenceOffsetForRV-r17 INTEGER (0..3) OPTIONAL, -- Need R

 p0-PUSCH-Alpha2-r17 P0-PUSCH-AlphaSetId OPTIONAL, -- Need R

 powerControlLoopToUse2-r17 ENUMERATED {n0, n1} OPTIONAL, -- Need R

 cg-COT-SharingList-r17 SEQUENCE (SIZE (1..50722)) OF CG-COT-Sharing-r17 OPTIONAL, -- Need R

 periodicityExt-r17 INTEGER (1..40960) OPTIONAL, -- Need R

 repK-v1710 ENUMERATED {n12, n16, n24, n32} OPTIONAL, -- Need R

 nrofHARQ-Processes-v1700 INTEGER(17..32) OPTIONAL, -- Need M

 harq-ProcID-Offset2-v1700 INTEGER (16..31) OPTIONAL, -- Need R

 configuredGrantTimer-v1700 INTEGER(33..288) OPTIONAL, -- Need R

 cg-minDFI-Delay-v1710 INTEGER (238..3584) OPTIONAL -- Need R

 ]],

 [[

 harq-ProcID-Offset-v1730 INTEGER (16..31) OPTIONAL, -- Need R

 cg-nrofSlots-r17 INTEGER (1..320) OPTIONAL -- Need R

 ]]

}

CG-UCI-OnPUSCH ::= CHOICE {

 dynamic SEQUENCE (SIZE (1..4)) OF BetaOffsets,

 semiStatic BetaOffsets

}

CG-COT-Sharing-r16 ::= CHOICE {

 noCOT-Sharing-r16 NULL,

 cot-Sharing-r16 SEQUENCE {

 duration-r16 INTEGER (1..39),

 offset-r16 INTEGER (1..39),

 channelAccessPriority-r16 INTEGER (1..4)

 }

}

CG-COT-Sharing-r17 ::= CHOICE {

 noCOT-Sharing-r17 NULL,

 cot-Sharing-r17 SEQUENCE {

 duration-r17 INTEGER (1..319),

 offset-r17 INTEGER (1..319)

 }

}

CG-StartingOffsets-r16 ::= SEQUENCE {

 cg-StartingFullBW-InsideCOT-r16 SEQUENCE (SIZE (1..7)) OF INTEGER (0..6) OPTIONAL, -- Need R

 cg-StartingFullBW-OutsideCOT-r16 SEQUENCE (SIZE (1..7)) OF INTEGER (0..6) OPTIONAL, -- Need R

 cg-StartingPartialBW-InsideCOT-r16 INTEGER (0..6) OPTIONAL, -- Need R

 cg-StartingPartialBW-OutsideCOT-r16 INTEGER (0..6) OPTIONAL -- Need R

}

BetaOffsetsCrossPriSelCG-r17 ::= CHOICE {

 dynamic-r17 SEQUENCE (SIZE (1..4)) OF BetaOffsetsCrossPri-r17,

 semiStatic-r17 BetaOffsetsCrossPri-r17

}

CG-SDT-Configuration-r17 ::= SEQUENCE {

 cg-SDT-RetransmissionTimer INTEGER (1..64) OPTIONAL, -- Need R

 sdt-SSB-Subset-r17 CHOICE {

 shortBitmap-r17 BIT STRING (SIZE (4)),

 mediumBitmap-r17 BIT STRING (SIZE (8)),

 longBitmap-r17 BIT STRING (SIZE (64))

 } OPTIONAL, -- Need S

 sdt-SSB-PerCG-PUSCH-r17 ENUMERATED {oneEighth, oneFourth, half, one, two, four, eight, sixteen} OPTIONAL, -- Need M

 sdt-P0-PUSCH-r17 INTEGER (-16..15) OPTIONAL, -- Need M

 sdt-Alpha-r17 ENUMERATED {alpha0, alpha04, alpha05, alpha06, alpha07, alpha08, alpha09, alpha1} OPTIONAL, -- Need M

 sdt-DMRS-Ports-r17 CHOICE {

 dmrsType1-r17 BIT STRING (SIZE (8)),

 dmrsType2-r17 BIT STRING (SIZE (12))

 } OPTIONAL, -- Need M

 sdt-NrofDMRS-Sequences-r17 INTEGER (1..2) OPTIONAL -- Need M

}

-- TAG-CONFIGUREDGRANTCONFIG-STOP

-- ASN1STOP

|  |
| --- |
| *ConfiguredGrantConfig* field descriptions |
| ***antennaPort***Indicates the antenna port(s) to be used for this configuration, and the maximum bitwidth is 5. See TS 38.214 [19], clause 6.1.2, and TS 38.212 [17], clause 7.3.1. The UE ignores this field in case of CG-SDT. |
| ***autonomousTx***If this field is present, the Configured Grant configuration is configured with autonomous transmission, see TS 38.321 [3]. |
| ***betaOffsetCG-UCI***Beta offset for CG-UCI in CG-PUSCH, see TS 38.213 [13], clause 9.3 |
| ***cg-betaOffsetsCrossPri0, cg-betaOffsetsCrossPri1***Selection between and configuration of dynamic and semi-static beta-offset for multiplexing HARQ-ACK in CG-PUSCH with different priorities.The field *cg-betaOffsetsCrossPri0* indicates multiplexing LP HARQ-ACK in HP CG-PUSCH. This field is configured only if *phy-PriorityIndex-r16* is configured with value *p1*.The field *cg-betaOffsetsCrossPri1* indicates multiplexing HP HARQ-ACK in LP CG-PUSCH. This field is configured only if *phy-PriorityIndex-r16* is configured with value *p0*. |
| ***cg-COT-SharingList***Indicates a table for COT sharing combinations (see 37.213 [48], clause 4.1.3). One row of the table can be set to noCOT-Sharing to indicate that there is no channel occupancy sharing. If the *cg-RetransmissionTimer-r16* is configured and the UE operates as an initiating device in semi-static channel access mode (see TS 37.213 [48], clause 4.3), then c*g-COT-SharingList-r16* is configured*.* |
| ***cg-COT-SharingOffset***Indicates the offset from the end of the slot where the COT sharing indication in UCI is enabled where the offset in symbols is equal to 14\*n, where n is the signaled value for *cg-COT-SharingOffset*. Applicable when *ul-toDL-COT-SharingED-Threshold-r16* is not configured (see 37.213 [48], clause 4.1.3). |
| ***cg-DMRS-Configuration***DMRS configuration (see TS 38.214 [19], clause 6.1.2.3). |
| ***cg-minDFI-Delay***Indicates the minimum duration (in unit of symbols) from the ending symbol of the PUSCH to the starting symbol of the PDCCH containing the downlink feedback indication (DFI) carrying HARQ-ACK for this PUSCH. The HARQ-ACK received before this minimum duration is not considered as valid for this PUSCH (see TS 38.213 [13], clause 10.5). The following minimum duration values are supported, depending on the configured subcarrier spacing [symbols]:15 kHz: 7, m\*14, where m = {1, 2, 3, 4}30 kHz: 7, m\*14, where m = {1, 2, 3, 4, 5, 6, 7, 8}60 kHz: 7, m\*14, where m = {1, 2, 3, 4, 5, 6, 7, 8, 9, 10, 11, 12, 13, 14, 15, 16}120 kHz: 7, m\*14, where m = {1, 2, 3, 4, 5, 6, 7, 8, 9, 10, 11, 12, 13, 14, 15, 16, 17, 18, 19, 20, 21, 22, 23, 24, 25, 26, 27, 28, 29, 30, 31, 32}480 kHz: m\*14, where m = {2, 4, 8, 12, 16, 20, 24, 28, 32, 36, 40, 44, 48, 52, 56, 60, 64, 68, 72, 76, 80, 84, 88, 92, 96, 100, 104, 108, 112, 116, 120, 124, 128}960 kHz: m\*14, where m = {4, 8, 16, 24, 32, 40, 48, 56, 64, 72, 80, 88, 96, 104, 112, 120, 128, 136, 144, 152, 160, 168, 176, 184, 192, 200, 208, 216, 224, 232, 240, 248, 256} |
| ***cg-nrofPUSCH-InSlot***Indicates the number of consecutive PUSCH configured to CG within a slot where the SLIV indicating the first PUSCH and additional PUSCH appended with the same length (see TS 38.214 [19], clause 6.1.2.3). The network can only configure this field if *cg-RetransmissionTimer* is configured. |
| ***cg-nrofSlots***Indicates the number of allocated slots in a configured grant periodicity following the time instance of configured grant offset (see TS 38.214 [19], clause 6.1.2.3). *cg-nrofSlots-r17* is only applicable for operation with shared spectrum channel access in FR2-2. When *cg-nrofSlots-r17* is configured, the UE shall ignore *cg-nrofSlots-r16*. The network can only configure this field if *cg-RetransmissionTimer* is configured. |
| ***cg-RetransmissionTimer***Indicates the initial value of the configured retransmission timer (see TS 38.321 [3]) in multiples of *periodicity*. The value of *cg-RetransmissionTimer* is always less than or equal to the value of *configuredGrantTimer.* This field is always configured together with *harq-ProcID-Offset*. This field is not configured for operation in licensed spectrum or simultaneously with *harq-ProcID-Offset2.* The network does not configure this field for CG-SDT. |
| ***cg-StartingOffsets***This field is not applicable for a UE which is allowed to operate as an initiating device in semi-static channel access mode, i.e., not applicable for a UE configured with UE FFP parameters (e.g. period, offset) regardless whether the UE would initiate its own COT or would share gNB's COT. |
| ***cg-UCI-Multiplexing***If present, this field indicates that in the case of PUCCH overlapping with CG-PUSCH(s) within a PUCCH group, the CG-UCI and HARQ-ACK are jointly encoded (see TS 38.213 [13], clause 9). |
| ***configuredGrantConfigIndex***Indicates the index of the Configured Grant configurations within the BWP. |
| ***configuredGrantConfigIndexMAC***Indicates the index of the Configured Grant configurations within the MAC entity. |
| ***configuredGrantTimer***Indicates the initial value of the configured grant timer (see TS 38.321 [3]) in multiples of periodicity. When *cg-RetransmissonTimer* is configured, if HARQ processes are shared among different configured grants on the same BWP, *configuredGrantTimer \* periodicity* is set to the same value for the configurations that share HARQ processes on this BWP. The value of the extension *configuredGrantTimer* is 2 times the configured value. |
| ***dmrs-SeqInitialization***The network configures this field if *transformPrecoder* is disabled or when the value of *sdt-NrofDMRS-Sequences* is set to 1. Otherwise, the field is absent. |
| ***frequencyDomainAllocation***Indicates the frequency domain resource allocation, see TS 38.214 [19], clause 6.1.2, and TS 38.212 [17], clause 7.3.1). |
| ***frequencyHopping***The value *intraSlot* enables 'Intra-slot frequency hopping' and the value *interSlot* enables 'Inter-slot frequency hopping'. If the field is absent, frequency hopping is not configured. The field *frequencyHopping* applies to configured grant for 'pusch-RepTypeA' (see TS 38.214 [19], clause 6.3.1). |
| ***frequencyHoppingOffset***Frequency hopping offset used when frequency hopping is enabled (see TS 38.214 [19], clause 6.1.2 and clause 6.3). |
| ***frequencyHoppingPUSCH-RepTypeB***Indicates the frequency hopping scheme for Type 1 CG when *pusch-RepTypeIndicator* is set to 'pusch-RepTypeB' (see TS 38.214 [19], clause 6.1). The value *interRepetition* enables 'Inter-repetition frequency hopping', and the value *interSlot* enables 'Inter-slot frequency hopping'. If the field is absent, the frequency hopping is not enabled for Type 1 CG. |
| ***harq-ProcID-Offset***For operation with shared spectrum channel access configured with *cg-RetransmissionTimer-r16*, this configures the range of HARQ process IDs which can be used for this configured grant where the UE can select a HARQ process ID within [*harq-procID-offset, ..,* (*harq-procID-offset + nrofHARQ-Processes* – 1)]. *harq-ProcID-Offset-v1730* is only applicable for operation with shared spectrum channel access in FR2-2*.* If the field *harq-ProcID-Offset-v1730* is present, the UE shall ignore the *harq-ProcID-Offset-r16*. The network does not configure this field for CG-SDT. |
| ***harq-ProcID-Offset2***Indicates the offset used in deriving the HARQ process IDs, see TS 38.321 [3], clause 5.4.1. This field is not configured together with *cg-RetransmissionTimer-r16*. If the field *harq-ProcID-Offset2-v1700* is present, the UE shall ignore the *harq-ProcID-Offset2-r16*. |
| ***mappingPattern***Indicates whether the UE should follow Cyclical mapping pattern or Sequential mapping pattern when two SRS resource sets are configured in *srs-ResourceSetToAddModList* or *srs-ResourceSetToAddModListDCI-0-2* with usage 'codebook' or 'noncodebook' for PUSCH transmission with a Type 1 configured grant and/or a Type 2 configured grant as described in clause 6.1.2.3 of TS 38.214 [19] |
| ***mcs-Table***Indicates the MCS table the UE shall use for PUSCH without transform precoding. If the field is absent the UE applies the value *qam64*. |
| ***mcs-TableTransformPrecoder***Indicates the MCS table the UE shall use for PUSCH with transform precoding. If the field is absent the UE applies the value *qam64*. |
| ***mcsAndTBS***The modulation order, target code rate and TB size (see TS 38.214 [19], clause 6.1.2). The NW does not configure the values 28~31 in this version of the specification. |
| ***nrofHARQ-Processes***The number of HARQ processes configured. It applies for both Type 1 and Type 2. See TS 38.321 [3], clause 5.4.1. If the UE is configured with *nrofHARQ-Processes-v1700, the* UE shall ignore *nrofHARQ-Processes (without suffix)*. |
| ***pathlossReferenceIndex***Indicates the reference signal index used as PUSCH pathloss reference (see TS 38.213 [13], clause 7.1.1). In case of CG-SDT, the UE does not use this field. |
| ***pathlossReferenceIndex2***Indicates the reference signal used as PUSCH pathloss reference for the second SRS resource set. When this field is present, pathlossReferenceIndex indicates the reference signal used as PUSCH pathloss reference for the first SRS resource set  |
| ***p0-PUSCH-Alpha***Index of the *P0-PUSCH-AlphaSet* to be used for this configuration. |
| ***p0-PUSCH-Alpha2***Index of the *P0-PUSCH-AlphaSet* to be used for second SRS resource set. If this field is present, the *p0-PUSCH-Alpha* provides index for the P0-PUSCH-AlphaSet to be used for first SRS resource set. |
| ***periodicity***Periodicity for UL transmission without UL grant for type 1 and type 2 (see TS 38.321 [3], clause 5.8.2).The following periodicities are supported depending on the configured subcarrier spacing [symbols]:15 kHz: 2, 7, n\*14, where n={1, 2, 4, 5, 8, 10, 16, 20, 32, 40, 64, 80, 128, 160, 320, 640}30 kHz: 2, 7, n\*14, where n={1, 2, 4, 5, 8, 10, 16, 20, 32, 40, 64, 80, 128, 160, 256, 320, 640, 1280}60 kHz with normal CP 2, 7, n\*14, where n={1, 2, 4, 5, 8, 10, 16, 20, 32, 40, 64, 80, 128, 160, 256, 320, 512, 640, 1280, 2560}60 kHz with ECP: 2, 6, n\*12, where n={1, 2, 4, 5, 8, 10, 16, 20, 32, 40, 64, 80, 128, 160, 256, 320, 512, 640, 1280, 2560}120 kHz: 2, 7, n\*14, where n={1, 2, 4, 5, 8, 10, 16, 20, 32, 40, 64, 80, 128, 160, 256, 320, 512, 640, 1024, 1280, 2560, 5120}480 and 960 kHz: n\*14, where n={1, 2, 4, 5, 8, 10, 16, 20, 32, 40, 64, 80, 128, 160, 256, 320, 512, 640, 1024, 1280, 2560, 5120}In case of SDT, the network does not configure periodicity values less than 5ms. |
| ***periodicityExt***This field is used to calculate the periodicity for UL transmission without UL grant for type 1 and type 2 (see TS 38.321 [3], clause 5.8.2). If this field is present, the field *periodicity* is ignored.The following periodicites are supported depending on the configured subcarrier spacing [symbols]:15 kHz: *periodicityExt*\*14, where *periodicityExt* has a value between 1 and 640.30 kHz: *periodicityExt*\*14, where *periodicityExt* has a value between 1 and 1280.60 kHz with normal CP: *periodicityExt*\*14, where *periodicityExt* has a value between 1 and 2560.60 kHz with ECP: *periodicityExt*\*12, where *periodicityExt* has a value between 1 and 2560.120 kHz: *periodicityExt*\*14, where *periodicityExt* has a value between 1 and 5120.480 kHz: *periodicityExt*\*14, where *periodicityExt* has a value between 1 and 20480.960 kHz: *periodicityExt*\*14, where *periodicityExt* has a value between 1 and 40960.In case of SDT, the network does not configure periodicity values less than 5ms. |
| ***phy-PriorityIndex***Indicates the PHY priority of CG PUSCH at least for PHY-layer collision handling. Value *p0* indicates low priority and value *p1* indicates high priority. The network does not configure this for CG-SDT. |
| ***powerControlLoopToUse***Closed control loop to apply (see TS 38.213 [13], clause 7.1.1). |
| ***powerControlLoopToUse2***Closed control loop to apply to second SRS resource set (see TS 38.213 [13], clause 7.1.1). If this field is present, the *powerControlLoopToUse* applies to the first SRS resource set. |
| ***precodingAndNumberOfLayers***Indicates the precoding and number of layers (see TS 38.212 [17], clause 7.3.1.1.2, and TS 38.214 [19], clause 6.1.2.3). In case of CG-SDT, network sets this field to 1. |
| ***precodingAndNumberOfLayers2***Indicates the precoding and number of layers for the second SRS resource set. When this field is present, *precodingAndNumberOfLayers* indicated the precoding and number of layers for the first SRS resource set. |
| ***pusch-RepTypeIndicator***Indicates whether UE follows the behavior for PUSCH repetition type A or the behavior for PUSCH repetition type B for each Type 1 configured grant configuration. The value *pusch-RepTypeA* enables the 'PUSCH repetition type A' and the value *pusch-RepTypeB* enables the 'PUSCH repetition type B' (see TS 38.214 [19], clause 6.1.2.3). The value *pusch-RepTypeB* is not configured simultaneously with *cg-nrofPUSCH-InSlot-r16* and *cg-nrofSlots-r16*. The network does not configure this field if *cg-RetransmissionTimer-r16* is configured for CG operation with shared spectrum channel access. |
| ***rbg-Size***Selection between configuration 1 and configuration 2 for RBG size for PUSCH. The UE does not apply this field if *resourceAllocation* is set to *resourceAllocationType1*. Otherwise, the UE applies the value *config1* when the field is absent. Note: *rbg-Size* is used when the *transformPrecoder* parameter is disabled. |
| ***repK-RV***The redundancy version (RV) sequence to use. See TS 38.214 [19], clause 6.1.2. The network configures this field if repetitions are used, i.e., if *repK* is set to *n2*, *n4* or *n8*. This field is not configured when *cg-RetransmissionTimer* is configured. Otherwise, the field is absent. |
| ***repK***Number of repetitions K, see TS 38.214 [19]. If the field *repK-v1710* is present, the UE shall ignore the *repK* (without suffix). |
| ***resourceAllocation***Configuration of resource allocation type 0 and resource allocation type 1. For Type 1 UL data transmission without grant, *resourceAllocation* should be *resourceAllocationType0* or *resourceAllocationType1*. |
| ***rrc-ConfiguredUplinkGrant***Configuration for "configured grant" transmission with fully RRC-configured UL grant (Type1). If this field is absent the UE uses UL grant configured by DCI addressed to CS-RNTI (Type2). |
| ***sequenceOffsetForRV***Configures the RV offset for the starting RV for the first repetition (first actual repetition in PUSCH repetition Type B) towards the second 'SRS resource set' for PUSCH configured in either *srs-ResourceSetToAddModList* or *srs-ResourceSetToAddModListDCI-0-2* with usage 'codebook' or 'noncodebook'. |
| ***srs-ResourceIndicator***Indicates the SRS resource to be used. The network does not configure this for CG-SDT. |
| ***srs-ResourceIndicator2***Indicates the SRS resource to be used for the second SRS resource set. When this field is present, the srs-ResourceIndicator is used for the first SRS resource set. |
| ***startingFromRV0***This field is used to determine the initial transmission occasion of a transport block for a given RV sequence, see TS 38.214 [19], clause 6.1.2.3.1. The network does not configure this field if *cg-RetransmissionTimer-r16* is configured for CG operation. |
| ***timeDomainAllocation, timeDomainAllocation-v1710***Indicates a combination of start symbol and length and PUSCH mapping type, see TS 38.214 [19], clause 6.1.2 and TS 38.212 [17], clause 7.3.1.If the field *timeDomainAllocation-v1710* is present, the UE shall ignore *timeDomainAllocation* field (without suffix). |
| ***timeDomainOffset***Offset related to the reference SFN indicated by *timeReferenceSFN*, see TS 38.321 [3], clause 5.8.2. *timeDomainOffset-r17* is only applicable to 480 kHz and 960 kHz. If *timeDomainOffset-r17* is present, the UE shall ignore *timeDomainOffset* (without suffix). |
| ***timeReferenceSFN***Indicates SFN used for determination of the offset of a resource in time domain. The UE uses the closest SFN with the indicated number preceding the reception of the configured grant configuration, see TS 38.321 [3], clause 5.8.2. If the field *timeReferenceSFN* is not present, the reference SFN is 0. |
| ***transformPrecoder***Enables or disables transform precoding for *type1* and *type2*. If the field is absent, the UE enables or disables transform precoding in accordance with the field *msg3-transformPrecoder* in *RACH-ConfigCommon* from *rach-ConfigCommon* included directly within BWP configuration (i.e., not included in *additionalRACH-ConfigList*), see TS 38.214 [19], clause 6.1.3. |
| ***uci-OnPUSCH***Selection between and configuration of dynamic and semi-static beta-offset. For Type 1 UL data transmission without grant, *uci-OnPUSCH* should be set to *semiStatic.* The network does not configure this for CG-SDT. |

|  |
| --- |
| *CG-COT-Sharing* field descriptions |
| ***channelAccessPriority***Indicates the Channel Access Priority Class that the gNB can assume when sharing the UE initiated COT (see 37.213 [48], clause 4.1.3). |
| ***duration***Indicates the number of DL transmission slots within UE initiated COT (see 37.213 [48], clause 4.1.3). |
| ***offset***Indicates the number of DL transmission slots from the end of the slot where CG-UCI is detected after which COT sharing can be used (see 37.213 [48], clause 4.1.3). |

|  |
| --- |
| *CG-StartingOffsets* field descriptions |
| ***cg-StartingFullBW-InsideCOT***A set of configured grant PUSCH transmission starting offsets (see TS 38.211[16], Table 5.3.1-2) which indicates the length of a CP extension of the first symbol that is located before the configured resource when frequency domain resource allocation includes all interlaces in the allocated RB set(s) and the CG PUSCH resource is inside gNB COT (see TS 38.214 [19], clause 6.1.2.3). |
| ***cg-StartingFullBW-OutsideCOT***A set of configured grant PUSCH transmission starting offset indices (see TS 38.211[16], Table 5.3.1-2) which indicates the length of a CP extension of the first symbol that is located before the configured resource when frequency domain resource allocation includes all interlaces in the allocated RB set(s) and the CG PUSCH resource is outside gNB COT (see TS 38.214 [19], clause 6.1.2.3). |
| ***cg-StartingPartialBW-InsideCOT***A set of configured grant PUSCH transmission starting offset index (see TS 38.211[16], Table 5.3.1-2) which indicates the length of a CP extension of the first symbol that is located before the configured resource when frequency domain resource allocation does not include all interlaces in the allocated RB set(s) and the CG PUSCH resource is inside gNB COT (see TS 38.214 [19], clause 6.1.2.3). |
| ***cg-StartingPartialBW-OutsideCOT***A set of configured grant PUSCH transmission starting offset index (see TS 38.211[16], Table 5.3.1-2) which indicates the length of a CP extension of the first symbol that is located before the configured resource when frequency domain resource allocation does not include all interlaces in the allocated RB set(s) and the CG PUSCH resource is outside gNB COT (see TS 38.214 [19], clause 6.1.2.3). |

|  |
| --- |
| *CG-SDT-Configuration* field descriptions |
| ***cg-SDT-RetransmissionTimer***Indicates the initial value of the configured grant retransmission timer used for the initial transmission of CG-SDT with CCCH message (see TS 38.321 [3]) in multiples of *periodicity*. |
| ***sdt-DMRS-Ports***Indicates the set of DMRS ports for SSB to PUSCH mapping (see TS 38.213 [13]). In case of a RedCap-specific initial downlink BWP that is associated with NCD-SSB, the SSB is the NCD-SSB. Otherwise, the SSB is the CD-SSB. |
| ***sdt-NrofDMRS-Sequences***Indicates the number of DMRS sequences for SSB to PUSCH mapping (see TS 38.213 [13]). In case of a RedCap-specific initial downlink BWP that is associated with NCD-SSB, the SSB is the NCD-SSB. Otherwise, the SSB is the CD-SSB. |
| ***sdt-SSB-Subset***Indicates SSB subset for SSB to CG PUSCH mapping within one CG configuration. If this field is absent, UE assumes the SSB set includes all actually transmitted SSBs. In case of a RedCap-specific initial downlink BWP that is associated with NCD-SSB, the SSB is the NCD-SSB. Otherwise, the SSB is the CD-SSB. |
| ***sdt-SSB-PerCG-PUSCH***The number of SSBs per CG PUSCH (see TS 38.213 [13]). Value *one* corresponds to 1 SSBs per CG PUSCH, value *two* corresponds to 2 SSBs per CG PUSCH and so on. In case of a RedCap-specific initial downlink BWP that is associated with NCD-SSB, the SSB is the NCD-SSB. Otherwise, the SSB is the CD-SSB. |
| ***sdt-P0-PUSCH***Indicates P0 value for PUSCH for CG SDT in steps of 1dB (see TS 38.213 [13]). When this field is configured, the UE ignores the *p0-PUSCH-Alpha*. |
| ***sdt-Alpha***Indicates alpha value for PUSCH for CG SDT. *alpha0* indicates value 0 is used *alpha04* indicates value 4 is used and so on (see TS 38.213 [13]). When this field is configured, the UE ignores the *p0-PUSCH-Alpha*. |

|  |  |
| --- | --- |
| Conditional Presence | Explanation |
| *LCH-BasedPrioritization* | This field is optionally present, Need R, if *lch-BasedPrioritization* is configured in the MAC entity. It is absent otherwise. |
| *RepTypeB* | The field is optionally present if pusch-RepTypeIndicator is set to pusch-RepTypeB, Need S, and absent otherwise. |
| *CG-List* | The field is mandatory present when included in *configuredGrantConfigToAddModList-r16*, otherwise the field is absent. |
| *CG-IndexMAC* | The field is mandatory present if at least one configured grant is configured by *configuredGrantConfigToAddModList-r16* in any BWP of this MAC entity, otherwise it is optionally present, need R. |
| *SRSsets* | This field is mandatory present when UE is configured with two SRS sets configured in either *srs-ResourceSetToAddModList* or *srs-ResourceSetToAddModListDCI-0-2* with usage codebook or non-codebook. Otherwise it is absent, Need R |

#### – *CSI-MeasConfig*

The IE *CSI-MeasConfig* is used to configure CSI-RS (reference signals) belonging to the serving cell in which *CSI-MeasConfig* is included, channel state information reports to be transmitted on PUCCH on the serving cell in which *CSI-MeasConfig* is included and channel state information reports on PUSCH triggered by DCI received on the serving cell in which *CSI-MeasConfig* is included. See also TS 38.214 [19], clause 5.2.

*CSI-MeasConfig* information element

-- ASN1START

-- TAG-CSI-MEASCONFIG-START

CSI-MeasConfig ::= SEQUENCE {

 nzp-CSI-RS-ResourceToAddModList SEQUENCE (SIZE (1..maxNrofNZP-CSI-RS-Resources)) OF NZP-CSI-RS-Resource OPTIONAL, -- Need N

 nzp-CSI-RS-ResourceToReleaseList SEQUENCE (SIZE (1..maxNrofNZP-CSI-RS-Resources)) OF NZP-CSI-RS-ResourceId OPTIONAL, -- Need N

 nzp-CSI-RS-ResourceSetToAddModList SEQUENCE (SIZE (1..maxNrofNZP-CSI-RS-ResourceSets)) OF NZP-CSI-RS-ResourceSet

 OPTIONAL, -- Need N

 nzp-CSI-RS-ResourceSetToReleaseList SEQUENCE (SIZE (1..maxNrofNZP-CSI-RS-ResourceSets)) OF NZP-CSI-RS-ResourceSetId

 OPTIONAL, -- Need N

 csi-IM-ResourceToAddModList SEQUENCE (SIZE (1..maxNrofCSI-IM-Resources)) OF CSI-IM-Resource OPTIONAL, -- Need N

 csi-IM-ResourceToReleaseList SEQUENCE (SIZE (1..maxNrofCSI-IM-Resources)) OF CSI-IM-ResourceId OPTIONAL, -- Need N

 csi-IM-ResourceSetToAddModList SEQUENCE (SIZE (1..maxNrofCSI-IM-ResourceSets)) OF CSI-IM-ResourceSet OPTIONAL, -- Need N

 csi-IM-ResourceSetToReleaseList SEQUENCE (SIZE (1..maxNrofCSI-IM-ResourceSets)) OF CSI-IM-ResourceSetId OPTIONAL, -- Need N

 csi-SSB-ResourceSetToAddModList SEQUENCE (SIZE (1..maxNrofCSI-SSB-ResourceSets)) OF CSI-SSB-ResourceSet OPTIONAL, -- Need N

 csi-SSB-ResourceSetToReleaseList SEQUENCE (SIZE (1..maxNrofCSI-SSB-ResourceSets)) OF CSI-SSB-ResourceSetId OPTIONAL, -- Need N

 csi-ResourceConfigToAddModList SEQUENCE (SIZE (1..maxNrofCSI-ResourceConfigurations)) OF CSI-ResourceConfig

 OPTIONAL, -- Need N

 csi-ResourceConfigToReleaseList SEQUENCE (SIZE (1..maxNrofCSI-ResourceConfigurations)) OF CSI-ResourceConfigId

 OPTIONAL, -- Need N

 csi-ReportConfigToAddModList SEQUENCE (SIZE (1..maxNrofCSI-ReportConfigurations)) OF CSI-ReportConfig OPTIONAL, -- Need N

 csi-ReportConfigToReleaseList SEQUENCE (SIZE (1..maxNrofCSI-ReportConfigurations)) OF CSI-ReportConfigId

 OPTIONAL, -- Need N

 reportTriggerSize INTEGER (0..6) OPTIONAL, -- Need M

 aperiodicTriggerStateList SetupRelease { CSI-AperiodicTriggerStateList } OPTIONAL, -- Need M

 semiPersistentOnPUSCH-TriggerStateList SetupRelease { CSI-SemiPersistentOnPUSCH-TriggerStateList } OPTIONAL, -- Need M

 ...,

 [[

 reportTriggerSizeDCI-0-2-r16 INTEGER (0..6) OPTIONAL -- Need R

 ]],

 [[

 sCellActivationRS-ConfigToAddModList-r17 SEQUENCE (SIZE (1..maxNrofSCellActRS-r17)) OF SCellActivationRS-Config-r17 OPTIONAL, -- Need N

 sCellActivationRS-ConfigToReleaseList-r17 SEQUENCE (SIZE (1..maxNrofSCellActRS-r17)) OF SCellActivationRS-ConfigId-r17 OPTIONAL -- Need N

 ]]

}

-- TAG-CSI-MEASCONFIG-STOP

-- ASN1STOP

|  |
| --- |
| *CSI-MeasConfig* field descriptions |
| ***aperiodicTriggerStateList***Contains trigger states for dynamically selecting one or more aperiodic and semi-persistent reporting configurations and/or triggering one or more aperiodic CSI-RS resource sets for channel and/or interference measurement (see TS 38.214 [19], clause 5.2.1). |
| ***csi-IM-ResourceSetToAddModList***Pool of *CSI-IM-ResourceSet* which can be referred to from *CSI-ResourceConfig* or from MAC CEs. |
| ***csi-IM-ResourceToAddModList***Pool of *CSI-IM-Resource* which can be referred to from *CSI-IM-ResourceSet*. |
| ***csi-ReportConfigToAddModList***Configured CSI report settings as specified in TS 38.214 [19] clause 5.2.1.1. |
| ***csi-ResourceConfigToAddModList***Configured CSI resource settings as specified in TS 38.214 [19] clause 5.2.1.2. |
| ***csi-SSB-ResourceSetToAddModList***Pool of CSI-SSB-ResourceSet which can be referred to from *CSI-ResourceConfig*. |
| ***nzp-CSI-RS-ResourceSetToAddModList***Pool of *NZP-CSI-RS-ResourceSet* which can be referred to from *CSI-ResourceConfig* or from MAC CEs. |
| ***nzp-CSI-RS-ResourceToAddModList***Pool of *NZP-CSI-RS-Resource* which can be referred to from *NZP-CSI-RS-ResourceSet*. |
| ***reportTriggerSize, reportTriggerSizeDCI-0-2***Size of CSI request field in DCI (bits) (see TS 38.214 [19], clause 5.2.1.5.1). The field *reportTriggerSize* applies to DCI format 0\_1 and the field *reportTriggerSizeDCI-0-2* applies to DCI format 0\_2 (see TS 38.214 [19], clause 5.2.1.5.1). |
| ***scellActivationRS-ConfigToAddModList***Configured RS for fast SCell activation as specified in TS 38.214 [19] clause 5.2.1.5.3.. |

– *PDCCH-Config*

The IE *PDCCH-Config* is used to configure UE specific PDCCH parameters or MBS multicast PDCCH parameters such as control resource sets (CORESET), search spaces and additional parameters for acquiring the PDCCH. If this IE is used for the scheduled SCell in case of cross carrier scheduling, the fields other than *searchSpacesToAddModList* and *searchSpacesToReleaseList* are absent. If the IE is used for a dormant BWP, the fields other than *controlResourceSetToAddModList* and *controlResourceSetToReleaseList* are absent. If this IE is used for MBS CFR, the field *downlinkPreemptiom,tpc-PUSCH, tpc-SRS, uplinkCancellation, monitoringCapabilityConfig,* and *searchSpaceSwitchConfig* are absent.

***PDCCH-Config* information element**

-- ASN1START

-- TAG-PDCCH-CONFIG-START

PDCCH-Config ::= SEQUENCE {

 controlResourceSetToAddModList SEQUENCE(SIZE (1..3)) OF ControlResourceSet OPTIONAL, -- Need N

 controlResourceSetToReleaseList SEQUENCE(SIZE (1..3)) OF ControlResourceSetId OPTIONAL, -- Need N

 searchSpacesToAddModList SEQUENCE(SIZE (1..10)) OF SearchSpace OPTIONAL, -- Need N

 searchSpacesToReleaseList SEQUENCE(SIZE (1..10)) OF SearchSpaceId OPTIONAL, -- Need N

 downlinkPreemption SetupRelease { DownlinkPreemption } OPTIONAL, -- Need M

 tpc-PUSCH SetupRelease { PUSCH-TPC-CommandConfig } OPTIONAL, -- Need M

 tpc-PUCCH SetupRelease { PUCCH-TPC-CommandConfig } OPTIONAL, -- Need M

 tpc-SRS SetupRelease { SRS-TPC-CommandConfig} OPTIONAL, -- Need M

 ...,

 [[

 controlResourceSetToAddModListSizeExt-v1610 SEQUENCE (SIZE (1..2)) OF ControlResourceSet OPTIONAL, -- Need N

 controlResourceSetToReleaseListSizeExt-r16 SEQUENCE (SIZE (1..5)) OF ControlResourceSetId-r16 OPTIONAL, -- Need N

 searchSpacesToAddModListExt-r16 SEQUENCE(SIZE (1..10)) OF SearchSpaceExt-r16 OPTIONAL, -- Need N

 uplinkCancellation-r16 SetupRelease { UplinkCancellation-r16 } OPTIONAL, -- Need M

 monitoringCapabilityConfig-r16 ENUMERATED { r15monitoringcapability,r16monitoringcapability } OPTIONAL, -- Need M

 searchSpaceSwitchConfig-r16 SearchSpaceSwitchConfig-r16 OPTIONAL -- Need R

 ]],

 [[

 searchSpacesToAddModListExt-v1700 SEQUENCE(SIZE (1..10)) OF SearchSpaceExt-v1700 OPTIONAL, -- Need N

 monitoringCapabilityConfig-v1710 ENUMERATED { r17monitoringcapability } OPTIONAL, -- Need M

 searchSpaceSwitchConfig-r17 SearchSpaceSwitchConfig-r17 OPTIONAL, -- Need R

 pdcch-SkippingDurationList-r17 SEQUENCE(SIZE (1..3)) OF SCS-SpecificDuration-r17 OPTIONAL -- Need R

 ]]

}

SearchSpaceSwitchConfig-r16 ::= SEQUENCE {

 cellGroupsForSwitchList-r16 SEQUENCE(SIZE (1..4)) OF CellGroupForSwitch-r16 OPTIONAL, -- Need R

 searchSpaceSwitchDelay-r16 INTEGER (10..52) OPTIONAL -- Need R

}

SearchSpaceSwitchConfig-r17 ::= SEQUENCE {

 searchSpaceSwitchTimer-r17 SCS-SpecificDuration-r17 OPTIONAL, -- Need R

 searchSpaceSwitchDelay-r17 INTEGER (10..52) OPTIONAL -- Need R

}

CellGroupForSwitch-r16 ::= SEQUENCE(SIZE (1..16)) OF ServCellIndex

SCS-SpecificDuration-r17 ::= INTEGER (1..166)

-- TAG-PDCCH-CONFIG-STOP

-- ASN1STOP

|  |
| --- |
| ***PDCCH-Config* field descriptions** |
| ***controlResourceSetToAddModList, controlResourceSetToAddModListSizeExt***List of UE specifically configured Control Resource Sets (CORESETs) to be used by the UE. The network restrictions on configuration of CORESETs per DL BWP are specified in TS 38.213 [13], clause 10.1 and TS 38.306 [26]. The UE shall consider entries in *controlResourceSetToAddModList* and in *controlResourceSetToAddModListSizeExt* as a single list, i.e. an entry created using *controlResourceSetToAddModList* can be modified using *controlResourceSetToAddModListSizeExt* (or deleted using *controlResourceSetToReleaseListSizeExt*) and vice-versa. In case network reconfigures control resource set with the same *ControlResourceSetId* as used for *commonControlResourceSet* or *commonControlResourceSetExt* configured via *PDCCH-ConfigCommon* or via *SIB20*, the configuration from *PDCCH-Config* always takes precedence and should not be updated by the UE based on *servingCellConfigCommon* or based on *SIB20*. |
| ***controlResourceSetToReleaseList, controlResourceSetToReleaseListSizeExt***List of UE specifically configured Control Resource Sets (CORESETs) to be released by the UE. This field only applies to CORESETs configured by *controlResourceSetToAddModList* or *controlResourceSetToAddModListSizeExt* and does not release the field *commonControlResourceSet* configured by *PDCCH-ConfigCommon* and *commonControlResourceSetExt* configured by *SIB20*. |
| ***downlinkPreemption***Configuration of downlink preemption indications to be monitored in this cell (see TS 38.213 [13], clause 11.2). |
| ***monitoringCapabilityConfig***Configures either Rel-15 PDCCH monitoring capability, Rel-16 PDCCH monitoring capability or Rel-17 PDCCH monitoring capability for PDCCH monitoring on a serving cell (see TS 38.213 [13], clause 10.1). Value *r15monitoringcapability* enables the Rel-15 monitoring capability, and value *r16monitoringcapability* enables the Rel-16 PDCCH monitoring capability. *r17monitoringcapability* enables the Rel-17 PDCCH multi-slot monitoring capability. For 480 and 960 kHz SCS, only value *r17monitoringcapability* is applicable. |
| ***pdcch-SkippingDurationList***Provides one or more values to derive the skipping duration in unit of slots, as specified in TS 38.213 [13], clause 10.4. The DCI which schedules data indicates which of the values is to be applied (see TS 38.213 [13], clause 10.4). For the 15kHz SCS, for each entry, only the first 26 values are valid and correspond to {1, 2, 3, …, 20, 30, 40, 50, 60, 80, 100}. For the 30kHz SCS, for each entry, only the first 46 values are valid and correspond to {1, 2, 3, …, 40, 60, 80, 100, 120, 160, 200}. For the 60kHz SCS, for each entry, only the first 86 values are valid and correspond to {1, 2, 3, …, 80, 120, 160, 200, 240, 320, 400}. For the 120kHz SCS, for each entry, the 166 values correspond to {1, 2, 3, …, 160, 240, 320, 400, 480, 640, 800}. For the 480kHz SCS, for each entry, the 166 values correspond to {4, 8, 12, …, 640, 960, 1280, 1600, 1920, 2560, 3200}. For the 960kHz SCS, for each entry, the 166 values correspond to {8, 16, 24, …, 1280, 1920, 2560, 3200, 3840, 5120, 6400}. |
| ***searchSpacesToAddModList, searchSpacesToAddModListExt***List of UE specifically configured Search Spaces or MBS multicast Search Spaces. The network configures at most 10 Search Spaces per BWP per cell (including UE-specific and common Search Spaces). If the network includes *searchSpacesToAddModListExt*, it includes the same number of entries, and listed in the same order, as in *searchSpacesToAddModList* in each of them. |
| ***searchSpaceSwitchConfig***Configuration to control the UE behavior to switch from search space group X back to search space group 0, as specified in clause 10 of TS 38.213 [13]. The network only configures either *searchSpaceSwitchConfig-r16* or *searchSpaceSwitchConfig-r17* for a UE. |
| ***tpc-PUCCH***Enable and configure reception of group TPC commands for PUCCH. |
| ***tpc-PUSCH***Enable and configure reception of group TPC commands for PUSCH. |
| ***tpc-SRS***Enable and configure reception of group TPC commands for SRS. |
| ***uplinkCancellation***Configuration of uplink cancellation indications to be monitored in this cell (see TS 38.213 [13], clause 11.2A). |

|  |
| --- |
| ***SearchSpaceSwitchConfig* field descriptions** |
| ***cellGroupsForSwitchList***The list of serving cells which are bundled for the search space group switching purpose (see TS 38.213 [13], clause 10.4). A serving cell can belong to only one *CellGroupForSwitch*. The network configures the same list for all BWPs of serving cells in the same *CellGroupForSwitch.* |
| ***searchSpaceSwitchDelay***Indicates the value to be applied by a UE for Search Space Set Group switching; corresponds to the P value in TS 38.213 [13], clause 10.4. The network configures the same value for all BWPs of serving cells in the same *CellGroupForSwitch.* For 120/480/960 kHz SCS, only values 40,41, ... 52 are valid and the actual value = field value \* SCS/120 kHz i.e. field value 40 corresponds to 40 with 120 kHz SCS, 160 with 480 kHz SCS and 320 with 960 kHz SCS, and so on. |
| ***searchSpaceSwitchTimer***Timer (in unit of slots) to control the UE behavior to switch from search space group X back to search space group 0, as specified in clause 10 of TS 38.213 [13]. For the 15kHz SCS, only the first 26 values are valid and correspond to {1, 2, 3, …, 20, 30, 40, 50, 60, 80, 100}. For the 30kHz SCS, only the first 46 values are valid and correspond to {1, 2, 3, …, 40, 60, 80, 100, 120, 160, 200}. For the 60kHz SCS, only the first 86 values are valid and correspond to {1, 2, 3, …, 80, 120, 160, 200, 240, 320, 400}. For the 120kHz SCS, the 166 values correspond to {1, 2, 3, …, 160, 240, 320, 400, 480, 640, 800}. For the 480kHz SCS, the 166 values correspond to {4, 8, 12, …, 640, 960, 1280, 1600, 1920, 2560, 3200}. For the 960kHz SCS, the 166 values correspond to {8, 16, 24, …, 1280, 1920, 2560, 3200, 3840, 5120, 6400}. |

<Text omitted>

– *SearchSpace*

The IE *SearchSpace* defines how/where to search for PDCCH candidates. Each search space is associated with one *ControlResourceSet*. For a scheduled SCell in the case of cross carrier scheduling, except for *nrofCandidates*, all the optional fields are absent (regardless of their presence conditions). For a scheduled SpCell in the case of the cross carrier scheduling, if the search space is linked to another search space in the scheduling SCell, all the optional fields of this search space in the scheduled SpCell are absent (regardless of their presence conditions) except for *nrofCandidates*.

***SearchSpace* information element**

-- ASN1START

-- TAG-SEARCHSPACE-START

SearchSpace ::= SEQUENCE {

 searchSpaceId SearchSpaceId,

 controlResourceSetId ControlResourceSetId OPTIONAL, -- Cond SetupOnly

 monitoringSlotPeriodicityAndOffset CHOICE {

 sl1 NULL,

 sl2 INTEGER (0..1),

 sl4 INTEGER (0..3),

 sl5 INTEGER (0..4),

 sl8 INTEGER (0..7),

 sl10 INTEGER (0..9),

 sl16 INTEGER (0..15),

 sl20 INTEGER (0..19),

 sl40 INTEGER (0..39),

 sl80 INTEGER (0..79),

 sl160 INTEGER (0..159),

 sl320 INTEGER (0..319),

 sl640 INTEGER (0..639),

 sl1280 INTEGER (0..1279),

 sl2560 INTEGER (0..2559)

 } OPTIONAL, -- Cond Setup4

 duration INTEGER (2..2559) OPTIONAL, -- Need S

 monitoringSymbolsWithinSlot BIT STRING (SIZE (14)) OPTIONAL, -- Cond Setup

 nrofCandidates SEQUENCE {

 aggregationLevel1 ENUMERATED {n0, n1, n2, n3, n4, n5, n6, n8},

 aggregationLevel2 ENUMERATED {n0, n1, n2, n3, n4, n5, n6, n8},

 aggregationLevel4 ENUMERATED {n0, n1, n2, n3, n4, n5, n6, n8},

 aggregationLevel8 ENUMERATED {n0, n1, n2, n3, n4, n5, n6, n8},

 aggregationLevel16 ENUMERATED {n0, n1, n2, n3, n4, n5, n6, n8}

 } OPTIONAL, -- Cond Setup

 searchSpaceType CHOICE {

 common SEQUENCE {

 dci-Format0-0-AndFormat1-0 SEQUENCE {

 ...

 } OPTIONAL, -- Need R

 dci-Format2-0 SEQUENCE {

 nrofCandidates-SFI SEQUENCE {

 aggregationLevel1 ENUMERATED {n1, n2} OPTIONAL, -- Need R

 aggregationLevel2 ENUMERATED {n1, n2} OPTIONAL, -- Need R

 aggregationLevel4 ENUMERATED {n1, n2} OPTIONAL, -- Need R

 aggregationLevel8 ENUMERATED {n1, n2} OPTIONAL, -- Need R

 aggregationLevel16 ENUMERATED {n1, n2} OPTIONAL -- Need R

 },

 ...

 } OPTIONAL, -- Need R

 dci-Format2-1 SEQUENCE {

 ...

 } OPTIONAL, -- Need R

 dci-Format2-2 SEQUENCE {

 ...

 } OPTIONAL, -- Need R

 dci-Format2-3 SEQUENCE {

 dummy1 ENUMERATED {sl1, sl2, sl4, sl5, sl8, sl10, sl16, sl20} OPTIONAL, -- Cond Setup

 dummy2 ENUMERATED {n1, n2},

 ...

 } OPTIONAL -- Need R

 },

 ue-Specific SEQUENCE {

 dci-Formats ENUMERATED {formats0-0-And-1-0, formats0-1-And-1-1},

 ...,

 [[

 dci-Formats-MT-r16 ENUMERATED {formats2-5} OPTIONAL, -- Need R

 dci-FormatsSL-r16 ENUMERATED {formats0-0-And-1-0, formats0-1-And-1-1, formats3-0, formats3-1,

 formats3-0-And-3-1} OPTIONAL, -- Need R

 dci-FormatsExt-r16 ENUMERATED {formats0-2-And-1-2, formats0-1-And-1-1And-0-2-And-1-2}

 OPTIONAL -- Need R

 ]]

 }

 } OPTIONAL -- Cond Setup2

}

SearchSpaceExt-r16 ::= SEQUENCE {

 controlResourceSetId-r16 ControlResourceSetId-r16 OPTIONAL, -- Cond SetupOnly2

 searchSpaceType-r16 SEQUENCE {

 common-r16 SEQUENCE {

 dci-Format2-4-r16 SEQUENCE {

 nrofCandidates-CI-r16 SEQUENCE {

 aggregationLevel1-r16 ENUMERATED {n1, n2} OPTIONAL, -- Need R

 aggregationLevel2-r16 ENUMERATED {n1, n2} OPTIONAL, -- Need R

 aggregationLevel4-r16 ENUMERATED {n1, n2} OPTIONAL, -- Need R

 aggregationLevel8-r16 ENUMERATED {n1, n2} OPTIONAL, -- Need R

 aggregationLevel16-r16 ENUMERATED {n1, n2} OPTIONAL -- Need R

 },

 ...

 } OPTIONAL, -- Need R

 dci-Format2-5-r16 SEQUENCE {

 nrofCandidates-IAB-r16 SEQUENCE {

 aggregationLevel1-r16 ENUMERATED {n1, n2} OPTIONAL, -- Need R

 aggregationLevel2-r16 ENUMERATED {n1, n2} OPTIONAL, -- Need R

 aggregationLevel4-r16 ENUMERATED {n1, n2} OPTIONAL, -- Need R

 aggregationLevel8-r16 ENUMERATED {n1, n2} OPTIONAL, -- Need R

 aggregationLevel16-r16 ENUMERATED {n1, n2} OPTIONAL -- Need R

 },

 ...

 } OPTIONAL, -- Need R

 dci-Format2-6-r16 SEQUENCE {

 ...

 } OPTIONAL, -- Need R

 ...

 }

 } OPTIONAL, -- Cond Setup3

 searchSpaceGroupIdList-r16 SEQUENCE (SIZE (1.. 2)) OF INTEGER (0..1) OPTIONAL, -- Need R

 freqMonitorLocations-r16 BIT STRING (SIZE (5)) OPTIONAL -- Need R

}

SearchSpaceExt-v1700 ::= SEQUENCE {

 monitoringSlotPeriodicityAndOffset-v1710 CHOICE {

 sl32 INTEGER (0..31),

 sl64 INTEGER (0..63),

 sl128 INTEGER (0..127),

 sl5120 INTEGER (0..5119),

 sl10240 INTEGER (0..10239),

 sl20480 INTEGER (0..20479)

 } OPTIONAL, -- Cond Setup5

 monitoringSlotsWithinSlotGroup-r17 CHOICE {

 slotGroupLength4-r17 BIT STRING (SIZE (4)),

 slotGroupLength8-r17 BIT STRING (SIZE (8))

 } OPTIONAL, -- Need R

 duration-r17 INTEGER (4..20476) OPTIONAL, -- Need R

 searchSpaceType-r17 SEQUENCE{

 common-r17 SEQUENCE {

 dci-Format4-0-r17 SEQUENCE {

 ...

 } OPTIONAL, -- Need R

 dci-Format4-1-r17 SEQUENCE {

 ...

 } OPTIONAL, -- Need R

 dci-Format4-2-r17 SEQUENCE {

 ...

 } OPTIONAL, -- Need R

 dci-Format4-1-AndFormat4-2-r17 SEQUENCE {

 ...

 } OPTIONAL, -- Need R

 dci-Format2-7-r17 SEQUENCE {

 nrofCandidates-PEI-r17 SEQUENCE {

 aggregationLevel4-r17 ENUMERATED {n0, n1, n2, n3, n4} OPTIONAL, -- Need R

 aggregationLevel8-r17 ENUMERATED {n0, n1, n2} OPTIONAL, -- Need R

 aggregationLevel16-r17 ENUMERATED {n0, n1} OPTIONAL -- Need R

 },

 ...

 } OPTIONAL -- Need R

 }

 } OPTIONAL, -- Need R

 searchSpaceGroupIdList-r17 SEQUENCE (SIZE (1.. 3)) OF INTEGER (0.. maxNrofSearchSpaceGroups-1-r17) OPTIONAL, -- Cond DedicatedOnly

 searchSpaceLinkingId-r17 INTEGER (0..maxNrofSearchSpacesLinks-1-r17) OPTIONAL -- Cond DedicatedOnly

}

-- TAG-SEARCHSPACE-STOP

-- ASN1STOP

|  |
| --- |
| ***SearchSpace* field descriptions** |
| ***common***Configures this search space as common search space (CSS) and DCI formats to monitor. |
| ***controlResourceSetId***The CORESET applicable for this SearchSpace. Value 0 identifies the common CORESET#0 configured in MIB and in *ServingCellConfigCommon*. Values 1..*maxNrofControlResourceSets-1* identify CORESETs configured in System Information or by dedicated signalling. The CORESETs with *non-zero controlResourceSetId* are configured in the same BWP as this *SearchSpace* except *commonControlResourceSetExt* which is configured by SIB20. If the field *controlResourceSetId-r16* is present, UE shall ignore the *controlResourceSetId* (without suffix). |
| ***dummy1, dummy2***This field is not used in the specification. If received it shall be ignored by the UE. |
| ***dci-Format0-0-AndFormat1-0***If configured, the UE monitors the DCI formats 0\_0 and 1\_0 according to TS 38.213 [13], clause 10.1. |
| ***dci-Format2-0***If configured, UE monitors the DCI format 2\_0 according to TS 38.213 [13], clause 10.1, 11.1.1. |
| ***dci-Format2-1***If configured, UE monitors the DCI format 2\_1 according to TS 38.213 [13], clause 10.1, 11.2. |
| ***dci-Format2-2***If configured, UE monitors the DCI format 2\_2 according to TS 38.213 [13], clause 10.1, 11.3. |
| ***dci-Format2-3***If configured, UE monitors the DCI format 2\_3 according to TS 38.213 [13], clause 10.1, 11.4 |
| ***dci-Format2-4***If configured, UE monitors the DCI format 2\_4 according to TS 38.213 [13], clause 11.2A. |
| ***dci-Format2-5***If configured, IAB-MT monitors the DCI format 2\_5 according to TS 38.213 [13], clause 14. |
| ***dci-Format2-6***If configured, UE monitors the DCI format 2\_6 according to TS 38.213 [13], clause 10.1, 10.3. DCI format 2\_6 can only be configured on the SpCell. |
| ***dci-Format2-7***If configured, UE monitors the DCI format 2\_7 according to TS 38.213 [13], clause 10.1, 10.4A. |
| ***dci-Format4-0***If configured, the UE monitors the DCI format 4\_0 with CRC scrambled by MCCH-RNTI/G-RNTI according to TS 38.213 [13], clause [10.1]. |
| ***dci-Format4-1-AndFormat4-2***If configured, the UE monitors the DCI format 4\_1 and 4\_2 with CRC scrambled by G-RNTI/G-CS-RNTI according to TS 38.213 [13], clause [11.1]. |
| ***dci-Format4-1***If configured, the UE monitors the DCI format 4\_1 with CRC scrambled by G-RNTI/G-CS-RNTI according to TS 38.213 [13], clause [10.1]. |
| ***dci-Format4-2***If configured, the UE monitors the DCI format 4\_2 with CRC scrambled by G-RNTI/G-CS-RNTI according to TS 38.213 [13], clause [10.1]. |
| ***dci-Formats***Indicates whether the UE monitors in this USS for DCI formats 0-0 and 1-0 or for formats 0-1 and 1-1. |
| ***dci-FormatsExt***If this field is present, the field *dci-Formats* is ignored and *dci-FormatsExt* is used instead to indicate whether the UE monitors in this USS for DCI format 0\_2 and 1\_2 or formats 0\_1 and 1\_1 and 0\_2 and 1\_2 (see TS 38.212 [17], clause 7.3.1 and TS 38.213 [13], clause 10.1). This field is not configured for operation with shared spectrum channel access in this release*.* |
| ***dci-Formats-MT***Indicates whether the IAB-MT monitors the DCI formats 2-5 according to TS 38.213 [13], clause 14. |
| ***dci-FormatsSL***Indicates whether the UE monitors in this USS for DCI formats 0-0 and 1-0 or for formats 0-1 and 1-1 or for format 3-0 or for format 3-1 or for formats 3-0 and 3-1. If this field is present, the field *dci-Formats* is ignored and *dci-FormatsSL* is used. |
| ***duration***Number of consecutive slots that a SearchSpace lasts in every occasion, i.e., upon every period as given in the *periodicityAndOffset*. If the field is absent, the UE applies the value 1 slot, except for DCI format 2\_0. The UE ignores this field for DCI format 2\_0. The maximum valid duration is periodicity-1 (periodicity as given in the *monitoringSlotPeriodicityAndOffset*).For SCS 480 kHz and SCS 960 kHz, duration-r17 is used, and the configured duration is restricted to be an integer multiple of L slots and smaller than periodicity, where L is the configured length of the bitmap *monitoringSlotsWithinSlotGroup-r17*. If *duration-r17* is absent, the UE assumes the duration in slots is equal to L. The maximum valid duration is periodicity-L.For IAB-MT, duration indicates number of consecutive slots that a SearchSpace lasts in every occasion, i.e., upon every period as given in the *periodicityAndOffset*. If the field is absent, the IAB-MT applies the value 1 slot, except for DCI format 2\_0 and DCI format 2\_5. The IAB-MT ignores this field for DCI format 2\_0 and DCI format 2\_5. The maximum valid duration is periodicity-1 (periodicity as given in the *monitoringSlotPeriodicityAndOffset*). |
| ***freqMonitorLocations***Defines an association of the search space to multiple monitoring locations in the frequency domain and indicates whether the pattern configured in the associated CORESET is replicated to a specific RB set, see TS 38.213, clause 10.1. Each bit in the bitmap corresponds to one RB set, and the leftmost (most significant) bit corresponds to RB set 0 in the BWP. A bit set to 1 indicates that a frequency domain resource allocation replicated from the pattern configured in the associated CORESET is mapped to the RB set. |
| ***monitoringSlotPeriodicityAndOffset***Slots for PDCCH Monitoring configured as periodicity and offset.For SCS 15, 30, 60, and 120 kHz and if the UE is configured to monitor:- DCI format 2\_1, only the values 'sl1', 'sl2' or 'sl4' are applicable.- DCI format 2\_0, only the values ′sl1′, ′sl2′, ′sl4′, ′sl5′, ′sl8′, ′sl10′, ′sl16′, and ′sl20′ are applicable (see TS 38.213 [13], clause 10).- DCI format 2\_4, only the values 'sl1', 'sl2', 'sl4', 'sl5', 'sl8' and 'sl10' are applicable.For SCS 480 kHz and if the UE is configured to monitor:- DCI format 2\_0, only the values 'sl4', 'sl8', 'sl16', 'sl20', 'sl32', 'sl40', 'sl64', and 'sl80' are applicable.- DCI format 2\_1, only the values ′sl4′, ′sl8′, and ′sl16′ are applicable.- DCI format 2\_4, only the values 'sl4', 'sl8', 'sl16', 'sl20', 'sl32', 'sl40' are applicable.For SCS 960 kHz and if the UE is configured to monitor:- DCI format 2\_0, only the values 'sl8', 'sl16', 'sl32', 'sl40', 'sl64', 'sl80', 'sl128', and 'sl160' are applicable.- DCI format 2\_1, only the values ′sl8′, ′sl16′, and 'sl32' are applicable.- DCI format 2\_4, only the values 'sl8', 'sl16', 'sl32', 'sl40', 'sl64', 'sl80' are applicable.For SCS 480 kHz and SCS 960 kHz, and the configured periodicity and offset are restricted to be an integer multiple of L slots, where L is the configured length of the bitmap provided by *monitoringSlotsWithinSlotGroup-r17*, i.e. for a given periodicity, the offset has a range of {0, L, 2\*L, …, L\*FLOOR(1/L\*(periodicity-1))}.For IAB-MT, If the IAB-MT is configured to monitor DCI format 2\_1, only the values 'sl1', 'sl2' or 'sl4' are applicable. If the IAB-MT is configured to monitor DCI format 2\_0 or DCI format 2\_5, only the values ′sl1′, ′sl2′, ′sl4′, ′sl5′, ′sl8′, ′sl10′, ′sl16′, and ′sl20′ are applicable (see TS 38.213, clause 10).If *monitoringSlotPeriodicityAndOffset-v1710* is present, any previously configured *monitoringSlotPeriodicityAndOffset* is released, and if *monitoringSlotPeriodicityAndOffset* is present, any previously configured *monitoringSlotPeriodicityAndOffset-v1710* is released. |
| ***monitoringSlotsWithinSlotGroup***Indicates which slot(s) within a slot group are configured for multi-slot PDCCH monitoring. The first (leftmost, most significant) bit represents the first slot in the slot group, the second bit represents the second slot in the slot group, and so on. A bit set to '1' indicates that the corresponding slot is configured for multi-slot PDCCH monitoring (see TS 38.213 [13], clause 10). The number of slots for multi-slot PDCCH monitoring is configured according to clause 10 in TS 38.213 [13]. |
| ***monitoringSymbolsWithinSlot***The first symbol(s) for PDCCH monitoring in the slots configured for (multi-slot) PDCCH monitoring (see *monitoringSlotPeriodicityAndOffset* and *duration*). The most significant (left) bit represents the first OFDM in a slot, and the second most significant (left) bit represents the second OFDM symbol in a slot and so on. The bit(s) set to one identify the first OFDM symbol(s) of the control resource set within a slot. If the cyclic prefix of the BWP is set to extended CP, the last two bits within the bit string shall be ignored by the UE or IAB-MT.For DCI format 2\_0, the first one symbol applies if the *duration* of CORESET (in the IE *ControlResourceSet*) identified by *controlResourceSetId* indicates 3 symbols, the first two symbols apply if the *duration* of CORESET identified by *controlResourceSetId* indicates 2 symbols, and the first three symbols apply if the *duration* of CORESET identified by *controlResourceSetId* indicates 1 symbol.See TS 38.213 [13], clause 10.For IAB-MT: For DCI format 2\_0 or DCI format 2\_5, the first one symbol applies if the duration of CORESET (in the IE *ControlResourceSet*) identified by *controlResourceSetId* indicates 3 symbols, the first two symbols apply if the *duration* of CORESET identified by *controlResourceSetId* indicates 2 symbols, and the first three symbols apply if the *duration* of CORESET identified by *controlResourceSetId* indicates 1 symbol.See TS 38.213 [13], clause 10. |
| ***nrofCandidates-CI***The number of PDCCH candidates specifically for format 2-4 for the configured aggregation level. If an aggregation level is absent, the UE does not search for any candidates with that aggregation level. The network configures only one aggregationLevel and the corresponding number of candidates (see TS 38.213 [13], clause 10.1). |
| ***nrofCandidates-PEI***The number of PDCCH candidates specifically for format 2-7 for the configured aggregation level. |
| ***nrofCandidates-SFI***The number of PDCCH candidates specifically for format 2-0 for the configured aggregation level. If an aggregation level is absent, the UE does not search for any candidates with that aggregation level. The network configures only one aggregationLevel and the corresponding number of candidates (see TS 38.213 [13], clause 11.1.1). For a search space configured with *freqMonitorLocations-r16*, only value ′n1′ is valid. |
| ***nrofCandidates***Number of PDCCH candidates per aggregation level. The number of candidates and aggregation levels configured here applies to all formats unless a particular value is specified or a format-specific value is provided (see inside *searchSpaceType*). If configured in the *SearchSpace* of a cross carrier scheduled cell, this field determines the number of candidates and aggregation levels to be used on the linked scheduling cell (see TS 38.213 [13], clause 10). |
| ***searchSpaceGroupIdList-r16, searchSpaceGroupIdList-r17***List of search space group IDs which the search space is associated with. The network configures at most 2 search space groups per BWP where the group ID is either 0 or 1 if *searchSpaceGroupIdList-r16* is included. The network configures at most 3 search space groups per BWP where the group ID is either 0, 1 or 2 if *searchSpaceGroupIdList-r17* is included. And if *searchSpaceGroupIdList-r17* is included, *searchSpaceGroupIdList-r16* is ignored. |
| ***searchSpaceId***Identity of the search space. SearchSpaceId = 0 identifies the *searchSpaceZero* configured via PBCH (MIB) or *ServingCellConfigCommon* and may hence not be used in the *SearchSpace* IE. The *searchSpaceId* is unique among the BWPs of a Serving Cell. In case of cross carrier scheduling, search spaces with the same *searchSpaceId* in scheduled cell and scheduling cell are linked to each other. The UE applies the search space for the scheduled cell only if the DL BWPs in which the linked search spaces are configured in scheduling cell and scheduled cell are both active.For an IAB-MT, the search space defines how/where to search for PDCCH candidates for an IAB-MT where each search space is associated with one ControlResearchSet and for a scheduled cell in the case of cross carrier scheduling, except for nrofCandidates, all the optional fields are absent. |
| ***SearchSpaceLinkingId***This parameter is used to link two search spaces of same type in the same BWP. If two search spaces have the same SearchSpaceLinkingId UE assumes these search spaces are linked to PDCCH repetition REF. When PDCCH repetition is monitored in two linked search space (SS) sets, the UE does not expect a third monitored SS set to be linked with any of the two linked SS sets. The two linked SS sets have the same SS set type (USS/CSS). The two linked SS sets have the same DCI formats to monitor. For intra-slot PDCCH repetition: The two SS sets should have the same periodicity and offset (monitoringSlotPeriodicityAndOffset), and the same duration. For linking monitoring occasions across the two SS sets that exist in the same slot: The two SS sets have the same number of monitoring occasions within a slot and n-th monitoring occasion of one SS set is linked to n-th monitoring occasion of the other SS set. The following SS sets cannot be linked with another SS set for PDCCH repetition: SS set 0, *searchSpaceSIB1*, *searchSpaceOtherSystemInformation*, *pagingSearchSpace*, *ra-SearchSpace*, *searchSpaceMCCH*, *searchSpaceMTCH*, *peiSearchSpace*, and *sdt-SearchSpace*. SS set configured by *recoverySearchSpaceId* cannot be linked to another SS set for PDCCH repetition. When a scheduled serving cell is configured to be cross-carrier scheduled by a scheduling serving cell, two PDCCH candidates (with the same AL and candidate index associated with the scheduled serving cell) are linked only if the corresponding two SS sets in the scheduling serving cell are linked and two SS sets in the scheduled serving cell with the same SS set IDs are also linked.This parameter is not applicable to search space configured with *dci-FormatsSL* for monitoring format 3-0 or format 3-1 or for monitoring formats 3-0 and format 3-1. |
| ***searchSpaceType***Indicates whether this is a common search space (present) or a UE specific search space as well as DCI formats to monitor for. |
| ***ue-Specific***Configures this search space as UE specific search space (USS). The UE monitors the DCI format with CRC scrambled by C-RNTI, CS-RNTI (if configured), and SP-CSI-RNTI (if configured) |

|  |  |
| --- | --- |
| **Conditional Presence** | **Explanation** |
| *DedicatedOnly* | In PDCCH-Config, the field is optionally present, Need R. Otherwise it is absent, Need R. |
| *Setup* | This field is mandatory present upon creation of a new *SearchSpace*. It is optionally present, Need M, otherwise. |
| *Setup2* | This field is mandatory present when a new *SearchSpace* is set up, if the same *SearchSpace* ID is not included in *searchSpacesToAddModListExt-r16* of the parent IE with the field *searchSpaceType-r16* or *searchSpaceType-r17* included. Otherwise it is optionally present, Need M. |
| *Setup3* | This field is mandatory present when a new *SearchSpace* is set up, if the same *SearchSpace* ID is not included in *searchSpacesToAddModListExt* (without suffix) of the parent IE with the field *searchSpaceType* (without suffix) included. Otherwise it is optionally present, Need M. |
| *Setup4* | This field is mandatory present upon creation of a new *SearchSpace* if *monitoringSlotPeriodicityAndOffset-v1710* is not included. It is optionally present, Need M, otherwise. |
| *Setup5* | This field is mandatory present upon creation of a new *SearchSpace* if *monitoringSlotPeriodicityAndOffset* (without suffix) is not included. It is optionally present, Need M, otherwise. |
| *SetupOnly* | This field is mandatory present upon creation of a new *SearchSpace*. It is absent, Need M, otherwise. |
| *SetupOnly2* | In PDCCH-Config, the field is optionally present upon creation of a new SearchSpace and absent, Need M upon reconfiguration of an existing SearchSpace.In PDCCH-ConfigCommon, the field is absent. |

<Text omitted>

– *SemiStaticChannelAccessConfig*

The IE *SemiStaticChannelAccessConfig* is used to configure channel access parameters when the network is operating in semi-static channel access mode (see clause 4.3 in TS 37.213 [48].

***SemiStaticChannelAccessConfig* information element**

-- ASN1START

-- TAG-SEMISTATICCHANNELACCESSCONFIG-START

SemiStaticChannelAccessConfig-r16 ::= SEQUENCE {

 period-r16 ENUMERATED {ms1, ms2, ms2dot5, ms4, ms5, ms10}

}

-- TAG-SEMISTATICCHANNELACCESSCONFIG-STOP

-- ASN1STOP

|  |
| --- |
| ***SemiStaticChannelAccessConfig* field descriptions** |
| ***period***Indicates the periodicity of the semi-static channel access mode (see TS 37.213 [48], clause 4.3). Value ms1 corresponds to 1 ms, value ms2 corresponds to 2 ms, value ms2dot5 corresponds to 2.5 ms, and so on. |

<Text omitted>

– *ServingCellConfig*

The IE *ServingCellConfig* is used to configure (add or modify) the UE with a serving cell, which may be the SpCell or an SCell of an MCG or SCG. The parameters herein are mostly UE specific but partly also cell specific (e.g. in additionally configured bandwidth parts). Reconfiguration between a PUCCH and PUCCHless SCell is only supported using an SCell release and add.

***ServingCellConfig* information element**

-- ASN1START

-- TAG-SERVINGCELLCONFIG-START

ServingCellConfig ::= SEQUENCE {

 tdd-UL-DL-ConfigurationDedicated TDD-UL-DL-ConfigDedicated OPTIONAL, -- Cond TDD

 initialDownlinkBWP BWP-DownlinkDedicated OPTIONAL, -- Need M

 downlinkBWP-ToReleaseList SEQUENCE (SIZE (1..maxNrofBWPs)) OF BWP-Id OPTIONAL, -- Need N

 downlinkBWP-ToAddModList SEQUENCE (SIZE (1..maxNrofBWPs)) OF BWP-Downlink OPTIONAL, -- Need N

 firstActiveDownlinkBWP-Id BWP-Id OPTIONAL, -- Cond SyncAndCellAdd

 bwp-InactivityTimer ENUMERATED {ms2, ms3, ms4, ms5, ms6, ms8, ms10, ms20, ms30,

 ms40,ms50, ms60, ms80,ms100, ms200,ms300, ms500,

 ms750, ms1280, ms1920, ms2560, spare10, spare9, spare8,

 spare7, spare6, spare5, spare4, spare3, spare2, spare1 } OPTIONAL, --Need R

 defaultDownlinkBWP-Id BWP-Id OPTIONAL, -- Need S

 uplinkConfig UplinkConfig OPTIONAL, -- Need M

 supplementaryUplink UplinkConfig OPTIONAL, -- Need M

 pdcch-ServingCellConfig SetupRelease { PDCCH-ServingCellConfig } OPTIONAL, -- Need M

 pdsch-ServingCellConfig SetupRelease { PDSCH-ServingCellConfig } OPTIONAL, -- Need M

 csi-MeasConfig SetupRelease { CSI-MeasConfig } OPTIONAL, -- Need M

 sCellDeactivationTimer ENUMERATED {ms20, ms40, ms80, ms160, ms200, ms240,

 ms320, ms400, ms480, ms520, ms640, ms720,

 ms840, ms1280, spare2,spare1} OPTIONAL, -- Cond ServingCellWithoutPUCCH

 crossCarrierSchedulingConfig CrossCarrierSchedulingConfig OPTIONAL, -- Need M

 tag-Id TAG-Id,

 dummy1 ENUMERATED {enabled} OPTIONAL, -- Need R

 pathlossReferenceLinking ENUMERATED {spCell, sCell} OPTIONAL, -- Cond SCellOnly

 servingCellMO MeasObjectId OPTIONAL, -- Cond MeasObject

 ...,

 [[

 lte-CRS-ToMatchAround SetupRelease { RateMatchPatternLTE-CRS } OPTIONAL, -- Need M

 rateMatchPatternToAddModList SEQUENCE (SIZE (1..maxNrofRateMatchPatterns)) OF RateMatchPattern OPTIONAL, -- Need N

 rateMatchPatternToReleaseList SEQUENCE (SIZE (1..maxNrofRateMatchPatterns)) OF RateMatchPatternId OPTIONAL, -- Need N

 downlinkChannelBW-PerSCS-List SEQUENCE (SIZE (1..maxSCSs)) OF SCS-SpecificCarrier OPTIONAL -- Need S

 ]],

 [[

 supplementaryUplinkRelease-r16 ENUMERATED {true} OPTIONAL, -- Need N

 tdd-UL-DL-ConfigurationDedicated-IAB-MT-r16 TDD-UL-DL-ConfigDedicated-IAB-MT-r16 OPTIONAL, -- Cond TDD\_IAB

 dormantBWP-Config-r16 SetupRelease { DormantBWP-Config-r16 } OPTIONAL, -- Need M

 ca-SlotOffset-r16 CHOICE {

 refSCS15kHz INTEGER (-2..2),

 refSCS30KHz INTEGER (-5..5),

 refSCS60KHz INTEGER (-10..10),

 refSCS120KHz INTEGER (-20..20)

 } OPTIONAL, -- Cond AsyncCA

 dummy2 SetupRelease { DummyJ } OPTIONAL, -- Need M

 intraCellGuardBandsDL-List-r16 SEQUENCE (SIZE (1..maxSCSs)) OF IntraCellGuardBandsPerSCS-r16 OPTIONAL, -- Need S

 intraCellGuardBandsUL-List-r16 SEQUENCE (SIZE (1..maxSCSs)) OF IntraCellGuardBandsPerSCS-r16 OPTIONAL, -- Need S

 csi-RS-ValidationWithDCI-r16 ENUMERATED {enabled} OPTIONAL, -- Need R

 lte-CRS-PatternList1-r16 SetupRelease { LTE-CRS-PatternList-r16 } OPTIONAL, -- Need M

 lte-CRS-PatternList2-r16 SetupRelease { LTE-CRS-PatternList-r16 } OPTIONAL, -- Need M

 crs-RateMatch-PerCORESETPoolIndex-r16 ENUMERATED {enabled} OPTIONAL, -- Need R

 enableTwoDefaultTCI-States-r16 ENUMERATED {enabled} OPTIONAL, -- Need R

 enableDefaultTCI-StatePerCoresetPoolIndex-r16 ENUMERATED {enabled} OPTIONAL, -- Need R

 enableBeamSwitchTiming-r16 ENUMERATED {true} OPTIONAL, -- Need R

 cbg-TxDiffTBsProcessingType1-r16 ENUMERATED {enabled} OPTIONAL, -- Need R

 cbg-TxDiffTBsProcessingType2-r16 ENUMERATED {enabled} OPTIONAL -- Need R

 ]],

 [[

 directionalCollisionHandling-r16 ENUMERATED {enabled} OPTIONAL, -- Need R

 channelAccessConfig-r16 SetupRelease { ChannelAccessConfig-r16 } OPTIONAL -- Need M

 ]],

 [[

 nr-dl-PRS-PDC-Info-r17 SetupRelease {NR-DL-PRS-PDC-Info-r17} OPTIONAL, -- Need M

 semiStaticChannelAccessConfigUE-r17 SetupRelease {SemiStaticChannelAccessConfigUE-r17} OPTIONAL, -- Need M

 mimoParam-r17 SetupRelease {MIMOParam-r17} OPTIONAL, -- Need M

 channelAccessMode2-r17 ENUMERATED {enabled} OPTIONAL, -- Need R

 timeDomainHARQ-BundlingType1-r17 ENUMERATED {enabled} OPTIONAL, -- Need R

 nrofHARQ-BundlingGroups-r17 ENUMERATED {n1, n2, n4} OPTIONAL, -- Need R

 fdmed-ReceptionMulticast-r17 ENUMERATED {true} OPTIONAL, -- Need R

 moreThanOneNackOnlyMode-r17 ENUMERATED {mode2} OPTIONAL, -- Need S

 tci-ActivatedConfig-r17 TCI-ActivatedConfig-r17 OPTIONAL, -- Cond TCI\_ActivatedConfig

 directionalCollisionHandling-DC-r17 ENUMERATED {enabled} OPTIONAL, -- Need R

 lte-NeighCellsCRS-AssistInfoList-r17 SetupRelease { LTE-NeighCellsCRS-AssistInfoList-r17 } OPTIONAL -- Need M

 ]],

 [[

 lte-NeighCellsCRS-Assumptions-r17 ENUMERATED {false} OPTIONAL -- Need R

 ]]

}

UplinkConfig ::= SEQUENCE {

 initialUplinkBWP BWP-UplinkDedicated OPTIONAL, -- Need M

 uplinkBWP-ToReleaseList SEQUENCE (SIZE (1..maxNrofBWPs)) OF BWP-Id OPTIONAL, -- Need N

 uplinkBWP-ToAddModList SEQUENCE (SIZE (1..maxNrofBWPs)) OF BWP-Uplink OPTIONAL, -- Need N

 firstActiveUplinkBWP-Id BWP-Id OPTIONAL, -- Cond SyncAndCellAdd

 pusch-ServingCellConfig SetupRelease { PUSCH-ServingCellConfig } OPTIONAL, -- Need M

 carrierSwitching SetupRelease { SRS-CarrierSwitching } OPTIONAL, -- Need M

 ...,

 [[

 powerBoostPi2BPSK BOOLEAN OPTIONAL, -- Need M

 uplinkChannelBW-PerSCS-List SEQUENCE (SIZE (1..maxSCSs)) OF SCS-SpecificCarrier OPTIONAL -- Need S

 ]],

 [[

 enablePL-RS-UpdateForPUSCH-SRS-r16 ENUMERATED {enabled} OPTIONAL, -- Need R

 enableDefaultBeamPL-ForPUSCH0-0-r16 ENUMERATED {enabled} OPTIONAL, -- Need R

 enableDefaultBeamPL-ForPUCCH-r16 ENUMERATED {enabled} OPTIONAL, -- Need R

 enableDefaultBeamPL-ForSRS-r16 ENUMERATED {enabled} OPTIONAL, -- Need R

 uplinkTxSwitching-r16 SetupRelease { UplinkTxSwitching-r16 } OPTIONAL, -- Need M

 mpr-PowerBoost-FR2-r16 ENUMERATED {true} OPTIONAL -- Need R

 ]]

}

DummyJ ::= SEQUENCE {

 maxEnergyDetectionThreshold-r16 INTEGER(-85..-52),

 energyDetectionThresholdOffset-r16 INTEGER (-20..-13),

 ul-toDL-COT-SharingED-Threshold-r16 INTEGER (-85..-52) OPTIONAL, -- Need R

 absenceOfAnyOtherTechnology-r16 ENUMERATED {true} OPTIONAL -- Need R

}

ChannelAccessConfig-r16 ::= SEQUENCE {

 energyDetectionConfig-r16 CHOICE {

 maxEnergyDetectionThreshold-r16 INTEGER (-85..-52),

 energyDetectionThresholdOffset-r16 INTEGER (-13..20)

 } OPTIONAL, -- Need R

 ul-toDL-COT-SharingED-Threshold-r16 INTEGER (-85..-52) OPTIONAL, -- Need R

 absenceOfAnyOtherTechnology-r16 ENUMERATED {true} OPTIONAL -- Need R

}

IntraCellGuardBandsPerSCS-r16 ::= SEQUENCE {

 guardBandSCS-r16 SubcarrierSpacing,

 intraCellGuardBands-r16 SEQUENCE (SIZE (1..4)) OF GuardBand-r16

}

GuardBand-r16 ::= SEQUENCE {

 startCRB-r16 INTEGER (0..274),

 nrofCRBs-r16 INTEGER (0..15)

}

DormancyGroupID-r16 ::= INTEGER (0..4)

DormantBWP-Config-r16::= SEQUENCE {

 dormantBWP-Id-r16 BWP-Id OPTIONAL, -- Need M

 withinActiveTimeConfig-r16 SetupRelease { WithinActiveTimeConfig-r16 } OPTIONAL, -- Need M

 outsideActiveTimeConfig-r16 SetupRelease { OutsideActiveTimeConfig-r16 } OPTIONAL -- Need M

}

WithinActiveTimeConfig-r16 ::= SEQUENCE {

 firstWithinActiveTimeBWP-Id-r16 BWP-Id OPTIONAL, -- Need M

 dormancyGroupWithinActiveTime-r16 DormancyGroupID-r16 OPTIONAL -- Need R

}

OutsideActiveTimeConfig-r16 ::= SEQUENCE {

 firstOutsideActiveTimeBWP-Id-r16 BWP-Id OPTIONAL, -- Need M

 dormancyGroupOutsideActiveTime-r16 DormancyGroupID-r16 OPTIONAL -- Need R

}

UplinkTxSwitching-r16 ::= SEQUENCE {

 uplinkTxSwitchingPeriodLocation-r16 BOOLEAN,

 uplinkTxSwitchingCarrier-r16 ENUMERATED {carrier1, carrier2}

}

MIMOParam-r17 ::= SEQUENCE {

 additionalPCI-ToAddModList-r17 SEQUENCE (SIZE(1..maxNrofAdditionalPCI-r17)) OF SSB-MTC-AdditionalPCI-r17 OPTIONAL, -- Need N

 additionalPCI-ToReleaseList-r17 SEQUENCE (SIZE(1..maxNrofAdditionalPCI-r17)) OF AdditionalPCIIndex-r17 OPTIONAL, -- Need N

 unifiedTCI-StateType-r17 ENUMERATED {separate, joint} OPTIONAL, -- Need R

 uplink-PowerControlToAddModList-r17 SEQUENCE (SIZE (1..maxUL-TCI-r17)) OF Uplink-powerControl-r17 OPTIONAL, -- Need N

 uplink-PowerControlToReleaseList-r17 SEQUENCE (SIZE (1..maxUL-TCI-r17)) OF Uplink-powerControlId-r17 OPTIONAL, -- Need N

 sfnSchemePDCCH-r17 ENUMERATED {sfnSchemeA,sfnSchemeB} OPTIONAL, -- Need R

 sfnSchemePDSCH-r17 ENUMERATED {sfnSchemeA,sfnSchemeB} OPTIONAL -- Need R

}

-- TAG-SERVINGCELLCONFIG-STOP

-- ASN1STOP

|  |
| --- |
| ***ChannelAccessConfig* field descriptions** |
| ***absenceOfAnyOtherTechnology***Presence of this field indicates absence on a long term basis (e.g. by level of regulation) of any other technology sharing the carrier; absence of this field indicates the potential presence of any other technology sharing the carrier, as specified in TS 37.213 [48] clauses 4.2.1 and 4.2.3. |
| ***energyDetectionConfig***Indicates whether to use the *maxEnergyDetectionThreshold* or the *energyDetectionThresholdOffset* (see TS 37.213 [48], clause 4.2.3)*.* |
| ***energyDetectionThresholdOffset***Indicates the offset to the default maximum energy detection threshold value. Unit in dB. Value -13 corresponds to -13dB, value -12 corresponds to -12dB, and so on (i.e. in steps of 1dB) as specified in TS 37.213 [48], clause 4.2.3. |
| ***maxEnergyDetectionThreshold***Indicates the absolute maximum energy detection threshold value. Unit in dBm. Value -85 corresponds to -85 dBm, value -84 corresponds to -84 dBm, and so on (i.e. in steps of 1dBm) as specified in TS 37.213 [48], clause 4.2.3. |
| ***ul-toDL-COT-SharingED-Threshold***Maximum energy detection threshold that the UE should use to share channel occupancy with gNB for DL transmission as specified in TS 37.213 [48], clause 4.1.3 for downlink channel access and clause 4.2.3 for uplink channel access. This field is not applicable in semi-static channel access mode. |

|  |
| --- |
| ***ServingCellConfig* field descriptions** |
| ***additionalPCI-ToAddModList***List of information for the additional SSB with different PCI than the serving cell PCI. The additional SSBs with different PCIs are not used for serving cell quality derivation. |
| ***bwp-InactivityTimer***The duration in ms after which the UE falls back to the default Bandwidth Part (see TS 38.321 [3], clause 5.15). When the network releases the timer configuration, the UE stops the timer without switching to the default BWP. |
| ***ca-SlotOffset***Slot offset between the primary cell (PCell/PSCell) and the SCell in unaligned frame boundary with slot alignment and partial SFN alignment inter-band CA. Based on this field, the UE determines the time offset of the SCell as specified in clause 4.5 of TS 38.211 [16]. The granularity of this field is determined by the reference SCS for the slot offset (i.e. the maximum of PCell/PSCell lowest SCS among all the configured SCSs in DL/UL *SCS-SpecificCarrierList* in *ServingCellConfigCommon* or *ServingCellConfigCommonSIB* and this serving cell's lowest SCS among all the configured SCSs in DL/UL *SCS-SpecificCarrierList* in *ServingCellConfigCommon* or *ServingCellConfigCommonSIB*).The Network configures at most single non-zero offset duration in ms (independent on SCS) among CCs in the unaligned CA configuration. If the field is absent, the UE applies the value of 0. The slot offset value can only be changed with SCell release and add. |
| ***cbg-TxDiffTBsProcessingType1, cbg-TxDiffTBsProcessingType2***Indicates whether processing types 1 and 2 based CBG based operation is enabled according to Rel-16 UE capabilities. |
| ***channelAccessConfig***List of parameters used for access procedures of operation with shared spectrum channel access (see TS 37.213 [48). |
| ***channelAccessMode2***If present, this field indicates that the UE shall apply channel access procedures for operation with shared spectrum channel access in accordance with TS 37.213 [48], clause 4.4 for FR2-2. If absent, the UE does not apply these channel access procedures. The network always configures this field if channel access procedures are required for the serving cell within this region by regulations.Overwrites the corresponding field in *ServingCellConfigCommon* or *ServingCellConfigCommonSIB* for this serving cell. |
| ***crossCarrierSchedulingConfig***Indicates whether this serving cell is cross-carrier scheduled by another serving cell or whether it cross-carrier schedules another serving cell. If the field *other* is configured for an SpCell (i.e., the SpCell is cross-carrier scheduled by another serving cell), the SpCell can be additionally scheduled by the PDCCH on the SpCell. |
| ***crs-RateMatch-PerCORESETPoolIndex***Indicates how UE performs rate matching when both lte-CRS-PatternList1-r16 and lte-CRS-PatternList2-r16 are configured as specified in TS 38.214 [19], clause 5.1.4.2. |
| ***csi-RS-ValidationWithDCI***Indicates how the UE performs periodic and semi-persistent CSI-RS reception in a slot. The presence of this field indicates that the UE uses DCI detection to validate whether to receive CSI-RS (see TS 38.213 [13], clause 11.1). |
| ***defaultDownlinkBWP-Id***The initial bandwidth part is referred to by BWP-Id = 0. ID of the downlink bandwidth part to be used upon expiry of the BWP inactivity timer. This field is UE specific. When the field is absent the UE uses the initial BWP as default BWP. (see TS 38.213 [13], clause 12 and TS 38.321 [3], clause 5.15). |
| ***directionalCollisionHandling***Indicates that this serving cell is using directional collision handling between a reference and other cell(s) for half-duplex operation in TDD CA with same SCS as specified in TS 38.213 [13], clause 11.1. The half-duplex operation only applies within the same frequency range and cell group.The network only configures this field for TDD serving cells that are using the same SCS. |
| ***directionalCollisionHandling-DC***For the IAB-MT, it indicates that this serving cell is using directional collision handling between a reference and other cell(s) for half-duplex operation in TDD NR-DC with same SCS within same cell group or cross different cell groups. |
| ***dormantBWP-Config***The dormant BWP configuration for an SCell. This field can be configured only for a (non-PUCCH) SCell. |
| ***downlinkBWP-ToAddModList***List of additional downlink bandwidth parts to be added or modified. (see TS 38.213 [13], clause 12). |
| ***downlinkBWP-ToReleaseList***List of additional downlink bandwidth parts to be released. (see TS 38.213 [13], clause 12). |
| ***downlinkChannelBW-PerSCS-List***A set of UE specific channel bandwidth and location configurations for different subcarrier spacings (numerologies). Defined in relation to Point A. The UE uses the configuration provided in this field only for the purpose of channel bandwidth and location determination. If absent, UE uses the configuration indicated in *scs-SpecificCarrierList* in *DownlinkConfigCommon* / *DownlinkConfigCommonSIB*. Network only configures channel bandwidth that corresponds to the channel bandwidth values defined in TS 38.101-1 [15] and TS 38.101-2 [39]. |
| ***dummy1, dummy 2***This field is not used in the specification. If received it shall be ignored by the UE. |
| ***enableBeamSwitchTiming***Indicates the aperiodic CSI-RS triggering with beam switching triggering behaviour as defined in clause 5.2.1.5.1 of TS 38.214 [19]. |
| ***enableDefaultTCI-StatePerCoresetPoolIndex***Presence of this field indicates the UE shall follow the release 16 behavior of default TCI state per CORESETPoolindex when the UE is configured by higher layer parameter PDCCH-Config that contains two different values of CORESETPoolIndex in ControlResourceSet is enabled. |
| ***enableTwoDefaultTCI-States***Presence of this field indicates the UE shall follow the release 16 behavior of two default TCI states for PDSCH when at least one TCI codepoint is mapped to two TCI states is enabled |
| ***fdmed-ReceptionMulticast***Indicates the Type-1 HARQ codebook generation as specified in TS 38.213 [13], clause 9.1.2.1. |
| ***firstActiveDownlinkBWP-Id***If configured for an SpCell, this field contains the ID of the DL BWP to be activated or to be used for RLM, BFD and measurements if included in an *RRCReconfiguration* message contained in an NR or E-UTRA RRC message indicating that the SCG is deactivated, upon performing the RRC (re-)configuration. If the field is absent, the RRC (re-)configuration does not impose a BWP switch. If the field is absent for the PSCell at SCG deactivation, the UE considers the previously activated DL BWP as the BWP to be used for RLM, BFD and measurements. If the field is absent for the PSCell at SCG activation, the DL BWP to be activated is the DL BWP previously to be used for RLM, BFD and measurements.If configured for an SCell, this field contains the ID of the downlink bandwidth part to be used upon activation of an SCell. The initial bandwidth part is referred to by BWP-Id = 0.Upon reconfiguration with *reconfigurationWithSync*, the network sets the *firstActiveDownlinkBWP-Id* and *firstActiveUplinkBWP-Id* to the same value. |
| ***initialDownlinkBWP***The dedicated (UE-specific) configuration for the initial downlink bandwidth-part (i.e., DL BWP#0). If any of the optional IEs are configured within this IE, the UE considers the BWP#0 to be an RRC configured BWP (from UE capability viewpoint). Otherwise, the UE does not consider the BWP#0 as an RRC configured BWP (from UE capability viewpoint). Network always configures the UE with a value for this field if no other BWPs are configured. NOTE1 |
| ***intraCellGuardBandsDL-List, intraCellGuardBandsUL-List***List of intra-cell guard bands in a serving cell for operation with shared spectrum channel access in FR1. If not configured, the guard bands are defined according to 38.101-1 [15], see TS 38.214 [19], clause 7. For operation in licensed spectrum, this field is absent, and no UE action is required. |
| ***lte-CRS-PatternList1***A list of LTE CRS patterns around which the UE shall do rate matching for PDSCH. The LTE CRS patterns in this list shall be non-overlapping in frequency. The network does not configure this field and *lte-CRS-ToMatchAround* simultaneously. |
| ***lte-CRS-PatternList2***A list of LTE CRS patterns around which the UE shall do rate matching for PDSCH scheduled with a DCI detected on a CORESET with CORESETPoolIndex configured with 1. This list is configured only if CORESETPoolIndex configured with 1. The first LTE CRS pattern in this list shall be fully overlapping in frequency with the first LTE CRS pattern in lte-CRS-PatternList1, The second LTE CRS pattern in this list shall be fully overlapping in frequency with the second LTE CRS pattern in lte-CRS-PatternList1, and so on. Network configures this field only if the field *lte-CRS-ToMatchAround* is not configured and there is at least one ControlResourceSet in one DL BWP of this serving cell with *coresetPoolIndex* set to 1. |
| ***lte-CRS-ToMatchAround***Parameters to determine an LTE CRS pattern that the UE shall rate match around. |
| ***lte-NeighCellsCRS-AssistInfoList***A list of LTE neighbour cells configuration information which is used to assist the UE to perform CRS interference mitigation (CRS-IM) in scenarios with overlapping spectrum for LTE and NR (see TS 38.101-4 [59]). If the field is included, it replaces any previous list, i.e. all the entries of the list are replaced and each of the *LTE-NeighCellsCRS-AssistInfo* entries is considered to be newly created and the conditions and Need codes for setup of the entry apply. |
| ***lte-NeighCellsCRS-Assumptions***If the field is not configured, the following default network configuration assumptions are valid for all LTE neighbour cells for the purpose of CRS interference mitigation (CRS-IM) in scenarios with overlapping spectrum for LTE and NR (see TS 38.101-4 [59]).- The CRS port number is the same as the one indicated in *RateMatchPatternLTE-CRS* if configured for the serving cell.- The CRS port number is 4 if *RateMatchPatternLTE-CRS* is not configured for the serving cell.- The channel bandwidth and centre frequency are the same as the ones indicated in *RateMatchPatternLTE-CRS* if configured for the serving cell.- The MBSFN configuration is the same as the one indicated in *RateMatchPatternLTE-CRS* if configured for the serving cell. If *RateMatchPatternLTE-CRS* is not configured for the serving cell, MBSFN subframe is not configured.- Network-based CRS interference mitigation (i.e., CRS muting), as in *crs-IntfMitigConfig* specified in TS 36.331 [10], is not enabled.If the field is configured (i.e. false) and *LTE-NeighCellsCRS-AssistInfoList* is configured, the configuration provided in *LTE-NeighCellsCRS-AssistInfoList* overrides the default network configuration assumptions.If the field is configured (i.e. false) and *LTE-NeighCellsCRS-AssistInfoList* is not configured, it is up to the UE implementation whether to apply CRS-IM operation. |
| ***nr-dl-PRS-PDC-Info***Configures the DL PRS for propagation delay compensation. When configured, the UE measures the UE Rx-Tx time difference based on the reference signals configured in this field. |
| ***nrofHARQ-BundlingGroups***Indicates the number of HARQ bundling groups for type2 HARQ-ACK codebook. |
| ***pathlossReferenceLinking***Indicates whether UE shall apply as pathloss reference either the downlink of SpCell (PCell for MCG or PSCell for SCG) or of SCell that corresponds with this uplink (see TS 38.213 [13], clause 7). |
| ***pdsch-ServingCellConfig***PDSCH related parameters that are not BWP-specific. |
| ***rateMatchPatternToAddModList***Resources patterns which the UE should rate match PDSCH around. The UE rate matches around the union of all resources indicated in the rate match patterns. Rate match patterns defined here on cell level apply only to PDSCH of the same numerology. See TS 38.214 [19], clause 5.1.4.1. If a *RateMatchPattern* with the same *RateMatchPatternId* is configured in both *ServingCellConfig/ServingCellConfigCommon* and in SIB20/MCCH, the entire *RateMatchPattern* configuration shall be the same, including the set of RBs/REs indicated by the patterns for the rate matching around, and they are counted as a single rate match pattern in the total configured rate match patterns as defined in TS 38.214 [19]. |
| ***sCellDeactivationTimer***SCell deactivation timer in TS 38.321 [3]. If the field is absent, the UE applies the value infinity. |
| ***sfnSchemePDCCH***This parameter is used to configure SFN scheme for PDCCH: sfnSchemeA or sfnSchemeB as specified (see TS 38.214 [19], clause 5.1). If network includes both *sfnSchemePDCCH* and *sfnSchemePDSCH*, same value shall be configured. |
| ***sfnSchemePDSCH***This parameter is used to configure SFN scheme for PDSCH: sfnSchemeA or sfnSchemeB as specified (see TS 38.214 [19], clause 5.1). If network includes both *sfnSchemePDCCH* and *sfnSchemePDSCH*, same value shall be configured. |
| ***semiStaticChannelAccessConfigUE***When this field is configured and when *channelAccessMode-r16* (see IE ServingCellConfigCommon and IE ServingCellConfigCommonSIB) is configured to *semiStatic*, the UE operates in semi-static channel access mode and can initiate a channel occupancy periodically (see TS 37.213 [48], Clause 4.3).The period can be configured independently from period configured in *SemiStaticChannelAccessConfig-r16* if the UE indicates the corresponding capability. Otherwise, the periodicity configured by *periodUE-r17* is an integer multiple of or an integer factor of the periodicity indicated by *period* in *SemiStaticChannelAccessConfig-r16.* |
| ***servingCellMO****measObjectId* of the *MeasObjectNR* in *MeasConfig* which is associated to the serving cell. For this *MeasObjectNR*, the following relationship applies between this MeasObjectNR and *frequencyInfoDL* in *ServingCellConfigCommon* of the serving cell: if *ssbFrequency* is configured, its value is the same as the *absoluteFrequencySSB* and if *csi-rs-ResourceConfigMobility* is configured, the value of its *subcarrierSpacing* is present in one entry of the *scs-SpecificCarrierList*, *csi-RS-CellListMobility* includes an entry corresponding to the serving cell (with *cellId* equal to *physCellId* in *ServingCellConfigCommon*) and the frequency range indicated by the *csi-rs-MeasurementBW* of the entry in *csi-RS-CellListMobility* is included in the frequency range indicated by in the entry of the *scs-SpecificCarrierList*. |
| ***supplementaryUplink***Network may configure this field only when *supplementaryUplinkConfig* is configured in *ServingCellConfigCommon* or *supplementaryUplink* is configured in *ServingCellConfigCommonSIB*. |
| ***supplementaryUplinkRelease***If this field is included, the UE shall release the uplink configuration configured by *supplementaryUplink*. The network only includes either *supplementaryUplinkRelease* or *supplementaryUplink* at a time. |
| ***tag-Id***Timing Advance Group ID, as specified in TS 38.321 [3], which this cell belongs to. |
| ***tci-ActivatedConfig***If configured for an SCell, or if configured for the PSCell when the SCG is being activated upon the reception of the containing message, the UE shall consider the TCI states provided in this field as the activated TCI states for PDCCH/PDSCH reception on this serving cell.If configured for the PSCell when the SCG is indicated as deactivated in the containing message:- the UE shall consider the TCI states provided in this field as the TCI states to be activated for PDCCH/PDSCH reception upon a later SCG activation in which *tci-ActivatedConfig* is absent- if bfd-and-RLM is configured and no RS is configured in *RadioLinkMonitoringConfig* for RLM, respectively for BFD, the UE shall use the TCI states provided in this field for PDCCH as RS for RLM, respectively for BFD.When this field is absent for the PSCell and the SCG is being deactivated:- the UE shall consider the previously activated TCI states as the TCI states to be activated for PDCCH/PDSCH reception upon a later SCG activation in which *tci-ActivatedConfig* is absent- if *bfd-and-RLM* is configured and no RS is configured in *RadioLinkMonitoringConfig* for RLM, respectively for BFD, the UE shall use the previously activated TCI states for PDCCH as RS for RLM, respectively for BFD. |
| ***tdd-UL-DL-ConfigurationDedicated-IAB-MT***Resource configuration per IAB-MT D/U/F overrides all symbols (with a limitation that effectively only flexible symbols can be overwritten in Rel-16) per slot over the number of slots as provided by *TDD-UL-DL ConfigurationCommon*. |
| ***unifiedTCI-StateType***Indicates the unified TCI state type the UE is configured for this serving cell. The value *separate* means this serving cell is configured with *dl-OrJointTCI-StateList* for DL TCI state and *ul-TCI-ToAddModList* for UL TCI state. The value *joint* means this serving cell is configured with *dl-OrJointTCI-StateList* for joint TCI state for UL and DL operation. The network does not configure the field in a serving cell that is configured with more than one value for the *coresetPoolIndex.* |
| ***uplinkConfig***Network may configure this field only when *uplinkConfigCommon* is configured in *ServingCellConfigCommon* or *ServingCellConfigCommonSIB*. Addition or release of this field can only be done upon SCell addition or release (respectively). |
| ***uplink-PowerControlToAddModList***Configures UL power control parameters for PUSCH, PUCCH and SRS when field unifiedTCI-StateType is configured for this serving cell. |

|  |
| --- |
| ***UplinkConfig* field descriptions** |
| ***carrierSwitching***Includes parameters for configuration of carrier based SRS switching (see TS 38.214 [19], clause 6.2.1.3. |
| ***enableDefaultBeamPL-ForPUSCH0-0, enableDefaultBeamPL-ForPUCCH, enableDefaultBeamPL-ForSRS***When the parameter is present, UE derives the spatial relation and the corresponding pathloss reference Rs as specified in 38.213, clauses 7.1.1, 7.2.1, 7.3.1 and 9.2.2. The network only configures these parameters for FR2. |
| ***enablePL-RS-UpdateForPUSCH-SRS***When this parameter is present, the Rel-16 feature of MAC CE based pathloss RS updates for PUSCH/SRS is enabled. Network only configures this parameter when the UE is configured with *sri-PUSCH-PowerControl*. If this field is not configured, network configures at most 4 pathloss RS resources for PUSCH/PUCCH/SRS transmissions per BWP, not including pathloss RS resources for SRS transmissions for positioning. (See TS 38.213 [13], clause 7). |
| ***firstActiveUplinkBWP-Id***If configured for an SpCell, this field contains the ID of the UL BWP to be activated upon performing the RRC (re-)configuration. If the field is absent, the RRC (re-)configuration does not impose a BWP switch.If configured for an SCell, this field contains the ID of the uplink bandwidth part to be used upon activation of an SCell. The initial bandwidth part is referred to by BandiwdthPartId = 0. |
| ***initialUplinkBWP***The dedicated (UE-specific) configuration for the initial uplink bandwidth-part (i.e. UL BWP#0). If any of the optional IEs are configured within this IE as part of the IE *uplinkConfig*, the UE considers the BWP#0 to be an RRC configured BWP (from UE capability viewpoint). Otherwise, the UE does not consider the BWP#0 as an RRC configured BWP (from UE capability viewpoint). Network always configures the UE with a value for this field if no other BWPs are configured. NOTE1 |
| ***moreThanOneNackOnlyMode***Indicates the mode of NACK-only feedback in the PUCCH transmission, as specified in TS 38.213 [13], clause 18. If multicast CFR is not configured, this field is not included. Otherwise, if the field is absent, UE uses mode 1 for multicast CFR. |
| ***mpr-PowerBoost-FR2***Indicates whether UE is allowed to boost uplink transmission power by suspending in-band emission (IBE) requirements as specified in TS 38.101-2 [39]. Network only configures this field for FR2 serving cells. |
| ***powerBoostPi2BPSK***If this field is set to *true*, the UE determines the maximum output power for PUCCH/PUSCH transmissions that use pi/2 BPSK modulation according to TS 38.101-1 [15], clause 6.2.4. |
| ***pusch-ServingCellConfig***PUSCH related parameters that are not BWP-specific. |
| ***uplinkBWP-ToAddModList***The additional bandwidth parts for uplink to be added or modified. In case of TDD uplink- and downlink BWP with the same *bandwidthPartId* are considered as a BWP pair and must have the same center frequency. |
| ***uplinkBWP-ToReleaseList***The additional bandwidth parts for uplink to be released. |
| ***uplinkChannelBW-PerSCS-List***A set of UE specific channel bandwidth and location configurations for different subcarrier spacings (numerologies). Defined in relation to Point A. The UE uses the configuration provided in this field only for the purpose of channel bandwidth and location determination. If absent, UE uses the configuration indicated in *scs-SpecificCarrierList* in *UplinkConfigCommon* / *UplinkConfigCommonSIB*. Network only configures channel bandwidth that corresponds to the channel bandwidth values defined in TS 38.101-1 [15] and TS 38.101-2 [39]. |
| ***uplinkTxSwitchingPeriodLocation***Indicates whether the location of UL Tx switching period is configured in this uplink carrier in case of inter-band UL CA, SUL, or (NG)EN-DC, as specified in TS 38.101-1 [15] and TS 38.101-3 [34].In case of (NG)EN-DC, network always configures this field to TRUE for NR carrier (i.e. with (NG)EN-DC, the UL switching period always occurs on the NR carrier).In case of inter-band UL CA or SUL, for dynamic uplink Tx switching between 2 bands with 2 uplink carriers or 3 uplink carriers as defined in TS 38.101-1 [15], network configures this field to TRUE for the uplink carrier(s) on one band and configures this field to FALSE for the uplink carrier(s) on the other band. This field is set to the same value for the carriers on the same band. |
| ***uplinkTxSwitchingCarrier***Indicates that the configured carrier is carrier1 or carrier2 for dynamic uplink Tx switching, as defined in TS 38.101-1 [15] and TS 38.101-3 [34]. In case of (NG)EN-DC, network always configures the NR carrier as carrier 2.In case of inter-band UL CA or SUL, for dynamic uplink Tx switching between 2 bands with 2 uplink carriers or 3 uplink carriers as defined in TS 38.101-1 [15], network configures the uplink carrier(s) on one band as carrier1 and the uplink carrier(s) on the other band as carrier2. This field is set to the same value for the carriers on the same band. |

|  |
| --- |
| ***DormantBWP-Config* field descriptions** |
| ***dormancyGroupWithinActiveTime***This field contains the ID of an SCell group for Dormancy within active time, to which this SCell belongs. The use of the Dormancy within active time SCell groups is specified in TS 38.213 [13]. |
| ***dormancyGroupOutsideActiveTime***This field contains the ID of an SCell group for Dormancy outside active time, to which this SCell belongs. The use of the Dormancy outside active time SCell groups is specified in TS 38.213 [13]. |
| ***dormantBWP-Id***This field contains the ID of the downlink bandwidth part to be used as dormant BWP. If this field is configured, its value is different from *defaultDownlinkBWP-Id*, and at least one of the *withinActiveTimeConfig* and *outsideActiveTimeConfig* should be configured. |
| ***firstOutsideActiveTimeBWP-Id***This field contains the ID of the downlink bandwidth part to be activated when receiving a DCI indication for SCell dormancy outside active time. |
| ***firstWithinActiveTimeBWP-Id***This field contains the ID of the downlink bandwidth part to be activated when receiving a DCI indication for SCell dormancy within active time. |
| ***outsideActiveTimeConfig***This field contains the configuration to be used for SCell dormancy outside active time, as specified in TS 38.213 [13]. The field can only be configured when the cell group the SCell belongs to is configured with *dcp-Config*. |
| ***withinActiveTimeConfig***This field contains the configuration to be used for SCell dormancy within active time, as specified in TS 38.213 [13].  |

|  |
| --- |
| ***GuardBand* field descriptions** |
| ***startCRB***Indicates the starting RB of the guard band. |
| ***nrofCRB***Indicates the length of the guard band in RBs. When set to 0, zero-size guard band is used. |

NOTE 1: If the dedicated part of initial UL/DL BWP configuration is absent, the initial BWP can be used but with some limitations. For example, changing to another BWP requires *RRCReconfiguration* since DCI format 1\_0 doesn't support DCI-based switching.

|  |  |
| --- | --- |
| **Conditional Presence** | **Explanation** |
| *AsyncCA* | This field is mandatory present for SCells whose slot offset between the SpCell is not 0. Otherwise it is absent, Need S. |
| *MeasObject* | This field is mandatory present for the SpCell if the UE has a *measConfig*, and it is optionally present, Need M, for SCells. For RedCap UEs, this field is optionally present, Need M. |
| *SCellOnly* | This field is optionally present, Need R, for SCells. It is absent otherwise.  |
| *ServingCellWithoutPUCCH* | This field is optionally present, Need S, for SCells except PUCCH SCells. It is absent otherwise. |
| *SyncAndCellAdd* | This field is mandatory present for a SpCell upon reconfiguration with *reconfigurationWithSync* and upon *RRCSetup*/*RRCResume*.The field is optionally present for an SpCell, Need N, upon reconfiguration without *reconfigurationWithSync*.The field is mandatory present for an SCell upon addition, and absent for SCell in other cases, Need M. |
| *TCI\_ActivatedConfig* | This field is optional Need N for SCells if *sCellState* is configured, otherwise it is absent.This field is optional Need S for the PSCell when the SCG is indicated as deactivated or is being activated, otherwise it is absent.This field is absent for the PCell. |
| *TDD* | This field is optionally present, Need R, for TDD cells. It is absent otherwise. |
| *TDD\_IAB* | For IAB-MT, this field is optionally present, Need R, for TDD cells. It is absent otherwise. |

<Text omitted>

– *SRS-Config*

The IE *SRS-Config* is used to configure sounding reference signal transmissions. The configuration defines a list of SRS-Resources, a list of SRS-PosResources, a list of SRS-PosResourceSets and a list of SRS-ResourceSets. Each resource set defines a set of SRS-Resources or SRS-PosResources. The network triggers the transmission of the set of SRS-Resources or SRS-PosResources using a configured aperiodicSRS-ResourceTrigger (L1 DCI). The network does not configure SRS specific power control parameters, *alpha* (without suffix)*, p0* (without suffix) or *pathlossReferenceRS* if *unifiedTCI-StateType* is configured for the serving cell.

***SRS-Config* information element**

-- ASN1START

-- TAG-SRS-CONFIG-START

SRS-Config ::= SEQUENCE {

 srs-ResourceSetToReleaseList SEQUENCE (SIZE(1..maxNrofSRS-ResourceSets)) OF SRS-ResourceSetId OPTIONAL, -- Need N

 srs-ResourceSetToAddModList SEQUENCE (SIZE(1..maxNrofSRS-ResourceSets)) OF SRS-ResourceSet OPTIONAL, -- Need N

 srs-ResourceToReleaseList SEQUENCE (SIZE(1..maxNrofSRS-Resources)) OF SRS-ResourceId OPTIONAL, -- Need N

 srs-ResourceToAddModList SEQUENCE (SIZE(1..maxNrofSRS-Resources)) OF SRS-Resource OPTIONAL, -- Need N

 tpc-Accumulation ENUMERATED {disabled} OPTIONAL, -- Need S

 ...,

 [[

 srs-RequestDCI-1-2-r16 INTEGER (1..2) OPTIONAL, -- Need S

 srs-RequestDCI-0-2-r16 INTEGER (1..2) OPTIONAL, -- Need S

 srs-ResourceSetToAddModListDCI-0-2-r16 SEQUENCE (SIZE(1..maxNrofSRS-ResourceSets)) OF SRS-ResourceSet OPTIONAL, -- Need N

 srs-ResourceSetToReleaseListDCI-0-2-r16 SEQUENCE (SIZE(1..maxNrofSRS-ResourceSets)) OF SRS-ResourceSetId OPTIONAL, -- Need N

 srs-PosResourceSetToReleaseList-r16 SEQUENCE (SIZE(1..maxNrofSRS-PosResourceSets-r16)) OF SRS-PosResourceSetId-r16

 OPTIONAL, -- Need N

 srs-PosResourceSetToAddModList-r16 SEQUENCE (SIZE(1..maxNrofSRS-PosResourceSets-r16)) OF SRS-PosResourceSet-r16 OPTIONAL,-- Need N

 srs-PosResourceToReleaseList-r16 SEQUENCE (SIZE(1..maxNrofSRS-PosResources-r16)) OF SRS-PosResourceId-r16 OPTIONAL,-- Need N

 srs-PosResourceToAddModList-r16 SEQUENCE (SIZE(1..maxNrofSRS-PosResources-r16)) OF SRS-PosResource-r16 OPTIONAL -- Need N

 ]]

}

SRS-ResourceSet ::= SEQUENCE {

 srs-ResourceSetId SRS-ResourceSetId,

 srs-ResourceIdList SEQUENCE (SIZE(1..maxNrofSRS-ResourcesPerSet)) OF SRS-ResourceId OPTIONAL, -- Cond Setup

 resourceType CHOICE {

 aperiodic SEQUENCE {

 aperiodicSRS-ResourceTrigger INTEGER (1..maxNrofSRS-TriggerStates-1),

 csi-RS NZP-CSI-RS-ResourceId OPTIONAL, -- Cond NonCodebook

 slotOffset INTEGER (1..32) OPTIONAL, -- Need S

 ...,

 [[

 aperiodicSRS-ResourceTriggerList SEQUENCE (SIZE(1..maxNrofSRS-TriggerStates-2))

 OF INTEGER (1..maxNrofSRS-TriggerStates-1) OPTIONAL -- Need M

 ]]

 },

 semi-persistent SEQUENCE {

 associatedCSI-RS NZP-CSI-RS-ResourceId OPTIONAL, -- Cond NonCodebook

 ...

 },

 periodic SEQUENCE {

 associatedCSI-RS NZP-CSI-RS-ResourceId OPTIONAL, -- Cond NonCodebook

 ...

 }

 },

 usage ENUMERATED {beamManagement, codebook, nonCodebook, antennaSwitching},

 alpha Alpha OPTIONAL, -- Need S

 p0 INTEGER (-202..24) OPTIONAL, -- Cond Setup

 pathlossReferenceRS PathlossReferenceRS-Config OPTIONAL, -- Need M

 srs-PowerControlAdjustmentStates ENUMERATED { sameAsFci2, separateClosedLoop} OPTIONAL, -- Need S

 ...,

 [[

 pathlossReferenceRSList-r16 SetupRelease { PathlossReferenceRSList-r16} OPTIONAL -- Need M

 ]],

 [[

 usagePDC-r17 ENUMERATED {true} OPTIONAL, -- Need R

 availableSlotOffsetList-r17 SEQUENCE (SIZE(1..4)) OF AvailableSlotOffset-r17 OPTIONAL, -- Need R

 followUnifiedTCI-StateSRS-r17 ENUMERATED {enabled} OPTIONAL -- Need R

 ]]

}

AvailableSlotOffset-r17 ::= INTEGER (0..7)

PathlossReferenceRS-Config ::= CHOICE {

 ssb-Index SSB-Index,

 csi-RS-Index NZP-CSI-RS-ResourceId

}

PathlossReferenceRSList-r16 ::= SEQUENCE (SIZE (1..maxNrofSRS-PathlossReferenceRS-r16)) OF PathlossReferenceRS-r16

PathlossReferenceRS-r16 ::= SEQUENCE {

 srs-PathlossReferenceRS-Id-r16 SRS-PathlossReferenceRS-Id-r16,

 pathlossReferenceRS-r16 PathlossReferenceRS-Config

}

SRS-PathlossReferenceRS-Id-r16 ::= INTEGER (0..maxNrofSRS-PathlossReferenceRS-1-r16)

SRS-PosResourceSet-r16 ::= SEQUENCE {

 srs-PosResourceSetId-r16 SRS-PosResourceSetId-r16,

 srs-PosResourceIdList-r16 SEQUENCE (SIZE(1..maxNrofSRS-ResourcesPerSet)) OF SRS-PosResourceId-r16

 OPTIONAL, -- Cond Setup

 resourceType-r16 CHOICE {

 aperiodic-r16 SEQUENCE {

 aperiodicSRS-ResourceTriggerList-r16 SEQUENCE (SIZE(1..maxNrofSRS-TriggerStates-1))

 OF INTEGER (1..maxNrofSRS-TriggerStates-1) OPTIONAL, -- Need M

 ...

 },

 semi-persistent-r16 SEQUENCE {

 ...

 },

 periodic-r16 SEQUENCE {

 ...

 }

 },

 alpha-r16 Alpha OPTIONAL, -- Need S

 p0-r16 INTEGER (-202..24) OPTIONAL, -- Cond Setup

 pathlossReferenceRS-Pos-r16 CHOICE {

 ssb-IndexServing-r16 SSB-Index,

 ssb-Ncell-r16 SSB-InfoNcell-r16,

 dl-PRS-r16 DL-PRS-Info-r16

 } OPTIONAL, -- Need M

 ...

}

SRS-ResourceSetId ::= INTEGER (0..maxNrofSRS-ResourceSets-1)

SRS-PosResourceSetId-r16 ::= INTEGER (0..maxNrofSRS-PosResourceSets-1-r16)

SRS-Resource ::= SEQUENCE {

 srs-ResourceId SRS-ResourceId,

 nrofSRS-Ports ENUMERATED {port1, ports2, ports4},

 ptrs-PortIndex ENUMERATED {n0, n1 } OPTIONAL, -- Need R

 transmissionComb CHOICE {

 n2 SEQUENCE {

 combOffset-n2 INTEGER (0..1),

 cyclicShift-n2 INTEGER (0..7)

 },

 n4 SEQUENCE {

 combOffset-n4 INTEGER (0..3),

 cyclicShift-n4 INTEGER (0..11)

 }

 },

 resourceMapping SEQUENCE {

 startPosition INTEGER (0..5),

 nrofSymbols ENUMERATED {n1, n2, n4},

 repetitionFactor ENUMERATED {n1, n2, n4}

 },

 freqDomainPosition INTEGER (0..67),

 freqDomainShift INTEGER (0..268),

 freqHopping SEQUENCE {

 c-SRS INTEGER (0..63),

 b-SRS INTEGER (0..3),

 b-hop INTEGER (0..3)

 },

 groupOrSequenceHopping ENUMERATED { neither, groupHopping, sequenceHopping },

 resourceType CHOICE {

 aperiodic SEQUENCE {

 ...

 },

 semi-persistent SEQUENCE {

 periodicityAndOffset-sp SRS-PeriodicityAndOffset,

 ...

 },

 periodic SEQUENCE {

 periodicityAndOffset-p SRS-PeriodicityAndOffset,

 ...

 }

 },

 sequenceId INTEGER (0..1023),

 spatialRelationInfo SRS-SpatialRelationInfo OPTIONAL, -- Need R

 ...,

 [[

 resourceMapping-r16 SEQUENCE {

 startPosition-r16 INTEGER (0..13),

 nrofSymbols-r16 ENUMERATED {n1, n2, n4},

 repetitionFactor-r16 ENUMERATED {n1, n2, n4}

 } OPTIONAL -- Need R

 ]],

 [[

 spatialRelationInfo-PDC-r17 SetupRelease { SpatialRelationInfo-PDC-r17 } OPTIONAL, -- Need M

 resourceMapping-r17 SEQUENCE {

 startPosition-r17 INTEGER (0..13),

 nrofSymbols-r17 ENUMERATED {n1, n2, n4, n8, n10, n12, n14},

 repetitionFactor-r17 ENUMERATED {n1, n2, n4, n5, n6, n7, n8, n10, n12, n14}

 } OPTIONAL, -- Need R

 partialFreqSounding-r17 SEQUENCE {

 startRBIndexFScaling-r17 CHOICE{

 startRBIndexAndFreqScalingFactor2-r17 INTEGER (0..1),

 startRBIndexAndFreqScalingFactor4-r17 INTEGER (0..3)

 },

 enableStartRBHopping-r17 ENUMERATED {enable} OPTIONAL -- Need R

 } OPTIONAL, -- Need R

 transmissionComb-n8-r17 SEQUENCE {

 combOffset-n8-r17 INTEGER (0..7),

 cyclicShift-n8-r17 INTEGER (0..5)

 } OPTIONAL, -- Need R

 srs-TCI-State-r17 CHOICE {

 srs-UL-TCI-State TCI-UL-StateId-r17,

 srs-DLorJointTCI-State TCI-StateId

 } OPTIONAL -- Need R

 ]],

 [[

 repetitionFactor-v1730 ENUMERATED {n3} OPTIONAL, -- Need R

 srs-DLorJointTCI-State-v1730 SEQUENCE {

 cellAndBWP-r17 ServingCellAndBWP-Id-r17

 } OPTIONAL -- Cond DLorJointTCI-SRS

 ]]

}

SRS-PosResource-r16::= SEQUENCE {

 srs-PosResourceId-r16 SRS-PosResourceId-r16,

 transmissionComb-r16 CHOICE {

 n2-r16 SEQUENCE {

 combOffset-n2-r16 INTEGER (0..1),

 cyclicShift-n2-r16 INTEGER (0..7)

 },

 n4-r16 SEQUENCE {

 combOffset-n4-r16 INTEGER (0..3),

 cyclicShift-n4-r16 INTEGER (0..11)

 },

 n8-r16 SEQUENCE {

 combOffset-n8-r16 INTEGER (0..7),

 cyclicShift-n8-r16 INTEGER (0..5)

 },

 ...

 },

 resourceMapping-r16 SEQUENCE {

 startPosition-r16 INTEGER (0..13),

 nrofSymbols-r16 ENUMERATED {n1, n2, n4, n8, n12}

 },

 freqDomainShift-r16 INTEGER (0..268),

 freqHopping-r16 SEQUENCE {

 c-SRS-r16 INTEGER (0..63),

 ...

 },

 groupOrSequenceHopping-r16 ENUMERATED { neither, groupHopping, sequenceHopping },

 resourceType-r16 CHOICE {

 aperiodic-r16 SEQUENCE {

 slotOffset-r16 INTEGER (1..32) OPTIONAL, -- Need S

 ...

 },

 semi-persistent-r16 SEQUENCE {

 periodicityAndOffset-sp-r16 SRS-PeriodicityAndOffset-r16,

 ...,

 [[

 periodicityAndOffset-sp-Ext-r16 SRS-PeriodicityAndOffsetExt-r16 OPTIONAL -- Need R

 ]]

 },

 periodic-r16 SEQUENCE {

 periodicityAndOffset-p-r16 SRS-PeriodicityAndOffset-r16,

 ...,

 [[

 periodicityAndOffset-p-Ext-r16 SRS-PeriodicityAndOffsetExt-r16 OPTIONAL -- Need R

 ]]

 }

 },

 sequenceId-r16 INTEGER (0..65535),

 spatialRelationInfoPos-r16 SRS-SpatialRelationInfoPos-r16 OPTIONAL, -- Need R

 ...

}

SRS-SpatialRelationInfo ::= SEQUENCE {

 servingCellId ServCellIndex OPTIONAL, -- Need S

 referenceSignal CHOICE {

 ssb-Index SSB-Index,

 csi-RS-Index NZP-CSI-RS-ResourceId,

 srs SEQUENCE {

 resourceId SRS-ResourceId,

 uplinkBWP BWP-Id

 }

 }

}

SRS-SpatialRelationInfoPos-r16 ::= CHOICE {

 servingRS-r16 SEQUENCE {

 servingCellId ServCellIndex OPTIONAL, -- Need S

 referenceSignal-r16 CHOICE {

 ssb-IndexServing-r16 SSB-Index,

 csi-RS-IndexServing-r16 NZP-CSI-RS-ResourceId,

 srs-SpatialRelation-r16 SEQUENCE {

 resourceSelection-r16 CHOICE {

 srs-ResourceId-r16 SRS-ResourceId,

 srs-PosResourceId-r16 SRS-PosResourceId-r16

 },

 uplinkBWP-r16 BWP-Id

 }

 }

 },

 ssb-Ncell-r16 SSB-InfoNcell-r16,

 dl-PRS-r16 DL-PRS-Info-r16

}

SSB-Configuration-r16 ::= SEQUENCE {

 ssb-Freq-r16 ARFCN-ValueNR,

 halfFrameIndex-r16 ENUMERATED {zero, one},

 ssbSubcarrierSpacing-r16 SubcarrierSpacing,

 ssb-Periodicity-r16 ENUMERATED { ms5, ms10, ms20, ms40, ms80, ms160, spare2,spare1 } OPTIONAL, -- Need S

 sfn0-Offset-r16 SEQUENCE {

 sfn-Offset-r16 INTEGER (0..1023),

 integerSubframeOffset-r16 INTEGER (0..9) OPTIONAL -- Need R

 } OPTIONAL, -- Need R

 sfn-SSB-Offset-r16 INTEGER (0..15),

 ss-PBCH-BlockPower-r16 INTEGER (-60..50) OPTIONAL -- Cond Pathloss

}

SSB-InfoNcell-r16 ::= SEQUENCE {

 physicalCellId-r16 PhysCellId,

 ssb-IndexNcell-r16 SSB-Index OPTIONAL, -- Need S

 ssb-Configuration-r16 SSB-Configuration-r16 OPTIONAL -- Need S

}

DL-PRS-Info-r16 ::= SEQUENCE {

 dl-PRS-ID-r16 INTEGER (0..255),

 dl-PRS-ResourceSetId-r16 INTEGER (0..7),

 dl-PRS-ResourceId-r16 INTEGER (0..63) OPTIONAL -- Need S

}

SRS-ResourceId ::= INTEGER (0..maxNrofSRS-Resources-1)

SRS-PosResourceId-r16 ::= INTEGER (0..maxNrofSRS-PosResources-1-r16)

SRS-PeriodicityAndOffset ::= CHOICE {

 sl1 NULL,

 sl2 INTEGER(0..1),

 sl4 INTEGER(0..3),

 sl5 INTEGER(0..4),

 sl8 INTEGER(0..7),

 sl10 INTEGER(0..9),

 sl16 INTEGER(0..15),

 sl20 INTEGER(0..19),

 sl32 INTEGER(0..31),

 sl40 INTEGER(0..39),

 sl64 INTEGER(0..63),

 sl80 INTEGER(0..79),

 sl160 INTEGER(0..159),

 sl320 INTEGER(0..319),

 sl640 INTEGER(0..639),

 sl1280 INTEGER(0..1279),

 sl2560 INTEGER(0..2559)

}

SRS-PeriodicityAndOffset-r16 ::= CHOICE {

 sl1 NULL,

 sl2 INTEGER(0..1),

 sl4 INTEGER(0..3),

 sl5 INTEGER(0..4),

 sl8 INTEGER(0..7),

 sl10 INTEGER(0..9),

 sl16 INTEGER(0..15),

 sl20 INTEGER(0..19),

 sl32 INTEGER(0..31),

 sl40 INTEGER(0..39),

 sl64 INTEGER(0..63),

 sl80 INTEGER(0..79),

 sl160 INTEGER(0..159),

 sl320 INTEGER(0..319),

 sl640 INTEGER(0..639),

 sl1280 INTEGER(0..1279),

 sl2560 INTEGER(0..2559),

 sl5120 INTEGER(0..5119),

 sl10240 INTEGER(0..10239),

 sl40960 INTEGER(0..40959),

 sl81920 INTEGER(0..81919),

 ...

}

SRS-PeriodicityAndOffsetExt-r16 ::= CHOICE {

 sl128 INTEGER(0..127),

 sl256 INTEGER(0..255),

 sl512 INTEGER(0..511),

 sl20480 INTEGER(0..20479)

}

SpatialRelationInfo-PDC-r17 ::= SEQUENCE {

 referenceSignal CHOICE {

 ssb-Index SSB-Index,

 csi-RS-Index NZP-CSI-RS-ResourceId,

 dl-PRS-PDC NR-DL-PRS-ResourceID-r17,

 srs SEQUENCE {

 resourceId SRS-ResourceId,

 uplinkBWP BWP-Id

 },

 ...

 },

 ...

}

-- TAG-SRS-CONFIG-STOP

-- ASN1STOP

|  |
| --- |
| ***SRS-Config* field descriptions** |
| ***tpc-Accumulation***If the field is absent, UE applies TPC commands via accumulation. If disabled, UE applies the TPC command without accumulation (this applies to SRS when a separate closed loop is configured for SRS) (see TS 38.213 [13], clause 7.3). |

|  |
| --- |
| ***SRS-Resource, SRS-PosResource* field descriptions** |
| ***cyclicShift-n2***Cyclic shift configuration (see TS 38.214 [19], clause 6.2.1). |
| ***cyclicShift-n4***Cyclic shift configuration (see TS 38.214 [19], clause 6.2.1). |
| ***cyclicShift-n8***Cyclic shift configuration (see TS 38.214 [19], clause 6.2.1). |
| ***enableStartRBHopping***When this RRC parameter is configured, start RB location hopping is enabled for partial frequency sounding in different SRS frequency hopping periods for periodic/semi-persistent/aperiodic SRS as described in Clause 6.4.1.4 in TS 38.211. |
| ***freqHopping***Includes parameters capturing SRS frequency hopping (see TS 38.214 [19], clause 6.2.1). For CLI SRS-RSRP measurement, the network always configures this field such that *b-hop* > *b-SRS*. |
| ***groupOrSequenceHopping***Parameter(s) for configuring group or sequence hopping (see TS 38.211 [16], clause 6.4.1.4.2). For CLI SRS-RSRP measurement, the network always configures this parameter to 'neither'. |
| ***nrofSRS-Ports***Number of ports. For CLI SRS-RSRP measurement, the network always configures this parameter to 'port1'. |
| ***periodicityAndOffset-p, periodicityAndOffset-p-Ext***Periodicity and slot offset for this SRS resource. All values are in "number of slots". Value *sl1* corresponds to a periodicity of 1 slot, value *sl2* corresponds to a periodicity of 2 slots, and so on. For each periodicity the corresponding offset is given in number of slots. For periodicity *sl1* the offset is 0 slots (see TS 38.214 [19], clause 6.2.1). For CLI SRS-RSRP measurement, *sl1280* and *sl2560* cannot be configured. For *SRS-PosResource*, values *sl20480*, *sl40960* and *sl81920* cannot be configured for SCS=15kHz, values *sl40960* and *sl81920* cannot be configured for SCS=30kHz, and value *sl81920* cannot be configured for SCS=60kHz.When *periodicityAndOffset-p-Ext* is present, *periodicityAndOffset-p* shall be ignored by the UE. |
| ***periodicityAndOffset-sp, periodicityAndOffset-sp-Ext***Periodicity and slot offset for this SRS resource. All values are in "number of slots". Value *sl1* corresponds to a periodicity of 1 slot, value *sl2* corresponds to a periodicity of 2 slots, and so on. For each periodicity the corresponding offset is given in number of slots. For periodicity *sl1* the offset is 0 slots (see TS 38.214 [19], clause 6.2.1). For *SRS-PosResource*, values *sl20480*, *sl40960* and *sl81920* cannot be configured for SCS=15kHz, values *sl40960* and *sl81920* cannot be configured for SCS=30kHz, and value *sl81920* cannot be configured for SCS=60kHz.When *periodicityAndOffset-sp-Ext* is present, *periodicityAndOffset-sp* shall be ignored by the UE. |
| ***ptrs-PortIndex***The PTRS port index for this SRS resource for non-codebook based UL MIMO. This is only applicable when the corresponding *PTRS-UplinkConfig* is set to CP-OFDM. The *ptrs-PortIndex* configured here must be smaller than the *maxNrofPorts* configured in the *PTRS-UplinkConfig* (see TS 38.214 [19], clause 6.2.3.1). This parameter is not applicable to CLI SRS-RSRP measurement. |
| ***resourceMapping***OFDM symbol location of the SRS resource within a slot including *nrofSymbols* (number of OFDM symbols), *startPosition* (value 0 refers to the last symbol, value 1 refers to the second last symbol, and so on) and *repetitionFactor* (see TS 38.214 [19], clause 6.2.1 and TS 38.211 [16], clause 6.4.1.4). The configured SRS resource does not exceed the slot boundary. If *resourceMapping-r16* is signalled, UE shall ignore the *resourceMapping* (without suffix). If *resourceMapping-r17* is signalled, *resourceMapping-r16* is not signalled and the UE shall ignore the *resourceMapping* (without suffix) and only the values of nrofSymbols which are integer multiples of the configured repetitionFactor can be configured. The network can only signal *repetitionFactor-v1730* if *resourceMapping-r17* is signalled. When *repetitionFactor-v1730* is signalled, the UE shall ignore *repetitionFactor-r17*. For CLI SRS-RSRP measurement, the network always configures *nrofSymbols* and *repetitionFactor* to 'n1'. |
| ***resourceType***Periodicity and offset for semi-persistent and periodic SRS resource, or slot offset for aperiodic SRS resource for positioning (see TS 38.214 [19], clause 6.2.1). For CLI SRS-RSRP measurement, only 'periodic' is applicable for *resourceType*. |
| ***sequenceId***Sequence ID used to initialize pseudo random group and sequence hopping (see TS 38.214 [19], clause 6.2.1). |
| ***spatialRelationInfo***Configuration of the spatial relation between a reference RS and the target SRS. Reference RS can be SSB/CSI-RS/SRS (see TS 38.214 [19], clause 6.2.1). This parameter is not applicable to CLI SRS-RSRP measurement. This field is not configured if *unifiedTCI-StateType* is configured for the serving cell. |
| ***spatialRelationInfo-PDC***Configuration of the spatial relation between a reference RS and the target SRS. Reference RS can be SSB/CSI-RS/SRS/DL-PRS-PDC (see TS 38.214 [19], clause 6.2.1). The field is present in case of *resourceType=periodic* and *usagePDC-r17=true* in the *SRS-ResourceSet*, otherwise the field is absent. |
| ***spatialRelationInfoPos***Configuration of the spatial relation between a reference RS and the target SRS. Reference RS can be SSB/CSI-RS/SRS/DL-PRS (see TS 38.214 [19], clause 6.2.1).If the IE *srs-ResourceId-Ext* is present, the IE *srs-ResourceId* in *spatialRelationInfoPos* represents the index from 0 to 63. Otherwise the IE *srs-ResourceId* in *spatialRelationInfoPos* represents the index from 0 to 31. |
| ***srs-RequestDCI-0-2***Indicate the number of bits for "SRS request"in DCI format 0\_2. When the field is absent, then the value of 0 bit for "SRS request" in DCI format 0\_2 is applied. If the parameter *srs-RequestDCI-0-2* is configured to value 1, 1 bit is used to indicate one of the first two rows of Table 7.3.1.1.2-24 in TS 38.212 [17] for triggered aperiodic SRS resource set. If the value 2 is configured, 2 bits are used to indicate one of the rows of Table 7.3.1.1.2-24 in TS 38.212 [17]. When UE is configured with *supplementaryUplink*, an extra bit (the first bit of the SRS request field) is used for the non-SUL/SUL indication. |
| ***srs-RequestDCI-1-2***Indicate the number of bits for "SRS request" in DCI format 1\_2. When the field is absent, then the value of 0 bit for "SRS request" in DCI format 1\_2 is applied. When the UE is configured with *supplementaryUplink*, an extra bit (the first bit of the SRS request field) is used for the non-SUL/SUL indication (see TS 38.214 [19], clause 6.1.1.2). |
| ***srs-ResourceSetToAddModListDCI-0-2***List of SRS resource set to be added or modified for DCI format 0\_2 (see TS 38.212 [17], clause 7.3.1). |
| ***srs-ResourceSetToReleaseListDCI-0-2***List of SRS resource set to be released for DCI format 0\_2 (see TS 38.212 [17], clause 7.3.1). |
| ***srs-TCI-State***Configuration of either a UL TCI state or a joint TCI state for the SRS resource. In case of *UL TCI-State*, refers to the TCI state defined in *ul-TCI-StateList* in the *BWP-UplinkDedicated* where the *SRS-Config* is configured. In case of joint TCI state, refers to a TCI state defined in *dl-OrJointTCI-StateList* in *pdsch-Config* of the *BWP-DownlinkDedicated* and serving cell indicated by *cellAndBWP*.This field is absent when the SRS resource is in an *SRS-ResourceSet* configured with *followUnifiedTCI-StateSRS-r17* or when the field *unifiedTCI-StateType* is not configured to the serving cell which the SRS resource is located in. |
| ***startRBIndexAndFreqScalingFactor***Configures the UE with the startRBIndex and freqScalingFactor for partial frequency sounding as described in Clause 6.4.1.4 in TS 38.211. The startRBIndexForFScaling2 gives the startRBIndex when freqScalingFactor is 2 and the startRBIndexForFScaling4 gives the startRBIndex when FreqScalingFactor is 4  |
| ***transmissionComb, transmissionComb-n8***Comb value (2 or 4 or 8) and comb offset (0..combValue-1) (see TS 38.214 [19], clause 6.2.1). |

|  |
| --- |
| ***SRS-ResourceSet, SRS-PosResourceSet* field descriptions** |
| ***alpha***alpha value for SRS power control (see TS 38.213 [13], clause 7.3). When the field is absent the UE applies the value 1. |
| ***aperiodicSRS-ResourceTriggerList***An additional list of DCI "code points" upon which the UE shall transmit SRS according to this SRS resource set configuration (see TS 38.214 [19], clause 6). When the field is not included during a reconfiguration of *SRS-ResourceSet* of *resourceType* set to *aperiodic*, UE maintains this value based on the Need M; that is, this list is not considered as an extension of *aperiodicSRS-ResourceTrigger* for purpose of applying the general rule for extended list in clause 6.1.3. |
| ***aperiodicSRS-ResourceTrigger***The DCI "code point" upon which the UE shall transmit SRS according to this SRS resource set configuration (see TS 38.214 [19], clause 6). |
| ***associatedCSI-RS***ID of CSI-RS resource associated with this SRS resource set in non-codebook based operation (see TS 38.214 [19], clause 6.1.1.2). |
| ***availableSlotOffset***Indicates the number of available slots from slot n+k to the slot where the aperiodic SRS resource set is transmitted, where slot n is the slot with the triggering DCI, and k is the legacy triggering offset (slotOffset, not based on availabel slot) as described in clause 6.2.1 of TS 38.214. |
| ***csi-RS***ID of CSI-RS resource associated with this SRS resource set. (see TS 38.214 [19], clause 6.1.1.2). |
| ***dl-PRS***This field indicates a PRS configuration. |
| ***followUnifiedTCI-StateSRS***When set to enabled, for SRS resource Set, the UE applies the "indicated" UL only TCI or joint TCI as specified in TS 38.214 [19], clause 5.1.5. This parameter may be configured for aperiodic SRS for BM or SRS of any time-domain behavior for codebook, non-codebook, and antenna switching. |
| ***p0***P0 value for SRS power control. The value is in dBm. Only even values (step size 2) are allowed (see TS 38.213 [13], clause 7.3). |
| ***pathlossReferenceRS***A reference signal (e.g. a CSI-RS config or a SS block) to be used for SRS path loss estimation (see TS 38.213 [13], clause 7.3). |
| ***pathlossReferenceRS-Pos***A reference signal (e.g. a SS block or a DL-PRS config) to be used for SRS path loss estimation (see TS 38.213 [13], clause 7.3). |
| ***pathlossReferenceRSList***Multiple candidate pathloss reference RS(s) for SRS power control, where one candidate RS can be mapped to SRS Resource Set via MAC CE (clause 6.1.3.27 in TS 38.321 [3]). The network can only configure this field if *pathlossReferenceRS* is not configured in the same *SRS-ResourceSet*. |
| ***resourceType***Time domain behavior of SRS resource configuration, see TS 38.214 [19], clause 6.2.1. The network configures SRS resources in the same resource set with the same time domain behavior on periodic, aperiodic and semi-persistent SRS. The aperiodic SRS is not applicable for the UE in RRC\_INACTIVE. |
| ***slotOffset***An offset in number of slots between the triggering DCI and the actual transmission of this *SRS-ResourceSet*. If the field is absent the UE applies no offset (value 0). |
| ***srs-PowerControlAdjustmentStates***Indicates whether hsrs,c(i) = fc(i,1) or hsrs,c(i) = fc(i,2) (if twoPUSCH-PC-AdjustmentStates are configured) or separate close loop is configured for SRS. This parameter is applicable only for Uls on which UE also transmits PUSCH. If absent or release, the UE applies the value sameAs-Fci1 (see TS 38.213 [13], clause 7.3). |
| ***srs-ResourceIdList, srs-PosResourceIdList***The IDs of the SRS-Resources/SRS-PosResource used in this *SRS-ResourceSet/SRS-PosResourceSet*. If this *SRS-ResourceSet* is configured with usage set to codebook, the *srs-ResourceIdList* contains at most 2 entries. If this *SRS-ResourceSet* is configured with *usage* set to *nonCodebook*, the *srs-ResourceIdList* contains at most 4 entries. |
| ***srs-ResourceSetId, srs-PosResourceSetId***The ID of this resource set. It is unique in the context of the BWP in which the parent *SRS-Config* is defined. |
| ***ssb-IndexServing***Indicates SSB index belonging to a serving cell where the SRS is configured. |
| ***ssb-Ncell***This field indicates a SSB configuration from neighboring cell. |
| ***usage***Indicates if the SRS resource set is used for beam management, codebook based or non-codebook based transmission or antenna switching. See TS 38.214 [19], clause 6.2.1. Reconfiguration between codebook based and non-codebook based transmission is not supported. |
| ***usagePDC***If configured, it indicates that this SRS resource set is used for propagation delay compensation. The field can be present in only one *SRS-ResourceSet*. |

|  |
| --- |
| ***SRS-SpatialRelationInfoPos* field descriptions** |
| ***csi-RS-IndexServing***Indicates CSI-RS index belonging to a serving cell. |
| ***dl-PRS***This field indicates a PRS configuration. |
| ***resourceSelection***Indicates whether the configured SRS spatial relation resource is a *SRS-Resource* or *SRS-PosResource*. |
| ***servingCellId***The serving Cell ID of the source SSB, CSI-RS, or SRS for the spatial relation of the target SRS resource. If this field is absent the SSB, the CSI-RS, or the SRS is from the same serving cell where the SRS is configured. |
| ***ssb-IndexServing***Indicates SSB index belonging to a serving cell. |
| ***ssb-Ncell***This field indicates a SSB configuration from neighboring cell. |

|  |
| --- |
| ***SSB-InfoNCell* field descriptions** |
| ***physicalCellId***This field specifies the physical cell ID of the neighbour cell for which SSB configuration is provided. |
| ***ssb-IndexNcell***This field specifies the index of the SSB for a neighbour cell. See TS 38.213 [13]. If this field is absent, the UE determines the *ssb-IndexNcell* of the *physicalCellId*based on its SSB measurement from the cell. |
| ***ssb-Configuration***This field specifies the full configuration of the SSB. If this field is absent, the UE obtains the configuration for the SSB from *nr-SSB-Config* received as part of DL-PRS assistance data in LPP*,* see TS 37.355 [49], by looking up the corresponding SSB configuration using the field *physicalCellId*. |

|  |
| --- |
| ***DL-PRS-Info* field descriptions** |
| ***dl-PRS-ID***This field specifies the UE specific TRP ID (see TS 37.355 [49]) for which PRS configuration is provided.  |
| ***dl-PRS-ResourceSetId***This field specifies the PRS-ResourceSet ID of a PRS resourceSet. |
| ***dl-PRS-ResourceId***This field specifies the PRS-Resource ID of a PRS resource. If this field is absent, the UE determines the *dl-PRS-ResourceID* based on its PRS measurement from the TRP (see TS 37.355 [49]) and DL-PRS Resource Set. |

|  |
| --- |
| ***SSB-Configuration* field descriptions** |
| ***halfFrameIndex***Indicates whether SSB is in the first half or the second half of the frame.Value zero indicates the first half and value 1 indicates the second half. |
| ***integerSubframeOffset***Indicates the subframe boundary offset of the cell in which SSB is transmited. |
| ***sfn0-Offset***Indiactes the time offset of the SFN0 slot 0 for the cell with respect to SFN0 slot 0 of serving cell. |
| ***sfn-Offset***Specifies the SFN offset between the cell in which SSB is transmited and serving cell. The offset corresponds to the number of full radio frames counted from the beginning of a radio frame #0 of serving cell to the beginning of the closest subsequent radio frame #0 of the cell in which SSB is transmitted. |
| ***sfn-SSB-Offset***Indicates the SFN offset of the transmitted SSB relative to the start of the SSB period. Value 0 indicates that the SSB is transmitted in the first system frame, value 1 indicates that SSB is transmitted in the second system frame and so on. The network configures this field according to the field *ssb-Periodicity* such that the indicated system frame does not exceed the configured SSB periodicity. |
| ***ssb-Freq***Indicates the frequency of the SSB. |
| ***ss-PBCH-BlockPower***Average EPRE of the resources elements that carry secondary synchronization signals in dBm that the NW used for SSB transmission, see TS 38.213 [13], clause 7. |
| ***ssb-Periodicity***Indicates the periodicity of the SSB. If the field is absent, the UE applies the value ms5. (see TS 38.213 [13], clause 4.1) |
| ***ssbSubcarrierSpacing***Subcarrier spacing of SSB.Only the following values are applicable depending on the used frequency:FR1: 15 or 30 kHzFR2-1: 120 or 240 kHzFR2-2: 120, 480, or 960 kHz |

|  |  |
| --- | --- |
| **Conditional Presence** | **Explanation** |
| *Setup* | This field is mandatory present upon configuration of *SRS-ResourceSet* or *SRS-Resource* and optionally present, Need M, otherwise. |
| *NonCodebook* | This field is optionally present, Need M, in case of non-codebook based transmission, otherwise the field is absent. |
| *Pathloss* | The field is mandatory present if the IE *SSB-InfoNcell* is included in *pathlossReferenceRS-Pos*; otherwise it is optionally present, Need R |
| *DLorJointTCI-SRS* | The field is mandatory present if srs-DLorJointTCI-State is configured, otherwise it is absent Need R. |

*Next change*

### 6.3.3 UE capability information elements

<Text omitted>

– *Phy-Parameters*

The IE *Phy-Parameters* is used to convey the physical layer capabilities.

***Phy-Parameters* information element**

-- ASN1START

-- TAG-PHY-PARAMETERS-START

Phy-Parameters ::= SEQUENCE {

 phy-ParametersCommon Phy-ParametersCommon OPTIONAL,

 phy-ParametersXDD-Diff Phy-ParametersXDD-Diff OPTIONAL,

 phy-ParametersFRX-Diff Phy-ParametersFRX-Diff OPTIONAL,

 phy-ParametersFR1 Phy-ParametersFR1 OPTIONAL,

 phy-ParametersFR2 Phy-ParametersFR2 OPTIONAL

}

Phy-Parameters-v16a0 ::= SEQUENCE {

 phy-ParametersCommon-v16a0 Phy-ParametersCommon-v16a0 OPTIONAL

}

Phy-ParametersCommon ::= SEQUENCE {

 csi-RS-CFRA-ForHO ENUMERATED {supported} OPTIONAL,

 dynamicPRB-BundlingDL ENUMERATED {supported} OPTIONAL,

 sp-CSI-ReportPUCCH ENUMERATED {supported} OPTIONAL,

 sp-CSI-ReportPUSCH ENUMERATED {supported} OPTIONAL,

 nzp-CSI-RS-IntefMgmt ENUMERATED {supported} OPTIONAL,

 type2-SP-CSI-Feedback-LongPUCCH ENUMERATED {supported} OPTIONAL,

 precoderGranularityCORESET ENUMERATED {supported} OPTIONAL,

 dynamicHARQ-ACK-Codebook ENUMERATED {supported} OPTIONAL,

 semiStaticHARQ-ACK-Codebook ENUMERATED {supported} OPTIONAL,

 spatialBundlingHARQ-ACK ENUMERATED {supported} OPTIONAL,

 dynamicBetaOffsetInd-HARQ-ACK-CSI ENUMERATED {supported} OPTIONAL,

 pucch-Repetition-F1-3-4 ENUMERATED {supported} OPTIONAL,

 ra-Type0-PUSCH ENUMERATED {supported} OPTIONAL,

 dynamicSwitchRA-Type0-1-PDSCH ENUMERATED {supported} OPTIONAL,

 dynamicSwitchRA-Type0-1-PUSCH ENUMERATED {supported} OPTIONAL,

 pdsch-MappingTypeA ENUMERATED {supported} OPTIONAL,

 pdsch-MappingTypeB ENUMERATED {supported} OPTIONAL,

 interleavingVRB-ToPRB-PDSCH ENUMERATED {supported} OPTIONAL,

 interSlotFreqHopping-PUSCH ENUMERATED {supported} OPTIONAL,

 type1-PUSCH-RepetitionMultiSlots ENUMERATED {supported} OPTIONAL,

 type2-PUSCH-RepetitionMultiSlots ENUMERATED {supported} OPTIONAL,

 pusch-RepetitionMultiSlots ENUMERATED {supported} OPTIONAL,

 pdsch-RepetitionMultiSlots ENUMERATED {supported} OPTIONAL,

 downlinkSPS ENUMERATED {supported} OPTIONAL,

 configuredUL-GrantType1 ENUMERATED {supported} OPTIONAL,

 configuredUL-GrantType2 ENUMERATED {supported} OPTIONAL,

 pre-EmptIndication-DL ENUMERATED {supported} OPTIONAL,

 cbg-TransIndication-DL ENUMERATED {supported} OPTIONAL,

 cbg-TransIndication-UL ENUMERATED {supported} OPTIONAL,

 cbg-FlushIndication-DL ENUMERATED {supported} OPTIONAL,

 dynamicHARQ-ACK-CodeB-CBG-Retx-DL ENUMERATED {supported} OPTIONAL,

 rateMatchingResrcSetSemi-Static ENUMERATED {supported} OPTIONAL,

 rateMatchingResrcSetDynamic ENUMERATED {supported} OPTIONAL,

 bwp-SwitchingDelay ENUMERATED {type1, type2} OPTIONAL,

 ...,

 [[

 dummy ENUMERATED {supported} OPTIONAL

 ]],

 [[

 maxNumberSearchSpaces ENUMERATED {n10} OPTIONAL,

 rateMatchingCtrlResrcSetDynamic ENUMERATED {supported} OPTIONAL,

 maxLayersMIMO-Indication ENUMERATED {supported} OPTIONAL

 ]],

 [[

 spCellPlacement CarrierAggregationVariant OPTIONAL

 ]],

 [[

 -- R1 9-1: Basic channel structure and procedure of 2-step RACH

 twoStepRACH-r16 ENUMERATED {supported} OPTIONAL,

 -- R1 11-1: Monitoring DCI format 1\_2 and DCI format 0\_2

 dci-Format1-2And0-2-r16 ENUMERATED {supported} OPTIONAL,

 -- R1 11-1a: Monitoring both DCI format 0\_1/1\_1 and DCI format 0\_2/1\_2 in the same search space

 monitoringDCI-SameSearchSpace-r16 ENUMERATED {supported} OPTIONAL,

 -- R1 11-10: Type 2 configured grant release by DCI format 0\_1

 type2-CG-ReleaseDCI-0-1-r16 ENUMERATED {supported} OPTIONAL,

 -- R1 11-11: Type 2 configured grant release by DCI format 0\_2

 type2-CG-ReleaseDCI-0-2-r16 ENUMERATED {supported} OPTIONAL,

 -- R1 12-3: SPS release by DCI format 1\_1

 sps-ReleaseDCI-1-1-r16 ENUMERATED {supported} OPTIONAL,

 -- R1 12-3a: SPS release by DCI format 1\_2

 sps-ReleaseDCI-1-2-r16 ENUMERATED {supported} OPTIONAL,

 -- R1 14-8: CSI trigger states containing non-active BWP

 csi-TriggerStateNon-ActiveBWP-r16 ENUMERATED {supported} OPTIONAL,

 -- R1 20-2: Support up to 4 SMTCs configured for an IAB node MT per frequency location, including IAB-specific SMTC window periodicities

 separateSMTC-InterIAB-Support-r16 ENUMERATED {supported} OPTIONAL,

 -- R1 20-3: Support RACH configuration separately from the RACH configuration for UE access, including new IAB-specific offset and scaling factors

 separateRACH-IAB-Support-r16 ENUMERATED {supported} OPTIONAL,

 -- R1 20-5a: Support semi-static configuration/indication of UL-Flexible-DL slot formats for IAB-MT resources

 ul-flexibleDL-SlotFormatSemiStatic-IAB-r16 ENUMERATED {supported} OPTIONAL,

 -- R1 20-5b: Support dynamic indication of UL-Flexible-DL slot formats for IAB-MT resources

 ul-flexibleDL-SlotFormatDynamics-IAB-r16 ENUMERATED {supported} OPTIONAL,

 dft-S-OFDM-WaveformUL-IAB-r16 ENUMERATED {supported} OPTIONAL,

 -- R1 20-6: Support DCI Format 2\_5 based indication of soft resource availability to an IAB node

 dci-25-AI-RNTI-Support-IAB-r16 ENUMERATED {supported} OPTIONAL,

 -- R1 20-7: Support T\_delta reception.

 t-DeltaReceptionSupport-IAB-r16 ENUMERATED {supported} OPTIONAL,

 -- R1 20-8: Support of Desired guard symbol reporting and provided guard symbok reception.

 guardSymbolReportReception-IAB-r16 ENUMERATED {supported} OPTIONAL,

 -- R1 18-8 HARQ-ACK codebook type and spatial bundling per PUCCH group

 harqACK-CB-SpatialBundlingPUCCH-Group-r16 ENUMERATED {supported} OPTIONAL,

 -- R1 19-2: Cross Slot Scheduling

 crossSlotScheduling-r16 SEQUENCE {

 non-SharedSpectrumChAccess-r16 ENUMERATED {supported} OPTIONAL,

 sharedSpectrumChAccess-r16 ENUMERATED {supported} OPTIONAL

 } OPTIONAL,

 maxNumberSRS-PosPathLossEstimateAllServingCells-r16 ENUMERATED {n1, n4, n8, n16} OPTIONAL,

 extendedCG-Periodicities-r16 ENUMERATED {supported} OPTIONAL,

 extendedSPS-Periodicities-r16 ENUMERATED {supported} OPTIONAL,

 codebookVariantsList-r16 CodebookVariantsList-r16 OPTIONAL,

 -- R1 11-6: PUSCH repetition Type A

 pusch-RepetitionTypeA-r16 SEQUENCE {

 sharedSpectrumChAccess-r16 ENUMERATED {supported} OPTIONAL,

 non-SharedSpectrumChAccess-r16 ENUMERATED {supported} OPTIONAL

 } OPTIONAL,

 -- R1 11-4b: DL priority indication in DCI with mixed DCI formats

 dci-DL-PriorityIndicator-r16 ENUMERATED {supported} OPTIONAL,

 -- R1 12-1a: UL priority indication in DCI with mixed DCI formats

 dci-UL-PriorityIndicator-r16 ENUMERATED {supported} OPTIONAL,

 -- R1 16-1e: Maximum number of configured pathloss reference RSs for PUSCH/PUCCH/SRS by RRC for MAC-CE based pathloss reference RS update

 maxNumberPathlossRS-Update-r16 ENUMERATED {n4, n8, n16, n32, n64} OPTIONAL,

 -- R1 18-9: Usage of the PDSCH starting time for HARQ-ACK type 2 codebook

 type2-HARQ-ACK-Codebook-r16 ENUMERATED {supported} OPTIONAL,

 -- R1 16-1g-1: Resources for beam management, pathloss measurement, BFD, RLM and new beam identification across frequency ranges

 maxTotalResourcesForAcrossFreqRanges-r16 SEQUENCE {

 maxNumberResWithinSlotAcrossCC-AcrossFR-r16 ENUMERATED {n2, n4, n8, n12, n16, n32, n64, n128} OPTIONAL,

 maxNumberResAcrossCC-AcrossFR-r16 ENUMERATED {n2, n4, n8, n12, n16, n32, n40, n48, n64, n72, n80, n96, n128, n256}

 OPTIONAL

 } OPTIONAL,

 -- R1 16-2a-4: HARQ-ACK for multi-DCI based multi-TRP - separate

 harqACK-separateMultiDCI-MultiTRP-r16 SEQUENCE {

 maxNumberLongPUCCHs-r16 ENUMERATED {longAndLong, longAndShort, shortAndShort} OPTIONAL

 } OPTIONAL,

 -- R1 16-2a-4: HARQ-ACK for multi-DCI based multi-TRP - joint

 harqACK-jointMultiDCI-MultiTRP-r16 ENUMERATED {supported} OPTIONAL,

 -- R4 9-1: BWP switching on multiple CCs RRM requirements

 bwp-SwitchingMultiCCs-r16 CHOICE {

 type1-r16 ENUMERATED {us100, us200},

 type2-r16 ENUMERATED {us200, us400, us800, us1000}

 } OPTIONAL

 ]],

 [[

 targetSMTC-SCG-r16 ENUMERATED {supported} OPTIONAL,

 supportRepetitionZeroOffsetRV-r16 ENUMERATED {supported} OPTIONAL,

 -- R1 11-12: in-order CBG-based re-transmission

 cbg-TransInOrderPUSCH-UL-r16 ENUMERATED {supported} OPTIONAL

 ]],

 [[

 -- R4 6-3: Dormant BWP switching on multiple CCs RRM requirements

 bwp-SwitchingMultiDormancyCCs-r16 CHOICE {

 type1-r16 ENUMERATED {us100, us200},

 type2-r16 ENUMERATED {us200, us400, us800, us1000}

 } OPTIONAL,

 -- R1 16-2a-8: Indicates that retransmission scheduled by a different CORESETPoolIndex for multi-DCI multi-TRP is not supported.

 supportRetx-Diff-CoresetPool-Multi-DCI-TRP-r16 ENUMERATED {notSupported} OPTIONAL,

 -- R1 22-10: Support of pdcch-MonitoringAnyOccasionsWithSpanGap in case of cross-carrier scheduling with different SCSs

 pdcch-MonitoringAnyOccasionsWithSpanGapCrossCarrierSch-r16 ENUMERATED {mode2, mode3} OPTIONAL

 ]],

 [[

 -- R1 16-1j-1: Support of 2 port CSI-RS for new beam identification

 newBeamIdentifications2PortCSI-RS-r16 ENUMERATED {supported} OPTIONAL,

 -- R1 16-1j-2: Support of 2 port CSI-RS for pathloss estimation

 pathlossEstimation2PortCSI-RS-r16 ENUMERATED {supported} OPTIONAL

 ]],

 [[

 mux-HARQ-ACK-withoutPUCCH-onPUSCH-r16 ENUMERATED {supported} OPTIONAL

 ]],

 [[

 -- R1 31-1: Support of Desired Guard Symbol reporting and provided guard symbol reception.

 guardSymbolReportReception-IAB-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 31-2: support of restricted IAB-DU beam reception

 restricted-IAB-DU-BeamReception-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 31-3: support of recommended IAB-MT beam transmission for DL and UL beam

 recommended-IAB-MT-BeamTransmission-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 31-4: support of case 6 timing alignment indication reception

 case6-TimingAlignmentReception-IAB-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 31-5: support of case 7 timing offset indication reception and case 7 timing at parent-node indication reception

 case7-TimingAlignmentReception-IAB-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 31-6: support of desired DL Tx power adjustment reporting and DL Tx power adjustment reception

 dl-tx-PowerAdjustment-IAB-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 31-7: support of desired IAB-MT PSD range reporting

 desired-ul-tx-PowerAdjustment-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 31-8: support of monitoring DCI Format 2\_5 scrambled by AI-RNTI for indication of FDM soft resource availability to an IAB node

 fdm-SoftResourceAvailability-DynamicIndication-r17 ENUMERATED{supported} OPTIONAL,

 -- R1 31-10: Support of updated T\_delta range reception

 updated-T-DeltaRangeReception-r17 ENUMERATED{supported} OPTIONAL,

 -- R1 30-5: Support slot based dynamic PUCCH repetition indication for PUCCH formats 0/1/2/3/4

 slotBasedDynamicPUCCH-Rep-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 25-1: Support of HARQ-ACK deferral in case of TDD collision

 sps-HARQ-ACK-Deferral-r17 SEQUENCE {

 non-SharedSpectrumChAccess-r17 ENUMERATED {supported} OPTIONAL,

 sharedSpectrumChAccess-r17 ENUMERATED {supported} OPTIONAL

 } OPTIONAL,

 -- R1 23-1-1k Maximum number of configured CC lists (per UE)

 unifiedJointTCI-commonUpdate-r17 INTEGER (1..4) OPTIONAL,

 -- R1 23-2-1c PDCCH repetition with a single span of three contiguous OFDM symbols that is within the first four OFDM symbols in a slot

 mTRP-PDCCH-singleSpan-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 27-23: Support of more than one activated PRS processing windows across all active DL BWPs

 supportedActivatedPRS-ProcessingWindow-r17 ENUMERATED {n2, n3, n4} OPTIONAL,

 cg-TimeDomainAllocationExtension-r17 ENUMERATED {supported} OPTIONAL

 ]],

 [[

 -- R1 25-20: Propagation delay compensation based on legacy TA procedure for TN and licensed

 ta-BasedPDC-TN-NonSharedSpectrumChAccess-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 31-11: Directional Collision Handling in DC operation

 directionalCollisionDC-IAB-r17 ENUMERATED {supported} OPTIONAL

 ]],

 [[

 dummy1 ENUMERATED {supported} OPTIONAL,

 dummy2 ENUMERATED {supported} OPTIONAL,

 dummy3 ENUMERATED {supported} OPTIONAL,

 dummy4 ENUMERATED {supported} OPTIONAL,

 srs-AdditionalRepetition-r17 ENUMERATED {supported} OPTIONAL,

 pusch-Repetition-CG-SDT-r17 ENUMERATED {supported} OPTIONAL

 ]]

}

Phy-ParametersCommon-v16a0 ::= SEQUENCE {

 srs-PeriodicityAndOffsetExt-r16 ENUMERATED {supported} OPTIONAL

}

Phy-ParametersXDD-Diff ::= SEQUENCE {

 dynamicSFI ENUMERATED {supported} OPTIONAL,

 twoPUCCH-F0-2-ConsecSymbols ENUMERATED {supported} OPTIONAL,

 twoDifferentTPC-Loop-PUSCH ENUMERATED {supported} OPTIONAL,

 twoDifferentTPC-Loop-PUCCH ENUMERATED {supported} OPTIONAL,

 ...,

 [[

 dl-SchedulingOffset-PDSCH-TypeA ENUMERATED {supported} OPTIONAL,

 dl-SchedulingOffset-PDSCH-TypeB ENUMERATED {supported} OPTIONAL,

 ul-SchedulingOffset ENUMERATED {supported} OPTIONAL

 ]]

}

Phy-ParametersFRX-Diff ::= SEQUENCE {

 dynamicSFI ENUMERATED {supported} OPTIONAL,

 dummy1 BIT STRING (SIZE (2)) OPTIONAL,

 twoFL-DMRS BIT STRING (SIZE (2)) OPTIONAL,

 dummy2 BIT STRING (SIZE (2)) OPTIONAL,

 dummy3 BIT STRING (SIZE (2)) OPTIONAL,

 supportedDMRS-TypeDL ENUMERATED {type1, type1And2} OPTIONAL,

 supportedDMRS-TypeUL ENUMERATED {type1, type1And2} OPTIONAL,

 semiOpenLoopCSI ENUMERATED {supported} OPTIONAL,

 csi-ReportWithoutPMI ENUMERATED {supported} OPTIONAL,

 csi-ReportWithoutCQI ENUMERATED {supported} OPTIONAL,

 onePortsPTRS BIT STRING (SIZE (2)) OPTIONAL,

 twoPUCCH-F0-2-ConsecSymbols ENUMERATED {supported} OPTIONAL,

 pucch-F2-WithFH ENUMERATED {supported} OPTIONAL,

 pucch-F3-WithFH ENUMERATED {supported} OPTIONAL,

 pucch-F4-WithFH ENUMERATED {supported} OPTIONAL,

 pucch-F0-2WithoutFH ENUMERATED {notSupported} OPTIONAL,

 pucch-F1-3-4WithoutFH ENUMERATED {notSupported} OPTIONAL,

 mux-SR-HARQ-ACK-CSI-PUCCH-MultiPerSlot ENUMERATED {supported} OPTIONAL,

 uci-CodeBlockSegmentation ENUMERATED {supported} OPTIONAL,

 onePUCCH-LongAndShortFormat ENUMERATED {supported} OPTIONAL,

 twoPUCCH-AnyOthersInSlot ENUMERATED {supported} OPTIONAL,

 intraSlotFreqHopping-PUSCH ENUMERATED {supported} OPTIONAL,

 pusch-LBRM ENUMERATED {supported} OPTIONAL,

 pdcch-BlindDetectionCA INTEGER (4..16) OPTIONAL,

 tpc-PUSCH-RNTI ENUMERATED {supported} OPTIONAL,

 tpc-PUCCH-RNTI ENUMERATED {supported} OPTIONAL,

 tpc-SRS-RNTI ENUMERATED {supported} OPTIONAL,

 absoluteTPC-Command ENUMERATED {supported} OPTIONAL,

 twoDifferentTPC-Loop-PUSCH ENUMERATED {supported} OPTIONAL,

 twoDifferentTPC-Loop-PUCCH ENUMERATED {supported} OPTIONAL,

 pusch-HalfPi-BPSK ENUMERATED {supported} OPTIONAL,

 pucch-F3-4-HalfPi-BPSK ENUMERATED {supported} OPTIONAL,

 almostContiguousCP-OFDM-UL ENUMERATED {supported} OPTIONAL,

 sp-CSI-RS ENUMERATED {supported} OPTIONAL,

 sp-CSI-IM ENUMERATED {supported} OPTIONAL,

 tdd-MultiDL-UL-SwitchPerSlot ENUMERATED {supported} OPTIONAL,

 multipleCORESET ENUMERATED {supported} OPTIONAL,

 ...,

 [[

 csi-RS-IM-ReceptionForFeedback CSI-RS-IM-ReceptionForFeedback OPTIONAL,

 csi-RS-ProcFrameworkForSRS CSI-RS-ProcFrameworkForSRS OPTIONAL,

 csi-ReportFramework CSI-ReportFramework OPTIONAL,

 mux-SR-HARQ-ACK-CSI-PUCCH-OncePerSlot SEQUENCE {

 sameSymbol ENUMERATED {supported} OPTIONAL,

 diffSymbol ENUMERATED {supported} OPTIONAL

 } OPTIONAL,

 mux-SR-HARQ-ACK-PUCCH ENUMERATED {supported} OPTIONAL,

 mux-MultipleGroupCtrlCH-Overlap ENUMERATED {supported} OPTIONAL,

 dl-SchedulingOffset-PDSCH-TypeA ENUMERATED {supported} OPTIONAL,

 dl-SchedulingOffset-PDSCH-TypeB ENUMERATED {supported} OPTIONAL,

 ul-SchedulingOffset ENUMERATED {supported} OPTIONAL,

 dl-64QAM-MCS-TableAlt ENUMERATED {supported} OPTIONAL,

 ul-64QAM-MCS-TableAlt ENUMERATED {supported} OPTIONAL,

 cqi-TableAlt ENUMERATED {supported} OPTIONAL,

 oneFL-DMRS-TwoAdditionalDMRS-UL ENUMERATED {supported} OPTIONAL,

 twoFL-DMRS-TwoAdditionalDMRS-UL ENUMERATED {supported} OPTIONAL,

 oneFL-DMRS-ThreeAdditionalDMRS-UL ENUMERATED {supported} OPTIONAL

 ]],

 [[

 pdcch-BlindDetectionNRDC SEQUENCE {

 pdcch-BlindDetectionMCG-UE INTEGER (1..15),

 pdcch-BlindDetectionSCG-UE INTEGER (1..15)

 } OPTIONAL,

 mux-HARQ-ACK-PUSCH-DiffSymbol ENUMERATED {supported} OPTIONAL

 ]],

 [[

 -- R1 11-1b: Type 1 HARQ-ACK codebook support for relative TDRA for DL

 type1-HARQ-ACK-Codebook-r16 ENUMERATED {supported} OPTIONAL,

 -- R1 11-8: Enhanced UL power control scheme

 enhancedPowerControl-r16 ENUMERATED {supported} OPTIONAL,

 -- R1 16-1b-1: TCI state activation across multiple CCs

 simultaneousTCI-ActMultipleCC-r16 ENUMERATED {supported} OPTIONAL,

 -- R1 16-1b-2: Spatial relation update across multiple CCs

 simultaneousSpatialRelationMultipleCC-r16 ENUMERATED {supported} OPTIONAL,

 cli-RSSI-FDM-DL-r16 ENUMERATED {supported} OPTIONAL,

 cli-SRS-RSRP-FDM-DL-r16 ENUMERATED {supported} OPTIONAL,

 -- R1 19-3: Maximum MIMO Layer Adaptation

 maxLayersMIMO-Adaptation-r16 ENUMERATED {supported} OPTIONAL,

 -- R1 12-5: Configuration of aggregation factor per SPS configuration

 aggregationFactorSPS-DL-r16 ENUMERATED {supported} OPTIONAL,

 -- R1 16-1g: Resources for beam management, pathloss measurement, BFD, RLM and new beam identification

 maxTotalResourcesForOneFreqRange-r16 SEQUENCE {

 maxNumberResWithinSlotAcrossCC-OneFR-r16 ENUMERATED {n2, n4, n8, n12, n16, n32, n64, n128} OPTIONAL,

 maxNumberResAcrossCC-OneFR-r16 ENUMERATED {n2, n4, n8, n12, n16, n32, n40, n48, n64, n72, n80, n96, n128, n256}

 OPTIONAL

 } OPTIONAL,

 -- R1 16-7: Extension of the maximum number of configured aperiodic CSI report settings

 csi-ReportFrameworkExt-r16 CSI-ReportFrameworkExt-r16 OPTIONAL

 ]],

 [[

 twoTCI-Act-servingCellInCC-List-r16 ENUMERATED {supported} OPTIONAL

 ]],

 [[

 -- R1 22-11: Support of 'cri-RI-CQI' report without non-PMI-PortIndication

 cri-RI-CQI-WithoutNon-PMI-PortInd-r16 ENUMERATED {supported} OPTIONAL

 ]],

 [[

 -- R1 25-11: 4-bits subband CQI for TN and licensed

 cqi-4-BitsSubbandTN-NonSharedSpectrumChAccess-r17 ENUMERATED {supported} OPTIONAL

 ]]

}

Phy-ParametersFR1 ::= SEQUENCE {

 pdcch-MonitoringSingleOccasion ENUMERATED {supported} OPTIONAL,

 scs-60kHz ENUMERATED {supported} OPTIONAL,

 pdsch-256QAM-FR1 ENUMERATED {supported} OPTIONAL,

 pdsch-RE-MappingFR1-PerSymbol ENUMERATED {n10, n20} OPTIONAL,

 ...,

 [[

 pdsch-RE-MappingFR1-PerSlot ENUMERATED {n16, n32, n48, n64, n80, n96, n112, n128,

 n144, n160, n176, n192, n208, n224, n240, n256} OPTIONAL

 ]],

 [[

 -- R1 22-12: PDCCH monitoring with a single span of three contiguous OFDM symbols that is within the first four OFDM symbols in a

 -- slot

 pdcch-MonitoringSingleSpanFirst4Sym-r16 ENUMERATED {supported} OPTIONAL

 ]]

}

Phy-ParametersFR2 ::= SEQUENCE {

 dummy ENUMERATED {supported} OPTIONAL,

 pdsch-RE-MappingFR2-PerSymbol ENUMERATED {n6, n20} OPTIONAL,

 ...,

 [[

 pCell-FR2 ENUMERATED {supported} OPTIONAL,

 pdsch-RE-MappingFR2-PerSlot ENUMERATED {n16, n32, n48, n64, n80, n96, n112, n128,

 n144, n160, n176, n192, n208, n224, n240, n256} OPTIONAL

 ]],

 [[

 -- R1 16-1c: Support of default spatial relation and pathloss reference RS for dedicated-PUCCH/SRS and PUSCH

 defaultSpatialRelationPathlossRS-r16 ENUMERATED {supported} OPTIONAL,

 -- R1 16-1d: Support of spatial relation update for AP-SRS via MAC CE

 spatialRelationUpdateAP-SRS-r16 ENUMERATED {supported} OPTIONAL,

 maxNumberSRS-PosSpatialRelationsAllServingCells-r16 ENUMERATED {n0, n1, n2, n4, n8, n16} OPTIONAL

 ]]

}

-- TAG-PHY-PARAMETERS-STOP

-- ASN1STOP

|  |
| --- |
| ***Phy-ParametersFRX-Diff* field descriptions** |
| ***csi-RS-IM-ReceptionForFeedback/ csi-RS-ProcFrameworkForSRS/ csi-ReportFramework***These fields are optionally present in *fr1-fr2-Add-UE-NR-Capabilities* in *UE-NR-Capability*. They shall not be set in any other instance of the IE *Phy-ParametersFRX-Diff*. If the network configures the UE with serving cells on both FR1 and FR2 bands, these parameters, if present, limit the corresponding parameters in *MIMO-ParametersPerBand*. |

### 6.3.4 Other information elements

<Text omitted>

– *AppLayerMeasConfig*

The IE *AppLayerMeasConfig* indicates configuration of application layer measurements.

***AppLayerMeasConfig* information element**

-- ASN1START

-- TAG-APPLAYERMEASCONFIG-START

AppLayerMeasConfig-r17 ::= SEQUENCE {

 measConfigAppLayerToAddModList-r17 SEQUENCE (SIZE (1..maxNrofAppLayerMeas-r17)) OF MeasConfigAppLayer-r17 OPTIONAL, -- Need N

 measConfigAppLayerToReleaseList-r17 SEQUENCE (SIZE (1..maxNrofAppLayerMeas-r17)) OF MeasConfigAppLayerId-r17 OPTIONAL, -- Need N

 rrc-SegAllowed-r17 ENUMERATED {enabled} OPTIONAL, -- Need R

 ...

}

MeasConfigAppLayer-r17 ::= SEQUENCE {

 measConfigAppLayerId-r17 MeasConfigAppLayerId-r17,

 measConfigAppLayerContainer-r17 OCTET STRING (SIZE (1..8000)) OPTIONAL, -- Need N

 serviceType-r17 ENUMERATED {streaming, mtsi, vr, spare5, spare4, spare3, spare2, spare1} OPTIONAL, -- Need M

 pauseReporting-r17 BOOLEAN OPTIONAL, -- Need M

 transmissionOfSessionStartStop-r17 BOOLEAN OPTIONAL, -- Need M

 ran-VisibleParameters-r17 SetupRelease {RAN-VisibleParameters-r17} OPTIONAL, -- Cond ServiceType

 ...

}

RAN-VisibleParameters-r17 ::= SEQUENCE {

 ran-VisiblePeriodicity-r17 ENUMERATED {ms120, ms240, ms480, ms640, ms1024} OPTIONAL, -- Need S

 numberOfBufferLevelEntries-r17 INTEGER (1..8) OPTIONAL, -- Need R

 reportPlayoutDelayForMediaStartup-r17 BOOLEAN OPTIONAL, -- Need M

 ...

}

-- TAG-APPLAYERMEASCONFIG-STOP

-- ASN1STOP

|  |
| --- |
| ***AppLayerMeasConfig* field descriptions** |
| ***measConfigAppLayerContainer***The field contains configuration of application layer measurements, see Annex L (normative) in TS 26.247 [68], clause 16.5 in TS 26.114 [69] and TS 26.118 [70]. |
| ***pauseReporting***The field indicates whether the transmission of *measReportAppLayerContainer* is paused or not. Value *true* indicates the transmission of *measReportAppLayerContainer* is paused; value *false* indicates the transmission of *measReportAppLayerContainer* is not paused. |
| ***ran-VisibleParameters***The field indicates whether RAN visible application layer measurements shall be reported or not. |
| ***rrc-SegAllowed***This field indicates that RRC segmentation of *MeasurementReportAppLayer* is enabled. It may be present only if the UE supports RRC segmentation of the *MeasurementReportAppLayer* message in UL***.*** |
| ***serviceType***Indicates the type of application layer measurement. Value *streaming* indicates Quality of Experience Measurement Collection for streaming services (see TS 26.247 [68]), value *mtsi* indicates Quality of Experience Measurement Collection for MTSI (see TS 26.114 [69]) and value *vr* indicates Quality of Experience Measurement Collection for VR service (see TS 26.118 [70]). The network always configures *serviceType* when application layer measurements are initially configured and at *fullConfig*. |
| ***transmissionOfSessionStartStop***Value *true* indicates that the UE shall transmit indications when the measurement session in the application layer starts and stops. Value *false* indicates that the UE shall not transmit any session status indications. The UE transmits a session start indication upon configuration of this field set to value *true* if a session already has started in the application layer. |

|  |
| --- |
| ***RAN-VisibleParameters* field descriptions** |
| ***numberOfBufferLevelEntries***The field contains the maximum number of buffer level entries that can be reported for RAN visible application layer measurements. This field is also used by application layer to calculate the interval of RAN visible buffer level measurement, which is equal to the periodicity of RAN visible application layer measurements reporting divided by *numberOfBufferLevelEntries*. |
| ***ran-VisiblePeriodicity***The field indicates the periodicity of RAN visible application layer measurements reporting. Value *ms120* indicates 120 ms, value *ms240* indicates 240 ms and so on. If this field is absent, the periodicity of RAN visible application layer measurements reporting is the same as the reporting periodicity indicated in *measConfigAppLayerContainer.* |
| ***reportPlayoutDelayForMediaStartup***The field indicates whether the UE shall report Playout Delay for Media Startup for RAN visible application layer measurements. |

|  |  |
| --- | --- |
| **Conditional Presence** | **Explanation** |
| *ServiceType* | This field is optionally present, Need M, when *serviceType* is set to *streaming* or *vr*. Otherwise, it is absent. |

*End of changes*