**3GPP TSG-RAN WG2 Meeting #123 *R2-23XXX***

**Toulouse, France, August 21 – 25, 2023**

Agenda Item: 7.4.2.3

Source: Huawei, HiSilicon

**Title:** **Summary of [Post122][058][Mob18] Contents of Cell Switch MAC CE**

Document for: Discussion and Decision

# Introduction

* [Post122][058][Mob18] Contents of Cell Switch MAC CE (Huawei)

Scope: Starting from proposals to R2 122 viewed in the light of agreements taken so far. Determine potentially agreeable points and points for discussion at R2 123 (open points)

Intended Outcome: Report

Deadline: Long

**Contact information**

|  |  |
| --- | --- |
| **Company** | **Name (Email)** |
| Huawei, HiSilicon | Yulong (shiyulong5@huawei.com) |
| Samsung | Anil Agiwal (anilag@samsung.com) |
| MediaTek | Li-Chuan Tseng (li-chuan.tseng@mediatek.com) |
| Futurewei | Jialin Zou (jialinzou88@yahoo.com) |
| Qualcomm | Ozcan Ozturk (oozturk@qti.qualcomm.com) |
| Apple | Naveen Palle ( naveen.palle@apple.com) |
| CATT | Rui Zhou(zhourui@catt.cn) |
| ZTE | Fei Dong (dong.fei@zte.com.cn) |
| Ericsson | Antonino Orsino (antonino.orsino@ericsson.com) |
|  |  |
|  |  |
|  |  |
|  |  |

**Related proposals @RAN2#122 meeting**

|  |  |
| --- | --- |
| **Tdoc** | **Proposal** |
| [R2-2304688](file:///D:\Tdoc%20review\RAN2%23122\word\R2-2304688%20Discussions%20on%20cell%20switch.docx) CATT | Proposal 1: The LTM triggering MAC CE can include the following information,   * TCI state indication information; * TA information for target cell; * Value of LTM supervisor timer; * Preamble index for intra-DU CFRA-based LTM, FFS for inter-DU.   Proposal 2: The BWP indication information is not included in the LTM triggering MAC CE.  Proposal 3: Do not support SCell activation/deactivation via the LTM triggering MAC CE. |
| [R2-2304720](file:///D:\Tdoc%20review\RAN2%23122\word\R2-2304720_Remaining%20issues%20for%20Cell%20Switching.doc) Samsung Electronics Co., Ltd | Proposal 1: RAN2 to discuss and agree on one of the following options  Option 1: BWP IDs of BWPs to activate upon receiving cell change command are always signaled in MAC CE used for cell change.  Option 2: For LTM, the fields’ firstActiveUplinkBWP and firstActiveDownlinkBWP are signaled in L1/L2 inter-cell mobility candidate (target) configuration. If BWP IDs of BWPs to activate are not included in MAC CE used for cell change, UE activates and uses BWPs indicated by these fields upon receiving cell change command.  Proposal 7: RAN2 to discuss and agree on one of the following for RA resources for RA upon cell switch command   * Approach 1: UE is configured with CFRA resources (list of one or more [preamble index/PO index/SSB index]) in candidate cell configuration in same manner as configured during the legacy handover/reconfiguration with sync i.e. by signaling rach-ConfigDedicated in candidate cell configuration. Common RACH configuration/parameters from RACH-ConfigCommon/ RACH-ConfigCommonTwoStepRA of BWP selected are used during RA procedure.   + Principles of RA type selection, carrier selection as in legacy handover/reconfiguration with sync are applied. * Approach 2: UE is configured with CFRA resources (list of one or more [preamble index/PO index/SSB index]) in cell switch command. Common RACH configuration/parameters from RACH-ConfigCommon/ RACH-ConfigCommonTwoStepRA of BWP selected are used during RA procedure. The advantage of this is that UE can be configured with CFRA resources for SSB (s) based on latest measurement results. * Approach 3: UE is not configured with CFRA resources. Common RACH configuration/parameters from RACH-ConfigCommon/ RACH-ConfigCommonTwoStepRA of BWP selected are used during RA procedure.   Proposal 8: Value indicating that the UE shall apply the TA of one source cell is not signalled in cell switch command. |
| [R2-2304889](file:///D:\Tdoc%20review\RAN2%23122\word\R2-2304889%20Open%20Issues%20for%20LTM%20Procedure.docx) MediaTek Inc. | Proposal 2: In RACH-less LTM, network should provide UL grant for the first UL message in target cell. RAN2 to discuss the method, e.g.,   * Configured grant in candidate RRC configuration, or * UL grant field in LTM command MAC CE. |
| [R2-2304891](file:///D:\Tdoc%20review\RAN2%23122\word\R2-2304891%20Triggering%20MAC%20CE%20for%20LTM.docx) MediaTek Inc. | Proposal 1: The LTM command MAC CE should include at least the following fields:   * + Candidate configuration identity: [2] bits   + TCI state ID(s): [7] bits for joint/DL TCI state, [6] bits for UL TCI state   + Joint or separate TCI state indication: 1 bit   + DL/UL indication: 1 bit   + TA value: [12] bits   + BWP IDs: 2 bits for DL BWP and 2 bits for UL BWP   Proposal 2: Wait for RAN1 decision on the following fields in LTM command MAC CE:   * Triggering of aperiodic TRS transmitted from the target cell * Triggering the CSI acquisition of the target cell and reporting to the target cell * Triggering of aperiodic SRS transmission to the target cell * Additional TCI state activation   Proposal 3: RAN2 to decide the following fields in the LTM command MAC CE, after agreements on related discussions:   * Serving cell index * SCell activation/deactivation * CFRA resources availability * UL grant for the first message * C-RNTI |
| [R2-2304909](file:///D:\Tdoc%20review\RAN2%23122\word\R2-2304909_Remaining%20issues%20on%20LTM%20procedures.docx) vivo | Proposal 6: A CFRA resource indication can be introduced in LTM cell switch command. Only when the indication indicates CFRA resource is available, UE applies the CFRA resource configured in the candidate cell configuration to access the target cell during LTM.  Proposal 7: Dedicated RACH resource can be included in LTM cell switch command. If LTM cell switch command indicates RACH resource (shared by multiple UE in S-DU, S-DU ensures no collision occurs), UE applies the RACH resource to access the target cell.  Proposal 8: For RACH-less LTM, a candidate cell can provide a UL resource poor to source DU. And source DU can dynamically allocate the UL resource of the pool to UE in LTM cell switch command. UE can use the indicated UL resource to send the first UL PDU in the target cell. |
| [R2-2304911](file:///D:\Tdoc%20review\RAN2%23122\word\R2-2304911_RRC%20configuration%20for%20LTM.docx) vivo | Proposal 12: UE determines the BWPs (for DL and UL) to be activated upon the execution of LTM based on the firstActivateDownlinkBWP-Id and firstActivateUplinkBWP-Id within the configuration of target cell(s).  Proposal 13: Upon the reception of LTM cell switch command, UE performs target SCell activation/deactivation based on the indication (i.e. sCellState field) within the pre-configured RRC configuration of target SCells. |
| [R2-2304953](file:///D:\Tdoc%20review\RAN2%23122\word\R2-2304953%20cell%20switch_v1.docx) Fujitsu | Proposal 1: At least the following information can be included in the LTM cell switch command MAC CE:   * Information to identify the target cell(s), FFS for the details, e.g. a set ID, a candidate configuration index and the indication of SpCell * TA related information * Unified TCI state index for the target cell, depending on RAN1 * Active DL and UL BWPs for the target cell, if it is different from the first active BWP signaled by RRC configuration   Proposal 2: In addition to existing SCell activation/deactivation mechanisms, the SCell activation/ deactivation state can be included in the LTM cell switch command MAC CE for intra-DU case so that the SCell activation/deactivation will be performed simultaneously with SpCell change.  Proposal 4: RAN2 to discuss how to handle the activated SCells which are unchanged after the LTM cell switch. |
| [R2-2305167](file:///D:\Tdoc%20review\RAN2%23122\word\R2-2305167%20NR%20MOB%20MAC%20CE.docx) Interdigital, Inc. | Proposal 1: The content of the cell switch MAC CE at least consists of:   1. Candidate configuration ID (already agreed) 2. TA related information (agreed by RAN1) 3. 1 joint or 1 pair of UL and DL unified TCI State index for the target Cell (agreed by RAN1) 4. Active DL and UL BWPs for the target cell (agreed by RAN1) 5. FFS RAN1: Triggering of aperiodic TRS transmitted from the target cell 6. FFS RAN1: Triggering the CSI acquisition of the target cell and reporting to the target cell 7. FFS RAN1: Triggering of aperiodic SRS transmission to the target cell 8. FFS RAN1: C-RNTI   FFS: the presence of each field (i.e. always present or configurable)  Proposal 2: By default the initial SCell state on the target cell after LTM cell switch is based on RRC configuration sCellState. At least for the intra-DU case, NW may indicate a new SpCell candidate configuration index and perform SCell activation/deactivation simultaneously using MAC CE.  Proposal 3: BWP can be indicated in the RRC configuration of candidate cells, MAC CE indication in cell switch command is optional.  Proposal 4: RAN2 to discuss whether the cell switch MAC CE may contain an indication of RACH resource and/or UL grant for the target cell. |
| [R2-2305295](file:///D:\Tdoc%20review\RAN2%23122\word\R2-2305295%20-%20Discussion%20on%20MAC%20CE%20content%20and%20partial%20MAC%20reset%20for%20LTM.docx) OPPO | [Proposal 1 LTM cell switch MAC CE can indicate TCI state info, i.e., 1 joint or 1 pair of UL and DL unified TCI State index for the target cell.](#_Toc134795825)  [Proposal 2 LTM cell switch MAC CE can contain TA info, if any.](#_Toc134795826)  [Proposal 3 SCell activation/deactivation indication is not contained in LTM cell switch MAC CE.](#_Toc134795827)  [Proposal 4 BWP information is not contained in LTM cell switch MAC CE.](#_Toc134795828)  [Proposal 5 CFRA resource is not contained in LTM cell switch MAC CE.](#_Toc134795829) |
| [R2-2305541](file:///D:\Tdoc%20review\RAN2%23122\word\R2-2305541%20LTM%20command%20MAC%20CE%20content%20and%20RAN3%20LS%20reply.docx) Huawei, HiSilicon, CATT, ZTE Corporation, Sanechips, vivo, China Unicom | Proposal 1: To support SCell activation simultaneously with LTM execution, the network (target cell) can set the “sCellState-r16” in the candidate configuration by RRC as supported currently, i.e. no need to include the SCell activation/deactivation in LTM MAC CE.  Proposal 2: In inter-DU LTM, RAN2 excludes to include the active BWP ID in the LTM MAC CE. (FFS for intra-DU LTM) |
| [R2-2305576](file:///D:\Tdoc%20review\RAN2%23122\word\R2-2305576%20Contents%20of%20cell%20switch%20MAC%20CE.docx) Xiaomi | Proposal 1: The initial SCell state can be indicated by sCellState-r16 or the cell switch MAC CE.  Proposal 2: The dedicated PRACH resource can be indicated by the cell switch MAC CE. |
| [R2-2305641](file:///D:\Tdoc%20review\RAN2%23122\word\R2-2305641%3fFurther%20considerations%20on%20cell%20switch.doc) CMCC | Proposal 1: RAN2 to confirm that TCI state is supported in an MAC CE carrying LTM switch command.  Proposal 2: RAN2 to confirm that TA value is supported in an MAC CE carrying LTM switch command.  Proposal 3: RAN2 to confirm that L2 reset indication is not included in an MAC CE carrying LTM switch command.  Proposal 4: RAN2 to confirm that CFRA resource are not included in the MAC CE carrying LTM switch command.  Proposal 5: RAN2 to confirm that CFRA indication (i.e., valid or invalid) is included in the MAC CE carrying LTM switch command. |
| [R2-2305649](file:///D:\Tdoc%20review\RAN2%23122\word\R2-2305649%20Cell%20switch.docx) NEC | Proposal 3: If RAN2 can agree that the network can send the SCell Activation/Deactivation MAC CE with the LTM cell switch command MAC CE, it is up to network whether to activate/deactivate SCell(s) at LTM cell switch for intra-DU LTM. |
| [R2-2305908](file:///D:\Tdoc%20review\RAN2%23122\word\R2-2305908%20_Discussion%20On%20RRC%20Reconfiguration%20Aspects.docx) Nokia, Nokia Shanghai Bell | Proposal 3: BWP to be used upon the LTM execution is either indicated directly within the candidate cell configuration for L1/L2 inter-cell mobility using RRC Configuration message or indicated in the LTM triggering using MAC CE.  Proposal 4: If Option 2 is followed, the notification from the source to the target about the BWP used before the LTM is FFS. |
| [R2-2305909](file:///D:\Tdoc%20review\RAN2%23122\word\R2-2305909_On%20the%20cell%20switch%20in%20LTMmand.docx) Nokia, Nokia Shanghai Bell | For deciding the cell index three options exist:   1. Source DU determines the cell index: In this option, the Source DU associates the PCI of the prepared target cell with the cell index, and it provides the association between the cell index and PCI to CU which in turn send it to the UE (and the other DUs, in case of Dynamic Switching). 2. CU determines the cell index: In this option the CU associates the PCI of the prepared target cell with the cell index, and it provides the association between the cell index and PCI to Source DU (and the other DUs, in case of Dynamic Switching) and to the UE 3. UE uses the ID of the target cell configuration (i.e., RRC configuration for L1/2 mobility) as cell index: In this option the CU informs the (source) DU about the ID of the target cell configuration.   Proposal 7: RAN2 to decide which of the options 1, 2, and 3 should be followed for indicating the target cell index in the LTM MAC CE. |
| [R2-2306010](file:///D:\Tdoc%20review\RAN2%23122\word\R2-2306010-%20Discussion%20on%20RRC%20aspects%20for%20LTM.docx) Ericsson | [Proposal 7 The BWP to be used by the UE upon the execution of the LTM cell switch procedure can be indicated directly within the LTM candidate cell configuration.](#_Toc134736810)  [Proposal 8 If UL/DL BWP IDs are included in the LTM cell switch command and are also present within the LTM candidate cell configuration, the UE shall consider as valid the one received in the LTM cell switch command (and ignore the ones in the LTM candidate cell configuration).](#_Toc134736811) |
| [R2-2306013](file:///D:\Tdoc%20review\RAN2%23122\word\R2-2306013-%20LTM%20cell%20switch%20command%20and%20UE%20actions.docx) Ericsson | [Proposal 3 The BWP information in the LTM cell switch command MAC CE is indicated using BWP-ID referring to one of the configured BWPs within the LTM candidate cell configuration.](#_Toc134739287)  [Proposal 4 The BWP information in the LTM cell switch command MAC CE contains the BWP-ID the UE shall apply as firstActiveDownlinkBWP and firstActiveUplinkBWP.](#_Toc134739288)  [Proposal 5 As in legacy, the same BWP-ID is applied for both firstActiveDownlinkBWP and firstActiveUplinkBWP.](#_Toc134739289)  [Proposal 6 The TCI-state information in the LTM cell switch command MAC CE refers to a TCI-state configured within the LTM candidate cell configuration.](#_Toc134739290)  [Proposal 7 The initial state of an SCell upon an LTM cell switch is part of the LTM candidate cell configuration.](#_Toc134739291)  [Proposal 8 Existing MAC CEs for SCell activation/deactivation are supported to change the state of an SCell upon the execution of an LTM cell switch (the MAC CE for SCell activation/deactivation is sent after the LTM cell switch MAC CE).](#_Toc134739292) |
| [R2-2306479](file:///D:\Tdoc%20review\RAN2%23122\word\R2-2306479%20Discussion%20on%20LTM%3fcommand%3fMAC%3fCE%3fcontent%3fand%3fRAN3%3fLS%3freply.docx) China Unicom | Proposal 2: Candidate SCell activation/deactivation information can be included in RRCReconfiguration message at the LTM preparation phase. Candidate SCell activation/deactivation can be optionally included in LTM MAC CE for intra-DU case. |
| R2-2304883 Futurewei | Proposal 3: Consider using the cell switch command MAC CE to carry the target TA or the source TA adjustment with indication in the MAC CE showing which type of TA is carried. |

**Issue collection for [Post122][058]**

Following information is to be discussed in the long email [Post122][058][Mob18] Contents of Cell Switch MAC CE, on whether it can be included in the cell switch MAC CE (also about its format).

|  |  |  |  |
| --- | --- | --- | --- |
| **Information** | | **Clarification** | |
| TA related information | TA value | It can be included. | The discussion point may be on the format design in MAC CE.  (pending on running CR discussion) |
| TA as zero | The need is confirmed by RAN1, and details on the format is up to RAN2.  *”From RAN 1 perspective, without performing PDCCH-ordered RACH for candidate cell(s), RACH-less mechanism can be supported by indicating TA value of target cell as TA=0 or keeping the same value as source cell in cell switch command.*” |
| TA same as source TAG/cell |
| UE-based TA measurement | We may need to postpone the discussion, until RAN4 confirms the feasibility and RAN1 concludes on the detailed solution. |
| Beam indication/TCI state ID | | It can be included. |
| Active BWP ID | | RAN2 to discuss the need of active BWP ID in LTM cell switch MAC CE, in addtion to the legacy *firstActiveUplinkBWP* and *firstActiveDownlinkBWP* in RRC configuration.  Also to clarify the applicable scenario:   * intra-DU or inter-DU; * RACH-less or RACH-based cell switch; | |
| SCell activation/deactivation indication | | RAN2 to discuss the need of SCell activation/deactivation in LTM cell switch MAC CE, in addtion to the legacy “*sCellState-r16*” in RRC configuration.  Also to clarify the applicable scenario: intra-DU or inter-DU. | |
| CFRA resource | CF CFRA preamble index | Motivation is to reduce the RACH resource reservation.  Source cell can select the CFRA resource among the RACH resource shared by mulitple served UEs, by indicating the dedicated preable in LTM cell switch MAC CE.  Also, it may indicate whether the CFRA resource in candidate configuration is available/valid or not (e.g. if the pre-configured RA resource is release/reallocated by target cell).  Also to clarify the applicable scenario: intra-DU or inter-DU. | |
| CFRA resources availability/validity indication |
| UL grant (to be used by target cell) | | This is considered as the optimizaiton to the CG configured in RRC, which is related to the FFS in RAN2 agreement: ”*Configured grant can be used for RACH-less LTM, for the first UL data transmission to the target cell, the UE selects the configured grant occasion, which is associated with the beam indicated in the LTM MAC CE (as set by source cell). FFS further optimization*”  Is it dynamic grant like the UL grant in RAR? Is it still type1 like configured grant? Is it a index of some shared CG pool? | |
| C-RNTI (to be used by target cell) | | RAN2 to discuss the need of C-RNTI in LTM cell switch MAC CE, in addition to the legacy *newUE-Identity* in *ReconfigurationWithSync* in RRC configuration.  See the RAN1#113 meeting agreement  ”*Whether C-RNTI that is to be used by target cell needs to be included within the MAC-CE containing cell switch command will be left to RAN2 decision.*” | |
| Value of LTM supervisor timer | | This is related to whether LTM reuses the same timer for both RACH-less and RACH-based cell switch.  Even if the RACH-less specific timer is agreed, it is still the baseline to consider using RRC to configure the timer value. | |

**Question A: Do you see the need of any other information to be included in the LTM cell switch MAC CE?**

|  |  |  |
| --- | --- | --- |
| **Companies** | **Other more content to be discussed** | **Motivation/Clarification** |
| Futurewei | Indication of TA type and usage | In last RAN1 meeting, the following agreements have been reached:  “*From RAN 1 perspective, UE-based TA measurement (UE derives TA based on Rx timing difference between current serving cell and candidate cell as well as TA value for the current serving cell) is supported.”*  “*From RAN 1 perspective, without performing PDCCH-ordered RACH for candidate cell(s), RACH-less mechanism can be supported by indicating TA value of target cell as TA=0 or keeping the same value as source cell in cell switch command.”*  RAN2 needs to support the above RAN1 agreements and ensure the accuracy of the current serving cell TA used for the case that the target cell TA is the same as current serving cell TA, or the case that target TA is derived from current serving cell TA and the RSTD of the serving and target cells. A 2-bit field can be added to indicate the following four cases of TA type and usage of the content of the TA field, e.g.:  00: The TA field contains the TA of the target cell. When the TA  field is set to ‘0’, it is the case of target cell TA=0.  01: The TA field contains the most recent dynamic change over the  TA of current serving cell, and the target cell TA = source cell  TA.  10: The TA field contains the most recent dynamic change over the  TA of current serving cell, and the target cell TA is derived  based on the current source cell TA and RSTD of the source and  target cells.  11: The TA field is absent and the UE needs to perform random  access to the target cell. |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

Some outstanding open issues in the Editor’s Notes of MAC running CR are also to be discussed in the long email [Post122][058][Mob18] Contents of Cell Switch MAC CE:

|  |  |
| --- | --- |
| **Open issue** | **Description/clarification** |
| #1 | For LTM completion, how UE to determine the successful reception of its first UL data by the network (left over issue which may need a new MAC CE in MAC):  -Option 1: RLC ACK of RRCReconfigurationComplete message  -Option 2: C-RNTI addressed PDCCH  -Option 3: UE Contention Resolution identify MAC CE |
| #2 | The fields size in MAC CEs:   * “Target Configuration ID” field in the LTM Command MAC CE, i.e. the maximum number of candiate cells in RRC configured LTM * 8/16/? * Considering the MAC CE format to be OCT aligned; * The maximum number for CHO candidate is 8; * “Candidate Cell ID” field in the Candidate Cell TCI States Activation/Deactivation MAC CE, i.e. the maximum number of candiate cells in RRC configured TCI state * 4/8/? * Note the maximum number of reported cell in L1 measurement report is 4, as agreed by RAN1. * “Cell indicator” in PDCCH order for early RACH, i.e. the maximum number of candiate cells in RRC configured early RACH resource * 4/8/? * Note the maximum number of reported cell in L1 measurement report is 4 at one time, as agreed by RAN1. |
|  |  |

**Question B: Do you see any other critical issue that can be discussed in this email discussion [Post122][058][Mob18] Contents of Cell Switch MAC CE?**

|  |  |  |
| --- | --- | --- |
| **Companies** | **Issue?** | **Motivation/Clarification** |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

# Discussion

**2.1 TA information in LTM MAC CE**

RAN1 agreement and LS to RAN4 (R1-2306259):

|  |
| --- |
| RAN1 has confirmed the following working assumption, which was made in RAN1#112:  **Working Assumption**  From RAN 1 perspective, UE-based TA measurement (UE derives TA based on Rx timing difference between current serving cell and candidate cell as well as TA value for the current serving cell) is supported.   * Corresponding UE capability is to be introduced to support UE-based TA measurement * For a UE reports support of this capability, configuration of UE-based TA measurement is supported * FFS: other impacts on RAN1 spec   RAN1 respectfully asks RAN4 to analyze the feasibility of supporting this mechanism. |

On top of the endorsed MAC running CR R2-2306924, we will continue following discussion.

If RAN4 confirms the feasibility and RAN1 completes the design of this UE based TA measurement in August meeting, the LTM MAC CE needs to address the following cases: (If it is not eventually concluded by RAN4/RAN1, then there is no such case 2)

* **Case 1**: RACH-based (actual TA value not needed in the MAC CE)
* **Case 2**: RACH-less with UE based TA measurement (actual TA value not needed in the MAC CE)
* **Case 3**: RACH-less with actual TA value provided (including the zero or same value)

Rapporteur has following way forward as starting point:

**WF1: Postpone the design/discussion to October meeting for more RAN1/4 progress on UE based TA measurement** (since the MAC CE design could be simpler without case 2).

**WF2: Use 2-bits filed to directly indicate the case 1/2/3. The TA field is included in case 3.**

* If RAN1/4 does not complete the supporting of UE based TA measurement, use only 1-bit to indicate case 1 or 3.The TA field is included in case 3. [i.e. fallback to the above highlight behavior]
* Note that the TA field is already 12 bits. If this is optional field, it means the optional TA field itself causes two octets (12bits TA + 4bits R).

**WF3: Use 1-bit field to indicate whether it is case 2 or not. If it is not case 2 (e.g. when this filed is set to 0), one specific value (e.g. FFF) of the TA field indicates the case 1; otherwise, it is case 3.**

* If RAN1/4 does not complete the supporting of UE based TA measurement, one specific value (e.g. FFF) of TA field indicates the case 1; otherwise, it is case 3. [i.e. fallback to the above highlight behavior]
* Note that the TA field is already 12 bits. If this is mandatory field, it can be combined with some R and the Target Configuration ID field as the first two mandatory octets (e.g. 1bit R+ 3bits Target ID+ 12bits TA).

**Q1: Which WF do you prefer on the format of the TA information in LTM MAC CE?**

|  |  |  |
| --- | --- | --- |
| **Companies** | **WF 1/2/3?** | **Comments** |
| Samsung | None | In our view, there is no need to indicate the three cases. It is sufficient to indicate whether TA is included or not in MAC CE. One bit is sufficient for this. |
| MediaTek | 1 | Our understanding is that RAN4 has concern on the timing difference between sites (“synchronous” network only means the timing difference is below some threshold), which may make UE-based TA measurement infeasible. Although we support this method, we may wait for RAN4 conclusion before working on RAN2 MAC CE details. |
| Futurewei | WF 2 with modification | As indicated in our answer to question A, we would suggest using 2-bit field to indicate:  00: The TA field contains the TA of the target cell. When the TA  field is set to ‘0’, it is the case of target cell TA=0.  01: The TA field contains the most recent dynamic change over the  TA of current serving cell, and the target cell TA = the most updated  source cell TA.  10: The TA field contains the most recent dynamic change over the  TA of current serving cell, and the target cell TA is derived based on  the current source cell TA and RSTD of the source and target cells.  11: The TA field is absent and the UE needs to perform random  access to the target cell.  The case ‘00’ of target TA is available covers the special value of target TA=0.  The cases, ‘01’: target TA the same as serving cell TA, and ‘10’: UE based TA measurement, depend on the accuracy of the source cell TA, in these cases the most recent delta source cell TA should be delivered to the UE via the cell switch command MAC CE.  If the network thinks the UE must perform random access, the indication should be set to ‘11’.  In our view, “**Case 3**: RACH-less with actual TA value provided” cannot include the case that the target TA value is same as the source cell TA value since the network/source cell does not maintain the absolute source cell TA of the UE. The source cell only updates the delta source TA to the UE and the UE maintains the most updated absolute TA for UL TX. Therefore, “the target TA value is same as the source cell TA value” has to be a separate case, and anyway 2-bit indication is required. Even for the target TA = source TA case, to ensure the accuracy of the target TA, the most recent source TA should be used. It is desirable to use the cell switch command MAC CE to carry the current source TA-change over the previously determined source TA to let the UE getting the most updated source serving cell TA.  In our view, for inter-DU mobility, we cannot assume source and target DUs are precisely synchronized. The network should compensate the inaccuracy caused by the asynchronization between the DUs. With network compensation, the UE measured TA should be accurate enough. |
| Qualcomm | None | RAN1 agreed that “configuration” of UE-based TA measurement is supported. It is not clear why this configuration has to be an indication in the LTM MAC CE. Configuration typically refers to RRC configuration. If that’s the case, case 2 is dropped as it will not impact the MAC CE design. All what remains is whether the LTM MAC CE carries a TA value or not. |
| CATT | None | Similar understanding as Samsung. The TA information is optionally included in the LTM command MAC CE, and one bit is sufficient to indicate whether this field is present or not. As for if UE-based TA is supported, when TA is not included, whether RACH or RACH-Less should be performed, it can be further discussed after RAN4 conclusion. |
| ZTE | None | UE can automatically obtain the TA value of the candidate cell when UE based TA acquisition is configured via RRC, it is irrelevant with the TA field provided in MAC CE. Therefore, in our understanding, only 1-bit indication is enough: If the 1-bit indication is set to 1 which means TA value of the target cell is present in the LTM Cell switch MAC CE; if the 1-bit indication is set to 0 which means TA value of the target cell is not present in the LTM Cell switch MAC CE. |
| Apple | None | We do not want MAC CE to indicate about the UE based TA derivation (can be configured with RRC) |
| Ericsson | 1 | We in principle agree with Samsung proposal, but since the discussion in RAN1 and RAN4 is still ongoing it makes sense to wait and then implement the necessary signalling. |

**Summary: TBD**

**2.2 Active BWP ID in LTM MAC CE**

RAN1 achieved some consideration on the content of the LTM MAC CE, including the active DL and UL BWPs for the target cell.

|  |
| --- |
| From RAN1 point of view, at least the following information can be included in the cell switch command, which is conveyed by MAC CE   * + Information to identify the target cell(s)     - The details including bit number are designed by RAN2   + TA related information (details up to the discussion in A.I. 9.10.2)   + 1 joint or 1 pair of UL and DL unified TCI State index for the target Cell     - Note: discussion on target SpCell is not precluded   + Active DL and UL BWPs for the target cell   + FFS: Triggering of aperiodic TRS transmitted from the target cell   + FFS: Triggering the CSI acquisition of the target cell and reporting to the target cell   + FFS: Triggering of aperiodic SRS transmission to the target cell   + FFS: C-RNTI * FFS: the presence of each field (i.e. always present or configurable)   **Conclusion**   * Whether active DL and UL BWP of the target Cell/SpCell field, within the cell switch command, is always present or not is left to RAN2 decision. |

It should be RAN2 final discussion on how to indicate the active BWP ID (RRC vs. MAC CE), by considering the corresponding network side coordination and other aspects which may be agnostic to other WGs.

This “active BWP ID” in LTM MAC CE introduces the **dynamic change** of active BWP of the target cell, which may be different with the *firstActiveUplinkBWP-Id* and *firstActiveDownlinkBWP-Id* as in RRC pre-configuration.

The **motivation should be first clarified** on: 1) why target cell wants to change its decision upon trigger LTM, compared to the one provided in the pre-configuration phase; 2) why source cell needs to be involved in the decision of active BWP ID (BWP switch) of target configuration, which is supposed to be target cell strategy.

Note that the RP#100 conclusion has exclude the CSI-RS based L1 measurement for LTM candidate, which means the source cell has no measurement result on the BWP level for its judgment to dynamically change the active BWP ID.

**Q2a: Which option do you prefer on how to determine the active BWP ID of target cell?**

* **Option 1: Only based on the legacy *firstActiveUplinkBWP-Id* and *firstActiveDownlinkBWP-Id* in RRC (pre)configuration corresponding to the target cell.**
* **Option 2: Using optional fields of “active UL/DL BWP ID” in LTM cell switch MAC CE. When included in the LTM MAC CE, it overrides the legacy *firstActiveUplinkBWP-Id* and *firstActiveDownlinkBWP-Id* in RRC (pre)configuration of the target cell.**

|  |  |  |
| --- | --- | --- |
| **Companies** | **Option?** | **Comments** (Please clarify the technical motivation) |
| Huawei, HiSilicon | Option 1 | Source cell should always follow the target cell decision on the first BWP, which is the target cell strategy based on e.g. traffic load on different BWPs. |
| Samsung | Option 2 | RAN1 has agreed to include BWP ID(s) in MAC CE. As per RAN1 conclusion, whether BWP IDs are always present or not is up to RAN2.   * Whether active DL and UL BWP of the target Cell/SpCell field, within the cell switch command, is always present or not is left to RAN2 decision.   Unless there is feasibility issue we prefer to follow RAN1 agreement. |
| MediaTek | Option 1 | BWP assignment is based on long-term factors (e.g., traffic load) and needs not to be very flexible. Assignment in candidate RRC configuration should be feasible. |
| Futurewei | Option 1 | This BWP is used at the target cell and has to be determined by the target cell. The initial BWP at the target cell for mobility is not a fast change configuration and need not to be determined at the cell switch. If the BWP is notified by the MAC CE, the source cell needs to negotiate with the target cell to get the BWP from the target cell before issuing the cell switch command MAC CE. This activity will delay the cell switch. Unless we see benefit for doing this from a use case. |
| Qualcomm | Option 1 at least for inter-DU | We think Option 1 is sufficient for inter-DU scenario for the reasons listed by the rapporteur.  For intra-DU scenario, dynamically modifying the active BWP may provide scheduling flexibility, but we don’t have a strong view on this. |
| CATT | Option 1 |  |
| ZTE | Option 1 for both inter-DU intra-DU,cases, option 2 is only for intra-DU LTM | Option 1 can be supported as the baseline. Option 2 is somewhat an enhancement, the main benefits from this enhancement is that UE can be directly put into the suitable BWP of the target cell so that the time gap due to BWP switch after LTM can be saved. However, we do not think such time gap due to BWP switch is a big issue, but for containing the BWP Id in the LTM Cell switch MAC CE must cause the extra interaction between two DUs in the case of inter-DU LTM, this kind of delay is LTM delay which shall be reduced as much as possible from our point of view. So based on above discussion, we support option 2 as optional which is only for intra-DU case. |
| Apple | Option 2 | We already have dynamic BWP changes with DCI… and since LTM cell switch is considered generally as lower layer procedure, why limit to RRC configured BWP (esp when subsequent LTM is being designed for). |
| Ericsson | Option 2 | Relying on the BWP IDs within the LTM candidate cell configuration is too limiting. If the network wants to switch the UE among BWPs (e.g., a “normal” BWP and a “power saving” BWP) depending on the UE traffic, this would not be possible. Also, this imply that after an LTM cell switch the network would need to send an RRCReconfiguration to the UE thus breaking the principle of subsequent LTM.  We prefer to honor the RAN1 agreement, unless there is a feasibility concern (also in line of what Samsung has clarified). |

**Q2b: If your answer to Q2a is option-2, please also clarify whether the applicable scenario of the active BWP ID in LTM MAC CE is only for intra-DU, or also for inter-DU. Otherwise, you may skip this question.**

If you consider this is also for inter-DU, please clarify the F1AP signaling on how can the target DU know the updated active BWP ID (if it is source DU decision), and on how the source DU knows the updated decision on active BWP ID (if it is target DU decision).

|  |  |  |
| --- | --- | --- |
| **Companies** | **Only intra-DU, or both intra-/inter-DU?** | **Comments** |
| Samsung | both | In our view the interaction between source DU and target DU is anyways needed e.g. for TCI state, if the source DU/target DU, decides TCI state to be included in LTM MAC CE, it needs to be informed to target DU/source DU. |
| Qualcomm | Only intra-DU or none | Scheduling decisions of separate DUs are independent. Therefore, the source DU should NOT include active BWP on behalf of the target DU. Introducing coordination among DUs defers LTM triggering and may cause UE RLF. |
| ZTE | Only intra-DU or none. |  |
| Apple | Both |  |
| Ericsson | Both |  |
|  |  |  |

As to the option-2, some details are still to be clarified:

* For RACH-based cell switch, the active UL BWP is supposed to be configured with RACH resource/configuration. If the active UL BWP can be dynamically changed, how to dynamically re-configure the RACH resource if the active UL BWP ID in LTM MAC CE is different with *firstActiveUplinkBWP-Id* in RRC, where the RACH should be configured. Or, do we assume all UL BWPs has to be configured with RACH?
* For RACH-less cell switch, if configured grant is used for the first UL data transmission, how to dynamically re-configure the CG resource on the updated active UL BWP, if it is different with RRC configured one. Or, do we assume all UL BWPs should be configured with CG resource?

**Q2c: If your answer to Q2a is option-2, please also clarify whether the applicable scenario of active BWP ID in LTM MAC CE is for RACH-based and/or RACH-less cell switch. Otherwise, you may skip this question.**

|  |  |  |
| --- | --- | --- |
| **Companies** | **RACH-based, or RACH-less, or both?** | **Comments** |
|  | both | For RACH based, indicated BWP should be one of the BWPs configured with RACH resource/configuration. UE will apply the configuration of indicated BWP.  For RACH less, CG configuration can be common and applied to the BWP indicated. |
| Apple | Both |  |
| Ericsson | Both |  |
|  |  |  |
|  |  |  |
|  |  |  |

**Summary: TBD**

**2.3 SCell activation/deactivation in LTM MAC CE**

In order to support the simultaneously SCell activation upon LTM trigger, some companies propose to include the SCell activation/deactivation in LTM MAC CE, in addition to the legacy “*sCellState-r16*” in RRC pre-configuration of the target cell.

This **dynamic update** of SCell state may come from following motivations: the L1 measurement result to a candidate SCell changes a lot upon LTM execution, compared to the previous L3 measurement result upon RRC pre-configuration.

The similar situation exists also in CHO. And, in RAN1, it is not clear yet on whether the L1 measurement report can explicitly indicate the candidate SCell and whether the source cell can differentiate if the reported RS is for candidate PCell or candidate SCell.

Please note, for the SCell simultaneous activation upon LTM execution, there is no performance difference for LTM interruption time, between RRC pre-configured and MAC CE indicated manners.

**Q3a: Which option do you prefer to support the SCell activation simultaneously with LTM cell switch execution?**

* **Option 1: SCell state is based on the legacy *sCellState-r16* in RRC (pre)configuration corresponding to the target cell.**
* **Option 2: Using optional fields in LTM cell switch MAC CE to indicate the SCell activation/deactivation state. When included in the LTM MAC CE, it overrides the legacy *sCellState-r16* in RRC (pre)configuration of the target cell.**

|  |  |  |
| --- | --- | --- |
| **Companies** | **Option?** | **Comments** |
| Huawei, HiSilicon | Option 1 | It is the target cell strategy to decide the SCell activation/deactivation, based on the UE traffic amount (i.e. how many carrier is required for UE traffic load).  Even if the RSRP of some candidate SCell (with *sCellState-r16* set to “*activated*” in RRC) becomes weak at the time of LTM cell switch, the BFD and BFR can be used in the worst case with no critical issue (i.e. no need of dynamic control by the source cell). |
| Samsung | Option 1 | In our understanding, RAN2 has not yet agreed to support simultaneous SCell activation during LTM. L1 measurement report for candidate SCells may not be supported. It means NW has to blindly configure the SCell in the LTM candidate configuration.  However, if it will be introduced option 1 is better than option 2 i.e. NW preconfigure the SCell if it is required. |
| MediaTek | Option 1 | Agree with Huawei |
| Futurewei | Option 1 | Agree with Huawei. |
| Qualcomm | Option 1 at least for inter-DU |  |
| CATT | Option 1 |  |
| ZTE | Option 1 |  |
| Ericsson | Option 1 but | We just want to clarify that with Option 1 the network has to configure SCells blindly and this may be inefficient for performance point of view.  If L1 measurements on SCell of LTM candidate cells will be supported, with Option 1 these will be useless.  Therefore, if we go for Option 1, we should inform RAN1 about this since L1 measurements on SCells of LTM candidate cells will not be needed. |

**Q3b: If your answer to Q3a is option-2, please also clarify whether the applicable scenario of the SCell activation/deactivation in LTM MAC CE is only for intra-DU, or also for inter-DU. Otherwise, you may skip this question.**

If you consider this is also for inter-DU, please clarify the F1AP signaling efforts:

* on how can the target DU know the updated SCell state (if it is source DU decision);
* on how the source DU knows the updated decision on SCell state (if it is target DU decision);
* on how the target DU knows the latest L1 measurement result on SCell, just in case it may change the decision (if it is target DU decision);

|  |  |  |
| --- | --- | --- |
| **Companies** | **Only intra-DU, or both intra-/inter-DU?** | **Comments** |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

**Summary: TBD**

**2.4 CFRA resource in LTM MAC CE**

There are some proposals to include the CFRA resource related information in LTM MAC CE, like following:

* Understanding 1: CFRA preamble index;
* Understanding 2: CFRA resources availability/validity indication;
* Other?

The motivation seems to save some reserved CFRA resource at LTM candidate cell side. The opponent view may be that NW can also choose to use CBRA for LTM cell switch, if the RACH resource is considered as limited at candidate cell.

Understanding 1 seems similar to the PDCCH order indicated preamble index, which makes the RRC configured shared/contention-based resource as dedicated for this UE.

Understanding 2 seems to withdraw/confirm the CFRA resource configured in RRC.

**Q4a: Do you agree the need of CFRA resource related information in LTM cell switch MAC CE?**

|  |  |  |
| --- | --- | --- |
| **Companies** | **Yes** (include) or **No** (not include)? | **Comments** (please clarify the detailed format (e.g. which understanding) of this kind of CFRA information, if you prefer to include) |
| Samsung | Yes | CFRA resource configured by RRC may not be valid at the time cell switch. So, validity timer or validity indication in LTM MAC CE can be useful.  CFRA resource (SSB index/Preamble index) in LTM MAC CE is also useful at least for FR2. Based on latest measurement, network can indicate CFRA resource for best beam in the LTM MAC CE. |
| MediaTek | No | CFRA configuration is not small (not just preamble index) and should be provided in candidate RRC configuration.  Availability of CFRA resources upon LTM execution may be an issue. However, having availability bit in MAC CE means that source cell needs to check with target cell before sending the MAC CE, which introduces extra delay. A simpler way would be that the target cell ensures that CFRA resources are available upon LTM execution. Note that we do not expect a large number of candidates, so no need to worry that many CFRA resources are reserved for UEs eventually do not come. |
| Futurewei | No | In our understanding, the option other than source/target CFRA resource negotiation indicated by MTK is to pre-maintain a small pool of preambles of a candidate cell at the source cell with a smaller number of preambles shared by a larger number of UEs such that preamble resources may be saved by different UEs reusing the same preamble at different time. However, it is difficult to determine the size of the pool of preambles at different time to be maintained at the source cell. If large number of UEs are switching to a target cell in short period of time, smaller number of preambles cannot prevent collision. If time spread for UEs to perform cell switch is long enough, locking a pool of multiple preambles of a candidate cell at the source cell wastes resources. Configuring the dedicated preamble at RRC pre-configuration is sufficient and more efficient. It appears to us for CFRA, maintaining a pool of target cell preambles at the source cell and using cell switch command to indicate a preamble from the pool to the UE may not save preamble resources in some cases and may cause collision in some other scenarios. The complexity is also increased a lot. |
| Qualcomm | No | This should be RRC-configuration. In LTM, we optimize for RACH-less LTM execution. RACH-based LTM execution is not main mode of operation. We do not expect limitation on CFRA resources if network chooses to do RACH-based execution. |
| CATT | Yes | The LTM command MAC CE can indicate the preamble index, and by this way not much dedicated RACH resource will be reserved by each candidate cell for possible UE access. Like the RACH resource reserved for early TA acquisition, the same RACH resource or separate RACH resource can also be reserved for LTM execution. The candidate cell can provide a RACH resource pool for multiple UEs. |
| ZTE | No | LTM support both RACH-less and RACH based cell switch. From NW perspective, for reducing the LTM delay, in the case of intra-DU LTM, RACH-less LTM is preferable as there is no additional inter-DU interaction for the TA obtained from early TA acquisition. While in the case of inter-DU LTM, RACH based LTM is preferable with a same reason. With above logics, assuming that RACH dedicated resource are carried in the LTM Cell switch MAC CE, the preferable scenario is inter-DU LTM, however, it needs extra interaction between two DUs for allocating RACH resources before transferring the LTM Cell switch MAC CE which may cause extra LTM delay, the gain is not absolute with a certain price to pay.. so we do not see any need to have this kind of enhancement. |
| Apple | No | An index to RRC config is enough. |
| Ericsson | No | We can rely on CFRA provided within the LTM candidate cell configuration. |

**Q4b: If the answer to Q4a is yes, clarify the applicable scenario of CFRA resource related information in LTM MAC CE is only intra-DU or also or inter-DU. Otherwise, you may skip this question.**

|  |  |  |
| --- | --- | --- |
| **Companies** | **Only intra-DU, or both intra-/inter-DU?** | **Comments** (If you consider this is also for inter-DU, please clarify the F1AP signaling efforts) |
| CATT | both | When source make the LTM execution decision, and choose the CFRA resource for the UE, the source DU indicate the UE ID and associated CFRA resource to the target DU via CU. |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

**Summary: TBD**

**2.5 UL grant in LTM MAC CE**

There are some proposals to include the UL grant related information to be used at target cell in the LTM cell switch MAC CE, which is supposed to be the enhancement, in addition to the CG configured in RRC and PDCCH monitoring of DG at target cell. However, it is not clear on the detailed format and how it is supposed to work, like:

* Is it kind of dynamic grant like the UL grant in RAR?
* Is it an index of some shared CG pool configured by RRC?

**Q5: Do you agree need of UL grant related information in LTM cell switch MAC CE?**

|  |  |  |
| --- | --- | --- |
| **Companies** | **Yes** (include) or **No** (not include)? | **Comments** (please clarify the details if you are supportive to this enhancement) |
| Samsung | Yes | UL grant as in RAR can be included |
| MediaTek | No | We believe that it is enough to have UL grant using CG in candidate RRC configuration and PDCCH monitoring. Also, we don’t think source can provide the info in MAC CE because it depends on target. |
| Futurewei | No | We have similar view as MediaTek. Legacy RAR is from the target cell while LTM cell switch MAC CE is from the source cell. If the source cell gets the target cell grant via negotiation at cell switch, it is even worse than DG with more delay. Otherwise, it the MAC CE carries the target cell grant, the grant has to be notified to the source cell at the preparation phase, then using MAC CE to deliver the grant to the UE. It is not clear why don’t we directly using RRC pre-configuration to carry the grant to the UE at the preparation phase. |
| Qualcomm | No | The UE determines what UL grant to use based on RRC configuration:   * If target cell configuration provides PDCCH search space, the UE waits for PDCCH from the target cell. * If target cell configuration provides CG configuration, the UE uses the latter.   We do not see the need to yet another solution where the grant for transmission to the target cell comes from the source cell. Such solutions anyway do not work for inter-DU. Their benefit for intra-DU is questionable. |
| CATT | No | Agree with MediaTek that the agreed UL grant methods are sufficient.  For CG manner, From the UE side, it is clear which CG resource should be used according to the selected beam, no more information is needed. |
| ZTE | No | If we support this, the extra interaction between two DUs before transferring LTM Cell switch MAC CE are needed for inter-DU LTM which must cause the extra LTM delay. |
| Apple | No | No need for this optimization. |
| Ericsson | No | Agree with MediaTek |

**Summary: TBD**

**2.6 C-RNTI in LTM MAC CE**

RAN1#113 meeting agreement “*Whether C-RNTI that is to be used by target cell needs to be included within the MAC-CE containing cell switch command will be left to RAN2 decision*”.

**Q6: Do you agree need of C-RNTI in LTM cell switch MAC CE, in addition to the legacy *newUE-Identity* in *ReconfigurationWithSync* in RRC configuration?**

|  |  |  |
| --- | --- | --- |
| **Companies** | **Yes** (include) or **No** (not include)? | **Comments** |
| Samsung | No | Do not see need to dynamically update C-RNTI |
| MediaTek | No | C-RNTI can be provided in candidate RRC configuration |
| Futurewei |  | Has some sympathy on the motivation. Consider C-RNTI also a resource at each cell since the number of C-RNTI per cell is limited. If C-RNTI is pre-configured by RRC for candidate cells, the C-RNTI is locked at a candidate cell before the candidate cell becomes the serving cell of the UE. More C-RNTI resources are consumed. If the delay introduced by source/target negotiation during a cell switch is acceptable, the source cell can negotiate C-RNTI with the target cell first, then send it to the UE via cell switch command. C-RNTI is only assigned to the UE when cell switch occurs. In this case, C-RNTI resource is saved at the cost of increased delay of the cell switch. For delay sensitive LTM, RRC pre-configuring C-RNTI (no in MAC CE) is preferred. |
| Qualcomm | No | This is *historically* an RRC configuration during handovers, including CHO. No reason for it to be carried in a MAC CE? |
| CATT | No |  |
| ZTE | No | For inter-DU LTM case, the extra interaction between 2 DUs are needed if the C-RNTI is carried in the LTM MAC CE, given that the C-RNTI is sufficient for each cell, we do not think there is any necessary include C-RNTI in the MAC CE. |
| Apple | No | Not needed in DL (in MAC CE) |
| Ericsson | No |  |

**Summary: TBD**

**2.7 LTM supervisor timer in LTM MAC CE**

This is somehow related to whether LTM uses the same supervisor timer for both RACH-less and RACH-based cell switch.

Even if the RACH-less specific timer is agreed, it still should be the baseline to consider using RRC to configure a RRC layer timer value.

**Q7: Do you agree need of the LTM supervisor timer value in LTM cell switch MAC CE?**

Please clarify your views on the motivation to have different configured value of LTM supervisor timer for RACH-less and RACH-based cell switch. And, also to clarify why RRC configured value is not sufficient.

|  |  |  |
| --- | --- | --- |
| **Companies** | **Yes** (include) or **No** (not include)? | **Comments** |
| Samsung | No |  |
| MediaTek | No | Note that in legacy handover, t304 is generated by target. In current RRC running CR, t3xx is outside candidate config, meaning that it’s generated by source. We may need to clarify which node generates the timer. |
| Futurewei | No | RRC configuring the supervisor timer value is sufficient. |
| Qualcomm | No | It is sufficient to use the RRC configured parameter as in legacy. |
| CATT | see comments | Two separate supervisor timer values can be used for RACH based LTM case and RACH-less based LTM case. RACH-Less based LTM procedure should have less latency requirment than RACH based LTM procedure. Shorter timer value should be applied for RACH-less case. |
| ZTE | No | It is not clear to us the motivation to indicate the supervisor timer in LTM MAC CE. |
| Apple | No |  |
| Ericsson | No | We already agree that the supervision timer is an RRC timer. |

**Summary: TBD**

**2.8 LTM completion determination**

For LTM completion, how UE to determine the successful reception of its first UL data by the network (leftover issue which may need a new MAC CE in MAC running CR):

* Option 1: RLC ACK of *RRCReconfigurationComplete* message
* Option 2: C-RNTI addressed PDCCH
* Option 3: UE Contention Resolution identify MAC CE

Some agreement from NTN WI RACH-less handover discussion: ”*LTE approach (of confirming the HO completion) is reused for both pre-allocated grant and dynamic grant. FFS any enhancement to the confirmation of RACH-less HO completion, e.g. the NW does not send the UE Contention Resolution Identity MAC CE, and sends PDCCH/PDSCH addressed to C-RNTI*”

**Q8: Do you agree to use UE Contention Resolution Identity MAC CE (option 3) for UE to determine the successful reception of its first UL data by the network, in RACH-less cell switch?**

|  |  |  |
| --- | --- | --- |
| **Companies** | **Yes** or **No** (which option)? | **Comments** (Please clarify the critical issue why not to go with the approach considered by NTN and LTE RACH-less) |
| Samsung | Option 2 | In our understanding UL grant used by UE to send first UL data is dedicated to UE. So, option 2 seems sufficient. |
| MediaTek | Option 2 | We prefer Opt.2 and think it is sufficient. If network must send a MAC CE (e.g., due to robustness concern), we suggest defining a new MAC CE. UE Contention Resolution Identity MAC CE is for RACH procedure, and it’s a bit strange to use it in RACH-less LTM. |
| Futurewei | Option 2 with clarification | We think C-RNTI addressed PDCCH scheduled further DL/UL transmission would be sufficient. If there is no immediate follow up data transmission, a new DL cell switch completion MAC CE can be transmitted. Agree with MTK, the contention resolution MAC CE does not fit in LTM cell switch case. |
| Qualcomm | Option 2 (do not copy LTE or NTN) | In LTE, the CRC for PDCCH was 16 bits, so the false alarm rate is of concern. This was one of the justifications for using MAC CE in LTE RACH-less design.  In NR, the CRC for PDCCH is 24 bits, so the false alarm rate is very low. That’s why any PDCCH addressing the UE’s C-RNTI (for UL scheduling or for DL scheduling) is sufficient.  If NR RACH-less NTN copied the LTE solution, we do not have to do so since it is unjustifiable to send a 48-bit MAC CE whose content the UE will ignore anyway.  Option 1 incurs high latency. |
| CATT | Yes | No issue found by going with the approach considered by NTN and LTE RACH-less |
| ZTE | Option 2 | Option 2 is easier and sufficient |
| Apple | Op2 | Similar reasons that we discussed in earlier question. |
| Ericsson | Option 2 (ok also with Option 1) |  |

**Summary: TBD**

**2.9 Fields size in MAC CEs**

Following fields are somehow related and may impact the design of the new MAC CEs in MAC running CR (mainly on how many octets are required in the format).

* **A:** “Target Configuration ID” field in the LTM Cell Switch Command MAC CE, i.e. the maximum number of LTM candiate cells in RRC configuration;
* **B:** “Candidate Cell ID” field in the Candidate Cell TCI States Activation/Deactivation MAC CE, i.e. the maximum number of candiate cells with RRC configured TCI state;
* **C:** “Cell indicator” field in PDCCH order for early RACH, i.e. the maximum number of candiate cells with RRC configured early RACH resource;

Some observations:

The maximum number for CHO candidate is 8;

The maximum number of reported cell in L1 measurement report is 4, as agreed by RAN1.

**Q9: Do you agree following proposal:**

* **A:** The size of “Target Configuration ID” field in the LTM Command MAC CE is 3-bits, i.e. the maximum number of LTM candiate cells in RRC configuration is 8.
* **B:** The size of “Candidate Cell ID” field in the Candidate Cell TCI States Activation/Deactivation MAC CE is 2-bits, i.e. the maximum number of candiate cells with RRC configured TCI state is 4.
* **C:** The size “Cell indicator” field in PDCCH order for early RACH is 2-bits, i.e. the maximum number of candiate cells with RRC configured early RACH resource is 4.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Companies** | **Yes** or **No** (other value)? | | | **Comments** (if no, any other suggestion?) |
| Field A | Field B | Field C |
| Samsung |  |  |  | We can wait for RRC discussion |
| MediaTek |  |  |  | Wait for RRC discussion |
| Futurewei |  |  |  | The rapporteur suggested number sounds reasonable. Can be further discussed. |
| Qualcomm | Yes | No | No | The three numbers should be the same. Any candidate cell may be RRC-configured with TCI states to be activated/deactivated by the MAC CE (though that won’t happen for all cells concurrently). Early RACH can be triggered towards any of the candidate cells. |
| CATT | Yes | No | No | Agree with Qualcomm |
| ZTE |  |  |  | Wait for RRC discussion |
| Apple |  |  |  | Defer to RRC. |
| Ericsson |  |  |  | We in principle agree with Qualcomm, but we can wait this to be discussed in RRC first. |

**Summary: TBD**

# Conclusion and proposals

TBD

# Reference

1. [R2-2304688](file:///D:\Tdoc%20review\RAN2%23122\word\R2-2304688%20Discussions%20on%20cell%20switch.docx) Discussions on Cell Switch CATT
2. [R2-2304720](file:///D:\Tdoc%20review\RAN2%23122\word\R2-2304720_Remaining%20issues%20for%20Cell%20Switching.doc) Remaining issues for Cell Switching Samsung Electronics Co., Ltd
3. [R2-2304889](file:///D:\Tdoc%20review\RAN2%23122\word\R2-2304889%20Open%20Issues%20for%20LTM%20Procedure.docx) Open Issues for LTM Procedure MediaTek Inc.
4. [R2-2304891](file:///D:\Tdoc%20review\RAN2%23122\word\R2-2304891%20Triggering%20MAC%20CE%20for%20LTM.docx) Triggering MAC CE for LTM MediaTek Inc.
5. [R2-2304909](file:///D:\Tdoc%20review\RAN2%23122\word\R2-2304909_Remaining%20issues%20on%20LTM%20procedures.docx) Remaining issues on LTM procedures vivo
6. [R2-2304911](file:///D:\Tdoc%20review\RAN2%23122\word\R2-2304911_RRC%20configuration%20for%20LTM.docx) RRC configuration for LTM vivo
7. [R2-2304953](file:///D:\Tdoc%20review\RAN2%23122\word\R2-2304953%20cell%20switch_v1.docx) Discussions on LTM cell switch execution Fujitsu
8. [R2-2305167](file:///D:\Tdoc%20review\RAN2%23122\word\R2-2305167%20NR%20MOB%20MAC%20CE.docx) LTM MAC CE content and functionality Interdigital, Inc.
9. [R2-2305295](file:///D:\Tdoc%20review\RAN2%23122\word\R2-2305295%20-%20Discussion%20on%20MAC%20CE%20content%20and%20partial%20MAC%20reset%20for%20LTM.docx) Discussion on MAC CE content and partial MAC reset for LTM OPPO
10. [R2-2305541](file:///D:\Tdoc%20review\RAN2%23122\word\R2-2305541%20LTM%20command%20MAC%20CE%20content%20and%20RAN3%20LS%20reply.docx) LTM command MAC CE content and RAN3 LS reply Huawei, HiSilicon, CATT, ZTE Corporation, Sanechips, vivo, China Unicom
11. [R2-2305576](file:///D:\Tdoc%20review\RAN2%23122\word\R2-2305576%20Contents%20of%20cell%20switch%20MAC%20CE.docx) Contents of cell switch MAC CE Xiaomi
12. [R2-2305641](file:///D:\Tdoc%20review\RAN2%23122\word\R2-2305641%3fFurther%20considerations%20on%20cell%20switch.doc) Further considerations on cell switch CMCC
13. [R2-2305649](file:///D:\Tdoc%20review\RAN2%23122\word\R2-2305649%20Cell%20switch.docx) Further discussion on cell switch NEC
14. [R2-2305908](file:///D:\Tdoc%20review\RAN2%23122\word\R2-2305908%20_Discussion%20On%20RRC%20Reconfiguration%20Aspects.docx) Discussion on RRC Reconfiguration Aspects Nokia, Nokia Shanghai Bell
15. [R2-2305909](file:///D:\Tdoc%20review\RAN2%23122\word\R2-2305909_On%20the%20cell%20switch%20in%20LTMmand.docx) On the cell switch in LTM Nokia, Nokia Shanghai Bell
16. [R2-2306010](file:///D:\Tdoc%20review\RAN2%23122\word\R2-2306010-%20Discussion%20on%20RRC%20aspects%20for%20LTM.docx) Discussion on RRC aspects for LTM Ericsson
17. [R2-2306013](file:///D:\Tdoc%20review\RAN2%23122\word\R2-2306013-%20LTM%20cell%20switch%20command%20and%20UE%20actions.docx) LTM cell switch command and UE actions Ericsson
18. [R2-2306479](file:///D:\Tdoc%20review\RAN2%23122\word\R2-2306479%20Discussion%20on%20LTM%3fcommand%3fMAC%3fCE%3fcontent%3fand%3fRAN3%3fLS%3freply.docx) Discussion on LTM command MAC CE content and RAN3 LS reply China Unicom
19. R2-2304883 Discussion on issues at lower layer mobility with RACH-less Futurewei