**3GPP TSG-RAN WG2 Meeting #122 R2-23xxxx**

**Incheon, Korea, May 22nd – 26th, 2023**

**Agenda item: 4.2.1**

**Source: MediaTek Inc.**

**Title: [Post122][102][IoT NTN] UTC reference point (Mediatek)**

**Document for: Discussion and Decision**

# 1 Introduction

This document is aimed at discussing on the UTC reference time and identify potential agreements for possible convergence.

* [Post122][102][IoT NTN] UTC reference point (Mediatek)

      Scope: Continue the discussion on CR4934

      Intended outcome: Agreeable CR in R2-2306668

      Deadline: June 2nd 10:00 UTC

# 2 Contact

|  |  |
| --- | --- |
| Company | Delegate Contact |
| MediaTek | Abhishek Roy (Abhishek.Roy@mediatek.com) |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |

# 3 Discussion

In eMTC and NB-IoT, the UTC time info and reference time info were carried in the SIB16(-NB).

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| – *SystemInformationBlockType16*The IE *SystemInformationBlockType16* contains information related to GPS time and Coordinated Universal Time (UTC). The UE may use the parameters provided in this system information block to obtain the UTC, the GPS and the local time.NOTE: The UE may use the time information for numerous purposes, possibly involving upper layers e.g. to assist GPS initialisation, to synchronise the UE clock (a.o. to determine MBMS session start/ stop).***SystemInformationBlockType16* information element**-- ASN1STARTSystemInformationBlockType16-r11 ::= SEQUENCE { timeInfo-r11 SEQUENCE { timeInfoUTC-r11 INTEGER (0..549755813887), dayLightSavingTime-r11 BIT STRING (SIZE (2)) OPTIONAL, -- Need OR leapSeconds-r11 INTEGER (-127..128) OPTIONAL, -- Need OR localTimeOffset-r11 INTEGER (-63..64) OPTIONAL -- Need OR } OPTIONAL, -- Need OR lateNonCriticalExtension OCTET STRING OPTIONAL, ..., [[ timeReferenceInfo-r15 TimeReferenceInfo-r15 OPTIONAL -- Need OR ]]}-- ASN1STOP

| ***SystemInformationBlockType16* field descriptions** |
| --- |
| ***dayLightSavingTime***It indicates if and how daylight saving time (DST) is applied to obtain the local time. The semantics is the same as the semantics of the *Daylight Saving Time* IE in TS 24.301 [35] and TS 24.008 [49]. The first/leftmost bit of the bit string contains the b2 of octet 3, i.e. the value part of the *Daylight Saving Time* IE, and the second bit of the bit string contains b1 of octet 3. |
| ***leapSeconds***Number of leap seconds offset between GPS Time and UTC. UTC and GPS time are related i.e. GPS time -*leapSeconds* = UTC time. |
| ***localTimeOffset***Offset between UTC and local time in units of 15 minutes. Actual value = field value \* 15 minutes. Local time of the day is calculated as UTC time + *localTimeOffset*. |
| ***timeInfoUTC***Coordinated Universal Time corresponding to the SFN boundary at or immediately after the ending boundary of the SI-window in which *SystemInformationBlockType16* is transmitted. The field counts the number of UTC seconds in 10 ms units since 00:00:00 on Gregorian calendar date 1 January, 1900 (midnight between Sunday, December 31, 1899 and Monday, January 1, 1900). NOTE 1.This field is excluded when estimating changes in system information, i.e. changes of *timeInfoUTC* should neither result in system information change notifications nor in a modification of *systemInfoValueTag* in SIB1. |

NOTE 1: The UE may use this field together with the leapSeconds field to obtain GPS time as follows: GPS Time (in seconds) = timeInfoUTC (in seconds) - 2,524,953,600 (seconds) + leapSeconds, where 2,524,953,600 is the number of seconds between 00:00:00 on Gregorian calendar date 1 January, 1900 and 00:00:00 on Gregorian calendar date 6 January, 1980 (start of GPS time).– *TimeReferenceInfo****TimeReferenceInfo* information elements**-- ASN1STARTTimeReferenceInfo-r15 ::= SEQUENCE { time-r15 ReferenceTime-r15, uncertainty-r15 INTEGER (0..12) OPTIONAL, -- Need OR timeInfoType-r15 ENUMERATED {localClock} OPTIONAL, -- Need OR referenceSFN-r15 INTEGER (0..1023) OPTIONAL -- Cond TimeRef}ReferenceTime-r15 ::= SEQUENCE { refDays-r15 INTEGER (0..72999), refSeconds-r15 INTEGER (0..86399), refMilliSeconds-r15 INTEGER (0..999), refQuarterMicroSeconds-r15 INTEGER (0..3999)}-- ASN1STOP

| ***TimeReferenceInfo* field descriptions** |
| --- |
| ***referenceSFN***This field indicates the reference SFN for time reference information. The *time* field indicates the time at the ending boundary of the SFN indicated by *referenceSFN*. The UE considers the frame indicated by the *referenceSFN* nearest to the frame where the field is received.If the *time* field is included in *SystemInformationBlockType16* and the *referenceSFN* field is not included, the *time* field indicates the time at the SFN boundary at or immediately after the ending boundary of the SI-window in which *SystemInformationBlockType16* is transmitted. |
| ***time, timeInfoType***This field indicates time reference with 0.25 us granularity. The indicated time is referenced at the network, i.e., without compensating for RF propagation delay. The indicated time in 0.25 us unit from the origin is *refDays*\*86400\*1000\*4000 + *refSeconds*\*1000\*4000 + *refMilliSeconds*\*4000 + *refQuarterMicroSeconds*. The *refDays* field specifies the sequential number of days (with day count starting at 0) from the origin of the *time* field. If *timeInfoType* is not included, the origin of the *time* field is 00:00:00 on Gregorian calendar date 6 January, 1980 (start of GPS time). If *timeInfoType* is set to *localClock*, the interpretation of the origin of the *time* is unspecified and left up to upper layers.If *time* field is included in *SystemInformationBlockType16*, this field is excluded when estimating changes in system information, i.e. changes of *time* should neither result in system information change notifications nor in a modification of *systemInfoValueTag* in SIB1. |
| ***uncertainty***This field indicates the number of LSBs which may be inaccurate in the *refQuarterMicroSeconds* field. If *uncertainty* is absent, the uncertainty of *refQuarterMicroSeconds* is not specified. |
| **Conditional presence** | **Explanation** |
| *TimeRef* | The field is mandatory present if *TimeReferenceInfo* is included in *DLInformationTransfer* message; otherwise the field is not present. |

 |

When the UE acquires the network broadcasted SIB16(-NB), the absolute timing info carried in SIB16(-NB) is no longer correct due to the long propagation delay for IoT NTN. The propagation delay has to be compensated to get accurate timing. The network cannot compensate the propagation delay for broadcasted signalling, as the UEs are in different places. It has to be on the UE to do this compensation. This has been discussed briefly during RAN2# 122 (online and offline).

Some companies have raised concerns and confusion that there are also timing information in many radio resources (e.g., SPS, PUR) which corresponds to certain SFN. However, for SFN only, there is no issue as UE can just refer to that SFN. Network already takes into account the propagation delay when scheduling resources to UE. However, EpochTime and UTC timing information are carried in SIB and thus network has no way to compensate this information for each UE. Network composes the Ephemeris Info/UTC timing info at a timing point (RP timing), and UE receives it after a propagation delay. Hence, UE needs to know the starting point of the propagation delay (between RP and UE) for this compensation. It has been defined that the starting point (i.e., reference point) of epoch time in SIB31(-NB) is the uplink time synchronization reference point (i.e., RP).

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *– SystemInformationBlockType31*The IE *SystemInformationBlockType31* contains satellite assistance information for the serving cell. *SystemInformationBlockType31* is only signalled in a NTN cell.*SystemInformationBlockType31* information element-- ASN1STARTSystemInformationBlockType31-r17 ::= SEQUENCE { servingSatelliteInfo-r17 ServingSatelliteInfo-r17, lateNonCriticalExtension OCTET STRING OPTIONAL, ...}ServingSatelliteInfo-r17 ::= SEQUENCE { ephemerisInfo-r17 CHOICE { stateVectors EphemerisStateVectors-r17, orbitalParameters EphemerisOrbitalParameters-r17 }, nta-CommonParameters-17 SEQUENCE { nta-Common-r17 INTEGER (0..8316827) OPTIONAL, -- Need OP nta-CommonDrift-r17 INTEGER (-261935..261935) OPTIONAL, -- Need OP nta-CommonDriftVariation-r17 INTEGER (0..29479) OPTIONAL -- Need OP }, ul-SyncValidityDuration-r17 ENUMERATED {s5, s10, s15, s20, s25, s30, s35, s40, s45, s50, s55, s60, s120, s180, s240, s900}, epochTime-r17 SEQUENCE { startSFN-r17 INTEGER (0..1023), startSubFrame-r17 INTEGER (0..9) } OPTIONAL, -- Need OP k-Offset-r17 INTEGER (0..1023), k-Mac-r17 INTEGER (1..512) OPTIONAL, -- Need OP ...}-- ASN1STOP

| *SystemInformationBlockType31* field descriptions |
| --- |
| ***epochTime***Epoch time of the satellite ephemeris data and common TA parameters, see TS 36.213 [23]. The reference point for epoch time of the serving satellite ephemeris and Common TA parameters is the uplink time synchronization reference point.*epochTime* is the starting time of a DL subframe indicated by *startSFN* and *startSubframe*. For serving cell, the *startSFN* indicates the current SFN or the next upcoming SFN after the frame where the message indicating the *epochTime* is received.If the field is absent, the UE uses the starting time of the DL subframe corresponding to the end of the SI window during which the SI message carrying SIB31 is transmitted.E-UTRAN always includes *epochTime* when *SystemInformationBlockType31* is provided through dedicated signalling.In case of handover or conditional handover, this field is based on the timing of the target cell, i.e. the *startSFN* and *startSubFrame* number indicated in this field refers to the SFN and sub-frame of the target cell, and UE considers the target cell epoch time (indicated by the *startSFN* and *startSubFrame* in this field) to be the frame nearest to the frame where *RRCConnectionReconfiguration* message is received. |
| ***k-Mac***Scheduling offset used when downlink and uplink frame timing are not aligned at the eNB, see TS 36.213 [23]. Unit in ms.If the field if absent, the UE uses the (default) value of 0. |
| ***k-Offset***Scheduling offset used in the timing relationships in NTN, see TS 36.213 [23]. Unit in ms. |
| ***nta-Common***Network-controlled common TA, see TS 36.213 [23]. Unit of μs.Step of 32.55208 ×10-3 μs. Actual value = field value \* 32.55208 ×10-3.If the field is absent, the UE uses the (default) value of 0. |
| ***nta-CommonDrift***Drift rate of the common TA, see TS 36.213 [23]. Unit of μs/s.Step of 0.2 ×10-3 μs/s. Actual value = field value \* 0.2 ×10-3.If the field is absent, the UE uses the (default) value of 0. |
| ***nta-CommonDriftVariation***Drift rate variation of the common TA, see TS 36.213 [23]. Unit of μs/s2.Step of 0.2 ×10-4 μs/s2. Actual value = field value \* 0.2 ×10-4.If the field is absent, the UE uses the (default) value of 0. |
| ***orbitalParameters***Instantaneous values of the satellite orbital parameters. The signalled values are only valid for the duration as defined by *ul-SyncValidityDuration* and *epochTime*. |
| ***stateVectors***Instantaneous values of the satellite state vectors. The signalled values are only valid for the duration as defined by *ul-SyncValidityDuration* and *epochTime*. |
| ***ul-SyncValidityDuration***Validity duration of the satellite ephemeris data and common TA parameters, i.e. maximum time duration (from *epochTime*) during which the UE can apply the satellite ephemeris without acquiring new satellite ephemeris, see TS 36.213 [23]. Unit in second.Value *s5* corresponds to 5 seconds, value *s10* corresponds to 10 seconds and so on. |

 |

Hence, for the timing info in SIB16(-NB), RAN2 should follow the same rule. The reference point of the propagation delay for timing info in SIB16(-NB) should also be the uplink time synchronization reference point (i.e., RP). After acquiring the SIB16(-NB), UE needs to compensate for the propagation delay between the UE and the RP. Based on this, the rapporteur asks the following question:

**Question 1: Do companies agree that the reference point of the propagation delay for timing info in SIB16(-NB) should be the uplink time synchronization reference point (i.e., RP)?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Agree/Disagree** | **Comments** |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

**Rapporteur Summary**

The CR [1] submitted in RAN2#122 has been revised to reflect some comments from companies during the previous discussion. The revised CR was put in the same folder as this discussion.

**Question 2: Do companies agree the revised CR?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Agree/Disagree** | **Comments** |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

**Rapporteur Summary**

# 4 Conclusion

**<To be Uploaded later>**

# 5 References

[1] R2-2306668 Clarify the reference point for UTC in SIB16 MediaTek Inc. CR Rel-17 36.331 17.4.0 4934 1 F LTE\_NBIOT\_eMTC\_NTN-Core