|  |
| --- |
| 3GPP TR 37.911 V0.0.1 (2023-06) |
| Technical Report |
| 3rd Generation Partnership Project;Technical Specification Group Radio Access Network;Study on self-evaluation towards the IMT-2020 submission of the 3GPP Satellite Radio Interface Technology(Release 18) |
|   |
|  |  |
|  |
| The present document has been developed within the 3rd Generation Partnership Project (3GPP TM) and may be further elaborated for the purposes of 3GPP.The present document has not been subject to any approval process by the 3GPPOrganizational Partners and shall not be implemented.This Specification is provided for future development work within 3GPPonly. The Organizational Partners accept no liability for any use of this Specification.Specifications and Reports for implementation of the 3GPP TM system should be obtained via the 3GPP Organizational Partners' Publications Offices. |

|  |
| --- |
|  |
| ***3GPP***Postal address3GPP support office address650 Route des Lucioles - Sophia AntipolisValbonne - FRANCETel.: +33 4 92 94 42 00 Fax: +33 4 93 65 47 16Internethttps://www.3gpp.org |
| ***Copyright Notification***No part may be reproduced except as authorized by written permission.The copyright and the foregoing restriction extend to reproduction in all media.© 2023, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).All rights reserved.UMTS™ is a Trade Mark of ETSI registered for the benefit of its members3GPP™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational PartnersLTE™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational PartnersGSM® and the GSM logo are registered and owned by the GSM Association |

Contents

Foreword 4

Introduction 5

1 Scope 6

2 References 6

3 Definitions of terms, symbols and abbreviations 6

3.1 Terms 6

3.2 Symbols 6

3.3 Abbreviations 6

4 Self-evaluation of eMBB-s technical performance 7

4.1 Peak data rate 7

4.2 Peak spectral efficiency 7

4.3 User experienced data rate 7

4.4 5th percentile user spectral efficiency 7

4.5 Average spectral efficiency 7

4.6 Area traffic capacity 7

4.7 Latency 7

4.7.1 User plane latency 7

4.7.2 Control plane latency 7

4.8 Energy efficiency 7

4.9 Mobility 7

4.10 Mobility interruption time 7

5 Self-evaluation of mMTC-s technical performance 7

5.1 Connection density 7

6 Self-evaluation of HTC-s technical performance 8

6.1 Reliability 8

7 Self-evaluation of generic requirements 8

7.1 Service aspects 8

7.2 Bandwidth 8

7.3 Spectrum 8

8 Conclusions 8

Annex <F> (informative): Change history 9

# 4 Self-evaluation of eMBB-s technical performance

## 4.10 Mobility interruption time

As defined in Report ITU-R M.2410 [4], mobility interruption time is the shortest time duration supported by the system during which a user terminal cannot exchange user plane packets with any base station during mobility transitions.

The mobility interruption time includes the time required to execute any radio access network procedure, radio resource control signalling protocol, or other message exchanges between the mobile station and the radio access network, as applicable to the candidate RIT/SRIT.

For NR NTN, the mobility interruption time is evaluated for the beam mobility scenario.

When moving within the same cell, the transmit-receive beam pair of the UE may need to be changed.

For DL data transmission during UE mobility, gNB can configure different beams for this UE at different slots. It ensures appropriate transmit beam allocation to the UE for continuous DL transmission. Therefore, DL data packet transmission is kept during beam pair switching at different slots.

For UL data transmission, PUSCH is sent using the beam configured by SRI (SRS resource indicator) by gNB. Accordingly, an appropriate gNB-side beam is selected for UL data reception. gNB may select different beams at different slots depending on the UE mobility. Therefore, UL data packet transmission is kept during beam pair switching at different slots.

Based on the above analysis, the UE can always exchange user plane packets with gNB during the mobility transitions. Therefore, 0ms mobility interruption time is achieved by NR for this scenario.