3GPP RAN WG2 Meeting #123 R2-230XXXX

Toulouse, France, Aug 21 – 25, 2023

|  |
| --- |
| *CR-Form-v12.1* |
| **CHANGE REQUEST** |
|  |
|  | **36.304** | **CR** | **XXXX** | **rev** | **-** | **Current version:** | **17.4.0** |  |
|  |
| *For* [*HE**LP*](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network | **x** | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  | 36.304 Running CR for Rel-18 IoT NTN  |
|  |  |
| ***Source to WG:*** | Nokia |
| ***Source to TSG:*** | R2 |
|  |  |
| ***Work item code:*** | IoT\_NTN\_enh |  | ***Date:*** | 2023-06-13 |
|  |  |  |  |  |
| ***Category:*** | **B** |  | ***Release:*** | Rel-18 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-15 (Release 15)Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)* |
|  |  |
| ***Reason for change:*** | Introduction of Release-18 enhancement for IoT-NTN |
|  |  |
| ***Summary of change:*** | This running CR captures the following RAN2 agreements related to the idle mode procedure for IoT-NTN until RAN2-122.**RAN2-123**For NB-IoT NTN, location-based measurement initiation can also be optionally used in RRC\_IDLE for cell re-selection purposes (like in NR-NTN), with the assumption that it is up to the UE to update GNSS location.**RAN2-122**R18 location and time-based trigger for measurements (for connected mode and for idle) apply to both NB-IoT and eMTC.**RAN2-121-bis**1. For eMTC NTN, for fixed cell, location-based measurement initiation can also be used in RRC\_IDLE for cell re-selection purposes (like in NR-NTN)2. For eMTC NTN, for moving cell, location-based measurement initiation can also be used in RRC\_IDLE for cell re-selection purposes (like in NR-NTN). FFS whether to consider a solution that does not require UE to update the GNSS for this same as in connected mode |
|  |  |
| ***Consequences if not approved:*** | No support for Release-18 enhancements for NTN in IoT |
|  |  |
| ***Clauses affected:*** | 5.2.4.2,5.2.4.2a.7.X |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  |  |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  |  |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  |  |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** | R2-230XXXX =-Changes based on RAN2-123 AgreementsR2-2306959 -Endorsed running CR after RAN2-122.R2-2308194 -Summary of changes updated. Base version for further updates in RAN2-123 |

Start of changes

#### 5.2.4.2 Measurement rules for cell re-selection

For NB-IoT measurement rules for cell re-selection is defined in clause 5.2.4.2.a.

When evaluating Srxlev and Squal of non-serving cells for reselection purposes, the UE shall use parameters provided by the serving cell.

Following rules are used by the UE to limit needed measurements:

- If the measurements are performed using RSS as specified in [10] and the serving cell fulfils Srxlev> SIntraSearchP: :

- If *distanceThresh* and *referenceLocation* are broadcasted in SIB31, and if UE supports location-based measurement initiation and has obtained its location information:

- If the distance between UE and the serving cell reference location is shorter than [distanceThresh] the UE may choose not to perform intra-frequency measurements.- Else,the UE shall perform intra-frequency measurements.

 - Else, the UE may choose not to perform intra-frequency measurements.

- Else if the serving cell fulfils Srxlev> SIntraSearchP and Squal > SIntraSearchQ :

- If *distanceThresh*  and *referenceLocation* [reference location] are broadcasted in SIB31, and if UE supports location-based measurement initiation and has obtained its location information:

- If the distance between UE and the serving cell reference location is shorter than [distanceThresh] the UE may choose not to perform intra-frequency measurements.

- Else,the UE shall perform intra-frequency measurements.

 - Else, the UE may choose not to perform intra-frequency measurements.

- Otherwise, the UE shall perform intra-frequency measurements.

- The UE shall apply the following rules for E-UTRAN inter-frequencies and inter-RAT frequencies which are indicated in system information and for which the UE has priority provided as defined in 5.2.4.1:

- For an E-UTRAN inter-frequency or inter-RAT frequency with a reselection priority higher than the reselection priority of the current E-UTRA frequency the UE shall perform measurements of higher priority E-UTRAN inter-frequency or inter-RAT frequencies according to TS 36.133 [10].

- For an E-UTRAN inter-frequency with an equal or lower reselection priority than the reselection priority of the current E-UTRA frequency and for inter-RAT frequency with lower reselection priority than the reselection priority of the current E-UTRAN frequency:

- If the measurements are performed using RSS as specified in [10] and the serving cell fulfils Srxlev > SnonIntraSearchP:,

- If *distanceThresh* and *referenceLocation* are broadcasted in SIB31, and if UE supports location-based measurement initiation and has obtained its location:

- If the distance between UE and serving cell reference location is shorter than *distanceThresh* the UE may choose not to perform measurements of E-UTRAN inter-frequencies or inter-RAT frequency cells of equal or lower priority unless the UE is triggered to measure an E-UTRAN inter-frequency which is configured with *redistributionInterFreqInfo*.

.

- Else, the UE shall perform measurements of E-UTRAN inter-frequencies or inter-RAT frequency cells of equal or lower priority according to TS 36.133 [10].

- Else, UE may choose not to perform measurements of E-UTRAN inter-frequencies or inter-RAT frequency cells of equal or lower priority unless the UE is triggered to measure an E-UTRAN inter-frequency which is configured with *redistributionInterFreqInfo*.

- Else if the serving cell fulfils Srxlev > SnonIntraSearchP and Squal > SnonIntraSearchQ:

- If *distanceThresh* and *referenceLocation* are broadcasted in SIB31, and if UE supports location-based measurement initiation and has obtained its location:

 - If the distance between UE and serving cell reference location is shorter than *distanceThresh* the UE may choose not to perform measurements of E-UTRAN inter-frequencies or inter-RAT frequency cells of equal or lower priority unless the UE is triggered to measure an E-UTRAN inter-frequency which is configured with *redistributionInterFreqInfo*.

 - Else, the UE shall perform measurements of E-UTRAN inter-frequencies or inter-RAT frequency cells of equal or lower priority according to TS 36.133 [10].

- Else, UE may choose not to perform measurements of E-UTRAN inter-frequencies or inter-RAT frequency cells of equal or lower priority unless the UE is triggered to measure an E-UTRAN inter-frequency which is configured with *redistributionInterFreqInfo*.

- Otherwise,the UE shall perform measurements of E-UTRAN inter-frequencies or inter-RAT frequency cells of equal or lower priority according to TS 36.133 [10].

- If the UE supports relaxed monitoring and *s-SearchDeltaP* is present in *SystemInformationBlockType3*, the UE may further limit the needed measurements, as specified in clause 5.2.4.12.

If *t-Service* is present in *SystemInformationBlockType3* of the serving cell, UE shall perform intra-frequency, inter-frequency or inter-RAT measurements, before the time *t-Service* regardless whether the serving cell fulfils Srxlev> SIntraSearchP and Squal > SIntraSearchQ, or Srxlev > SnonIntraSearchP and Squal > SnonIntraSearchQ. The exact time to start measurements before *t-Service* is up to UE implementation. UE shall perform measurements of higher priority inter-frequencies or inter-RAT frequencies regardless of the remaining service time of the serving cell.

Editor Note: When evaluating the location-based measurement initiation for earth moving cell, the current serving cell reference location is derived based on the ephemeris and *[referenceLocationInfo ]* by UE implementation.

#### 5.2.4.2a Measurement rules for cell re-selection for NB-IoT

When evaluating Srxlev and Squal of non-serving cells for reselection purposes, the UE shall use parameters provided by the serving cell.

Following rules are used by the UE to limit needed measurements:

- If the serving cell fulfils Srxlev> SIntraSearchP

- If *distanceThresh* and *referenceLocation are* broadcasted in *SystemInformationBlock31-NB*, and if UE supports location-based measurement initiation and has obtained its location:

- If the distance between UE and serving cell reference location is shorter than *[distanceThresh]* the UE may choose not to perform intra-frequency measurements.

- Else,the UE shall perform intra-frequency measurements.

 - Else, the UE may choose not to perform intra-frequency measurements.

- Otherwise, the UE shall perform intra-frequency measurements.

- The UE shall apply the following rules for NB-IoT inter-frequencies which are indicated in system information:

- If the serving cell fulfils Srxlev > SnonIntraSearchP:

- If *distanceThresh* and *referenceLocation are* broadcasted in *SystemInformationBlock31-NB*, and if UE supports location-based measurement initiation and has obtained its location:

- If the distance between UE and serving cell reference location is shorter than *[distanceThresh]* the UE may choose not to perform intra-frequency measurements.

- Else,the UE shall perform inter-frequency measurements.

 - Else, the UE may choose not to perform inter-frequency measurements.

- Otherwise,the UE shall perform inter-frequency measurements.

- If the UE supports relaxed monitoring and *s-SearchDeltaP* is present in *SystemInformationBlockType3-NB*, the UE may further limit the needed measurements, as specified in clause 5.2.4.12.

If *t-Service* is present in *SystemInformationBlockType3-NB* of the serving cell, UE shall perform intra-frequency or inter-frequency measurements before the time *t-Service* regardless whether the serving cell fulfils Srxlev> SIntraSearchP or Srxlev > SnonIntraSearchP. The exact time to start measurements before *t-Service* is up to UE implementation.

Editor Note: When evaluating the distance-based condition, the current serving cell reference location is derived based on the ephemeris and *[referenceLocationInfo ]* by UE implementation.

Next Change

## 7.X Paging Reception with Discontinuous coverage Enhancements

Editor Note: UE changes for paging reception based on its awareness of in-coverage and out-of-coverage from upper layer. FFS updates based on SA2 LS Response or SA2 CR for this functionality.

End of changes