3GPP TSG RAN WG2 Meeting #123bis R2-230xxxx

**Xiamen, China, October 09-13, 2023**

**Agenda item:** 7.x.x

**Source:** Intel Corporation

**Title:** Outcome of email discussion [POST123][753][eRedCap] on UE Capabilities for Rel-18 eRedCap

**Document for:** Discussion and decision

# Introduction

This document aims to review the running CRs on UE capabilities for Rel-18 eRedCap and to also discuss the open topics identified during RAN2#123 meeting.

* [Post123][753] Running eRedCap CRs for 38306 and 38331 for capabilities (Intel)

Scope: Implement agreements reached so far in the running CRs.

Intended outcome: Running CRs submitted to next meeting.

Please provide your inputs **before/by Tuesday September 19th EOD PST** to have few days afterwards to further review the report and updated CRs (as official email discussion deadline is Friday September 22nd, 2023).

The following are RAN2 agreements relevant to this discussion:

***Organizational***

***[RAN2#122]***

* *We will use the approach suggested by P1a above when implementing the running CRs and the rapporteurs will identify if there are issues with this approach and we can discuss further in later meetings.*

*Proposal 1a: In the R18 specification descriptions, the R17 legacy texts for RedCap UEs descriptions are NOT inherited/applied by default to the eRedCap UEs, i.e. we use following terminologies:*

*- “(e)RedCap UE” to describe the same behaviors for both RedCap and eRedCap UEs;*

*- “RedCap UE” to describe the RedCap UE only/specific behaviors;*

*- “eRedCap UE” to describe the eRedCap UE only/specific new behaviors.*

***RRC\_INACTIVE eDRX above 10.24 sec***

***[RAN2#121bis-e]***

* *Introduce an optional UE capability with signalling for Rel-18 enhanced eDRX in RRC\_INACTIVE.*
* *UE can support Rel-18 enhanced eDRX, only if it supports Rel-17 RRC\_IDLE eDRX. TBD if it must also support Rel-17 RRC\_INACTIVE eDRX.*

***[RAN2#122]***

* *UE can support Rel-18 INACTIVE eDRX (which comprises eDRX cycles and PTWs), even if it doesn’t support Rel-17 INACTIVE eDRX.*

***eRedCap UE***

***[RAN2#121bis-e]***

* *A Rel-18 eRedCap UE should be able to indicate its support via new UE capability signaling specific to Rel-18 eRedCap.*

***[RAN2#123]***

* *The support of Rel-18 eRedCap (FG 48-1 and 48-2) is defined as independently of Rel-17 RedCap (FG 28-1) understanding that RAN1 also agreed that UE supporting Rel-18 eRedCap feature(s) indicate support of this FG 48-1 instead of FG 28-1 (supportOfRedCap-r17).*
* *New UE capability (referred e.g., as supportOfEnhancedRedCap-r18) is defined to capture FG 48-1 (i.e., RedCap UE with reduced peak data rate and reduced baseband bandwidth in FR1) with the corresponding details explained in RAN1 feature list (R1-2306223).*
* *New UE capability (referred e.g., supportOfNotReducedBB-BW-r18) is defined to capture FG 48-2 (i.e., RedCap UE with reduced peak data rate without reduced baseband bandwidth in FR1) with the corresponding details explained in RAN1 feature list (R1-2306223).*
* *To remove from RAN2 running Capability CRs any reference to supportOfEnhancedRedCap-r18 as it is part of RAN1 feature list and its corresponding TP should be captured as part of Mega-Capability CRs. If so, to agree to the update done on UE capabilities running CR to 38.306 and 38.331 in R2-2307657 and R2-2307659.*
* *We will create a temporary CR for RAN1 eRedCap features*
* *To add in the list of functional components for the supportOfEnhancedRedCap-r18 the support of eRedCap early indication based on Msg3 and MsgA PUSCH.*
* *A Rel-18 eRedCap UE (both FG 48-1 and FG 48-2) can also support all RAN2-centric Rel-17 RedCap UE capabilities in the same manner.*
  + *Discuss during CR implementation how to capture this in TS 38.306: option 1) add in the field description of R18 eRedCap capability (i.e. supportOfEnhancedRedCap-r18) the following statement “all supportOfRedCap-r17 related capabilities specified in this specification remain applicable for Rel-18 RedCap UEs, unless indicated otherwise” or option 2) update the field description of the RAN2-centric Rel-17 RedCap UE capabilities to be applicable to (e)RedCap UEs.*
* *To include the following in “section 4.2.x.1 Definition of eRedCap UE” of TS 38.306:*

*eRedCap UE is the UE with reduced peak data rate and, with or without reduced baseband bandwidth in FR1:The maximum bandwidth is 20 MHz for FR1. UE features and corresponding capabilities related to UE bandwidths wider than 20 MHz in FR1 are not supported by eRedCap UEs. eRedCap UEs do not support operation in FR2. The specifications and capabilities of a RedCap UE are also applicable to eRedCap UEs unless stated otherwise.”*

* *Section 4 on “Supported max data rate for DL/UL” in TS 38.306 needs to be updated to include RAN1 agreement on the new value(s) of X for which the legacy constraint “vLayers·Qm·f ≥ 4” is relaxed by capturing the following TP: “For single carrier NR SA operation, the UE (except a UE indicating supportOfERedCap-r18) shall support a data rate for the carrier that is no smaller than the data rate computed using the above formula, with J=1 CC and component vLayers(j)⋅Qmj⋅fj is no smaller than 4. For UE indicating supportOfEnhancedRedCap-r18 in single carrier NR SA operation, the UE shall support a data rate for the carrier that is no smaller than the data rate computed using the above formula, with J=1 CC and component vLayers(j)⋅Qmj⋅fj is no smaller than 0.75 if UE does not indicate supportOfNotReducedBB-BW-r18 or 3.2 if UE also indicates supportOfNotReducedBB-BW-r18.”).*

The following are RAN1 agreements on feature list [1] relevant to this discussion (the latest inputs were provided in RAN1 LS [2]):

|  |  |  |
| --- | --- | --- |
| **Feature #** | **48-1** | **48-2** |
| **Group** | **RedCap UE with reduced peak data rate and reduced baseband bandwidth in FR1** | **RedCap UE with reduced peak data rate without reduced baseband bandwidth in FR1** |
| **Components** | The following components are the same as for *supportOfRedCap-r17* (28-1):  1. Maximum FR1 RedCap UE bandwidth is 20 MHz.  3. Early indication of RedCap UE in Msg.1 for 4-step RACH  4. Separate initial UL BWP for RedCap UEs  - It includes the configuration(s) needed for RedCap UE to perform random access  - Enabling/disabling of frequency hopping for common PUCCH resources  5. Separate initial DL BWP for RedCap UEs  - It includes CSS/CORESET for random access  - For separate initial DL BWP used for paging, CD-SSB is included  - For separate initial DL BWP only used for RACH, SSB may or may not be included  - For separate initial DL BWP used in connected mode as BWP#0 configuration option 1, CD-SSB is included  6. 1 UE-specific RRC configured DL BWP per carrier  7. 1 UE-specific RRC configured UL BWP per carrier  8. RRC reconfiguration of any parameters related to BWP  9. UE-specific RRC configured DL BWP with CD-SSB or NCD-SSB  10. NCD-SSB based measurements in RRC-configured DL BWP  The following components are new compared to *supportOfRedCap-r17* (28-1):  11. DL/UL peak data rate target of 10 Mbps corresponding to *vLayers*·*Qm*·*f* = 3.2  12. Maximum number of PDSCH/PUSCH PRBs that can be scheduled for unicast per slot of 25 PRBs for 15 kHz SCS and 12 PRBs for 30 kHz SCS  13. Relaxed processing timeline of 1/0.5 ms for 15/30 kHz SCS when the RAR PDSCH and MsgB PDSCH (if supported) is larger than 25/12 PRBs for 15/30 kHz SCS  14. Network-configurable additional separate early indication in Msg1 for Rel-18 eRedCap UEs  FFS whether to add additional components | Component 13 in FG 48-1 is supported by FG 48-2 during initial access.  The capabilities of FG 48-2 are the same as for FG 48-1 except that the following restriction does not apply:  12. Maximum number of PDSCH/PUSCH PRBs that can be scheduled for unicast per slot of 25 PRBs for 15 kHz SCS and 12 PRBs for 30 kHz SCS  Component 11 in FG 48-1 does not apply and DL/UL peak data rate target of 10 Mbps corresponding to *vLayers*·*Qm*·*f* = 0.75 when *vLayers* = 1 and *vLayers*·*Qm*·*f* = 0.8 when *vLayers* = 2 |
| **Pre-req.** |  | 48-1 |
| **Need for gNB to know if feature is supported** | Y | Y |
| **Consequence if the feature is not supported by the UE** | Network assumes the UE is not a RedCap UE with reduced peak data rate without reduced baseband bandwidth in FR1 | Network assumes the UE is not a RedCap UE with reduced peak data rate without reduced baseband bandwidth in FR1 |
| **Type** | Per UE | Per UE |
| **FDD/ TDD diff** | No | No |
| **FR1/ FR2 diff** | FR1 only | FR1 only |
| **Note** | A UE supporting this FG is not required to support FG 6-1.  A UE supporting this FG is not allowed to support FG 28-1.  The specifications for a UE supporting FG 28-1 (‘RedCap UE’) also apply for a UE supporting this FG (FG 48-1) unless stated otherwise.  It is up to RAN2 whether/how to capture the capabilities for early indication of RedCap UE in Msg 3 and Msg A.  It is up to RAN2 whether/how to capture the capabilities for additional separate early indication of Rel-18 eRedCap UE in Msg 3 and Msg A PUSCH. |  |
| **Mandatory/ Optional** | Optional with capability signaling  UEs supporting Rel-18 eRedCap UE complexity reduction feature(s) indicate support of this FG instead of FG 28-1 (supportOfRedCap-r17). | Optional with capability signaling |

In addition, RAN1 also provided inputs on their agreements on the reduced peak data rate for Rel-18 eRedCap UEs in LS [3] as it seems to have specification impacts at least on TS 36.306 clause 4.1.2 (‘Supported max data rate for DL/UL’):

* *The UE signals peak data rate related parameters vLayers, Qm and f corresponding to 10 Mbps.*
  + *No new values for the above parameters will be introduced for Rel-18 eRedCap.*
* *For UE peak data rate reduction with UE BB bandwidth reduction (i.e., FG 48-1),*
  + *The 10-Mbps peak rate target corresponds to a vLayers·Qm·f of 3.2.*
  + *25 PRBs for and 12 PRBs for for  is always assumed in the UE supported max data rate expression in TS 38.306 for any given band.*
* *For UE peak data rate reduction without UE BB bandwidth reduction (i.e., FG 48-2),*
  + *When vLayers = 1, the 10-Mbps peak rate target corresponds to a vLayers·Qm·f of 0.75.*
  + *When vLayers = 2, the peak rate target corresponds to a vLayers·Qm·f of 0.8.*
  + *106 PRBs for and 51 PRBs for for  is always assumed in the UE supported max data rate expression in TS 38.306 for any given band.*
* *In all cases, the same value for vLayers·Qm·f is used for DL and UL.*

On summary, considering above agreements/updates, this document aims to collect companies’ inputs on the suggested TPs for the temporary CRs on RAN1 lead features, and the draft CRs on RAN2 lead features/topics.

# Companies’ point of contact (PoC)

|  |  |  |
| --- | --- | --- |
| **Company’s name** | **PoC’s name** | **PoC’s email address** |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

# Discussion

## [RAN1 lead features] Temporary CRs to TS 38.306 and 38.331 on UE Capabilities for eRedCap

1. Do you agree with the way eRedCap terminology is updated in the description of **FG 48-1,** i.e. *enhRedCap-r18*(related TP is highlighted in pink on the temporary CR to TS 38.306 which captures the agreed details on **RAN1 lead features** of UE Capabilities for eRedCap)? If not, please indicate your suggested TP.

|  |  |  |
| --- | --- | --- |
| **Company’s name** | **Yes/No** | **Comments, if any** |
|  |  |  |
|  |  |  |
|  |  |  |

1. Do you agree with the way proposed to capture **the differences between FG 48-1 and FG 48-2,** i.e. *enhRedCap-r18* and *notReducedBB-BW-r18* (related TP is highlighted in blue on the temporary CR to TS 38.306 which captures the agreed details on **RAN1 lead features** of UE Capabilities for eRedCap)? If not, please indicate your suggested TP.

|  |  |  |
| --- | --- | --- |
| **Company’s name** | **Yes/No** | **Comments, if any** |
|  |  |  |
|  |  |  |
|  |  |  |

1. Please indicate if you have any other input/comments on the temporary CRs to TS 38.306 and 38.331 which captures the agreed details on **RAN1 lead features** of UE Capabilities for eRedCap.

|  |  |  |  |
| --- | --- | --- | --- |
| **Company’s name** | **TS #** | **Section** | **Comments, if any** |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |

## [RAN2 lead features/topics] Drafted CRs to TS 38.306 and 38.331 on UE Capabilities for eRedCap

1. Do you agree with the way that it is captured that **Rel-18 eRedCap UE can support all RAN2-centric Rel-17 RedCap capabilities** (related TP is highlighted in pink on the drafted CRs to TS 38.306 which captures the agreed details on **RAN2 lead features** of UE Capabilities for eRedCap)? If not, please indicate your suggested preference/TP.

This question is related to the following RAN2#123 agreement:

* *A Rel-18 eRedCap UE (both FG 48-1 and FG 48-2) can also support all RAN2-centric Rel-17 RedCap UE capabilities in the same manner.*
  + *Discuss during CR implementation how to capture this in TS 38.306: option 1) add in the field description of R18 eRedCap capability (i.e. supportOfEnhancedRedCap-r18) the following statement “all supportOfRedCap-r17 related capabilities specified in this specification remain applicable for Rel-18 RedCap UEs, unless indicated otherwise” or option 2) update the field description of the RAN2-centric Rel-17 RedCap UE capabilities to be applicable to (e)RedCap UEs.*

|  |  |  |
| --- | --- | --- |
| **Company’s name** | **Yes/No** | **Comments, if any** |
|  |  |  |
|  |  |  |
|  |  |  |

1. Please indicate if you have any other input/comments on the drafted CRs to TS 38.306 and 38.331 which captures the agreed details on **RAN2 lead features/topics** of UE Capabilities for eRedCap during RAN2#123 meeting.

|  |  |  |  |
| --- | --- | --- | --- |
| **Company’s name** | **TS #** | **Section** | **Comments, if any** |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |

# Report <<To be added>>

*<<Report from this email discussion [to be added by rapporteur] >>*

1. xxxx.

# Conclusion

The proposals captured are the following:

**Proposal 1.** xxxx.

# Reference

1. R1-2308521, Updated RAN1 UE features list for Rel-18 NR after RAN1#114, August 2023.
2. R1-2308523, LS on Rel-18 RAN1 UE features list for NR after RAN1#114, From: RAN1, To: RAN2, Ccing: RAN4, August 2023.
3. R1-2308610, LS on reduced peak data rate for Rel-18 eRedCap UEs, Rel-18, From: RAN1, To: RAN2, Ccing: RAN4, August 2023.