**3GPP TSG-RAN WG2 Meeting #124 *R2-231xxxx***

**Chicago, US, 13-17, 2023**

|  |
| --- |
| *CR-Form-v12.2* |
| **CHANGE REQUEST** |
|  |
|  |  | **CR** |  | **rev** |  | **Current version:** | **17.6.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network | **X** | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  | UE capabilities for Rel-18 eRedCap WI |
|  |  |
| ***Source to WG:*** | Intel Corporation |
| ***Source to TSG:*** | R2 |
|  |  |
| ***Work item code:*** | NR\_redcap\_enh-Core |  | ***Date:*** | 2023-11-23 |
|  |  |  |  |  |
| ***Category:*** | **B** |  | ***Release:*** |  |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)Rel-19 (Release 19)* |
|  |  |
| ***Reason for change:*** | Introduction of UE capabilities for Rel-18 eRedCap WI  |
|  |  |
| ***Summary of change:*** | 1. Define a UE capability *extendedDRX-CycleInactive-r18* as part of IE *MAC-Parameters*.
2. Define a UE capability *eRedCapIgnoreCapabilityFiltering-r18* as part of IE *ERedCapParameters*.
 |
|  |  |
| ***Consequences if not approved:*** | Rel-18 eRedCap feature is not completed |
|  |  |
| ***Clauses affected:*** | 6.3.3 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** | **x** |  |  Other core specifications  | TS/TR 38.306 CR ...  |
| ***affected:*** |  | **xx** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  |  |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

1. ***Modified section***

### 6.3.3 UE capability information elements

\*\*\* OMITTED TEXT \*\*\*

– *ERedCapParameters*

The IE *ERedCapParameters* is used to indicate the UE capabilities supported by eRedCap UEs.

***ERedCapParameters* information element**

-- ASN1START

-- TAG-EREDCAPPARAMETERS-START

ERedCapParameters-r18::= SEQUENCE {

 eRedCapIgnoreCapabilityFiltering-r18 ENUMERATED {supported} OPTIONAL

}

-- TAG-EREDCAPPARAMETERS-STOP

-- ASN1STOP

1. ***Modified section***

– *MAC-Parameters*

The IE *MAC-Parameters* is used to convey capabilities related to MAC.

***MAC-Parameters* information element**

-- ASN1START

-- TAG-MAC-PARAMETERS-START

MAC-Parameters ::= SEQUENCE {

 mac-ParametersCommon MAC-ParametersCommon OPTIONAL,

 mac-ParametersXDD-Diff MAC-ParametersXDD-Diff OPTIONAL

}

MAC-Parameters-v1610 ::= SEQUENCE {

 mac-ParametersFRX-Diff-r16 MAC-ParametersFRX-Diff-r16 OPTIONAL

}

MAC-Parameters-v1700 ::= SEQUENCE {

 mac-ParametersFR2-2-r17 MAC-ParametersFR2-2-r17 OPTIONAL

}

MAC-ParametersCommon ::= SEQUENCE {

 lcp-Restriction ENUMERATED {supported} OPTIONAL,

 dummy ENUMERATED {supported} OPTIONAL,

 lch-ToSCellRestriction ENUMERATED {supported} OPTIONAL,

 ...,

 [[

 recommendedBitRate ENUMERATED {supported} OPTIONAL,

 recommendedBitRateQuery ENUMERATED {supported} OPTIONAL

 ]],

 [[

 recommendedBitRateMultiplier-r16 ENUMERATED {supported} OPTIONAL,

 preEmptiveBSR-r16 ENUMERATED {supported} OPTIONAL,

 autonomousTransmission-r16 ENUMERATED {supported} OPTIONAL,

 lch-PriorityBasedPrioritization-r16 ENUMERATED {supported} OPTIONAL,

 lch-ToConfiguredGrantMapping-r16 ENUMERATED {supported} OPTIONAL,

 lch-ToGrantPriorityRestriction-r16 ENUMERATED {supported} OPTIONAL,

 singlePHR-P-r16 ENUMERATED {supported} OPTIONAL,

 ul-LBT-FailureDetectionRecovery-r16 ENUMERATED {supported} OPTIONAL,

 -- R4 8-1: MPE

 tdd-MPE-P-MPR-Reporting-r16 ENUMERATED {supported} OPTIONAL,

 lcid-ExtensionIAB-r16 ENUMERATED {supported} OPTIONAL

 ]],

 [[

 spCell-BFR-CBRA-r16 ENUMERATED {supported} OPTIONAL

 ]],

 [[

 srs-ResourceId-Ext-r16 ENUMERATED {supported} OPTIONAL

 ]],

 [[

 enhancedUuDRX-forSidelink-r17 ENUMERATED {supported} OPTIONAL,

 --27-10: Support of UL MAC CE based MG activation request for PRS measurements

 mg-ActivationRequestPRS-Meas-r17 ENUMERATED {supported} OPTIONAL,

 --27-11: Support of DL MAC CE based MG activation request for PRS measurements

 mg-ActivationCommPRS-Meas-r17 ENUMERATED {supported} OPTIONAL,

 intraCG-Prioritization-r17 ENUMERATED {supported} OPTIONAL,

 jointPrioritizationCG-Retx-Timer-r17 ENUMERATED {supported} OPTIONAL,

 survivalTime-r17 ENUMERATED {supported} OPTIONAL,

 lcg-ExtensionIAB-r17 ENUMERATED {supported} OPTIONAL,

 harq-FeedbackDisabled-r17 ENUMERATED {supported} OPTIONAL,

 uplink-Harq-ModeB-r17 ENUMERATED {supported} OPTIONAL,

 sr-TriggeredBy-TA-Report-r17 ENUMERATED {supported} OPTIONAL,

 extendedDRX-CycleInactive-r17 ENUMERATED {supported} OPTIONAL,

 simultaneousSR-PUSCH-DiffPUCCH-groups-r17 ENUMERATED {supported} OPTIONAL,

 lastTransmissionUL-r17 ENUMERATED {supported} OPTIONAL

 ]],

 [[

 extendedDRX-CycleInactive-r18 ENUMERATED {supported} OPTIONAL

 ]]

}

MAC-ParametersFRX-Diff-r16 ::= SEQUENCE {

 directMCG-SCellActivation-r16 ENUMERATED {supported} OPTIONAL,

 directMCG-SCellActivationResume-r16 ENUMERATED {supported} OPTIONAL,

 directSCG-SCellActivation-r16 ENUMERATED {supported} OPTIONAL,

 directSCG-SCellActivationResume-r16 ENUMERATED {supported} OPTIONAL,

 -- R1 19-1: DRX Adaptation

 drx-Adaptation-r16 SEQUENCE {

 non-SharedSpectrumChAccess-r16 MinTimeGap-r16 OPTIONAL,

 sharedSpectrumChAccess-r16 MinTimeGap-r16 OPTIONAL

 } OPTIONAL,

 ...

}

MAC-ParametersFR2-2-r17 ::= SEQUENCE {

 directMCG-SCellActivation-r17 ENUMERATED {supported} OPTIONAL,

 directMCG-SCellActivationResume-r17 ENUMERATED {supported} OPTIONAL,

 directSCG-SCellActivation-r17 ENUMERATED {supported} OPTIONAL,

 directSCG-SCellActivationResume-r17 ENUMERATED {supported} OPTIONAL,

 drx-Adaptation-r17 SEQUENCE {

 non-SharedSpectrumChAccess-r17 MinTimeGapFR2-2-r17 OPTIONAL,

 sharedSpectrumChAccess-r17 MinTimeGapFR2-2-r17 OPTIONAL

 } OPTIONAL,

 ...

}

MAC-ParametersXDD-Diff ::= SEQUENCE {

 skipUplinkTxDynamic ENUMERATED {supported} OPTIONAL,

 logicalChannelSR-DelayTimer ENUMERATED {supported} OPTIONAL,

 longDRX-Cycle ENUMERATED {supported} OPTIONAL,

 shortDRX-Cycle ENUMERATED {supported} OPTIONAL,

 multipleSR-Configurations ENUMERATED {supported} OPTIONAL,

 multipleConfiguredGrants ENUMERATED {supported} OPTIONAL,

 ...,

 [[

 secondaryDRX-Group-r16 ENUMERATED {supported} OPTIONAL

 ]],

 [[

 enhancedSkipUplinkTxDynamic-r16 ENUMERATED {supported} OPTIONAL,

 enhancedSkipUplinkTxConfigured-r16 ENUMERATED {supported} OPTIONAL

 ]]

}

MinTimeGap-r16 ::= SEQUENCE {

 scs-15kHz-r16 ENUMERATED {sl1, sl3} OPTIONAL,

 scs-30kHz-r16 ENUMERATED {sl1, sl6} OPTIONAL,

 scs-60kHz-r16 ENUMERATED {sl1, sl12} OPTIONAL,

 scs-120kHz-r16 ENUMERATED {sl2, sl24} OPTIONAL

}

MinTimeGapFR2-2-r17 ::= SEQUENCE {

 scs-120kHz-r17 ENUMERATED {sl2, sl24} OPTIONAL,

 scs-480kHz-r17 ENUMERATED {sl8, sl96} OPTIONAL,

 scs-960kHz-r17 ENUMERATED {sl16, sl192} OPTIONAL

}

-- TAG-MAC-PARAMETERS-STOP

-- ASN1STOP

\*\*\* OMITTED TEXT \*\*\*

1. ***Modified section***

– *UE-NR-Capability*

The IE *UE-NR-Capability* is used to convey the NR UE Radio Access Capability Parameters, see TS 38.306 [26].

***UE-NR-Capability* information element**

-- ASN1START

-- TAG-UE-NR-CAPABILITY-START

UE-NR-Capability ::= SEQUENCE {

 accessStratumRelease AccessStratumRelease,

 pdcp-Parameters PDCP-Parameters,

 rlc-Parameters RLC-Parameters OPTIONAL,

 mac-Parameters MAC-Parameters OPTIONAL,

 phy-Parameters Phy-Parameters,

 rf-Parameters RF-Parameters,

 measAndMobParameters MeasAndMobParameters OPTIONAL,

 fdd-Add-UE-NR-Capabilities UE-NR-CapabilityAddXDD-Mode OPTIONAL,

 tdd-Add-UE-NR-Capabilities UE-NR-CapabilityAddXDD-Mode OPTIONAL,

 fr1-Add-UE-NR-Capabilities UE-NR-CapabilityAddFRX-Mode OPTIONAL,

 fr2-Add-UE-NR-Capabilities UE-NR-CapabilityAddFRX-Mode OPTIONAL,

 featureSets FeatureSets OPTIONAL,

 featureSetCombinations SEQUENCE (SIZE (1..maxFeatureSetCombinations)) OF FeatureSetCombination OPTIONAL,

 lateNonCriticalExtension OCTET STRING (CONTAINING UE-NR-Capability-v15c0) OPTIONAL,

 nonCriticalExtension UE-NR-Capability-v1530 OPTIONAL

}

-- Regular non-critical Rel-15 extensions:

UE-NR-Capability-v1530 ::= SEQUENCE {

 fdd-Add-UE-NR-Capabilities-v1530 UE-NR-CapabilityAddXDD-Mode-v1530 OPTIONAL,

 tdd-Add-UE-NR-Capabilities-v1530 UE-NR-CapabilityAddXDD-Mode-v1530 OPTIONAL,

 dummy ENUMERATED {supported} OPTIONAL,

 interRAT-Parameters InterRAT-Parameters OPTIONAL,

 inactiveState ENUMERATED {supported} OPTIONAL,

 delayBudgetReporting ENUMERATED {supported} OPTIONAL,

 nonCriticalExtension UE-NR-Capability-v1540 OPTIONAL

}

UE-NR-Capability-v1540 ::= SEQUENCE {

 sdap-Parameters SDAP-Parameters OPTIONAL,

 overheatingInd ENUMERATED {supported} OPTIONAL,

 ims-Parameters IMS-Parameters OPTIONAL,

 fr1-Add-UE-NR-Capabilities-v1540 UE-NR-CapabilityAddFRX-Mode-v1540 OPTIONAL,

 fr2-Add-UE-NR-Capabilities-v1540 UE-NR-CapabilityAddFRX-Mode-v1540 OPTIONAL,

 fr1-fr2-Add-UE-NR-Capabilities UE-NR-CapabilityAddFRX-Mode OPTIONAL,

 nonCriticalExtension UE-NR-Capability-v1550 OPTIONAL

}

UE-NR-Capability-v1550 ::= SEQUENCE {

 reducedCP-Latency ENUMERATED {supported} OPTIONAL,

 nonCriticalExtension UE-NR-Capability-v1560 OPTIONAL

}

UE-NR-Capability-v1560 ::= SEQUENCE {

 nrdc-Parameters NRDC-Parameters OPTIONAL,

 receivedFilters OCTET STRING (CONTAINING UECapabilityEnquiry-v1560-IEs) OPTIONAL,

 nonCriticalExtension UE-NR-Capability-v1570 OPTIONAL

}

UE-NR-Capability-v1570 ::= SEQUENCE {

 nrdc-Parameters-v1570 NRDC-Parameters-v1570 OPTIONAL,

 nonCriticalExtension UE-NR-Capability-v1610 OPTIONAL

}

-- Late non-critical Rel-15 extensions:

UE-NR-Capability-v15c0 ::= SEQUENCE {

 nrdc-Parameters-v15c0 NRDC-Parameters-v15c0 OPTIONAL,

 partialFR2-FallbackRX-Req ENUMERATED {true} OPTIONAL,

 nonCriticalExtension UE-NR-Capability-v15g0 OPTIONAL

}

UE-NR-Capability-v15g0 ::= SEQUENCE {

 rf-Parameters-v15g0 RF-Parameters-v15g0 OPTIONAL,

 nonCriticalExtension UE-NR-Capability-v15j0 OPTIONAL

}

UE-NR-Capability-v15j0 ::= SEQUENCE {

 -- Following field is only for REL-15 late non-critical extensions

 lateNonCriticalExtension OCTET STRING OPTIONAL,

 nonCriticalExtension UE-NR-Capability-v16a0 OPTIONAL

}

-- Regular non-critical Rel-16 extensions:

UE-NR-Capability-v1610 ::= SEQUENCE {

 inDeviceCoexInd-r16 ENUMERATED {supported} OPTIONAL,

 dl-DedicatedMessageSegmentation-r16 ENUMERATED {supported} OPTIONAL,

 nrdc-Parameters-v1610 NRDC-Parameters-v1610 OPTIONAL,

 powSav-Parameters-r16 PowSav-Parameters-r16 OPTIONAL,

 fr1-Add-UE-NR-Capabilities-v1610 UE-NR-CapabilityAddFRX-Mode-v1610 OPTIONAL,

 fr2-Add-UE-NR-Capabilities-v1610 UE-NR-CapabilityAddFRX-Mode-v1610 OPTIONAL,

 bh-RLF-Indication-r16 ENUMERATED {supported} OPTIONAL,

 directSN-AdditionFirstRRC-IAB-r16 ENUMERATED {supported} OPTIONAL,

 bap-Parameters-r16 BAP-Parameters-r16 OPTIONAL,

 referenceTimeProvision-r16 ENUMERATED {supported} OPTIONAL,

 sidelinkParameters-r16 SidelinkParameters-r16 OPTIONAL,

 highSpeedParameters-r16 HighSpeedParameters-r16 OPTIONAL,

 mac-Parameters-v1610 MAC-Parameters-v1610 OPTIONAL,

 mcgRLF-RecoveryViaSCG-r16 ENUMERATED {supported} OPTIONAL,

 resumeWithStoredMCG-SCells-r16 ENUMERATED {supported} OPTIONAL,

 resumeWithStoredSCG-r16 ENUMERATED {supported} OPTIONAL,

 resumeWithSCG-Config-r16 ENUMERATED {supported} OPTIONAL,

 ue-BasedPerfMeas-Parameters-r16 UE-BasedPerfMeas-Parameters-r16 OPTIONAL,

 son-Parameters-r16 SON-Parameters-r16 OPTIONAL,

 onDemandSIB-Connected-r16 ENUMERATED {supported} OPTIONAL,

 nonCriticalExtension UE-NR-Capability-v1640 OPTIONAL

}

UE-NR-Capability-v1640 ::= SEQUENCE {

 redirectAtResumeByNAS-r16 ENUMERATED {supported} OPTIONAL,

 phy-ParametersSharedSpectrumChAccess-r16 Phy-ParametersSharedSpectrumChAccess-r16 OPTIONAL,

 nonCriticalExtension UE-NR-Capability-v1650 OPTIONAL

}

UE-NR-Capability-v1650 ::= SEQUENCE {

 mpsPriorityIndication-r16 ENUMERATED {supported} OPTIONAL,

 highSpeedParameters-v1650 HighSpeedParameters-v1650 OPTIONAL,

 nonCriticalExtension UE-NR-Capability-v1690 OPTIONAL

}

UE-NR-Capability-v1690 ::= SEQUENCE {

 ul-RRC-Segmentation-r16 ENUMERATED {supported} OPTIONAL,

 nonCriticalExtension UE-NR-Capability-v1700 OPTIONAL

}

-- Late non-critical extensions from Rel-16 onwards:

UE-NR-Capability-v16a0 ::= SEQUENCE {

 phy-Parameters-v16a0 Phy-Parameters-v16a0 OPTIONAL,

 rf-Parameters-v16a0 RF-Parameters-v16a0 OPTIONAL,

 nonCriticalExtension UE-NR-Capability-v16c0 OPTIONAL

}

UE-NR-Capability-v16c0 ::= SEQUENCE {

 rf-Parameters-v16c0 RF-Parameters-v16c0 OPTIONAL,

 nonCriticalExtension UE-NR-Capability-v16d0 OPTIONAL

}

UE-NR-Capability-v16d0 ::= SEQUENCE {

 featureSets-v16d0 FeatureSets-v16d0 OPTIONAL,

 nonCriticalExtension SEQUENCE {} OPTIONAL

}

-- Regular non-critical Rel-17 extensions:

UE-NR-Capability-v1700 ::= SEQUENCE {

 inactiveStatePO-Determination-r17 ENUMERATED {supported} OPTIONAL,

 highSpeedParameters-v1700 HighSpeedParameters-v1700 OPTIONAL,

 powSav-Parameters-v1700 PowSav-Parameters-v1700 OPTIONAL,

 mac-Parameters-v1700 MAC-Parameters-v1700 OPTIONAL,

 ims-Parameters-v1700 IMS-Parameters-v1700 OPTIONAL,

 measAndMobParameters-v1700 MeasAndMobParameters-v1700,

 appLayerMeasParameters-r17 AppLayerMeasParameters-r17 OPTIONAL,

 redCapParameters-r17 RedCapParameters-r17 OPTIONAL,

 ra-SDT-r17 ENUMERATED {supported} OPTIONAL,

 srb-SDT-r17 ENUMERATED {supported} OPTIONAL,

 gNB-SideRTT-BasedPDC-r17 ENUMERATED {supported} OPTIONAL,

 bh-RLF-DetectionRecovery-Indication-r17 ENUMERATED {supported} OPTIONAL,

 nrdc-Parameters-v1700 NRDC-Parameters-v1700 OPTIONAL,

 bap-Parameters-v1700 BAP-Parameters-v1700 OPTIONAL,

 musim-GapPreference-r17 ENUMERATED {supported} OPTIONAL,

 musimLeaveConnected-r17 ENUMERATED {supported} OPTIONAL,

 mbs-Parameters-r17 MBS-Parameters-r17,

 nonTerrestrialNetwork-r17 ENUMERATED {supported} OPTIONAL,

 ntn-ScenarioSupport-r17 ENUMERATED {gso, ngso} OPTIONAL,

 sliceInfoforCellReselection-r17 ENUMERATED {supported} OPTIONAL,

 ue-RadioPagingInfo-r17 UE-RadioPagingInfo-r17 OPTIONAL,

 -- R4 17-2 UL gap pattern for Tx power management

 ul-GapFR2-Pattern-r17 BIT STRING (SIZE (4)) OPTIONAL,

 ntn-Parameters-r17 NTN-Parameters-r17 OPTIONAL,

 nonCriticalExtension UE-NR-Capability-v1740 OPTIONAL

}

UE-NR-Capability-v1740 ::= SEQUENCE {

 redCapParameters-v1740 RedCapParameters-v1740,

 nonCriticalExtension UE-NR-Capability-v1750 OPTIONAL

}

UE-NR-Capability-v1750 ::= SEQUENCE {

 crossCarrierSchedulingConfigurationRelease-r17 ENUMERATED {supported} OPTIONAL,

 nonCriticalExtension UE-NR-Capability-v1800 OPTIONAL

}

-- Regular non-critical Rel-18 extensions:

UE-NR-Capability-v1800 ::= SEQUENCE {

 eRedCapParameters-r18 ERedCapParameters-r18 OPTIONAL,

 nonCriticalExtension SEQUENCE{} OPTIONAL

}

UE-NR-CapabilityAddXDD-Mode ::= SEQUENCE {

 phy-ParametersXDD-Diff Phy-ParametersXDD-Diff OPTIONAL,

 mac-ParametersXDD-Diff MAC-ParametersXDD-Diff OPTIONAL,

 measAndMobParametersXDD-Diff MeasAndMobParametersXDD-Diff OPTIONAL

}

UE-NR-CapabilityAddXDD-Mode-v1530 ::= SEQUENCE {

 eutra-ParametersXDD-Diff EUTRA-ParametersXDD-Diff

}

UE-NR-CapabilityAddFRX-Mode ::= SEQUENCE {

 phy-ParametersFRX-Diff Phy-ParametersFRX-Diff OPTIONAL,

 measAndMobParametersFRX-Diff MeasAndMobParametersFRX-Diff OPTIONAL

}

UE-NR-CapabilityAddFRX-Mode-v1540 ::= SEQUENCE {

 ims-ParametersFRX-Diff IMS-ParametersFRX-Diff OPTIONAL

}

UE-NR-CapabilityAddFRX-Mode-v1610 ::= SEQUENCE {

 powSav-ParametersFRX-Diff-r16 PowSav-ParametersFRX-Diff-r16 OPTIONAL,

 mac-ParametersFRX-Diff-r16 MAC-ParametersFRX-Diff-r16 OPTIONAL

}

BAP-Parameters-r16 ::= SEQUENCE {

 flowControlBH-RLC-ChannelBased-r16 ENUMERATED {supported} OPTIONAL,

 flowControlRouting-ID-Based-r16 ENUMERATED {supported} OPTIONAL

}

BAP-Parameters-v1700 ::= SEQUENCE {

 bapHeaderRewriting-Rerouting-r17 ENUMERATED {supported} OPTIONAL,

 bapHeaderRewriting-Routing-r17 ENUMERATED {supported} OPTIONAL

}

MBS-Parameters-r17 ::= SEQUENCE {

 maxMRB-Add-r17 INTEGER (1..16) OPTIONAL

}

-- TAG-UE-NR-CAPABILITY-STOP

-- ASN1STOP

|  |
| --- |
| ***UE-NR-Capability* field descriptions** |
| ***featureSetCombinations***A list of *FeatureSetCombination:s* for *supportedBandCombinationList* in *UE-NR-Capability*. The *FeatureSetDownlink:s* and *FeatureSetUplink:s* referred to from these *FeatureSetCombination:s* are defined in the *featureSets* list in *UE-NR-Capability*. |

|  |
| --- |
| ***UE-NR-Capability-v1540 field descriptions*** |
| ***fr1-fr2-Add-UE-NR-Capabilities***This instance of *UE-NR-CapabilityAddFRX-Mode* does not include any other fields than *csi-RS-IM-ReceptionForFeedback*/ *csi-RS-ProcFrameworkForSRS*/ *csi-ReportFramework*. |

\*\*\* OMITTED TEXT \*\*\*

***End of the modified section***