**3GPP TSG-RAN WG2#125 *R2-2401680***

**Athens, Greece, 26th – 1st March 2024**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.2* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  |  | **CR** | 0372 | **rev** | **1** | **Current version:** |  |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network | **X** | Core Network |  |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | Restriction of cell list for NCR-MT cell reselection | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | Samsung | | | | | | | | | |
| ***Source to TSG:*** | R2 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | NR\_netcon\_repeater | | | | |  | ***Date:*** | | | 2024-03-01 |
|  |  | | | |  | |  | | |  |
| ***Category:*** | F |  | | | | | ***Release:*** | | | Rel-18 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-16 (Release 16) Rel-17 (Release 17) Rel-18 (Release 18) Rel-19 (Release 19)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | NCR-MT may be configured with allowed and/or forbidden cell list for cell reselection from OAM server (specified in TS 38.300) while allow- and/or exclude-listed cells in SIB3/4 may be signaled in the NCR-MT’s camped cell. Since ones in SIB3/4 are not only for NCR-MT but mainly for access UEs, NCR-MT should not use these lists if OAM already configured NCR-MT with allowed and/or forbidden cell lists.  The expected operation of NCR-MT would be like below:   |  |  |  |  | | --- | --- | --- | --- | | Cases | NCR-OAM   configured forbidden cell list | NCR-OAM   configured allowed cell list | Expected   NCR-MT behaviour | | 1 | not   configured | not   configured | NCR-MT follows the “excluded cell list” and “allowed cell list” broadcasted in SIB. | | 2 | configured | not   configured | NCT-MT   cannot access the cell that belongs to either “OAM configured forbidden cell   list” or “excluded cell list” broadcasted in SIB.  If “allowed cell list” is broadcasted in SIB, the NCR-MT can only access those cells. | | 3 | not   configured | configured | NCR-MT can only access the cell that belongs to the OAM configured allowed cell list. | | 4 | configured | configured | NCR-MT can only access the cell that belongs to the OAM configured allowed cell list. | | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | The following behaviour has been specified:  NCR-MT may be configured with additional allowed cell list and/or forbidden cell list, see TS 38.300 [2]. The NCR-MT shall consider only the allowed cell list, if configured by OAM as candidates for cell reselection (ignore above exclude-listed cells and/or allow-listed cells). The NCR-MT shall not consider the cells for cell reselection in the forbidden cell list, if configured by OAM. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | NCR-MT doesn’t know which cell lists should be used for cell reselection, if allowed cell list and/or forbidden cell lists, and exclude-listed cells and/or allow-listed cell are signaled. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | 5.2.4.1 | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  | **X** | Other core specifications | | | | TS/TR ... CR ... | | |
| ***affected:*** | |  | **X** | Test specifications | | | | TS/TR ... CR ... | | |
| ***(show related CRs)*** | |  | **X** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | |  | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | | R2-2400322 is revised to this. | | | | | | | | |

*START OF CHANGE*

5.2.4.1 Reselection priorities handling

Absolute priorities of different NR frequencies or inter-RAT frequencies may be provided to the UE in the system information, in the *RRCRelease* message, or by inheriting from another RAT at inter-RAT cell (re)selection. In the case of system information, an NR frequency or inter-RAT frequency may be listed without providing a priority (i.e. the field *cellReselectionPriority* is absent for that frequency). If any fields with *cellReselectionPriority* or *nsag-CellReselectionPriority* are provided in dedicated signalling, the UE shall ignore any fields with *cellReselectionPriority* and *nsag-CellReselectionPriority* provided in system information.

When UE is in camped normally state, if it supports slice-based cell reselection and has received the network slice(s) and NSAG information from NAS to be used for cell reselection, UE shall derive reselection priorities according to clause 5.2.4.11.

NOTE 00: UE derives reselection priorities according to clause 5.2.4.11 also in case *SIB16* (see TS 38.331 [3]) is not broadcast in the camped cell.

If UE is in *camped on any cell* state, UE shall only apply the priorities provided by system information from current cell, and the UE preserves priorities provided by dedicated signalling and *deprioritisationReq* received in *RRCRelease* unless specified otherwise. When the UE in camped normally state, has only dedicated priorities other than for the current frequency, the UE shall consider the current frequency to be the lowest priority frequency (i.e. lower than any of the network configured values). When the HSDN capable UE is in High-mobility state, the UE shall always consider the HSDN cells to be the highest priority (i.e., higher than any other network configured priorities). When the HSDN capable UE is not in High-mobility state, the UE shall always consider HSDN cells to be the lowest priority (i.e., lower than any other network configured priorities). If the UE is configured to perform both NR sidelink communication and V2X sidelink communication, the UE may consider the frequency providing both NR sidelink communication configuration and V2X sidelink communication configuration to be the highest priority. If the UE is configured to perform NR sidelink communication and not perform V2X communication, the UE may consider the frequency providing NR sidelink communication configuration to be the highest priority. If the UE is configured to perform V2X sidelink communication and not perform NR sidelink communication, the UE may consider the frequency providing V2X sidelink communication configuration to be the highest priority. If the UE is configured to perform ranging/sidelink positioning, the UE may consider the frequency providing ranging/sidelink positioning configuration to be the highest priority.

A UE on a vehicle with a mobile-IAB cell may consider the frequency for which a mobile-IAB cell is the best cell to be the highest priority. The UE identifies a mobile-IAB cell by *mobileIAB-Cell* in SIB1 (see TS 38.331 [3]). The UE may narrow its search scope for mobile-IAB cell(s) by *mobileIAB-InfoList-r18* if broadcasted in SIB4 (see TS 38.331 [3]). A non-mobile-IAB cell may be excluded from this mobile IAB frequency prioritization for up to 300 seconds.

NOTE 0a: The frequency only providing the anchor frequency configuration should not be prioritized for V2X service during cell reselection, as specified in TS 38.331[3].

NOTE 0b: When UE is configured to perform NR sidelink communication or V2X sidelink communication performs cell reselection, it may consider the frequencies providing the intra-carrier and inter-carrier configuration have equal priority in cell reselection.

NOTE 0c: The prioritization among the frequencies which UE considers to be the highest priority frequency is left to UE implementation unless otherwise stated.

NOTE 0d: The UE is configured to perform V2X sidelink communication or NR sidelink communication, if it has the capability and is authorized for the corresponding sidelink operation.

NOTE 0e: When UE is configured to perform both NR sidelink communication and V2X sidelink communication, but cannot find a frequency which can provide both NR sidelink communication configuration and V2X sidelink communication configuration, UE may consider the frequency providing either NR sidelink communication configuration or V2X sidelink communication configuration to be the highest priority.

NOTE 0f: Void.

NOTE 0g: How the UE determines itself to be on a vehicle with a mobile-IAB cell is left to the UE's implementation.

The UE shall only perform cell reselection evaluation for NR frequencies and inter-RAT frequencies that are given in system information and for which the UE has a priority provided.

If the MBS broadcast capable UE is receiving or interested to receive an MBS broadcast service(s) and can only receive this MBS broadcast service(s) by camping on a frequency on which it is provided, the UE may consider that frequency to be the highest priority during the MBS broadcast session as specified in TS 38.300 [2] as long as the two following conditions are fulfilled:

1) SIB1 scheduling information of the cell reselected by the UE due to frequency prioritization for MBS contains SIB20;

2) Either:

- One or more MBS FSAI(s) of that frequency is indicated in SIB21 of the serving cell and the same MBS FSAI(s) is also indicated for this MBS broadcast service in MBS User Service Description (USD) as specified in TS 26.346 [20], or

- SIB21 is not provided in the serving cell and that frequency is included in the USD of this service, or

- SIB21 is provided in the serving cell but does not provide the frequency mapping for the concerned service, and that frequency is included in the USD of this service.

NOTE 0g: It is up to UE implementation which frequency to select, when the USD provides multiple frequencies for the service the UE is interested in.

If the MBS broadcast capable UE is receiving or interested to receive an MBS broadcast service, the UE may consider cell reselection candidate frequencies at which it cannot receive the MBS broadcast service to be of the lowest priority during the MBS broadcast session as specified in TS 38.300 [2], as long as SIB1 scheduling information of the cell contains SIB20 on the MBS frequency which the UE monitors and as long as the condition 2) above is fulfilled for the serving cell.

NOTE 0h: Example scenarios in which such down-prioritisation may be needed include the cases where camping is not possible for the UE on the MBS broadcast frequency (e.g. the MBS broadcast frequency belongs to a PLMN different from UE's registered PLMN) while the UE can receive the MBS broadcast service when camped on another frequency than the MBS broadcast frequency or current frequency.

NOTE 0i: The frequency prioritization for MBS broadcast, NR sidelink communication, or V2X sidelink communication may override the re-selection priorities for slice-based cell reselection.

In case UE receives *RRCRelease* with *deprioritisationReq*, UE shall consider current frequency and stored frequencies due to the previously received *RRCRelease* with *deprioritisationReq* or all the frequencies of NR to be the lowest priority frequency (i.e. lower than any of the network configured values) while T325 is running irrespective of camped RAT. The UE shall delete the stored deprioritisation request(s) when a PLMN selection or SNPN selection is performed on request by NAS (TS 23.122 [9]).

NOTE 1: UE should search for a higher priority layer for cell reselection as soon as possible after the change of priority. The minimum related performance requirements specified in TS 38.133 [8] are still applicable.

NOTE 1a: The UE does not consider MBS broadcast, NR sidelink communication or V2X sidelink communication functionality to replace cell reselection priorities caused by HSDN or *deprioritisationReq* functionality.

The UE shall delete priorities provided by dedicated signalling when:

- the UE enters a different RRC state; or

- the optional validity time of dedicated priorities (T320) expires; or

- the UE receives an *RRCRelease* message with the field *cellReselectionPriorities* absent; or

- a PLMN selection or SNPN selection is performed on request by NAS (TS 23.122 [9]).

NOTE 2: Equal priorities between RATs are not supported.

The UE shall not consider any exclude-listed cells as candidate for cell reselection.

The UE shall consider only the allow-listed cells, if configured, as candidates for cell reselection.

NCR-MT may be configured with additional allowed cell list and/or forbidden cell list, see TS 38.300 [2]. The NCR-MT shall consider only the allowed cell list, if configured by OAM as candidates for cell reselection (ignore above exclude-listed cells and/or allow-listed cells). The NCR-MT shall not consider the cells for cell reselection in the forbidden cell list, if configured by OAM.

The UE in RRC\_IDLE state shall inherit the priorities provided by dedicated signalling and the remaining validity time (i.e. T320 in NR and E-UTRA), if configured, at inter-RAT cell (re)selection.

NOTE 3: The network may assign dedicated cell reselection priorities for frequencies not configured by system information.

*END OF CHANGE*