**3GPP TSG- Meeting #bis**

**China, -**

Agenda Item: 8.5.4

Source: OPPO

Title: Summary of [109]

Document for: Discussion, Decision

1. Introduction

This is to discuss the offline as follows.

* **[POST127][109][NES] (OPPO)**

 **Scope:** For each direction (N extension vs PF bundling): 1) List proposed options, 2) Discuss to understand each option better, 3) Down select options, 4) Discuss pros and cons for each direction or down-selected options (with the consideration of UE impacts, system impacts and specification job). F2F offline discussion in Brk3 room. => It is extended to long email discussion to continue detailed analysis of pros and cons for each direction.

 **Intended outcome:** Discussion summary in R2-2407598. => Updated discussion summary

**Deadline:** Long email discussion.

1. Stage-1 Discussion

In this section, the defined scope of the post email discussion is further expanded to dig into details.

**2.1 Issue-1: List proposed options**

Based on the conclusion from 125bis

For adaptation of paging occasions in time domain, RAN2 to study
a) bundle paging frames and
b) extend the values of N to have increased interval between PFs (e.g. T/64, T/128 ...) and compensating decrease in number of PFs by increasing POs per PF.

For option-a), as discussed during AT-127 [109], there are multiple sub-options of approach a), for which there is one left issue, i.e.,

Proposal 2 For option-a), R2 further discuss whether to allow gaps between bundled PFs.

* Can be discussed as part of long email discussion.

**Q1-1: for option-a), do you agree to allow gaps between bundled PFs?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Agree/Disagree** | **Comment** |
|  |  |  |
|  |  |  |

For option-a), as discussed during AT-127 [109], there are multiple sub-options, it was a bit difficult to make down-selection between sub-options due to the limited time. So now the attempt as follows to see if any possibility to converge.

|  |  |  |  |
| --- | --- | --- | --- |
| **Option** | **Source** | **Formula** | **Comment** |
| **a-1** | **Intel, 6471** | **(SFN + PF\_offset) mod T = G\*(UE\_ID mod L)** | **L: the number of consecutive PFs within a PF bundle (i.e., PF bundle size)****G: the frame gap between consecutive PFs** |
| **a-2** | **Apple, 6671** | **(SFN + PF\_offset) mod T = (T div N)\*(~~UE\_ID~~ SubGroup\_ID mod N)** |  |
| **a-3** | **Apple, 6671** | **(SFN + PF\_offset) mod T = ~~(T div N)\*~~(UE\_ID Mod N)** |  |
| **a-4** | **CATT, 7004** | **(SFN + PF\_offset) mod T = G\*(UE\_ID mod N)** | **G: the frame gap between consecutive PFs.** |
| **a-5** | **Vivo, 6723** | **(SFN + PF\_offset) mod T = SFN [(UE\_ID mod N)]** |  |
| **a-6** | **Vivo, 6723** | **Rel-19 PF = legacy PF +[ (UE\_ID mod (N\_new/N+factor)) – (factor-1)]** |  |
| **a-7** | **Lenovo, 6809** | **only one fixed PO is used in a cell specific Paging DRX Cycle** |  |
| **a-8** | **Samsung, 6348** | **(SFN +PF\_Offset) mod T = (D div N) \* (UE\_ID mod N).** | **N (#of PFs in duration D at the beginning of DRX cycle) = D, D/2, D/4, D/8 ,..** |

**Q1-2: For option-a), which sub-option you prefer?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Preferred sub-option** | **Comment** |
|  |  |  |
|  |  |  |

On the other hand, there seems no much further details to clarify for option-b).

Overall, it is good to understand if there is any major issue missing, in order to clarify either option.

**Q1-3: Besides the issues above, any major issue remains, in order to clarify the key idea for either option-a) or option-b)?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Any major left issue?****Yes/No** | **Comment** |
|  |  |  |
|  |  |  |

**2.2 Issue-2: Discuss to understand each option better**

It seems the scope is the same as issue-1 above.

**2.3 Issue-4: Discuss pros and cons for each direction or down-selected options (with the consideration of UE impacts, system impacts and specification job)**

Although this is the last bullet in email scope, it seems helpful to discuss this first, before going to the 3rd bullet here.

From email rapporteur perspective, it seems clearer that option-b) has requires less specification effort since it aims at keeping the legacy formula as it was, and the effort comes from the additional value range for the corresponding parameters. While option-a) would come with a revised formula.

**Q2-1: Given that option-b) tends to keep the legacy formula as it was but just extended value range, while option-a) tends to go for a revised formula, do you agree that the specification job for option-b) is less?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Agree/Disagree** | **Comment** |
| OPPO | Agree |  |
|  |  |  |

And then the option-a) would be motivated only if there is a major performance difference. While during AT-127, as clarified and concluded



**Figure 1 Option-a) vs. Option-b) in terms of PO location in time domain (discussed in AT-127 [109])**

As clarified in 304 as follows:

NOTE 1: A PO associated with a PF may start in the PF or after the PF.

NOTE 2: The PDCCH monitoring occasions for a PO can span multiple radio frames. When *SearchSpaceId* other than 0 is configured for *paging-SearchSpace* the PDCCH monitoring occasions for a PO can span multiple periods of the paging search space.

And thus 127 agreed that

Proposal 3 R2 observe that the option-a) and option-b) can be designed to configure the PO:s at same time position.

**Q2-2: Given clarification (as concluded in R2#127) that PO does not have to be limited to the time period of the corresponding PF, and thus option-b) can reach same time position for POs, do you think there would be a major difference for the system performance of the two options? If Yes, please clarify the difference in your view.**

|  |  |  |
| --- | --- | --- |
| **Company** | **Any major performance difference? Yes/No?** | **Comment** |
| OPPO | No | Based on same time position for the PO:s, we have not understood the reason for a performance difference between the two options.  |
|  |  |  |

1. Stage-2 Discussion

**2.4 Issue-3: Down select options**

Given the clarification during 127 and the discussion above, it would be helpful to understand companies view, regarding the two options.

1. Conclusion

Based on the offline, we reached the following WF