**3GPP TSG-RAN WG2 Meeting #129 R2-250xxxx**

**Athens, Greece, 17th – 21st Feb., 2025**

**Agenda Item: 8.6.3**

**Source: vivo**

**Title: Summary of [POST128][109][MOB] MAC running CR – Open issues (vivo)**

**Document for: Discussion and Decision**

# 1 Introduction

This paper summarizes the post meeting email discussion for the open issues for the MAC running CR. Please note that this paper only includes some stage-3 issues related to how to generate the MAC specification or the issues which have not been proposed/discussed in companies’ contributions before.

**[POST128][109][MOB] MAC running CR (vivo)**

**Scope:** Prepare 38.321 running CR capturing all RAN2 agreements, identify stage 3 issues (possibly with rapporteur’s suggestion) that need to be discussed, and discuss them.

**Intended outcome:** 38.321 running CR, to be endorsed next meeting, and discussion summary.

**Deadline: Long email discussion**

Based on the companies' inputs, the proposals have been formulated at the conclusion section.

Please fill in the contact information in the table below

|  |  |  |
| --- | --- | --- |
| **Company** | **Contact Person** | **Email Address** |
| vivo | Chenli | chenli5g@vivo.com |

# 2. Discussion

## 2.0 General

In MAC specification (also in other specifications?), “LTM” means “intra-CU LTM” by now. After introducing Rel-19 “inter-CU LTM”, there are a lot of change places for “LTM” which are applicable for both legacy “intra-CU LTM” and Rel-19 “inter-CU LTM” “conditional intra-CU LTM”, e.g. PDCCH ordered early RACH, early TA acquisition, CG-based [and DG-based] RACH-less, etc. How to capture/Whether to differentiate them is up to further discussion.

How to capture/differentiate them in the MAC (and other specifications)?

* Option 1: “LTM” in specification means “intra-CU LTM” as legacy, “inter-CU LTM” “Conditional intra-CU LTM” in Rel-19 should be captured as “inter-CU LTM” “Conditional intra-CU LTM” specifically.
* Option 2: “LTM” in specification means “both intra-CU, inter-CU LTM and Conditional intra-CU LTM”. “intra-CU LTM”, “inter-CU LTM” “Conditional intra-CU LTM” specific part, if any, should be clearly captured for “intra-CU LTM”, “inter-CU LTM” and “Conditional intra-CU LTM”, separately.
* Others, please specify.

Note: Option 2 means we need to clean up the current MAC specification to check whether “LTM” needs to be updated as “intra-CU LTM” if “inter-CU LTM” or “Conditional intra-CU LTM” has different behaviour.

Rapporteur understands that almost all procedures in the MAC specification for Rel-18 intra-CU LTM could be reused for Rel-19 inter-CU LTM. Thus, in the latest version of running MAC CR, Option 2 is adopted, i.e. “LTM” in the specification means “intra-CU LTM, inter-CU LTM, [and Conditional intra-CU LTM”.

***Question 0:* Companies are invited to provide preference/comment if any different understanding as Rapporteur above.**

|  |  |  |
| --- | --- | --- |
| **Company** | **Option(s)** | **Comment** |
|  |  |  |
|  |  |  |

## 2.1 inter-CU LTM

For Rel-18 intra-CU LTM, we discussed the cross-feature issues for LTM and concluded the intra-CU LTM won’t coexist with the NR-U or NES. On the other hand, it could coexist with coverage enhancement, MIMO 2TA and (e)RedCap, which has the impacts on MAC specification as follows [1]:

|  |
| --- |
| 5.1.1b Selection of the set of Random Access resources for the Random Access procedure ------omit------  1> if contention-free Random Access Resources have been provided for this Random Access procedure in the LTM Cell Switch Command MAC CE and a non-zero Msg1 repetition number is indicated in the LTM Cell Switch Command MAC CE:  2> assume that Msg1 repetition is applicable and that the Msg1 repetition number applicable for the current Random Access procedure is the Msg1 repetition number indicated in the LTM Cell Switch Command MAC CE.  ------omit------  1> else if contention-free Random Access Resources have been provided for this Random Access procedure in the LTM Cell Switch Command MAC CE:  2> if RedCap is applicable for this Random Access procedure:  3> if a non-zero Msg1 repetition number is indicated in the LTM Cell Switch Command MAC CE:  4> select the set of Random Access resources that is only configured with RedCap indication and Msg1 repetition indication and associated with the indicated Msg1 repetition number for this Random Access procedure.  3> else:  4> if there is one set of Random Access resources available that is only configured with RedCap indication:  5> select this set of Random Access resources for this Random Access procedure.  4> else:  5> select the set of Random Access resources that is not associated with any feature indication (as specified in clause 5.1.1c) for this Random Access procedure.  2> else if eRedCap is applicable for this Random Access procedure:  3> if a non-zero Msg1 repetition number is indicated in the LTM Cell Switch Command MAC CE:  4> select the set of Random Access resources that is only configured with eRedCap indication and Msg1 repetition indication and associated with the indicated Msg1 repetition number for this Random Access procedure.  3> else:  4> if there is one set of Random Access resources available that is only configured with eRedCap indication:  5> select this set of Random Access resources for this Random Access procedure.  4> else if there is one set of Random Access resources available that is only configured with RedCap indication:  5> select this set of Random Access resources for this Random Access procedure.  4> else:  5> select the set of Random Access resources that is not associated with any feature indication (as specified in clause 5.1.1c) for this Random Access procedure.  2> else:  3> if a non-zero Msg1 repetition number is indicated in the LTM Cell Switch Command MAC CE:  4> select the set of Random Access resources that is only configured with Msg1 repetition indication and associated with the indicated Msg1 repetition number for this Random Access procedure.  3> else:  4> select the set of Random Access resources that is not associated with any feature indication (as specified in clause 5.1.1c) for this Random Access procedure. 6.1.3.75 LTM Cell Switch Command MAC CE The LTM Cell Switch Command MAC CE is identified by MAC subheader with eLCID as specified in Table 6.2.1-1b. It has a variable size with following fields (Figure 6.1.3.75-1):  - R: Reserved bit, set to 0;  - Target Configuration ID: This field indicates the index of candidate target configuration to apply for LTM cell switch, corresponding to *ltm-CandidateId* minus 1as specified in TS 38.331 [5]. The length of the field is 3 bits;  - Timing Advance Command: This field indicates whether the TA is valid for the LTM target cell (i.e. the SpCell corresponding to the target configuration indicated by Target Configuration ID field). If the value of this field is set to FFF, this field indicates that no valid timing adjustment is available for the PTAG of the LTM target cell; otherwise, this field indicates the index value *TA* used to control the amount of timing adjustment that the MAC entity has to apply in TS 38.213 [6], and that the UE can skip the Random Access procedure for this LTM cell switch. If *tag-Id-ptr* is configured for the TCI state indicated by the UL TCI state ID field, if present, or by the TCI state ID field otherwise, in the LTM target cell and *tag-Id-ptr* is set to value *n1*, this field indicates the TA for the TAG indicated by the *tag2-Id* of the LTM target cell; otherwise, this field indicates the TA for the TAG indicated by the *tag-id* of the LTM target cell. The length of the field is 12 bits; |

Since we have not discussed the same issue for inter-CU LTM, an FFS is kept for whether to follow the same principle as Rel-18 intra-CU LTM.

***Question1: Do companies agree that, the Rel-19 inter-CU LTM follows the same handling as Rel-18 intra-CU LTM on coexistence issues? In detail, Rel-19 inter-CU LTM could coexist with CovE, (e)RedCap and MIMO 2 TA while couldn’t coexist with NRU/NES.***

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes/No** | **Comment** |
|  |  |  |
|  |  |  |

For Rel-18 intra-CU LTM, we agreed the CFRA resource for cell switch could be provided in LTM Cell Switch MAC CE, which is as follows:



Figure 6.1.3.75-1: LTM Cell Switch Command MAC CE

Since we have not discussed the same issue for inter-CU LTM, an FFS is kept for whether the CFRA resource could also be included in the LTM Cell Switch Command MAC CE for inter-CU LTM.

***Question2:* Whether the CFRA resource configuration could be included in LTM cell switch command MAC CE for inter-CU LTM?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes/No** | **Comment** |
|  |  |  |
|  |  |  |

***Rapporteur believe other open issues on inter-CU LTM could be discussed based on companies contributions.***

## 2.2 L1 event triggered measurement reporting

In RAN2#126 meeting, we reached the following agreements on LTM event evaluation:

|  |
| --- |
| For LTM event evaluation, TTT, hysteresis for entering/leaving, and/or beam specific (FFS for cell specific) offset can be applied. FFS on the need of measurement reporting once leaving condition is met. |

An FFS that whether the cell specific offset is used for the L1 event evaluation. Though in the later RAN2#127 meeting, we agreed *Beam level measurement result, not cell level measurement result, is used LTM event evaluation*. It does not exclude the corresponding cell specific offset, since UE could also consider the cell specific offset for beam measurement results.

Based on the above, we would like to ask the following question:

***Question3: Do companies agree that the cell specific offset is used for LTM L1 event evaluation?***

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes/No** | **Comment** |
|  |  |  |
|  |  |  |

RAN1 has agreed the L1-RSRP measurement is used for event triggered reporting which is as follows:

|  |
| --- |
| Agreement   * SSB based L1-RSRP measurements is supported for event triggered reporting * CSI-RS based L1-RSRP measurements is supported for event triggered reporting * FFS: CSI-RS based L1-SINR measurements is supported for event triggered reporting   **Conclusion**  There is no consensus in RAN1 on the support L1-SINR measurement based on CSI-RS for candidate cells |

In the legacy L3 measurement based event triggered report, the “trigger quantity” could be different from the “report quantity” [2]:

|  |
| --- |
| For cell and beam measurements, reporting quantities can be any combination of quantities (i.e. only RSRP; only RSRQ; only SINR; RSRP and RSRQ; RSRP and SINR; RSRQ and SINR; RSRP, RSRQ and SINR; only RSCP; only EcN0; RSCP and EcN0), irrespective of the trigger quantity, and for CLI measurements, reporting quantities can be either SRS-RSRP or CLI-RSSI. |

However, there is no report quantity in Rel-18 LTM L1 measurement, in this case, the UE always performs L1-RSRP measurement. According to the RAN1 agreement, it seems the L1-SINR may be introduced for Rel-19 LTM. While for simplicity, the trigger quantity for LTM L1 event triggered measurement should be the same as the report quantity. In this way, there is no need to introduce the report quantity.

***Question4: Do companies agree that the trigger quantity for LTM L1 event triggered measurement should be the same as the report quantity?***

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes/No** | **Comment** |
|  |  |  |
|  |  |  |

***Rapporteur believe other open issues on L1 event triggered measurement report could be discussed based on companies contributions.***

## 2.3 Conditional LTM

***Rapporteur believe all open issues could be discussed based on companies contributions.***

# 3 Examining the running CR

This section is used to collect general comments on Running MAC CR for Mob Ph4.

***Question6: Any comments on the running CR?***

|  |  |  |
| --- | --- | --- |
| **Company** | **Issue** | **Suggestion** |
|  |  |  |

4 Conclusion

Based on the discussion above, we propose that

5 Reference

1. TS 3GPP 38.321 V18.4.0
2. TS 3GPP 38.331 V18.4.0