**3GPP TSG RAN WG2 Meeting #129 R2-250xxxx  
 Wuhan, China, 7th - 11th April 2025**

**Agenda item: 8.4.1**

**Source: Apple**

**Title: Collection of comments to 38.321 CR for LP-WUS**

**WID/SID: NR\_LPWUS-Core – Release 19**

**Document for: Discussion and Decision**

# 1 Introduction

This is a summary document on collection of comments to TS 38.321 CR for LP-WUS during below running CR discussion:

* [Post129][210][LPWUS] Running CR for TS 38.321 (Apple)

Intended outcome: Running CR for submission to the next meeting

Deadline: Long

# 2 Collection of comments

Please provide your comments in below table, and Rapporteur will response. Please do not insert any comments in running CR directly, which is hard for Rapporteur to follow all comments.

And based on existing EN and your comments, Rapporteur will identify stage 3 open issues.

|  |  |  |
| --- | --- | --- |
| **Company** | **Detailed comments** | **Rapporteur response** |
| NEC | LP-WUS Low-Power Wake-Up Signal  **Comment-1: seems like different spec use different term, e.g., in TS 38.304 running CR, it is Low Power-Wake Up Signal, need to align in the end.**  - lpwus\_PDCCHMonitoringTimer (Optional): the duration after the LP-WUS occasion in which a LP-WUS indicates the UE's PDCCH monitoring activity for the MAC entity.  **Comment-2: for the name definition, RAN2 has not decided yet. In our understanding, the definition of active time is broader than that of PDCCH timer (e.g., CSI reporting can be done in active time including this new timer I believe). Therefore we prefer to name it as *drx-onDurationTimer-LPWUS* (e.g., just referred from MBS).**  1> if LP-WUS monitoring is configured and no DRX group is in Active Time:  <omit>  4> if all LP-WUS monitoring occasion(s) in time domain, as specified in TS 38.213 [6], associated with the current DRX cycle occurred in Active Time considering…  **Comment-3: I am not sure if we specify [no DRX group is in active time] in 1>, do we still need 4> ?**  **Suggest to remove [no DRX group is in active time] in 1>, the clarification for LP-WUS monitoring outside active time can be reflected in other part or spec.**  2> if lpwus\_PDCCHMonitoringTimer is configured (i.e., LP-WUS Option 1-2):  3> if LP-WUS indication is received from lower layer indicated to start lpwus\_PDCCHMonitoringTimer, as specified in TS 38.213 [6]:  4> start lpwus\_PDCCHMonitoringTimer from the beginning of the subframe indicated from lower layer.  **Comment-4: do we need to consider what if LP-WUS (opt 1-2) occasion occurred in active time (just refer to LP-WUS opt 1-1)?** |  |
| Xiaomi | 1> if LP-WUS monitoring is configured and no DRX group is in Active Time:  …  4> if all LP-WUS monitoring occasion(s) in time domain, as specified in TS 38.213 [6], associated with the current DRX cycle occurred in Active Time considering grants/assignments/DRX Command MAC CE/Long DRX Command MAC CE received and Scheduling Request sent until 4 ms prior to start of the last LP-WUS occasion, or during a measurement gap, or when the MAC entity monitors for a PDCCH transmission on the search space indicated by recoverySearchSpaceId of the SpCell identified by the C-RNTI while the ra-ResponseWindow is running (as specified in clause 5.1.4):  5> start drx-onDurationTimer after drx-SlotOffset from the beginning of the subframe.  **Comment 1:** we also think the above two parts are contradicting with each other. Maybe remove one of those.  On the other hand, we think it is still unclear for option 1-1 whether UE still monitors LP-WUS during DRX active time/during measurement gap/will RAR window running.  **Comment 2:** there are some occurrences of lpwus\_PDCCHMonitoringTimer with/without “for the DRX group”. Better to align, i.e. add “for the DRX group” |  |
| Huawei, HiSilicon | Serving Cells of a MAC entity may be configured by RRC in two DRX groups with separate DRX parameters. When RRC does not configure a secondary DRX group, there is only one DRX group and all Serving Cells belong to that one DRX group. When two DRX groups are configured, each Serving Cell is uniquely assigned to either of the two groups. The DRX parameters that are separately configured for each DRX group are: *drx-onDurationTimer*, *drx-InactivityTimer*. The DRX parameters that are common to the DRX groups are: *drx-SlotOffset*, *drx-RetransmissionTimerDL*, *drx-RetransmissionTimerUL*, *drx-LongCycleStartOffset*, *drx-NonIntegerLongCycleStartOffset*, *drx-ShortCycle* (optional), *drx-NonIntegerShortCycle* (optional), *drx-ShortCycleTimer* (optional), *drx-HARQ-RTT-TimerDL*, and *drx-HARQ-RTT-TimerUL*.  - *drx-onDurationTimer,* *drx-InactivityTimer* or *lpwus\_PDCCHMonitoringTimer* configured for the DRX group is running; or  **Comment 1:** there is no conclusion whether LP-WUS can be configured with secondary DRX or not, so it is unclear whether the lpwus\_PDCCHMonitoringTimer can be “**for the DRX group**” or common to the DRX groups. A Editor’s Note or “[*lpwus\_PDCCHMonitoringTimer*]” can be added. Same issue exists for many places.  **Comment 2:** The “lpwus\_PDCCHMonitoringTimer” needs to be added in the first paragraph above, but FFS whether it is for each DRX group or common to the DRX groups. “lpwus\_PDCCHMonitoringTimer” also needs to be added in “RRC controls DRX operation by configuring the following parameters:” part.  4> if all LP-WUS monitoring occasion(s) in time domain, as specified in TS 38.213 [6], associated with the current DRX cycle occurred in Active Time considering grants/assignments/DRX Command MAC CE/Long DRX Command MAC CE received and Scheduling Request sent until 4 ms prior to start of the last LP-WUS occasion, or during a measurement gap, or when the MAC entity monitors for a PDCCH transmission on the search space indicated by *recoverySearchSpaceId* of the SpCell identified by the C-RNTI while the *ra-ResponseWindow* is running (as specified in clause 5.1.4):  5> start *drx-onDurationTimer* after *drx-SlotOffset* from the beginning of the subframe.  **Comment 3:** a new parameter and name for “drx-SlotOffset” is needed for LP-WUS option 1-1 to distinguish it from DCP, it is provided in LP-WUS configuration. And this new parameter needs to be added in “RRC controls DRX operation by configuring the following parameters:” part.  Agreement: In option 1-2, a new timer triggered by LPWUS is introduced. When this new timer is running, UE is in C-DRX active time. When UE is not in C-DRX active time, UE goes back to LPWUS monitoring.  **Comment 4:** For above agreement, currently we can only know that new timer impacts active time and PDCCH monitoring. But “ When UE is not in C-DRX active time, UE goes back to LPWUS monitoring” is not reflected in the spec. There is no any description for the UE behaviour of LP-WUS monitoring. |  |
| InterDigital | **Comment:** It is not meaningful to write the conditions for Long DRX cycle again for LP-WUS option 1-1 while they’re already available in the specification. Option 1-2 can be separated as it is not dependent on the DRX cycle.  One can just use “else if” condition after the DCP conditions for LP-WUS option 1-1. Option 1-2 can be separated as currently implemented since it does not depend on the DRX cycle.  Ie., for example:  1> if the Long DRX cycle is used for a DRX group and the *drx-NonIntegerLongCycleStartOffset* is not configured, and [(SFN × 10) + subframe number] modulo (*drx-LongCycle*) = *drx-StartOffset*; or  1> if the Long DRX cycle is used for a DRX group and the *drx-NonIntegerLongCycleStartOffset* is configured, and floor([(*DRX\_SFN\_COUNTER* × 10240) + (SFN × 10) + subframe number] modulo (*drx-NonIntegerLongCycle*)) = *drx-StartOffset*:  2> if DCP monitoring is configured for the active DL BWP as specified in TS 38.213 [6], clause 10.3:  (…)  2> else if *lpwus\_PDCCHMonitoringTimer* is not configured:  3> if LP-WUS monitoring is configured:  4> if LP-WUS indication associated with the current DRX cycle received from lower layer indicated to start *drx-onDurationTimer*, as specified in TS 38.213 [6]; or  4> if all LP-WUS monitoring occasion(s) in time domain, as specified in TS 38.213 [6], associated with the current DRX cycle occurred in Active Time considering grants/assignments/DRX Command MAC CE/Long DRX Command MAC CE received and Scheduling Request sent until 4 ms prior to start of the last LP-WUS occasion, or during a measurement gap, or when the MAC entity monitors for a PDCCH transmission on the search space indicated by *recoverySearchSpaceId* of the SpCell identified by the C-RNTI while the *ra-ResponseWindow* is running (as specified in clause 5.1.4):  5> start *drx-onDurationTimer* after *drx-SlotOffset* from the beginning of the subframe.  3> else:  4> start *drx-onDurationTimer* for this DRX group after *drx-SlotOffset* from the beginning of the subframe.  **[Sharp 001]:** Agree with comments from InterDigital. Regarding the wording, we prefer to swap 2> and 3>:  2> else if LP-WUS monitoring is configured:  3> if *lpwus\_PDCCHMonitoringTimer* is not configured:  Xxxxxx;  2> else:  3> start drx-onDurationTimer for this DRX group after drx-SlotOffset from the beginning of the subframe. |  |
| Sharp 002 | 1. if LP-WUS monitoring is configured and no DRX group is in Active Time:   **Comment:** For R16 DCP, no monitoring DCP during Active time is specified in RAN1 spec, then for LP-WUS the similar thing can be captured in RAN1 spec and the highlighted part seems unnecessary in RAN2 spec. |  |
| Sharp 003 | 1> if DCP monitoring is configured for the active DL BWP as specified in TS 38.213 [6], clause 10.3, or if LP-WUS monitoring is configured as specified in TS 38.213 [6], clause 10.X; and  ……  3> if *ps-TransmitPeriodicL1-RSRP* or *lpwus-TransmitPeriodicL1-RSRP* is not configured with value *true*:  4> not report periodic CSI that is L1-RSRP on PUCCH.  **Comment:** As per ASN.1 we understand “*ps-TransmitPeriodicL1-RSRP* is not configured with value *true*” means *ps-TransmitPeriodicL1-RSRP* is absent. Then based on 1> and 3>, if LP-WUS monitoring is configured, *lpwus-TransmitPeriodicL1-RSRP* is set to *true*, UE should report periodic CSI, however DCP monitoring is not configured, *ps-TransmitPeriodicL1-RSRP* must be absent, then the UE cannot report periodic CSI. It could be changed as below:  3> if DCP monitoring is configured and *ps-TransmitPeriodicL1-RSRP* is not configured with value true, or  3> if LP-WUS monitoring is configured and *lpwus-TransmitPeriodicL1-RSRP* is not configured with value true:  The same comment on *ps-TransmitOtherPeriodicCSI* and *lpwus-TransmitOtherPeriodicCSI*. |  |
|  |  |  |
|  |  |  |
|  |  |  |

# 3 Conclusion

Based on post-meeting email discussion, Rapporteur identify the following stage 3 open issues: