3GPP RAN WG2 Meeting #130 R2-25xxxxx

Malta, Malta May 19th – 23rd, 2025

Agenda Item: X.X.X

Source: Ericsson

Title: Remaining RRC open issues in feature AIML PHY

Document for: Discussion, Decision

# Introduction

The following document includes a list of open issues according to the following email discussion:

**[POST129bis][016][AI PHY] 38.331 Running CR (Ericsson)**

 Intended outcome:

1. Update CR based on agreements from RAN2#129bis
2. List of remaining open issues

 Deadline: Long

Companies are invited to provide feedback on open issue list by: **2 May 2025**

# Remaining open issues for specification TS 38.331

## LCM for UE-sided model for Beam Management use case

**Open issue RRC-1: Cause of inapplicability**

**Issue description:** It isFFS how to define the simple cause value of inapplicability related to model availability and how to capture it in the spec.

This issue refers to the RAN2#129bis agreement:

|  |
| --- |
| Together with inapplicability reporting, UE further indicates a simple cause value of inapplicability FFS how to define this simple cause related to model availability and how we capture it in the spec |

The issue is captured as an editor’s note in the running CR, clause 5.3.5.3.

**Proposed resolution:** It is suggested that companies provide contributions to the following meeting to resolve the issue.

**Open issue RRC-2: Content of *otherConfig* for enabling applicability reports in UAI**

**Issue description:** It is not yet clarified what the content (if any) of the UAI configuration should be, to enable the UE to report applicability in UAI, e.g. applicability updates/changes as agreed for option A. For instance, this configuration could be just a flag or could contain further information.

The issue is captured as an editor’s note in the running CR, clause 6.3.4.

**Proposed resolution:** It is suggested that companies provide contributions to the following meeting to resolve the issue.

**Open issue RRC-3: UE data collection request**

**Issue description:** For UE-side data collection**,** the details of UAI signaling for the UE start/stop request and especially the following aspects are not yet clarified:

* how to refer in UAI to a preferred radio resource candidate configuration from a list of candidate configurations provided by NW
* where/what the NW provides as candidate configurations
* what the content of *otherConfig* for enabling UE data collection requests in UAI should be (e.g. just a flag, the list of candidate UE data collection configurations, etc.).

This issue refers to the RAN2#129bis agreements:

The UE can request measurement configuration for data collection of AI/ML based beam management. The request can contain one or more of the following:

• An indication on start/stop of data collection

• Preferred configuration from a list of candidate configurations provided by NW. Details of signaling are FFS. It is up to network what it configures at the end.

Introduce UAI message for UE request of data collection measurement configuration. And it is up to UE implementation when to send the request.

The issue is captured as an editor’s notes in the running CR, clause 5.7.4.3, 6.2.2, and 6.3.4.

**Proposed resolution:** It is suggested that companies provide contributions to the following meeting to resolve the issue.

### Open issues requiring further RAN1 progress

**Open issue RRC-4: Definition of ‘applicable AI/ML functionality’**

**Issue description:** How to update the definition of ‘applicable AI/ML functionality’ in clause 3.1, e.g. replace 'functionality', and align it with RAN1 specs and with TS 38.300.

The issue is captured as an editor’s note in the running CR, in clause 3.1. The running CR also contains an example initial definition.

**Proposed resolution:** Suggest to wait for RAN1 progress.

**Open issue RRC-5: Applicability reporting for option B in *RRCReconfigurationComplete***

**Issue description:** It isFFS whether the applicability report for option B (sets of inference related parameters) can be included in *RRCReconfigurationComplete* (or if it can only be included in UAI).

This issue refers to the following RAN2#129bis agreement, based on which the overall design for option B requires further input from RAN1:

|  |
| --- |
| **Agreements on option B**1 RAN2 assumes UE receives RRCReconfiguration message including one set or multiple sets of inference related parameters via OtherConfig for option B. This assumption can be confirmed (i.e., whether to reconsider CSI-ReportConfig) after receiving Option B inference related parameters (e.g., in RAN1 RRC parameters list). Potential aspects to consider if RAN2 revisit:- To reconsider CSI-ReportConfig for option B, for example, if the list of inference related parameters is fully contained within existing CSI-ReportConfig.- to take into accounts UE behaviour when confirming the assumption e.g., whether option A and option B result in different UE behavior |

The issue is captured as an editor’s note in the running CR, clause 5.3.5.3.

**Proposed resolution:** Suggest to wait for RAN1 to provide the list of inference related parameters for option B.

**Open issue RRC-6: Terminology throughout RRC specs**

**Issue description:** It isFFS how to consistently update the AIML related terminology throughout the document (e.g. whether to adopt the terms 'measurement prediction', 'prediction configuration', etc.).

The issue is captured as an editor’s note in the running CR, clause 5.3.5.3.

**Proposed resolution:** Suggest to wait for RAN1 to provide the list of parameters for AI/ML beam management.

## NW side data collection

**Open issue RRC-7: NW control on retaining logged data at HO**

**Issue description:** Thesignaling details of the network control on how data should be retained at handover are FFS, based on the RAN2#129 bis agreement:

Introduce 1-bit indication on whether to release or retain un-retrieved data in RRCReconfiguration during/before HO. Source gNB decides whether the data should be kept. The indication is provided in RRCReconfiguration (i.e. not in RRC Reconfiguration from target cell). FFS signaling details.

The issue is captured as an editor’s note in the running CR, in clause 5.3.5.3 and 6.2.2.

It the rapporteur’s view, it should be clarified Whether/how the 1-bit indication can be sent during or before HO, taking into account that the source gNB decides whether the data should be kept. From the rapporteur perspective, it is not possible for the source gNB to add the 1-bit indication during HO, in the same RRCReconfiguration that encapsulates the RRCReconfiguration from the target gNB. Thus, the rapporteur sees the following two possible solutions for this issue:

* The source gNB sends the 1-bit indication to the UE before HO.
* The source gNB decides if the 1-bit indication is needed and, if so, sends it to the target gNB, which includes it in the RRCReconfiguration sent to the UE during HO. No RAN3 impact is expected if the transmission of the 1-bit indication is limited to the case in which the target gNB is from the same vendor as the source gNB.

**Proposed resolution:** It is suggested that companies provide contributions to the following meeting to resolve the issue.

**Open issue RRC-8: Reporting assistance information related to logged measurements**

**Issue description:** It is not yet clearwhat the *otherConfig* should contain to enable the UE to report assistance information via UAI, related to logging of radio measurements. For instance, should the low power, buffer full, and buffer threshold reached indications be all configured with a single bit, or should the configurations be separated?

This issue is related to the RAN2#129bis agreement:

|  |
| --- |
| **Agreements on availability indication*** Availability indication can be triggered due to:
	+ Full buffer being reached (if configured)
	+ Buffer threshold being reached (if configured).
	+ Low power (if configured)
* The UE send a UAI that indicates:
	+ Data is available
	+ Reason for trigger (full buffer, threshold)
	+ Low power indication
* The encoding of the data is available/UAI and the cause value is FFS

NOTE: it is up to UE Implementation how buffer threshold reached and low power is determined |

The issue is captured as an editor’s notes in the running CR, in clause 5.3.5.9, 5.7.4.3, 6.2.2, and 6.3.4.

**Proposed resolution:** It is suggested that companies provide contributions to the following meeting to resolve the issue.

**Open issue RRC-9: Further procedures for UE assistance information related to logging**

**Issue description:** It has not yet been discussed whether further procedures for UE reporting assistance information related to logging is need. Such further procedures may be, e.g. prohibit timers, indication that battery state is not low any longer, indication that the memory is not full any longer, etc.

The issue is captured as an editor’s note in the running CR, in clause 5.7.4.2 and 5.7.4.3.

**Proposed resolution:** It is suggested that companies provide contributions to the following meeting to resolve the issue.

**Open issue RRC-10: Time related content of logged data**

**Issue description:** It has not yet been clarified whatinformation needs to be included with the logged data, to indicate a time gap between the logged data entries (i.e. a gap that is longer than the logging data periodicity).

This issue refers to the RAN2#129bis agreement:

1. For temporal domain, the network is made aware whether there is a gap between two consecutive samples. FFS amount of gap and whether this is implicit or explicit

The issue is captured as an editor’s note in the running CR, in clause 5.7.10.3 and 6.2.2.

**Proposed resolution:** It is suggested that companies provide contributions to the following meeting to resolve the issue.

**Open issue RRC-11: RAN1 involvement for logged data for NW-side and UE-side data collection**

**Issue description:** Procedures for performing the L1 measurement results are captured in RAN1 specification, i.e. TS 38.214. Rapporteur assumes that the same should be applied for the case of radio measurements logging for the NW-side data collection and UE-side data collection. Hence RAN1 involvement is expected to capture procedures related to the radio measurements logging, e.g. in the UE variable *VarCSI-LogMeasReport* for the case of NW-side data collection.

From the rapporteur’s perspective, an LS should be sent to RAN1.

The issue is captured as an editor’s note in the running CR, in clause 5.7.10.3.

**Proposed resolution:** It is suggested that companies provide contributions to the following meeting to resolve the issue.

**Open issue RRC-12: Cell ID stored with logged data for NW-side data collection**

**Issue description:** It has not been clarified what type of cell ID the UE needs to log along with the logged data, in order to unambiguously identify the cell in which the UE performed the data logging, e.g. CGI, PCI-ARFCN etc.

The issue is captured as an editor’s note in the running CR, in clause 6.2.2.

**Proposed resolution:** It is suggested that companies provide contributions to the following meeting to resolve the issue.

**Open issue RRC-13: Where to include the logging configuration from NW to UE**

**Issue description:** It isFFS whether the logging configuration is included in the CSI framework (whether in *CSI-ReportConfig* or directly under *CSI-MeasConfig*) or at L3.

This issue was discussed in RAN2#129bis and the following outcome was captured:

|  |
| --- |
| * Next meeting proponents should work together and bring complete proposals to show specification impact and consider future use cases.
 |

The issue is captured as an editor’s note in the running CR, in clause 6.3.2.

**Proposed resolution:** It is suggested that companies provide contributions to the following meeting to resolve the issue.

**Open issue RRC-14: Multiplexing legacy logged data and AIML logged data in new SRB**

**Issue description:** RAN2#129bis agreed that

|  |
| --- |
| 2. New SRB can be configured for NW-side data collection (with lower priority) |

Given the agreement on the new SRB for the transmission of the *UEInformationResponse*, Rapporteur’s understanding is that the new SRB may be used also for the transmission of the legacy SON/MDT reports (e.g. logged MDT measurements, RLF-Report, RA-reports, successful HO reports, etc.), whenever the *UEInformationResponse* carries both a legacy SON/MDT report and AIML logged data. However, this would impact how legacy SON/MDT reporting is performed which can only be at the moment on SRB1 or SRB2.

From the specification perspective, this affects primarily RRC clause 5.7.10.3 and it would impact also other specifications, e.g. TS 37.320.

**Proposed resolution:** It is suggested that companies provide contributions to the following meeting to resolve the issue.

# Other identified open issues

Companies are invited to describe any other identified open issues not currently included within this document

|  |  |
| --- | --- |
| **Company** | **Other identified open issues? (please describe)** |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |

# Conclusions

*<To be filled after companies have provided feedback to the proposed resolutions for simple issues only. Please include the number of supporting companies (e.g., 18/20]) in brackets within the proposal>*

The following proposals have been provided based on feedback to the above document:

[Proposals for easy agreement]

*<List all proposals with consensus and/or may be easily agreed based on Rapporteur’s opinion>*

[Proposals for discussion]

*<List all proposals which will likely require further online/offline discussion to resolve>*

# References

1. XX

# Appendix (Optional)

*<Can include past meeting agreements etc.>*