3GPP TSG RAN WG2#129bis R2-250xxxx

Wuhan, China, 7th - 11th, April, 2025

**Title:** [Draft] LS on byte-aligned upper layer data SDU to CT1

**Response to:** -

**Release:** Rel-19

**Work Item:** Ambient\_IoT\_solutions

**Source:** vivo [to be RAN2]

**To:** CT1

**Cc:** RAN3, SA2

**Contact person:** Kimba Dit Adamou, Boubacar

kimba@vivo.com

**Send any reply LS to: 3GPP Liaisons Coordinator,** [**mailto:3GPPLiaison@etsi.org**](mailto:3GPPLiaison@etsi.org)

**Attachments:** -

# 1 Overall description

RAN2 has discussed the AIoT MAC PDU format design, and RAN2 has made the agreement to assume that for both R2D message and D2R message the upper layer data SDU to be contained in the AIoT MAC PDU is byte-aligned.

# 2 Actions

**To CT1:**

**ACTION:** RAN2 respectfully asks CT1 to take into account RAN2’s assumption and provide feedback if there is any concern.

# 3 Dates of next TSG RAN WG2 meetings

TSG RAN2 Meeting #130 19 - 23 May 2025 Malta, EU

TSG RAN2 Meeting #131 25 - 29 Aug 2025 Bangalore, India