**3GPP TSG-RAN WG2 Meeting #130 R2-250xxxx**

St Julian’s, Malta, 19-23 May 2025

**Agenda item: 8.13.1**

**Source: Samsung**

**Title: Summary on offline discussion on Rel-19 Relay Capability**

**WID/SID: NR\_SL\_relay\_multihop**

**Document for: Discussion and Decision**

# Introduction

This tdoc addresses the following e-mail discussion:

|  |
| --- |
| [Post130][401][Relay] Rel-19 relay capability (Samsung)  Scope: Develop draft CRs on relay capability for Rel-19, taking into account meeting agreements and resolving open issues where consensus can be found.  Intended outcome: Draft CRs to 38.306 and 38.331  Deadline: Long |

This post email discussion has two phases:

* **Phase 1**: Companies are invited to provide the comments and identify the issue that needs to be addressed, the deadline for phase 1 is  **Aug 1st, 2025 (10:00 UTC)**
* **Phase 2**: The CR will be provided according to the outcome of the phase 1 discussion, and the deadline for phased 2 is **Aug. 8th, 2025 (10:00 UTC)**

## Contact information

|  |  |
| --- | --- |
| **Company** | **Name (Email)** |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |

# Issue and discussion

In RAN2#130 meeting, the following agreements were reached:

Agreements:

Define a new capability for Rel-19 remote UE, e.g., remoteUE-MH-Operation-L2, with Rel-17 remote UE capability as a prerequisite.

As a baseline, implement the capability CR with a new capability for Rel-19 multihop relay UE, e.g., relayUE-MH-Operation-L2 with no distinction between last and intermediate cases. FFS if there is a need to distinguish last and intermediate (based, e.g., on the need for remote UE functionality in the intermediate relay).

There is no capability distinction between first and “non-first” intermediate relay UE.

Remote UE operation is a prerequisite for relay UE functionality (intermediate only if we decide to have the distinction between last and intermediate).

Meanwhile, the following proposals in R2-2504545 were not addressed during the meeting (P4 and P8 are removed since both are not applicable based on the current agreements):

Proposal 3: RAN2 is kindly asked to agree that the remote UE capability is the prerequisite of the capability of first/intermediate (non-first) relay UE.

~~Proposal 4: RAN2 is kindly asked to agree that the first relay UE capability is the prerequisite of the capability of intermediate (non-first) relay UE.~~

Proposal 5: RAN2 is kindly asked to agree the new band combination capability for multi-hop SL relay discovery, e.g., supportedBandCombListPerBS-MH-SL-RelayDiscovery.

Proposal 6: RAN2 is kindly asked to agree that capability for Rel-19 path switch, e.g., remoteUE-MH-PathSwitchOperation-L2-r18, which indicates the support of intra-gNB multi-hop indirect to direct path switching and intra-gNB multi-hop indirect to single-hop indirect path switching.

Proposal 7: RAN2 is kindly asked to discuss whether to define new capabilities for multi-hop L3 relay w.r.t L3 remote/first relay/intermediate relay(non-first)/last relay UE.

~~Proposal 8: RAN2 is kindly asked to discuss if the fast RRC setup scheme is agreed, whether a new capability w.r.t such optional feature is needed or not.~~

Thus, this discussion will be carried out starting from the above proposals.

**Issue 1: capability differentiation between last relay UE and intermediate relay UE**

This is related to “FFS if there is a need to distinguish last and intermediate (based, e.g., on the need for remote UE functionality in the intermediate relay)”. The discussion can consider the following aspects:

* **Aspect 1**: need of remote UE functionality of last relay UE
* **Aspect 2**: need of Uu functionality of intermediate relay UE. During online discussion, companies seem to think that the Uu functionality should be supported for intermediate relay UE.

In addition, according to RRC running CR, we have the following new IE defined for the intermediate relay UE for discovery with the editor note. This discussion is also related to how to conclude the editor note.

|  |  |  |
| --- | --- | --- |
| | *SL-RelayUE-ConfigMH* field descriptions | | --- | | ***sd-RSRP-ThreshDiscConfigMH***  Indicates the threshold of SD-RSRP for an Intermediate U2N Relay UE to evaluate AS layer conditions for discovery. The Intermediate U2N relay UE applies the value of this field to evaluate AS layer conditions to decide whether to forward the discovery solicitation message when performing the multi hop U2N Relay Discovery with Model B as specified in TS 23.304 [65]. |   Editor Note: FFS if these thresholds can also be used by Last U2N Relay UE to check AS condition before sending discovery response message to the intermediate Relay UE |

*Question 1: Is there a need to have capability differentiation between last relay UE and intermediate relay UE?*

|  |  |  |
| --- | --- | --- |
| Company | Yes/No | Comments |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

If there is a need to differentiate between last relay UE and intermediate relay UE, the resultant issue is how to indicate such capability. Two options can be considered:

* **Option 1**: define two new capabilities, LastRelayUE-MH-Operation-L2, and IntermediateRelayUE-MH-Operation-L2, where the remoteUE-MH-Operation-L2 is the prerequisite of IntermediateRelayUE-MH-Operation-L2;
* **Option 2**: keep relayUE-MH-Operation-L2 for both last relay UE and intermediate relay UE, while for intermediate relay UE, the remoteUE-MH-Operation-L2 also indicates.

*Question 2: How to indicate the capability of last relay UE and intermediate relay UE, if the capability differentiation is needed? If other options except the above Option 1&2 can be figured out, please indicate it below.*

|  |  |  |
| --- | --- | --- |
| Company | Option 1 or 2 | Comments |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

**Issue 2: band combination capability for multi-hop relay discovery**

In Rel-17, we have the supportedbandcombListPerBC-SL-RelayDiscovery which indicates, for a particular Uu band combination, the PC5 Relay discovery on which the UE supports simultaneous transmission/reception of PC5 data and Uu uplink/downlink respectively. Rel-19 may need a separate capability for multi-hop SL relay discovery.

*Question 3: is there a need to define the new band combination capability for multi-hop relay discovery?*

|  |  |  |
| --- | --- | --- |
| Company | Yes/No | Comments |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

**Issue 3: Capability for Rel-19 path switch**

In Rel-19, the path switch supports intra-gNB path switch with four scenarios, 1) MH indirect to direct (scenario A), 2) MH indirect to single-hop (scenario B), 3) direct to MH indirect (scenario C), and 4) single-hop indirect to MH indirect (scenario D). The following agreements were reached for path switch:

Agreements:

RAN2 will not address cases of service continuity towards a relay path with intermediate relays in idle/inactive under the current WID.

Agreements:

For scenario C, the legacy path-switching command and procedure are reused for the Remote UE and the target first Relay UE. Upon receiving the path-switching command, the Remote UE performs the legacy UE behavior toward the target first Relay UE. The (first)intermediate/last Relay UE belonging to the target path should be in the RRC-connected state.

For scenario D, the legacy path-switching command and procedure are reused for the Remote UE and the first Relay UE in the target path. Upon receiving the path-switching command, the Remote UE performs legacy UE behavior toward the first Relay UE on the target path. The (first)intermediate/last Relay UE belonging to the target path should be in the RRC-connected state.

It can be observed that the path switch towards the paths containing relay UE in RRC\_IDLE/INACTIVE is not allowed in Rel-19, which is different from Rel-17 and Rel-18. It is better to define new path switch capability for Rel-19.

*Question 4: is there a need to define the new capability for path switch Rel-19, e.g., remoteUE-MH-PathswitchOperation-L2?*

|  |  |  |
| --- | --- | --- |
| Company | Yes/No | Comments |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

**Issue 4: L3 relay capability**

We have reached the following agreements to address L2 MH relay design in RAN2:

RAN2 will focus solely on the L2 Multi-hop Relay design within the scope of this work item. This does not exclude that some work (e.g., discovery conditions, transmission resources) could be reused in L3 without specific impact under our WI.

It is reasonable to not define the capability related to L3 relay.

*Question 5: is there a need to define the new capability for L3 relay in Rel-19?*

|  |  |  |
| --- | --- | --- |
| Company | Yes/No | Comments |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

**Issue 5: Capability pre-requisite**

We have agreed the following pre-requisite:

* (already agreed) Remote UE capability is the pre-requisite of Rel-19 remote UE capability (i.e., remoteUE-MH-Operation-L2)
* Relay UE capability is the pre-requisite of Rel-19 relay UE capability (i.e., relayUE-MH-Operation-L2)

Depending on the discussion on new defined capability for Rel-19, the following potential pre-requisite can be considered:

* IntermediateRelayUE-MH-Operation-L2 (if defined, in Question 2): the pre-requisite is remoteUE-MH-Operation-L2
* remoteUE-MH-PathswitchOperation-L2 (if defined, in Question 4): the pre-requisite is remoteUE-MH-Operation-L2

*Question 6: Do you agree the above two additional pre-requisite if the corresponding capability is defined?*

|  |  |  |
| --- | --- | --- |
| Company | Yes/No | Comments |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

**Others**

*Question 7: Please indicate the additional capability, if any, which is not addressed in above discussion.*

|  |  |
| --- | --- |
| Company | Comments |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |

# 2 Conclusion