**3GPP TSG-RAN WG2 Meeting #131bis *R2-250xxxx***

**Prague, Czech Republic, 13 – 17 October 2025**

**Agenda item: 8.x.x**

**Source: Xiaomi**

**Title: Open issues of Rel-19 AIML air UE capabilities**

**Document for: Discussion and Decision**

# Introduction

As part of email discussion “[POST131][043][AI PHY] UE capabilities (Xiaomi)”, this document is to collect open issues on Rel-19 AIML air UE capabilities.

Phase 1: Companies are invited to provide input on open issue list no later than 19th Sep.

Phase 2: Rapporteur will further provide the resolution to each open issue afterwards. Companies further input on the open issue list and resolution are expected before 1st Oct.

|  |  |  |
| --- | --- | --- |
| **Company** | **Name** | **Email** |
| Samsung | Beom | s90.jeong@samsung.com |
| Lenovo | Congchi Zhang | zhangcc16@lenovo.com |
|  |  |  |
|  |  |  |
|  |  |  |

# Discussion

During previous discussion, rapporteur observes there’s only one open issue left:

***Open issue UECap-1: whether UE can support other memory sizes and indicate to network via optional capability signaling***

*Issue Description:*

This was discussed during the email discussion, and there are 5 companies think that UE can optionally indicate other AS layer memory sizes to network due to the following reasons:

- network flexibility for higher buffer threshold configuration

- common AS layer buffer might need larger memory size to support other use cases as well

4/9 companies don’t agree to indicate other memory size to network due to the following reasons:

- for Rel-19 data collection, no need for additional memory

- more memory size is up to UE implementation

- network can retrieve data based on UE buffer full indication

*Status in running CR:*

Not captured

Based on offline and online discussion, the supporting of additional memory sizes mainly motivated by supporting more flexible buffer-threshold based configuration. It seems reasonable to consider *dataThresholdAvailabiltyIndication-r19* as the prerequisite of this new capability (if introduced). If *dataThresholdAvailabiltyIndication-r19* is not supported, UE does not need to support additional memory size.

Therefore, rapporteur proposes with the following way-forward, where the candidate values consider memory size supported in *qoe-AdditionalMemoryMeasReport-r18* as baseline (except introducing a smaller value of 64kB):

**Proposal 1: Define *aiml-AdditionalMemoryReport-r19* to indicate the additional AS layer memory size the UE support for logged measurement of network-side data collection in addition to 64kB.**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| ***aiml-AdditionalMemoryReport-r19***Indicates whether the UE supports the additional AS layer memory size the UE support for logged measurement of network-side data collection in addition to 64kB. Value kB64 means the UE supports at least 64 kilobytes for this purpose, and so on. A UE supporting this feature shall also indicate support of *dataThresholdAvailabiltyIndication-r19*. | UE | No | No | No |

***AIML-Parameters* information element**

-- ASN1START

-- TAG-AIML-PARAMETERS-START

AIML-Parameters-r19 ::= SEQUENCE {

 applicabilityReportingCSI-r19 ENUMERATED {supported} OPTIONAL,

 applicabilityReportingOther-r19 ENUMERATED {supported} OPTIONAL,

 loggedDataCollection-r19 ENUMERATED {supported} OPTIONAL,

 eventBasedLoggedDataCollection-r19 ENUMERATED {supported} OPTIONAL,

 dataThresholdAvailabilityIndication-r19 ENUMERATED {supported} OPTIONAL,

 aiml-AdditionalMemoryReport-r19 ENUMERATED {kB64, kB128, kB256, kB512, kB1024}

OPTIONAL

}

-- TAG-AIML-PARAMETERS-STOP

-- ASN1STOP

**Q1: Do companies agree with above proposal and the relative TPs for this new introduced capability? Comment to the TP is also welcomed.**

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes/No** | **Comment** |
| Samsung | Yes but | We assume additional memory is also useful for NW to select the UE with large memory to collect much data, rather configuring multiple UEs. So, we agree with this proposal but some updates are suggested1. The proposed values (64KB, 128KB, …1024KB) are in addition to 64KB. It means UE’s total memory would be like 64+64=128KB, 128+64= 192KB, 256+64=320KB,…. In our understanding, common UE implementation usually supports the memory size as power of 2. In that sense, these sizes (128KB, 192KB, 320KB…) are not preferred. So, we suggest the memory as power of 2. It could be achieved with the following update:

|  |
| --- |
| ***aiml-AdditionalMemoryReport-r19***Indicates **~~whether the UE supports~~** the **~~additional~~** AS layer memory size the UE support**s** for logged measurement of network-side data collection **~~in addition to~~larger than** 64kB. Value kB**~~64~~128** means the UE supports at least **~~64~~128** kilobytes for this purpose, and so on.  |

 aiml-AdditionalMemoryReport-r19 ENUMERATED {**~~kB64~~**, kB128, kB256, kB512, kB1024} OPTIONAL}2. We are not sure if this capability should be dependant to *dataThresholdAvailabiltyIndication*. We think this capability is still useful for NW’s UE selection with large buffer and other potential use-cases |

Besides the above open issue, companies are invited to describe any identified open issues in the table below.

|  |  |  |
| --- | --- | --- |
| **Company** | **Description of open issues and potential resolution** | **Rapporteur comment** |
| Samsung | Given we agreed to report applicability in RRCResumeComplete message, the following update is needed:

| Definitions for parameters |
| --- |
| ***applicabilityReportingCSI-r19***Indicates whether the UE supports applicability reporting and/or its updates (via *RRCReconfigurationComplete* or via *UEAssistanceInformation* message or via RRCResumeComplete) based on inference configuration provided via *CSI-ReportConfig*, as specified in TS 38.331 [9]. It is mandatory if UE supports at least one of *aiml-BM-Case1-r19*, *aiml-BM-Case2-r19* and *aiml-CSI-Prediction-r19*. |
| ***applicabilityReportingOther-r19***Indicates whether the UE supports applicability reporting and/or its updates (via *RRCReconfigurationComplete* or via *UEAssistanceInformation* message or via RRCResumeComplete message) based on inference related configuration provided via *OtherConfig*, as specified in TS 38.331 [9].It is mandatory if UE supports at least one of *aiml-BM-Case1-r19* and *aiml-BM-Case2-r19*. |

 |  |
| Lenovo | [Terminology Alignment] 38.331To align with stage 2 CR. Suggest “AI/ML-based” beam management and “AI/ML-based” CSI prediction.  |  |
| Lenovo | [Terminology Alignment] 38.306Mixed use of “memory” and “buffer”As raised also over email, we have been using "buffer" during our WI discussion. On the other hand, when it comes to spec terminology w.r.t logging, we notice the term "memory" is actually used in MDT/QoE description.Suggest “full buffer indication” 🡪 “full memory indication”It is also relevant to 38.331, 38.300. Depending on relevant rapporteurs, we can either decide here (since term “memory” and “buffer” differs from capability point of view) or in other discussion. |  |
|  |  |  |
|  |  |  |

# Conclusion

In this contribution, we collect open issues of Rel-19 AIML air UE capabilities. Based on above discussion, following open issues are identified: