**3GPP TSG-CT WG3 Meeting #142 *C3-253229***

**Goteborg, SE, 25 - 29 August 2025**

|  |
| --- |
| *CR-Form-v12.3* |
| **CHANGE REQUEST** |
|  |
|  |  | **CR** | **0394** | **rev** | **1** | **Current version:** |  |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **X** |

|  |
| --- |
|  |
| ***Title:***  | EN resolution on Resources and Service operation provisioning |
|  |  |
| ***Source to WG:*** |  |
| ***Source to TSG:*** | CT3 |
|  |  |
| ***Work item code:*** | CAPIF\_Ph3 |  | ***Date:*** |  |
|  |  |  |  |  |
| ***Category:*** | **B** |  | ***Release:*** |  |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-17 (Release 17)Rel-18 (Release 18)Rel-19 (Release 19)Rel-20 (Release 20)* |
|  |  |
| ***Reason for change:*** | This CR is resolving ENs related to the Resources and Service Operations encoding in API discovery and API publishing CAPIF functionality.It is proposed to provide the following mapping:* Service API operation is represented as HTTP method supported at REST resource;
* API resource is mapped to the REST resource and provided in Service API operation description.

In CAPIF\_Publish\_Service\_API, it is proposed to provision the resources and service operations via representation of the services operations, i.e., the description of service operations conains the list of HTTP methods and related resource; thus, it is sufficient for provisioning of the available API resources. |
|  |  |
| ***Summary of change:*** | This CR resolving the ENs related to the Resources and Service Operations encoding in API discovery and API publishing CAPIF functionality. |
|  |  |
| ***Consequences if not approved:*** | The definition of the CAPIF\_Ph3 functionality cannot be completed in the stage 3. |
|  |  |
| ***Clauses affected:*** | 8.1.2.2.3.1, 8.1.4.1, 8.1.4.1, A.2 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ... |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** | This CR provides backward compatible feature for the following APIs:* TS29222\_CAPIF\_Discover\_Service\_API.yaml
 |
| ***()*** |  |
| ***This CR's revision history:*** |  |

**Additional discussion(if needed):**

**Proposed changes:**

\* \* \* First Change \* \* \* \*

###### 8.1.2.2.3.1 GET

The HTTP GET method enables to retrieve a list of APIs currently registered at the CCF and satisfying a number of filter criteria.

Table 8.1.2.2.3.1-1: URI query parameters supported by the GET method on this resource

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Name | Data type | P | Cardinality | Description | Applicability |
| api-invoker-id | string | M | 1 | It represents the identifier (assigned by the CCF) ofthe API invoker that is sending the request. It may also represent the identifier of the CCF that is sending the request if the request is sent over the CAPIF-6/6e reference point. (NOTE 1) |  |
| api-name | string | O | 0..1 | Contains the API name as {apiName} part of the URI structure as defined in clause 5.2.4 of 3GPP TS 29.122 [14]. |  |
| api-version | string | O | 0..1 | Contains the API major version conveyed in the URI (e.g. v1). |  |
| comm-type | CommunicationType | O | 0..1 | Communication type used by the API (e.g. REQUEST\_RESPONSE). |  |
| protocol | Protocol | O | 0..1 | Protocol used by the API. |  |
| aef-id | string | O | 0..1 | AEF identifier. |  |
| data-format | DataFormat | O | 0..1 | Data format used by the API (e.g. serialization protocol JSON). |  |
| api-cat | string | O | 0..1 | The service API category to which the service API belongs. |  |
| preferred-aef-loc | AefLocation | O | 0..1 | The preferred AEF location. If this parameter is present, the CCF shall try to discover a matched AEF location the service API supports. This parameter is ignored by the CCF if there is no matching record found. |  |
| req-api-prov-name | string | O | 0..1 | Represents the required API provider name. | RNAA |
| api-supported-features | SupportedFeatures | C | 0..1 | Features supported by the discovered service API indicated by api-name parameter. This may only be present if the api-name query parameter is present. | ApiSupportedFeatureQuery |
| ue-ip-addr | IpAddrInfo | O | 0..1 | Represents the UE IP address information. | RNAA |
| service-kpis | ServiceKpis | O | 0..1 | Contains information about service characteristics provided by the targeted service API(s). | EdgeApp\_2 |
| net-slice-info | array(NetSliceId) | O | 1..N | Contains the identifier(s) of the network slice(s) within which the API shall be available. | SliceBasedAPIExposure |
| grant-types | array(OAuthGrantType) | O | 1..N | Contains the OAuth grant types that need to be supported.This query parameter may be present only in case of RNAA, as defined in clause 6.5.3 of TS 33.122 [16]. Otherwise, it is not applicable and shall not be present. | RNAA |
| api-ids | array(string) | C | 1..N | Contains the identifier(s) of the targeted service APIs.(NOTE 3) | MultiStepDiscovery |
| supported-features | SupportedFeatures | O | 0..1 | Contains the list of supported features among the ones defined in clause 8.1.6.This attribute shall be present only when feature negotiation needs to take place. |  |
| resources-operations | array(ResOperInfo) | O | 1..N | Contains the list of supported API resource(s) and service operations.This query parameter may only be present if the "api-name" query parameter is present. | CAPIF\_Ext1 |
|  |  |  |  |  |  |
| NOTE 1: This parameter is not part of the API filter criteria so that it is not used in matching APIs published in the CCF.NOTE 2: In addition to the above standardized query parameters, the service consumer may also provide vendor-specific query parameter(s) as specified in clause 5.2.13.3 of 3GPP TS 29.122 [14]. The CCF shall use any received vendor-specific query parameters in the filtering process of the results to be returned in the response in a similar way and in addition to the standardized query parameters defined in this table. This capability may be signalled using the "VendSpecQueryParams" feature.NOTE 3: When the "MultiStepDiscovery" feature is supported and this query parameter is present, then all the other query parameters in this table shall be absent except the "supported-features" and "api-invoker-id" query parameters. |

This method shall support the request data structures specified in table 8.1.2.2.3.1-2 and the response data structures and response codes specified in table 8.1.2.2.3.1-3.

Table 8.1.2.2.3.1-2: Data structures supported by the GET Request Body on this resource

|  |  |  |  |
| --- | --- | --- | --- |
| Data type | P | Cardinality | Description |
| n/a |  |  |  |

Table 8.1.2.2.3.1-3: Data structures supported by the GET Response Body on this resource

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Data type | P | Cardinality | Responsecodes | Description |
| DiscoveredAPIs | M | 1 | 200 OK | The response body contains the result of the search over the list of registered APIs. |
| n/a |  |  | 307 Temporary Redirect | Temporary redirection.The response shall include a Location header field containing an alternative target URI of the resource located in an alternative CCF.Redirection handling is described in clause 5.2.10 of 3GPP TS 29.122 [14]. |
| n/a |  |  | 308 Permanent Redirect | Permanent redirection.The response shall include a Location header field containing an alternative target URI of the resource located in an alternative CCF.Redirection handling is described in clause 5.2.10 of 3GPP TS 29.122 [14]. |
| ProblemDetails | O | 0..1 | 414 URI Too Long | Indicates that the server refuses to process the request because the request-target is too long. |
| NOTE: The mandatory HTTP error status codes for the HTTP GET method listed in table 5.2.6-1 of 3GPP TS 29.122 [14] shall also apply. |

Table 8.1.2.2.3.1-4: Headers supported by the 307 Response Code on this resource

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Name | Data type | P | Cardinality | Description |
| Location | string | M | 1 | Contains an alternative target URI of the resource located in an alternative CCF. |

Table 8.1.2.2.3.1-5: Headers supported by the 308 Response Code on this resource

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Name | Data type | P | Cardinality | Description |
| Location | string | M | 1 | Contains an alternative target URI of the resource located in an alternative CCF. |

\* \* \* Next change \* \* \* \*

#### 8.1.4.1 General

This clause specifies the application data model supported by the API. Data types listed in clause 7.2 also apply to this API.

Table 8.1.4.1-1 specifies the data types defined specifically for the CAPIF\_Discover\_Service\_API.

Table 8.1.4.1-1: CAPIF\_Discover\_Service\_API specific Data Types

|  |  |  |  |
| --- | --- | --- | --- |
| Data type | Section defined | Description | Applicability |
| DiscoveredAPIs | Clause 8.1.4.2.2 | Represents a list of APIs currently registered at the CCF and satisfying a number of filter criteria provided by the service consumer. |  |
| IpAddrInfo | Clause 8.1.4.2.4 | Represents the UE IP address information. | RNAA |
| ResOperInfo | Clause 8.1.4.2.5 | Represents the resourse or service operation. | CAPIF\_Ext1 |

Table 8.1.4.1-2 specifies data types re-used by the CAPIF\_Discover\_Service\_API from other specifications, including a reference to their respective specifications, and when needed, a short description of their use within the CAPIF\_Discover\_Service\_API.

Table 8.1.4.1-2: Re-used Data Types

|  |  |  |  |
| --- | --- | --- | --- |
| Data type | Reference | Comments | Applicability |
| AefLocation | Clause 8.2.4.2.10 | Used to indicate the AEF location. |  |
| CommunicationType | Clause 8.2.4.3.5 | Used to indicate the communication type used by the API. |  |
| Ipv4Addr | 3GPP TS 29.122 [14] | Used to indicate an IPv4 address. | RNAA |
| Ipv6Addr | 3GPP TS 29.122 [14] | Used to indicate an IPv6 address. | RNAA |
| NetSliceId | 3GPP TS 29.435 [31] | Represents the identification information of a network slice. | SliceBasedAPIExposure |
| OAuthGrantType | Clause 8.5.4.3.4 | Represents the OAuth grant type. | RNAA |
| ProblemDetails | 3GPP TS 29.122 [14] | Used to represent additional information and details on an error response. |  |
| ServiceKpis | Clause 8.2.4.2.13 | Represents information about the service characteristics provided by a service API. | EdgeApp\_2 |
| SupportedFeatures | 3GPP TS 29.571 [19] | Represents the list of supported feature(s) and used to negotiate the applicability of the optional features. |  |

\* \* \* Next change \* \* \* \*

##### 8.1.4.2.5 Type: ResOperInfo

Table 8.1.4.2.5-1: Definition of type ResOperInfo

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description | Applicability |
| path | Uri | C | 0..1 | Represents the relative URI path after the API URI as defined in clause 5.2.4 of 3GPP TS 29.122 [14].This attribute shall not be present for custom service operation without associated resource. |  |
| operation | array(Operation) | O | 1..N | Represents the API service operation (i.e., HTTP method) supported at the resource provided in the "path" attribute.(NOTE) |  |
| customServOper | array(string) | O | 1..N | Represents the custom service operation name supported at the endpoint provided in the "path" attribute.(NOTE) |  |
| NOTE: These attributes are mutally exclusive. |

\* \* \* Next change \* \* \* \*

# A.2 CAPIF\_Discover\_Service\_API

openapi: 3.0.0

info:

 title: CAPIF\_Discover\_Service\_API

 description: |

 API for discovering service APIs.

 © 2025, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

 All rights reserved.

 version: "1.4.0-alpha.2"

externalDocs:

 description: 3GPP TS 29.222 V19.2.0 Common API Framework for 3GPP Northbound APIs

 url: https://www.3gpp.org/ftp/Specs/archive/29\_series/29.222/

servers:

 - url: '{apiRoot}/service-apis/v1'

 variables:

 apiRoot:

 default: https://example.com

 description: apiRoot as defined in clause 7.5 of 3GPP TS 29.222.

paths:

 /allServiceAPIs:

 get:

 description: >

 Discover published service APIs and retrieve a collection of APIs according

 to certain filter criteria.

 parameters:

 - name: api-invoker-id

 in: query

 description: >

 String identifying the API invoker assigned by the CAPIF core function.

 It also represents the CCF identifier in the CAPIF-6/6e interface.

 required: true

 schema:

 type: string

 - name: api-name

 in: query

 description: >

 API name, it is set as {apiName} part of the URI structure as defined

 in clause 5.2.4 of 3GPP TS 29.122.

 schema:

 type: string

 - name: api-version

 in: query

 description: API major version the URI (e.g. v1).

 schema:

 type: string

 - name: comm-type

 in: query

 description: Communication type used by the API (e.g. REQUEST\_RESPONSE).

 schema:

 $ref: 'TS29222\_CAPIF\_Publish\_Service\_API.yaml#/components/schemas/CommunicationType'

 - name: protocol

 in: query

 description: Protocol used by the API.

 schema:

 $ref: 'TS29222\_CAPIF\_Publish\_Service\_API.yaml#/components/schemas/Protocol'

 - name: aef-id

 in: query

 description: AEF identifer.

 schema:

 type: string

 - name: data-format

 in: query

 description: Data formats used by the API (e.g. serialization protocol JSON used).

 schema:

 $ref: 'TS29222\_CAPIF\_Publish\_Service\_API.yaml#/components/schemas/DataFormat'

 - name: api-cat

 in: query

 description: The service API category to which the service API belongs to.

 schema:

 type: string

 - name: preferred-aef-loc

 in: query

 description: The preferred AEF location.

 content:

 application/json:

 schema:

 $ref: 'TS29222\_CAPIF\_Publish\_Service\_API.yaml#/components/schemas/AefLocation'

 - name: req-api-prov-name

 in: query

 description: Represents the required API provider name.

 schema:

 type: string

 - name: api-supported-features

 in: query

 description: >

 Features supported by the discovered service API indicated by api-name parameter.

 This may only be present if api-name query parameter is present.

 schema:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

 - name: ue-ip-addr

 in: query

 description: Represents the UE IP address information.

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/IpAddrInfo'

 - name: service-kpis

 in: query

 description: >

 Contains iInformation about service characteristics provided by the targeted

 service API(s).

 content:

 application/json:

 schema:

 $ref: 'TS29222\_CAPIF\_Publish\_Service\_API.yaml#/components/schemas/ServiceKpis'

 - name: net-slice-info

 in: query

 description: >

 Contains the identifier(s) of the network slice(s) within which the API

 shall be available.

 content:

 application/json:

 schema:

 type: array

 items:

 $ref: 'TS29435\_NSCE\_PolicyManagement.yaml#/components/schemas/NetSliceId'

 minItems: 1

 - name: grant-types

 in: query

 description: Contains the OAuth grant types that need to be supported.

 required: false

 content:

 application/json:

 schema:

 type: array

 items:

 $ref: 'TS29222\_CAPIF\_Security\_API.yaml#/components/schemas/OAuthGrantType'

 minItems: 1

 - name: api-ids

 in: query

 description: >

 Contains the identifier(s) of the targeted service APIs.

 When this query parameter is present, then all the other query parameters shall be

 absent except the supported-features and api-invoker-id query parameters.

 required: false

 style: form

 explode: false

 schema:

 type: array

 items:

 type: string

 minItems: 1

 - name: resources

 in: query

 description: >

 Contains the list of supported API resource(s).

 required: false

 style: form

 explode: false

 schema:

 type: array

 items:

 $ref: 'TS29222\_CAPIF\_Publish\_Service\_API.yaml#/components/schemas/Resource'

 minItems: 1

 - name: custom-serv-opers

 in: query

 description: >

 Contains the list of supported API custom service operation(s).

 required: false

 content:

 application/json:

 schema:

 type: array

 items:

 $ref: 'TS29222\_CAPIF\_Publish\_Service\_API.yaml#/components/schemas/CustomOperation'

 minItems: 1

 - name: supported-features

 in: query

 description: Features supported by the NF consumer for the CAPIF Discover Service API.

 schema:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

 responses:

 '200':

 description: >

 The response body contains the result of the search over the list of registered APIs.

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/DiscoveredAPIs'

 '307':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/307'

 '308':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/308'

 '400':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/404'

 '406':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/406'

 '414':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/414'

 '429':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29122\_CommonData.yaml#/components/responses/default'

components:

 schemas:

 DiscoveredAPIs:

 type: object

 description: >

 Represents a list of APIs currently registered in the CAPIF core function

 and satisfying a number of filter criteria provided by the API consumer.

 properties:

 serviceAPIDescriptions:

 type: array

 items:

 $ref: 'TS29222\_CAPIF\_Publish\_Service\_API.yaml#/components/schemas/ServiceAPIDescription'

 minItems: 1

 description: >

 Description of the service API as published by the service. Each service

 API information shall include AEF profiles matching the filter criteria.

 suppFeat:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

 IpAddrInfo:

 type: object

 description: Represents the UE IP address information.

 properties:

 ipv4Addr:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/Ipv4Addr'

 ipv6Addr:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/Ipv6Addr'

 oneOf:

 - required: [ipv4Addr]

 - required: [ipv6Addr]

\* \* \* End of changes \* \* \* \*