**3GPP TSG CT WG3 Meeting #142 C3-253439**

**Goteborg, Sweden, 25 – 29 August, 2025 (Revision of C3-253xxx)**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.3* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  | **29.122** | **CR** | **0969** | **rev** | **-** | **Current version:** | **19.3.0** |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **X** |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | Support of reporting the QoS notification event with direction information | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | Huawei, Nokia | | | | | | | | | |
| ***Source to TSG:*** | CT3 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | XRM\_Ph2 | | | | |  | ***Date:*** | | | 2025-08-08 |
|  |  | | | |  | |  | | |  |
| ***Category:*** | **B** |  | | | | | ***Release:*** | | | Rel-19 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-17 (Release 17) Rel-18 (Release 18) Rel-19 (Release 19)  Rel-20 (Release 20)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | As defined in clause 6.1.3.18 TS 23.503, if the PCF receives a direction information together with the notification from the SMF, the PCF shall also forward the direction information to the AF. This CR proposes to support the reporting of direction information together with the QoS notification control. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | * Define QoSNotification and Direction data types and update UserPlaneEventReport data type to support the reporting of direction information together with the QoS notification control. * Enhance the ExtQoS\_v2 feature and update the OpenAPI file accordingly. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | The stage 2 requirement is not supported in stage 3. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | 5.14.2.1.1, 5.14.2.1.5, 5.14.2.1.16, 5.14.2.2.4, 5.14.4, A.14 | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  | **X** | Other core specifications | | | | TS/TR ... CR ... | | |
| ***affected:*** | |  | **X** | Test specifications | | | | TS/TR ... CR ... | | |
| ***(show related CRs)*** | |  | **X** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | | This CR introduces a backward compatible feature to the following API:  - TS29122\_AsSessionWithQoS.yaml | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | |  | | | | | | | | |

\*\*\* 1st Change \*\*\*

##### 5.14.2.1.1 Introduction

This clause defines data structures to be used in resource representations, including subscription resources.

Table 5.14.2.1.1-1 specifies data types re-used by the AsSessionWithQoS API from other specifications, including a reference to their respective specifications and when needed, a short description of their use within the AsSessionWithQoS API.

Table 5.14.2.1.1-1: AsSessionWithQoS API re-used Data Types

|  |  |  |  |
| --- | --- | --- | --- |
| Data type | Reference | Comments | Applicability |
| AcceptableServiceInfo | 3GPP TS 29.514 [52] | Acceptable service information. |  |
| AlternativeServiceRequirementsData | 3GPP TS 29.514 [52] | Contains alternative QoS related parameters and a reference to them. | AltQosWithIndParams\_5G, MultiMedia |
| AverWindow | 3GPP TS 29.571 [45] | Averaging Window. | EnQoSMon, GMEC |
| AverWindowRm | 3GPP TS 29.571 [45] | This data type is defined in the same way as the "AverWindow" data type, but with the OpenAPI "nullable: true" property. | EnQoSMon, GMEC |
| BatOffsetInfo | 3GPP TS 29.514 [52] | Contains the offset of the BAT and the optionally adjusted periodicity. | EnTSCAC |
| BitRate | 3GPP TS 29.571 [45] | String representing a bit rate that shall be formatted as follows:  Pattern: '^\d+(\.\d+)? (bps|Kbps|Mbps|Gbps|Tbps)$'  Examples:  "125 Mbps", "0.125 Gbps", "125000 Kbps" | EnQoSMon, ListUE\_5G, MultiMedia |
| BitRateRm | 3GPP TS 29.571 [45] | This data type is defined in the same way as the "BitRate" data type, but with the OpenAPI "nullable: true" property. | EnQoSMon, ListUE\_5G, MultiMedia |
| CapabilityReport | 3GPP TS 29.514 [52] | Indicates the capability is supported or not for the corresponding capability type. | QoSMonCapRepo |
| Dnn | 3GPP TS 29.571 [45] | Identifies a DNN. |  |
| DurationMilliSec | 3GPP TS 29.514 [52] | Indicates the time interval in units of milliseconds. | PowerSaving |
| DurationMilliSecRm | 3GPP TS 29.514 [52] | This data type is defined in the same way as the "DurationMilliSec" data type, but with the OpenAPI "nullable: true" property. | PowerSaving |
| EthFlowDescription | 3GPP TS 29.514 [52] | Defines a packet filter for an Ethernet flow.(NOTE 1) | EthAsSessionQoS\_5G, GMEC |
| EventsSubscReqData | 3GPP TS 29.514 [52] | Identifies the events the application subscribes to. | EnQoSMon |
| EventsSubscReqDataRm | 3GPP TS 29.514 [52] | This data type is defined in the same way as the "EventsSubscReqData" data type, but with the OpenAPI "nullable: true" property | EnQoSMon |
| ExtMaxDataBurstVol | 3GPP TS 29.571 [45] | Unsigned integer indicating Maximum Data Burst Volume (see clauses 5.7.3.7 and 5.7.4 of 3GPP TS 23.501 [8]), expressed in Bytes.  Minimum = 4096. Maximum = 2000000. |  |
| ExtMaxDataBurstVolRm | 3GPP TS 29.571 [45] | This data type is defined in the same way as the "ExtMaxDataBurstVol" data type, but with the OpenAPI "nullable: true" property. |  |
| Gpsi | 3GPP TS 29.571 [45] | Represents a GPSI. | GMEC |
| IpAddr | 3GPP TS 29.571 [45] | UE IP Address. | ListUE\_5G |
| MacAddr48 | 3GPP TS 29.571 [45] | MAC Address. | EthAsSessionQoS\_5G, enNB |
| MediaType | 3GPP TS 29.514 [52] | Indicates the media type of a single-modal data flow of a multi-modal service. | MultiMedia |
| MultiModalId | 3GPP TS 29.514 [52] | Represents multi-modal service identifier. | MultiMedia |
| MpxMediaInfo | 3GPP TS 29.514 [52] | Provides Multiplexed Media Information. | MpxMedia |
| NotifCapType | 3GPP TS 29.514 [52] | Indicates which QoS Monitoring capability report is applied. | QoSMonCapRepo |
| OnPathN6SigInfo | 3GPP TS 29.514 [52] | Represents the on-path N6 signaling information, with the OpenAPI "nullable: true" property. | OnPathN6MediaInfo |
| PacketDelBudget | 3GPP TS 29.571 [45] | Unsigned integer indicating Packet Delay Budget (see clauses 5.7.3.4 and 5.7.4 of 3GPP TS 23.501 [8])), expressed in milliseconds.  Minimum = 1. | TSC\_5G, RTLatency |
| PacketDelBudgetRm | 3GPP TS 29.571 [45] | This data type is defined in the same way as the "PacketDelBudget" data type, but with the OpenAPI "nullable: true" property. | TSC\_5G,  RTLatency |
| PacketErrRate | 3GPP TS 29.571 [45] | String representing Packet Error Rate (see clauses 5.7.3.5 and 5.7.4 of 3GPP TS 23.501 [8]), expressed as a "*scalar* x 10-k" where the scalar and the *exponent k are each encoded as one decimal digit*.  Pattern: '^([0-9]E-[0-9])$'  Examples:  Packer Error Rate 4x10-6 shall be encoded as "4E-6".  Packer Error Rate 10-2 shall be encoded as "1E-2". | ExtQoS\_5G |
| PacketErrRateRm | 3GPP TS 29.571 [45] | This data type is defined in the same way as the "PacketErrRate" data type, but with the OpenAPI "nullable: true" property. | ExtQoS\_5G |
| PdvMonitoringReport | 3GPP TS 29.514 [52] | Represents a PDV monitoring report. | EnQoSMon |
| PeriodicityInfo | 3GPP TS 29.514 [52] | Indicates the time period between the start of the two data bursts in Uplink and/or Downlink direction. | PowerSaving |
| PduSetQosPara | 3GPP TS 29.571 [45] | Represents the PDU Set level QoS parameters. | PDUSetHandling |
| PduSetQosParaRm | 3GPP TS 29.571 [45] | Represents the PDU Set level QoS parameters to be modified. | PDUSetHandling |
| PlmnIdNid | 3GPP TS 29.571 [45] | Identifies the network: the PLMN Identifier (the mobile country code and the mobile network code) or the SNPN Identifier (the PLMN Identifier and the NID). | enNB\_5G |
| ProtocolDescription | 3GPP TS 29.571 [45] | Represents Protocol description of the media flow | PDUSetHandling, PowerSaving  TrafficCharChange |
| ProtocolDescriptionRm | 3GPP TS 29.571 [45] | Represents the same as the "ProtocolDescription" data type, but with the OpenAPI "nullable: true" property. | PDUSetHandling, PowerSaving  TrafficCharChange |
| RateLimitRepo | 3GPP TS 29.514 [52] | Indicates the uplink/downlink data rate limitation information for the Non-GBR data flows. | RateLimitReport |
| RatType | 3GPP TS 29.571 [45] | Identifies the RAT Type. | enNB\_5G |
| ReportingFrequency | 3GPP TS 29.512 [8] | Indicates the frequency for the reporting, such as event triggered and/or periodic. (NOTE 2) |  |
| RequestedQosMonitoringParameter | 3GPP TS 29.512 [8] | Indicates the QoS information to be measured, e.g.UL packet delay, DL packet delay or round trip packet delay between the UE and the UPF is to be monitored when the QoS Monitoring for packet delay is enabled for the service data flow. (NOTE 2) |  |
| RttFlowReference | 3GPP TS 29.514 [52] | Identifies which Application Session Media Components contribute to the RT Latency requirement for two service data flows. | RTLatency |
| RttFlowReferenceRm | 3GPP TS 29.514 [52] | This data type is defined in the same way as the "RttFlowReference" data type, but with the OpenAPI "nullable: true" property. | RTLatency |
| ServAuthInfo | 3GPP TS 29.514 [52] | The authorization result of a request for QoS / QoS monitoring. | EnQoSMon |
| Snssai | 3GPP TS 29.571 [45] | Identifies the S-NSSAI. |  |
| SupportedFeatures | 3GPP TS 29.571 [45] | Used to negotiate the applicability of the optional features defined in table 5.14.4-1. |  |
| TemporalInValidity | 3GPP TS 29.565 [72] | Represents the temporal invalidity related information. | GMEC |
| TscaiInputContainer | 3GPP TS 29.514 [52] | TSCAI Input information container. | TSC\_5G, MultiMedia, GMEC |
| TscPriorityLevel | 3GPP TS 29.514 [52] | Represents priority of TSC Flows. | TSC\_5G |
| TscPriorityLevelRm | 3GPP TS 29.514 [52] | Represents the same as the TscPriorityLevel data type, but with the OpenAPI "nullable: true" property. | TSC\_5G |
| Uinteger | 3GPP TS 29.571 [45] | Unsigned Integer, i.e. only value 0 and integers above 0 are permissible.  Minimum = 0. |  |
| UintegerRm | 3GPP TS 29.571 [45] | This data type is defined in the same way as the "Uinteger" data type, but with the OpenAPI "nullable: true" property. |  |
| UplinkDownlinkSupport | 3GPP TS 29.514 [52] | Provides L4S support information. | L4S, GMEC |
| NOTE 1: In order to support a set of MAC addresses with a specific range in the traffic filter, feature MacAddressRange\_5G as specified in clause 5.14.4 shall be supported.  NOTE 2: In order to support QoS Monitoring, feature QoSMonitoring\_5G as specified in clause 5.14.4 shall be supported. | | |  |

Table 5.14.2.1.1-2 specifies the data types defined for the AsSessionWithQoS API.

Table 5.14.2.1.1-2: AsSessionWithQoS API specific Data Types

|  |  |  |  |
| --- | --- | --- | --- |
| Data type | Clause defined | Description | Applicability |
| AdditionInfoAsSessionWithQos | 5.14.2.1.11 | Describes additional error information specific for this API. |  |
| AsSessionWithQoSSubscription | 5.14.2.1.2 | Represents an individual AS session with required QoS subscription resource. |  |
| AsSessionWithQoSSubscriptionPatch | 5.14.2.1.3 | Represents parameters to modify an AS session with specific QoS subscription. |  |
| AsSessionMediaComponent | 5.14.2.1.13 | Represents media component data for a multi-modal service. It contains service data flow information for a single modal data flow of a multi-modal service. | MultiMedia |
| AsSessionMediaComponentRm | 5.14.2.1.14 | Represents the same as the AsSessionMediaComponent data type but with the "nullable: true" property. | MultiMedia |
|  |  |  |  |
| MultiModalFlows | 5.14.2.1.15 | Represents flow information within a single-modal data flow for a multi-modal service. | MultiMedia |
| ProblemDetailsAsSessionWithQos | 5.14.2.1.12 | ProblemDetails as defined in clause 5.2.12.12 extended with specific error information for this API, as described in AdditionInfoAsSessionWithQos. |  |
| QosMonitoringInformation | 5.14.2.1.6 | Represents QoS monitoring information. | QoSMonitoring\_5G, ListUE\_5G |
| QosMonitoringInformationRm | 5.14.2.1.7 | Represents the same as the QosMonitoringInformation data type but with the "nullable: true" property.  The "nullable: true" property is applicable only if the "EnQoSMon" feature is supported. | QoSMonitoring\_5G, ListUE\_5G |
| QosMonitoringReport | 5.14.2.1.8 | Represents a QoS monitoring report. | QoSMonitoring\_5G, ListUE\_5G |
|  |  |  |  |
| TscQosRequirement | 5.14.2.1.9 | Represents QoS requirements for time sensitive communication. | TSC\_5G, GMEC |
| TscQosRequirementRm | 5.14.2.1.10 | Represents the same as the TscQosRequirement data type but with the "nullable: true" property. | TSC\_5G, GMEC |
| UserPlaneEvent | 5.14.2.2.3 | Represents the user plane event. | enNB, GMEC |
| UserPlaneEventReport | 5.14.2.1.5 | Represents an event report for user plane. | enNB, GMEC |
| UserPlaneNotificationData | 5.14.2.1.4 | Represents the parameters to be conveyed in a user plane event(s) notification. | enNB, GMEC |
| UeAddInfo | 5.14.2.1.16 | Represents the UE address information. | ListUE\_5G |

\*\*\* Next Change \*\*\*

##### 5.14.2.1.5 Type: UserPlaneEventReport

This type represents an event report for user plane. It shall comply with the provisions defined in table 5.14.2.1.5-1.

Table 5.14.2.1.5-1: Definition of the UserPlaneEventReport data type

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Attribute name | Data type | Cardinality | Description | Applicability (NOTE 1) |
| event | UserPlaneEvent | 1 | Indicates the event reported by the SCEF. |  |
|  |  |  |  |  |
| accumulatedUsage | AccumulatedUsage | 0..1 | Contains the applicable information corresponding to the event. |  |
| flowIds | array(integer) | 0..N | Identifies the affected flows that were sent during event subscription. It may be omitted when the reported event applies to all the flows sent during the subscription.  (NOTE 2) |  |
| multiModFlows | array(MultiModalFlows) | 0..N | Each element of the array identifies the flow filters for the multi-modal data flows that were sent during event subscription and that are affected by the reported event. It may be omitted when the reported event applies to all the multi-modal data flows sent during the subscription.  (NOTE 2) | MultiMedia |
| appliedQosRef | string | 0..1 | The currently applied QoS reference (or applied individual QoS parameter set, if AltQosWithIndParams\_5G is supported). Applicable for event QOS\_NOT\_GUARANTEED or SUCCESSFUL\_RESOURCES\_ALLOCATION.  When it is omitted and the "event" attribute is QOS\_NOT\_GUARANTEED, the event report indicates that the lowest priority alternative QoS profile could not be fulfilled either.  When the "ExtQoS\_v2" feature is supported, the direction information namely QOS\_NOT\_GUARANTEED\_DL, QOS\_NOT\_GUARANTEED\_UL may be provided if the QoS targets of one or more SDFs are not being guaranteed. | AlternativeQoS\_5G, AltQosWithIndParams\_5G |
| altQosNotSuppInd | boolean | 0..1 | It may be set to true when the "event" attribute is QOS\_NOT\_GUARANTEED to indicate that alternative service requirements are not supported by the access network. The default value false shall apply if the attribute is not present. | AltQoSProfilesSupportReport, GMEC |
| plmnId | PlmnIdNid | 0..1 | Contains the PLMN Identifier or the SNPN Identifier.  This attribute may be present when the reported event is "PLMN\_CHG" and it is allowed to be exposed to the AF based on the local policy or local configuration. | enNB\_5G, GMEC |
| qosMonReports | array(QosMonitoringReport) | 0..N | Contains the QoS Monitoring Reporting information for packet delay. It shall be present when the notified event is "QOS\_MONITORING" and packet delay measurement error or packet delay measurements are available..  Only the "ulDelays", "dlDelays" and/or "rtDelays" attributes, or the "pdmf" attribute in QosMonitoringReport may be present. | QoSMonitoring\_5G, GMEC |
| pdvMonReports | array(PdvMonitoringReport) | 0..N | Contains the PDV Monitoring Reporting information. It shall be present when the notified event is "PACK\_DELAY\_VAR" and packet delay variations measurements are available.  (NOTE 3) | EnQoSMon, GMEC |
| ratType | RatType | 0..1 | Contains the RAT type.  This attribute may be present if applicable, the notified event is "ACCESS\_TYPE\_CHANGE" and it is allowed to be exposed to the AF based on the local policy or local configuration. | enNB\_5G, GMEC |
| batOffsetInfo | BatOffsetInfo | 0..1 | The BAT offset and the optionally adjusted periodicity. | EnTSCAC |
| aggrDataRateRpts | array(QosMonitoringReport) | 0..N | Contains QoS Monitoring for aggregated data rate reporting information. It shall be present when the notified event is "QOS\_MONITORING" and data rate measurements are available.  Only the "ulAggrDataRate" and/or "dlAggrDataRate" attributes in QosMonitoringReport may be present. | ListUE\_5G, GMEC |
| rttMonReports | array(QosMonitoringReport) | 0..N | Round-Trip delay for the indicated UL and DL QoS flows. It shall be present when the notified event is "RT\_DELAY\_TWO\_QOS\_FLOWS".  Only the "rtDelays" attributes in QosMonitoringReport may be present. | EnQoSMon, GMEC |
| qosMonDatRateReps | array(QosMonitoringReport) | 0..1 | Contains QoS Monitoring for data rate reporting information. It shall be present when the notified event is "QOS\_MONITORING" and data rate measurements are available.  Only the "ulDataRate" and/or "dlDataRate" attributes in QosMonitoringReport may be present. | EnQoSMon, GMEC |
| qosMonConInfoReps | array(QosMonitoringReport) | 0..N | Contains QoS Monitoring for congestion information (ECN marking percentage). It shall be present when the notified event is "QOS\_MONITORING" and congestion measurements are available.  Only the "ulConInfo" and/or "dlConInfo" attributes in QosMonitoringReport may be present. | EnQoSMon, GMEC |
| qosMonCapRepos | map(CapabilityReport) | 0..N | QoS Monitoring notification can be performed or not. The key of of the map is the attribute "capType".  It shall be present when the notified event is "QOS\_MON\_CAP\_REPO". | QoSMonCapRepo |
| rateLimitRepo | RatelimitRepo | 0..1 | Indicates the data rate limitation information for the Non-GBR service data flow(s).  It shall be present when the notified event is "RATE\_LIMIT\_INFO\_REPO". | RateLimitReport |
| NOTE 1: Properties marked with a feature as defined in clause 5.14.4 are applicable as described in clause 5.2.7. If no features are indicated, the related property applies for all the features.  NOTE 2: The attributes "flowIds" and "multiModFlows" are mutually exclusive.  NOTE 3: The PdvMonitoringReport data type does not include the "flows" attribute in this API. | | | | |

\*\*\* Next Change \*\*\*



\*\*\* Next Change \*\*\*



\*\*\* Next Change \*\*\*

### 5.14.4 Used Features

The table below defines the features applicable to the AsSessionWithQoS API. Those features are negotiated as described in subclause 5.2.7.

**Table 5.14.4-1: Features used by AsSessionWithQoS API**

|  |  |  |
| --- | --- | --- |
| **Feature Number** | **Feature** | **Description** |
| 1 | Notification\_websocket | The delivery of notifications over Websocket is supported according to clause 5.2.5.4. This feature requires that the Notification\_test\_event featute is also supported. |
| 2 | Notification\_test\_event | The testing of notifications connections is supported according to clause 5.2.5.3. |
| 3 | EthAsSessionQoS\_5G | Setting up required QoS for Ethernet UE. This feature may only be supported in 5G. |
| 4 | MacAddressRange\_5G | Indicates the support of a set of MAC addresses with a specific range in the traffic filter. This feature may only be supported in 5G. |
| 5 | AlternativeQoS\_5G | Indicates the support of alternative QoS requirements and the QoS notification (i.e. whether the QoS targets for SDF(s) are not guaranteed or guaranteed again). This feature may only be supported in 5G. |
| 6 | QoSMonitoring\_5G | Indicates the support of QoS Monitoring functionality and the report for packet delay monitoring. This feature may only be supported in 5G. |
| 7 | DisableUENotification\_5G | Indicates the support of disabling QoS flow parameters signalling to the UE when the SMF is notified by the NG-RAN of changes in the fulfilled QoS situation. This feature may only be supported in 5G. This feature requires that the AlternativeQoS\_5G feature is also supported. |
| 8 | TSC\_5G | Indicates the support of Time Sensitive Communication. This feature may only be supported in 5G. |
| 9 | AppId | Indicates the support of dynamically providing the Application Identifier via the API. |
| 10 | ExposureToEAS | This feature indicates the support of direct notification in 5GC. This feature requires that the QoSMonitoring\_5G feature is also supported. |
| 11 | enNB | Indicates the support of enhancements to the northbound interfaces. |
| 12 | AltQosWithIndParams\_5G | This feature indicates the support of provisioning Alternative Service Requirements with individual QoS parameters. This feature requires that the AlternativeQoS\_5G feature is also supported. |
| 13 | EnEthAsSessionQoS\_5G | Indicates the support of required QoS for Ethernet UE, allowing to indicate separately different UL and/or DL Ethernet flows. This feature may only be supported in 5G. |
| 14 | enNB\_5G | Indicates the support of enhancements to the northbound interfaces and only applicable to 5G. |
| 15 | PacketDelayFailureReport | Indicates the support of packet delay failure report as part of QoS Monitoring procedures. This feature requires that QoSMonitoring\_5G is supported. This feature may only be supported in 5G. |
| 16 | ToSTC\_5G | Indicates the support of Type of Service or Traffic Class. This feature may only be supported in 5G. |
| 17 | EnTSCAC | Indicates the support of extensions to TSCAC and the RAN feedback for BAT offset and adjusted periodicity.  This feature may only be supported in 5G, and requires that the TSC\_5G feature is also supported. |
| 18 | AltQoSProfilesSupportReport | This feature indicates the support of the report of whether Alternative QoS parameters are supported by the access network. This feature requires that AlternativeQoS\_5G and/or AltQosWithIndParams\_5G features are also supported. |
| 19 | ExtQoS\_5G | This feature indicates the support of extended QoS parameters. This feature may only be supported in 5G. |
| 20 | MultiMedia | Indicates the support for multi-modal or multimedia flows for single UE and multiple UE. This feature may only be supported in 5G. This feature may be used in eXtend Reality (XR) use cases. |
| 21 | ExtErrors | Indicates the support of additional application errors related to authorization or PDU Session availability. |
| 22 | QoSTiming\_5G | This feature indicates the support of QoS timing information for the transfer and support of data transmission (e.g., AI/ML transmission). This feature may only be supported in 5G. |
| 23 | ListUE\_5G | Indicates the support for the list of UEs This feature may only be supported in 5G. |
| 24 | GMEC | This feature indicates the support of Generic Group Management Exposure and Communication related enhancements.  The following functionalities are supported:  - Support AF requested QoS for a UE or group of UE(s) not identified by the UE address(es).  This feature may only be supported in 5G.  This feature requires the support of the "QoSMonitoring\_5G" and "AltQosWithIndParams\_5G" features. |
| 25 | PDUSetHandling | This feature indicates the support of PDU Set handling. This feature may be used for eXtended Reality (XR) and interactive media services.  This feature may only be supported in 5G. |
| 26 | RTLatency | This feature indicates the support of Round-Trip latency. This feature may be used for eXtended Reality (XR) and interactive media services.  This feature may only be supported in 5G. |
| 27 | EnQoSMon | This feature indicates the support of enhanced QoS monitoring functionality, i.e. the enhancement of packet delay QoS monitoring, and/or, the report of the congestion information, and/or, the RTT delay over two QoS flows, and/or, the data rate information, and/or, the Packet Delay Variation monitoring.  This feature requires that QoSMonitoring\_5G is supported.  In order to support the report of packet delay measurement failure, the PacketDelayFailureReport feature also requires to be supported.  This feature may only be supported in 5G. |
| 28 | PowerSaving | This feature indicates the support of the Power Saving for different traffic measurement**.**  This feature may only be supported in 5G. |
| 29 | L4S | This feature indicates the support of the AF indication of ECN marking for L4S support.  This feature may only be supported in 5G. |
| 30 | QoSMonCapRepo | This feature indicates the support QoS Monitoring Capability Report for packet delay and/or congestion.  This feature requires the support of the QoSMonitoring\_5G feature if packet delay is requested.  This feature requires that the EnQoSMon feature is supported if congestion is requested.  This feature requires that the EnQoSMon\_v2 feature is supported if available bitrate is requested.  This feature may only be supported in 5G. |
| 31 | TrafficCharChange | This feature indicates the support of dynamically changing traffic characteristics, including:  - the handling of Data Burst Size Marking Indication.  - the handling of Time to Next Burst Indication.  - the handling of Expedite Data Transfer with reflective QoS Indication for the Non-GBR flows.  This feature may only be supported in 5G. |
| 32 | MpxMedia | This feature indicates the support of uniquely identifying each media flow of multiplexed media with the provided Multiplexed Media Identification Information.  This feature may only be supported in 5G. |
| 33 | OnPathN6MediaInfo | This feature indicates the support of deliver media related information for encrypted traffic, including:  - Using on-path N6 signaling information to deliver media related information for encrypted traffic.  This feature may only be supported in 5G. |
| 34 | RateLimitReport | This feature indicates the support of AF request the 5GS to expose the data rate limitation information.  This feature may only be supported in 5G. |
| 35 | AcceptableQosDetails | This feature indicates the support of providing detailed information about the QoS that can be authorized in error responses of not authorized requests.  This feature may only be supported in 5G. |
| 36 | ExtQoS\_v2 | This feature indicates the enhancements on the support for the extensions to the QoS mechanisms, including:  - the support of PDU Set QoS parameters in Alternative QoS Profile when the PDUSetHandling feature is supported.  - the support of Averaging Window and Maximum Data Burst Volume parameters.  - the support of reporting the QoS targets for the indicated SDFs can no longer be guaranteed or can be guaranteed in the certain direction when the AlternativeQoS\_5G feature is supported.  This feature requires that AltQosWithIndParams\_5G feature is also supported.  This feature may only be supported in 5G. |
| 37 | EnQoSMon\_v2 | This feature indicates the enhancements on the QoS monitoring functionality, including:  - the reporting of available bitrate rate for a GBR QoS Flow.  This feature requires that the EnQoSMon feature is supported. |
| Feature: A short name that can be used to refer to the bit and to the feature, e.g. "Notification".  Description: A clear textual description of the feature. | | |

Editor's note: Available bitrate capability reporting dependency on the EnQoSMon\_v2 feature is FFS.

\*\*\* Next Change \*\*\*

# A.14 AsSessionWithQoS API

openapi: 3.0.0

info:

title: 3gpp-as-session-with-qos

version: 1.4.0-alpha.4

description: |

API for setting us an AS session with required QoS.

© 2025, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

All rights reserved.

externalDocs:

description: 3GPP TS 29.122 V19.3.0 T8 reference point for Northbound APIs

url: 'https://www.3gpp.org/ftp/Specs/archive/29\_series/29.122/'

security:

- {}

- oAuth2ClientCredentials: []

servers:

- url: '{apiRoot}/3gpp-as-session-with-qos/v1'

variables:

apiRoot:

default: https://example.com

description: apiRoot as defined in clause 5.2.4 of 3GPP TS 29.122.

paths:

/{scsAsId}/subscriptions:

get:

summary: Read all or queried active subscriptions for the SCS/AS.

operationId: FetchAllASSessionWithQoSSubscriptions

tags:

- AS Session with Required QoS Subscriptions

parameters:

- name: scsAsId

in: path

description: Identifier of the SCS/AS

required: true

schema:

type: string

- name: ip-addrs

in: query

description: The IP address(es) of the requested UE(s).

required: false

content:

application/json:

schema:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/IpAddr'

minItems: 1

- name: ip-domain

in: query

description: >

The IPv4 address domain identifier. The attribute may only be provided if IPv4 address

is included in the ip-addrs query parameter.

required: false

schema:

type: string

- name: mac-addrs

in: query

description: The MAC address(es) of the requested UE(s).

required: false

schema:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/MacAddr48'

minItems: 1

responses:

'200':

description: OK.

content:

application/json:

schema:

type: array

items:

$ref: '#/components/schemas/AsSessionWithQoSSubscription'

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'406':

$ref: 'TS29122\_CommonData.yaml#/components/responses/406'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

post:

summary: Creates a new subscription resource.

operationId: CreateASSessionWithQoSSubscription

tags:

- AS Session with Required QoS Subscriptions

parameters:

- name: scsAsId

in: path

description: Identifier of the SCS/AS

required: true

schema:

type: string

requestBody:

description: Request to create a new subscription resource

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/AsSessionWithQoSSubscription'

callbacks:

notificationDestination:

'{$request.body#/notificationDestination}':

post:

requestBody: # contents of the callback message

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/UserPlaneNotificationData'

responses:

'204':

description: No Content (successful notification)

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29122\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29122\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29122\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

responses:

'201':

description: Created (Successful creation of subscription)

content:

application/json:

schema:

$ref: '#/components/schemas/AsSessionWithQoSSubscription'

headers:

Location:

description: 'Contains the URI of the newly created resource'

required: true

schema:

type: string

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

description: Forbidden

content:

application/problem+json:

schema:

$ref: '#/components/schemas/ProblemDetailsAsSessionWithQos'

headers:

Retry-After:

description: >

Indicates the time the AF has to wait before making a new request. It can be a

non-negative integer (decimal number) indicating the number of seconds the AF

has to wait before making a new request or an HTTP-date after which the AF can

retry a new request.

schema:

type: string

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29122\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29122\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29122\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

/{scsAsId}/subscriptions/{subscriptionId}:

get:

summary: Read an active subscriptions for the SCS/AS and the subscription Id.

operationId: FetchIndASSessionWithQoSSubscription

tags:

- Individual AS Session with Required QoS Subscription

parameters:

- name: scsAsId

in: path

description: Identifier of the SCS/AS

required: true

schema:

type: string

- name: subscriptionId

in: path

description: Identifier of the subscription resource

required: true

schema:

type: string

responses:

'200':

description: OK (Successful get the active subscription)

content:

application/json:

schema:

$ref: '#/components/schemas/AsSessionWithQoSSubscription'

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'406':

$ref: 'TS29122\_CommonData.yaml#/components/responses/406'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

put:

summary: Updates/replaces an existing subscription resource.

operationId: UpdateIndASSessionWithQoSSubscription

tags:

- Individual AS Session with Required QoS Subscription

parameters:

- name: scsAsId

in: path

description: Identifier of the SCS/AS

required: true

schema:

type: string

- name: subscriptionId

in: path

description: Identifier of the subscription resource

required: true

schema:

type: string

requestBody:

description: Parameters to update/replace the existing subscription

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/AsSessionWithQoSSubscription'

responses:

'200':

description: OK (Successful update of the subscription)

content:

application/json:

schema:

$ref: '#/components/schemas/AsSessionWithQoSSubscription'

'204':

description: No Content (Successful update of the subscription)

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

description: Forbidden

content:

application/problem+json:

schema:

$ref: '#/components/schemas/ProblemDetailsAsSessionWithQos'

headers:

Retry-After:

description: >

Indicates the time the AF has to wait before making a new request. It can be a

non-negative integer (decimal number) indicating the number of seconds the AF

has to wait before making a new request or an HTTP-date after which the AF can

retry a new request.

schema:

type: string

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29122\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29122\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29122\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

patch:

summary: Updates/replaces an existing subscription resource.

operationId: ModifyIndASSessionWithQoSSubscription

tags:

- Individual AS Session with Required QoS Subscription

parameters:

- name: scsAsId

in: path

description: Identifier of the SCS/AS

required: true

schema:

type: string

- name: subscriptionId

in: path

description: Identifier of the subscription resource

required: true

schema:

type: string

requestBody:

required: true

content:

application/merge-patch+json:

schema:

$ref: '#/components/schemas/AsSessionWithQoSSubscriptionPatch'

responses:

'200':

description: OK. The subscription was modified successfully.

content:

application/json:

schema:

$ref: '#/components/schemas/AsSessionWithQoSSubscription'

'204':

description: No Content. The subscription was modified successfully.

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

description: Forbidden

content:

application/problem+json:

schema:

$ref: '#/components/schemas/ProblemDetailsAsSessionWithQos'

headers:

Retry-After:

description: >

Indicates the time the AF has to wait before making a new request. It can be a

non-negative integer (decimal number) indicating the number of seconds the AF

has to wait before making a new request or an HTTP-date after which the AF can

retry a new request.

schema:

type: string

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29122\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29122\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29122\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

delete:

summary: Deletes an already existing subscription.

operationId: DeleteIndASSessionWithQoSSubscription

tags:

- Individual AS Session with Required QoS Subscription

parameters:

- name: scsAsId

in: path

description: Identifier of the SCS/AS

required: true

schema:

type: string

- name: subscriptionId

in: path

description: Identifier of the subscription resource

required: true

schema:

type: string

responses:

'204':

description: No Content (Successful deletion of the existing subscription)

'200':

description: OK (Successful deletion of the existing subscription)

content:

application/json:

schema:

$ref: '#/components/schemas/UserPlaneNotificationData'

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

components:

securitySchemes:

oAuth2ClientCredentials:

type: oauth2

flows:

clientCredentials:

tokenUrl: '{tokenUrl}'

scopes: {}

schemas:

AsSessionWithQoSSubscription:

description: Represents an individual AS session with required QoS subscription resource.

type: object

properties:

self:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/Link'

supportedFeatures:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

dnn:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnn'

snssai:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

notificationDestination:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/Link'

exterAppId:

type: string

description: Identifies the external Application Identifier.

extGroupId:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/ExternalGroupId'

gpsi:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Gpsi'

flowInfo:

type: array

items:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/FlowInfo'

minItems: 1

description: Describe the data flow which requires QoS.

ethFlowInfo:

type: array

items:

$ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/EthFlowDescription'

minItems: 1

description: Identifies Ethernet packet flows.

enEthFlowInfo:

type: array

items:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/EthFlowInfo'

minItems: 1

description: >

Identifies the Ethernet flows which require QoS. Each Ethernet flow consists of a flow

idenifer and the corresponding UL and/or DL flows.

listUeAddrs:

type: array

items:

$ref: '#/components/schemas/UeAddInfo'

minItems: 1

description: Identifies the list of UE address.

multiModalId:

$ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/MultiModalId'

protoDescUl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/ProtocolDescription'

protoDescDl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/ProtocolDescription'

qosReference:

type: string

description: Identifies a pre-defined QoS information

altQoSReferences:

type: array

items:

type: string

minItems: 1

description: >

Identifies an ordered list of pre-defined QoS information. The lower the index of the

array for a given entry, the higher the priority.

altQosReqs:

type: array

items:

$ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/AlternativeServiceRequirementsData'

minItems: 1

description: >

Identifies an ordered list of alternative service requirements that include individual

QoS parameter sets. The lower the index of the array for a given entry, the higher the

priority.

disUeNotif:

description: >

Indicates whether the QoS flow parameters signalling to the UE when the SMF is notified

by the NG-RAN of changes in the fulfilled QoS situation is disabled (true) or

not (false). Default value is false. The fulfilled situation is either the QoS profile

or an Alternative QoS Profile.

type: boolean

ueIpv4Addr:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/Ipv4Addr'

ipDomain:

type: string

ueIpv6Addr:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/Ipv6Addr'

macAddr:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/MacAddr48'

usageThreshold:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/UsageThreshold'

sponsorInfo:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/SponsorInformation'

qosMonInfo:

$ref: '#/components/schemas/QosMonitoringInformation'

pdvMon:

$ref: '#/components/schemas/QosMonitoringInformation'

qosDuration:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/DurationSec'

qosInactInt:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/DurationSec'

directNotifInd:

type: boolean

description: >

Indicates whether the direct event notification is requested (true) or not (false) for

the provided and/or previously provided QoS monitoring parameter(s).

tscQosReq:

$ref: '#/components/schemas/TscQosRequirement'

l4sInd:

$ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/UplinkDownlinkSupport'

requestTestNotification:

type: boolean

description: >

Set to true by the SCS/AS to request the SCEF to send a test notification as defined

in clause 5.2.5.3. Set to false or omitted otherwise.

tempInValidity:

$ref: 'TS29565\_Ntsctsf\_QoSandTSCAssistance.yaml#/components/schemas/TemporalInValidity'

websockNotifConfig:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/WebsockNotifConfig'

events:

description: >

Represents the list of user plane event(s) to which the SCS/AS requests to subscribe to.

type: array

items:

$ref: '#/components/schemas/UserPlaneEvent'

minItems: 1

multiModDatFlows:

type: object

additionalProperties:

$ref: '#/components/schemas/AsSessionMediaComponent'

minProperties: 1

description: >

Contains media component data for a single-modal data flow(s).

The key of the map is the medCompN attribute.

pduSetQosDl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/PduSetQosPara'

pduSetQosUl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/PduSetQosPara'

rTLatencyInd:

type: boolean

description: >

Indicates the service data flow needs to meet the Round-Trip (RT) latency requirement of

the service, when it is included and set to "true".

The default value is "false" if omitted.

pdb:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/PacketDelBudget'

periodUl:

$ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/DurationMilliSec'

periodDl:

$ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/DurationMilliSec'

qosMonDatRate:

$ref: '#/components/schemas/QosMonitoringInformation'

avrgWndw:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/AverWindow'

servAuthInfo:

$ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/ServAuthInfo'

qosMonConReq:

$ref: '#/components/schemas/QosMonitoringInformation'

avlBitRateMon:

$ref: '#/components/schemas/QosMonitoringInformation'

qosMonCapRepoTypes:

type: array

items:

$ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/NotifCapType'

minItems: 1

description: >

Contains the type(s) of QoS Monitoring capability report is applied.

listUeConsDtRt:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/IpAddr'

minItems: 1

description: >

Identifies the list of UE addresses subject for Consolidated Data Rate monitoring.

datBurstSizeInd:

type: boolean

description: >

Indicates the Data Burst Size marking for the DL service data flow is supported, when

it is included and set to "true". The default value is "false" if omitted.

timetoNextBurstInd:

type: boolean

description: >

Indicates the Time to Next Burst for the DL service data flow is supported, when it is

included and set to "true". The default value is "false" if omitted.

onPathN6SigInfo:

$ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/OnPathN6SigInfo'

expTranInd:

type: boolean

description: >

Expedited Transfer Indication for the downlink traffic to enable expedited data transfer

with reflective QoS for the Non-GBR service data flow. "true": the expedited data

transfer of larger payload for XR application is enabled in the flow. "false": the

expedited data transfer of larger payload for XR application is not enabled in the flow.

The default value is "false" if omitted.

required:

- notificationDestination

AsSessionWithQoSSubscriptionPatch:

description: Represents parameters to modify an AS session with specific QoS subscription.

type: object

properties:

exterAppId:

type: string

description: Identifies the external Application Identifier.

flowInfo:

type: array

items:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/FlowInfo'

minItems: 1

description: Describe the IP data flow which requires QoS.

ethFlowInfo:

type: array

items:

$ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/EthFlowDescription'

minItems: 1

description: Identifies Ethernet packet flows.

enEthFlowInfo:

type: array

items:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/EthFlowInfo'

minItems: 1

description: >

Identifies the Ethernet flows which require QoS. Each Ethernet flow consists of a flow

idenifer and the corresponding UL and/or DL flows.

listUeAddrs:

type: array

items:

$ref: '#/components/schemas/UeAddInfo'

minItems: 1

description: Identifies the list of UE address.

qosReference:

type: string

description: Pre-defined QoS reference

altQoSReferences:

type: array

items:

type: string

minItems: 1

description: >

Identifies an ordered list of pre-defined QoS information. The lower the index of the

array for a given entry, the higher the priority.

altQosReqs:

type: array

items:

$ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/AlternativeServiceRequirementsData'

minItems: 1

description: >

Identifies an ordered list of alternative service requirements that include individual

QoS parameter sets. The lower the index of the array for a given entry, the higher the

priority.

disUeNotif:

type: boolean

description: >

Indicates whether the QoS flow parameters signalling to the UE when the SMF is notified

by the NG-RAN of changes in the fulfilled QoS situation is disabled (true) or

not (false). The fulfilled situation is either the QoS profile or an Alternative QoS

Profile.

usageThreshold:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/UsageThresholdRm'

qosMonInfo:

$ref: '#/components/schemas/QosMonitoringInformationRm'

pdvMon:

$ref: '#/components/schemas/QosMonitoringInformationRm'

directNotifInd:

type: boolean

description: >

Indicates whether the direct event notification is requested (true) or not (false) for

the provided QoS monitoring parameter(s).

notificationDestination:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/Link'

tscQosReq:

$ref: '#/components/schemas/TscQosRequirementRm'

l4sInd:

$ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/UplinkDownlinkSupport'

tempInValidity:

$ref: 'TS29565\_Ntsctsf\_QoSandTSCAssistance.yaml#/components/schemas/TemporalInValidity'

events:

description: >

Represents the updated list of user plane event(s) to which the SCS/AS requests to

subscribe to.

type: array

items:

$ref: '#/components/schemas/UserPlaneEvent'

minItems: 1

multiModDatFlows:

type: object

additionalProperties:

$ref: '#/components/schemas/AsSessionMediaComponentRm'

minProperties: 1

description: >

Contains media component data for a single-modal data flow(s).

The key of the map is the medCompN attribute.

pduSetQosDl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/PduSetQosParaRm'

pduSetQosUl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/PduSetQosParaRm'

rTLatencyInd:

type: boolean

nullable: true

description: >

Indicates the service data flow needs to meet the Round-Trip (RT) latency requirement of

the service, when it is included and set to "true".

pdb:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/PacketDelBudgetRm'

protoDescUl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/ProtocolDescriptionRm'

protoDescDl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/ProtocolDescriptionRm'

periodUl:

$ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/DurationMilliSecRm'

periodDl:

$ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/DurationMilliSecRm'

qosDuration:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/DurationSecRm'

qosInactInt:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/DurationSecRm'

qosMonDatRate:

$ref: '#/components/schemas/QosMonitoringInformationRm'

avrgWndw:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/AverWindowRm'

qosMonConReq:

$ref: '#/components/schemas/QosMonitoringInformationRm'

avlBitRateMon:

$ref: '#/components/schemas/QosMonitoringInformationRm'

qosMonCapRepoTypes:

type: array

items:

$ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/NotifCapType'

minItems: 1

description: >

Contains the type(s) of QoS Monitoring capability report is applied.

listUeConsDtRt:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/IpAddr'

minItems: 1

description: >

Identifies the list of UE addresses subject for Consolidated Data Rate monitoring.

datBurstSizeInd:

type: boolean

nullable: true

description: >

Indicates the Data Burst Size marking for the DL service data flow is supported, when

it is included and set to "true".

timetoNextBurstInd:

type: boolean

nullable: true

description: >

Indicates the Time to Next Burst for the DL service data flow is supported, when it is

included and set to "true". The default value is "false" if omitted.

onPathN6SigInfo:

$ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/OnPathN6SigInfo'

expTranInd:

type: boolean

nullable: true

description: >

Expedited Transfer Indication for the downlink traffic to enable expedited data transfer

with reflective QoS for the Non-GBR service data flow. "true": the expedited data

transfer of larger payload for XR application is enabled in the flow. "false":

the expedited data transfer of larger payload for XR application is not enabled in the

flow.

QosMonitoringInformation:

description: Represents QoS monitoring information.

type: object

properties:

reqQosMonParams:

type: array

items:

$ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/RequestedQosMonitoringParameter'

minItems: 1

repFreqs:

type: array

items:

$ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/ReportingFrequency'

minItems: 1

repThreshDl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

repThreshUl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

repThreshRp:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

conThreshDl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

conThreshUl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

waitTime:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/DurationSec'

repPeriod:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/DurationSec'

repThreshDatRateDl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

repThreshDatRateUl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

consDataRateThrDl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

consDataRateThrUl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

avlBitrateUlThrs:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

minItems: 1

description: Indicates a list of thresholds for uplink available bitrate reporting.

avlBitrateDlThrs:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

minItems: 1

description: Indicates a list of thresholds for downlink available bitrate reporting.

required:

- reqQosMonParams

- repFreqs

QosMonitoringInformationRm:

description: >

Represents the same as the QosMonitoringInformation data type but with

the nullable:true property.

type: object

properties:

reqQosMonParams:

type: array

items:

$ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/RequestedQosMonitoringParameter'

minItems: 1

repFreqs:

type: array

items:

$ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/ReportingFrequency'

minItems: 1

repThreshDl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/UintegerRm'

repThreshUl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/UintegerRm'

repThreshRp:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/UintegerRm'

conThreshDl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/UintegerRm'

conThreshUl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/UintegerRm'

waitTime:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/DurationSecRm'

repPeriod:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/DurationSecRm'

repThreshDatRateDl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRateRm'

repThreshDatRateUl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRateRm'

consDataRateThrDl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRateRm'

consDataRateThrUl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRateRm'

avlBitrateUlThrs:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRateRm'

minItems: 1

description: Indicates a list of thresholds for uplink available bitrate reporting.

avlBitrateDlThrs:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRateRm'

minItems: 1

description: Indicates a list of thresholds for downlink available bitrate reporting.

nullable: true

QosMonitoringReport:

description: Represents a QoS monitoring report.

type: object

properties:

ulDelays:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

minItems: 1

dlDelays:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

minItems: 1

rtDelays:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

minItems: 1

pdmf:

type: boolean

description: Represents the packet delay measurement failure indicator.

ulDataRate:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

dlDataRate:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

ulAggrDataRate:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

dlAggrDataRate:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

ulConInfo:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

dlConInfo:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

UserPlaneNotificationData:

description: Represents the parameters to be conveyed in a user plane event(s) notification.

type: object

properties:

transaction:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/Link'

eventReports:

type: array

items:

$ref: '#/components/schemas/UserPlaneEventReport'

minItems: 1

description: Contains the reported event and applicable information

required:

- transaction

- eventReports

UserPlaneEventReport:

description: Represents an event report for user plane.

type: object

properties:

event:

$ref: '#/components/schemas/UserPlaneEvent'

accumulatedUsage:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/AccumulatedUsage'

flowIds:

type: array

items:

type: integer

minItems: 1

description: >

Identifies the affected flows that were sent during event subscription. It might be

omitted when the reported event applies to all the flows sent during the subscription.

multiModFlows:

type: array

items:

$ref: '#/components/schemas/MultiModalFlows'

minItems: 1

description: >

Identifies the the flow filters for the single-modal data flows thatwere sent

during event subscription.

It may be omitted when the reported event applies to all the

single-modal data flows sent during the subscription.

appliedQosRef:

type: string

description: >

The currently applied QoS reference. Applicable for event QOS\_NOT\_GUARANTEED or

NOT\_GUARANTEED\_DL or NOT\_GUARANTEED\_UL or SUCCESSFUL\_RESOURCES\_ALLOCATION.

altQosNotSuppInd:

type: boolean

description: >

When present and set to true it indicates that the Alternative QoS profiles are not

supported by the access network. Applicable for event QOS\_NOT\_GUARANTEED.

plmnId:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/PlmnIdNid'

qosMonReports:

type: array

items:

$ref: '#/components/schemas/QosMonitoringReport'

minItems: 1

description: Contains the QoS Monitoring Reporting information

pdvMonReports:

type: array

items:

$ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/PdvMonitoringReport'

minItems: 1

description: Contains the PDV Monitoring Reporting information

ratType:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/RatType'

batOffsetInfo:

$ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/BatOffsetInfo'

rttMonReports:

type: array

items:

$ref: '#/components/schemas/QosMonitoringReport'

minItems: 1

description: Contains the round trip delay over two SDFs reporting information

qosMonDatRateReps:

type: array

items:

$ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/QosMonitoringReport'

minItems: 1

description: >

Contains QoS Monitoring for data rate information. It shall be present when the notified

event is "QOS\_MONITORING" and data rate measurements are available.

aggrDataRateRpts:

type: array

items:

$ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/QosMonitoringReport'

minItems: 1

description: >

Contains QoS Monitoring for aggregated data rate information. It shall be present when

the notified event is "QOS\_MONITORING" and data rate measurements are available.

qosMonConInfoReps:

type: array

items:

$ref: '#/components/schemas/QosMonitoringReport'

minItems: 1

description: >

Contains QoS Monitoring for congestion information. It shall be present when the

notified event is "QOS\_MONITORING" and congestion measurements are available.

qosMonCapRepos:

type: object

additionalProperties:

$ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/CapabilityReport'

minProperties: 1

description: >

QoS Monitoring notification can be performed or not. It shall be present when

the notified event is "QOS\_MON\_CAP\_REPO".The key of of the map is the attribute

"capType".

rateLimitRepo:

$ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/RateLimitRepo'

required:

- event

TscQosRequirement:

description: Represents QoS requirements for time sensitive communication.

type: object

properties:

reqGbrDl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

reqGbrUl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

reqMbrDl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

reqMbrUl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

maxTscBurstSize:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/ExtMaxDataBurstVol'

req5Gsdelay:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/PacketDelBudget'

reqPer:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/PacketErrRate'

priority:

$ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/TscPriorityLevel'

tscaiTimeDom:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

tscaiInputDl:

$ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/TscaiInputContainer'

tscaiInputUl:

$ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/TscaiInputContainer'

capBatAdaptation:

type: boolean

description: >

Indicates the capability for AF to adjust the burst sending time, when it is supported

and set to "true". The default value is "false" if omitted.

TscQosRequirementRm:

description: >

Represents the same as the TscQosRequirement data type but with the nullable:true property.

type: object

properties:

reqGbrDl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRateRm'

reqGbrUl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRateRm'

reqMbrDl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRateRm'

reqMbrUl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRateRm'

maxTscBurstSize:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/ExtMaxDataBurstVolRm'

req5Gsdelay:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/PacketDelBudgetRm'

reqPer:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/PacketErrRateRm'

priority:

$ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/TscPriorityLevelRm'

tscaiTimeDom:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/UintegerRm'

tscaiInputDl:

$ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/TscaiInputContainer'

tscaiInputUl:

$ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/TscaiInputContainer'

capBatAdaptation:

type: boolean

description: >

Indicates the capability for AF to adjust the burst sending time, when it is supported

and set to "true". The default value is "false" if omitted.

nullable: true

AdditionInfoAsSessionWithQos:

description: Describes additional error information specific for this API.

type: object

properties:

acceptableServInfo:

$ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/AcceptableServiceInfo'

ProblemDetailsAsSessionWithQos:

description: Extends ProblemDetails to also include the acceptable service info.

allOf:

- $ref: 'TS29122\_CommonData.yaml#/components/schemas/ProblemDetails'

- $ref: '#/components/schemas/AdditionInfoAsSessionWithQos'

AsSessionMediaComponent:

description: >

Representmedia component data for a single-modal data flow of a multi-modal service.

type: object

required:

- medCompN

allOf:

- not:

required: [altSerReqs,altSerReqsData]

- not:

required: [qosReference,altSerReqsData]

properties:

flowInfos:

type: array

items:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/FlowInfo'

minItems: 1

nullable: true

description: >

Contains the IP data flow(s) description for a single-modal data flow.

qosReference:

type: string

disUeNotif:

type: boolean

altSerReqs:

type: array

items:

type: string

minItems: 1

description: >

Contains alternative service requirements that include QoS references set

altSerReqsData:

type: array

items:

$ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/AlternativeServiceRequirementsData'

minItems: 1

description: >

Contains alternative service requirements that include individual QoS parameter sets.

marBwDl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

marBwUl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

medCompN:

type: integer

medType:

$ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/MediaType'

mirBwDl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

mirBwUl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

rTLatencyInd:

type: boolean

description: >

Indicates the service data flow needs to meet the Round-Trip (RT) latency requirement of

the service, when it is included and set to "true".

The default value is "false" if omitted.

pdb:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/PacketDelBudget'

rTLatencyIndCorreId:

$ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/RttFlowReference'

pduSetQosDl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/PduSetQosPara'

pduSetQosUl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/PduSetQosPara'

l4sInd:

$ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/UplinkDownlinkSupport'

protoDescDl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/ProtocolDescription'

protoDescUl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/ProtocolDescription'

periodUl:

$ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/DurationMilliSec'

periodDl:

$ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/DurationMilliSec'

evSubsc:

$ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/EventsSubscReqData'

datBurstSizeInd:

type: boolean

description: >

Indicates the Data Burst Size marking for the DL service data flow is supported, when

it is included and set to "true". The default value is "false" if omitted.

timetoNextBurstInd:

type: boolean

description: >

Indicates the Time to Next Burst for the DL service data flow is supported, when it is

included and set to "true". The default value is "false" if omitted.

onPathN6SigInfo:

$ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/OnPathN6SigInfo'

expTranInd:

type: boolean

description: >

Expedited Transfer Indication for the downlink traffic to enable expedited data transfer

with reflective QoS for the Non-GBR service data flow. "true": the expedited data

transfer of larger payload for XR application is enabled in the flow. "false": the

expedited data transfer of larger payload for XR application is not enabled in the flow.

The default value is "false" if omitted.

AsSessionMediaComponentRm:

description: >

Represents the AsSessionMediaComponent data type with nullable information.

type: object

required:

- medCompN

allOf:

- not:

required: [altSerReqs,altSerReqsData]

- not:

required: [qosReference,altSerReqsData]

properties:

flowInfos:

type: array

items:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/FlowInfo'

minItems: 1

nullable: true

description: >

Contains the IP data flow(s) description for a single-modal data flow.

qosReference:

type: string

nullable: true

altSerReqs:

type: array

items:

type: string

minItems: 1

description: >

Contains removable alternative service requirements that include set of QoS references

nullable: true

altSerReqsData:

type: array

items:

$ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/AlternativeServiceRequirementsData'

minItems: 1

description: >

Contains removable alternative service requirements that include individual QoS

parameter sets.

nullable: true

disUeNotif:

type: boolean

nullable: true

marBwDl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRateRm'

marBwUl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRateRm'

medCompN:

type: integer

medType:

$ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/MediaType'

mirBwDl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRateRm'

mirBwUl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRateRm'

rTLatencyInd:

type: boolean

nullable: true

description: >

Indicates the service data flow needs to meet the Round-Trip (RT) latency requirement of

the service, when it is included and set to "true".

The default value is "false" if omitted.

pdb:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/PacketDelBudgetRm'

rTLatencyIndCorreId:

$ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/RttFlowReferenceRm'

pduSetQosDl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/PduSetQosParaRm'

pduSetQosUl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/PduSetQosParaRm'

l4sInd:

$ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/UplinkDownlinkSupport'

protoDescDl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/ProtocolDescriptionRm'

protoDescUl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/ProtocolDescriptionRm'

periodUl:

$ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/DurationMilliSecRm'

periodDl:

$ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/DurationMilliSecRm'

evSubsc:

$ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/EventsSubscReqDataRm'

datBurstSizeInd:

type: boolean

nullable: true

description: >

Indicates the Data Burst Size marking for the DL service data flow is supported, when

it is included and set to "true".

timetoNextBurstInd:

type: boolean

nullable: true

description: >

Indicates the Time to Next Burst for the DL service data flow is supported, when it is

included and set to "true".

onPathN6SigInfo:

$ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/OnPathN6SigInfo'

expTranInd:

type: boolean

nullable: true

description: >

Expedited Transfer Indication for the downlink traffic to enable expedited data transfer

with reflective QoS for the Non-GBR service data flow. "true": the expedited data

transfer of larger payload for XR application is enabled in the flow. "false":

the expedited data transfer of larger payload for XR application is not enabled in the

flow.

nullable: true

MultiModalFlows:

description: Represents a flow information within a single-modal data flow.

type: object

properties:

medCompN:

type: integer

description: >

It contains the ordinal number of the single-modal data flow. Identifies the

single-modal data flow.

flowIds:

type: array

items:

type: integer

minItems: 1

description: >

Identifies the affected flow(s) within the single-modal data flow

(identified by the medCompN attribute).

It may be omitted when all flows are affected.

required:

- medCompN

UeAddInfo:

description: Represent the UE address information.

properties:

ueIpAddr:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/IpAddr'

portNumber:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/Port'

UserPlaneEvent:

anyOf:

- type: string

enum:

- SESSION\_TERMINATION

- LOSS\_OF\_BEARER

- RECOVERY\_OF\_BEARER

- RELEASE\_OF\_BEARER

- USAGE\_REPORT

- FAILED\_RESOURCES\_ALLOCATION

- QOS\_GUARANTEED

- QOS\_NOT\_GUARANTEED

- QOS\_MONITORING

- SUCCESSFUL\_RESOURCES\_ALLOCATION

- ACCESS\_TYPE\_CHANGE

- PLMN\_CHG

- L4S\_NOT\_AVAILABLE

- L4S\_AVAILABLE

- BAT\_OFFSET\_INFO

- RT\_DELAY\_TWO\_QOS\_FLOWS

- PACK\_DELAY\_VAR

- QOS\_MON\_CAP\_REPO

- RATE\_LIMIT\_INFO\_REPO

- type: string

description: >

This string provides forward-compatibility with future

extensions to the enumeration but is not used to encode

content defined in the present version of this API.

description: |

Represents the user plane event.

Possible values are:

- SESSION\_TERMINATION: Indicates that Rx session is terminated.

- LOSS\_OF\_BEARER : Indicates a loss of a bearer.

- RECOVERY\_OF\_BEARER: Indicates a recovery of a bearer.

- RELEASE\_OF\_BEARER: Indicates a release of a bearer.

- USAGE\_REPORT: Indicates the usage report event.

- FAILED\_RESOURCES\_ALLOCATION: Indicates the resource allocation is failed.

- QOS\_GUARANTEED: The QoS targets of one or more SDFs are guaranteed again.

- QOS\_NOT\_GUARANTEED: The QoS targets of one or more SDFs are not being guaranteed.

- QOS\_NOT\_GUARANTEED\_DL: The QoS targets of one or more SDFs are not being guaranteed in DL

direction.

- QOS\_NOT\_GUARANTEED\_UL: The QoS targets of one or more SDFs are not being guaranteed in UL

Direction.

- QOS\_MONITORING: Indicates a QoS monitoring event.

- SUCCESSFUL\_RESOURCES\_ALLOCATION: Indicates the resource allocation is successful.

- ACCESS\_TYPE\_CHANGE: Indicates an Access type change.

- PLMN\_CHG: Indicates a PLMN change.

- L4S\_NOT\_AVAILABLE: The ECN marking for L4S of one or more SDFs is not available.

- L4S\_AVAILABLE: The ECN marking for L4S of one or more SDFs is available again.

- BAT\_OFFSET\_INFO: Indicates the network provided BAT offset and the optionally adjusted

periodicity.

- RT\_DELAY\_TWO\_QOS\_FLOWS: Indicates round-trip delay on UL and DL flows over two QoS flows.

- PACK\_DELAY\_VAR: Indicates Packet Delay Variation is enabled for the SDF.

- QOS\_MON\_CAP\_REPO: Indicates whether the QoS Monitoring can be performed or not.

- RATE\_LIMIT\_INFO\_REPO: Indicates whether support of reporting rate limitation information.

\*\*\* End of Changes \*\*\*