**3GPP TSG- Meeting #**

**, , -**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.3* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  |  | **CR** |  | **rev** |  | **Current version:** |  |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **X** |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | Corrections related to the ML accuracy checking | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** |  | | | | | | | | | |
| ***Source to TSG:*** |  | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | eNetAE19 | | | | |  | ***Date:*** | | |  |
|  |  | | | |  | |  | | |  |
| ***Category:*** | **F** |  | | | | | ***Release:*** | | |  |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-17 (Release 17) Rel-18 (Release 18) Rel-19 (Release 19)  Rel-20 (Release 20)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | The description of the Nnwdaf\_MLModelTraining\_Subscribe service operation erroneously states that the NF service consumer may include the global ML model provided by the consumer as the "mLAccChkFlg" attribute. This attribite contains simply a flag to indicate accuracy checking.  Furthermore, the definition of the "mLAccChkFlg" attribute itself is wrongly written, lacking among others an explanation of what is meant with the "global ML model", which can actually by multiple models. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | Corrected the mistakes in the definition and usage of the "mLAccChkFlg" attribute. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | Wrong specification leading to different interpretations across different NWDAFs. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | 4.6.2.2.2, 5.5.6.2.2, 5.5.6.2.3, A.6 | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  | **X** | Other core specifications | | | | TS/TR ... CR ... | | |
| ***affected:*** | |  | **X** | Test specifications | | | | TS/TR ... CR ... | | |
| ***(show related CRs)*** | |  | **X** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | | This CR introduces backward compatible correction to the following APIs:  TS29520\_Nnwdaf\_MLModelTraining.yaml | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | |  | | | | | | | | |

\*\*\* First Change \*\*\*

4.6.2.2.2 Subscription for event notifications

Figure 4.6.2.2.2-1 shows a scenario where the NF service consumer sends a request to the NWDAF to subscribe for event notification(s) (as shown in 3GPP TS 23.288 [17]).

****

**Figure 4.6.2.2.2-1: NF service consumer subscribes to notifications**

The NF service consumer shall invoke the Nnwdaf\_MLModelTraining\_Subscribe service operation to subscribe to event notification(s). The NF service consumer shall send an HTTP POST request with "{apiRoot}/nnwdaf-mlmodeltraining/<apiVersion>/subscriptions" as Resource URI representing the "NWDAF ML Model Training Subscriptions", as shown in figure 4.6.2.2.2-1, step 1, to create a subscription for an "Individual NWDAF ML Model Training Subscription" according to the information in message body.

The NwdafMLModelTrainSubsc data structure provided in the request body shall include:

- an URI where to receive the requested notifications as the "notifUri" attribute;

- a description of the subscribed events as the "mLEventSubscs" attribute that, for each event, the MLEventSubscription data type shall include:

1) an event identifier as the "mLEvent" attribute;

2) event filter information as the "mLEventFilter" attribute; and

3) the ML Model Interoperability Information as the "modelInterInfo" attribute;

- a notification correlation identifier assigned by the NF service consumer for the requested notifications as "notifCorreId" attribute;

and may include:

- an identification of UE information for which data for ML model training is requested as the "tgtRepUe" attribute;

- the ML model information as the "mLModelInfos" attribute;

- the ML model training information as the "mLModelTrainInfos" attribute;

- identification of the ML procesure for training the ML model as the "mlCorreId" attribute;

- an indication of preparation request for ML model training as the "mLPreFlag" attribute;

- an indication of whether it is requested to use the local training data as the testing dataset to calculate the Model Accuracy of the global ML model provided by the consumer as the "mLAccChkFlg" attribute;

- the ML model training reporting information as the "mLTrainRepInfo" attribute;

- the round number of the training in a multi-round training process as the "roundInd" attribute;

- the reporting requirement information of the subscription as the "eventReq" attribute; and

- the indication of skipping the current FL round as the "skipFlInd" attribute.

Upon the reception of an HTTP POST request with: "{apiRoot}/nnwdaf-mlmodeltraining/<apiVersion>/subscriptions" as Resource URI and NwdafMLModelTrainSubsc data structure as request body, the NWDAF shall create a new subscription and store the subscription.

If the NWDAF created an "Individual NWDAF ML Model Training Subscription" resource, the NWDAF shall respond with "201 Created" with the message body containing a representation of the created subscription, as shown in figure 4.6.2.2.2-1, step 2. The NWDAF shall include a Location HTTP header field. The Location header field shall contain the URI of the created subscription i.e. "{apiRoot}/nnwdaf-mlmodeltraining/<apiVersion>/subscriptions/{subscriptionId}".

If the immediate reporting indication in the "immRep" attribute within the "eventReq" attribute sets to "true" during the event subscription, the NWDAF shall include the reports of the subscribed events, if available, as the "immReport" attribute in the HTTP POST response.

NOTE: Immediate and one-time reporting can be used in order to implement the Nnwdaf\_MLModelTrainingInfo service, which is defined in 3GPP TS 23.288 [17].

If not all the requested events in the subscription are accepted, then the NWDAF may include the "failEventReports" attribute indicating the event(s) for which the subscription failed and the associated reason(s).

If there is no associated ML model training available for all provided "mLEvent" attributes, the NWDAF shall send a "500 Internal Server Error" status code to the NF service consumer, including the "cause" attribute set to "UNAVAILABLE\_ML\_MODEL\_TRAINING\_FOR\_ALLEVENTS".

If there is no ML model training satisfying the requirements listed in "mLModelTrainInfos" attribute or the ML model cannot be downloaded successfully, the NWDAF which contains MTLF shall send a "403 Forbidden" status code to the NF service consumer, and it may include also the corresponding failure reason via a "problemDetails" attribute with the "cause" attribute set to "ML\_MODEL\_TRAINING\_REQS\_NOT\_MET", "ML\_TRAINING\_NOT\_COMPLETE", "OVERLOAD", or "NOT\_AVAILABLE\_FOR\_FL\_PROCESS\_ANYMORE".

If other errors occur when processing the HTTP POST request, the NWDAF shall send an HTTP error response as specified in clause 5.5.7.

\*\*\* Next Change \*\*\*

5.5.6.2.2 Type NwdafMLModelTrainSubsc

**Table 5.5.6.2.2-1: Definition of type NwdafMLModelTrainSubsc**

|  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Attribute name** | | **Data type** | | **P** | | **Cardinality** | | **Description** | | **Applicability** | |
| eventReq | | ReportingInformation | | O | | 0..1 | | Reporting requirement information of the subscription.  If omitted, the default values within the ReportingInformation data type apply. | |  | |
| failEventReports | | array(FailureEventInfoForMLModelTrain) | | O | | 1..N | | Supplied by the NWDAF containing MTLF when available, shall contain the event(s) that the subscription is not successful including the failure reason(s). | |  | |
| mlCorreId | | string | | C | | 0..1 | | Identifies the Machine Learning procedure for training the ML model.  It shall be present when the service is for Federated Learning. | |  | |
| mLEventSubscs | | array(MLEventSubscription) | | M | | 1..N | | Each element identifies the subscription for each event. The "modelInterInfo" attribute within the MLEventSubscription data type shall be provided. (NOTE 3) | |  | |
| mLModelInfos | | array(MLEventNotif) | | O | | 1..N | | Each element contains ML Model information for a specific analytics type. (NOTE 1) (NOTE 2) | |  | |
| immReport | | NwdafMLModelTrainNotif | | O | | 0..1 | | Immediately reported ML Model Training notifications. It may only be provided in the response of a subscription creation/update and only if the immediate reporting flag was set to "true" in the corresponding request. | |  | |
| mLModelTrainInfos | | array(MLModelTrainInfo) | | O | | 1..N | | Each element represents the ML Model training information for each event, include requirement on data availability and time availability. | |  | |
| mLPreFlag | | boolean | | C | | 0..1 | | Indicates whether the subscription is for preparation of ML Model training. Set to "true" if it is for ML training preparation, otherwise set to "false".  Default value is "false" if omitted.  It shall be present when the service is for preparation of Federated Learning. | |  | |
| mLAccChkFlg | | boolean | | O | | 0..1 | | Indicates whether it is requested to use the local training data as the testing dataset to calculate the Model Accuracy of the global ML model(s) provided by the NF service consumer in the "mLModelInfos" attribute. Possible values:  - "true": it is requested to use the local training data as the testing dataset to calculate the Model Accuracy.  - "false": it is not requested to use the local training data as the testing dataset to calculate the Model Accuracy.  Default value is "false" if omitted. | |  | |
| mLTrainRepInfo | | MLTrainReportInfo | | O | | 0..1 | | Indicates the training reporting information.  This attribute can be provided when the "notifMethod" attribute within the ReportingInformation structure is set to "ON\_EVENT\_DETECTION" in the "eventReq" attribute. | |  | |
| notifCorreId | | string | | M | | 1 | | The value of Notification Correlation ID in the corresponding notification. | |  | |
| notifUri | | Uri | | M | | 1 | | URI at which the NF service consumer requests to receive notifications. | |  | |
| roundInd | | Uinteger | | O | | 0..1 | | Indicates the round number of the training in a multi-round training process. | |  | |
| suppFeats | | SupportedFeatures | | C | | 0..1 | | List of Supported features used as described in clause 5.5.8.  It shall be supplied by NF service consumer in the POST requests that request the creation of an NWDAF ML Model Training Subscriptions resource and shall be supplied by the NWDAF in the reply of corresponding request. | |  | |
| tgtRepUe | | TargetUeInformation | | O | | 0..1 | | Indicates the UE(s) information for which data for ML model training is requested. | |  | |
| skipFlInd | | boolean | | O | | 0..1 | | Indicates whether to skip the current FL round or not.  Set to "true": Skipping the current FL round.  Set to "false": Not skipping the current FL round.  Default value is "false" if omitted. | |  | |
| NOTE 1: It is up to implementation to determine whether to include the "mlFile" arttribute in the "MLEventNotif" data structure considering ML Model file size, etc.  NOTE 2: Only the "event", "mlFile", "mLFileAddr", "mLModelAdrf", "modelUniqueId" and "useCaseCxt" attributes contained in MLEventNotif data type are applicable.  NOTE 3: The "useCaseCxt" attribute contained in MLEventSubscription data type is not applicable. | | | | | | | | | | | |

\*\*\* Next Change \*\*\*

5.5.6.2.3 Type NwdafMLModelTrainSubscPatch

**Table 5.5.6.2.3-1: Definition of type NwdafMLModelTrainSubscPatch**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Attribute name** | **Data type** | **P** | **Cardinality** | **Description** | **Applicability** |
| eventReq | ReportingInformation | O | 0..1 | Reporting requirement information of the subscription.  If omitted, the default values within the ReportingInformation data type apply. |  |
| mLModelInfos | array(MLEventNotif) | O | 1..N | Each element contains ML Model information for a specific analytics type. (NOTE 1) (NOTE 2) |  |
| mLModelTrainInfos | array(MLModelTrainInfo) | O | 1..N | Each element represents the ML Model training information, include requirement on data availability and time availability, training filter information. |  |
| mLPreFlag | boolean | O | 0..1 | Indicates whether the subscription is for preparation of ML Model training. Set to "true" if it is for ML training preparation, otherwise set to "false". |  |
| mLAccChkFlg | boolean | O | 0..1 | Indicates whether it is requested to use the local training data as the testing dataset to calculate the Model Accuracy of the global ML model provided by the NF service consumer in the "mLModelInfos" attribute.  Possible values:  - "true": it is requested to use the local training data as the testing dataset to calculate the Model Accuracy.  - "false": it is not requested to use the local training data as the testing dataset to calculate the Model Accuracy. |  |
| mLTrainRepInfo | MLTrainReportInfo | O | 0..1 | Indicates the training reporting information.  This attribute can be provided when the "notifMethod" attribute within the ReportingInformation structure is set to "ON\_EVENT\_DETECTION" in the "eventReq" attribute. |  |
| notifUri | Uri | O | 0..1 | URI at which the NF service consumer requests to receive notifications. |  |
| roundInd | Uinteger | O | 0..1 | Indicates the round number of the training in a multi-round training process. |  |
| tgtRepUe | TargetUeInformation | O | 0..1 | Indicates the UE(s) information for which data for ML model training is requested. |  |
| skipFlInd | boolean | O | 0..1 | Indicates whether to skip the current FL round or not.  Set to "true": Skipping the current FL round.  Set to "false": Not skipping the current FL round. |  |
| NOTE 1: It is up to implementation to determine whether to include the "mlFile" arttribute in the "MLEventNotif" data structure considering ML Model file size, etc.  NOTE 2: Only the "event", "mlFile", "mLFileAddr", "mLModelAdrf", "modelUniqueId" and "useCaseCxt" attributes contained in MLEventNotif data type are applicable. | | | | | |

\*\*\* Next Change \*\*\*

A.6 Nnwdaf\_MLModelTraining API

openapi: 3.0.0

info:

title: Nnwdaf\_MLModelTraining

version: 1.1.0-alpha.4

description: |

Nnwdaf\_MLModelTraining API Service.

© 2025, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

All rights reserved.

externalDocs:

description: 3GPP TS 29.520 V19.3.0; 5G System; Network Data Analytics Services.

url: https://www.3gpp.org/ftp/Specs/archive/29\_series/29.520/

servers:

- url: '{apiRoot}/nnwdaf-mlmodeltraining/v1'

variables:

apiRoot:

default: https://example.com

description: apiRoot as defined in clause 4.4 of 3GPP TS 29.501

security:

- {}

- oAuth2ClientCredentials:

- nnwdaf-mlmodeltraining

paths:

/subscriptions:

post:

summary: Create a new Individual NWDAF ML Model Training Subscription resource.

operationId: CreateNWDAFMLModelTrainingSubcription

tags:

- Subscriptions (Collection)

requestBody:

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/NwdafMLModelTrainSubsc'

responses:

'201':

description: Create a new Individual NWDAF ML Model Training Subscription resource.

content:

application/json:

schema:

$ref: '#/components/schemas/NwdafMLModelTrainSubsc'

headers:

Location:

description: >

Contains the URI of the newly created resource, according to the structure

{apiRoot}/nnwdaf-mlmodeltraining/v1/subscriptions/{subscriptionId}.

required: true

schema:

type: string

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29571\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29571\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29571\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'502':

$ref: 'TS29571\_CommonData.yaml#/components/responses/502'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

callbacks:

myNotification:

'{$request.body#/notifUri}':

post:

requestBody:

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/NwdafMLModelTrainNotif'

responses:

'204':

description: No Content, Notification was succesfull

'307':

$ref: 'TS29571\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29571\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29571\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29571\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29571\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'502':

$ref: 'TS29571\_CommonData.yaml#/components/responses/502'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

/subscriptions/{subscriptionId}:

put:

summary: update an existing Individual NWDAF ML Model Training Subscription

operationId: UpdateNWDAFMLModelTrainingSubcription

tags:

- Individual NWDAF ML Model Training Subscription (Document)

requestBody:

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/NwdafMLModelTrainSubsc'

parameters:

- name: subscriptionId

in: path

description: String identifying a subscription to the Nnwdaf\_MLModelTraining Service.

required: true

schema:

type: string

responses:

'200':

description: >

The Individual NWDAF ML Model Training Subscription resource was modified successfully

and a representation of that resource is returned.

content:

application/json:

schema:

$ref: '#/components/schemas/NwdafMLModelTrainSubsc'

'204':

description: >

The Individual NWDAF ML Model Training Subscription resource was modified successfully.

'307':

$ref: 'TS29571\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29571\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29571\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29571\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29571\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'502':

$ref: 'TS29571\_CommonData.yaml#/components/responses/502'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

patch:

summary: partial update an existing Individual NWDAF ML Model Training Subscription

operationId: PartialUpdateNWDAFMLModelTrainingSubcription

tags:

- Individual NWDAF ML Model Training Subscription (Document)

requestBody:

required: true

content:

application/merge-patch+json:

schema:

$ref: '#/components/schemas/NwdafMLModelTrainSubscPatch'

parameters:

- name: subscriptionId

in: path

description: String identifying a subscription to the Nnwdaf\_MLModelTraining Service.

required: true

schema:

type: string

responses:

'200':

description: >

The Individual NWDAF ML Model Training Subscription resource was partial modified

successfully and a representation of that resource is returned.

content:

application/json:

schema:

$ref: '#/components/schemas/NwdafMLModelTrainSubsc'

'204':

description: >

The Individual NWDAF ML Model Training Subscription resource was partial modified

successfully.

'307':

$ref: 'TS29571\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29571\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29571\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29571\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29571\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'502':

$ref: 'TS29571\_CommonData.yaml#/components/responses/502'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

delete:

summary: Delete an existing Individual NWDAF ML Model Training Subscription.

operationId: DeleteNWDAFMLModelTrainingSubcription

tags:

- Individual NWDAF ML Model Training Subscription (Document)

parameters:

- name: subscriptionId

in: path

description: String identifying a subscription to the Nnwdaf\_MLModelTraining Service.

required: true

schema:

type: string

responses:

'204':

description: >

No Content. The Individual NWDAF ML Model Training Subscription matching the

subscriptionId was deleted.

'307':

$ref: 'TS29571\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29571\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'502':

$ref: 'TS29571\_CommonData.yaml#/components/responses/502'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

components:

securitySchemes:

oAuth2ClientCredentials:

type: oauth2

flows:

clientCredentials:

tokenUrl: '{nrfApiRoot}/oauth2/token'

scopes:

nnwdaf-mlmodeltraining: Access to the Nnwdaf\_MLModelTraining API

schemas:

NwdafMLModelTrainSubsc:

description: Represents a ML Model Training subscription.

type: object

properties:

mLEventSubscs:

type: array

items:

$ref: 'TS29520\_Nnwdaf\_MLModelProvision.yaml#/components/schemas/MLEventSubscription'

minItems: 1

description: Subscribed events

notifUri:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

suppFeats:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

eventReq:

$ref: 'TS29523\_Npcf\_EventExposure.yaml#/components/schemas/ReportingInformation'

failEventReports:

type: array

items:

$ref: '#/components/schemas/FailureEventInfoForMLModelTrain'

minItems: 1

description: >

Supplied by the NWDAF containing MTLF when available, shall contain the event(s) that

the subscription is not successful including the failure reason(s).

mlCorreId:

type: string

description: String identifying the subscription is for a Federated Learning procedure.

mLModelInfos:

type: array

items:

$ref: 'TS29520\_Nnwdaf\_MLModelProvision.yaml#/components/schemas/MLEventNotif'

minItems: 1

description: Represents the ML Model information.

immReport:

$ref: '#/components/schemas/NwdafMLModelTrainNotif'

mLModelTrainInfos:

type: array

items:

$ref: '#/components/schemas/MLModelTrainInfo'

minItems: 1

description: Represents the ML Model training information.

mLPreFlag:

type: boolean

description: >

Indicates whether the subscription is for preparation of ML Model training. Set to

"true" if it is for ML training preparation, otherwise set to "false".

mLAccChkFlg:

type: boolean

description: >

Indicates whether it is requested to use the local training data as the testing dataset

to calculate the Model Accuracy of the global ML model provided by the consumer. Set to

"true" if this is requested, otherwise set to "false" or omitted.

mLTrainRepInfo:

$ref: '#/components/schemas/MLTrainReportInfo'

notifCorreId:

type: string

description: >

String identifying the Notification Correlation ID in the corresponding notification.

roundInd:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

tgtRepUe:

$ref: 'TS29520\_Nnwdaf\_EventsSubscription.yaml#/components/schemas/TargetUeInformation'

skipFlInd:

type: boolean

description: Indicates whether to skip the current FL round or not.

required:

- mLEventSubscs

- notifUri

- notifCorreId

NwdafMLModelTrainSubscPatch:

description: >

Represents parameters to request the modification of a ML Model Training subscription.

type: object

properties:

notifUri:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

eventReq:

$ref: 'TS29523\_Npcf\_EventExposure.yaml#/components/schemas/ReportingInformation'

mLModelInfos:

type: array

items:

$ref: 'TS29520\_Nnwdaf\_MLModelProvision.yaml#/components/schemas/MLEventNotif'

minItems: 1

description: Represents the ML Model information.

mLModelTrainInfos:

type: array

items:

$ref: '#/components/schemas/MLModelTrainInfo'

minItems: 1

description: Represents the ML Model training information.

mLPreFlag:

type: boolean

description: >

Indicates whether the subscription is for preparation of ML Model training. Set to

"true" if it is for ML training preparation, otherwise set to "false".

mLAccChkFlg:

type: boolean

description: >

Indicates whether it is requested to use the local training data as the testing dataset

to calculate the Model Accuracy of the global ML model(s) provided by the consumer.

mLTrainRepInfo:

$ref: '#/components/schemas/MLTrainReportInfo'

roundInd:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

tgtRepUe:

$ref: 'TS29520\_Nnwdaf\_EventsSubscription.yaml#/components/schemas/TargetUeInformation'

skipFlInd:

type: boolean

description: Indicates whether to skip the current FL round or not.

NwdafMLModelTrainNotif:

description: Represents notifications on events that occurred.

type: object

properties:

delayEventNotif:

$ref: '#/components/schemas/DelayEventNotif'

mlCorreId:

type: string

description: String identifying the subscription is for a Federated Learning procedure.

mLModelInfos:

type: array

items:

$ref: 'TS29520\_Nnwdaf\_MLModelProvision.yaml#/components/schemas/MLEventNotif'

minItems: 1

description: Represents the ML Model information.

notifCorreId:

type: string

description: >

String identifying the Notification Correlation ID in the corresponding notification.

roundInd:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

statusReport:

$ref: '#/components/schemas/StatusReportInfo'

termTrainReq:

$ref: '#/components/schemas/TermTrainCause'

required:

- notifCorreId

oneOf:

- required: [delayEventNotif]

- required: [mLModelInfos]

- required: [termTrainReq]

- required: [mLModelInfos, termTrainReq]

MLModelTrainInfo:

description: >

Represents the ML Model training information, include requirement on data availability and

time availability, training filter information.

type: object

properties:

dataAvReq:

$ref: '#/components/schemas/DataAvReq'

timeAvReq:

type: string

description: >

String representing the requirement on available time for the ML model training.

MLTrainReportInfo:

description: Represents the ML Model training reporting information.

type: object

properties:

maxResTime:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DurationSec'

FailureEventInfoForMLModelTrain:

description: Represents the failure event information for a ML Model Training subscription.

type: object

properties:

mLTrainEvent:

$ref: 'TS29520\_Nnwdaf\_EventsSubscription.yaml#/components/schemas/NwdafEvent'

failureCodeTrain:

$ref: '#/components/schemas/FailureCodeTrain'

required:

- mLTrainEvent

- failureCodeTrain

DataAvReq:

description: Represents the requirement on available data for the ML model training.

type: object

properties:

dataStatProps:

type: array

items:

$ref: 'TS29520\_Nnwdaf\_EventsSubscription.yaml#/components/schemas/DatasetStatisticalProperty'

minItems: 1

inpEvents:

type: array

items:

$ref: 'TS29574\_Ndccf\_DataManagement.yaml#/components/schemas/DccfEvent'

minItems: 1

minNumSamples:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

timeWindows:

type: array

items:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/TimeWindow'

minItems: 1

required:

- inpEvents

DelayEventNotif:

description: >

Indicating that the NWDAF containing MTLF is not able to complete the training of ML model

within the maximum response time, the cause code, and the expected time complete the

training.

type: object

properties:

delayEventInd:

type: boolean

description: >

Indicates that the NWDAF containing MTLF is not able to complete the training of ML

model within the maximum response time. Set to "true" if not able to complete the ML

model training on time, otherwise set to "false".

delayCause:

$ref: '#/components/schemas/DelayCause'

expCompTime:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DurationSec'

required:

- delayEventInd

StatusReportInfo:

description: >

Indicating status information generated by the NWDAF containing MTLF during ML model

training.

type: object

properties:

mlModelAcc:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

trainInDataInfo:

$ref: '#/components/schemas/TrainDataInfo'

TrainDataInfo:

description: Represents the training input data information.

type: object

properties:

areaInfo:

$ref: 'TS29554\_Npcf\_BDTPolicyControl.yaml#/components/schemas/NetworkAreaInfo'

maxValues:

type: array

items:

type: string

minItems: 1

description: >

Represents the maximum value of one dimension of data. The format of its value is out of

3GPP scope.

minValues:

type: array

items:

type: string

minItems: 1

description: >

Represents the minimum value of one dimension of data. The format of its value is out of

3GPP scope.

samplRatio:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

#

# ENUMERATIONS DATA TYPES

#

FailureCodeTrain:

anyOf:

- type: string

enum:

- UNAVAILABLE\_ML\_MODEL\_TRAIN

- type: string

description: >

This string provides forward-compatibility with future extensions to the enumeration but

is not used to encode content defined in the present version of this API.

description: |

Represents the failure reason.

Possible values are:

- UNAVAILABLE\_ML\_MODEL\_TRAIN: The ML model training is unavailable.

TermTrainCause:

anyOf:

- type: string

enum:

- NWDAF\_OVERLOAD

- NOT\_AVAILABLE\_ML\_TRAIN

- OTHERS

- type: string

description: >

This string provides forward-compatibility with future extensions to the enumeration but

is not used to encode content defined in the present version of this API.

description: |

Represents the reasons that ML Model Training to be terminated.

Possible values are:

- NWDAF\_OVERLOAD: The NWDAF is overloaded for the ML model training.

- NOT\_AVAILABLE\_ML\_TRAIN: The ML model training process is not available.

- OTHERS: Other cause.

DelayCause:

anyOf:

- type: string

enum:

- ML\_MODEL\_TRAIN\_FAILURE

- NEED\_MORE\_TIME

- OTHERS

- type: string

description: >

This string provides forward-compatibility with future extensions to the enumeration but

is not used to encode content defined in the present version of this API.

description: |

Represents the reasons for ML Model training delay.

Possible values are:

- ML\_MODEL\_TRAIN\_FAILURE: The ML model training is failure.

- NEED\_MORE\_TIME: The ML model training needs more time.

- OTHERS: Other cause.

\*\*\* End of Changes \*\*\*