**3GPP TSG-RAN4 Meeting #116 R4-2509718**

**Bengaluru, India, Aug.25th – 29th, 2025**

Source: CMCC

Title: TP for TR 38.194 6.5 Unwanted emissions and 6.5 Transmitter intermodulation

Agenda Item: 7.22.3.1

Document for: Approval

# **Introduction**

This TP will focus on 6.5 Unwanted emissions and 6.5 Transmitter intermodulation.

Following list approved agreements in previous meetings.

* #114 R4-2502859
  + Issue 1-5-3: OBUE. Agreement: Postpone OBUE requirements discussion after RAN4 make conclusion on ACLR.
* #114bis R4-2505097
  + Issue 1-5-4: Transmitter spurious emissions
    - Reuse the FR1 NR BS transmitter spurious emission requirement for A-IoT BS
    - Reuse the co-existence and co-location requirements of NR Micro BS
* #115 R4-2508101
  + Issue 1-5-1: Occupied bandwidth. The occupied bandwidth for each A-IoT carrier shall be less than the A-IoT BS channel bandwidth.
  + Issue 1-6: Transmitter intermodulation. No need

# **Reference**

[1]

# Text Proposal

**----- Start of TP -----**

## 6.5 Unwanted emissions

### 6.5.1 General

Unwanted emissions consist of out-of-band emissions and spurious emissions according to ITU definitions [2]. In ITU terminology, out of band emissions are unwanted emissions immediately outside the *BS channel bandwidth* resulting from the modulation process and non-linearity in the transmitter but excluding spurious emissions. Spurious emissions are emissions which are caused by unwanted transmitter effects such as harmonics emission, parasitic emission, intermodulation products and frequency conversion products, but exclude out of band emissions.

The out-of-band emissions requirement for the BS transmitter is specified both in terms of Adjacent Channel Leakage power Ratio (ACLR) and *operating band* unwanted emissions (OBUE).

The maximum offset of the *operating band* unwanted emissions mask from the *operating band* edge is ΔfOBUE. The Operating band unwanted emissions define all unwanted emissions in each supported downlink *operating band* plus the frequency ranges ΔfOBUE above and ΔfOBUE below each band. Unwanted emissions outside of this frequency range are limited by a spurious emissions requirement.

The values of ΔfOBUE are defined in table 6.5.1-1 for the NR *operating bands*.

Table 6.5.1-1: Maximum offset of OBUE outside the downlink *operating band*

|  |  |  |
| --- | --- | --- |
| BS type | *Operating band* characteristics | ΔfOBUE (MHz) |
| *BS type 1-C* | FDL,high – FDL,low ≤ 200 MHz | 10 |
|  | 200 MHz < FDL,high – FDL,low ≤ 900 MHz | 40 |
|  |  |  |

There is in addition a requirement for occupied bandwidth.

### 6.5.2 Occupied bandwidth

#### 6.5.2.1 General

The occupied bandwidth requirement shall apply during *transmitter ON period* for a single transmitted carrier. The minimum requirement below may be applied regionally. There may also be regional requirements to declare the occupied bandwidth.

For *BS type 1-C* this requirement shall be applied at the *antenna connector* supporting transmission in the *operating band*.

#### 6.5.2.2 Minimum requirement for *BS type 1-C*

The occupied bandwidth for each NR carrier shall be less than the *BS channel bandwidth*.

### 6.5.3 Adjacent Channel Leakage Power Ratio

#### 6.5.3.1 General

Adjacent Channel Leakage power Ratio (ACLR) is the ratio of the filtered mean power centred on the assigned channel frequency to the filtered mean power centred on an adjacent channel frequency.

The requirements shall apply outside the *Base Station RF Bandwidth* or *Radio Bandwidth* whatever the type of transmitter considered (single carrier or multi-carrier) and for all transmission modes foreseen by the manufacturer’s specification.

The requirement shall apply during the *transmitter ON period*.

#### 6.5.3.2 Limits and *Basic limits*

The ACLR is defined with a square filter of bandwidth equal to the transmission bandwidth configuration of the transmitted signal (BWConfig) centred on the assigned channel frequency and a filter centred on the adjacent channel frequency according to the tables below.

For operation in paired spectrum, the ACLR shall be higher than the value specified in table 6.5.3.2‑1 in band n8.

Table 6.5.3.2-1: Base station ACLR limit

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| *BS channel bandwidth* of *lowest/highest carrier* transmitted BWChannel (kHz) | BS adjacent channel centre frequency offset below the lowest or above the highest carrier centre frequency transmitted  (kHz) | Assumed adjacent channel carrier (informative) | Filter on the adjacent channel frequency and corresponding filter bandwidth | ACLR limit |
| 200 | 300 | NR of same BW | Square (180 kHz) | 40dB |
| 500 | NR of same BW | Square (180 kHz) | 45dB |
| 400 | 500 | NR of same BW | Square (360 kHz) | 40dB |
| 900 | NR of same BW | Square (360 kHz) | 45dB |
| 600 | 700 | NR of same BW | Square (540 kHz) | 40dB |
| 1300 | NR of same BW | Square (540 kHz) | 45dB |
| 800 | 900 | NR of same BW | Square (720 kHz) | 40dB |
| 1700 | NR of same BW | Square (720 kHz) | 45dB |

#### 6.5.3.3 Minimum requirement for *BS type 1-C*

The ACLR *limits* in table 6.5.3.2-1 shall apply for each *antenna connector*.

### 6.5.4 Operating band unwanted emissions

#### 6.5.4.1 General

Unless otherwise stated, the operating band unwanted emission (OBUE) limits in FR1 are defined from ΔfOBUE below the lowest frequency of each supported downlink *operating band* up to ΔfOBUE above the highest frequency of each supported downlink *operating band*. The values of ΔfOBUE are defined in table 6.5.1‑1 for the NR *operating bands*.

The requirements shall apply whatever the type of transmitter considered and for all transmission modes foreseen by the manufacturer’s specification.

*Basic limits* are specified in the tables below, where:

- Δf is the separation between the *channel edge* frequency and the nominal -3dB point of the measuring filter closest to the carrier frequency.

- f\_offset is the separation between the *channel edge* frequency and the centre of the measuring filter.

- f\_offsetmax is the offset to the frequency ΔfOBUE outside the downlink *operating band*, where ΔfOBUE is defined in table 6.5.1-1.

- Δfmax is equal to f\_offsetmax minus half of the bandwidth of the measuring filter.

For Medium Range BS, the requirements in clause 6.5.4.2.3 shall apply.

#### 6.5.4.2 *Basic limits*

##### 6.5.4.2.3 *Basic limits* for Medium Range BS

For A-IoT medium range BS (maximum output power 31 < Prated,c ≤ 38 dBm), emissions shall not exceed the maximum levels specified in Table 6.5.4.2.3-1.

Table 6.5.4.2.3-1: A-IoT medium range BS operating band unwanted emission limits, BS maximum output power 31 < Prated,c ≤ 38 dBm

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| BS R2D channel bandwidth | Frequency offset of measurement filter ‑3dB point, Δf | Frequency offset of measurement filter centre frequency, f\_offset | Minimum requirement | Measurement bandwidth |
| 200kHz | 0 MHz ≤ Δf < 0.05 MHz | 0.015 MHz ≤ f\_offset < 0.065 MHz |  | 30 kHz |
| 0.05 MHz ≤ Δf < 0.15 MHz | 0.065 MHz ≤ f\_offset < 0.165 MHz |  | 30 kHz |
| 0.15 MHz ≤ Δf < 0.6 MHz | 0.165MHz ≤ f\_offset < 0.615MHz |  | 30 kHz |
| 0.6 MHz ≤ Δf < 1 MHz | 0.615MHz ≤ f\_offset < 1.015MHz |  | 30 kHz |
| 1 MHz ≤ Δf ≤ 2.8 MHz | 1.5 MHz ≤ f\_offset < 3.3 MHz | Prated,c - 52 dB | 1 MHz |
| 2.8 MHz ≤ Δf ≤ 5 MHz | 3.3 MHz ≤ f\_offset < 5.5 MHz | min(Prated,c - 52 dB, -15dBm) | 1 MHz |
| 5 MHz ≤ Δf ≤ Δfmax | 5.5 MHz ≤ f\_offset < f\_offsetmax | Prated,c - 56 dB | 1 MHz |
| 400kHz | 0 MHz ≤ Δf < 0.4 MHz | 0.015 MHz ≤ f\_offset < 0.415 MHz | Prated,c -40dB - (- 0.015) dB | 30 kHz |
| 0.4 MHz ≤ Δf < 0.8 MHz | 0.415 MHz ≤ f\_offset < 0.815 MHz | Prated,c - 51dB- (-0.415) dB | 30 kHz |
| 0.8 MHz ≤ Δf < 1.6 MHz | 0.815 MHz ≤ f\_offset < 1.6 MHz | Prated,c - 56dB | 30 kHz |
| 1.6 MHz ≤ Δf < Δfmax | 1.6 MHz ≤ f\_offset < f\_offsetmax | -25dBm | 100kHz |
| 600kHz | 0 MHz ≤ Δf < 0.6 MHz | 0.015 MHz ≤ f\_offset < 0.615 MHz | Prated,c – 40dB - (-0.015) dB | 30 kHz |
| 0.6 MHz ≤ Δf < 1.2 MHz | 0.615 MHz ≤ f\_offset < 1.2 MHz | Prated,c – 53dB - (-0.615) dB | 30 kHz |
| 1.2 MHz ≤ Δf < 1.8 MHz | 1.2 MHz ≤ f\_offset < 1.8 MHz | Prated,c - 58dB | 30 kHz |
| 1.8 MHz ≤ Δf < Δfmax | 1.8 MHz ≤ f\_offset < f\_offsetmax | -25dBm | 100K |
| 800kHz | 0 MHz ≤ Δf < 0.8 MHz | 0.015 MHz ≤ f\_offset < 0.815 MHz | Prated,c – 40dB- (-0.015) dB | 30 kHz |
| 0.8 MHz ≤ Δf < 1.6 MHz | 0.815 MHz ≤ f\_offset < 1.6 MHz | Prated,c – 54dB- (-0.815) dB | 30 kHz |
| 1.6 MHz ≤ Δf < 2.4 MHz | 1.6 MHz ≤ f\_offset < 2.4 MHz | Prated,c - 59dB | 30 kHz |
| 2.4 MHz ≤ Δf < Δfmax | 2.4 MHz ≤ f\_offset < f\_offsetmax | -25dBm | 100K |

For A-IoT (maximum output power Prated,c ≤ 31 dBm), emissions shall not exceed the maximum levels specified in Tables 6.5.4.2.3-2.

Table 6.5.4.2.3-2: A-IoT medium range BS operating band unwanted emission limits, BS maximum output power Prated,c ≤ 31 dBm

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| BS R2D channel bandwidth | Frequency offset of measurement filter ‑3dB point, Δf | Frequency offset of measurement filter centre frequency, f\_offset | Minimum requirement | Measurement bandwidth |
| 200kHz | 0 MHz ≤ Δf < 0.05 MHz | 0.015 MHz ≤ f\_offset < 0.065 MHz |  | 30 kHz |
| 0.05 MHz ≤ Δf < 0.15 MHz | 0.065 MHz ≤ f\_offset < 0.165 MHz |  | 30 kHz |
| 0.15 MHz ≤ Δf < 0.6 MHz | 0.165MHz ≤ f\_offset < 0.615MHz |  | 30 kHz |
| 0.6 MHz ≤ Δf < 1 MHz | 0.615MHz ≤ f\_offset < 1.015MHz |  | 30 kHz |
| 1 MHz ≤ Δf ≤ 5 MHz | 1.5 MHz ≤ f\_offset < 5.5 MHz | -21 dBm | 1 MHz |
| 5 MHz ≤ Δf ≤ Δfmax | 5.5 MHz ≤ f\_offset < f\_offsetmax | -25 dBm | 1 MHz |
| 400kHz | 0 MHz ≤ Δf < 0.4 MHz | 0.015 MHz ≤ f\_offset < 0.415 MHz | -9dBm - (- 0.015) dB | 30 kHz |
| 0.4 MHz ≤ Δf < 0.8 MHz | 0.415 MHz ≤ f\_offset < 0.815 MHz | -20dBm- (-0.415) dB | 30 kHz |
| 0.8 MHz ≤ Δf < 1.6 MHz | 0.815 MHz ≤ f\_offset < 1.6 MHz | -25dBm | 30 kHz |
| 1.6 MHz ≤ Δf < Δfmax | 1.6 MHz ≤ f\_offset < f\_offsetmax | -25dBm | 100kHz |
| 600kHz | 0 MHz ≤ Δf < 0.6 MHz | 0.015 MHz ≤ f\_offset < 0.615 MHz | -9dBm - (-0.015) dB | 30 kHz |
| 0.6 MHz ≤ Δf < 1.2 MHz | 0.615 MHz ≤ f\_offset < 1.2 MHz | -22dBm - (-0.615) dB | 30 kHz |
| 1.2 MHz ≤ Δf < 1.8 MHz | 1.2 MHz ≤ f\_offset < 1.8 MHz | -27dBm | 30 kHz |
| 1.8 MHz ≤ Δf < Δfmax | 1.8 MHz ≤ f\_offset < f\_offsetmax | -25dBm | 100K |
| 800kHz | 0 MHz ≤ Δf < 0.8 MHz | 0.015 MHz ≤ f\_offset < 0.815 MHz | -9dBm - (-0.015) dB | 30 kHz |
| 0.8 MHz ≤ Δf < 1.6 MHz | 0.815 MHz ≤ f\_offset < 1.6 MHz | -23dBm - (-0.815) dB | 30 kHz |
| 1.6 MHz ≤ Δf < 2.4 MHz | 1.6 MHz ≤ f\_offset < 2.4 MHz | -28dBm | 30 kHz |
| 2.4 MHz ≤ Δf < Δfmax | 2.4 MHz ≤ f\_offset < f\_offsetmax | -25dBm | 100kHz |

#### 6.5.4.3 Minimum requirements for *BS type 1-C*

The operating band unwanted emissions for *BS type 1-C* for each *antenna connector* shall be below the applicable *basic limits* defined in clause 6.5.4.2.

### 6.5.5 Transmitter spurious emissions

#### 6.5.5.1 General

The transmitter spurious emission limits shall apply from 9 kHz to 12.75 GHz, excluding the frequency range from ΔfOBUE below the lowest frequency of each supported downlink *operating band*, up to ΔfOBUE above the highest frequency of each supported downlink *operating band*, where the ΔfOBUE is defined in table 6.5.1-1. For some *operating bands*, the upper limit is higher than 12.75 GHz in order to comply with the 5th harmonic limit of the downlink *operating band*, as specified in ITU-R recommendation SM.329 [2].

For a *multi-band connector*, for each supported *operating band* together with ΔfOBUE around the band is excluded from the transmitter spurious emissions requirement.

The requirements shall apply whatever the type of transmitter considered (single carrier or multi-carrier). It applies for all transmission modes foreseen by the manufacturer's specification.

The requirements shall also apply if the BS supports NB-IoT operation in NR in-band.

Unless otherwise stated, all requirements are measured as mean power (RMS).

#### 6.5.5.2 *Basic limits*

##### 6.5.5.2.1 General transmitter spurious emissions requirements

The *basic limits* of either table 6.5.5.2.1-1 (Category A limits) or table 6.5.5. 2.1-2 (Category B limits) shall apply. The application of either Category A or Category B limits shall be the same as for operating band unwanted emissions in clause 6.5.4.

Table 6.5.5.2.1-1: General BS transmitter spurious emission limits in FR1, Category A

|  |  |  |  |
| --- | --- | --- | --- |
| Spurious frequency range | *Basic limit* | *Measurement bandwidth* | Notes |
| 9 kHz – 150 kHz |  | 1 kHz | Note 1, Note 4 |
| 150 kHz – 30 MHz |  | 10 kHz | Note 1, Note 4 |
| 30 MHz – 1 GHz |  | 100 kHz | Note 1 |
| 1 GHz 12.75 GHz | -13 dBm | 1 MHz | Note 1, Note 2 |
| 12.75 GHz – 5th harmonic of the upper frequency edge of the DL *operating band* in GHz |  | 1 MHz | Note 1, Note 2, Note 3 |
| 12.75 GHz - 26 GHz | -13 dBm | 1 MHz | Note 1, Note 2, Note 5 |
| NOTE 1: *Measurement bandwidth*s as in ITU-R SM.329 [2], s4.1.  NOTE 2: Upper frequency as in ITU-R SM.329 [2], s2.5 table 1.  NOTE 3: Applies for Band for which the upper frequency edge of the DL *operating band* is greater than 2.55 GHz and less than or equal to 5.2 GHz..  NOTE 4: This spurious frequency range applies only to *BS type 1-C*.  NOTE 5: Applies for Band for which the upper frequency edge of the DL *operating band* is greater than 5.2 GHz. | | | |

Table 6.5.5.2.1-2: General BS transmitter spurious emission limits in FR1, Category B

|  |  |  |  |
| --- | --- | --- | --- |
| Spurious frequency range | *Basic limit* | *Measurement bandwidth* | Notes |
| 9 kHz – 150 kHz |  | 1 kHz | Note 1, Note 4 |
| 150 kHz – 30 MHz | -36 dBm | 10 kHz | Note 1, Note 4 |
| 30 MHz – 1 GHz |  | 100 kHz | Note 1 |
| 1 GHz – 12.75 GHz |  | 1 MHz | Note 1, Note 2 |
| 12.75 GHz – 5th harmonic of the upper frequency edge of the DL *operating band* in GHz | -30 dBm | 1 MHz | Note 1, Note 2, Note 3 |
| 12.75 GHz - 26 GHz | - 30 dBm | 1 MHz | Note 1, Note 2, Note 5 |
| NOTE 1: *Measurement bandwidth*s as in ITU-R SM.329 [2], s4.1.  NOTE 2: Upper frequency as in ITU-R SM.329 [2], s2.5 table 1.  NOTE 3: Applies for Band for which the upper frequency edge of the DL *operating band* is greater than 2.55 GHz and less than or equal to 5.2 GHz.  NOTE 4: This spurious frequency range applies only to *BS type 1-C*.  NOTE 5: Applies for Band for which the upper frequency edge of the DL *operating band* is greater than 5.2 GHz. | | | |

##### ~~6.5.5.2.2 Protection of the BS receiver of own or different BS~~

~~This requirement shall be applied for NR FDD operation in order to prevent the receivers of the BSs being desensitised by emissions from a BS transmitter. It is measured at the transmit~~ *~~antenna connector~~* ~~for~~ *~~BS type 1-C~~* ~~for any type of BS which has common or separate Tx/Rx~~ *~~antenna~~**~~connectors~~*~~.~~

~~The spurious emission~~ *~~basic limits~~* ~~are provided in table 6.5.5.2.2-1.~~

~~Table 6.5.5.2.2-1: BS spurious emissions~~ *~~basic limits~~* ~~for protection of the BS receiver~~

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| ~~BS class~~ | ~~Frequency range~~ | *~~Basic limits~~* | *~~Measurement bandwidth~~* | ~~Note~~ |
| ~~Medium Range BS~~ | ~~F~~~~UL,low~~ ~~– F~~~~UL,high~~ | ~~-91 dBm~~ | ~~100 kHz~~ |  |

##### 6.5.5.2.3 Additional spurious emissions requirements

These requirements may be applied for the protection of system operating in frequency ranges other than the BS downlink *operating band*. The limits may apply as an optional protection of such systems that are deployed in the same geographical area as the BS, or they may be set by local or regional regulation as a mandatory requirement for an NR *operating band*. It is in some cases not stated in the present document whether a requirement is mandatory or under what exact circumstances that a limit applies, since this is set by local or regional regulation. An overview of regional requirements in the present document is given in clause 4.5.

Some requirements may apply for the protection of specific equipment (UE, MS and/or BS) or equipment operating in specific systems (GSM, CDMA, UTRA, E-UTRA, NR, etc.) as listed below.

The spurious emission *basic limits* are provided in table 6.5.5.2.3 -1 for a BS where requirements for co-existence with the system listed in the first column apply. For a *multi-band connector*, the exclusions and conditions in the Note column of table 6.5.5.2.3 -1 apply for each supported *operating band*.

Table 6.5.5.2.3-1: BS spurious emissions *basic* *limits* for BS for co-existence with systems operating in other frequency bands

| System type for NR to co-exist with | Frequency range for co-existence requirement | *Basic limits* | *Measurement bandwidth* | Note |
| --- | --- | --- | --- | --- |
|  | 1805 – 1880 MHz | -47 dBm | 100 kHz | This requirement does not apply to BS operating in band n3. |
| DCS1800 | 1710 – 1785 MHz | -61 dBm | 100 kHz | This requirement does not apply to BS operating in band n3, since it is already covered by the requirement in clause 6.5.5.2.2. |
|  | 1930 – 1990 MHz | -47 dBm | 100 kHz | This requirement does not apply to BS operating in band n2, n25 or band n70. |
| PCS1900 | 1850 – 1910 MHz | -61 dBm | 100 kHz | This requirement does not apply to BS operating in band n2 or n25 since it is already covered by the requirement in clause 6.5.5.2.2. |
|  | 869 – 894 MHz | -57 dBm | 100 kHz | This requirement does not apply to BS operating in band n5 or n26. |
| GSM850 or CDMA850 | 824 – 849 MHz | -61 dBm | 100 kHz | This requirement does not apply to BS operating in band n5 or n26, since it is already covered by the requirement in clause 6.5.5.2.2. |
| UTRA FDD Band I or | 2110 – 2170 MHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in band n1 or n65 |
| E-UTRA Band 1 or NR Band n1 | 1920 – 1980 MHz | -49 dBm | 1 MHz | This requirement does not apply to BS operating in band n1 or n65, since it is already covered by the requirement in clause 6.5.5.2.2. |
| UTRA FDD Band II or | 1930 – 1990 MHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in band n2 or n70. |
| E-UTRA Band 2 or NR Band n2 | 1850 – 1910 MHz | -49 dBm | 1 MHz | This requirement does not apply to BS operating in band n2, since it is already covered by the requirement in clause 6.5.5.2.2. |
| UTRA FDD Band III or | 1805 – 1880 MHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in band n3. |
| E-UTRA Band 3 or NR Band n3 | 1710 – 1785 MHz | -49 dBm | 1 MHz | This requirement does not apply to BS operating in band n3, since it is already covered by the requirement in clause 6.5.5.2.2. |
| UTRA FDD Band IV or | 2110 – 2155 MHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in band n66 |
| E-UTRA Band 4 | 1710 – 1755 MHz | -49 dBm | 1 MHz | This requirement does not apply to BS operating in band n66, since it is already covered by the requirement in clause 6.5.5.2.2. |
| UTRA FDD Band V or | 869 – 894 MHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in band n5 or n26. |
| E-UTRA Band 5 or NR Band n5 | 824 – 849 MHz | -49 dBm | 1 MHz | This requirement does not apply to BS operating in band n5 or n26, since it is already covered by the requirement in clause 6.5.5.2.2. |
| UTRA FDD Band VI, XIX or | 860 – 890 MHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in band n18. |
| E-UTRA Band 6, 18, 19 or NR Band n18 | 815 – 830 MHz | -49 dBm | 1 MHz | This requirement does not apply to BS operating in band n18, since it is already covered by the requirement in clause 6.5.5.2.2. |
|  | 830 – 845 MHz | -49 dBm | 1 MHz |  |
| UTRA FDD Band VII or | 2620 – 2690 MHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in band n7. |
| E-UTRA Band 7 or NR Band n7 | 2500 – 2570 MHz | -49 dBm | 1 MHz | This requirement does not apply to BS operating in band n7, since it is already covered by the requirement in clause 6.5.5.2.2. |
| UTRA FDD Band IX or | 1844.9 – 1879.9 MHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in band n3. |
| E-UTRA Band 9 | 1749.9 – 1784.9 MHz | -49 dBm | 1 MHz | This requirement does not apply to BS operating in band n3, since it is already covered by the requirement in clause 6.5.5.2.2. |
| UTRA FDD Band X or | 2110 – 2170 MHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in band n66 |
| E-UTRA Band 10 | 1710 – 1770 MHz | -49 dBm | 1 MHz | This requirement does not apply to BS operating in band n66, since it is already covered by the requirement in clause 6.5.5.2.2. |
| UTRA FDD Band XI or XXI or | 1475.9 – 1510.9 MHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in band n50, n74, n75, n92, n94 or n109. |
| E-UTRA Band 11 or 21 | 1427.9 – 1447.9 MHz | -49 dBm | 1 MHz | This requirement does not apply to BS operating in band n50, n51, n74, n75, n76, n91, n92, n93, or n109. |
|  | 1447.9 – 1462.9 MHz | -49 dBm | 1 MHz | This requirement does not apply to BS operating in band n50, n74, n75, n92, n94 or n109. |
| UTRA FDD Band XII or | 729 – 746 MHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in band n12 or n85. |
| E-UTRA Band 12 or NR Band n12 | 699 – 716 MHz | -49 dBm | 1 MHz | This requirement does not apply to BS operating in band n12 or n85, since it is already covered by the requirement in clause 6.5.5.2.2.  For NR BS operating in n29, it applies 1 MHz below the Band n29 downlink operating band (Note 5). |
| UTRA FDD Band XIII or | 746 – 756 MHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in band n13. |
| E-UTRA Band 13 or NR Band n13 | 777 – 787 MHz | -49 dBm | 1 MHz | This requirement does not apply to BS operating in band n13, since it is already covered by the requirement in clause 6.5.5.2.2. |
| UTRA FDD Band XIV or | 758 – 768 MHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in band n14. |
| E-UTRA Band 14 or NR band n14 | 788 – 798 MHz | -49 dBm | 1 MHz | This requirement does not apply to BS operating in band n14, since it is already covered by the requirement in clause 6.5.5.2.2. |
|  | 734 – 746 MHz | -52 dBm | 1 MHz |  |
| E-UTRA Band 17 | 704 – 716 MHz | -49 dBm | 1 MHz | For NR BS operating in n29, it applies 1 MHz below the Band n29 downlink operating band (Note 5). |
| UTRA FDD Band XX or | 791 – 821 MHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in band n20 or n28. |
| E-UTRA Band 20 or NR Band n20 | 832 – 862 MHz | -49 dBm | 1 MHz | This requirement does not apply to BS operating in band n20, since it is already covered by the requirement in clause 6.5.5.2.2. |
| UTRA FDD Band XXII | 3510 – 3590 MHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in band n48, n77 or n78. |
| or E-UTRA Band 22 | 3410 – 3490 MHz | -49 dBm | 1 MHz | This requirement does not apply to BS operating in band n77 or n78. |
|  | 1525 – 1559 MHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in band n24. |
| E-UTRA Band 24 or NR Band n24 | 1626.5 – 1660.5 MHz | -49 dBm | 1 MHz | This requirement does not apply to BS operating in band n24, since it is already covered by the requirement in clause 6.5.5.2.2. |
| UTRA FDD Band XXV or | 1930 – 1995 MHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in band n2, n25 or n70. |
| E-UTRA Band 25 or NR band n25 | 1850 – 1915 MHz | -49 dBm | 1 MHz | This requirement does not apply to BS operating in band n25 since it is already covered by the requirement in clause 6.5.5.2.2. For BS operating in Band n2, it applies for 1910 MHz to 1915 MHz, while the rest is covered in clause 6.5.5.2.2. |
| UTRA FDD Band XXVI or | 859 – 894 MHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in band n5 or n26. |
| E-UTRA Band 26 or NR Band n26 | 814 – 849 MHz | -49 dBm | 1 MHz | This requirement does not apply to BS operating in band n26 since it is already covered by the requirement in clause 6.5.5.2.2. For BS operating in Band n5, it applies for 814 MHz to 824 MHz, while the rest is covered in clause 6.5.5.2.2. |
|  | 852 – 869 MHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in Band n5. |
| E-UTRA Band 27 | 807 – 824 MHz | -49 dBm | 1 MHz | This requirement also applies to BS operating in Band n28, starting 4 MHz above the Band n28 downlink *operating band* (Note 5). |
| E-UTRA Band 28 or | 758 – 803 MHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in band n20, n67 or n28. |
| NR Band n28 | 703 – 748 MHz | -49 dBm | 1 MHz | This requirement does not apply to BS operating in band n28, since it is already covered by the requirement in clause 6.5.5.2.2.  For BS operating in band n67, it applies for 703 MHz to 736 MHz. |
| E-UTRA Band 29 or NR Band n29 | 717 – 728 MHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in Band n29 or n85 |
| E-UTRA Band 30 or | 2350 – 2360 MHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in band n30 |
| NR Band n30 | 2305 – 2315 MHz | -49 dBm | 1 MHz | This requirement does not apply to BS operating in band n30, since it is already covered by the requirement in clause 6.5.5.2.2. |
| E-UTRA Band 31 or NR Band n31 | 462.5 – 467.5 MHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in band n31 or n72. |
| 452.5 – 457.5 MHz | -49 dBm | 1 MHz | This requirement does not apply to BS operating in band n31, since it is already covered by the requirement in clause 6.5.5.2.2. This requirement does not apply to BS operating in band n72. |
| UTRA FDD band XXXII or E-UTRA band 32 | 1452 – 1496 MHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in band n50, n74, n75, n92, n94 or n109 |
| UTRA TDD Band a) or E-UTRA Band 33 | 1900 – 1920 MHz | -52 dBm | 1 MHz |  |
| UTRA TDD Band a) or E-UTRA Band 34 or NR band n34 | 2010 – 2025 MHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in Band n34. |
| UTRA TDD Band b) or E-UTRA Band 35 | 1850 – 1910 MHz | -52 dBm | 1 MHz |  |
| UTRA TDD Band b) or E-UTRA Band 36 | 1930 – 1990 MHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in Band n2 or n25. |
| UTRA TDD Band c) or E-UTRA Band 37 | 1910 – 1930 MHz | -52 dBm | 1 MHz |  |
| UTRA TDD Band d) or E-UTRA Band 38 or NR Band n38 | 2570 – 2620 MHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in Band n38. |
| UTRA TDD Band f) or E-UTRA Band 39 or NR band n39 | 1880 – 1920MHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in Band n39. |
| UTRA TDD Band e) or E-UTRA Band 40 or NR Band n40 | 2300 – 2400MHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in Band n30 or n40. |
| E-UTRA Band 41 or NR Band n41, n90 | 2496 – 2690 MHz | -52 dBm | 1 MHz | This is not applicable to BS operating in Band n41, n53 or [n90]. |
| E-UTRA Band 42 | 3400 – 3600 MHz | -52 dBm | 1 MHz | This is not applicable to BS operating in Band n48, n77 or n78. |
| E-UTRA Band 43 | 3600 – 3800 MHz | -52 dBm | 1 MHz | This is not applicable to BS operating in Band n48, n77 or n78. |
| E-UTRA Band 44 | 703 – 803 MHz | -52 dBm | 1 MHz | This is not applicable to BS operating in Band n28. |
| E-UTRA Band 45 | 1447 – 1467 MHz | -52 dBm | 1 MHz |  |
| E-UTRA Band 46 or NR Band n46 | 5150 – 5925 MHz | -52 dBm | 1 MHz | This is not applicable to BS operating in Band n46, n96 or n102. |
| E-UTRA Band 47 | 5855 – 5925 MHz | -52 dBm | 1 MHz |  |
| E-UTRA Band 48 or NR Band n48 | 3550 – 3700 MHz | -52 dBm | 1 MHz | This is not applicable to BS operating in Band n48, n77 or n78. |
| E-UTRA Band 50 or NR band n50 | 1432 – 1517 MHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in Band n50, n51, n74, n75, n76, n91, n92, n93, n94 or n109. |
| E-UTRA Band 51 or NR Band n51 | 1427 – 1432 MHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in Band n50, n51, n75, n76, n91, n92, n93, n94 or n109. |
| E-UTRA Band 53 or NR Band n53 | 2483.5 - 2495 MHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in Band n41, n53 or n90. |
| E-UTRA Band 54 or NR Band n54 | 1670 – 1675 MHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in Band n54 |
| E-UTRA Band 65 or | 2110 – 2200 MHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in band n1 or n65. |
| NR Band n65 | 1920 – 2010 MHz | -49 dBm | 1 MHz | For BS operating in Band n1, it applies for 1980 MHz to 2010 MHz, while the rest is covered in clause 6.5.5.2.2.  This requirement does not apply to BS operating in band n65, since it is already covered by the requirement in clause 6.5.5.2.2. |
| E-UTRA Band 66 or | 2110 – 2200 MHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in band n66. |
| NR Band n66 | 1710 – 1780 MHz | -49 dBm | 1 MHz | This requirement does not apply to BS operating in band n66, since it is already covered by the requirement in clause 6.5.5.2.2. |
| E-UTRA Band 67 or NR Band n67 | 738 – 758 MHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in Band n28 or n67. |
| E-UTRA Band 68 | 753 -783 MHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in band n28. |
|  | 698-728 MHz | -49 dBm | 1 MHz | For BS operating in Band n28, this requirement applies between 698 MHz and 703 MHz, while the rest is covered in clause 6.5.5.2.2. |
| E-UTRA Band 69 | 2570 – 2620 MHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in Band n38. |
| E-UTRA Band 70 or | 1995 – 2020 MHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in band n2, n25 or n70 |
| NR Band n70 | 1695 – 1710 MHz | -49 dBm | 1 MHz | This requirement does not apply to BS operating in band n70, since it is already covered by the requirement in clause 6.5.5.2.2. |
| E-UTRA Band 71 or | 617 – 652 MHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in band n71 or n105 |
| NR Band n71 | 663 – 698 MHz | -49 dBm | 1 MHz | This requirement does not apply to BS operating in band n71 or n105, since it is already covered by the requirement in clause 6.5.5.2.2. |
| E-UTRA Band 72 or NR Band n72 | 461 – 466 MHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in band n31 or n72. |
| 451 – 456 MHz | -49 dBm | 1 MHz | This requirement does not apply to BS operating in band n72, since it is already covered by the requirement in clause 6.5.5.2.2. This requirement does not apply to BS operating in band n31. |
| E-UTRA Band 74 | 1475 – 1518 MHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in band n50, n74, n75, n92, n94 or n109. |
| or NR Band n74 | 1427 – 1470 MHz | -49 dBm | 1MHz | This requirement does not apply to BS operating in band n50, n51, n74, n75, n76, n91, n92, n93 or n94 or n109. |
| E-UTRA Band 75 or NR Band n75 | 1432 – 1517 MHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in Band n50, n51, n74, n75, n76, n91, n92, n93 or n94 or n109. |
| E-UTRA Band 76 or NR Band n76 | 1427 – 1432 MHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in Band n50, n51, n75, n76, n91, n92, n93, n94 or n109. |
| NR Band n77 | 3.3 – 4.2 GHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in Band n48, n77 or n78 |
| NR Band n78 | 3.3 – 3.8 GHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in Band n48, n77 or n78 |
| NR Band n79 | 4.4 – 5.0 GHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in Band n79 |
| NR Band n80 | 1710 – 1785 MHz | -49 dBm | 1 MHz | This requirement does not apply to BS operating in band n3, since it is already covered by the requirement in clause 6.5.5.2.2. |
| NR Band n82 | 832 – 862 MHz | -49 dBm | 1 MHz | This requirement does not apply to BS operating in band n20, since it is already covered by the requirement in clause 6.5.5.2.2. |
| NR Band n83 | 703 – 748 MHz | -49 dBm | 1 MHz | This requirement does not apply to BS operating in band n28, since it is already covered by the requirement in clause 6.5.5.2.2.  For BS operating in Band n67, it applies for 703 MHz to 736 MHz. |
| NR Band n84 | 1920 – 1980 MHz | -49 dBm | 1 MHz | This requirement does not apply to BS operating in band n1, since it is already covered by the requirement in clause 6.5.5.2.2. |
| E-UTRA Band 85 or NR Band n85 | 728 – 746 MHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in band n12 or n85.  For NR BS operating in n29, it applies 1 MHz below the Band n29 downlink operating band (Note 5). |
|  | 698 – 716 MHz | -49 dBm | 1 MHz | This requirement does not apply to BS operating in band n12 or n85, since it is already covered by the requirement in clause 6.5.5.2.2. |
| NR Band n86 | 1710 – 1780 MHz | -49 dBm | 1 MHz | This requirement does not apply to BS operating in band n66, since it is already covered by the requirement in clause 6.5.5.2.2. |
| NR Band n89 | 824 – 849 MHz | -49 dBm | 1 MHz | This requirement does not apply to BS operating in band n5, since it is already covered by the requirement in clause 6.5.5.2.2. |
|  | 1427 – 1432 MHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in Band n50, n51, n75, n76 or n109 |
| NR Band n91 | 832 – 862 MHz | -49 dBm | 1 MHz | This requirement does not apply to BS operating in band n20, since it is already covered by the requirement in clause 6.5.5.2.2. |
|  | 1432 – 1517 MHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in Band n50, n51, n74, n75, n76 or n109. |
| NR Band n92 | 832 – 862 MHz | -49 dBm | 1 MHz | This requirement does not apply to BS operating in band n20, since it is already covered by the requirement in clause 6.5.5.2.2. |
|  | 1427 – 1432 MHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in Band n50, n51, n75, n76 or n109. |
|  | 1432 – 1517 MHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in Band n50, n51, n74, n75, n76 or n109. |
| NR Band n95 | 2010 – 2025 MHz | -52 dBm | 1 MHz |  |
| NR Band n96 | 5925 – 7125 MHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in Band n46, n96, n102 or n104. |
| NR Band n97 | 2300 – 2400MHz | -52 dBm | 1 MHz |  |
| NR Band n98 | 1880 – 1920MHz | -52 dBm | 1 MHz |  |
| NR Band n99 | 1626.5 – 1660.5 MHz | -49 dBm | 1 MHz | This requirement does not apply to BS operating in band n24, since it is already covered by the requirement in clause 6.5.5.2.2. |
|  | 874.4 – 880 MHz | -49 dBm | 1 MHz | This requirement does not apply to BS operating in band n100, since it is already covered by the requirement in clause 6.5.5.2.2. |
| NR band n101 | 1900 – 1910 MHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in Band n101. |
| NR Band n102 | 5925 – 6425 MHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in Band n46, n96, n102 or n104. |
| E-UTRA Band 103 | 757 – 758 MHz | -52 dBm | 1 MHz |  |
|  | 787 – 788 MHz | -49 dBm | 1 MHz |  |
| NR Band n104 | 6425 – 7125 MHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in Band n96, n102 or n104 |
| NR Band n105 | 612 – 652 MHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in Band n71 or n105 |
|  | 663 – 703 MHz | -49 dBm | 1 MHz | This requirement does not apply to BS operating in n105, since it is already covered by the requirement in clause 6.5.5.2.2. |
| E-UTRA Band 106 or NR Band n106 | 935 - 940 MHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in Band n106 |
|  | 896 – 901 MHz | -49 dBm | 1 MHz | This requirement does not apply to BS operating in Band n5 or n26.  This requirement does not apply to BS operating in n106, since it is already covered by the requirement in clause 6.5.5.2.2. |
| NR Band n109 | 1432 – 1517 MHz | -52 dBm | 1 MHz | This requirement does not apply to BS operating in Band n50, n51, n74, n75, n76, n91, n92, n93, n94 or n109 |
| 703 –733MHz | -49 dBm | 1 MHz | This requirement does not apply to BS operating in band n28, since it is already covered by the requirement in clause 6.5.5.2.2. |

NOTE 1: As defined in the scope for spurious emissions in this clause, except for the cases where the noted requirements apply to a BS operating in Band n28, the co-existence requirements in table 6.5.5.2.3 -1 do not apply for the ΔfOBUE frequency range immediately outside the downlink *operating band* (see table 5.2-1). Emission limits for this excluded frequency range may be covered by local or regional requirements.

NOTE 2: Table 6.5.5.2.3 -1 assumes that two *operating bands*, where the frequency ranges in table 5.2-1 would be overlapping, are not deployed in the same geographical area. For such a case of operation with overlapping frequency arrangements in the same geographical area, special co-existence requirements may apply that are not covered by the 3GPP specifications.

NOTE 3: TDD base stations deployed in the same geographical area, that are synchronized and use the same or adjacent *operating bands* can transmit without additional co-existence requirements. For unsynchronized base stations, special co-existence requirements may apply that are not covered by the 3GPP specifications.

The following requirement may be applied for the protection of PHS. This requirement is also applicable at specified frequencies falling between ΔfOBUE below the lowest BS transmitter frequency of the downlink *operating band* and ΔfOBUE above the highest BS transmitter frequency of the downlink *operating band*. ΔfOBUE is defined in clause 6.5.1.

The spurious emission *basic limit* for this requirement is:

Table 6.5.5.2.3-2: BS spurious emissions *basic limits* for BS for co-existence with PHS

|  |  |  |  |
| --- | --- | --- | --- |
| Frequency range | *Basic limit* | *Measurement Bandwidth* | Note |
| 1884.5 – 1915.7 MHz | -41 dBm | 300 kHz | Applicable when co-existence with PHS system operating in 1884.5 – 1915.7 MHz |

Table 6.5.5.2.3-3: Void

##### 6.5.5.2.4 Co-location with other base stations

These requirements may be applied for the protection of other BS receivers when GSM900, DCS1800, PCS1900, GSM850, CDMA850, UTRA FDD, UTRA TDD, E-UTRA and/or NR BS are co-located with a BS.

The requirements assume a 30 dB coupling loss between transmitter and receiver and are based on co-location with base stations of the same class.

The *basic limits* are in table 6.5.5.2.4-1 for a BS where requirements for co-location with a BS type listed in the first column apply, depending on the declared Base Station class.

Table 6.5.5.2.4-1: BS spurious emissions *basic* limits for BS co-located with another BS

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Type of co-located BS | Frequency range for | *Basic limits* | | | Measurement | Note |
|  | co-location requirement | WA BS | MR BS | LA BS | bandwidth |  |
| GSM900 | 876 – 915 MHz | -98 dBm | -91 dBm | -70 dBm | 100 kHz |  |
| DCS1800 | 1710 – 1785 MHz | -98 dBm | -91 dBm | -80 dBm | 100 kHz |  |
| PCS1900 | 1850 – 1910 MHz | -98 dBm | -91 dBm | -80 dBm | 100 kHz |  |
| GSM850 or CDMA850 | 824 – 849 MHz | -98 dBm | -91 dBm | -70 dBm | 100 kHz |  |
| UTRA FDD Band I or E-UTRA Band 1 or NR Band n1 | 1920 – 1980 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| UTRA FDD Band II or E-UTRA Band 2 or NR Band n2 | 1850 – 1910 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| UTRA FDD Band III or E-UTRA Band 3 or NR Band n3 | 1710 – 1785 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| UTRA FDD Band IV or E-UTRA Band 4 | 1710 – 1755 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| UTRA FDD Band V or E-UTRA Band 5 or NR Band n5 | 824 – 849 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| UTRA FDD Band VI, XIX or E-UTRA Band 6, 19 | 830 – 845 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| UTRA FDD Band VII or E-UTRA Band 7 or NR Band n7 | 2500 – 2570 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| UTRA FDD Band VIII or E-UTRA Band 8 or NR Band n8 | 880 – 915 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| UTRA FDD Band IX or E-UTRA Band 9 | 1749.9 – 1784.9 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| UTRA FDD Band X or E-UTRA Band 10 | 1710 – 1770 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| UTRA FDD Band XI or E-UTRA Band 11 | 1427.9 –1447.9 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz | This is not applicable to BS operating in Band n50, n75, n91, n92, n93 or n94 |
| UTRA FDD Band XII or  E-UTRA Band 12 or NR Band n12 | 699 – 716 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| UTRA FDD Band XIII or  E-UTRA Band 13 or NR Band n13 | 777 – 787 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| UTRA FDD Band XIV or  E-UTRA Band 14 or NR Band n14 | 788 – 798 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| E-UTRA Band 17 | 704 – 716 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| E-UTRA Band 18 or NR Band n18 | 815 – 830 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| UTRA FDD Band XX or E-UTRA Band 20 or NR Band n20 | 832 – 862 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| UTRA FDD Band XXI or E-UTRA Band 21 | 1447.9 – 1462.9 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz | This is not applicable to BS operating in Band n50, n75, n92 or n94 |
| UTRA FDD Band XXII or E-UTRA Band 22 | 3410 – 3490 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz | This is not applicable to BS operating in Band n48, n77 or n78 |
| E-UTRA Band 24 or NR Band n24 | 1626.5 – 1660.5 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| UTRA FDD Band XXV or  E-UTRA Band 25 or NR Band n25 | 1850 – 1915 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| UTRA FDD Band XXVI or  E-UTRA Band 26 or NR Band n26 | 814 – 849 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| E-UTRA Band 27 | 807 – 824 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| E-UTRA Band 28 or NR Band n28 | 703 – 748 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| E-UTRA Band 30 or NR Band n30 | 2305 – 2315 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| E-UTRA Band 31 or NR Band n31 | 452.5 – 457.5 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| UTRA TDD Band a) or E-UTRA Band 33 | 1900 – 1920 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| UTRA TDD Band a) or E-UTRA Band 34 or NR band n34 | 2010 – 2025 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz | This is not applicable to BS operating in Band n34 |
| UTRA TDD Band b) or E-UTRA Band 35 | 1850 – 1910 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| UTRA TDD Band b) or E-UTRA Band 36 | 1930 – 1990 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz | This is not applicable to BS operating in Band n2 or band n25 |
| UTRA TDD Band c) or E-UTRA Band 37 | 1910 – 1930 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| UTRA TDD Band d) or E-UTRA Band 38 or NR Band n38 | 2570 – 2620 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz | This is not applicable to BS operating in Band n38. |
| UTRA TDD Band f) or E-UTRA Band 39 or NR band n39 | 1880 – 1920MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz | This is not applicable to BS operating in Band n39 |
| UTRA TDD Band e) or E-UTRA Band 40 or NR Band n40 | 2300 – 2400MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz | This is not applicable to BS operating in Band n30 or n40. |
| E-UTRA Band 41 or NR Band n41, n90 | 2496 – 2690 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz | This is not applicable to BS operating in Band n41, n53 or [n90] |
| E-UTRA Band 42 | 3400 – 3600 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz | This is not applicable to BS operating in Band n48, n77 or n78 |
| E-UTRA Band 43 | 3600 – 3800 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz | This is not applicable to BS operating in Band n48, n77 or n78 |
| E-UTRA Band 44 | 703 – 803 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz | This is not applicable to BS operating in Band n28 |
| E-UTRA Band 45 | 1447 – 1467 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| E-UTRA Band 46 or NR Band n46 | 5150 – 5925 MHz | N/A | -91 dBm | -88 dBm | 100 kHz | This is not applicable to BS operating in Band n46, n96 or n102 |
| E-UTRA Band 48 or NR Band n48 | 3550 – 3700 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz | This is not applicable to BS operating in Band n48, n77 or n78 |
| E-UTRA Band 50 or NR Band n50 | 1432 – 1517 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz | This is not applicable to BS operating in Band n51, n74, n75, n91, n92, n93 or n94 |
| E-UTRA Band 51 or NR Band n51 | 1427 – 1432 MHz | N/A | N/A | -88 dBm | 100 kHz | This is not applicable to BS operating in Band n50, n74, n75, n76, n91, n92, n93 or n94 |
| E-UTRA Band 53 or NR Band n53 | 2483.5 – 2495 MHz | N/A | -91 dBm | -88 dBm | 100 kHz | This is not applicable to BS operating in Band n41, n53 or n90 |
| E-UTRA Band 54 or NR Band n54 | 1670 – 1675 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz | This is not applicable to BS operating in Band n54 |
| E-UTRA Band 65 or NR Band n65 | 1920 – 2010 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| E-UTRA Band 66 or NR Band n66 | 1710 – 1780 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| E-UTRA Band 68 | 698 – 728 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| E-UTRA Band 70 or NR Band n70 | 1695 – 1710 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| E-UTRA Band 71 or NR Band n71 | 663 – 698 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| E-UTRA Band 72 or NR Band n72 | 451 – 456 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| E-UTRA Band 74 or NR Band n74 | 1427 – 1470 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz | This is not applicable to BS operating in Band n50, n51, n91, n92, n93 or n94 |
| NR Band n77 | 3.3 – 4.2 GHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz | This is not applicable to BS operating in Band n48, n77 or n78 |
| NR Band n78 | 3.3 – 3.8 GHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz | This is not applicable to BS operating in Band n48, n77 or n78 |
| NR Band n79 | 4.4 – 5.0 GHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| NR Band n80 | 1710 – 1785 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| NR Band n81 | 880 – 915 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| NR Band n82 | 832 – 862 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| NR Band n83 | 703 – 748 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| NR Band n84 | 1920 – 1980 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| E-UTRA Band 85 or NR Band 85 | 698 – 716 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| NR Band n86 | 1710 – 1780 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| NR Band n89 | 824 – 849 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| NR Band n91 | 832 – 862 MHz | N/A | N/A | -88 dBm | 100 kHz |  |
| NR Band n92 | 832 – 862 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| NR Band n93 | 880 – 915 MHz | N/A | N/A | -88 dBm | 100 kHz |  |
| NR Band n94 | 880 – 915 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| NR Band n95 | 2010 – 2025 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| NR Band n96 | 5925 – 7125 MHz | N/A | -90 dBm | -87 dBm | 100 kHz | This is not applicable to BS operating in Band n46,  n96, n102 or n104 |
| NR Band n97 | 2300 – 2400MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| NR Band n98 | 1880 – 1920MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| NR Band n99 | 1626.5 – 1660.5 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| NR Band n100 | 874.4 – 880 MHz | -96 dBm | NA | NA | 100 kHz |  |
| NR Band n101 | 1900 – 1910 MHz | -96 dBm | NA | NA | 100 kHz |  |
| NR Band n102 | 5925 – 6425 MHz | N/A | -90 dBm | -87 dBm | 100 kHz | This is not applicable to BS operating in Band n46, n96, n102 or n104 |
| E-UTRA Band 103 | 787 – 788 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| NR Band n104 | 6425 – 7125 MHz | -95 dBm | -90 dBm | -87 dBm | 100 kHz | This requirement does not apply to BS operating in Band n96, n102 or n104. |
| NR Band n105 | 663 – 703 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| E-UTRA Band 106 or NR Band n106 | 896 – 901 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| NR Band n109 | 703 – 733 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |

NOTE 1: As defined in the scope for spurious emissions in this clause, the co-location requirements in table 6.5.5.2.4-1 do not apply for the frequency range extending ΔfOBUE immediately outside the BS transmit frequency range of a downlink *operating band* (see table 5.2-1). The current state-of-the-art technology does not allow a single generic solution for co-location with other system on adjacent frequencies for 30dB BS-BS minimum coupling loss. However, there are certain site-engineering solutions that can be used. These techniques are addressed in TR 25.942 [4].

NOTE 2: Table 6.5.5.2.4-1 assumes that two *operating bands*, where the corresponding BS transmit and receive frequency ranges in table 5.2-1 would be overlapping, are not deployed in the same geographical area. For such a case of operation with overlapping frequency arrangements in the same geographical area, special co-location requirements may apply that are not covered by the 3GPP specifications.

NOTE 3: Co-located TDD base stations that are synchronized and using the same or adjacent *operating band* can transmit without special co-locations requirements. For unsynchronized base stations, special co-location requirements may apply that are not covered by the 3GPP specifications.

#### 6.5.5.3 Minimum requirements for *BS type 1-C*

The Tx spurious emissions for *BS type 1-C* for each *antenna connector* shall not exceed the *basic limits* specified in clause 6.5.5.2.

---End of changes---