**3GPP TSG-RAN4 Meeting #116 *R4-2509991***

|  |
| --- |
| *CR-Form-v12.3* |
| **CHANGE REQUEST** |
|  |
|  | 38.133 | **CR** |  | **rev** |  | **Current version:** | 19.1.0 |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **x** | Radio Access Network |  | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  | Draft CR on clarification of DL slots and UL slots in SBFD |
|  |  |
| ***Source to WG:*** | Apple |
| ***Source to TSG:*** | R4 |
|  |  |
| ***Work item code:*** | NR\_duplex\_evo-Core |  | ***Date:*** | 2025-08-14 |
|  |  |  |  |  |
| ***Category:*** | B |  | ***Release:*** | Rel-19 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-17 (Release 17)Rel-18 (Release 18)Rel-19 (Release 19) Rel-20 (Release 20)* |
|  |  |
| ***Reason for change:*** | To clarify that with SBFD, UE UL transmission can happen in UL slots or /transmission in SBFD slot and UE DL reception can happen in DL slots or reception in SBFD slot. |
|  |  |
| ***Summary of change:*** | In Section 3.6 Applicability of requirements in this specification version, make the above-stated clarfication |
|  |  |
| ***Consequences if not approved:*** | There is ambiguity in interpreting requirements for SBFD-aware UEs |
|  |  |
| ***Clauses affected:*** | 3.6 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  |  |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** | **x** |  |  Test specifications | TS 38.533 |
| ***(show related CRs)*** |  |  |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

# <Start of Change #1>

### 3.6.x Applicability of requirements for SBFD

If UE supports *supportSBFD* and SBFD is configured by network, in all applicable requirements hereafter the term “UL slot” includes UL slot or SBFD slot in which UE performs transmission, and the term “DL slot” includes DL slot or SBFD slot in which UE performs reception.

# <End of Change #1>