**3GPP TSG-RAN WG4 Meeting # 116R4-2510794**

**Bengalore, India,**

|  |
| --- |
| *CR-Form-v12.3* |
| **CHANGE REQUEST** |
|  |
|  | **38.133** | **CR** |  | **rev** |  | **Current version:** | **19.1.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  | Draft CR on Rel-19 SBFD UE to UE CLI handling |
|  |  |
| ***Source to WG:*** | Ericsson |
| ***Source to TSG:*** | R4 |
|  |  |
| ***Work item code:*** | NR\_duplex\_evo-Core |  | ***Date:*** | 2025-06-24 |
|  |  |  |  |  |
| ***Category:*** | B |  | ***Release:*** | 9  |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-17 (Release 17)Rel-18 (Release 18)Rel-19 (Release 19) Rel-20 (Release 20)* |
|  |  |
| ***Reason for change:*** | Clarification on Rel-19 SBFD requirements. Based on the endorsed draft Big CR R4-2508459Change 1:  remove the bracets |
|  |  |
| ***Summary of change:*** | Remove the bracets |
|  |  |
| ***Consequences if not approved:*** | The requirement SBFD CLI requirement is not complete  |
|  |  |
| ***Clauses affected:*** |  |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  |  |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  |  |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  |  |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

### <Start of Change 1>

9.x.3.6 Scheduling availability of UE during L1-CLI-RSSI measurements

Scheduling availability restrictions when the UE is performing L1-CLI-RSSI are described in the following clause.

##### 9.X.3.6.1 Scheduling availability of UE performing L1-CLI-RSSI measurement on FR1

The following scheduling restriction applies due to the L1-CLI-RSSI measurement:

* The UE is not expected to transmit PUCCH/PUSCH/SRS on OFDM symbols on which the UE performs L1-CLI-RSSI measurements.

When TDD intra-band carrier aggregation is configured, the scheduling restrictions on serving cell where CLI measurements are performed apply on all serving cells in the same band on the symbols that fully or partially overlap with restricted symbols.

When intra-band non-contiguous carrier aggregation is configured for a UE indicating *intraBandNR-CA-non-collocated-r18* and if *nonCollocatedTypeNR-CA-r18* is not provided, there are no scheduling restrictions on FR1 serving cell(s) to be measured and configured on the non-contiguous CC(s) in the same band. Otherwise, the scheduling restrictions on serving cell where CLI measurements are performed apply on all serving cells in the same band on the symbols that fully or partially overlap with restricted symbols if *nonCollocatedTypeNR-CA-r18* is provided.

##### 9.X.3.6.2 Scheduling availability of UE performing L1-CLI-RSSI measurement on FR2

The following scheduling restriction applies due to the L1-CLI-RSSI measurement:

* The UE is not expected to transmit PUCCH/PUSCH/SRS on OFDM symbols on which the UE performs L1-CLI-RSSI measurements.
* The UE is not expected to receive PDCCH/PDSCH/CSI-RS for tracking/CSI-RS for CQI on OFDM symbols on which the UE performs L1-CLI-RSSI measurements when RSSI resources are not TypeD QCL-ed with PDCCH/PDSCH/CSI-RS.

When TDD intra-band carrier aggregation is configured, the scheduling restrictions on serving cell where CLI measurements are performed apply on all serving cells in the same band on the symbols that fully or partially overlap with restricted symbols.

### <End of Change 1>