**3GPP TSG- RAN4 Meeting #116R4-251x**

**Bengaluru, India, 25th – 29th August, 2025**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.3* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  | **38.133** | **CR** |  | **rev** | **1** | **Current version:** | **19.1.0** |  |
|  | | | | | | | | |
| *For* [***HELP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network |  | Core Network |  |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | Draft CR on NR inter-frequency L1 measurement for XR | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | vivo | | | | | | | | | |
| ***Source to TSG:*** | R4 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | NR\_XR\_Ph3-Core | | | | |  | ***Date:*** | | | 2025-08-28 |
|  |  | | | |  | |  | | |  |
| ***Category:*** | B |  | | | | | ***Release:*** | | | Rel-19 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-17 (Release 17) Rel-18 (Release 18) Rel-19 (Release 19)  Rel-20 (Release 20)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | In the RAN4#114bis meeting, following agreement was made.  • Requirements in clause 9.15 NR inter-frequency L1 measurement with gaps are updated for gap skipping | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | * Updated inter-frequency L1 measurement requirements for gap skipping * Added UE behavior for L1 measurements: for UE supporting measurement gap occasion cancellation, the UE shall not perform the SSB/CSI-RS measurements during the cancelled gap occasions. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | No requirements for inter-frequency L1 measurement when gap skipping is enabled. Consequently, gap skipping and inter-frequency based LTM cannot work together.  UE behaviour of L1 measurements during cancelled gap is not specified. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | 9.15.5  8.1.2.2, 8.1.3.2, 8.5.2.2, 8.5.3.2  9.5.4, 9.8.4 | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  | **X** | Other core specifications | | | | TS/TR ... CR ... | | |
| ***affected:*** | | **X** |  | Test specifications | | | | TS 38.533 | | |
| ***(show related CRs)*** | |  | **X** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | |  | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | |  | | | | | | | | |

# <Start of Change #1>

### 9.15.5 L1-RSRP inter-frequency measurement requirements with measurement gaps

#### 9.15.5.1 Inter-frequency SSB based L1-RSRP reporting

The requirements specified in this clause are only applicable when

- *highSpeedMeasFlag-r16* is not configured, and

- *highSpeedMeasFlagFR2-r17* is not configured, and

- highSpeedMeasCA-Scell-r17 is not configured, and

- Concurrent gaps are not configured, and

- SSBs of the neighbor cell configured for inter-frequency L1-RSRP measurement are fully or partially overlapped with measurement gaps.

If an inter-frequency neighbor cell is known according to clause 9.15.2, the UE shall be capable of performing L1-RSRP measurements based on the configured SSB resource for L1-RSRP computation, and the UE physical layer shall be capable of reporting L1-RSRP measured over the measurement period of TL1-RSRP\_Measurement\_Period\_SSB\_Inter if *deriveSSB-IndexFromCellInter-r17* is enabled on target frequency layers or UE is indicated to report SSB based RRM measurement result with the associated SSB index (*reportQuantityRsIndexes* or *maxNrofRSIndexesToReport* is not configured) of the same cell. Otherwise, UE physical layer shall be capable of reporting L1-RSRP measured over the measurement period of TL1-RSRP\_Measurement\_Period\_SSB\_inter+TSSB\_time\_index\_inter, where TSSB\_time\_index\_inter is the time period used to acquire the index of the SSB being measured given in table 9.3.4.

The value of TL1-RSRP\_Measurement\_Period\_SSB\_Inter is defined in table 9.15.5.1-1 for FR1 and in table 9.15.5.1-3 for FR1 for the UE supporting *measurement gap occasion cancellation* provided that the configuration and conditions in clause 9.1.y.4 are met. The value of TL1-RSRP\_Measurement\_Period\_SSB\_Inter is defined in table 9.15.5.1-2 for FR2 and in table 9.15.5.1-4 for FR2 for the UE supporting *measurement gap occasion cancellation* provided that the configuration and conditions in clause 9.1.y.4 are met, where

- M= 2

- N = 8.

- CSSFinter: it is a carrier specific scaling factor and is determined according to CSSFwithin\_gap in clause 9.1.5.15 for L1-RSRP measurement conducted within measurement gaps.

Table 9.15.5.1-1: Inter-frequency L1-RSRP measurement period TL1-RSRP\_Measurement\_Period\_SSB\_Inter with measurement gapsin FR1

|  |  |
| --- | --- |
| Condition | TL1-RSRP\_Measurement\_Period\_SSB\_Inter |
| No DRX | Max(Treport, Ceil(M \* Kgap) × Max(MGRP, TSSB\_NBC) × CSSFinter) |
| DRX cycle ≤ 320 ms | Max(Treport, Ceil(M × 1.5 \* Kgap) × Max(MGRP, TSSB\_NBC, TDRX) × CSSFinter) |
| DRX cycle > 320 ms | Ceil(M \* Kgap) × TDRX × CSSFinter |
| NOTE 1: The definition of Kgap is the same as L3 measurement which is a scaling factor for a SSB frequency layer to be measured within an associated measurement gap pattern.  NOTE 2: If the UE is incapable of *multiCellL1-measRTD-greaterThan-CP-r18*, the requirements apply for the the cells configured by *LTM-CSI-ResourceConfig-r18* on which UE is required to perform L1 measurements, when the max RTD among the cells on the same inter-frequency layer is not larger than CP length.  NOTE 3: TSSB\_NBC is the periodicity of the neighbor cell SSB-Index configured for inter-frequency L1-RSRP measurement. TDRX is the DRX cycle length. TReport is the configured periodicity for reporting. | |

Table 9.15.5.1-2: Inter-frequency L1-RSRP measurement period TL1-RSRP\_Measurement\_Period\_SSB\_Inter with measurement gaps in FR2

|  |  |
| --- | --- |
| Condition | TL1-RSRP\_Measurement\_Period\_SSB\_Inter |
| No DRX | Max(Treport, Ceil(Kgap × M\*N)× Max(MGRP, TSSB\_NBC) × CSSFinter) |
| DRX cycle ≤ 320 ms | Max(Treport, Ceil(1.5 \* Kgap × M\*N) × Max(MGRP, TSSB\_NBC, TDRX) CSSFinter) |
| DRX cycle > 320 ms | Ceil(Kgap × M\*N) × TDRX × CSSFinter |
| NOTE 1: The definition of Kgap is the same as L3 measurement which is a scaling factor for a SSB frequency layer to be measured within an associated measurement gap pattern.  NOTE 2: If the UE is incapable of *multiCellL1-measRTD-greaterThan-CP-r18*, the requirements apply for the the cells configured by *LTM-CSI-ResourceConfig-r18* on which UE is required to perform L1 measurements, when the max RTD among the cells on the same inter-frequency layer is not larger than CP length.  NOTE 3: TSSB\_NBC is the periodicity of the neighbor cell SSB-Index configured for inter-frequency L1-RSRP measurement. TDRX is the DRX cycle length. TReport is the configured periodicity for reporting. | |

Table 9.15.5.1-3: Inter-frequency L1-RSRP measurement period TL1-RSRP\_Measurement\_Period\_SSB\_Inter for known cells in FR1 with measurement gap cancellation

|  |  |
| --- | --- |
| Condition | TL1-RSRP\_Measurement\_Period\_SSB\_Inter |
| No DRX | Max(Treport, Ceil((M+Lcancel) \* Kgap) × Max(MGRP, SSB period) × CSSFinter) |
| DRX cycle ≤ 320 ms | Max(Treport, Ceil((M+Lcancel) × 1.5 \* Kgap) × Max(MGRP, SSB period, DRX cycle) × CSSFinter) |
| DRX cycle > 320 ms | Ceil((M+Lcancel) \* Kgap) × DRX cycle × CSSFinter |
| NOTE 1: The definition of Kgap is the same as L3 measurement which is a scaling factor for a SSB frequency layer to be measured within an associated measurement gap pattern.  NOTE 2: If the UE is incapable of *multiCellL1-measRTD-greaterThan-CP-r18*, the requirements apply for the the cells configured by *LTM-CSI-ResourceConfig-r18* on which UE is required to perform L1 measurements, when the max RTD among the cells on the same inter-frequency layer is not larger than CP length.  NOTE 3: Lcancel is the number of gap occasions cancelled during measurement period TL1-RSRP\_Measurement\_Period\_SSB\_Inter. | |

Table 9.15.5.1-4: Inter-frequency L1-RSRP measurement period TL1-RSRP\_Measurement\_Period\_SSB\_Inter for known cells in FR2 with measurement gap cancellation

|  |  |
| --- | --- |
| Condition | TL1-RSRP\_Measurement\_Period\_SSB\_Inter |
| No DRX | Max(Treport, Ceil(Kgap × (M+Lcancel)\*N)× Max(MGRP, SSB period) × CSSFinter) |
| DRX cycle ≤ 320 ms | Max(Treport, Ceil(1.5 \* Kgap × (M+Lcancel)\*N) × Max(MGRP, SSB period, DRX cycle) × CSSFinter) |
| DRX cycle > 320 ms | Ceil(Kgap × (M+Lcancel)\*N) × DRX cycle × CSSFinter |
| NOTE 1: The definition of Kgap is the same as L3 measurement which is a scaling factor for a SSB frequency layer to be measured within an associated measurement gap pattern.  NOTE 2: If the UE is incapable of *multiCellL1-measRTD-greaterThan-CP-r18*, the requirements apply for the the cells configured by *LTM-CSI-ResourceConfig-r18* on which UE is required to perform L1 measurements, when the max RTD among the cells on the same inter-frequency layer is not larger than CP length.  NOTE 3: Lcancel is the number of gap occasions cancelled during measurement period TL1-RSRP\_Measurement\_Period\_SSB\_Inter. | |

# <End of Change #1>

# <Start of Change #2>

#### 8.1.2.2 Minimum requirement

UE shall be able to evaluate whether the downlink radio link quality on the configured RLM-RS resource estimated over the last TEvaluate\_out\_SSB period becomes worse than the threshold Qout\_SSB within TEvaluate\_out\_SSB evaluation period.

UE shall be able to evaluate whether the downlink radio link quality on the configured RLM-RS resource estimated over the last TEvaluate\_in\_SSB period becomes better than the threshold Qin\_SSB within TEvaluate\_in\_SSB evaluation period.

TEvaluate\_out\_SSB and TEvaluate\_in\_SSB are defined in table 8.1.2.2-1 for FR1.

TEvaluate\_out\_SSB and TEvaluate\_in\_SSB are defined in table 8.1.2.2-2 for FR2 with scaling factor N, where

- N=2, 4, or 6 for FR2-1 for UE supporting *fastBeamSweepingMultiRx-r18* according to the conditions in clause 3.6.19, and

- N=8 for other cases in FR2-1, and

- N=12 for FR2-2.

for FR2 power classes other than power class 6 or for FR2 power class 6 when *highSpeedMeasFlagFR2-r17* is not configured.

TEvaluate\_out\_SSB and TEvaluate\_in\_SSB are defined in table 8.1.2.2-3 for FR2 power class 6 UE configured with *highSpeedMeasFlagFR2-r17*.

TEvaluate\_out\_SSB and TEvaluate\_in\_SSB are defined in table 8.1.2.2-4 for FR1 (deactivated PSCell).

TEvaluate\_out\_SSB and TEvaluate\_in\_SSB are defined in table 8.1.2.2-5 for FR2 (deactivated PSCell) with scaling factor N=8 for FR2-1 and N=12 for FR2-2.

For a UE supporting *concurrentMeasGapsPreMG-r18* and when concurrent measurement gap(s) with Pre-MG(s) are configured, or a UE supporting *concurrentMeasGapsNCSG-r18* and when concurrent measurement gap(s) with NCSG(s) are configured, or a UE supporting *concurrentMeasGap-r17* or *musim-GapPreference-r17* or both *concurrentMeasGap-r17* and *musim-GapPreference-r17*, and when concurrent measurement gaps or periodic MUSIM gaps or both concurrent GAPs and periodic MUSIM gaps are configured,

- an RLM-RS resource occasion is not considered to be overlapped by a gap occasion if the gap occasion is dropped according to clauses 9.1.8 and 9.1.10,

P value for an RLM-RS resource to be measured is defined as

- Ntotal / Noutside\_MG in FR1

- Psharing factor \* Ntotal / Noutside\_MG in FR2 with Navailable = 0

- Ntotal / Navailable in FR2 with Navailable > 0

- For a window W of duration max(TL1, xRP\_max), where xRP\_max is the maximum xRP across all configured per-UE measurement gaps or periodic MUSIM gap(s) or NCSGs and per-FR measurement gaps or NCSGs, and, in case of Pre-MG, all activated per-UE measurement gaps and per-FR measurement gaps, within the same FR as serving cell, and starting at the beginning of any RLM-RS resource occasion:

- Ntotal is the total number of RLM-RS resource occasions within the window W, including those overlapped with GAP occasions, MUSIM gap occasions or SMTC occasions within the window W, and

- Noutside\_MG is the number of RLM-RS resource occasions that are not overlapped with any non-dropped GAP occasion nor non-dropped MUSIM gap occasion within the window W, and

- Navailable is the number of RLM-RS resource occasions that are not overlapped with any non-dropped GAP occasion nor non-dropped MUSIM gap occasion nor any SMTC occasion within the window W, and

- an RLM-RS resource occasion is considered to be overlapped with the MUSIM gap if it overlaps a MUSIM gap occasion, and

- TL1 is periodicity of the target RLM-RS.

- xRP = MGRP when configured GAP is activated Pre-MG or MG, and xRP = VIRP when configured GAP is NCSG.

Otherwise, for a UE neither supporting *concurrentMeasGap-r17* nor *concurrentMeasGapsPreMG-r18* nor *concurrentMeasGapsNCSG-r18* nor supporting *musim-GapPreference-r17* or when neither of the above configurations applies, i.e. concurrent measurement gaps, concurrent measurement gap(s) with Pre-MG(s), concurrent measurement gap(s) with NCSG(s), and periodic MUSIM gaps,

For FR1,

- , when in the monitored cell there are GAPs configured for intra-frequency, inter-frequency or inter-RAT measurements, and these GAPs are overlapping with some but not all occasions of the SSB; and

- P = 1 when in the monitored cell there are no GAPs overlapping with any occasion of the SSB.

For FR2

- , when RLM-RS resource is not overlapped with GAP and the RLM-RS resource is partially overlapped with SMTC occasion (TSSB < TSMTCperiod).

- P is Psharing factor, when the RLM-RS resource is not overlapped with GAP and RLM-RS resource is fully overlapped with SMTC occasion (TSSB = TSMTCperiod).

- , when the RLM-RS resource is partially overlapped with GAP and the RLM-RS resource is partially overlapped with SMTC occasion (TSSB < TSMTCperiod) and SMTC occasion is not overlapped with GAP and

- TSMTCperiod ≠ xRP or

- TSMTCperiod = xRP and TSSB < 0.5\*TSMTCperiod

- , when the RLM-RS is partially overlapped with GAP and the RLM-RS is partially overlapped with SMTC occasion (TSSB < TSMTCperiod) and SMTC occasion is not overlapped with GAP and TSMTCperiod = xRP and TSSB = 0.5 × TSMTCperiod

- , when the RLM-RS resource is partially overlapped with GAP and the RLM-RS resource is partially overlapped with SMTC occasion (TSSB < TSMTCperiod) and SMTC occasion is partially or fully overlapped with GAP

- , when the RLM-RS resource is partially overlapped with GAP and the RLM-RS resource is fully overlapped with SMTC occasion (TSSB = TSMTCperiod) and SMTC occasion is partially overlapped with GAP (TSMTCperiod < xRP)

where,

- Psharing factor = 1, if the RLM-RS resource outside GAP is

- not overlapped with the SSB symbols indicated by *SSB-ToMeasure* and 1 data symbol before each consecutive SSB symbols indicated by *SSB-ToMeasure* and 1 data symbol after each consecutive SSB symbols indicated by *SSB-ToMeasure*, given that *SSB-ToMeasure* is configured, where the *SSB-ToMeasure* is the union set of *SSB-ToMeasure* from all the configured measurement objects merged on the same serving carrier, and,

- not overlapped by the RSSI symbols indicated by *ss-RSSI-Measurement* and 1 data symbol before each RSSI symbol indicated by *ss-RSSI-Measurement* and 1 data symbol after each RSSI symbol indicated by *ss-RSSI-Measurement*, given that *ss-RSSI-Measurement* is configured.

- Psharing factor = 3, otherwise.

- If the higher layer in TS 38.331 [2] signalling of *smtc2*is present, TSMTCperiod follows *smtc2*; Otherwise TSMTCperiod follows *smtc1.* TSMTCperiod is the shortest SMTC period among all CCs in the same FR2 band, provided the SMTC offset of all CCs in FR2 have the same offset.

- When a GAP is configured only and the GAP is not NCSG,

- an RLM-RS resource or an SMTC occasion is considered to be overlapped with the GAP if it overlaps a GAP occasion, and

- xRP = MGRP

- Otherwise, when NCSG is configured,

- an RLM-RS resource or an SMTC occasion is considered to be overlapped with the GAP if

- it overlaps the VIL1 or VIL2 of NCSG, or

- it overlaps the ML of NCSG in FR2, and there exists a target carrier to be measured within NCSG that is intra-frequency carrier or inter-frequency carrier in the same band as the serving cell, or inter-frequency carrier in different band as the serving cell and UE does not support IBM between the target carrier and the serving cell,

- and

- xRP = VIRP

- If the UE is configured with Pre-MG only, an RLM-RS resource or an SMTC occasion is only considered to be overlapped by the Pre-MG if the Pre-MG is activated.

- When concurrent gaps or concurrent measurement gap(s) with Pre-MG(s) or concurrent measurement gap(s) with NCSG(s) are configured, an RLM-RS resource or an SMTC occasion is not considered as overlapped by a GAP occasion if the GAP occasion is dropped according to clause 9.1.8, clause 9.1.12, clause 9.1.13, respectively.

If the higher layer in TS 38.331 [2] signalling of *smtc2*is present, TSMTCperiod follows *smtc2*; Otherwise TSMTCperiod follows *smtc1.*

For UE supporting *measurement gap occasion cancellation*, the UE is not required to perform SSB measurements during the cancelled gap occasions.

Longer evaluation period would be expected if the combination of RLM-RS resource, SMTC occasion and GAP configurations does not meet previous conditions.

When the configured aperiodic MUSIM gap is overlapping with RLM-RS resource occasion, longer evaluation period would be expected.

When UE is configured with MUSIM gap(s), and if RLM-RS resource occasions are fully overlapped with MUSIM gap(s) or the union of MUSIM gap(s) and GAPs, no requirement applies for SSB based RLM.

For either an FR1 or FR2 serving cell, longer evaluation period would be expected during the period Tidentify\_CGI when the UE is requested to decode an NR CGI.

For either an FR1 or FR2 serving cell, longer evaluation period would be expected during the period Tidentify\_CGI,E-UTRAN when the UE is requested to decode an LTE CGI.

Table 8.1.2.2-1: Evaluation period TEvaluate\_out\_SSB and TEvaluate\_in\_SSB for FR1

|  |  |  |
| --- | --- | --- |
| Configuration | TEvaluate\_out\_SSB (ms) | TEvaluate\_in\_SSB (ms) |
| no DRX | Max(200, Ceil(10 × P) × TSSB) | Max(100, Ceil(5 × P) × TSSB) |
| DRX cycle≤320 ms | Max(200, Ceil(15 × P) × Max(TDRX,TSSB)) | Max(100, Ceil(7.5 × P) × Max(TDRX,TSSB)) |
| DRX cycle>320 ms | Ceil(10 × P) × TDRX | Ceil(5 × P) × TDRX |
| NOTE: TSSB is the periodicity of the SSB configured for RLM. TDRX is the DRX cycle length. | | |

Table 8.1.2.2-2: Evaluation period TEvaluate\_out\_SSB and TEvaluate\_in\_SSB for FR2

|  |  |  |
| --- | --- | --- |
| Configuration | TEvaluate\_out\_SSB (ms) | TEvaluate\_in\_SSB (ms) |
| no DRX | Max(200, Ceil(10 × P × N) × TSSB) | Max(100, Ceil(5 × P × N) × TSSB) |
| DRX cycle≤320 ms | Max(200, Ceil(15 × P × N) × Max(TDRX,TSSB)) | Max(100, Ceil(7.5 × P × N) × Max(TDRX,TSSB)) |
| DRX cycle>320 ms | Ceil(10 × P × N) × TDRX | Ceil(5 × P × N) × TDRX |
| NOTE: TSSB is the periodicity of the SSB configured for RLM. TDRX is the DRX cycle length. | | |

**Table 8.1.2.2-3: Evaluation period TEvaluate\_out\_SSB and TEvaluate\_in\_SSB for FR2 power class 6 UE configured with *highSpeedMeasFlagFR2-r17***

|  |  |  |
| --- | --- | --- |
| **Configuration** | **TEvaluate\_out\_SSB (ms)** | **TEvaluate\_in\_SSB (ms)** |
| no DRX | Max(200, Ceil(10 × P × N Note2) × TSSB) | Max(100, Ceil(5 × P × N Note2) × TSSB) |
| DRX cycle≤80 ms | Max(200, Ceil(15 × P × N Note2) × Max(TDRX,TSSB)) | Max(100, Ceil(7.5 × P × N Note2) × Max(TDRX,TSSB)) |
| NOTE 1: TSSB is the periodicity of the SSB configured for RLM. TDRX is the DRX cycle length.  NOTE 2: For a UE not supporting *simultaneousReceptionTwoQCL-r18* or when *highSpeedDeploymentTypeFR2-r17* is not configured as *bi-directional*, scaling factor N=2 when *highSpeedMeasFlagFR2-r17* is configured to set1 and scaling factor N=6 when *highSpeedMeasFlagFR2-r17* is configured to set2. For a UE supporting *simultaneousReceptionTwoQCL-r18* and when *highSpeedDeploymentTypeFR2-r17* is configured as *bidirectional*, scaling factor N=1.5 when *highSpeedMeasFlagFR2-r17* is configured to set1 and scaling factor N=4 when *highSpeedMeasFlagFR2-r17* is configured to set2 | | |

Table 8.1.2.2-4: Evaluation period TEvaluate\_out\_SSB and TEvaluate\_in\_SSB for FR1(deactivated PSCell)

|  |  |  |
| --- | --- | --- |
| Configuration | TEvaluate\_out\_SSB (ms) | TEvaluate\_in\_SSB (ms) |
| no DRX | Ceil(10 × P) × measCyclePSCell | Ceil(5 × P) × measCyclePSCell |
| DRX cycle≤ 320 ms | Ceil(15 × P) × Max(TDRX, measCyclePSCell) | Ceil(7.5 × P) × Max(TDRX, measCyclePSCell) |
| DRX cycle> 320 ms | Ceil(10 × P) × Max(TDRX, measCyclePSCell) | Ceil(5 × P) × Max(TDRX, measCyclePSCell) |
| NOTE: TDRX is the DRX cycle length of SCG. measCyclePSCell is the measurement cycle length of the deactivated PSCell. | | |

Table 8.1.2.2-5: Evaluation period TEvaluate\_out\_SSB and TEvaluate\_in\_SSB for FR2(deactivated PSCell)

|  |  |  |
| --- | --- | --- |
| Configuration | TEvaluate\_out\_SSB (ms) | TEvaluate\_in\_SSB (ms) |
| no DRX | Ceil(10 × P× N) × measCyclePSCell | Ceil(5 × P× N) × measCyclePSCell |
| DRX cycle≤ 320 ms | Ceil(15 × P× N) × Max(TDRX, measCyclePSCell) | Ceil(7.5 × P× N) × Max(TDRX, measCyclePSCell) |
| DRX cycle> 320 ms | Ceil(10 × P× N) × Max(TDRX, measCyclePSCell) | Ceil(5 × P× N) × Max(TDRX, measCyclePSCell) |
| NOTE: TDRX is the DRX cycle length of SCG. measCyclePSCell is the measurement cycle length of the deactivated PSCell. | | |

# <End of Change #2>

# <Start of Change #3>

#### 8.1.3.2 Minimum requirement

UE shall be able to evaluate whether the downlink radio link quality on the configured RLM-RS resource estimated over the last TEvaluate\_out\_CSI-RS period becomes worse than the threshold Qout\_CSI-RS within TEvaluate\_out\_CSI-RS evaluation period.

UE shall be able to evaluate whether the downlink radio link quality on the configured RLM-RS resource estimated over the last TEvaluate\_in\_CSI-RS ms period becomes better than the threshold Qin\_CSI-RS within TEvaluate\_in\_CSI-RS ms evaluation period.

- TEvaluate\_out\_CSI-RS and TEvaluate\_in\_CSI-RS are defined in table 8.1.3.2-1 for FR1.

- TEvaluate\_out\_CSI-RS and TEvaluate\_in\_CSI-RS are defined in table 8.1.3.2-2 for FR2 with scaling factor N=1.

- TEvaluate\_out\_CSI-RS and TEvaluate\_in\_CSI-RS are defined in table 8.1.3.2-3 for FR1 (deactivated PSCell).

- TEvaluate\_out\_CSI-RS and TEvaluate\_in\_CSI-RS are defined in table 8.1.3.2-4 for FR2 (deactivated PSCell) with scaling factor N=1.

The requirements of TEvaluate\_out\_CSI-RS and TEvaluate\_in\_CSI-RS apply provided that the CSI-RS for RLM is not in a resource set configured with repetition ON. The requirements do not apply when the CSI-RS resource in the active TCI state of CORESET is the same CSI-RS resource for RLM and the TCI state information of the CSI-RS resource is not given, wherein the TCI state information means QCL Type-D to SSB for L1-RSRP or CSI-RS with repetition ON.

For a UE supporting *concurrentMeasGapsPreMG-r18* and when concurrent measurement gap(s) with Pre-MG(s) are configured, or a UE supporting *concurrentMeasGapsNCSG-r18* and when concurrent measurement gap(s) with NCSG(s) are configured, or a UE supporting *concurrentMeasGap-r17* or *musim-GapPreference-r17* or both *concurrentMeasGap-r17* and *musim-GapPreference-r17,* and when concurrent measurement gaps or periodic MUSIM gaps or both concurrent GAPs and periodic MUSIM gaps are are configured,

- an RLM-RS resource occasion is not considered to be overlapped by a gap occasion if the gap occasion is dropped according to clauses 9.1.8 and 9.1.10,

- P value for an RLM-RS resource to be measured is defined as

- Ntotal / Noutside\_MG in FR1

- Psharing factor \* Ntotal / Noutside\_MG in FR2 with Navailable = 0

- Ntotal / Navailable in FR2 with Navailable > 0

- For a window W of duration max(TL1, xRP\_max), where xRP\_max is the maximum xRP across all configured per-UE measurement gaps or periodic MUSIM gap(s) or NCSGs and per-FR measurement gaps or NCSGs, and, in case of Pre-MG, all activated per-UE measurement gaps and per-FR measurement gaps, within the same FR as serving cell, and starting at the beginning of any RLM-RS resource occasion:

- Ntotal is the total number of RLM-RS resource occasions within the window W, including those overlapped with GAP occasions, MUSIM gap occasions or SMTC occasions within the window W, and

- Noutside\_MG is the number of RLM-RS resource occasions that are not overlapped with any non-dropped GAP occasion nor non-dropped MUSIM gap occasion within the window W, and

- Navailable is the number of RLM-RS resource occasions that are not overlapped with any non-dropped GAP occasion, nor non-dropped MUSIM gap occasion, nor any SMTC occasion within the window W, and

- an RLM-RS resource occasion is considered to be overlapped with the MUSIM gap if it overlaps a MUSIM gap occasion, and

- TL1 is periodicity of the target RLM-RS.

- xRP = MGRP when configured GAP is activated Pre-MG or MG, and xRP = VIRP when configured GAP is NCSG.

Otherwise, for a UE neither supporting *concurrentMeasGap-r17* nor *concurrentMeasGapsPreMG-r18* nor *concurrentMeasGapsNCSG-r18* nor supporting *musim-GapPreference-r17* or when neither of the above configurations applies, i.e. concurrent measurement gaps, concurrent measurement gap(s) with Pre-MG(s), concurrent measurement gap(s) with NCSG(s), and periodic MUSIM gaps,

For FR1,

- , when in the monitored cell there are GAPs configured for intra-frequency, inter-frequency or inter-RAT measurements, and these GAPs] are overlapping with some but not all occasions of the CSI-RS; and

- P=1 when in the monitored cell there are no GAPs overlapping with any occasion of the CSI-RS.

For FR2,

- P=1, when the RLM-RS resource is not overlapped with measurement gap and also not overlapped with SMTC occasion.

- , when the RLM-RS resource is partially overlapped with GAP and the RLM-RS resource is not overlapped with SMTC occasion (TCSI-RS < xRP)

- , when the RLM-RS resource is not overlapped with GAP and the RLM-RS resource is partially overlapped with SMTC occasion (TCSI-RS < TSMTCperiod).

- P = Psharing factor, when the RLM-RS resource is not overlapped with GAP and RLM-RS resource is fully overlapped with SMTC occasion (TCSI-RS = TSMTCperiod).

- , when the RLM-RS resource is partially overlapped with GAP and the RLM-RS resource is partially overlapped with SMTC occasion (TCSI-RS < TSMTCperiod) and SMTC occasion is not overlapped with GAP and

- TSMTCperiod ≠ xRP or

- TSMTCperiod = xRP and TCSI-RS < 0.5 × TSMTCperiod

- , when the RLM-RS resource is partially overlapped with GAP and the RLM-RS resource is partially overlapped with SMTC occasion (TCSI-RS < TSMTCperiod) and SMTC occasion is not overlapped with GAP and TSMTCperiod = xRP and TCSI-RS = 0.5 × TSMTCperiod

- , when the RLM-RS resource is partially overlapped with GAP and the RLM-RS resource is partially overlapped with SMTC occasion (TCSI-RS < TSMTCperiod) and SMTC occasion is partially or fully overlapped with GAP

- , when the RLM-RS resource is partially overlapped with GAP and the RLM-RS resource is fully overlapped with SMTC occasion (TCSI-RS = TSMTCperiod) and SMTC occasion is partially overlapped with GAP (TSMTCperiod < xRP)

where,

- Psharing factor = 1, if the RLM-RS resource outside GAP is

- not overlapped with the SSB symbols indicated by *SSB-ToMeasure* and 1 data symbol before each consecutive SSB symbols indicated by *SSB-ToMeasure* and 1 data symbol after each consecutive SSB symbols indicated by *SSB-ToMeasure*, given that *SSB-ToMeasure* is configured, where the *SSB-ToMeasure* is the union set of *SSB-ToMeasure* from all the configured measurement objects merged on the same serving carrier, and,

- not overlapped by the RSSI symbols indicated by *ss-RSSI-Measurement* and 1 data symbol before each RSSI symbol indicated by *ss-RSSI-Measurement* and 1 data symbol after each RSSI symbol indicated by *ss-RSSI-Measurement*, given that *ss-RSSI-Measurement* is configured.

- Psharing factor = 3, otherwise.

- If the higher layer in TS 38.331 [2] signalling of *smtc2*is present, TSMTCperiod follows *smtc2*; Otherwise TSMTCperiod follows *smtc1.* TSMTCperiod is the shortest SMTC period among all CCs in the same FR2 band, provided the SMTC offset of all CCs in FR2 have the same offset.

- When a GAP is configured only and the GAP is not NCSG,

- an RLM-RS resource or an SMTC occasion is considered to be overlapped with the GAP if it overlaps a GAP occasion, and

- xRP = MGRP

- Otherwise, when NCSG is configured,

- an RLM-RS resource or an SMTC occasion is considered to be overlapped with the GAP if

- it overlaps the VIL1 or VIL2 of NCSG, or

- it overlaps the ML of NCSG in FR2, and there exists a target carrier to be measured within NCSG that is intra-frequency carrier or inter-frequency carrier in the same band as the serving cell, or inter-frequency carrier in different band as the serving cell and UE does not support IBM between the target carrier and the serving cell,

- and

- xRP = VIRP

If the UE is configured with Pre-MG only, an RLM-RS resource or an SMTC occasion is only considered to be overlapped by the Pre-MG if the Pre-MG is activated.

When concurrent gaps or concurrent measurement gap(s) with Pre-MG(s) or concurrent measurement gap(s) with NCSG(s) are configured , an RLM-RS resource or an SMTC occasion is not considered to be overlapped by a GAP occasion if the GAP occasion is dropped according to clause 9.1.8, clause 9.1.12, clause 9.1.13, respectively.

If the higher layer in TS 38.331 [2] signalling of *smtc2*is present, TSMTCperiod follows *smtc2*; Otherwise TSMTCperiod follows *smtc1.*

NOTE: The overlap between CSI-RS for RLM and SMTC means that CSI-RS based RLM is within the SMTC window duration.

For UE supporting *measurement gap occasion cancellation*, the UE is not required to perform CSI-RS measurements during the cancelled gap occasions.

Longer evaluation period would be expected if the combination of RLM-RS resource, SMTC occasion and GAP configurations does not meet previous conditions.

When the configured aperiodic MUSIM gap is overlapping with RLM-RS resource occasion, longer evaluation period would be expected.

When UE is configured with MUSIM gap(s), and if RLM-RS resource occasions are fully overlapped with MUSIM gap(s) or the union of MUSIM gap(s) and GAPs, no requirement applies for CSI-RS based RLM.

For either an FR1 or FR2 serving cell, longer evaluation period would be expected during the period Tidentify\_CGI when the UE is requested to decode an NR CGI.

For either an FR1 or FR2 serving cell, longer evaluation period would be expected during the period Tidentify\_CGI,E-UTRAN when the UE is requested to decode an LTE CGI.

The values of Mout and Min used in table 8.1.3.2-1, table 8.1.3.2-2, table 8.1.3.2-3 and table 8.1.3.2-4 are defined as:

- Mout = 20 and Min = 10, if the CSI-RS resource configured for RLM is transmitted with higher layer CSI-RS parameter *density* [6, clause 7.4.1] set to 3 and over the bandwidth ≥ 24 PRBs.

Table 8.1.3.2-1: Evaluation period TEvaluate\_out\_CSI-RS and TEvaluate\_in\_CSI-RS for FR1

|  |  |  |
| --- | --- | --- |
| Configuration | TEvaluate\_out\_CSI-RS (ms) | TEvaluate\_in\_CSI-RS (ms) |
| no DRX | Max(200, Ceil(Mout×P)×TCSI-RS) | Max(100, Ceil(Min×P) × TCSI-RS) |
| DRX ≤ 320 ms | Max(200, Ceil(1.5×Mout×P)× Max(TDRX, TCSI-RS)) | Max(100, Ceil(1.5×Min×P)× Max(TDRX, TCSI-RS)) |
| DRX > 320 ms | Ceil(Mout×P) × TDRX | Ceil(Min×P) × TDRX |
| NOTE: TCSI-RS is the periodicity of the CSI-RS resource configured for RLM. The requirements in this table apply for TCSI-RS equal to 5 ms, 10 ms, 20 ms or 40 ms. TDRX is the DRX cycle length. | | |

Table 8.1.3.2-2: Evaluation period TEvaluate\_out\_CSI-RS and TEvaluate\_in\_CSI-RS for FR2

|  |  |  |
| --- | --- | --- |
| Configuration | TEvaluate\_out\_CSI-RS (ms) | TEvaluate\_in\_CSI-RS (ms) |
| no DRX | Max(200, Ceil(Mout×P×N)×TCSI-RS) | Max(100, Ceil(Min×P×N) × TCSI-RS) |
| DRX ≤ 320 ms | Max(200, Ceil(1.5×Mout×P×N)× Max(TDRX, TCSI-RS)) | Max(100, Ceil(1.5×Min×P×N)× Max(TDRX, TCSI-RS)) |
| DRX > 320 ms | Ceil(Mout×P×N) × TDRX | Ceil(Min×P×N) × TDRX |
| NOTE: TCSI-RS is the periodicity of the CSI-RS resource configured for RLM. The requirements in this table apply for TCSI-RS equal to 5 ms, 10 ms, 20 ms or 40 ms. TDRX is the DRX cycle length. | | |

Table 8.1.3.2-3: Evaluation period TEvaluate\_out\_CSI-RS and TEvaluate\_in\_CSI-RS for FR1 (deactivated PSCell)

|  |  |  |
| --- | --- | --- |
| Configuration | TEvaluate\_out\_CSI-RS (ms) | TEvaluate\_in\_CSI-RS (ms) |
| no DRX | Ceil(Mout×P) × measCyclePSCell | Ceil(Min×P) × measCyclePSCell |
| DRX ≤ 320 ms | Ceil(1.5 ×Mout×P) × Max(TDRX, measCyclePSCell) | Ceil(1.5 ×Min×P) × Max(TDRX, measCyclePSCell) |
| DRX > 320 ms | Ceil(Mout×P) × Max(TDRX, measCyclePSCell) | Ceil(Min×P) × Max(TDRX, measCyclePSCell) |
| NOTE: TDRX is the DRX cycle length of SCG. measCyclePSCell is the measurement cycle length of the deactivated PSCell. | | |

Table 8.1.3.2-4: Evaluation period TEvaluate\_out\_CSI-RS and TEvaluate\_in\_CSI-RS for FR2 (deactivated PSCell)

|  |  |  |
| --- | --- | --- |
| Configuration | TEvaluate\_out\_CSI-RS (ms) | TEvaluate\_in\_CSI-RS (ms) |
| no DRX | Ceil(Mout×P×N) × measCyclePSCell | Ceil(Min×P×N) × measCyclePSCell |
| DRX ≤ 320 ms | Ceil(1.5 × Mout×P×N) × Max(TDRX, measCyclePSCell) | Ceil(1.5 × Min×P×N) × Max(TDRX, measCyclePSCell) |
| DRX > 320 ms | Ceil(Mout×P×N) × Max(TDRX, measCyclePSCell) | Ceil(Min×P×N) × Max(TDRX, measCyclePSCell) |
| NOTE: TDRX is the DRX cycle length of SCG. measCyclePSCell is the measurement cycle length of the deactivated PSCell. | | |

# <End of Change #3>

# <Start of Change #4>

#### 8.5.2.2 Minimum requirement

UE shall be able to evaluate whether the downlink radio link quality on the configured SSB resource in set estimated over the last TEvaluate\_BFD\_SSB period becomes worse than the threshold Qout\_LR\_SSB within TEvaluate\_BFD\_SSB period.

The value of TEvaluate\_BFD\_SSB is defined in table 8.5.2.2-1 or table 8.5.2.2-4 (deactivated PSCell) for FR1.

The value of TEvaluate\_BFD\_SSB is defined in table 8.5.2.2-2 or table 8.5.2.2-5 (deactivated PSCell) for FR2 with scaling factor N, where

- N = 2, 4 or 6 for serving cell in FR2-1 for UE supporting *fastBeamSweepingMultiRx-r18* according to the conditions in clause 3.6.19,

- N=8 for other cases in FR2-1, and

- N=12 for FR2-2,

for FR2 power classes other than power class 6 or for FR2 power class 6 when *highSpeedMeasFlagFR2-r17* is not configured.

The value of TEvaluate\_BFD\_SSB is defined in table 8.5.2.2-5 (deactivated PSCell) for FR2 with scaling factor N=8 for FR2-1 and N=12 for FR2-2, for FR2 power classes other than power class 6 or for FR2 class 6 when *highSpeedMeasFlagFR2-r17* is not configured.

The value of TEvaluate\_BFD\_SSB is defined in table 8.5.2.2-3 for FR2 power class 6 UE configured with *highSpeedMeasFlagFR2-r17*.

For a UE supporting [*support for Case 1 requirements*] and when concurrent measurement gap(s) with Pre-MG(s) are configured, or a UE supporting [*support for Case 2 requirements*] and when concurrent measurement gap(s) with NCSG(s) are configured, or a UE supporting *concurrentMeasGap-r17* or *[musim-GapPreference-r17]* or both *concurrentMeasGap-r17* and *[musim-GapPreference-r17],* and when concurrent gaps or periodic MUSIM gaps or both concurrent GAPs and periodic MUSIM gaps are configured,

- an SSB resource occasion for beam failure detection is not considered to be overlapped by a gap occasion if the gap occasion is dropped according to clauses 9.1.8 and 9.1.10,

- P value for a BFD-RS resource to be measured is defined as

- Ntotal / Noutside\_MG in FR1

- Psharing factor \* Ntotal / Noutside\_MG in FR2 with Navailable = 0

- Ntotal / Navailable in FR2 with Navailable> 0

- For a window W of duration max(TL1, xRP\_max), where xRP\_max is the maximum xRP across all configured per-UE measurement gaps or periodic MUSIM gap(s) or NCSGs and per-FR measurement gaps or NCSGs, and, in case of Pre-MG, all activated per-UE measurement gaps and per-FR measurement gaps, within the same FR as serving cell, and starting at the beginning of any BFD-RS resource occasion:

- Ntotal is the total number of BFD-RS resource occasions within the window W, including those overlapped with GAP occasions, MUSIM gap occasions or SMTC occasions within the window W, and

- Noutside\_MG is the number of BFD-RS resource occasions that are not overlapped with any non-dropped GAP occasion nor non-dropped MUSIM gap occasion within the window W, and

- Navailable is the number of BFD-RS resource occasions that are not overlapped with any non-dropped GAP occasion nor non-dropped MUSIM gap occasion nor any SMTC occasion within the window W, and

- an SSB resource occasion for beam failure detection is considered to be overlapped with the MUSIM gap if it overlaps a MUSIM gap occasion, and- TL1 is periodicity of the target BFD-RS.

- xRP = MGRP when configured GAP is activated Pre-MG or MG, and xRP = VIRP when configured GAP is NCSG.

Otherwise, for a UE neither supporting *concurrentMeasGap-r17* nor *[support for Case 1 requirements]* nor *[support for Case 2 requirements]* nor supporting *[musim-GapPreference-r17]* or when neither of the above configurations applies, i.e. concurrent measurement gaps, concurrent measurement gap(s) with Pre-MG(s) and concurrent measurement gap(s) with NCSG(s), and periodic MUSIM gaps,

For FR1,

- , when in the monitored cell there are GAPs configured for intra-frequency, inter-frequency or inter-RAT measurements, which are overlapping with some but not all occasions of the SSB.

- P=1 when in the monitored cell there are no GAPs overlapping with any occasion of the SSB.

For FR2

- , when BFD-RS resource is not overlapped with GAPs and the BFD-RS resource is partially overlapped with SMTC occasion (TSSB < TSMTCperiod).

- P = Psharing factor, when the BFD-RS resource is not overlapped with GAP and the BFD-RS resource is fully overlapped with SMTC occasion (TSSB = TSMTCperiod).

- , when the BFD-RS resource is partially overlapped with GAP and the BFD-RS resource is partially overlapped with SMTC occasion (TSSB < TSMTCperiod) and SMTC occasion is not overlapped with GAP and

- TSMTCperiod ≠ xRP or

- TSMTCperiod = xRP and TSSB < 0.5\*TSMTCperiod

- , when the BFD-RS resource is partially overlapped with GAP and the BFD-RS resource is partially overlapped with SMTC occasion (TSSB < TSMTCperiod) and SMTC occasion is not overlapped with GAP and TSMTCperiod = xRP and TSSB = 0.5\*TSMTCperiod

- , when the BFD-RS resource is partially overlapped with GAP (TSSB <xRP) and the BFD-RS resource is partially overlapped with SMTC occasion (TSSB < TSMTCperiod) and SMTC occasion is partially or fully overlapped with GAP.

- , when the BFD-RS resource is partially overlapped with GAP and the BFD-RS resource is fully overlapped with SMTC occasion (TSSB = TSMTCperiod) and SMTC occasion is partially overlapped with GAP (TSMTCperiod < xRP)

where,

- Psharing factor = 1, if the BFD-RS resource outside GAP is

- not overlapped with the SSB symbols indicated by *SSB-ToMeasure* and 1 data symbol before each consecutive SSB symbols indicated by *SSB-ToMeasure* and 1 data symbol after each consecutive SSB symbols indicated by *SSB-ToMeasure*, given that *SSB-ToMeasure* is configured, where the *SSB-ToMeasure* is the union set of *SSB-ToMeasure* from all the configured measurement objects merged on the same serving carrier, and,

- not overlapped by the RSSI symbols indicated by *ss-RSSI-Measurement* and 1 data symbol before each RSSI symbol indicated by *ss-RSSI-Measurement* and 1 data symbol after each RSSI symbol indicated by *ss-RSSI-Measurement*, given that *ss-RSSI-Measurement* is configured.

- Psharing factor = 3, otherwise.

- If the higher layer in TS 38.331 [2] signalling of *smtc2* is configured, TSMTCperiod corresponds to the value of higher layer parameter *smtc2*; Otherwise TSMTCperiod corresponds to the value of higher layer parameter *smtc1*. TSMTCperiod is the shortest SMTC period among all CCs in the same FR2 band, given the SMTC offset of all CCs in FR2 provided the same offset.

- When a GAP is configured only and the GAP is not NCSG,

- a BFD-RS resource or an SMTC occasion is considered to be overlapped with the GAP if it overlaps a GAP occasion, and

- xRP = MGRP

- Otherwise, when NCSG only is configured,

- a BFD-RS resource or an SMTC occasion is considered to be overlapped with the GAP if

- it overlaps the VIL1 or VIL2 of NCSG, or

it overlaps the ML of NCSG in FR2, and there exists a target carrier to be measured within NCSG that is intra-frequency carrier or inter-frequency carrier in the same band as the serving cell, or inter-frequency carrier in different band as the serving cell and UE does not support IBM between the target carrier and the serving cell,

- and

- xRP = VIRP

- If the UE is configured with Pre-MG only, a BFD-RS resource or an SMTC occasion is only considered to be overlapped by the Pre-MG if the Pre-MG is activated.

- When concurrent gaps or concurrent measurement gap(s) with Pre-MG(s) or concurrent measurement gap(s) with NCSG(s) are configured, a BFD-RS resource or an SMTC occasion is not considered to be overlapped by a GAP occasion if the GAP occasion is dropped according to clause 9.1.8, clause 9.1.12, clause 9.1.13, respectively.

For UE supporting *measurement gap occasion cancellation*, the UE is not required to perform SSB measurements during the cancelled gap occasions.

Longer evaluation period would be expected if the combination of BFD-RS resource, SMTC occasion and GAP configurations does not meet previous conditionsFor either an FR1 or FR2 serving cell, longer evaluation period would be expected during the period Tidentify\_CGI when the UE is requested to decode an NR CGI.

When the configured aperiodic MUSIM gap is overlapping with SSB resource occasion for beam failure detection, longer evaluation period would be expected.

When UE is configured with MUSIM gap(s), and if SSB resource occasions for beam failure detection are fully overlapped with MUSIM gap(s), or the union of MUSIM gap(s) and GAPs, no requirement applies for SSB based beam failure detection.

For either an FR1 or FR2 serving cell, longer BFD evaluation period would be expected during the period Tidentify\_CGI,E-UTRAN when the UE is requested to decode an LTE CGI.

Table 8.5.2.2-1: Evaluation period TEvaluate\_BFD\_SSB for FR1

|  |  |
| --- | --- |
| Configuration | TEvaluate\_BFD\_SSB (ms) |
| no DRX | Max(50, Ceil(5 × P) × TSSB) |
| DRX cycle ≤ 320 ms | Max(50, Ceil(7.5 × P) × Max(TDRX,TSSB)) |
| DRX cycle > 320 ms | Ceil(5 × P) × TDRX |
| NOTE: TSSB is the periodicity of SSB in the set . TDRX is the DRX cycle length. | |

Table 8.5.2.2-2: Evaluation period TEvaluate\_BFD\_SSB for FR2

|  |  |
| --- | --- |
| Configuration | TEvaluate\_BFD\_SSB (ms) |
| no DRX | Max(50, Ceil(5 × P × N) × TSSB) |
| DRX cycle ≤ 320 ms | Max(50, Ceil(7.5 × P × N) × Max(TDRX,TSSB)) |
| DRX cycle > 320 ms | Ceil(5 × P × N) × TDRX |
| NOTE: TSSB is the periodicity of SSB in the set . TDRX is the DRX cycle length. | |

**Table 8.5.2.2-3: Evaluation period TEvaluate\_BFD\_SSB for FR2 power class 6 UE configured with *highSpeedMeasFlagFR2-r17***

|  |  |
| --- | --- |
| **Configuration** | **TEvaluate\_BFD\_SSB (ms)** |
| no DRX | Max(50, Ceil(5 × P × N Note2) × TSSB) |
| DRX cycle ≤ 80 ms | Max(50, Ceil(7.5 × P × N Note2) × Max(TDRX,TSSB)) |
| Note 1: TSSB is the periodicity of SSB in the set . TDRX is the DRX cycle length.  Note 2: scaling factor N=2 when *highSpeedMeasFlagFR2-r17* is configured to set1 or scaling factor N=6 when *highSpeedMeasFlagFR2-r17* is configured to set2, if UE is not supporting *simultaneousReceptionTwoQCL-r18* or when *highSpeedDeploymentTypeFR2-r17* is not configured as bidirectional; Scaling factor N=1.5 when *highSpeedMeasFlagFR2-r17* is configured to set1 or scaling factor N=4 when *highSpeedMeasFlagFR2-r17* is configured to set2, if UE is supporting *simultaneousReceptionTwoQCL-r18* and when *highSpeedDeploymentTypeFR2-r17* is configured as bidirectional. | |

Table 8.5.2.2-4: Evaluation period TEvaluate\_BFD\_SSB for deactivated PSCell in FR1

|  |  |
| --- | --- |
| Configuration | TEvaluate\_BFD\_SSB (ms) |
| no DRX | Ceil(5 × P) × measCyclePscell |
| DRX cycle ≤ 320 ms | Ceil(7.5 × P) × Max(measCyclePscell, TDRX) |
| DRX cycle > 320 ms | Ceil(5 × P) × Max(measCyclePscell, TDRX) |
| NOTE: DRX cycle is the configured DRX cycle of the PSCell. measCyclePSCell is the measurement cycle length of the deactivated PSCell. | |

Table 8.5.2.2-5: Evaluation period TEvaluate\_BFD\_SSB for deactivated PSCell in FR2

|  |  |
| --- | --- |
| Configuration | TEvaluate\_BFD\_SSB (ms) |
| no DRX | Ceil(5 × P × N) × measCyclePscell |
| DRX cycle ≤ 320 ms | Ceil(7.5 × P × N) × Max(measCyclePscell, TDRX) |
| DRX cycle > 320 ms | Ceil(5 × P × N) × Max(measCyclePscell, TDRX) |
| NOTE: DRX cycle is the configured DRX cycle of the PSCell. measCyclePSCell is the measurement cycle length of the deactivated PSCell. | |

# <End of Change #4>

# <Start of Change #5>

#### 8.5.3.2 Minimum requirement

UE shall be able to evaluate whether the downlink radio link quality on the CSI-RS resource in set estimated over the last TEvaluate\_BFD\_CSI-RS period becomes worse than the threshold Qout\_LR\_CSI-RS within TEvaluate\_BFD\_CSI-RS period.

The value of TEvaluate\_BFD\_CSI-RS is defined in table 8.5.3.2-1 or table 8.5.3.2-3 (deactivated PSCell) for FR1.

The value of TEvaluate\_BFD\_CSI-RS is defined in table 8.5.3.2-2 or table 8.5.3.2-4 (deactivated PSCell) for FR2 with N=1. The requirements of TEvaluate\_BFD\_CSI-RS apply provided that the CSI-RS for BFD is not in a resource set configured with repetition ON. The requirements shall not apply when the CSI-RS resource in the active TCI state of CORESET is the same CSI-RS resource for BFD and the TCI state information of the CSI-RS resource is not given, wherein the TCI state information means QCL Type-D to SSB for L1-RSRP or CSI-RS with repetition ON.

- For a UE supporting *concurrentMeasGapsPreMG-r18* and when concurrent measurement gap(s) with Pre-MG(s) are configured, or a UE supporting *concurrentMeasGapsNCSG-r18* and when concurrent measurement gap(s) with NCSG(s) are configured, or a UE supporting *concurrentMeasGap-r17* or *[musim-GapPreference-r17]* or both *concurrentMeasGap-r17* and *musim-GapPreference-r17,* and when concurrent gaps or periodic MUSIM gaps or both concurrent GAPs and periodic MUSIM gaps are configured,

- an CSI-RS resource occasion for beam failure detection is not considered to be overlapped by a gap occasion if the gap occasion is dropped according to clause 9.1.8 and 9.1.10,

- P value for a BFD-RS resource to be measured is defined as

- Ntotal / Noutside\_MG in FR1

- Psharing factor \* Ntotal / Noutside\_MG in FR2 with Navailable = 0

- Ntotal / Navailable in FR2 with Navailable> 0

- For a window W of duration max(TL1, xRP\_max), where xRP\_max is the maximum xRP across all configured per-UE measurement gaps or MUSIM gap(s) or NCSGs and per-FR measurement gaps or NCSGs, and, in case of Pre-MG, all activated per-UE measurement gaps and per-FR measurement gaps, within the same FR as serving cell, and starting at the beginning of any BFD-RS resource occasion:

- Ntotal is the total number of BFD-RS resource occasions within the window W, including those overlapped with GAP occasions, MUSIM gap occasions or SMTC occasions within the window W, and

- Noutside\_MG is the number of BFD-RS resource occasions that are not overlapped with any non-dropped GAP occasion nor non-dropped MUSIM gap occasion within the window W, and

- Navailable is the number of BFD-RS resource occasions that are not overlapped with any non-dropped GAP occasion nor non-dropped MUSIM gap occasion nor any SMTC occasion within the window W, and

- an CSI-RS resource occasion for beam failure detection is considered to be overlapped with the MUSIM gap if it overlaps a MUSIM gap occasion, and

TL1 is periodicity of the target BFD-RS.

- xRP = MGRP when configured GAP is activated Pre-MG or MG, and xRP = VIRP when configured GAP is NCSG.

Otherwise, for a UE neither supporting *concurrentMeasGap-r17* nor *concurrentMeasGapsPreMG-r18* nor *concurrentMeasGapsNCSG-r18* nor supporting *musim-GapPreference-r17* or when neither of the above configurations applies, i.e. concurrent measurement gaps, concurrent measurement gap(s) with Pre-MG(s) and concurrent measurement gap(s) with NCSG(s), and periodic MUSIM gaps,For FR1,

For FR1,

- , when in the monitored cell there are GAPs configured for intra-frequency, inter-frequency or inter-RAT measurements, which are overlapping with some but not all occasions of the CSI-RS.

- P = 1 when in the monitored cell there are no GAPs overlapping with any occasion of the CSI-RS.

For FR2,

- P = 1, when the BFD-RS resource is not overlapped with GAP and also not overlapped with SMTC occasion.

- , when the BFD-RS resource is partially overlapped with GAP and the BFD-RS resource is not overlapped with SMTC occasion (TCSI-RS < xRP)

- , when the BFD-RS resource is not overlapped with GAP and the BFD-RS resource is partially overlapped with SMTC occasion (TCSI-RS < TSMTCperiod).

- P = Psharing factor, when the BFD-RS resource is not overlapped with GAP and the BFD-RS resource is fully overlapped with SMTC occasion (TCSI-RS = TSMTCperiod).

- , when the BFD-RS resource is partially overlapped with GAP and the BFD-RS resource is partially overlapped with SMTC occasion (TCSI-RS < TSMTCperiod) and SMTC occasion is not overlapped with GAP and

- TSMTCperiod ≠ xRP or

- TSMTCperiod = xRP and TCSI-RS < 0.5 × TSMTCperiod

- , when the BFD-RS resource is partially overlapped with GAP and the BFD-RS resource is partially overlapped with SMTC occasion (TCSI-RS < TSMTCperiod) and SMTC occasion is not overlapped with GAP and TSMTCperiod = xRP and TCSI-RS = 0.5 × TSMTCperiod

- , when the BFD-RS resource is partially overlapped with GAP (TCSI-RS < xRP) and the BFD-RS resource is partially overlapped with SMTC occasion (TCSI-RS < TSMTCperiod) and SMTC occasion is partially or fully overlapped with GAP.

- , when the BFD-RS resource is partially overlapped with GAP and the BFD-RS resource is fully overlapped with SMTC occasion (TCSI-RS = TSMTCperiod) and SMTC occasion is partially overlapped with GAP (TSMTCperiod < xRP)

where,

- Psharing factor = 1, if the BFD-RS resource outside gap is

- not overlapped with the SSB symbols indicated by *SSB-ToMeasure* and 1 data symbol before each consecutive SSB symbols indicated by *SSB-ToMeasure* and 1 data symbol after each consecutive SSB symbols indicated by *SSB-ToMeasure*, given that *SSB-ToMeasure* is configured, where the *SSB-ToMeasure* is the union set of *SSB-ToMeasure* from all the configured measurement objects merged on the same serving carrier, and,

- not overlapped by the RSSI symbols indicated by *ss-RSSI-Measurement* and 1 data symbol before each RSSI symbol indicated by *ss-RSSI-Measurement* and 1 data symbol after each RSSI symbol indicated by *ss-RSSI-Measurement*, given that *ss-RSSI-Measurement* is configured.

- Psharing factor = 3, otherwise.

- If the higher layer in TS 38.331 [2] signalling of *smtc2* is configured, TSMTCperiod corresponds to the value of higher layer parameter *smtc2*; Otherwise TSMTCperiod corresponds to the value of higher layer parameter *smtc1*. TSMTCperiod is the shortest SMTC period among all CCs in the same FR2 band, provided the SMTC offset of all CCs in FR2 have the same offset.

- When a GAP is configured only and the GAP is not NCSG,

- a BFD-RS resource or an SMTC occasion is considered to be overlapped with the GAP if it overlaps a GAP occasion, and

- xRP = MGRP

- Otherwise, when NCSG GAP only is configured,

- a BFD-RS resource or an SMTC occasion is considered to be overlapped with the GAP if

- it overlaps the VIL1 or VIL2 of NCSG, or

- it overlaps the ML of NCSG in FR2, and there exists a target carrier to be measured within NCSG that is intra-frequency carrier or inter-frequency carrier in the same band as the serving cell, or inter-frequency carrier in different band as the serving cell and UE does not support IBM between the target carrier and the serving cell,

- and

- xRP = VIRP

- If the UE is configured with Pre-MG only, a BFD-RS resource or an SMTC occasion is only considered to be overlapped by the Pre-MG if the Pre-MG is activated.

- When concurrent gaps or concurrent measurement gap(s) with Pre-MG(s) or concurrent measurement gap(s) with NCSG(s) are configured, a BFD-RS resource or an SMTC occasion is not considered to be overlapped by a GAP occasion if the GAP occasion is dropped according to clause 9.1.8, clause 9.1.12, clause 9.1.13, respectively.

NOTE: The overlap between CSI-RS for BFD and SMTC means that CSI-RS for BFD is within the SMTC window duration.

For UE supporting *measurement gap occasion cancellation*, the UE is not required to perform CSI-RS measurements during the cancelled gap occasions.

Longer evaluation period would be expected if the combination of the BFD-RS resource, SMTC occasion and GAP configurations does not meet previous conditions.

For either an FR1 or FR2 serving cell, longer evaluation period would be expected during the period Tidentify\_CGI when the UE is requested to decode an NR CGI.

When the configured aperiodic MUSIM gap is overlapping with CSI-RS resource occasion for beam failure detection, longer evaluation period would be expected.

When UE is configured with MUSIM gap(s), and if CSI-RS resource occasions for beam failure detection are fully overlapped with MUSIM gap(s), or the union of MUSIM gap(s) and GAPs, no requirement applies for CSI-RS based beam failure detection.

For either an FR1 or FR2 serving cell, longer BFD evaluation period would be expected during the period Tidentify\_CGI,E-UTRAN when the UE is requested to decode an LTE CGI.

The values of MBFD used in table 8.5.3.2-1 and table 8.5.3.2-2 are defined as

- MBFD = 10, if the CSI-RS resource(s) in set  used for BFD is transmitted with Density = 3 and over the bandwidth ≥ 24 PRBs.

The values of PBFD used in table 8.5.3.2-1 and table 8.5.3.2-2 are defined as

For each CSI-RS resource in the set  configured for PCell or PSCell in EN-DC or NE-DC or SA; or PCell in NR-DC

- PBFD = 1.

For each CSI-RS resource in the set  configured for PSCell in NR-DC

- PBFD = 2 if UE is configured for beam failure detection on SCell, 1 otherwise.

For each CSI-RS resource in the set  configured for a SCell

- PBFD = Z in EN-DC or NE-DC or SA.

- PBFD = 2\* Z in NR-DC.

- Where Z is the number of band(s) on which UE is performing beam failure detection only for SCell.

Table 8.5.3.2-1: Evaluation period TEvaluate\_BFD\_CSI-RS for FR1

|  |  |
| --- | --- |
| Configuration | TEvaluate\_BFD\_CSI-RS (ms) |
| no DRX | Max(50, Ceil(MBFD × P × PBFD) × TCSI-RS) |
| DRX cycle ≤ 320 ms | Max(50, Ceil(1.5 × MBFD × P × PBFD) × Max(TDRX, TCSI-RS)) |
| DRX cycle > 320 ms | Ceil(MBFD × P × PBFD) × TDRX |
| NOTE: TCSI-RS is the periodicity of CSI-RS resource in the set . TDRX is the DRX cycle length. | |

Table 8.5.3.2-2: Evaluation period TEvaluate\_BFD\_CSI-RS for FR2

|  |  |
| --- | --- |
| Configuration | TEvaluate\_BFD\_CSI-RS (ms) |
| no DRX | Max(50, Ceil(MBFD × P × N × PBFD) × TCSI-RS) |
| DRX cycle ≤ 320 ms | Max(50, Ceil(1.5 × MBFD × P × N × PBFD) × Max(TDRX, TCSI-RS)) |
| DRX cycle > 320 ms | Ceil(MBFD × P × N × PBFD) × TDRX |
| NOTE: TCSI-RS is the periodicity of CSI-RS resource in the set . TDRX is the DRX cycle length. | |

Table 8.5.3.2-3: Evaluation period TEvaluate\_BFD\_CSI-RS for deactivated PSCell in FR1

|  |  |
| --- | --- |
| **Configuration** | **TEvaluate\_BFD\_CSI-RS (ms)** |
| no DRX | Ceil(MBFD × P × PBFD) × measCyclePscell |
| DRX cycle ≤ 320 ms | Ceil(1.5 × MBFD × P × PBFD) × Max(TDRX, measCyclePscell) |
| DRX cycle > 320 ms | Ceil(MBFD × P × PBFD) × Max(TDRX, measCyclePscell) |
| NOTE: DRX cycle is the configured DRX cycle of the PSCell. measCyclePSCell is the measurement cycle length of the deactivated PSCell. | |

Table 8.5.3.2-4: Evaluation period TEvaluate\_BFD\_CSI-RS for deactivated PSCell in FR2

|  |  |
| --- | --- |
| **Configuration** | **TEvaluate\_BFD\_CSI-RS (ms)** |
| no DRX | Ceil(MBFD × P × N × PBFD) × measCyclePscell |
| DRX cycle ≤ 320 ms | Ceil(1.5 × MBFD × P × N × PBFD) × Max(TDRX, measCyclePscell) |
| DRX cycle > 320 ms | Ceil(MBFD × P × N × PBFD) × Max(TDRX, measCyclePscell) |
| NOTE: DRX cycle is the configured DRX cycle of the PSCell. measCyclePSCell is the measurement cycle length of the deactivated PSCell. | |

# <End of Change #5>

# <Start of Change #6>

### 9.5.4 L1-RSRP measurement requirements

#### 9.5.4.1 SSB based L1-RSRP Reporting

When *groupBasedBeamReporting-r17* is not configured, the UE shall be capable of performing L1-RSRP measurements based on the configured SSB resource for L1-RSRP computation, and the UE physical layer shall be capable of reporting L1-RSRP measured over the measurement period of TL1-RSRP\_Measurement\_Period\_SSB.

When *groupBasedBeamReporting-r17* is configured, the UE shall be capable of performing L1-RSRP measurements based on the two configured SSB resource sets for L1-RSRP, and the UE physical layer shall be capable of reporting group-based L1-RSRP measured over the measurement period of TL1-RSRP\_Measurement\_Period\_SSB.

When there is no L1-RSRP measurement on LTM neighbor cell(s) to measure within active BWP, the value of TL1-RSRP\_Measurement\_Period\_SSB is defined in table 9.5.4.1-1 for FR1, the value of TL1-RSRP\_Measurement\_Period\_SSB is defined in table 9.5.4.1-2 for FR2 when *highSpeedMeasFlagFR2-r17* is not configured and if *groupBasedBeamReporting-r17* is not configured, and defined in table 9.5.4.1-2A for FR2-1 when *highSpeedMeasFlagFR2-r17* is not configured and if *groupBasedBeamReporting-r17* is configured, and defined in table 9.5.4.1-3 for FR2 power class 6 UE when *highSpeedMeasFlagFR2-r17* is configured, where

- M=1 if higher layer parameter *timeRestrictionForChannelMeasurement* is configured, and M=3 otherwise

- The value of N in table 9.5.4.1-2A is 2, 4 or 6 in FR2-1 for UE supporting *fastBeamSweepingMultiRx-r18* according to the conditions described in clause 3.6.19.

- The value of N in table 9.5.4.1-2 is 8.

- The value of N in table 9.5.4.1-3 is 8.

For a UE supporting [*support for Case 1 requirements*] and when concurrent measurement gap(s) with Pre-MG(s) are configured, or a UE supporting [*support for Case 2 requirements*] and when concurrent measurement gap(s) with NCSG measurement gap(s) are configured, or a UE supporting *concurrentMeasGap-r17* or *musim-GapPreference-r17* or both concurrent GAP and *musim-GapPreference-r17* and when concurrent gaps or periodic MUSIM gaps or both concurrent gaps and periodic MUSIM gaps are configured,

- an SSB or an SMTC occasion is not considered to be overlapped by a gap occasion if the gap occasion is dropped according to clause 9.1.8 and 9.1.10,

- P value for SSB resource to be measured is defined as

- Ntotal / Noutside\_MG in FR1

- Psharing factor \* Ntotal / Noutside\_MG in FR2 with Navailable = 0

- Ntotal / Navailable in FR2 with Navailable > 0

- For a window W of duration max(TL1, xRP\_max), where xRP\_max is the maximum xRP across all configured per-UE GAPs , periodic MUSIM gap(s) and per-FR GAPs, and, in case of Pre-MG, all activated per-UE measurement gaps and per-FR measurement gaps, within the same FR as serving cell, and starting at the beginning of any SSB resource occasion:

Ntotal is the total number of SSB resource occasions within the window, including those overlapped with GAP occasions, MUSIM gap occasions or SMTC occasions within the window, and

- Noutside\_MG is the number of SSB resource occasions that are not overlapped with any non-dropped GAP occasion nor non-dropped MUSIM gap occasion within the window W, and

- Navailable is the number of SSB resource occasions that are not overlapped with any non-dropped GAP occasion, non-dropped MUSIM gap occasion nor any SMTC occasion within the window W.

- an SSB or an SMTC occasion is considered to be overlapped with the MUSIM gap if it overlaps a MUSIM gap occasion.

- TL1 is periodicity of the target SSB.

- xRP = MGRP when configured GAP is activated Pre-MG or MG, and xRP = VIRP when configured GAP is NCSG.

Otherwise, for a UE neither supporting *concurrentMeasGap-r17* nor *[support for Case 1 requirements]* nor *[support for Case 2 requirements]* or when neither of the above configurations applies, i.e. concurrent measurement gaps, concurrent measurement gap(s) with Pre-MG(s) and concurrent measurement gap(s) with NCSG(s) and UE does not support *musim-GapPreference-r17* or when no MUSIM gaps are configured,

For FR1,

- P=, when in the monitored cell there are GAPs configured for intra-frequency, inter-frequency or inter-RAT measurements, which are overlapping with some but not all occasions of the SSB; and

- P=1 when in the monitored cell there are no GAPs overlapping with any occasion of the SSB.

For FR2,

P1=, when SSB is not overlapped with measurement gap and SSB is partially overlapped with SMTC occasion (TSSB < TSMTCperiod).

- P1 is PL1\_sharing\*Psharing factor, when SSB is not overlapped with measurement gap and SSB is fully overlapped with SMTC occasion (TSSB = TSMTCperiod).

- P1=, when SSB is partially overlapped with GAP and SSB is partially overlapped with SMTC occasion (TSSB < TSMTCperiod) and SMTC occasion is not overlapped with GAP and

- TSMTCperiod ≠ xRP or

- TSMTCperiod = xRP and TSSB < 0.5\*TSMTCperiod

- P is , when SSB is partially overlapped with GAP and SSB is partially overlapped with SMTC occasion (TSSB < TSMTCperiod) and SMTC occasion is not overlapped with GAP and TSMTCperiod = xRP and TSSB = 0.5\*TSMTCperiod

- P1=, when SSB is partially overlapped with GAP (TSSB < xRP) and SSB is partially overlapped with SMTC occasion (TSSB < TSMTCperiod) and SMTC occasion is partially or fully overlapped with GAP.

- P is , when SSB is partially overlapped with measurement gap and SSB is fully overlapped with SMTC occasion (TSSB = TSMTCperiod) and SMTC occasion is partially overlapped with GAP (TSMTCperiod < xRP)

- If SSB resource from the cell with different PCI is configured for L1-RSRP measurement, and P2 is valid accoding to clause 9.13.4.1, and any symbol of the SSBs from serving cell and cell with different PCI are overlapping or adjacent (in time domain)

- P = , if P1\*TSSB < P2\*TSSB\_CDP.

- P = P1, if P1\*TSSB > P2\*TSSB\_CDP.

- P = 2\*P1, if P1\*TSSB = P2\*TSSB\_CDP.

- Otherwise, P = P1

Where:

- TSSB = *ssb-periodicityServingCell* of the serving cell

- TSMTCperiod = the configured SMTC period

- TSSB\_CDP = SSB periodicity of the cell with PCI different from serving cell

- Psharing factor = 1, if the SSB configured for L1-RSRP measurement outside gap is

- not overlapped with the SSB symbols indicated by *SSB-ToMeasure* and 1 data symbol before each consecutive SSB symbols indicated by *SSB-ToMeasure* and 1 data symbol after each consecutive SSB symbols indicated by *SSB-ToMeasure*, given that *SSB-ToMeasure* is configured, where the *SSB-ToMeasure* is the union set of *SSB-ToMeasure* from all the configured measurement objects merged on the same serving carrier, and,

- not overlapped by the RSSI symbols indicated by *ss-RSSI-Measurement* and 1 data symbol before each RSSI symbol indicated by *ss-RSSI-Measurement* and 1 data symbol after each RSSI symbol indicated by *ss-RSSI-Measurement*, given that *ss-RSSI-Measurement* is configured.

- Psharing factor = 3, otherwise.

- PL1\_sharing = 2, if SSB resource from the cell with different PCI is configured for L1-RSRP measurement, and Psharing\_factor,CDP is used in clause 9.13.4.1, and any symbol of the SSBs from serving cell and cell with different PCI are overlapping or adjacent (in time domain). PL1\_sharing = 1, otherwise.

- TSSB = *ssb-periodicityServingCell*

- TSMTCperiod = the configured SMTC period

- When a measurement gap is configured and the measurement gap is not NCSG,

- an SSB or an SMTC occasion is considered to be overlapped with the GAP if it overlaps a measurement gap occasion, and

- xRP = MGRP

- If the UE is configured with Pre-MG, an SSB or an SMTC occasion is only considered to be overlapped by the Pre-MG if the Pre-MG is activated.

- Otherwise, when NCSG measurement gap only is configured,

- an SSB or an SMTC occasion is considered to be overlapped with the GAP if

- it overlaps the VIL1 or VIL2 of NCSG, or

- it overlaps the ML of NCSG in FR2, and there exists a target carrier to be measured within NCSG that is intra-frequency carrier or inter-frequency carrier in the same band as the serving cell, or inter-frequency carrier in different band as the serving cell and UE does not support IBM between the target carrier and the serving cell,

- and

- xRP = VIRP

The value of TL1-RSRP\_Measurement\_Period\_SSB is defined in table 9.5.4.1-4 for UE incapable of *multiCellL1-measRTD-greaterThan-CP-r18* in FR1, table 9.5.4.1-5 for UE capable of *multiCellL1-measRTD-greaterThan-CP-r18* in FR1, table 9.5.4.1-6 for UE incapable of *multiCellL1-measRTD-greaterThan-CP-r18* in FR2 and table 9.5.4.1-7 for UE capable of *multiCellL1-measRTD-greaterThan-CP-r18* in FR2 when there is L1-RSRP measurement on LTM neighbor cell(s) to measure within active BWP, where

- M=1 if higher layer parameter *timeRestrictionForChannelMeasurement* is configured, and M=3 otherwise

- N= 8 in table 9.5.4.1-6 and table 9.5.4.1-7.

- P value for SSB resource to be measured is defined as

- Ntotal / Noutside\_MG in FR1

- Psharing factor \* Ntotal / Noutside\_MG in FR2 with Navailable = 0

- Ntotal / Navailable in FR2 with Navailable > 0

For a window W of duration max (TL1, MGRP\_max), where MGRP max is the maximum MGRP across all configured per-UE measurement gaps and per-FR measurement gaps within the same FR as serving cell, and starting at the beginning of any SSB resource occasion:

- Ntotal is the total number of SSB resource occasions within the window, including those overlapped with measurement gap occasions or SMTC occasions within the window, and

- Noutside\_MG is the number of SSB resource occasions that are not overlapped with any measurement gap occasion within the window W

- Navailable is the number of SSB resource occasions that are not overlapped with any measurement gap occasion nor any SMTC occasion within the window W

- TL1 is periodicity of the target SSB.

- Psharing factor = 1, if the SSB configured for L1-RSRP measurement outside measurement gap is

- not overlapped with the SSB symbols indicated by *SSB-ToMeasure* and 1 data symbol before each consecutive SSB symbols indicated by *SSB-ToMeasure* and 1 data symbol after each consecutive SSB symbols indicated by *SSB-ToMeasure*, given that *SSB-ToMeasure* is configured, where the *SSB-ToMeasure* is the union set of *SSB-ToMeasure* from all the configured measurement objects merged on the same serving carrier, and,

- not overlapped with the RSSI symbols indicated by *ss-RSSI-Measurement* and 1data symbol before each RSSI symbol indicated by *ss-RSSI-Measurement* and 1 data symbol after each RSSI symbol indicated by *ss-RSSI-Measurement*, given that *ss-RSSI-Measurement* is configured,

- Psharing factor = 3, otherwise.

- PL1\_sharing is defined as

- When number of neighboring cells configured with SSB based L1-RSRP measurement is 1

- PL1\_sharing = 2, if any symbol of the SSBs from serving cell and neighbor cell are overlapping or adjacent (in time domain)

- PL1\_sharing = 1, otherwise

- When number of neighboring cells configured with SSB based L1-RSRP measurement is more than 1

- PL1\_sharing = 3.

Note: RRM requirements are not applicable when L1 measurement on the cells with different PCI and LTM L1 measurement on neighbour cells are both configured.

If the high layer in TS 38.331 [2] signaling of *smtc2* is configured, TSMTCperiod corresponds to the value of higher layer parameter *smtc2*; Otherwise TSMTCperiod corresponds to the value of higher layer parameter *smtc1*. TSMTCperiod is the shortest SMTC period among all CCs in the same FR2 band, provided the SMTC offset of all CCs in FR2 have the same offset.

For UE supporting *measurement gap occasion cancellation*, the UE is not required to perform SSB measurements during the cancelled gap occasions.

Longer evaluation period would be expected if the combination of SSB, SMTC occasion and GAP configurations does not meet previous conditions.

When UE is configured with aperiodic MUSIM gap and the aperiodic MUSIM gap is overlapping with SSB resource occasion for L1-RSRP, longer evaluation period would be expected.

When UE is configured with MUSIM gap(s), and SSB resource occasions for L1-RSRP are fully overlapped with MUSIM gap(s) or fully overlapped with the union of MUSIM gap(s) and GAPs, no requirement applies for the SSB based L1-RSRP measurement.

For either an FR1 or FR2 serving cell, longer evaluation period would be expected during the period Tidentify\_CGI when the UE is requested to decode an NR CGI.

For either an FR1 or FR2 serving cell, longer L1 RSRP measurement period would be expected during the period Tidentify\_CGI,E-UTRAN when the UE is requested to decode an LTE CGI.

Table 9.5.4.1-1: Measurement period TL1-RSRP\_Measurement\_Period\_SSB for FR1

|  |  |
| --- | --- |
| Configuration | TL1-RSRP\_Measurement\_Period\_SSB (ms) |
| non-DRX | max(TReport, ceil(M\*P)\*TSSB) |
| DRX cycle ≤ 320 ms | max(TReport, ceil(K \*M\*P)\*max(TDRX,TSSB)) |
| DRX cycle > 320 ms | ceil(M\*P)\*TDRX |
| Note 1: TSSB = *ssb-periodicityServingCell* is the periodicity of the SSB-Index configured for L1-RSRP measurement. TDRX is the DRX cycle length. TReport is configured periodicity for reporting.  Note 2: K = 1 when TSSB ≤ 40 ms and *highSpeedMeasFlag-r16 or highSpeedMeasCA-Scell-r17* are configured; otherwise, K = 1.5.  Note 3: When *highSpeedMeasFlag-r16* is configured, the requirements apply only to UE supporting either *measurementEnhancement-r16* or *intraNR-MeasurementEnhancement-r16. or measurementEnhancementCA-r17* | |

Table 9.5.4.1-2: Measurement period TL1-RSRP\_Measurement\_Period\_SSB for FR2

|  |  |
| --- | --- |
| Configuration | TL1-RSRP\_Measurement\_Period\_SSB (ms) |
| non-DRX | max(TReport, ceil(M\*P\*N)\*TSSB) |
| DRX cycle ≤ 320 ms | max(TReport, ceil(1.5\*M\*P\*N)\*max(TDRX,TSSB)) |
| DRX cycle > 320 ms | ceil(1.5\*M\*P\*N)\*TDRX |
| Note: TSSB = *ssb-periodicityServingCell* is the periodicity of the SSB-Index configured for L1-RSRP measurement. TDRX is the DRX cycle length. TReport is configured periodicity for reporting. | |

Table 9.5.4.1-2A: Measurement period TL1-RSRP\_Measurement\_Period\_SSB configured with *groupBasedBeamReporting-r17* for FR2-1

|  |  |
| --- | --- |
| Configuration | TL1-RSRP\_Measurement\_Period\_SSB (ms) |
| non-DRX | max(TReport, ceil(M\*P\*N)\*TSSB) |
| DRX cycle ≤ 320 ms | max(TReport, ceil(1.5\*M\*P\*N)\*max(TDRX,TSSB)) |
| DRX cycle > 320 ms | ceil(1.5\*M\*P\*N)\*TDRX |
| Note1: TSSB = *ssb-periodicityServingCell* is the periodicity of the SSB-Index configured for L1-RSRP measurement. TDRX is the DRX cycle length. TReport is configured periodicity for reporting. | |

**Table 9.5.4.1-3: Measurement period TL1-RSRP\_Measurement\_Period\_SSB configured with *highSpeedMeasFlagFR2-r17* for FR2-1**

|  |  |
| --- | --- |
| **Configuration** | **TL1-RSRP\_Measurement\_Period\_SSB (ms)** |
| non-DRX | max(TReport, ceil(M\*P\*N1Note2)\*TSSB) |
| DRX cycle ≤ 80 ms | max(TReport, ceil(M\*P\*N1Note2\*M2)\*max(TDRX,TSSB)) |
| 80 ms< DRX ≤ 320 ms | max(TReport, ceil(1.5\*M\*P\*N)\*max(TDRX,TSSB)) |
| DRX cycle > 320 ms | ceil(1.5\*M\*P\*N)\*TDRX |
| Note1: TSSB = *ssb-periodicityServingCell* is the periodicity of the SSB-Index configured for L1-RSRP measurement. TDRX is the DRX cycle length. TReport is configured periodicity for reporting.  Note 2: Scaling factor N1 = 2 when *highSpeedMeasFlagFR2-r17* = set1 or scaling factor N1 = 6 when *highSpeedMeasFlagFR2-r17* = set2, if UE does not support *simultaneousReceptionTwoQCL-r18* or when *highSpeedDeploymentTypeFR2-r17* is not configured as bidirectional. Scaling factor N1 = 1.5 when *highSpeedMeasFlagFR2-r17* is configured to set1 or scaling factor N1 = 4 when *highSpeedMeasFlagFR2-r17* is configured to set2, if UE supports *simultaneousReceptionTwoQCL-r18* and when *highSpeedDeploymentTypeFR2-r17* is configured as bidirectional.  Note 3: M2 = 1.5 if SMTC periodicity > 40 ms; otherwise M2 = 1 | |

Table 9.5.4.1-4: Measurement period TL1-RSRP\_Measurement\_Period\_SSB in FR1 for UE incapable of *multiCellL1-measRTD-greaterThan-CP-r18*

|  |  |
| --- | --- |
| Configuration | TL1-RSRP\_Measurement\_Period\_SSB\_intra (ms) |
| non-DRX | max(TReport, ceil(M\*P)\*TSSB) |
| DRX cycle ≤ 320 ms | max(TReport, ceil(K \*M\*P)\*max(TDRX,TSSB)) |
| DRX cycle > 320 ms | ceil(M\*P)\*TDRX |
| Note 1: TSSB = *ssb-periodicityServingCell* is the periodicity of the SSB-Index configured for L1-RSRP measurement. TDRX is the DRX cycle length. TReport is configured periodicity for reporting.  Note 2: K = 1.5.  Note 3: The requirements apply if the actual RTD between serving cell and neighbor cell is not larger than CP. | |

Table 9.5.4.1-5: Measurement period TL1-RSRP\_Measurement\_Period\_SSB in FR1 for UE capable of *multiCellL1-measRTD-greaterThan-CP-r18*

|  |  |
| --- | --- |
| Configuration | TL1-RSRP\_Measurement\_Period\_SSB\_intra (ms) |
| non-DRX | max(TReport, ceil(M\*P)\*TSSB) |
| DRX cycle ≤ 320 ms | max(TReport, ceil(K \*M\*P)\*max(TDRX,TSSB)) |
| DRX cycle > 320 ms | ceil(M\*P)\*TDRX |
| Note 1: TSSB = *ssb-periodicityServingCell* is the periodicity of the SSB-Index configured for L1-RSRP measurement. TDRX is the DRX cycle length. TReport is configured periodicity for reporting.  Note 2: K = 1.5. | |

Table 9.5.4.1-6: Measurement period TL1-RSRP\_Measurement\_Period\_SSB in FR2 for UE incapable of *multiCellL1-measRTD-greaterThan-CP-r18*

|  |  |
| --- | --- |
| Configuration | TL1-RSRP\_Measurement\_Period\_SSB\_intra (ms) |
| non-DRX | max(TReport, ceil(M\*P\*PL1\_sharing\*N)\*TSSB) |
| DRX cycle ≤ 320 ms | max(TReport, ceil(1.5\*M\*P\*PL1\_sharing \*N)\*max(TDRX,TSSB) ) |
| DRX cycle > 320 ms | ceil(1.5\*M\*P\*PL1\_sharing\*N)\*TDRX |
| Note 1: TSSB *= ssb-periodicityServingCell* is the periodicity of the SSB-Index configured for L1-RSRP measurement. TDRX is the DRX cycle length. TReport is configured periodicity for reporting.  Note 2: The requirements apply if the actual RTD between serving cell and neighbor cell is not larger than CP. | |

Table 9.5.4.1-7: Measurement period TL1-RSRP\_Measurement\_Period\_SSB in FR2 for UE capable of *multiCellL1-measRTD-greaterThan-CP-r18*

|  |  |
| --- | --- |
| Configuration | TL1-RSRP\_Measurement\_Period\_SSB\_intra (ms) |
| non-DRX | max(TReport, ceil(M\*P\*PL1\_sharing\*N)\*TSSB) |
| DRX cycle ≤ 320 ms | max(TReport, ceil(1.5\*M\*P\*PL1\_sharing\*N)\*max(TDRX,TSSB)) |
| DRX cycle > 320 ms | ceil(1.5\*M\*P\*PL1\_sharing\*N)\*TDRX |
| NOTE 1: TSSB = *ssb-periodicityServingCell* is the periodicity of the SSB-Index configured for L1-RSRP measurement. TDRX is the DRX cycle length. TReport is configured periodicity for reporting. | |

#### 9.5.4.2 CSI-RS based L1-RSRP Reporting

When *groupBasedBeamReporting-r17* is not configured, the UE shall be capable of performing L1-RSRP measurements based on the configured CSI-RS resource for L1-RSRP computation, and the UE physical layer shall be capable of reporting L1-RSRP measured over the measurement period of TL1-RSRP\_Measurement\_Period\_CSI-RS.

When *groupBasedBeamReporting-r17* is configured, the UE shall be capable of performing L1-RSRP measurements based on the two configured CSI-RS resource sets for L1-RSRP, and the UE physical layer shall be capable of reporting group-based L1-RSRP measured over the measurement period of TL1-RSRP\_Measurement\_Period\_CSI-RS.

The value of TL1-RSRP\_Measurement\_Period\_CSI-RS is defined in table 9.5.4.2-1 for FR1 and in table 9.5.4.2-2 for FR2, where

- For periodic and semi-persistent CSI-RS resources, M=1 if higher layer parameter *timeRestrictionForChannelMeasurement* is configured, and M=3 otherwise

- For aperiodic CSI-RS resources M=1

- For periodic CSI-RS resources in a resource set configured with higher layer parameter *repetition* set to OFF, N=1. The requirements apply if *qcl-InfoPeriodicCSI-RS* is configured for all the resources in the resource set and for each resource one RS has QCL-TypeD with

- SSB for L1-RSRP measurement, or

- another CSI-RS in resource set configured with repetition ON.

- For periodic CSI-RS resources in a resource set configured with higher layer parameter *repetition* set to ON, N=ceil(*maxNumberRxBeam* / Nres\_per\_set) for table 9.5.4.2-2, where Nres\_per\_set is number of resources in the resource set. The requirements apply provided *qcl-InfoPeriodicCSI-RS* is configured with QCL-TypeD for all resources in the resource set.

- For semi-persistent CSI-RS resources in a resource set configured with higher layer parameter *repetition* set to OFF, N=1. The requirements apply provided TCI state is provided for all resources in the resource set in the MAC CE activating the resource set and for each resource one RS has QCL-TypeD with

- SSB for L1-RSRP measurement, or

- another CSI-RS in resource set configured with repetition ON.

- For semi-persistent CSI-RS resources in a resource set configured with higher layer parameter *repetition* set to ON, N=ceil(*maxNumberRxBeam* / Nres\_per\_set), where Nres\_per\_set is number of resources in the resource set. The requirements apply provided TCI state is provided with QCL-TypeD for all resources in the resource set in the MAC CE activating the resource set.

- For aperiodic CSI-RS resources in a resource set configured with higher layer parameter *repetition* set to OFF, N=1. The requirements apply provided *qcl-info* is configured for all resources in the resource set and for each resource one RS has QCL-TypeD with

- SSB for L1-RSRP measurement, or

- another CSI-RS in resource set configured with repetition ON.

- For aperiodic CSI-RS resources in a resource set configured with higher layer parameter *repetition* set to ON, N=1. UE is not required to meet the accuracy requirements in clauses 10.1.19.2 and 10.1.20.2 if number of resources in the resource set is smaller than *maxNumberRxBeam*. The requirements apply provided *qcl-info* is configured with QCL-TypeD for all resources in the resource set.

For a UE supporting [*support for Case 1 requirements*] and when concurrent measurement gap(s) with Pre-MG(s) are configured, or a UE supporting [*support for Case 2 requirements*] and when concurrent measurement gap(s) with NCSG measurement gap(s) are configured, or a UE supporting *concurrentMeasGap-r17* or *musim-GapPreference-r17* or both concurrent measurement gap and *musim-GapPreference-r17* and when concurrent gaps or periodic MUSIM gaps or both concurrent gaps and periodic MUSIM gaps are configured,

- a CSI-RS or an SMTC occasion is not considered to be overlapped by a gap occasion if the gap occasion is dropped according to clauses 9.1.8 and 9.1.10,

- P value for a CSI-RS resource to be measured is defined as

- Ntotal / Noutside\_MG in FR1

- Psharing factor \* Ntotal / Noutside\_MG in FR2 with Navailable = 0

- Ntotal / Navailable in FR2 with Navailable > 0

- For a window W of duration max(TL1, xRP\_max), where xRP\_max is the maximum xRP across all configured per-UE measurement gaps or NCSGs, MUSIM gap(s)and per-FR measurement gaps or NCSGs, and, in case of Pre-MG, all activated per-UE measurement gaps and per-FR measurement gaps, within the same FR as serving cell, and starting at the beginning of any CSI-RS resource occasion:

- Ntotal is the total number of CSI-RS resource occasions within the window W, including those overlapped with measurement gap occasions, MUSIM gap occasions or SMTC occasions within the window W, and

- Noutside\_MG is the number of CSI-RS resource occasions that are not overlapped with any non-dropped GAP occasions nor non-dropped MUSIM gap occasion within the window W, and

- Navailable is the number of CSI-RS resource occasions that are not overlapped with any non-dropped GAP occasions, non-dropped MUSIM gap occasion nor any SMTC occasion within the window W.

- a CSI-RS or an SMTC occasion is considered to be overlapped with the MUSIM gap if it overlaps a MUSIM gap occasion.

- xRP = MGRP when configured GAP is activated Pre-MG or MG, and xRP = VIRP when configured GAP is NCSG.

TL1 is periodicity of the target CSI-RS.

Otherwise, for a UE neither supporting *concurrentMeasGap-r17* nor *[support for Case 1 requirements]* nor *[support for Case 2 requirements]* or when neither of the above configurations applies, i.e. concurrent measurement gaps, concurrent measurement gap(s) with Pre-MG(s) and concurrent measurement gap(s) with NCSG measurement gap(s), and UE does not support *musim-GapPreference-r17* or when no MUSIM gaps are configured.

For FR1,

- P=, when in the monitored cell there are GAPs configured for intra-frequency, inter-frequency or inter-RAT measurements, which are overlapping with some but not all occasions of the CSI-RS; and

- P=1 when in the monitored cell there are no GAPs overlapping with any occasion of the CSI-RS.

For FR2,

- P=1, when CSI-RS is not overlapped with a GAP and also not overlapped with SMTC occasion.

- P=, when CSI-RS is partially overlapped with GAP and CSI-RS is not overlapped with SMTC occasion (TCSI-RS < xRP)

- P=, when CSI-RS is not overlapped with GAP and CSI-RS is partially overlapped with SMTC occasion (TCSI-RS < TSMTCperiod).

- P=Psharing factor, when CSI-RS is not overlapped with GAP and CSI-RS is fully overlapped with SMTC occasion (TCSI-RS = TSMTCperiod).

- P=1, when aperiodic CSI-RS resource is not overlapped with GAP

- P=, when CSI-RS is partially overlapped with GAP and CSI-RS is partially overlapped with SMTC occasion (TCSI-RS < TSMTCperiod) and SMTC occasion is not overlapped with GAP and

- TSMTCperiod ≠ xRP or

- TSMTCperiod = xRP and TCSI-RS < 0.5\*TSMTCperiod

- P=, when CSI-RS is partially overlapped with GAP and CSI-RS is partially overlapped with SMTC occasion (TCSI-RS < TSMTCperiod) and SMTC occasion is not overlapped with GAP and TSMTCperiod = xRP and TCSI-RS = 0.5\*TSMTCperiod

- P=, when CSI-RS is partially overlapped with GAP (TCSI-RS < xRP) and CSI-RS is partially overlapped with SMTC occasion (TCSI-RS < TSMTCperiod) and SMTC occasion is partially or fully overlapped with GAP.

- P=, when CSI-RS is partially overlapped with GAP and CSI-RS is fully overlapped with SMTC occasion (TCSI-RS = TSMTCperiod) and SMTC occasion is partially overlapped with GAP (TSMTCperiod < xRP)

Where:

- Psharing factor = 1, if the CSI-RS configured for L1-RSRP measurement outside gap is

- not overlapped with the SSB symbols indicated by *SSB-ToMeasure* and 1 data symbol before each consecutive SSB symbols indicated by *SSB-ToMeasure* and 1 data symbol after each consecutive SSB symbols indicated by *SSB-ToMeasure*, given that *SSB-ToMeasure* is configured, where the *SSB-ToMeasure* is the union set of *SSB-ToMeasure* from all the configured measurement objects merged on the same serving carrier, and,

- not overlapped by the RSSI symbols indicated by *ss-RSSI-Measurement* and 1 data symbol before each RSSI symbol indicated by *ss-RSSI-Measurement* and 1 data symbol after each RSSI symbol indicated by *ss-RSSI-Measurement*, given that *ss-RSSI-Measurement* is configured.

- Psharing factor = 3, otherwise.

TSMTCperiod = the configured SMTC period.

TCSI-RS = the periodicity of CSI-RS configured for L1-RSRP measurement

- When a measurement gap is configured and the measurement gap is not NCSG,

- a CSI-RS or an SMTC occasion is considered to be as overlapped with the GAP if it overlapps a measurement gap occasion, and

- xRP = MGRP

- If the UE is configured with Pre-MG, a CSI-RS or an SMTC occasion is only considered to be overlapped by the Pre-MG if the Pre-MG is activated.

- Otherwise, when NCSG measurement gap only is configured,

- a CSI-RS or an SMTC occasion is considered to be as overlapped with the GAP if

- it overlaps the VIL1 or VIL2 of NCSG, or

- it overlaps the ML of NCSG in FR2, and there exists a target carrier to be measured within NCSG that is intra-frequency carrier or inter-frequency carrier in the same band as the serving cell, or inter-frequency carrier in different band as the serving cell and UE does not support IBM between the target carrier and the serving cell,

- and

- xRP = VIRP

For UE supporting *measurement gap occasion cancellation*, the UE is not required to perform CSI-RS measurements during the cancelled gap occasions.

When UE is configured with aperiodic MUSIM gap and the aperiodic MUSIM gap is overlapping with CSI-RS resource occasion for L1-RSRP, longer evaluation period would be expected.

When UE is configured with MUSIM gap(s), and CSI-RS resource occasions for L1-RSRP are fully overlapped with MUSIM gap(s) or fully overlapped with the union of MUSIM gap(s) and GAPs, no requirement applies for the CSI-RS based L1-RSRP measurement.

Table 9.5.4.2-1: Measurement period TL1-RSRP\_Measurement\_Period\_CSI-RS for FR1

|  |  |
| --- | --- |
| Configuration | TL1-RSRP\_Measurement\_Period\_CSI-RS (ms) |
| non-DRX | max(TReport, ceil(M\*P)\*TCSI-RS) |
| DRX cycle ≤ 320 ms | max(TReport, ceil(K \*M\*P)\*max(TDRX,TCSI-RS)) |
| DRX cycle > 320 ms | ceil(M\*P)\*TDRX |
| NOTE 1: TCSI-RS is the periodicity of CSI-RS configured for L1-RSRP measurement. TDRX is the DRX cycle length. TReport is configured periodicity for reporting.  NOTE 2: the requirements are applicable provided that the CSI-RS resource configured for L1-RSRP measurement is transmitted with Density = 3.  NOTE 3: K = 1 when TCSI-RS ≤ 40 ms and *highSpeedMeasFlag-r16 or highSpeedMeasCA-Scell-r17* are configured; otherwise K = 1.5.  NOTE 4: When *highSpeedMeasFlag-r16* is configured, the requirements apply only to UE supporting either *measurementEnhancement-r16* or *intraNR-MeasurementEnhancement-r16 or measurementEnhancementCA-r17.* | |

Table 9.5.4.2-2: Measurement period TL1-RSRP\_Measurement\_Period\_CSI-RS for FR2

|  |  |
| --- | --- |
| Configuration | TL1-RSRP\_Measurement\_Period\_CSI-RS (ms) |
| non-DRX | max(TReport, ceil(M\*P\*N)\*TCSI-RS) |
| DRX cycle ≤ 320 ms | max(TReport, ceil(1.5\*M\*P\*N)\*max(TDRX,TCSI-RS)) |
| DRX cycle > 320 ms | ceil(M\*P\*N)\*TDRX |
| NOTE 1: TCSI-RS is the periodicity of CSI-RS configured for L1-RSRP measurement. TDRX is the DRX cycle length. TReport is configured periodicity for reporting.  NOTE 2: the requirements are applicable provided that the CSI-RS resource configured for L1-RSRP measurement is transmitted with Density = 3. | |

Table 9.5.4.2-2A: Void

# <End of Change #6>

# <Start of Change #7>

### 9.8.4 L1-SINR measurement requirements

#### 9.8.4.1 L1-SINR reporting with CSI-RS based CMR and no dedicated IMR configured

edicated resource configured as IMR for L1-SINR computation, and the UE physical layer shall be capable of reporting L1-SINR measured over the measurement period of TL1-SINR\_Measurement\_Period\_CSI-RS\_CMR\_Only.

The value of TL1-SINR\_Measurement\_Period\_CSI-RS\_CMR\_Only is defined in table 9.8.4.1-1 for FR1 and in table 9.8.4.1-2 for FR2, where

For the value of M,

- For periodic and semi-persistent CSI-RS resources as CMR, M=1 if higher layer parameter *timeRestrictionForChannelMeasurement* is configured, and M=3 otherwise;

- For aperiodic CSI-RS resources as CMR, M=1.

For the value of N in FR2

- For periodic CSI-RS resources as CMR in a resource set configured with higher layer parameter *repetition* set to OFF, N=1. The requirements apply if *qcl-InfoPeriodicCSI-RS* is configured for all the resources in the resource set and for each resource one RS has QCL-TypeD with

- SSB for L1-RSRP or L1-SINR measurement, or

- another CSI-RS in resource set configured with repetition ON.

- For periodic CSI-RS resources as CMR in a resource set configured with higher layer parameter *repetition* set to ON, N=ceil(*maxNumberRxBeam* / Nres\_per\_set), where Nres\_per\_set is number of resources in the resource set. The requirements apply provided *qcl-InfoPeriodicCSI-RS* is configured for all resources in the resource set.

- For semi-persistent CSI-RS resources as CMR in a resource set configured with higher layer parameter *repetition* set to OFF, N=1. The requirements apply provided TCI state is provided for all resources in the resource set in the MAC CE activating the resource set and for each resource has QCL-TypeD with

- SSB for L1-RSRP or L1-SINR measurement, or

- another CSI-RS in resource set configured with repetition ON.

- For semi-persistent CSI-RS resources as CMR in a resource set configured with higher layer parameter *repetition* set to ON, N=ceil(*maxNumberRxBeam* / Nres\_per\_set), where Nres\_per\_set is number of resources in the resource set. The requirements apply provided TCI state is provided for all resources in the resource set in the MAC CE activating the resource set.

- For aperiodic CSI-RS resources as CMR in a resource set configured with higher layer parameter *repetition* set to OFF, N=1. The requriements apply provided *qcl-info* is configured for all resources in the resource set and for each resource has QCL-TypeD with

- SSB for L1-RSRP or L1-SINR measurement, or

- another CSI-RS in resource set configured with repetition ON.

- For aperiodic CSI-RS resources as CMR in a resource set configured with higher layer parameter *repetition* set to ON, N=1. UE is not required to meet the accuracy requirements in clauses 10.1.28.1 and 10.1.28.3 if number of resources in the resource set is smaller than *maxNumberRxBeam*. The requriements apply provided *qcl-info* is configured for all resources in the resource set.

For a UE supporting [*support for Case 1 requirements*] and when concurrent measurement gap(s) with Pre-MG(s) are configured, or a UE supporting [*support for Case 2 requirements*] and when concurrent GAP(s) with NCSG(s) are configured, or a UE supporting *concurrentMeasGap-r17* or *musim-GapPreference-r17* or both concurrent measurement gap and *musim-GapPreference-r17* and when concurrent GAPs or periodic MUSIM gaps or both concurrent gaps and periodic MUSIM gaps are configured,

- a CSI-RS or an SMTC occasion is not considered to be overlapped by a gap occasion if the gap occasion is dropped according to 9.1.8 and 9.1.10,

- P value for a CSI-RS resource to be measured is defined as

- Ntotal / Noutside\_MG in FR1

- Psharing factor \* Ntotal / Noutside\_MG in FR2 with Navailable = 0

- Ntotal / Navailable in FR2 with Navailable > 0

- For a window W of duration max(TL1, xRP\_max), where xRP\_max is the maximum xRP across all configured per-UE GAPs or periodic MUSIM gap(s) and per-FR GAPs, and, in case of Pre-MG, all activated per-UE measurement gaps and per-FR measurement gaps, within the same FR as serving cell, and starting at the beginning of any CSI-RS resource occasion:

- Ntotal is the total number of CSI-RS resource occasions within the window, including those overlapped with GAP occasions, MUSIM gap occasions or SMTC occasions within the window, and

- Noutside\_MG is the number of CSI-RS resource occasions that are not overlapped with any non-dropped GAP occasion nor non-dropped MUSIM gap occasion within the window W, and

- Navailable is the number of CSI-RS resource occasions that are not overlapped with any non-dropped GAP occasion, non-dropped MUSIM gap occasion nor any SMTC occasion within the window W.

- a CSI-RS or an SMTC occasion is considered to be overlapped with the MUSIM gap if it overlaps a MUSIM gap occasion.

- TL1 is periodicity of the target CSI-RS.

- xRP = MGRP when configured GAP is activated Pre-MG or MG, and xRP = VIRP when configured GAP is NCSG.

Otherwise, for a UE neither supporting *concurrentMeasGap-r17* nor *[support for Case 1 requirements]* nor *[support for Case 2 requirements]* or when neither of the above configurations applies, i.e. concurrent measurement gaps, concurrent measurement gap(s) with Pre-MG(s) and concurrent GAP(s) with NCSG(s) and UE does not support *musim-GapPreference-r17* or when no MUSIM gaps are configured,

For the value of P in FR1,

- P=, when in the monitored cell there are GAP configured for intra-frequency, inter-frequency or inter-RAT measurements, which are overlapping with some but not all occasions of the CSI-RS; and

- P=1 when in the monitored cell there are no GAPs overlapping with any occasion of the CSI-RS.

For the value of P in FR2,

- P=1, when CSI-RS is not overlapped with GAP and also not overlapped with SMTC occasion.

- P=, when CSI-RS is partially overlapped with GAP and CSI-RS is not overlapped with SMTC occasion (TCSI-RS < xRP)

- P=, when CSI-RS is not overlapped with GAP and CSI-RS is partially overlapped with SMTC occasion (TCSI-RS < TSMTCperiod).

- P is Psharing factor,, when CSI-RS is not overlapped with GAP and CSI-RS is fully overlapped with SMTC occasion (TCSI-RS = TSMTCperiod).

- P=, when CSI-RS is partially overlapped with [measurement gap] and CSI-RS is partially overlapped with SMTC occasion (TCSI-RS < TSMTCperiod) and SMTC occasion is not overlapped with GAP and

- TSMTCperiod ≠ xRP or

- TSMTCperiod = xRP and TCSI-RS < 0.5\*TSMTCperiod

- P=, when CSI-RS is partially overlapped with GAP and CSI-RS is partially overlapped with SMTC occasion (TCSI-RS < TSMTCperiod) and SMTC occasion is not overlapped with GAP and TSMTCperiod = xRP and TCSI-RS = 0.5\*TSMTCperiod

- P=, when CSI-RS is partially overlapped with GAP (TCSI-RS < xRP) and CSI-RS is partially overlapped with SMTC occasion (TCSI-RS < TSMTCperiod) and SMTC occasion is partially or fully overlapped with GAP.

- P=, when CSI-RS is partially overlapped with GAP and CSI-RS is fully overlapped with SMTC occasion (TCSI-RS = TSMTCperiod) and SMTC occasion is partially overlapped with GAP (TSMTCperiod < xRP)

Where:

Psharing factor = 1, if the CSI-RS configured for L1-SINR measurement outside gap is

not overlapped with the SSB symbols indicated by *SSB-ToMeasure* and 1 data symbol before each consecutive SSB symbols indicated by *SSB-ToMeasure* and 1 data symbol after each consecutive SSB symbols indicated by *SSB-ToMeasure*, given that *SSB-ToMeasure* is configured, where the *SSB-ToMeasure* is the union set of *SSB-ToMeasure* from all the configured measurement objects merged on the same serving carrier, and,

not overlapped by the RSSI symbols indicated by *ss-RSSI-Measurement* and 1 data symbol before each RSSI symbol indicated by *ss-RSSI-Measurement* and 1 data symbol after each RSSI symbol indicated by *ss-RSSI-Measurement*, given that *ss-RSSI-Measurement* is configured.

- Psharing factor = 3, otherwise.

- TSMTCperiod = the configured SMTC1 period or SMTC2 period if configured.

- TCSI-RS = the periodicity of CSI-RS configured for L1-SINR measurement

- When a measurement gap is configured and the measurement gap is not NCSG,

- a CSI-RS is considered to be overlapped with the GAP if it overlaps a measurement gap occasion, and

- xRP = MGRP

- If the UE is configured with Pre-MG, a CSI-RS reourse or an SMTC occasion is only considered to be overlapped by the Pre-MG if the Pre-MG is activated.

- Otherwise, when NCSG measurement gap only is configured,

- a CSI-RS is considered to be overlapped with the GAP if

- it overlaps the VIL1 or VIL2 of NCSG, or

- it overlaps the ML of NCSG in FR2, and there exists a target carrier to be measured within NCSG that is intra-frequency carrier or inter-frequency carrier in the same band as the serving cell, or inter-frequency carrier in different band as the serving cell and UE does not support IBM between the target carrier and the serving cell,

- and

- xRP = VIRP

If the high layer in TS 38.331 [2] signaling of *smtc2* is configured, TSMTCperiod corresponds to the value of higher layer parameter *smtc2*; Otherwise TSMTCperiod corresponds to the value of higher layer parameter *smtc1*.

Note: The overlap between CSI-RS for L1-SINR measurement and SMTC means that CSI-RS for L1-SINR measurement is within the SMTC window duration.

For UE supporting *measurement gap occasion cancellation*, the UE is not required to perform CSI-RS measurements during the cancelled gap occasions.

When UE is configured with aperiodic MUSIM gap and the aperiodic MUSIM gap is overlapping with CSI-RS resource occasion for L1-SINR, longer evaluation period would be expected.

When UE is configured with MUSIM gap(s), and CSI-RS resource occasions for L1-SINR are fully overlapped with MUSIM gap(s) or fully overlapped with the union of MUSIM gap(s) and GAPs, no requirement applies for the CSI-RS based L1-SINR measurement.

Longer evaluation period would be expected if the combination of CSI-RS, SMTC occasion and GAP configurations does not meet previous conditions.

Table 9.8.4.1-1: Measurement period TL1-SINR\_Measurement\_Period\_CSI-RS\_CMR\_Only for FR1

|  |  |
| --- | --- |
| Configuration | TL1-SINR\_Measurement\_Period\_CSI-RS\_CMR\_Only (ms) |
| non-DRX | max(TReport, ceil(M\*P)\*TCSI-RS) |
| DRX cycle ≤ 320 ms | max(TReport, ceil(1.5\*M\*P)\*max(TDRX,TCSI-RS)) |
| DRX cycle > 320 ms | ceil(M\*P)\*TDRX |
| NOTE 1: TCSI-RS is the periodicity of CSI-RS configured for L1-SINR measurement. TDRX is the DRX cycle length. TReport is configured periodicity for reporting.  NOTE 2: the requirements are applicable provided that the CSI-RS resource configured for L1-SINR measurement is transmitted with Density = 3. | |

Table 9.8.4.1-2: Measurement period TL1-SINR\_Measurement\_Period\_CSI-RS\_CMR\_Only for FR2

|  |  |
| --- | --- |
| Configuration | TL1-SINR\_Measurement\_Period\_CSI-RS\_CMR\_Only (ms) |
| non-DRX | max(TReport, ceil(M\*P\*N)\*TCSI-RS) |
| DRX cycle ≤ 320 ms | max(TReport, ceil(1.5\*M\*P\*N)\*max(TDRX,TCSI-RS)) |
| DRX cycle > 320 ms | ceil(M\*P\*N)\*TDRX |
| NOTE 1: TCSI-RS is the periodicity of CSI-RS configured for L1-SINR measurement. TDRX is the DRX cycle length. TReport is configured periodicity for reporting.  NOTE 2: the requirements are applicable provided that the CSI-RS resource configured for L1-SINR measurement is transmitted with Density = 3. | |

9.8.4.2 L1-SINR reporting with SSB based CMR and dedicated IMR configured

The UE shall be capable of performing L1-SINR measurements with the SSB configured as CMR and dedicated resource configured as IMR for L1-SINR computation, in which the NZP-CSI-RS or CSI-IM resource configured as dedicated IMR shall be 1-to-1 mapped to SSB configured as CMR, with the same periodicity. The UE physical layer shall be capable of reporting L1-SINR measured over the measurement period of TL1-SINR\_Measurement\_Period\_SSB\_CMR\_IMR.

The requirements in this clause are not applicable if NZP-CSI-RS or CSI-IM resource configured as dedicated IMR is scheduled with different periodicity as SSB configured as CMR.

The value of TL1-SINR\_Measurement\_Period\_SSB\_CMR\_IMR is defined in table 9.8.4.2-1 for FR1 and in table 9.8.4.2-2 for FR2 when *highSpeedMeasFlagFR2-r17* is not configured, and defined in table 9.8.4.2-3 for FR2 power class 6 UE when *highSpeedMeasFlagFR2-r17* is configured, where

For the value of M

- For periodic or semi-persistent NZP CSI-RS or CSI-IM resource as dedicated IMR, M=1 if the higher layer parameters *timeRestrictionForChannelMeasurements* and/or *timeRestrictionForInterferenceMeasurements* are configured, and M=3 otherwise;

For the value of N in FR2

- N = 2, 4 or 6 in FR2-1 for UE supporting *fastBeamSweepingMultiRx-r1*8, according to the conditions described in clause 3.6.19,

- N = 8 otherwise.

P is defined as the maximum value between PCMR and PIMR, i.e., P = max(PCMR, PIMR), where

- the value of PCMR shall be derived in the same way as the value of P used for SSB based L1-RSRP measurement in clause 9.5.4.1, in which the occasions and period of the SSB for CMR shall be used instead.

- the value of PIMR shall be derived in the same way as the value of P used for CSI-RS based L1-RSRP measurement in clause 9.5.4.2, in which the occasions and period of the NZP CSI-RS for NZP-IMR or CSI-IM for ZP-IMR shall be used instead.

For UE supporting *measurement gap occasion cancellation*, the UE is not required to perform SSB measurements during the cancelled gap occasions.

Longer evaluation period would be expected if the combination of SSB, SMTC occasion and measurement gap configurations does not meet previous conditions.

For L1-SINR measurement with SSB as CMR and CSI-RS or CSI-IM as IMR, the requirement shall apply if the CSI-RS is configured as IMR with repetition field as “repetition = OFF” or CSI-IM is configured as IMR.

For L1-SINR measurement with SSB as CMR and CSI-RS/CSI-IM as IMR, no requirement shall apply if SSB occasions for CMR or CSI-RS/CSI-IM occasions for IMR are fully overlapped with the configured measurement gap

Table 9.8.4.2-1: Measurement period TL1-SINR\_Measurement\_Period\_SSB\_CMR\_IMR for FR1

|  |  |
| --- | --- |
| Configuration | TL1-SINR\_Measurement\_Period\_SSB\_CMR\_IMR (ms) |
| non-DRX | max(TReport, ceil(M\*P)\*TSSB) |
| DRX cycle ≤ 320 ms | max(TReport, ceil(1.5\*M\*P)\*max(TDRX,TSSB)) |
| DRX cycle > 320 ms | ceil(M\*P)\*TDRX |
| NOTE 1: TSSB = ssb-periodicityServingCell is the periodicity of the SSB-Index configured for L1-SINR channel measurement. TDRX is the DRX cycle length. TReport is configured periodicity for reporting.  NOTE 2: The requirements are applicable provided that the CSI-RS resource configured for interference measurement shall be 1-to-1 mapped to SSB configured for channel measurement, with the same periodicity. | |

Table 9.8.4.2-2: Measurement period TL1-SINR\_Measurement\_Period\_SSB\_CMR\_IMR for FR2

|  |  |
| --- | --- |
| Configuration | TL1-SINR\_Measurement\_Period\_SSB\_CMR\_IMR (ms) |
| non-DRX | max(TReport, ceil(M\*P\*N)\*TSSB) |
| DRX cycle ≤ 320 ms | max(TReport, ceil(1.5\*M\*P\*N)\*max(TDRX,TSSB)) |
| DRX cycle > 320 ms | ceil(1.5\*M\*P\*N)\*TDRX |
| NOTE 1: TSSB = ssb-periodicityServingCell is the periodicity of the SSB-Index configured for L1-SINR measurement. TDRX is the DRX cycle length. TReport is configured periodicity for reporting.  NOTE 2: The requirements are applicable provided that the CSI-RS resource configured for interference measurement shall be 1-to-1 mapped to SSB configured for channel measurement, with the same periodicity. | |

Table 9.8.4.2-3: Measurement period TL1-SINR\_Measurement\_Period\_SSB\_CMR\_IMR configured with *highSpeedMeasFlagFR2-r17* for FR2-1

|  |  |
| --- | --- |
| Configuration | TL1-SINR\_Measurement\_Period\_SSB\_CMR\_IMR (ms) |
| non-DRX | max(TReport, ceil(M\*P\*N1Note 3)\*TSSB) |
| DRX cycle ≤ 80 ms | max(TReport, ceil(M\*P\*N1Note 3\*M2)\*max(TDRX,TSSB)) |
| 80 ms< DRX cycle ≤ 320 ms | max(TReport, ceil(1.5\*M\*P\*N)\*max(TDRX,TSSB)) |
| DRX cycle > 320 ms | ceil(1.5\*M\*P\*N)\*TDRX |
| NOTE 1: TSSB = ssb-periodicityServingCell is the periodicity of the SSB-Index configured for L1-SINR measurement. TDRX is the DRX cycle length. TReport is configured periodicity for reporting.  NOTE 2: The requirements are applicable provided that the CSI-RS resource configured for interference measurement shall be 1-to-1 mapped to SSB configured for channel measurement, with the same periodicity.  NOTE 3: N1 = 2 when *highSpeedMeasFlagFR2-r17* = set1; N1 = 6 when *highSpeedMeasFlagFR2-r17* = set2.  NOTE 4: M2 = 1.5 if SMTC periodicity > 40 ms; otherwise M2 = 1 | |

#### 9.8.4.3 L1-SINR reporting with CSI-RS based CMR and dedicated IMR configured

The UE shall be capable of performing L1-SINR measurements with the CSI-RS resource configured as CMR and dedicated resource configured as IMR for L1-SINR computation, in which the NZP-CSI-RS or CSI-IM resource configured as dedicated IMR shall be 1-to-1 mapped to CSI-RS resource configured as CMR, with the same periodicity. The UE physical layer shall be capable of reporting L1-SINR measured over the measurement period of TL1-SINR\_Measurement\_Period\_CSI-RS\_CMR\_IMR.

The requirements in this clause are not applicable if NZP-CSI-RS or CSI-IM resource configured as dedicated IMR is scheduled with different periodicity as CSI-RS resource configured as CMR.

The value of TL1-SINR\_Measurement\_Period\_CSI-RS\_CMR\_IMR is defined in table 9.8.4.3-1 for FR1 and in table 9.8.4.3-2 for FR2, where

For the value of M,

- M=1 shall be applied if

- aperiodic NZP-CSI-RS as CMR or dedicated IMR, or

- aperiodic CSI-IMR as dedicated IMR, or

- periodic and semi-persistent NZP-CSI-RS as CMR or dedicated IMR and the higher layer parameters *timeRestrictionForChannelMeasurement* and/or *timeRestrictionForInterferenceMeasurements* are configured, or

- periodic and semi-persistent CSI-IM as dedicated IMR and the higher layer parameters *timeRestrictionForChannelMeasurement* and/or *timeRestrictionForInterferenceMeasurements* are configured;

- M=3 otherwise.

For the value of N in FR2

- For periodic CSI-RS resources as CMR in a resource set configured with higher layer parameter *repetition* set to OFF, N=1. The requirements apply if *qcl-InfoPeriodicCSI-RS* is configured for all the resources in the resource set and for each resource one RS has QCL-TypeD with

- SSB for L1-RSRP or L1-SINR measurement, or

- another CSI-RS in resource set configured with repetition ON.

- For periodic CSI-RS resources as CMR in a resource set configured with higher layer parameter *repetition* set to ON, N=ceil(*maxNumberRxBeam* / Nres\_per\_set), where Nres\_per\_set is number of resources in the resource set. The requirements apply provided *qcl-InfoPeriodicCSI-RS* is configured for all resources in the resource set.

- For semi-persistent CSI-RS resources as CMR in a resource set configured with higher layer parameter *repetition* set to OFF, N=1. The requirements apply provided TCI state is provided for all resources in the resource set in the MAC CE activating the resource set and for each resource has QCL-TypeD with

- SSB for L1-RSRP or L1-SINR measurement, or

- another CSI-RS in resource set configured with repetition ON.

- For semi-persistent CSI-RS resources as CMR in a resource set configured with higher layer parameter *repetition* set to ON, N=ceil(*maxNumberRxBeam* / Nres\_per\_set), where Nres\_per\_set is number of resources in the resource set. The requirements apply provided TCI state is provided for all resources in the resource set in the MAC CE activating the resource set.

- For aperiodic CSI-RS resources as CMR in a resource set configured with higher layer parameter *repetition* set to OFF, N=1. The requriements apply provided *qcl-info* is configured for all resources in the resource set and for each resource has QCL-TypeD with

- SSB for L1-RSRP or L1-SINR measurement, or

- another CSI-RS in resource set configured with repetition ON.

- For aperiodic CSI-RS resources as CMR in a resource set configured with higher layer parameter *repetition* set to ON, N=1. UE is not required to meet the accuracy requirements in clause 10.1.28.1 and 10.1.28.3 if number of resources in the resource set is smaller than *maxNumberRxBeam*. The requriements apply provided *qcl-info* is configured for all resources in the resource set.

P is defined as the maximum value between PCMR and PIMR, i.e., P = max(PCMR, PIMR), where

- The value of PCMR and PIMR shall be derived in the same way as the value of P used for CSI-RS based L1-RSRP measurement in clause 9.5.4.2, in which the occasions and period of the CSI-RS for CMR and NZP CSI-RS for NZP-IMR or CSI-IM for ZP-IMR shall be used instead respectively.

For UE supporting *measurement gap occasion cancellation*, the UE is not required to perform CSI-RS measurements during the cancelled gap occasions.

Longer evaluation period would be expected if the combination of CSI-RS, SMTC occasion and measurement gap configurations does not meet previous conditions.

For L1-SINR measurement with CSI-RS as CMR and CSI-RS as IMR, the requirement shall apply only if CSI-RS resources as CMR and IMR are configured with the same repetition field and the number of CSI-RS resources in the resource sets for CMR and IMR are same.

For L1-SINR measurement with CSI-RS as CMR and CSI-IM as IMR, the requirement shall apply only if the number of CSI-RS resources in the resource set for CMR and the number of CSI-IM resources in the resource set for IMR are same.

For L1-SINR measurement with CSI-RS as CMR and CSI-RS/CSI-IM as IMR, no requirement shall apply if CSI-RS occasions for CMR or CSI-RS/CSI-IM occasions for IMR are fully overlapped with the configured measurement gap.

Table 9.8.4.3-1: Measurement period TL1-SINR\_Measurement\_Period\_CSI-RS\_CMR\_IMR for FR1

|  |  |
| --- | --- |
| Configuration | TL1-SINR\_Measurement\_Period\_CSI-RS\_CMR\_IMR (ms) |
| non-DRX | max(TReport, ceil(M\*P)\*TCSI-RS) |
| DRX cycle ≤ 320 ms | max(TReport, ceil(1.5\*M\*P)\*max(TDRX,TCSI-RS)) |
| DRX cycle > 320 ms | ceil(M\*P)\*TDRX |
| NOTE 1: TCSI-RS is the periodicity of CSI-RS configured for L1-SINR measurement. TDRX is the DRX cycle length. TReport is configured periodicity for reporting.  NOTE 2: the requirements are applicable provided that the CSI-RS resource configured for L1-SINR measurement is transmitted with Density = 3.  NOTE 3: The requirements are applicable provided that the CSI-RS resource configured for interference measurement shall be 1-to-1 mapped to CSI-RS configured for channel measurement, with the same periodicity. | |

Table 9.8.4.3-2: Measurement period TL1-SINR\_Measurement\_Period\_CSI-RS\_CMR\_IMR for FR2

|  |  |
| --- | --- |
| Configuration | TL1-SINR\_Measurement\_Period\_CSI-RS\_CMR\_IMR (ms) |
| non-DRX | max(TReport, ceil(M\*P\*N)\*TCSI-RS) |
| DRX cycle ≤ 320 ms | max(TReport, ceil(1.5\*M\*P\*N)\*max(TDRX,TCSI-RS)) |
| DRX cycle > 320 ms | ceil(M\*P\*N)\*TDRX |
| NOTE 1: TCSI-RS is the periodicity of CSI-RS configured for L1-SINR measurement. TDRX is the DRX cycle length. TReport is configured periodicity for reporting.  NOTE 2: the requirements are applicable provided that the CSI-RS resource configured for L1-SINR measurement is transmitted with Density = 3.  NOTE 3: The requirements are applicable provided that the CSI-RS resource configured for interference measurement shall be 1-to-1 mapped to CSI-RS configured for channel measurement, with the same periodicity. | |

# <End of Change #7>