**3GPP TSG-SA5 Meeting #162 *S5-253513***

**Goteborg, Sweden, 25 - 29 August 2025**

**Title: Reply LS on signalling feasibility of dataset and parameter sharing**

**Response to: R2-2503169/S5-253287**

**Release: Release 19**

**Work Item: NR\_AIML\_air-Core**

**Source: SA5**

**To: RAN2**

**Cc: RAN, SA, RAN1, RAN3, SA2, SA3**

**Contact person: Shi Xiaoli**

[**shixiaoli@huawei.com**](mailto:shixiaoli@huawei.com)

**Send any reply LS to: 3GPP Liaisons Coordinator,** [**mailto:3GPPLiaison@etsi.org**](mailto:3GPPLiaison@etsi.org)

**Attachments:** **None**

1. Overall description

SA5 would like to thank RAN2 for sharing the LS on signalling feasibility of dataset and parameter sharing.

RAN2 discussed the candidate solutions and feasibility of standardized signaling for NW-side sharing dataset/model parameter to UE or UE-side training entity for below options:

1. Dataset sharing consisting of {(Target CSI, CSI feedback)}
2. Encoder parameter sharing
3. Encoder parameter sharing + dataset sharing consisting of {target CSI}

The LS concluded on the following approach for non-OTA transferring of dataset/model parameters.

|  |  |  |  |
| --- | --- | --- | --- |
| **Alternative 1 (non-OTA approach):**  **gNB** -> **NW dataset/model parameters collection entity** -> **UE training entity** (a server inside MNO or an OTT server)     |  | | --- | |  | |  | |   **NOTE: The data transfer (up to RAN1 further details on what to transfer) between gNB and NW dataset/model parameters collection entity (OAM/CN) in Alternative 1, if needed, is up to RAN3/SA2/SA5.** |

The LS asks SA5 to confirm RAN2 assumption on non-OTA candidate solutions described in Table 1.

Table 1. non-OTA candidate solutions

|  |  |  |
| --- | --- | --- |
| **Option** | **Impacted WG** | **Specification impact/Implementation impact** |
| OAM -> UE-side training entity (a server inside MNO or an OTT server), where OAM is NW-side dataset/model parameter collection entity | SA5, SA3 | Up to SA5  (any intermediate node between OAM and UE-side OTT server is up to SA5; CN involvement if needed is up to SA2/SA5 discussion) |
| CN -> UE-side training entity (a server inside MNO or an OTT server), where CN is NW-side dataset/model parameter collection entity | SA2, SA3 | Up to SA2  (any intermediate node between CN and UE-side OTT server is up to SA2) |
| gNB -> OAM/CN -> UE-side training entity (a server inside MNO or an OTT server), where gNB is NW-side dataset/model parameter collection entity | RAN3, SA2, SA5, SA3 | Up to RAN3, SA2, SA5  (any intermediate node between gNB/OAM, OAM/UE-side OTT server, CN/UE-side OTT server is up to RAN3/SA2/SA5) |

**SA5 feedback:**

SA5 Rel-19 existing data collection architecture related to data collection supports the data transmission from gNB to OAM as defined in TS 32.422, TS 28.552 and TS 28.554. For management data transmission from OAM to UE-side training entity, SA5 confirms that it is feasible for OAM to transfer the collected data to UE-side training entity, as long as the UE-side training entity becomes an authorized MnS consumer as defined in TS 28.533 and TS 28.537.

SA5 needs more details to evaluate whether dataset/model parameters can serve as a category for management data from TSG RAN2.

1. Actions

**To RAN2**

**ACTION:** SA5 kindly asks RAN2 to take the above feedback into account and to confirm if SA5 assumption is correct.

1. Dates of next TSG SA WG5 meetings

SA5#163 13 October - 17 October 2025 China

SA5#164 17 November - 21 November 2025 Dallas , US