**3GPP TSG-SA5 Meeting #162 *S5-253851***

**Goteborg, Sweden, 25 - 29 August 2025**

**Title: Reply LS on Reply LS to S5-251090 on MWAB-gNB Configurations**

**Response to: R2-2504380/S5-253289**

**Release: Release 19**

**Work Item: AdNRM\_Ph4**

**Source: SA5**

**To: SA2**

**Cc:**

**Contact person: Deepanshu Gautam**

 **deepanshu.g@samsung.com**

**Send any reply LS to: 3GPP Liaisons Coordinator,****mailto:3GPPLiaison@etsi.org**

**Attachments:** **None**

1. Overall description

SA5 thanks SA2 for providing detailed answer to the questions. SA5 would like to inform that we have agreed the related CR, as attached, fulfilling the following OAM configuration stated in the LS.

*“It is expected the OAM of the MWAB Broadcasted PLMN/SNPN is aware of location in which the MWAB operation can be authorized and also can obtain MWAB's current location.”*

Further, SA5 need to clarify on the following question:

Question: SA5 would like to further clarify if the Traffic Descriptor for Xn, N2 and N3 need to be configured from OAM to MWAB-gNB.

1. Actions

**To SA2**

**ACTION:** SA5 kindly asks SA2 and RAN3 to provide answers to the above questions

1. Dates of next TSG SA WG5 meetings

SA5#163 13 October - 17 October 2025 China

SA5#164 17 November - 21 November 2025 Dallas , US