**3GPP TSG-SA4 Meeting #131-bis-e *S4-250441***

**Online, , 11th Apr 2025 - 17th Apr 2025**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.3* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  | **26.113** | **CR** | **0006** | **rev** | **-** | **Current version:** | **18.2.0** |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **x** | Radio Access Network |  | Core Network | **x** |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | Extensions to 26.113 for supporting dynamically changing traffic characteristics | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | Huawei, HiSilicon | | | | | | | | | |
| ***Source to TSG:*** |  | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | FS\_5G\_RTP\_Ph2 | | | | |  | ***Date:*** | | | 2025-04-04 |
|  |  | | | |  | |  | | |  |
| ***Category:*** | **B** |  | | | | | ***Release:*** | | | Rel-19 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-17 (Release 17) Rel-18 (Release 18) Rel-19 (Release 19)  Rel-20 (Release 20)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | 5G RTP Ph2 includes the objective to do normative work for dynamically changing traffic characteristics | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | Adds the singaling in 26.113 for in-band signaling of dynamcially changing traffic characteristics | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | Feature not supported, 5G RTP ph2 objective is not met | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | |  | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  | **x** | Other core specifications | | | | TS/TR ... CR ... | | |
| ***affected:*** | |  | **x** | Test specifications | | | | TS/TR ... CR ... | | |
| ***(show related CRs)*** | |  | **x** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | |  | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | |  | | | | | | | | |

## 10.3 Dynamic Policy API

The Dynamic Policy API allows the RTC Media Session Handler of the RTC Client or the ICE Function of the RTC AS or the WebRTC Signalling Function of the RTC AS to request a specific QoS and/or charging policy to be applied to the application flows of an RTC session. The Dynamic Policy API is invoked as a result of SDP negotiation during the WebRTC signalling phase of the RTC session.

The relevant procedures are specified in clause 5.3.3 of TS 26.510 [3].

The resource structure and the data model are specified in clause 9.3 of TS 26.510 [3].

If specific QoS with PDU Set parameters is desired, and PDU Set marking is not enabled for the selected Policy Template as specified in clause 5.3.3.2 of TS 26.510 [3], the Media Session Handler shall additionally populate the mediaTransportParameters property of the Application‌Flow‌Description object (see clause 5.5.4.13 of TS 29.571 [36]) as follows when creating or updating a Dynamic Policy Instance based on that Policy Template:

- The transportProto property shall be set to the value SRTP.

- The rtpHeaderExtInfo object (see clause 5.5.4.14 of TS 29.571 [36]) shall be omitted.

- The rtpPayloadInfoList property shall contain a single member populated as follows:

- rtpPayloadTypeList shall be set to the *RTP Payload Type* value(s) to be used by the RTC endpoint (e.g., the RTC Access Function of an RTC Client) for the negotiated SRTP session(s) to be carried by the application flow in question.

- rtpPayloadFormat shall be populated as appropriate in the absence of RTP header extensions.

If PDU Set marking is enabled for the selected Policy Template as specified in clause 5.3.3.2 of TS 26.510 [3], the Media Session Handler shall additionally populate the mediaTransportParameters property of the Application‌Flow‌Description object (see clause 5.5.4.13 of TS 29.571 [36]) as follows when creating or updating a Dynamic Policy Instance based on that Policy Template:

- The transportProto property shall be set to the value SRTP.

- The properties of the rtpHeaderExtInfo object (see clause 5.5.4.14 of TS 29.571 [36]) shall be populated as follows:

- rtpHeaderExtType shall be set to PDU\_SET\_MARKING.

- rtpHeaderExtId shall be set to the value of the *ID* field to be used by the RTC endpoint (e.g., the RTC Access Function of an RTC Client) in the *RTP Header Extension for PDU Set Marking* on the application flow in question, as specified in clause 4.2 of TS 26.522 [37]. The value of this parameter is negotiated via the SDP offer/answer procedure during the WebRTC signalling phase of the RTC session.

- longFormat shall be set according to the use of the one- or two-byte *RTP Header Extension for PDU Set Marking*, as specified in clause 4.2.1 of TS 26.522 [37]. The value of this parameter is negotiated via the SDP offer/answer procedure during the WebRTC signalling phase of the RTC session.

- pduSetSizeActive shall be set to reflect the presence of the *PDU Set Size* field in the *RTP Header Extension for PDU Set Marking*, as specified in clause 4.2.4 of TS 26.522 [37]. The value of this parameter is negotiated via the SDP offer/answer procedure during the WebRTC signalling phase of the RTC session.

NOTE: The intention of the RTC Access Function of the RTC Client to include the optional NPDS (Number of PDUs in the PDU Set) field in the *RTP Header Extension for PDU Set Marking* is not yet signalled in advance to the 5G Core by means of a Boolean flag in the RtpHeaderExtInfo specified in clause 5.5.4.14 of TS 29.571 [36].

- The rtpPayloadInfoList property shall contain a single member populated as follows:

- rtpPayloadTypeList shall be set to the *RTP Payload Type* value(s) to be used by the RTC endpoint (e.g., the RTC Access Function of an RTC Client) for the negotiated SRTP session(s) to be carried by the application flow in question.

- rtpPayloadFormat shall be omitted because RTP header extensions are present.

In all PDUs it contributes at reference point RTC‑4m or RTC‑12 that fall within the scope of the application flow description, the RTC Access Function (Media Access Function) shall use the protocol indicated in transportProto; it shall set the SRTP header fields in accordance with rtpPayloadInfoList; and it shall include a one- or two- byte (consistent with the signalled length) *RTP Header Extension for PDU Set Marking* in the SRTP header with fields set according to the values declared in the rtpHeaderExtInfo property per above.

If marking for dynamically changing traffic characteristics is enabled for the selected Policy Template as specified in clause 5.3.3.2 of TS 26.510 [3], the Media Session Handler shall additionally populate the mediaTransportParameters property of the Application‌Flow‌Description object (see clause 5.5.4.13 of TS 29.571 [36]) as follows when creating or updating a Dynamic Policy Instance based on that Policy Template:

- The transportProto property shall be set to the value SRTP.

- The properties of the rtpHeaderExtInfo object (see clause 5.5.4.14 of TS 29.571 [36]) shall be populated as follows:

- rtpHeaderExtType shall be set to DYN\_TRAFFIC\_MARKING.

NOTE: This is pending on an update in CT4 to add DYN\_TRAFFIC\_MARKING to 29.571

- rtpHeaderExtId shall be set to the value of the *ID* field to be used by the RTC endpoint (e.g., the RTC Access Function of an RTC Client) in the *RTP Header Extension for Dynamially Changing Traffic Characteristics* on the application flow in question, as specified in clause 4.5 of TS 26.522 [37]. The value of this parameter is negotiated via the SDP offer/answer procedure during the WebRTC signalling phase of the RTC session.

- longFormat shall be set according to the use of the one- or two-byte *RTP Header Extension for Dynamically changing traffic characteristics*, as specified in clause 4.5 of TS 26.522 [37]. The value of this parameter is negotiated via the SDP offer/answer procedure during the WebRTC signalling phase of the RTC session.

- The rtpPayloadInfoList property shall contain a single member populated as follows:

- rtpPayloadTypeList shall be set to the *RTP Payload Type* value(s) to be used by the RTC endpoint (e.g., the RTC Access Function of an RTC Client) for the negotiated (S)RTP session(s) to be carried by the application flow in question.

- rtpPayloadFormat shall be omitted because RTP header extensions are present.

In all PDUs it contributes at reference point RTC‑4m or RTC‑12 that fall within the scope of the application flow description, the RTC Access Function (Media Access Function) shall use the protocol indicated in transportProto; it may set the SRTP header fields in accordance with rtpPayloadInfoList; and it should include a one- or two- byte (consistent with the signalled length) *RTP Header Extension for Dynamically Changing Traffic Characteristics* in the SRTP header with fields set according to the values declared in the rtpHeaderExtInfo property per above to indicate the dynamically changing traffic characteristic.