**3GPP TSG-SA5 Meeting #140-eS5-216394**

**e-meeting, 15 - 24 November 2021**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.1* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  |  | **CR** |  | **rev** |  | **Current version:** |  |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network | **X** | Core Network | **X** |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | Clarify communication service in requirement CSA-CON-06 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | Ericsson**,** Deutsche Telekom | | | | | | | | | |
| ***Source to TSG:*** | S5 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | COSLA | | | | |  | ***Date:*** | | | 2021-10-28 |
|  |  | | | |  | |  | | |  |
| ***Category:*** | **F** |  | | | | | ***Release:*** | | | Rel-16 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-15 (Release 15) Rel-16 (Release 16) Rel-17 (Release 17) Rel-18 (Release 18)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | Communication services are assured by control loops that monitor and adjust the resources over which the communication services are provided. In REQ-CSA\_CON-06 the phrase “which communication service” is used. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | 1. Update requirement REQ-CSA-CON-06 by adding a NOTE clarifying what in the management system represents a communication service. 2. Editorial update: REQ-CSA-CON-17 is to start on new line. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | Ambiguity in requirement may lead to incompatible implementations | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | 6.2 | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  | **X** | Other core specifications | | | | TS/TR ... CR ... | | |
| ***affected:*** | |  | **X** | Test specifications | | | | TS/TR ... CR ... | | |
| ***(show related CRs)*** | |  | **X** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | |  | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | |  | | | | | | | | |

|  |
| --- |
| **1st change** |

# 2 References

The following documents contain provisions which, through reference in this text, constitute provisions of the present document.

- References are either specific (identified by date of publication, edition number, version number, etc.) or non‑specific.

- For a specific reference, subsequent revisions do not apply.

- For a non-specific reference, the latest version applies. In the case of a reference to a 3GPP document (including a GSM document), a non-specific reference implicitly refers to the latest version of that document *in the same Release as the present document*.

[1] 3GPP TR 21.905: "Vocabulary for 3GPP Specifications".

[2] 3GPP TS 22.261: "Service requirements for the 5G system".

[3] 3GPP TS 28.550: "Management and orchestration; Performance assurance".

[4] 3GPP TS 28.531: "Management and orchestration; Provisioning".

[5] ETSI GS ZSM 002 (V1.1.1) (2019-08): "Zero-touch network and Service Management (ZSM); Reference Architecture".

[6] 3GPP TS 28.545: "Management and orchestration; Fault Supervision (FS)".

[7] 3GPP TS 28.552: "Management and orchestration; 5G performance measurements".

[8] 3GPP TS 28.554: "Management and orchestration; 5G end to end Key Performance Indicators (KPI)".

[9] 3GPP TS 28.532: "Management and orchestration; Generic management services".

[x] 3GPP TS 23.003: " Numbering, addressing and identification"

|  |
| --- |
| **1.5th change** |

2

## 3.3 Abbreviations

For the purposes of the present document, the abbreviations given in 3GPP TR 21.905 [1] and the following apply. An abbreviation defined in the present document takes precedence over the definition of the same abbreviation, if any, in 3GPP TR 21.905 [1].

CN Core Network

CS Communication Service

CSA Communication Service Assurance

CSC Communication Service Customer

CSP Communication Service Provider

eMBB enhanced Mobile BroadBand

KPI Key Performance Indicator

MDAS Management Data Analytics Service

MnS Management Service

NF Network Function

NSI NetworkSlice Instance

NSSI NetworkSlice Subnet Instance

NSP NetworkSlice Provider

NWDAF Network Data Analytics Function

QoE Quality of Experience

SD Slice Differentiator

SLA Service Level agreement

SLS Service Level Specification

S-NSSAI Single Network Slice Selection Assistance Information

SST Slice/ServiceType

|  |
| --- |
| **2nd change** |

## 6.2 Requirements

**REQ-CSA-CON-01** The 3GPP management system shall have the capability to take actions for a set of communication services serving certain group of UEs based on the target SLS.

**REQ-CSA-CON-02** The 3GPP management system shall have the capability to collect service experience information.

**REQ-CSA-CON-03** The 3GPP management system shall have the capability to analyse the performance information related to the set of communication services serving certain group of UEs.

**REQ-CSA-CON-04** The 3GPP management system shall have the capability to modify the configuration parameters related to the set of communication services serving certain group of UEs.

**REQ-CSA-CON-05** The 3GPP management system shall have the capability to collect NSI related data from one or more 5GC NF(s).

NOTE 1: An example for NSI related data may be QoE data.

**REQ-CSA-CON-06** The 3GPP management system shall have the capability to derive which communication service is associated to the QoE data from the collected NSI related QoE data.

NOTE 3: A communication service in the 3GPP management system is identified by an S-NSSAI (the Slice/ServiceType, SST in the S-NSSAI identifies a communication service which can be detailed using the SliceDifferentiattor, SD), see TS 23.003 [x].

**REQ-CSA-CON-07** The 3GPP management system shall have the capability to ascertain SLS breach.

**REQ-CSA-CON-08** The 3GPP management system shall have the capability to perform the root cause analysis (e.g., identifying the underlying reason) for an SLS breach.

**REQ-CSA-CON-09** The 3GPP management system shall have the capability to take corrective actions to ensure the target goal.

**REQ-CSA-CON-10** The 3GPP management system shall have the capability to translate network slice requirements to cross domain network slicesubnet SLS goal and single domain network slicesubnet SLS goal.

**REQ-CSA-CON-11** The 3GPP management system shall have the capability to collect single domain SLS analysis as input to cross domain SLS analysis.

**REQ-CSA-CON-12** The 3GPP management system shall have the capability to allow its authorized consumer to control the SLS assurance (e.g. specify the SLS to be assured, enable/disable, specify the assurance time and update the SLS assurance requirements).

**REQ-CSA-CON-13** The 3GPP management system shall have the capability to allow its authorized consumer to obtain the SLS assurance fulfilment status information.

NOTE 2: The management system refers to the producer of management service for SLS assurance.

**REQ-CSA-CON-14** The 3GPP management system shall have the capability to do network prediction (e.g. network resource usage and network performance) by analysing the network operation information in special scenarios.

**REQ-CSA-CON-15** The 3GPP management system shall have the capability to take actions such asnetwork configuration and perform network resource reallocation according to the network prediction results.

**REQ-CSA-CON-16** The 3GPP management system shall have the capability to allow its authorized consumer to limit the set of action capabilities executable by an assurance closed loop.

**REQ-CSA-CON-17** The 3GPP management system shall allow an authorized consumer to set a condition to enable/disable an ACCL.

**REQ-LCM-CON-01** The 3GPP management system shall have the capability of lifecycle management of a closed control loop.

|  |
| --- |
| **End of changes** |