**3GPP TSG-SA5 Meeting #****140e *S5-216447 revision of S5-216042***

**e-meeting 15th - 24th November 2021**

**Source: Nokia, Nokia Shanghai Bell, Huawei, Asiainfo, Ericsson**

**Title: Description of Information Elements of an Intent**

**Document for: Approval**

**Agenda Item: 6.4.10**

# 1 Decision/action requested

***The group is asked to discuss and approve.***

# 2 References

[1] 3GPP draft TS 28.312: “Management and orchestration; Intent driven management services for mobile networks v0.5.0”.

# 3 Rationale

This contribution proposes to Describe Information Elements of an Intent

.

# 4 Detailed proposal

It proposes to make the following changes to TS 28.312[1].

|  |
| --- |
| **1st Change** |

## 4.n General concept of Intent Content

### 4.n.1 Intent Expectation

In the most basic form, a consumer may use an intent to express to the producer the need for:

" an object O with characteristics S".

Where the characteristics S reflect the requirements, goals and contexts for the object.

The object may be a 3GPP managed object like a slice, subnetwork (e.g. radio network) or other objects like a service . The consumer may desire the same requirements, goals and contexts for multiple objects , in which case the intent may be stated for a list of objects as

" objects {O1,O2, …ON} with characteristics S"

However, the consumer may wish to state different requirements, goal and contexts for different objects. It is in that case necessary to distinguish the requirements, goal and contexts to be achieved for each object. Correspondingly, the combination of requirements, goals and constraints for each object may be termed as the IntentExpectation. Also the consumer may wish to distinguish the requirements, goal and context for different objects , in this case, the combination of requirements, goals and constraints for each instance may be contained in a separate IntentExpectations or requirements, goals and constraints for the multiple instances may be combined in a single IntentExpectation.

### 4.n.2 Expectation Targets

For a given intent expectation, the desired characteristics of the object(s) are the expectation targets to be achieved. The targets may include the metrics that characterize the performance of the object(s) or some abstract index that expresses the behavior of the object(s)). A given intent expectation may include multiple targets on the same object. A consumer may for example require for the Slice object(s) that User throughput > 5Mbps and latency < 1ms.The expectation targets may also be context specific, i.e. the intent may require a specific targets given a specific context. As such with the characteristics as a combination of intent targets and contexts, the intent expectation may be stated as

"ensure that for

ApplicableObject O,

Target\_1 is T\_1, Conext\_1 is C\_1

….,

Target\_m is T\_m, Context\_k is C\_k;

Each Target expresses an aspect of the characteristics of the object under consideration, i.e. it expresses a desired outcome on a specific object State attribute. Each of the object state attributes may be set to be equivalent to a specific value or constrained to a value or a range of values, e.g. as listed in Table 1. The combination of the name of state attribute (or simply the targetName), the condition constraining the attribute and the value or value range for the attribute is the target, i.e. the target is the tuple

target = [ targetName, condition, value range ]

Table 1: Example intent targets for different Objects

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **example of target** | **ApplicableObject** | **targetName** | **Condition** | **Value range** |
| example 1 | Slice | Coverage area | Is at least | 40km radius |
| example 2 | Communication Service | User throughput | Is greater than | 2Mbps |

### 4.n.3 IntentObjects

The object (s) for which a given expectation is addressed can be expressed with the object's identifier.

### 4.n.4 Context

Each target may be constrained to only be achieved for a very specific set of constraints. For example, the consumer may state that: *"ensure that handoverFailureRate < 2% if Load > 80%"*, where the target *"HandoverFailureRate < 2%"* is only to be achieved only in the context *"Load > 80%"*.

Similar to the target, the context is also a tuple of < attribute, condition, value range > but which the values having a different semantics.

Although contexts and targets have the same structure, to distinguish between what must be achieved and the context which is only to be considered as required conditions, the Context has to be explicitly stated separate from the target. For example, if the consumer may wish that the Radio Link Failure rate (RLF) is less than 2% when the load is more than 50%. If the context (i.e. load > 50%) is not explicitly stated/modelled as context, the producer could interpret the request to mean (RLF<2% and load > 50%).

For a given expectation, the specific list of targets may be desired to be achieved for given combined contexts, i.e., besides the Target, an expectation may state a list of contexts which apply to all targets within the intent expectation. Similarly, there may be contexts that apply to all expectations within a given intent. Correspondingly, both Intent expectations and intents should be modelled to contain aggregate contexts that apply to all the contained sub elements.

Editor’s Note: whether using the context or constraint is FFS, which needs to discuss together  with intent definition.

|  |
| --- |
| **End of changes** |