**3GPP TSG-SA5 Meeting #142-e *S5-222368rev1***

**e-meeting, 4 - 12 April 2022**

|  |
| --- |
| *CR-Form-v12.1* |
| **CHANGE REQUEST** |
|  |
|  | **32.256** | **CR** | **0003** | **rev** |  | **Current version:** | **17.0.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **X** |

|  |
| --- |
|  |
| ***Title:***  | Add charging requirement for AMF to support NR RedCap |
| ***、*** |  |
| ***Source to WG:*** | China Mobile Com. Corporation |
| ***Source to TSG:*** | S5 |
|  |  |
| ***Work item code:*** | ARCH\_NR\_REDCAP |  | ***Date:*** | 2022-03-25 |
|  |  |  |  |  |
| ***Category:*** | **B** |  | ***Release:*** | Rel-17 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-15 (Release 15)Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)* |
|  |  |
| ***Reason for change:*** | According to clause 5.41 TS 23.501, The NFs interacting with CHF shall include the NR RedCap as RAT type. Therefore, AMF shall provide the "NR RedCap" as RAT Type to the CHF. |
|  |  |
| ***Summary of change:*** | Add charging requirement to support NR RedCap. |
|  |  |
| ***Consequences if not approved:*** | Misalignment with TS 23.501. |
|  |  |
| ***Clauses affected:*** | 5.2.1.X (New) |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

|  |
| --- |
| **First change** |

#### 5.2.1.X NR REDCAP Charging

The AMF provides for NR RedCap UE using NR the RAT Type NR\_REDCAP, according to clause 5.41 of 3GPP TS 23.501 [200].

|  |
| --- |
| **End of change** |