**3GPP TSG-SA5 Meeting #145eS5-233477**

**15 August to 24 August 2022, E-meeting**

**Source: China Mobile**

**Title: pCR 28.912 issue#4.5.1 Intent report potential solution#1 enhancement**

**Document for: approval**

**Agenda Item: 6.7.3.2**

# 1 Decision/action requested

***The group is asked to discuss and agree on the proposal.***

# 2 References

[1] 3GPP TR 28.912 “Study on enhanced intent driven management services for mobile networks ” V1.2.0 (2023-03)

# 3 Rationale

Intent report potential solution # 1 provides feasible solutions for intent report. However, in the current solution, the conditions for generating intent reports can only be configured through the reportingPeriod parameter, and more complex intent report generation conditions cannot be supported. Moreover, in the current solution, the content of the intent report cannot be customized. Hence it is proposed to introduc report expectation as part of intent IOC, with which MnS consumer can express potential requirements for flexible customization on both the content selection and generation timing of intent report.

Minor corrections in Figure 4.5.2.1-1 is also proposed.

# 4 Detailed proposal

|  |
| --- |
| **Start of Modified** |

## 4.5 Issue#4.5: Intent Report

### 4.5.1 Description

In TS 28.312 [2], the Fulfilment information (including the intentFulfilmentinfo, expectationfulfilmentInfo and targetfulfilmentInfo) are defined for the MnS consumer to monitor the intent fulfilment information. The intent report also can contain the current and optional predicted value for performance indicated by corresponding expectation targets (e.g. WeakRSRPRatio for the weakRSRPRatioTarget, Average UL RAN UE Throughput for aveULRANUEThptTarget), which can be used by MnS consumer to validate whether the intent is really fulfilled and to evaluate whether the intent (especially for expectation targets) needs to be updated if needed (improve the target value when corresponding target is fulfilled or reduce the target value when corresponding target is not fulfilled or not fulfilled with the reason of target confliction). Besides, intent conflict information which send by MnS producer to MnS consumer is another type of intent report information. So, following are the three types of information needs to be monitored by MnS consumer:

* Intent Fulfilment information, which represents the properties of a specific fulfilment information for an aspect of the intent (i.e. either an expectation, a target or the whole intent). The detailed information see clause 6.2.1.3.6 in TS 28.312 [2].
* Achieved values for targets, which represent current performance values for corresponding expectation targets.
* Intent conflict information, which represents conflict type (i.e., intent conflict, expectation conflict and target conflict) and possible solution recommendation to address the conflicts.

Different MnS consumer may have different requirements for intent report (e.g. Some MnS consumer may want to have corresponding performance value information while others don't want, Different MnS consumer may want to calculate or monitor the performance value in different period).

While the report (with the current performance values for corresponding expectation targets) is provided at the end of each observation period, the consumer may also wish to know whether the fulfilment info was consistent for the entire observation period. For example, the intent expectation may be reported FULFILLED at the end of observation period. However, may be possible that within observation period the intent expectation was NOTFULFILLED. The consumer may wish to know this information. This information can be important for the MnS consumer to understand whether the observation period they specified need an update (e.g shortened) or not. Moreover, it helps the MnS consumer to understand whether their expectation is fulfilled during the entire observation period which also gives transparency to the MnS consumer to update their observation period and/or expectations targets specified in the intent.

MnS consumer can also require different intent reports to be generated in different situations. Based on the content selection criteria, Mns consumer can obtain reports of different content according to different conditions. For example, possible to ask for a report about all elements of the intent when the system is getting degraded. If the system complies again, a shorter report might be sufficient.

Reports also can be generated and sent based on events. Events describe significant situations in the operation of intent, and indicate that the intent has reached a particular state. For example, these events can include intent being accepted, intent being rejected, or intent being degraded, etc. The intent driven MnS should allow MnS consumers to require for which events, a report shall be generated by MnS producer. Moreover, MnS consumers can propose other customized requirements for intent report, such as combining complex requirements for frequency, triggering events, and content selection.

**REQ-Intent\_Driven\_MnS\_Report-1:** The intent driven MnS should have the capability to enable the MnS consumer to request intent report information.

**REQ-Intent\_Driven\_MnS\_Report-2:** The intent driven MnS should have the capability to enable the MnS consumer to obtain intent report information with current performance value for corresponding expectation targets.

**REQ-Intent\_Driven\_MnS\_Report-3:** The intent driven MnS should have the capability to enable the MnS consumer to obtain intent report information with intent fulfilment information.

**REQ-Intent\_Driven\_MnS\_Report-4:** The intent driven MnS should have the capability to enable the MnS consumer to obtain intent report information with intent conflict information.

**REQ-Intent\_Driven\_MnS\_Report\_05:** The intent driven MnS should have capability enabling MnS consumer to specify the content of the report.

**REQ-Intent\_Driven\_MnS\_Report\_06:** The intent driven MnS should have capability enabling MnS consumer to configure the frequency, triggering events or other conditions of the intent reporting.

**REQ-Intent\_Driven\_MnS\_Report\_07:** The intent driven MnS should allow MnS consumers to receive reports, with different content and intervals.

**REQ-Intent\_Driven\_MnS\_Report\_08:** The intent driven MnS should allow MnS consumer to obtain reports with current values for specified expectation targets.

**REQ-Intent\_Driven\_MnS\_Report\_09:** The intent driven MnS should have capability enabling MnS consumer to obtain intent report information with current context information for corresponding expectation targets.

**REQ-Intent\_Driven\_MnS\_Report\_10:** The intent driven MnS should allow reports to contain information on whether the fulfilment info was consistent throughout the observation period.

**REQ-Intent\_Driven\_MnS\_Report\_11:** The intent driven MnS should have capability enabling MnS consumer to specify the content selection criteria of the report.

|  |
| --- |
| **End of Modified** |