3GPP TS 28.537 V19.1.0 (2025-03)

Technical Specification

3rd Generation Partnership Project;

Technical Specification Group Services and System Aspects;

Management and orchestration;

Management capabilities

(Release 19)

**



The present document has been developed within the 3rd Generation Partnership Project (3GPP TM) and may be further elaborated for the purposes of 3GPP..  
The present document has not been subject to any approval process by the 3GPPOrganizational Partners and shall not be implemented.  
This Specification is provided for future development work within 3GPPonly. The Organizational Partners accept no liability for any use of this Specification.  
Specifications and Reports for implementation of the 3GPP TM system should be obtained via the 3GPP Organizational Partners' Publications Offices.

***3GPP***

Postal address

3GPP support office address

650 Route des Lucioles - Sophia Antipolis

Valbonne - FRANCE

Tel.: +33 4 92 94 42 00 Fax: +33 4 93 65 47 16

Internet

http://www.3gpp.org

***Copyright Notification***

No part may be reproduced except as authorized by written permission.  
The copyright and the foregoing restriction extend to reproduction in all media.

© 2024, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

All rights reserved.

UMTS™ is a Trade Mark of ETSI registered for the benefit of its members

3GPP™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners  
LTE™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners

GSM® and the GSM logo are registered and owned by the GSM Association

Contents

Foreword 5

1 Scope 7

2 References 7

3 Definitions of terms, symbols and abbreviations 7

3.1 Terms 7

3.2 Symbols 7

3.3 Abbreviations 8

4 Heartbeat 8

4.1 Overview 8

4.2 Specification level requirements 8

4.2.1 Use cases 8

4.2.1.1 Configuring heartbeat notification periodicity 8

4.2.1.2 Requesting immediate heartbeat notification 9

4.2.1.3 Emitting periodic heartbeat notifications 9

4.2.2 Requirements 9

4.2.2.1 Requirements for controlling heartbeat 9

4.2.2.2 Requirements for notifying heartbeat 10

4.3 Procedures for heartbeat 10

4.3.1 Procedure for configuring heartbeat notification periodicity 10

4.3.2 Procedure for requesting immediate heartbeat notification 10

4.3.3 Procedure for notifying periodic heartbeat notifications 11

5 Discovery of Management Services 12

5.1 Overview 12

5.2 Specification level requirements 12

5.2.1 Use cases 12

5.2.1.1 Adding a new management service producer to MnS registry 12

5.2.1.2 Removing a management service producer from MnS registry 13

5.2.1.3 MnS Consumer retrieves management service information from MnS registry 13

5.2.1.4 Providing detailed capabilities about management service 13

5.2.1.5 MnS Consumer retrieves detailed capabilities about management service 14

5.2.2 Requirements 14

6 Managing management data 14

6.1 Producing and reporting management data 14

6.1.1 Description 14

6.1.2 Void 15

6.1.3 Requirements 15

6.2 Coordinating management data production 16

6.2.1 Description 16

6.2.2 Use cases 16

6.2.3 Requirements 16

6.3 Storing management data 16

6.3.1 Description 16

6.3.2 Void 17

6.3.3 Requirements 17

6.4 Managing external management data 17

6.4.1 Description 17

6.4.2 Void 17

6.4.3 Requirements 17

6.5 Discovery of management data 18

6.5.1 Description 18

6.5.2 Void 18

6.5.3 Requirements 18

7 File management 18

7.1 File transfer 18

7.1.1 Description 18

7.1.2 Void 18

7.1.3 Requirements 18

7.2 File retrieval from a MnS producer by a MnS consumer 19

7.2.1 Description 19

7.2.2 Void 19

7.2.3 Requirements 19

7.3 File push from a MnS producer to a MnS consumer 19

7.3.1 Description 19

7.3.2 Void 19

7.3.3 Requirements 19

7.4 File download from a MnS consumer to a MnS producer 20

7.4.1 Description 20

7.4.2 Void 20

7.4.3 Requirements 20

Annex A (informative): Heartbeat PlantUML source code 20

A.1 Procedure for configuring heartbeat notification periodicity 20

A.2 Procedure for requesting immediate heartbeat notification 21

A.3 Procedure for notifying periodic heartbeat notifications 21

Annex B (informative): Change history 23

# Foreword

This Technical Specification has been produced by the 3rd Generation Partnership Project (3GPP).

The contents of the present document are subject to continuing work within the TSG and may change following formal TSG approval. Should the TSG modify the contents of the present document, it will be re-released by the TSG with an identifying change of release date and an increase in version number as follows:

Version x.y.z

where:

x the first digit:

1 presented to TSG for information;

2 presented to TSG for approval;

3 or greater indicates TSG approved document under change control.

y the second digit is incremented for all changes of substance, i.e. technical enhancements, corrections, updates, etc.

z the third digit is incremented when editorial only changes have been incorporated in the document.

In the present document, certain modal verbs have the following meanings:

**shall** indicates a mandatory requirement to do something

**shall not** indicates an interdiction (prohibition) to do something

The constructions "shall" and "shall not" are confined to the context of normative provisions, and do not appear in Technical Reports.

The constructions "must" and "must not" are not used as substitutes for "shall" and "shall not". Their use is avoided insofar as possible, and they are not used in a normative context except in a direct citation from an external, referenced, non-3GPP document, or so as to maintain continuity of style when extending or modifying the provisions of such a referenced document.

**should** indicates a recommendation to do something

**should not** indicates a recommendation not to do something

**may** indicates permission to do something

**need not** indicates permission not to do something

The construction "may not" is ambiguous and is not used in normative elements. The unambiguous constructions "might not" or "shall not" are used instead, depending upon the meaning intended.

**can** indicates that something is possible

**cannot** indicates that something is impossible

The constructions "can" and "cannot" shall not to be used as substitutes for "may" and "need not".

**will** indicates that something is certain or expected to happen as a result of action taken by an agency the behaviour of which is outside the scope of the present document

**will not** indicates that something is certain or expected not to happen as a result of action taken by an agency the behaviour of which is outside the scope of the present document

**might** indicates a likelihood that something will happen as a result of action taken by some agency the behaviour of which is outside the scope of the present document

**might not** indicates a likelihood that something will not happen as a result of action taken by some agency the behaviour of which is outside the scope of the present document

In addition:

**is** (or any other verb in the indicative mood) indicates a statement of fact

**is not** (or any other negative verb in the indicative mood) indicates a statement of fact

The constructions "is" and "is not" do not indicate requirements.

# 1 Scope

The present document specifies use cases, requirements and procedures for management capabilities of 5G networks.

# 2 References

The following documents contain provisions which, through reference in this text, constitute provisions of the present document.

- References are either specific (identified by date of publication, edition number, version number, etc.) or non‑specific.

- For a specific reference, subsequent revisions do not apply.

- For a non-specific reference, the latest version applies. In the case of a reference to a 3GPP document (including a GSM document), a non-specific reference implicitly refers to the latest version of that document *in the same Release as the present document*.

[1] 3GPP TR 21.905: "Vocabulary for 3GPP Specifications".

[2] 3GPP TS 28.532: "Management and orchestration; Generic management services".

[3] 3GPP TS 28.533: " Management and orchestration; Architecture framework".

[4] 3GPP TS 28.552: "Management and orchestration; 5G performance measurements".

[5] 3GPP TS 28.554: "Management and orchestration; 5G end to end Key Performance Indicators (KPI)".

[6] 3GPP TS 32.422: "Telecommunication management; Subscriber and equipment trace; Trace control and configuration management".

[7] 3GPP TS 32.404: "Telecommunication management; Performance Management (PM); Performance measurements; Definitions and template".

[8] 3GPP TS 32.423: "Telecommunication management; Subscriber and equipment trace: Trace data definition and management".

[9] 3GPP TS 28.622: "Telecommunication management; Generic Network Resource Model (NRM) Integration Reference Point (IRP); Information Service (IS) "

[10] 3GPP TS 28.623: "Telecommunication management; Generic Network Resource Model (NRM) Integration Reference Point (IRP); Solution Set (SS) definitions "

# 3 Definitions of terms, symbols and abbreviations

## 3.1 Terms

For the purposes of the present document, the terms given in 3GPP TR 21.905 [1] and the following apply. A term defined in the present document takes precedence over the definition of the same term, if any, in 3GPP TR 21.905 [1].

**Trace metrics:** This term is defined in TS 32.422 [6].

## 3.2 Symbols

Void.

## 3.3 Abbreviations

For the purposes of the present document, the abbreviations given in 3GPP TR 21.905 [1] and the following apply. An abbreviation defined in the present document takes precedence over the definition of the same abbreviation, if any, in 3GPP TR 21.905 [1].

MnS Management Service

# 4 Heartbeat

## 4.1 Overview

The communication between Management Service (MnS) producers and MnS consumers shall be monitored, and communication link breaks between them shall be discovered by MnS consumers as early as possible. The behaviour of the MnS consumers, after detection of communication failure, is outside the scope of the present document.

## 4.2 Specification level requirements

### 4.2.1 Use cases

#### 4.2.1.1 Configuring heartbeat notification periodicity

| Use case stage | Evolution/Specification | <<Uses>> Related use |
| --- | --- | --- |
| **Goal** | To configure the periodicity at which the management service producer shall emit heartbeat notifications to its authorized management service consumer. |  |
| **Actors and Roles** | An authorized consumer of the management service. |  |
| **Telecom resources** | The management service producer. |  |
| **Assumptions** | N/A |  |
| **Pre-conditions** | The periodicity requested by the management service consumer has a valid value. |  |
| **Begins when** | The management service consumer sends a request to the management service producer to set the periodicity at which it shall emit heartbeat notifications. |  |
| **Step 1** | The management service producer receives the request and sets its internal countdown timer to a value (which can be zero) equal to the periodicity requested by the management service consumer. |  |
| **Step 2** | The management service producer sends a heartbeat notification to all authorized management service consumer(s), provided they previously subscribed to heartbeat notifications. |  |
| **Ends when** | All the steps identified above are successfully completed. |  |
| **Exceptions** | One of the steps identified above fails. |  |
| **Post-conditions** | The notification periodicity has been configured according to the management service consumer request.  A heartbeat notification is sent out to all authorized management service consumer(s). |  |
| **Traceability** | REQ-HB-CTRL-2. |  |

#### 4.2.1.2 Requesting immediate heartbeat notification

| Use case stage | Evolution/Specification | <<Uses>> Related use |
| --- | --- | --- |
| **Goal** | To trigger the emission of an immediate heartbeat notification by the management service producer. |  |
| **Actors and Roles** | An authorized consumer of the management service. |  |
| **Telecom resources** | The management service producer. |  |
| **Assumptions** | N/A |  |
| **Pre-conditions** | N/A |  |
| **Begins when** | The soliciting management service consumer sends a request to the management service producer to emit immediately a heartbeat notification. |  |
| **Step 1** | The management service producer receives the request and sends immediately a heartbeat notification to all authorized management service consumer(s) who had previously subscribed to heartbeat notifications.  The management service producer countdown timer is not impacted. |  |
| **Ends when** | All the steps identified above are successfully completed. |  |
| **Exceptions** | One of the steps identified above fails. |  |
| **Post-conditions** | The immediate heartbeat notification has been emitted according to the soliciting management service consumer request. |  |
| **Traceability** | REQ-HB-CTRL-3, REQ-HB-NOTIF-2. |  |

#### 4.2.1.3 Emitting periodic heartbeat notifications

| Use case stage | Evolution/Specification | <<Uses>> Related use |
| --- | --- | --- |
| **Goal** | To send periodic heartbeat notifications at the periodicity requested by the management service consumer. |  |
| **Actors and Roles** | An authorized producer of the management service. |  |
| **Telecom resources** | The management service consumer. |  |
| **Assumptions** | The heartbeat notification periodicity has been configured according to the management service consumer request. | Configuring heartbeat notification periodicity |
| **Pre-conditions** | N/A |  |
| **Begins when** | The internal countdown timer managed by the management service producer has reached the value 0. |  |
| **Step 1** | The management service producer sends a heartbeat notification to all authorized management service consumer(s), provided they previously subscribed to heartbeat notifications. |  |
| **Step 2** | The management service producer resets its internal countdown timer to the value of the heartbeat notification periodicity. | Configuring heartbeat notification periodicity |
| **Ends when** | All the steps identified above are successfully completed. |  |
| **Exceptions** | One of the steps identified above fails. |  |
| **Post-conditions** | The periodic heartbeat notification has been emitted to all authorized management service consumer(s) at the requested periodicity. |  |
| **Traceability** | REQ-HB-NOTIF-1. |  |

### 4.2.2 Requirements

#### 4.2.2.1 Requirements for controlling heartbeat

REQ-HB-CTRL-1: The management service producer shall have the capability to allow its authorized consumer to read the heartbeat period.

REQ-HB-CTRL-2: The management service producer shall have the capability to allow its authorized consumer to set the heartbeat period.

REQ-HB-CTRL-3: The management service producer shall have the capability to allow its authorized consumer to request the emission of an immediate heartbeat notification.

#### 4.2.2.2 Requirements for notifying heartbeat

REQ-HB-NOTIF-1: The management service producer shall have the capability to send periodic heartbeat notifications to its authorized consumer at the frequency specified by the management service consumer.

REQ-HB-NOTIF-2: The management service producer shall have the capability to send immediate heartbeat notifications to its authorized consumer, upon request from the management service consumer.

## 4.3 Procedures for heartbeat

### 4.3.1 Procedure for configuring heartbeat notification periodicity

Figure 4.3.1-1 illustrates the procedure for configuring the periodicity of heartbeat notifications using operations and notifications of the provisioning MnS (see clause 11.1.1 of [2]).




Figure 4.3.1-1: Procedure for configuring heartbeat notification periodicity

### 4.3.2 Procedure for requesting immediate heartbeat notification

Figure 4.3.2-1 illustrates the procedure for requesting immediate heartbeat notification using operations and notifications of the provisioning MnS (see clause 11.1.1 of [2]).




Figure 4.3.2-1: Procedure for requesting immediate heartbeat notification

### 4.3.3 Procedure for notifying periodic heartbeat notifications

Figure 4.3.3-1 illustrates the procedure for notifying periodic heartbeat notifications using operations and notifications of the provisioning MnS (see clause 11.1.1 of [2]).




Figure 4.3.3-1: Procedure for notifying periodic heartbeat notifications

## 4.4 Solutions

### 4.4.1 Stage 2 definition

Following are the stage 2 definitions for controlling heartbeat:

* The operations and notifications of generic provisioning MnS defined in clause 11.1 in TS 28.532 [2].
* The Heartbeat notification control NRM fragment defined in clause 4.3.21 and clause 4.3.22 in TS 28.622 [9].

Following are the stage 2 definition for notifying heartbeat

* The Heartbeat notification defined in clause 11.4 in TS 28.532 [2].

### 4.4.2 Stage 3 definition

Following are the stage 3 definition for controlling heartbeat

* RESTful HTTP-based solution set

- RESTful HTTP-based solution set for generic provisioning management service is defined in clause 12.1.1 in TS 28.532 [2]. Correponding OpenAPI document "TS28532\_ProvMnS.yaml" in clause A.1 in TS 28.532 [2].

- OpenAPI document "TS28623\_SubscriptionControlNrm.yaml" in clause 4.3 in TS 28.623 [10].

* YANG/Netconf-based solution set

- YANG/Netconf-based solution set for generic provisioning management service is defined in clause 12.1.3 in TS 28.532 [2].

- YANG model "\_3gpp-common-subscription-control.yang" in clause 4.4. in TS 28.623 [10].

Following are the stage 3 definition for notifying heartbeat

- RESTful HTTP-based solution set for heartbeat notification is defined in clause 12.1.1 in TS 28.532 [2].

- OpenAPI document " TS28532\_HeartbeatNtf.yaml " in clause A.5 in TS 28.532 [2].

# 5 Discovery of Management Services

## 5.1 Overview

To enable communication between MnS Consumers and MnS Producers, MnS Consumers need mechanisms to discover management service information available in the 3GPP management system, and their management capabilities. To this end, MnS Producers and their management capabilities need to be exposed in the 3GPP management system.

From management service perspective the following information can be exposed:

- Identifying data describing an MnS, e.g. name, version, type

- Capabilities of an MnS, e.g. supported operations, supported notifications

From MnS Consumer perspective such information can be used for different purposes, including:

- MnS Producer discovery: allows MnS Consumer to discover identifying information about an MnS Producer instance. In short, allows MnS Consumer to know which MnS Producers instances are exposed.

- MnS Producer Capabilities retrieval: allows MnS Consumer to retrieve capability information about an MnS Producer instance. In short, allows MnS Consumer to know what an MnS Producer instance is capable of.

In case an exposed MnS Producer instance’s information changes the 3GPP management system needs to be updated.

MnS Consumers wishing to discover MnS Producer instances might have different questions. For example, an MnS Consumer may wish to know which MnS Producers manage a certain geographical area or civic location. Or, after receiving an alarm notification specifying that a specific NF is alarmed, they may wish to know the MnS Producers from which they can request management data from that NF or to retrieve the configuration of that NF.

## 5.2 Specification level requirements

### 5.2.1 Use cases

#### 5.2.1.1 Adding a new management service producer to MnS registry

| Use case stage | Evolution/Specification | <<Uses>> Related use |
| --- | --- | --- |
| **Goal** | Add a MnS producer to a 3GPP management system. |  |
| **Actors and Roles** | MnS Producer, MnS Registry |  |
| **Telecom resources** | MnS producer.  MnS discovery service producer. |  |
| **Assumptions** | MnS producer is ready to be added to MnS registry. |  |
| **Pre-conditions** | The MnS Producer is available. |  |
| **Begins when** | There is a need for a MnS producer to be exposed via MnS registry. |  |
| **Step 1 (M)** | The MnS producer is added to the MnS registry. |  |
| **Ends when** | All the steps identified above are successfully completed. |  |
| **Exceptions** | One of the mandatory steps fails. |  |
| **Post-conditions** | MnS discovery service producer has stored the MnS information. |  |
| **Traceability** | REQ-DMS-1 |  |

#### 5.2.1.2 Removing a management service producer from MnS registry

| Use case stage | Evolution/Specification | <<Uses>> Related use |
| --- | --- | --- |
| **Goal** | Remove a MnS producerfrom MnS registry.. |  |
| **Actors and Roles** | Network operator. |  |
| **Telecom resources** | MnS producer. |  |
| **Assumptions** | - |  |
| **Pre-conditions** | The management service producer is no longer required in the MnS registry. |  |
| **Begins when** | The management service is ready to be removed from MnS Registry. |  |
| **Step 1 (M)** | The management service producer is removed from the MnS Registry. |  |
| **Ends when** | All the steps identified above are successfully completed. |  |
| **Exceptions** | One of the mandatory steps fails. |  |
| **Post-conditions** | MnS discovery service producer has removed the MnS information related to the MnS Producer. |  |
| **Traceability** | REQ-DMS-1 |  |

#### 5.2.1.3 MnS Consumer retrieves management service information from MnS registry

| Use case stage | Evolution/Specification | <<Uses>> Related use |
| --- | --- | --- |
| **Goal** | MnS consumer retrieves information from MnS registry. |  |
| **Actors and Roles** | MnS Consumer |  |
| **Telecom resources** | MnS registry |  |
| **Assumptions** | MnS consumer is authorized to obtain the MnS information for the available management service(s) from MnS discovery service producer. |  |
| **Pre-conditions** | MnS information exists in MnS registry. |  |
| **Begins when** | MnS Consumer needs to access a specific MnS Producer(s). |  |
| **Step 1 (M)** | MnS Consumer queries MnS Registry with filter criteria based on the management service(s) of interest. |  |
| **Step 2 (M)** | MnS Consumer receives response with MnS Info for the management service(s) which match the criteria. |  |
| **Ends when** | All the steps identified above are successfully completed. |  |
| **Exceptions** | One of the mandatory steps fails. |  |
| **Post-conditions** | MnS Consumer has basic information about the management service(s). |  |
| **Traceability** | REQ-DMS-2, REQ-DMS-3, REQ-DMS-4 |  |

NOTE: MnS information refer to the information used by the consumer to discover the producers of specific Management Services and to derive the addresses of the Management Service.

#### 5.2.1.4 Providing detailed capabilities about management service

| Use case stage | Evolution/Specification | <<Uses>> Related use |
| --- | --- | --- |
| **Goal** | Management service detailed capabilities are exposed. |  |
| **Actors and Roles** |  |  |
| **Telecom resources** | - |  |
| **Assumptions** | Management service detailed capabilities are available. |  |
| **Pre-conditions** | Management service detailed capabilities are ready to be exposed. |  |
| **Begins when** | MnS Producer wants to expose its detailed capabilities. |  |
| **Step 1 (M)** | Management service detailed capabilities are exposed by MnS Producer. |  |
| **Post-conditions** | Management services detailed capabilities have been exposed. |  |
| **Traceability** |  |  |

#### 5.2.1.5 MnS Consumer retrieves detailed capabilities about management service

| Use case stage | Evolution/Specification | <<Uses>> Related use |
| --- | --- | --- |
| **Goal** | MnS Consumer retrieves detailed capabilities for specific MnS Producer(s). |  |
| **Actors and Roles** | MnS Consumer |  |
| **Telecom resources** | - |  |
| **Assumptions** | Management service has ability to expose its detailed capabilities. |  |
| **Pre-conditions** | Authorized MnS Consumer knows location and method to retrieve detailed capabilities. |  |
| **Begins when** | MnS Consumer requires to retrieve detailed capabilities of specific MnS Producer(s). |  |
| **Step 1 (M)** | MnS Consumer reads detailed capabilities from MnS Producer of interest. |  |
| **Post-conditions** | MnS Consumer has retrieved detailed capabilities of specific MnS Producer(s). |  |
| **Traceability** |  |  |

### 5.2.2 Requirements

**REQ-DMS-1:** The 3GPP management system shall provide capabilities allowing MnS producers to register their management capabilities (including the endpoint address) at MnS discovery service producer for use by MnS consumers wishing to interact with these MnS producers.

**REQ-DMS-2:** The 3GPP management system shall provide capabilities allowing MnS consumers to retrieve the management capabilities registered at MnS discovery service producer by MnS producers.

**REQ-DMS-3:** The 3GPP management system shall provide capabilities allowing to discover MnS producers that are managing a specified managed entity.

**REQ-DMS-4:** The 3GPP management system shall provide capabilities allowing to discover the managed entities a MnS producer is responsible for.

### 5.2.3 Solutions

#### 5.2.3.1 Stage 2 definition

Following are the stage 2 definition for Discovery of Management Services:

- The operations and notifications of generic provisioning MnS defined in clause 11.1 in TS 28.532 [2].

- The MnSRegistry NRM fragment defined in clause 4.3.41 and clause 4.3.42 in TS 28.622 [9].

#### 5.2.3.2 Stage 3 definition

Following are the stage 3 definition for Discovery of Management Services:

- RESTful HTTP-based solution set

- RESTful HTTP-based solution set for generic provisioning management service is defined in clause 12.1.1 in TS 28.532 [2]. OpenAPI document "TS28532\_ProvMnS.yaml" in clause A.1 in TS 28.532 [2].

- OpenAPI document " TS28623\_MnSRegistryNrm.yaml" in clause 4.3 in TS 28.623 [10].

- YANG/Netconf-based solution set

- YANG/Netconf-based solution set for generic provisioning management service is defined in clause 12.1.3 in 3GPP TS 28.532 [2].

- YANG model " 3gpp-common-mnsregistry.yang" in clause 4.4 TS 28.623 [10].

### 5.3 Usage of MnS Registry for different deployment scenarios

Following are potential deployment scenarios for MnS Registry (i.e. act as discover MnS producer):

**- Deployment scenario #1: Separate MnSRegistry.** The MnS Registry and a concrete MnS producer are separate entities with a published interface between them. In this scenario, the MnS Registry is used to store the MnS information for MnS instances provided by different MnFs, especially for different MnFs from different vendors. Following is one example, MnF\_1 needs to register MnS\_1 information in the MnS Registry implemented in MnF\_3, and MnF\_2 needs to discover/retrieve the MnS\_1 information from MnF\_3 to consume MnS\_1 provided by MnF\_1. In this scenario, MnS Registry needs to support both registry and discovery/retrieve capabilities.




Figure 5.3-1 Example of Separate MnSRegistry deployment scenario

**- Deployment scenario #2: Embedded MnSRegistry.** The MnsRegistry and a concrete MnS producer are hosted by the same entity with an implementation specific interface between them. The MnS Registry is implemented in an MnF and used to store the MnS Information for MnS instances provided by the MnF itself. Following is one example, MnF\_3 needs to retrieve/discover MnS\_1 information in the MnSRegistry implemented in MnF\_1. In this scenario, MnS Registry supports discovery/retrieve capabilities only.




Figure 5.3-2 Example of Embedded MnSRegistry deployment scenario

# 6 Managing management data

## 6.1 Producing and reporting management data

### 6.1.1 Description

Management data is referring to data produced by radio access network functions, core network functions or management functions and used for management purposes. Management data specified by 3GPP for 5G management is classified into 5G performance measurements as defined by TS 28.552 [4], 5G end to end key performance indicators as defined by TS 28.554 [5] and Trace metrics as defined by TS 32.423 [8]. The combined performance measurements and key performance indicators are also called performance metrics.

Management data is produced on request. Therefore, the 3GPP management system needs to enable a data consumer to request management data to be produced. The data requester needs to specify the type of data to be produced as well as the radio access network functions, core network functions and management functions where the data shall be produced. The target managed object instances can be identified in multiple ways:

- The requester can specify the target managed object instances based on the managed object tree (as defined in the 3GPP Network Resource Models) representing the network and management functions. The simplest approach is to directly identify the managed object instances where data shall be produced. More sophisticated approaches allow to specify one or more subtrees where data shall be produced and may allow also to specify managed object classes to select only object instances of specific classes.

- The requester can specify one or multiple of the following selection criteria. The system needs to translate this information into the target managed object instances. The selection criteria need to be deterministic in such a way that the target node(s) can be selected unambiguously.

- Area of interest: In a big network, it makes sense to specify a limited area for which data shall be produced. The area of interest can be expressed for example with a geographical area, one or several cells or one or several tracking areas. The target managed object instances represent network functions serving that area of interest. Geographical areas can be expressed for example with multiple longitude-latitude pairs that define a convex polygon. In the radio domain the geographical area needs to be mapped to the coverage area of cells supported by RAN NE(s). The managed object instances (e.g. NRCellCU, GNBDUFunction) providing service to these cells can be identified as target managed object instances. Of course the coverage area of the target cell(s) will usually not exactly map to the described shape of the geographical area because, on the one side, the coverage area of cell has no sharp borders due to fast fading effects, on the other side, the coverage area of cells may vary slightly e.g. due to adaptation of the antenna downtilt angle or beamforming configurations. For the mapping between the geographical area and the corresponding managed object instances the cell coverage status at the time of the request shall be used. Later changes affecting the cell coverage shall not be reflected for the mapping.

- Domain e.g RAN, CN: A consumer might only be interested in analysing and understanding the performance of a particular domain like RAN or Core e.g in case of recurrent issues, a consumer may want to have understanding of a particular domain only for further actions. In such a scenario, it should be possible to indicate the domain from where consumer wants measurements for its usage.

- Traffic type e.g user plane or control plane: 5G brings clear separation (CUPS) of user plane and control plane in a network, a consumer may leverage it to identify target managed object instances to have measurements from. For example, the measurement report may be expected from user plane nodes only.

- Slice type e.g eMBB, URLLC: Consumer may mention a particular slice type (eMBB, URLLC, mIoT, V2X, HMTC) as the selection criteria. It may help in narrowing down the target managed object instances, which are part of provided slice type(s).

This MnS to request management data in a simple way shall not be exposed at any network function.

The management data can be requested according to a certain time scheduler. The consumer can e.g. specify a start and stop time or can request for data at specific days of a week or specific hours of a day..

After production the data needs to be reported to the data consumers. Reporting can be based on multiple reporting methods such as file or streaming. Data reporting needs to be requested by the data consumer. The requestor needs to specify the control parameters for reporting such as the reporting method and the address the data shall be delivered to.

Depending on access rights and security settings, data consumers may be subject to restrictions regarding the data they can access.

Data is always produced in some context. The data describing this context is called context data. Context data contains information on all interrelated conditions in which the management data is produced. This includes for example the configuration of the measured network functions, information on the network entity where the network function is running such as vendor name or software version, but also alarms associated to the network function or load conditions.

Data consumers processing managemen data in an effort to accomplish some task typically benefit when taking context data into account. For that reason data consumers should be able to obtain the context data for the management data they obtain. However, access to certain management data does not automaticlly imply access to all context data. Access to management data and access to context data may be subject to different data security and data protection considerations.

### 6.1.2 Void

### 6.1.3 Requirements

REQ-MDM-PR-1: The 3GPP management system shall enable an authorized data consumer to request management data (specified by 3GPP) to be produced.

REQ-MDM-PR-2: The 3GPP management system shall enable an authorized data consumer to request management data specified by 3GPP to be produced by certain managed object instance(s) only. The selection criteria to determine the managed object instance(s) shall be deterministic in such a way that the target node(s) can be selected unambiguously. The managed object instances can be targeted based on:

- Area of interest (e.g. list of cells, list of tracking areas or geographical area).

- Domain (CN or RAN).

- User plane or control plane.

- Slice type (e.g. eMBB, URLLC, mIoT, V2X, HMTC).

The MnS to request management data specified by 3GPP in a simple way shall not be exposed at any network function.

The mapping of geographical area to corresponding managed object instances reflects the cell coverage status at the time of the request.

REQ-MDM-PR-3: The 3GPP management system shall enable an authorized data consumer to request management data specified by 3GPP to be produced according to a certain time scheduler.

REQ-MDM-PR-4: The 3GPP management system shall enable an authorized data consumer to request management data (specified by 3GPP) to be reported to the requesting or another authorized data consumer.

REQ-MDM-PR-5: The 3GPP management system shall enable an authorized data consumer to obtain context data for management data. Access to management data does not imply access to context data. Different data privacy considerations may apply.

NOTE: The term "management data specified by 3GPP" relates to

- 5G performance measurements as defined by TS 28.552 [4]

- 5G end to end key performance indicators as defined by TS 28.554 [5], and

- Trace metrics as defined by TS 32.423 [8].

### 6.1.4 Solutions

#### 6.1.4.1 Stage 2 definition

Following are the stage 2 definition for producing and reporting management data.

- The operations and notifications of generic provisioning MnS defined in clause 11.1 in TS 28.532 [2].

- The ManagementDataCollection control NRM fragment defined in clause 4.3.47 in TS 28.622 [9].

#### 6.1.4.2 Stage 3 definition

Following are the stage 3 definition for MnS Registry and Discovery management capability.

- RESTful HTTP-based solution set

- RESTful HTTP-based solution set for generic provisioning management service is defined in clause 12.1.1 in 3GPP TS 28.532 [2]. OpenAPI document "TS28532\_ProvMnS.yaml" in clause A.1 in TS 28.532 [2].

- OpenAPI document " TS28623\_ManagementDataCollectionNrm.yaml " in clause 4.3 in TS 28.623 [10].

- YANG/Netconf-based solution set

- YANG/Netconf-based solution set for generic provisioning management service is defined in clause 12.1.3 in 3GPP TS 28.532 [2].

- YANG model "\_3gpp-common-managementdatacollection.yang " in clause 4.4 in TS 28.623 [10].

## 6.2 Coordinating management data production

### 6.2.1 Description

Many consumers can request network or management functions to produce management data. In this context it is beneficial to coordinate data requests at the management level to optimize management data production.

### 6.2.2 Void

### 6.2.3 Requirements

REQ-MDM-C-1: The 3GPP management system shall coordinate requests from several data consumers to avoid producing multiple times the same data at a certain point of time.

## Note: The definition of “same data” is not addressed in the current document.6.3 Storing management data

### 6.3.1 Description

Storing management data enables reusage of management data for multiple management purposes.

For example, AI/ML models need input data collected over a certain period of time for training purposes. A specific set of collected data may serve different purposes and can therefore be input to multiple AI/ML services. For example, management data collected in a geographical area may be used also for another geographical area when the scenarios in the areas are statistically similar.

Another use case for storing produced data is related to the fact that multiple sets of training data from similar scenarios are typically required. For example, one set of data produced for the rush hour in a subway station on a single weekday is typically not enough for profiling. Many sets produced on many workdays are required.

Stored data is useful when management functions can discover which data has been produced and stored in the past to check if the currently needed data is already available.

### 6.3.2 Void

### 6.3.3 Requirements

REQ-MDM-S-1: The 3GPP management system shall support the storing of produced management data.

REQ-MDM-S-2: The 3GPP management system shall enable an authorized data consumer to discover stored management data.

REQ-MDM-S-3: The 3GPP management system shall enable an authorized data consumer to retrieve stored management data.

## 6.4 Managing external management data

### 6.4.1 Description

Management data which is specified by 3GPP (clause 6.1.1) can be enriched by additional data not specified by 3GPP. This so-called external management data can be produced by data sources of different nature (e.g. sensors) with different formats.

Note that management data that is not defined by 3GPP but specified based on 3GPP defined management data definition templates and frameworks (such as the measurement definition template in TS 32.404 [7]) is not considered as external management data.

External management data can be used for example as additional input for network optimization and prediction.

The management system should be able to manage this kind of data. That means data consumers should be able to request external management data to be produced and reported. The management system should provide support for storing it.

The definition of external data sources and the data formats they use is out of scope of this specification.

The target is to define generic management mechanisms that can cope with any kind of external data sources and data formats.

### 6.4.2 Void

### 6.4.3 Requirements

REQ-MDM-ED-1: The 3GPP management system shall enable an authorized data consumer to request external management data to be produced.

REQ-MDM-ED-2: The 3GPP management system shall enable an authorized data consumer to request external management data to be reported to the requesting or another authorized data consumer.

REQ-MDM-ED-3: The 3GPP management system shall support the storing of produced external management data.

REQ-MDM-ED-4: The 3GPP management system shall enable an authorized data consumer to discover stored external management data.

REQ-MDM-ED-5: The 3GPP management system shall enable an authorized data consumer to retrieve stored external management data.

NOTE: The term "external management data" relates to data not specified by 3GPP.

## 6.5 Discovery of management data

### 6.5.1 Description

Discovery of management data mechanism allows MnS consumers to discover what management data can be produced by the 3GPP management system without direct involvement of those MnS services producing the data, which can be time and resource consuming process.

For this mechanism to work MnS producers as entities producing data, need to register what data they can produce by adding a corresponding record in the 3GPP management system.

NOTE: The term "management data produced by 3GPP management system" relates to

- 5G performance measurements as defined by TS 28.552 [4]

- 5G end to end key performance indicators as defined by TS 28.554 [5], and

- Trace metrics as defined by TS 32.423 [8].

### 6.5.2 Void

### 6.5.3 Requirements

REQ-MDM-DIS-1: The 3GPP management system shall enable an authorized data consumer to discover what management data can be produced by 3GPP management system.

# 7 File management

## 7.1 File transfer

### 7.1.1 Description

File management deals with transferring files between MnS producers and MnS consumers.

Existing file transfer protocols are used. These protocols need to comply to requirements specified in this clause.

### 7.1.2 Void

### 7.1.3 Requirements

REQ-FM-G-1: The file transfer protocol shall preserve the formatting of the file during exchange.

REQ-FM-G-2: The file transfer protocol shall preserve the encoding of the file during exchange.

REQ-FM-G-3: The MnS producer shall support at least one of the following file transfer protocols: SFTP, FTPES, HTTPS.

REQ-FM-G-4: The MnS consumer shall use the file transfer protocol supported by the MnS producer.

## 7.2 File retrieval from a MnS producer by a MnS consumer

### 7.2.1 Description

File retrieval is when the MnS consumer retrieves (gets) a file from the MnS producer. Either the MnS consumer retrieves a file from the MnS producer because the MnS consumer receives a file ready notification from the MnS producer or the MnS consumer reads the list of available (ready) files on the MnS producer and decides to retrieve an available file.

### 7.2.2 Void

### 7.2.3 Requirements

REQ-FM-R-1: The MnS producer shall support the capability allowing a MnS consumer to retrieve (get) a file from the MnS producer.

REQ-FM-R-2: The MnS producer shall support the capability allowing a MnS consumer to retrieve the list of files available for transfer from the MnS producer.

REQ-FM-R-3: The MnS producer shall support the capability to inform a MnS consumer about files that are available for retrieval.

REQ-FM-R-4: The MnS producer shall support the capability to inform a MnS consumer about errors that occurred during the preparation of a file.

REQ-FM-R-5: The information transferred to a MnS consumer about an available file shall allow associating the file to the process on the MnS producer that generated the file, if any such process exists and has an identifier.

REQ-FM-R-6: The MnS producer shall support the capability allowing a MnS consumer to indicate to the MnS producer, that the MnS consumer does not need a file anymore, such that the MnS producer hides the file in responses to subsequent read requests or decide to delete it altogether.

### 7.2.4 Solutions

#### 7.2.4.1 Stage 2 definition

Following are the stage 2 definition for File retrieval from a MnS producer by a MnS consumer.

- The operations and notifications of generic provisioning MnS defined in clause 11.1 in 3GPP TS 28.532 [2].

- The File retrieval NRM fragment defined inTS 28.622 [9].

#### 7.2.4.1 Stage 3 definition

Following are the stage 3 definition for File retrieval from a MnS producer by a MnS consumer.

- RESTful HTTP-based solution set

- RESTful HTTP-based solution set for generic provisioning management service is defined in clause 12.1.1 in 3GPP TS 28.532 [2]. Corresponding OpenAPI document "TS28532\_ProvMnS.yaml" in clause A.1 in TS 28.532 [2].

- OpenAPI document " TS28623\_FileManagementNrm.yaml " in clause 4.3 in TS 28.623 [10].

- YANG/Netconf-based solution set

- YANG/Netconf-based solution set for generic provisioning management service is defined in clause 12.1.3 in 3GPP TS 28.532 [2].

- YANG model "\_3gpp-common-files.yang " in clause 4.4 TS 28.623 [10].

## 7.3 File push from a MnS producer to a MnS consumer

### 7.3.1 Description

For file push, the MnS producer pushes a file to the MnS consumer or a designated file server. The voidMnS consumer configures the MnS Producer to push a file based on an event occuring on the MnS producer, such as the availability of a file.

### 7.3.2 Void

### 7.3.3 Requirements

REQ-FM-P-1: void

REQ-FM-P-2: void

REQ-FM-P-3: void

REQ-FM-P-4: The MnS producer shall support the capability to push a file to the MnS consumer or a designated file server when configured by a MnS consumer.

REQ-FM-P-5: The MnS producer shall support the capability for a MnS consumer to configure the MnS producer to push a file to the MnS consumer or a designated file server based on an event occurring on the MnS producer.

REQ-FM-P-6: The MnS producer shall support the capability to inform the MnS consumer, that has configured a file push, or any other MnS consumer about the completion of that file push.

## 7.4 File download from a MnS consumer to a MnS producer

### 7.4.1 Description

File download is when the MnS producer gets a file from the MnS consumer or a designated file server because the MnS consumer requests the MnS producer to download the file.

### 7.4.2 Void

### 7.4.3 Requirements

REQ-FM-D-1: The MnS producer shall support the capability to download a file from a MnS consumer or a designated file server when triggered by a MnS consumer.

REQ-FM-D-2: The MnS producer shall support the capability allowing a MnS consumer to trigger the MnS producer to download a file from the MnS consumer or a designated file server.

REQ-FM-D-3: The MnS producer shall support the capability to inform the MnS consumer that has triggered a file download, or any other consumer about the progress of that file download.

### 7.4.4 Solutions

#### 7.4.4.1 Stage 2 definition

Following are the stage 2 definition for File download from a MnS consumer to a MnS producer.

* The operations and notifications of generic provisioning MnS defined in clause 11.1 in 3GPP TS 28.532 [2].
* The File download NRM fragment defined in clause 4.3.46 in TS 28.622 [9].

#### 7.4.4.2 Stage 3 definition

Following are the stage 3 definition for File download from a MnS consumer to a MnS producer.

* RESTful HTTP-based solution set

- RESTful HTTP-based solution set for generic provisioning management service is defined in clause 12.1.1 in 3GPP TS 28.532 [2]. Corresponding OpenAPI document "TS28532\_ProvMnS.yaml" in clause A.1 in TS 28.532 [2].

- OpenAPI document " TS28623\_FileManagementNrm.yaml " in clause 4.3 in TS 28.623 [10].

* YANG/Netconf-based solution set

- YANG/Netconf-based solution set for generic provisioning management service is defined in clause 12.1.3 in 3GPP TS 28.532 [2].

- YANG model "\_3gpp-common-filemanagement.yang" in clause 4.4 in TS 28.623 [10].

Annex A (informative):   
Heartbeat PlantUML source code

# A.1 Procedure for configuring heartbeat notification periodicity

The following PlantUML source code is used to describe the procedure for configuring heartbeat notification periodicity, as depicted by Figure 4.3.1-1:

@startuml

title "Configuring heartbeat notification periodicity"

actor "MnS Consumer" as CONS

participant "MnS Producer" as PROV

CONS -> PROV: modifyMOIAttributes ('heartbeatNtfPeriod', newHeartbeatPeriodValue)

rnote over PROV

Internal Countdown Timer := newHeartbeatPeriodValue

endrnote

PROV -> CONS: notifyHeartbeat notification

note left

Provided he previously

subscribed to heartbeat

notifications

end note

rnote over PROV

Start countdown immediately

endrnotehide footbox

@enduml

# A.2 Procedure for requesting immediate heartbeat notification

The following PlantUML source code is used to describe the procedure for requesting immediate heartbeat notification, as depicted by Figure 4.3.2-1:

@startuml

title "Requesting immediate heartbeat notification"

actor "MnS Consumer" as CONS

participant "MnS Producer" as PROV

collections "Other MnS Consumers" as OTHER

CONS -> PROV: modifyMOIAttributes ('triggerHeartbeatNtf', TRUE)

rnote over PROV

Send immediate heartbeat notification

to all MnS Consumers who previously

subscribed to heartbeat notifications

endrnote

PROV -> CONS: notifyHeartbeat notification

PROV -> OTHER: notifyHeartbeat notification

rnote over PROV

triggerHeartbeatNtf:= FALSE

endrnote

hide footbox

@enduml

# A.3 Procedure for notifying periodic heartbeat notifications

The following PlantUML source code is used to describe the procedure for notifying periodic heartbeat notifications, as depicted by Figure 4.3.3-1:

@startuml

title "Notifying periodic heartbeat notifications"

actor "MnS Producer" as PROV

collections "MnS Consumers" as CONS

rnote over PROV

Send heartbeat notification to all

MnS Consumers who previously

subscribed to heartbeat notifications

endrnote

PROV -> CONS: notifyHeartbeat notification

rnote over PROV

Reinitialize its internal countdown

timer to the value of heartbeatNtfPeriod

endrnote

rnote over PROV

Start countdown

endrnotehide footbox

@enduml

Annex B (informative):  
Change history

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Change history** | | | | | | | |
| **Date** | **Meeting** | **TDoc** | **CR** | **Rev** | **Cat** | **Subject/Comment** | **New version** |
| 2020-03 | SA#87-e |  |  |  |  | Upgrade to changecontrol version | 16.0.0 |
| 2021-03 | SA#91e | SP-210152 | 0003 | - | B | Add use cases for discovery of management services | 17.0.0 |
| 2021-09 | SA#93e | SP-210864 | 0004 | 1 | C | Add support for discovery of management services | 17.1.0 |
| 2021-09 | SA#93e | SP-210876 | 0005 | - | B | Add requirements for data management | 17.1.0 |
| 2021-09 | SA#93e | SP-210875 | 0006 | - | B | Add requirements for file management | 17.1.0 |
| 2021-12 | SA#94e | SP-211467 | 0007 | 1 | C | Clarifications into existing use cases | 17.2.0 |
| 2021-12 | SA#94e | SP-211467 | 0008 | - | C | Clarifications into existing requirements | 17.2.0 |
| 2022-06 | SA#96 | SP-220564 | 0009 | 1 | F | Editorial Corrections | 17.3.0 |
| 2022-06 | SA#96 | SP-220505 | 0010 | - | B | Add requirements for management data collection and discovery | 17.3.0 |
| 2023-12 | SA#102 | SP-231452 | 0013 | 1 | F | Clarify management service discovery use cases | 17.4.0 |
| 2024-04 | - | - | - | - | - | Update to Rel-18 version (MCC) | 18.0.0 |
| 2024-04 | SA#104 | SP-240804 | 0015 | - | A | Rel-18 CR TS 28.537 Remove unsatisfied requirements related to file push triggered by MnS consumer | 18.1.0 |
| 2024-04 | SA#104 | SP-240804 | 0020 | - | A | Rel-18 CR TS 28.537 Remove undefined use case clause | 18.1.0 |
| 2024-09 | SA#105 | SP-241162 | 0022 | - | A | Rel-18 CR TS 28.537 Correction on file push requirement | 18.2.0 |
| 2024-12 | SA#106 | SP-241640 | 0027 | - | F | Rel-19 CR 28.537 Clarification of external management data | 19.0.0 |
| 2024-12 | SA#106 | SP-241640 | 0028 | - | D | Rel-19 CR 28.537 Correction of requirement labels | 19.0.0 |
| 2024-12 | SA#106 | SP-241640 | 0029 | - | F | Rel-19 CR 28.537 Introduce missing definition of term “trace metrics” | 19.0.0 |
| 2025-03 | SA#107 | SP-250160 | 0030 | 2 | B | Rel-19 TS 28.537 Usage of MnS Registry NRM fragment for MnS Registry and Discovery for different deployment scenarios | 19.1.0 |
| 2025-03 | SA#107 | SP-250160 | 0032 | 1 | B | Rel-19 CR TS 28.537 Change MnS provider to MnS producer | 19.1.0 |
| 2025-03 | SA#107 | SP-250149 | 0033 | 1 | F | Rel 19 CR TS 28.537 Remove editors notes | 19.1.0 |
| 2025-03 | SA#107 | SP-250149 | 0034 | 1 | D | Rel-19 CR TS 28.537 Add reference for solution description (NRM fragment) for each management capability | 19.1.0 |