**3GPP TSG-CT WG1 Meeting #156C1-255702**

**Göteborg, Sweden; 25th – 29th August 2025**

|  |
| --- |
| *CR-Form-v12.2* |
| **CHANGE REQUEST** |
|  |
|  | **24.549** | **CR** | **0049** | **rev** | **-** | **Current version:** | **18.4.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  | Update of info and externalDocs fields |
|  |  |
| ***Source to WG:*** | Lenovo |
| ***Source to TSG:*** | C1 |
|  |  |
| ***Work item code:*** | TEI19 |  | ***Date:*** | 2025-09-01 |
|  |  |  |  |  |
| ***Category:*** | **F** |  | ***Release:*** | Rel-19 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)Rel-19 (Release 19)* |
|  |  |
| ***Reason for change:*** | CR #0047 modifies ETC\_Configuration API has been agreed and the version number of the corresponding OpenAPI file thus needs to be incremented.New TS version number is 19.0.0 and the "description" field of the "externalDocs" object in the ETC\_Configuration API and NSCE\_SliceInfo API are to be updated. |
|  |  |
| ***Summary of change:*** | The ETC\_Configuration API version number set to value "1.1.0-alpha.1".The TS version number in the "description" field of the "externalDocs" object is changed to "19.0.0". |
|  |  |
| ***Consequences if not approved:*** | Incorrect API version number and incorrect TS version number in the "description" field of the "externalDocs" object. |
|  |  |
| ***Clauses affected:*** | C.2, C.3 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

\*\*\* First Change \*\*\*

# C.2 ETC\_Configuration API

openapi: 3.0.0

info:

 title: ETC\_Configuration

 version: 1.1.0-alpha.1

 description: |

 API for event triggered network slice adaptation configuration.

 © 2025, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

 All rights reserved.

externalDocs:

 description: >

 3GPP TS 24.549 V19.0.0 Application Data Analytics Enablement Service; Stage 3.

 url: https://www.3gpp.org/ftp/Specs/archive/24\_series/24.549/

security:

 - {}

 - oAuth2ClientCredentials: []

servers:

 - url: '{apiRoot}/su\_nsc/v1'

 variables:

 apiRoot:

 default: https://example.com

 description: apiRoot as defined in clause 5.2.4 of 3GPP TS 29.122.

paths:

 /val-services/{valServiceId}/configurations/{configurationId}:

 put:

 description: >

 Perfomrs event triggered network slice adaptation.

 operationId: EventTriggeredNetworkAdaptation

 tags:

 - Event triggered network adaptation (Document)

 parameters:

 - name: valServiceId

 description: String identifying the resource.

 in: path

 required: true

 schema:

 type: string

 - name: configurationId

 description: String identifying the resource.

 in: path

 required: true

 schema:

 type: string

 requestBody:

 required: true

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/NwSliceAdptEvent'

 responses:

 '204':

 description: >

 No Content. The requested network slice adaptation is successfullyprocessed.

 '307':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/307'

 '308':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/308'

 '400':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29122\_CommonData.yaml#/components/responses/default'

components:

 securitySchemes:

 oAuth2ClientCredentials:

 type: oauth2

 flows:

 clientCredentials:

 tokenUrl: '{tokenUrl}'

 scopes: {}

 schemas:

 NwSliceAdptEvent:

 description: >

 Represents the event associated with triggered network slice adaptation

 with the underlying network.

 type: object

 properties:

 valUeIds:

 type: array

 minItems: 1

 items:

 $ref: 'TS29549\_SS\_UserProfileRetrieval.yaml#/components/schemas/ValTargetUe'

 sliceId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

 dnn:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnn'

 appReqs:

 $ref: '#/components/schemas/AppReqs'

 required:

 - valUeIds

 - sliceId

 AppReqs:

 description: Represents requirements for the requested application.

 type: object

 properties:

 timeIntervals:

 type: array

 minItems: 1

 items:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/DurationSec'

 area:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/LocationArea'

 ratType:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/RatType'

\*\*\* End of Changes \*\*\*