**3GPP TSG- Meeting #**

**, , -**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.2* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  |  | **CR** |  | **rev** |  | **Current version:** |  |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **X** |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | for analytics | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | Nokia, Nokia Shanghai Bell, Ericsson | | | | | | | | | |
| ***Source to TSG:*** | C3 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | UPEAS | | | | |  | ***Date:*** | | |  |
|  |  | | | |  | |  | | |  |
| ***Category:*** | **B** |  | | | | | ***Release:*** | | |  |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-16 (Release 16) Rel-17 (Release 17) Rel-18 (Release 18) Rel-19 (Release 19)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | As per 23.501 clause 5.8.2.17, the UPF may expose information using the Nupf\_EventExposure service and "the NWDAF can subscribe to the UPF event exposure service directly". However, the current stage 3 model does not allow this, because it does not include UPF subscriptions, notifications, and event types.  Note that the DataSubscription and DataNotification data types defined in 29.575 are re-used by the NWDAF and DCCF in 29.520 and 29.574, respectively, in order to collect and store data from the possible data sources. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | Extended the ADRF data model to support UPF as a data source for analytics. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | Not fulfilled stage 2 requirement. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | 2, 3.3, 5.1.6.1, 5.1.6.2.8, 5.1.6.2.9, 5.1.8, A.2 | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  | **X** | Other core specifications | | | | TS/TR ... CR ... | | |
| ***affected:*** | |  | **X** | Test specifications | | | | TS/TR ... CR ... | | |
| ***(show related CRs)*** | |  | **X** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | | This CR introduces a backwards compatible feature in the OpenAPI file of the Nadrf\_DataManagement API. | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | |  | | | | | | | | |

\* \* \* \* First change \* \* \* \*

2 References

The following documents contain provisions which, through reference in this text, constitute provisions of the present document.

- References are either specific (identified by date of publication, edition number, version number, etc.) or non‑specific.

- For a specific reference, subsequent revisions do not apply.

- For a non-specific reference, the latest version applies. In the case of a reference to a 3GPP document (including a GSM document), a non-specific reference implicitly refers to the latest version of that document *in the same Release as the present document*.

[1] 3GPP TR 21.905: "Vocabulary for 3GPP Specifications".

[2] 3GPP TS 23.501: "System Architecture for the 5G System; Stage 2".

[3] 3GPP TS 23.502: "Procedures for the 5G System; Stage 2".

[4] 3GPP TS 29.500: "5G System; Technical Realization of Service Based Architecture; Stage 3".

[5] 3GPP TS 29.501: "5G System; Principles and Guidelines for Services Definition; Stage 3".

[6] OpenAPI: "OpenAPI 3.0.0 Specification", <https://github.com/OAI/OpenAPI-Specification/blob/master/versions/3.0.0.md>.

[7] 3GPP TR 21.900: "Technical Specification Group working methods".

[8] 3GPP TS 33.501: "Security architecture and procedures for 5G system".

[9] IETF RFC 6749: "The OAuth 2.0 Authorization Framework".

[10] 3GPP TS 29.510: "5G System; Network Function Repository Services; Stage 3".

[11] IETF RFC 7540: "Hypertext Transfer Protocol Version 2 (HTTP/2)".

[12] IETF RFC 8259: "The JavaScript Object Notation (JSON) Data Interchange Format".

[13] IETF RFC 7807: "Problem Details for HTTP APIs".

[14] 3GPP TS 23.288: "Architecture enhancements for 5G System (5GS) to support network data analytics services".

[15] 3GPP TS 29.520: "5G System; Network Data Analytics Services; Stage 3".

[16] 3GPP TS 29.571: "5G System; Common Data Types for Service Based Interfaces; Stage 3".

[17] 3GPP TS 29.508: "5G System; Session Management Event Exposure Service; Stage 3".

[18] 3GPP TS 29.518: "5G System; Access and Mobility Management Services; Stage 3".

[19] 3GPP TS 29.503: "5G System; Unified Data Management Services; Stage 3".

[20] 3GPP TS 29.517: "5G System; Application Function Event Exposure Services; Stage 3".

[21] 3GPP TS 29.591: "5G System; Network Exposure Function Southbound Services; Stage 3".

[22] 3GPP TS 29.122: "T8 reference point for Northbound APIs".

[23] 3GPP TS 29.574: "5G System; Data Collection Coordination Services; Stage 3".

[24] 3GPP TS 29.576: "5G System; Messaging Framework Adaptor Services; Stage 3".

[25] 3GPP TS 29.536: "5G System; Network Slice Admission Control Services; Stage 3".

[26] 3GPP TS 29.564: "5G System; User Plane Function Services; Stage 3".

\* \* \* \* Next change \* \* \* \*

3.3 Abbreviations

For the purposes of the present document, the abbreviations given in 3GPP TR 21.905 [1] and the following apply. An abbreviation defined in the present document takes precedence over the definition of the same abbreviation, if any, in 3GPP TR 21.905 [1].

ADRF Analytics Data Repository Function

AF Application Function

AMF Access and Mobility Management Function

DCCF Data Collection Coordination Function

MFAF Messaging Framework Adaptor Function

NEF Network Exposure Function

NF Network Function

NRF Network Repository Function

NWDAF Network Data Analytics Function

NSACF Network Slice Admission Control Function

SMF Session Management Function

UDM Unified Data Management

UPF User Plane Function

\* \* \* \* Next change \* \* \* \*

5.1.6.1 General

This clause specifies the application data model supported by the Nadrf\_DataManagement API.

Table 5.1.6.1-1 specifies the data types defined for the Nadrf\_DataManagement service based interface protocol.

**Table 5.1.6.1-1: Nadrf\_DataManagement specific Data Types**

|  |  |  |  |
| --- | --- | --- | --- |
| **Data type** | **Clause defined** | **Description** | **Applicability** |
| DataNotification | 5.1.6.2.9 | Represents a data subscription notification of one of various possible data sources. |  |
| DataSubscription | 5.1.6.2.8 | Contains information about Data specification. |  |
| NadrfDataRetrievalNotification | 5.1.6.2.5 | Represents a notification that corresponds with an Individual ADRF Data Retrieval Subscription resource. |  |
| NadrfDataRetrievalSubscription | 5.1.6.2.4 | Represents an Individual ADRF Data Retrieval Subscription resource. |  |
| NadrfDataStoreRecord | 5.1.6.2.2 | Represents an Individual ADRF Data Store Record resource. |  |
| NadrfDataStoreSubscription | 5.1.6.2.3 | Contains information to be used by the ADRF to create a Data or Analytics subscription. |  |
| NadrfDataStoreSubscriptionRef | 5.1.6.2.6 | Contains a reference to a request for a Data or Analytics subscription. |  |
| NadrfStoredDataSpec | 5.1.6.2.7 | Contains information about Data or Analytics specification. |  |

Table 5.1.6.1-2 specifies data types re-used by the Nadrf\_DataManagement service based interface protocol from other specifications, including a reference to their respective specifications and when needed, a short description of their use within the Nadrf\_DataManagement service based interface.

**Table 5.1.6.1-2: Nadrf\_DataManagement re-used Data Types**

|  |  |  |  |
| --- | --- | --- | --- |
| **Data type** | **Reference** | **Comments** | **Applicability** |
| AfEventExposureNotif | 3GPP TS 29.517 [20] | Represents notifications on AF event(s) that occurred for an Individual AF Event Subscription resource. |  |
| AfEventExposureSubsc | 3GPP TS 29.517 [20] | Represents AF event subscription. |  |
| AmfEventNotification | 3GPP TS 29.518 [18] | Represents notifications on AMF event(s) that occurred for an Individual AMF Event Subscription resource. |  |
| AmfEventSubscription | 3GPP TS 29.518 [18] | Represents AMF event subscription. |  |
| DateTime | 3GPP TS 29.571 [16] | Identifies the time. |  |
| EeSubscription | 3GPP TS 29.503 [19] | Represents UDM event subscription. |  |
| FetchInstruction | 3GPP TS 29.576 [24] | The fetch instruction indicates that the data or analytics can be fetched by the consumer. |  |
| FormattingInstruction | 3GPP TS 29.574 [23] | DCCF formatting Instructions. |  |
| MonitoringReport | 3GPP TS 29.503 [19] | UDM Monitoring Report. |  |
| NefEventExposureNotif | 3GPP TS 29.591 [21] | Represents notifications on network exposure event(s) that occurred for an Individual Network Exposure Event Subscription resource. |  |
| NefEventExposureSubsc | 3GPP TS 29.591 [21] | Represents NEF event subscription. |  |
| NfInstanceId | 3GPP TS 29.571 [16] | NF instance identifier. |  |
| NfSetId | 3GPP TS 29.571 [16] | NF set identifier. |  |
| NnwdafEventsSubscription | 3GPP TS 29.520 [15] | Represents an NWDAF analytics subscription. |  |
| NnwdafEventsSubscriptionNotification | 3GPP TS 29.520 [15] | Represents an NWDAF analytics subscription notification. |  |
| NotificationData | 3GPP TS 29.510 [10] | Represents an NRF event notification. |  |
| NotificationData | 3GPP TS 29.564 [26] | Represents a UPF event notification. | UpEvents |
| NsmfEventExposure | 3GPP TS 29.508 [17] | Represents SMF event subscription. |  |
| NsmfEventExposureNotification | 3GPP TS 29.508 [17] | Represents SMF event notification. |  |
| ProcessingInstruction | 3GPP TS 29.574 [23] | DCCF processing Instructions. |  |
| SACEventReport | 3GPP TS 29.536 [25] | Represents an NSACF event notification. |  |
| SACEventSubscription | 3GPP TS 29.536 [25] | Represents and NSACF event subscription. |  |
| SubscriptionData | 3GPP TS 29.510 [10] | Represents an NRF event subscription. |  |
| SupportedFeatures | 3GPP TS 29.571 [6] | Used to negotiate the applicability of the optional features defined in table 5.1.8-1. |  |
| TimeWindow | 3GPP TS 29.122 [22] | Represents a time window. |  |
| UpfEventSubscription | 3GPP TS 29.564 [26] | Represents a UPF event subscription. | UpEvents |
| Uri | 3GPP TS 29.571 [16] | URI. |  |

\* \* \* \* Next change \* \* \* \*

5.1.6.2.8 Type: DataSubscription

**Table 5.1.6.2.8-1: Definition of type DataSubscription**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Attribute name** | **Data type** | **P** | **Cardinality** | **Description** | **Applicability** |
| amfDataSub | AmfEventSubscription | C | 0..1 | Represents requested AMF Events subscription.  (NOTE) |  |
| smfDataSub | NsmfEventExposure | C | 0..1 | Represents requested SMF Events subscription.  (NOTE) |  |
| udmDataSub | EeSubscription | C | 0..1 | Represents requested UDM Events subscription.  (NOTE) |  |
| nefDataSub | NefEventExposureSubsc | C | 0..1 | Represents requested NEF Events subscription.  (NOTE) |  |
| afDataSub | AfEventExposureSubsc | C | 0..1 | Represents requested AF Events subscription.  (NOTE) |  |
| nrfDataSub | SubscriptionData | C | 0..1 | Represents requested NRF Events subscription.  (NOTE) |  |
| nsacfDataSub | SACEventSubscription | C | 0..1 | Represents requested NSACF Events subscription.  (NOTE) |  |
| upfDataSub | UpfEventSubscription | C | 0..1 | Represents requested UPF Events subscription.  (NOTE) | UpEvents |
| NOTE: Exactly one of these attributes shall be provided. | | | | | |

\* \* \* \* Next change \* \* \* \*

5.1.6.2.9 Type: DataNotification

**Table 5.1.6.2.9-1: Definition of type DataNotification**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Attribute name** | **Data type** | **P** | **Cardinality** | **Description** | **Applicability** |
| afEventNotifs | array(AfEventExposureNotif) | C | 1..N | List of notifications on AF event(s). (NOTE 1) |  |
| amfEventNotifs | array(AmfEventNotification) | C | 1..N | List of notifications on AMF event(s). (NOTE 1) |  |
| smfEventNotifs | array(NsmfEventExposureNotification) | C | 1..N | List of notifications on SMF event(s). (NOTE 1) |  |
| udmEventNotifs | array(MonitoringReport) | C | 1..N | List of monitoring reports containing information about UDM event(s). (NOTE 1) |  |
| nefEventNotifs | array(NefEventExposureNotif) | C | 1..N | List of notifications on network exposure event(s). (NOTE 1) |  |
| nrfEventNotifs | array(NotificationData) | C | 1..N | List of notifications on NRF event(s) as defined in 3GPP TS 29.510 [10]. (NOTE 1) |  |
| nsacfEventNotifs | array(SACEventReport) | C | 1..N | List of notifications on NSACF event(s). (NOTE 1) |  |
| upfEventNotifs | array(NotificationData) | C | 1..N | List of notifications on UPF event(s) as defined in 3GPP TS 29.564 [26]. (NOTE 1) | UpEvents |
| timeStamp | DateTime | O | 0..1 | Indicates the timestamp for the event(s). (NOTE 2) |  |
| NOTE 1: Exactly one of these attributes shall be provided.  NOTE 2: The "timeStamp" attribute within the DataNotification data type may be provided if any of the "timeStamp" attribute within AfEventNotification contained in the AfEventExposureNotif, or within AmfEventReport contained in the AmfEventNotification, or within EventNotification contained in the NsmfEventExposureNotification, or within MonitoringReport, or within NefEventNotification contained in the NefEventExposureNotif, or within SACEventReportItem contained in the SACEventReport, or, if the UpEvents feature is supported, within the NotificationItem contained in the NotificationData data type is not provided. | | | | | |

\* \* \* \* Next change \* \* \* \*

5.1.8 Feature negotiation

The optional features in table 5.1.8-1 are defined for the Nadrf\_DataManagement API. They shall be negotiated using the extensibility mechanism defined in clause 6.6 of 3GPP TS 29.500 [4].

**Table 5.1.8-1: Supported Features**

|  |  |  |
| --- | --- | --- |
| **Feature number** | **Feature Name** | **Description** |
| 1 | MultiProcessingInstruction | Indicates the support of multiple processing instructions. |
| 2 | UpEvents | Indicates the support of UPF events. |

\* \* \* \* Next change \* \* \* \*

A.2 Nadrf\_DataManagement API

openapi: 3.0.0

info:

version: 1.1.0-alpha.2

title: Nadrf\_DataManagement

description: |

ADRF Data Management Service.

© 2023, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

All rights reserved.

externalDocs:

description: 3GPP TS 29.575 V18.1.0; 5G System; Analytics Data Repository Services; Stage 3.

url: 'https://www.3gpp.org/ftp/Specs/archive/29\_series/29.575/'

#

servers:

- url: '{apiRoot}/nadrf-datamanagement/v1'

variables:

apiRoot:

default: https://example.com

description: apiRoot as defined in clause 4.4 of 3GPP TS 29.501.

#

security:

- oAuth2ClientCredentials:

- nadrf-datamanagement

- {}

#

paths:

/data-store-records:

post:

summary: Creates a new Individual Data Store Record resource.

operationId: CreateADRFDataStoreRecord

tags:

- ADRF Data Store Records (Collection)

requestBody:

content:

application/json:

schema:

$ref: '#/components/schemas/NadrfDataStoreRecord'

required: true

description: ADRF data store record to be stored.

responses:

'201':

description: Successful creation of new Individual ADRF Data Store Record resource.

headers:

Location:

description: >

Contains the URI of the newly created resource, according to the structure

{apiRoot}/nadrf-datamanagement/<apiVersion>/data-store-records/{storeTransId}

required: true

schema:

type: string

content:

application/json:

schema:

$ref: '#/components/schemas/NadrfDataStoreRecord'

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29571\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29571\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29571\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'502':

$ref: 'TS29571\_CommonData.yaml#/components/responses/502'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

get:

summary: Retrieves existing Individual ADRF Data Store Records.

operationId: GetAdrfDataStoreRecords

tags:

- ADRF Data Store Records (Collection)

parameters:

- name: store-trans-id

description: A storage transaction identifier of a data store record in ADRF.

in: query

required: false

schema:

type: string

- name: fetch-correlation-ids

description: Fetch correlation identifiers received as part of fetch instruction.

in: query

required: false

style: form

explode: false

schema:

type: array

items:

type: string

minItems: 1

responses:

'200':

description: Data store records are returned.

content:

application/json:

schema:

$ref: '#/components/schemas/NadrfDataStoreRecord'

'204':

description: No matching ADRF data were found.

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'406':

$ref: 'TS29571\_CommonData.yaml#/components/responses/406'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'502':

$ref: 'TS29571\_CommonData.yaml#/components/responses/502'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

/data-store-records/{storeTransId}:

delete:

summary: Delete an existing Individual ADRF Data Store Record.

operationId: DeleteADRFDataStoreRecord

tags:

- Individual ADRF Data Store Record (Document)

parameters:

- name: storeTransId

in: path

description: String identifying a Data Store Record in ADRF.

required: true

schema:

type: string

responses:

'204':

description: >

No Content. The Individual ADRF Data Store Record resource matching the

storeTransId was deleted.

'307':

$ref: 'TS29571\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29571\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'502':

$ref: 'TS29571\_CommonData.yaml#/components/responses/502'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

/data-retrieval-subscriptions:

post:

summary: Creates a new Individual ADRF Data Retrieval Subscription resource.

operationId: CreateADRFDataRetrievalSubscription

tags:

- ADRF Data Retrieval Subscriptions (Collection)

requestBody:

content:

application/json:

schema:

$ref: '#/components/schemas/NadrfDataRetrievalSubscription'

required: true

description: Individual ADRF Data Retrieval Subscription resource to be created.

responses:

'201':

description: Created a new Individual ADRF Data Retrieval Subscription resource.

headers:

Location:

description: >

Contains the URI of the newly created resource, according to the structure

{apiRoot}/nadrf-datamanagement/<apiVersion>/data-retrieval-subscriptions/{subscriptionId}

required: true

schema:

type: string

content:

application/json:

schema:

$ref: '#/components/schemas/NadrfDataRetrievalSubscription'

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29571\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29571\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29571\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'502':

$ref: 'TS29571\_CommonData.yaml#/components/responses/502'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

callbacks:

adrfDataRetrievalNotification:

'{$request.body#/notificationURI}':

post:

requestBody:

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/NadrfDataRetrievalNotification'

responses:

'204':

description: The receipt of the Notification is acknowledged.

'307':

$ref: 'TS29571\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29571\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29571\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29571\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29571\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'502':

$ref: 'TS29571\_CommonData.yaml#/components/responses/502'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

/data-retrieval-subscriptions/{subscriptionId}:

delete:

summary: Delete an existing Individual ADRF Data Retrieval Subscription resource.

operationId: DeleteADRFDataRetrievalSubscription

tags:

- Individual ADRF Data Retrieval Subscription (Document)

parameters:

- name: subscriptionId

in: path

description: >

String identifying a data retrieval subscription to the Nadrf\_DataManagement

Service.

required: true

schema:

type: string

responses:

'204':

description: >

No Content. The Individual ADRF Data Retrieval Subscription resource matching

the subscriptionId was deleted.

'307':

$ref: 'TS29571\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29571\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'502':

$ref: 'TS29571\_CommonData.yaml#/components/responses/502'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

/request-storage-sub:

post:

summary: Triggers the creation of a new ADRF Storage Subscription.

operationId: CreateADRFStorageSubscription

tags:

- ADRF Storage Subscriptions

requestBody:

content:

application/json:

schema:

$ref: '#/components/schemas/NadrfDataStoreSubscription'

required: true

responses:

'200':

description: >

Successful response with reference used to identify the subscription at the ADRF.

content:

application/json:

schema:

$ref: '#/components/schemas/NadrfDataStoreSubscriptionRef'

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29571\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29571\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29571\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'502':

$ref: 'TS29571\_CommonData.yaml#/components/responses/502'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

/request-storage-sub-removal:

post:

summary: Triggers the removal of ADRF storage subscription.

operationId: DeleteADRFStorageSubscription

tags:

- ADRF Storage Subscriptions

requestBody:

content:

application/json:

schema:

$ref: '#/components/schemas/NadrfDataStoreSubscriptionRef'

required: true

responses:

'204':

description: >

No Content. The ADRF Storage Subscription matching the provided reference was deleted.

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29571\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29571\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29571\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'502':

$ref: 'TS29571\_CommonData.yaml#/components/responses/502'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

/remove-stored-data-analytics:

post:

summary: Remove ADRF data based on data or analytics specification.

operationId: DeleteADRFData

tags:

- ADRF Stored Data

requestBody:

content:

application/json:

schema:

$ref: '#/components/schemas/NadrfStoredDataSpec'

required: true

responses:

'204':

description: No Content. The ADRF data matching the provided specification is deleted.

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29571\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29571\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29571\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'502':

$ref: 'TS29571\_CommonData.yaml#/components/responses/502'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

#

components:

securitySchemes:

oAuth2ClientCredentials:

type: oauth2

flows:

clientCredentials:

tokenUrl: '{nrfApiRoot}/oauth2/token'

scopes:

nadrf-datamanagement: Access to the nadrf-datamanagement API

#

schemas:

#

NadrfDataStoreRecord:

description: Represents an Individual ADRF Data Store Record.

type: object

oneOf:

- allOf:

- required: [anaSub]

- required: [anaNotifications]

- allOf:

- required: [dataSub]

- required: [dataNotif]

properties:

dataNotif:

$ref: '#/components/schemas/DataNotification'

anaNotifications:

type: array

items:

$ref: 'TS29520\_Nnwdaf\_EventsSubscription.yaml#/components/schemas/NnwdafEventsSubscriptionNotification'

minItems: 1

description: List of analytics subscription notifications.

anaSub:

type: array

items:

$ref: 'TS29520\_Nnwdaf\_EventsSubscription.yaml#/components/schemas/NnwdafEventsSubscription'

minItems: 1

description: >

Represents the subscription information of the corresponding analytics notification.

dataSub:

type: array

items:

$ref: '#/components/schemas/DataSubscription'

minItems: 1

description: >

Represents the subscription information of the corresponding data notification.

suppFeat:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

#

NadrfDataStoreSubscription:

description: >

Contains information to be used by the ADRF to create a Data or Analytics subscription.

type: object

allOf:

- oneOf:

- required: [anaSub]

- required: [dataSub]

- oneOf:

- required: [targetNfId]

- required: [targetNfSetId]

properties:

anaSub:

$ref: 'TS29520\_Nnwdaf\_EventsSubscription.yaml#/components/schemas/NnwdafEventsSubscription'

dataSub:

$ref: '#/components/schemas/DataSubscription'

targetNfId:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/NfInstanceId'

targetNfSetId:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/NfSetId'

formatInstruct:

$ref: 'TS29574\_Ndccf\_DataManagement.yaml#/components/schemas/FormattingInstruction'

procInstruct:

$ref: 'TS29574\_Ndccf\_DataManagement.yaml#/components/schemas/ProcessingInstruction'

multiProcInstructs:

type: array

items:

$ref: 'TS29574\_Ndccf\_DataManagement.yaml#/components/schemas/ProcessingInstruction'

minItems: 1

description: Processing instructions to be used for sending event notifications.

suppFeat:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

#

NadrfDataRetrievalSubscription:

description: Represents an Individual ADRF Data Retrieval Subscription.

type: object

required:

- notifCorrId

- notificationURI

- timePeriod

oneOf:

- required: [anaSub]

- required: [dataSub]

properties:

anaSub:

$ref: 'TS29520\_Nnwdaf\_EventsSubscription.yaml#/components/schemas/NnwdafEventsSubscription'

dataSub:

$ref: '#/components/schemas/DataSubscription'

notificationURI:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

timePeriod:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/TimeWindow'

notifCorrId:

type: string

description: Notification correlation identifier.

consTrigNotif:

type: boolean

description: >

It indicates that notifications shall be buffered (sending only fetch instructions

to the NF service consumer) until the NF service consumer requests their delivery

using Nadrf\_DataManagement Service.

suppFeat:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

#

NadrfDataRetrievalNotification:

description: >

Represents a notification that corresponds with an Individual ADRF Data

Retrieval Subscription.

type: object

required:

- notifCorrId

- timeStamp

oneOf:

- required: [anaNotifications]

- required: [dataNotif]

- required: [fetchInstruct]

properties:

notifCorrId:

type: string

description: Notification correlation identifier.

anaNotifications:

type: array

items:

$ref: 'TS29520\_Nnwdaf\_EventsSubscription.yaml#/components/schemas/NnwdafEventsSubscriptionNotification'

minItems: 1

description: List of analytics subscription notifications.

dataNotif:

$ref: '#/components/schemas/DataNotification'

fetchInstruct:

$ref: 'TS29576\_Nmfaf\_3caDataManagement.yaml#/components/schemas/FetchInstruction'#

terminationReq:

type: boolean

description: >

It indicates the termination of the data management subscription that requested by the

ADRF.

timeStamp:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

#

NadrfDataStoreSubscriptionRef:

description: Contains a reference to a request for a Data or Analytics subscription.

type: object

required:

- transRefId

properties:

transRefId:

type: string

description: Transaction reference identifier.

#

NadrfStoredDataSpec:

description: Contains information about Data or Analytics specification.

type: object

required:

- timePeriod

oneOf:

- required: [dataSpec]

- required: [anaSpec]

properties:

dataSpec:

$ref: '#/components/schemas/DataSubscription'

anaSpec:

$ref: 'TS29520\_Nnwdaf\_EventsSubscription.yaml#/components/schemas/NnwdafEventsSubscription'

timePeriod:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/TimeWindow'

#

DataSubscription:

description: Contains a data specification.

type: object

oneOf:

- required: [amfDataSub]

- required: [smfDataSub]

- required: [udmDataSub]

- required: [nefDataSub]

- required: [afDataSub]

- required: [nrfDataSub]

- required: [nsacfDataSub]

properties:

amfDataSub:

$ref: 'TS29518\_Namf\_EventExposure.yaml#/components/schemas/AmfEventSubscription'

smfDataSub:

$ref: 'TS29508\_Nsmf\_EventExposure.yaml#/components/schemas/NsmfEventExposure'

udmDataSub:

$ref: 'TS29503\_Nudm\_EE.yaml#/components/schemas/EeSubscription'

afDataSub:

$ref: 'TS29517\_Naf\_EventExposure.yaml#/components/schemas/AfEventExposureSubsc'

nefDataSub:

$ref: 'TS29591\_Nnef\_EventExposure.yaml#/components/schemas/NefEventExposureSubsc'

nrfDataSub:

$ref: 'TS29510\_Nnrf\_NFManagement.yaml#/components/schemas/SubscriptionData'

nsacfDataSub:

$ref: 'TS29536\_Nnsacf\_SliceEventExposure.yaml#/components/schemas/SACEventSubscription'

#

DataNotification:

description: Represents a Data Subscription Notification.

type: object

oneOf:

- required: [amfEventNotifs]

- required: [smfEventNotifs]

- required: [udmEventNotifs]

- required: [nefEventNotifs]

- required: [afEventNotifs]

- required: [nrfEventNotifs]

- required: [nsacfEventNotifs]

- required: [upfEventNotifs]

properties:

amfEventNotifs:

type: array

items:

$ref: 'TS29518\_Namf\_EventExposure.yaml#/components/schemas/AmfEventNotification'

minItems: 1

description: List of notifications of AMF events.

smfEventNotifs:

type: array

items:

$ref: 'TS29508\_Nsmf\_EventExposure.yaml#/components/schemas/NsmfEventExposureNotification'

minItems: 1

description: List of notifications of SMF events.

udmEventNotifs:

type: array

items:

$ref: 'TS29503\_Nudm\_EE.yaml#/components/schemas/MonitoringReport'

minItems: 1

description: List of notifications of UDM events.

nefEventNotifs:

type: array

items:

$ref: 'TS29591\_Nnef\_EventExposure.yaml#/components/schemas/NefEventExposureNotif'

minItems: 1

description: List of notifications of NEF events.

afEventNotifs:

type: array

items:

$ref: 'TS29517\_Naf\_EventExposure.yaml#/components/schemas/AfEventExposureNotif'

minItems: 1

description: List of notifications of AF events.

nrfEventNotifs:

type: array

items:

$ref: 'TS29510\_Nnrf\_NFManagement.yaml#/components/schemas/NotificationData'

minItems: 1

description: List of notifications of NRF events.

nsacfEventNotifs:

type: array

items:

$ref: 'TS29536\_Nnsacf\_SliceEventExposure.yaml#/components/schemas/SACEventReport'

minItems: 1

description: List of notifications of NSACF events.

upfEventNotifs:

type: array

items:

$ref: 'TS29564\_Nupf\_EventExposure.yaml#/components/schemas/NotificationData'

minItems: 1

description: List of notifications of UPF events.

timeStamp:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

#

\* \* \* \* End of changes \* \* \* \*