**3GPP TSG-CT WG3 Meeting #131C3-235422**

**Chicago, USA, 9 - 13 November, 2023**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.2* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  | **29.520** | **CR** | **0832** | **rev** | **-** | **Current version:** | **18.3.0** |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **X** |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | IETF RFC 7540, RFC 7807 obsoleted by RFC 9113 and RFC 9457 respectively | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | China Mobile | | | | | | | | | |
| ***Source to TSG:*** | CT3 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | SBIProtoc18 | | | | |  | ***Date:*** | | | 2023-11-06 |
|  |  | | | |  | |  | | |  |
| ***Category:*** | **F** |  | | | | | ***Release:*** | | | Rel-18 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-16 (Release 16) Rel-17 (Release 17) Rel-18 (Release 18) Rel-19 (Release 19)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | As indicated by C3-234018, IETF RFC 9113 ("HTTP/2", published in June 2022) obsoletes RFC 7540.  IETF RFC 9457 ("Problem Details for HTTP APIs") obsoletes RFC 7807. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | * Update the RFC references. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | Reference to a obsoleted RFC. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | 2, 5.1.2.1, 5.1.2.2.2, 5.2.2.1, 5.2.2.2.2, 5.3.2.1, 5.3.2.2.2, 5.4.2.1, 5.4.2.2.2, 5.5.2.1, 5.5.2.2.2 | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | | **X** |  | Other core specifications | | | | TS 29.501 CR 0148 | | |
| ***affected:*** | |  | **X** | Test specifications | | | | TS/TR ... CR ... | | |
| ***(show related CRs)*** | |  | **X** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | | This CR does not impact the OpenAPI file. | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | |  | | | | | | | | |

**Additional discussion(if needed):**

**Proposed changes:**

\*\*\* 1st Change \*\*\*

# 2 References

The following documents contain provisions which, through reference in this text, constitute provisions of the present document.

- References are either specific (identified by date of publication, edition number, version number, etc.) or non‑specific.

- For a specific reference, subsequent revisions do not apply.

- For a non-specific reference, the latest version applies. In the case of a reference to a 3GPP document (including a GSM document), a non-specific reference implicitly refers to the latest version of that document *in the same Release as the present document*.

[1] 3GPP TR 21.905: "Vocabulary for 3GPP Specifications".

[2] 3GPP TS 23.501: "System Architecture for the 5G System; Stage 2".

[3] Void.

[4] 3GPP TS 23.503: "Policy and Charging Control Framework for the 5G System; Stage 2".

[5] 3GPP TS 29.513: "5G System; Policy and Charging Control signalling flows and QoS parameter mapping; Stage 3".

[6] 3GPP TS 29.500: "5G System; Technical Realization of Service Based Architecture; Stage 3".

[7] 3GPP TS 29.501: "5G System; Principles and Guidelines for Services Definition; Stage 3".

[8] 3GPP TS 29.571: "5G System; Common Data Types for Service Based Interfaces; Stage 3".

[9] IETF RFC 9113: "HTTP/2".

[10] IETF RFC 8259: "The JavaScript Object Notation (JSON) Data Interchange Format".

[11] OpenAPI: "OpenAPI Specification Version 3.0.0", https://spec.openapis.org/oas/v3.0.0

[12] 3GPP TS 29.510: "5G System; Network Function Repository Services; Stage 3".

[13] 3GPP TS 33.501: "Security architecture and procedures for 5G system".

[14] IETF RFC 6749: "The OAuth 2.0 Authorization Framework".

[15] IETF RFC 9457: "Problem Details for HTTP APIs".

[16] 3GPP TR 21.900: "Technical Specification Group working methods".

[17] 3GPP TS 23.288: "Architecture enhancements for 5G System (5GS) to support network data analytics services".

[18] 3GPP TS 29.554: "5G System; Background Data Transfer Policy Control Service; Stage 3".

[19] 3GPP TS 29.122: "T8 reference point for Northbound APIs".

[20] 3GPP TS 29.523: "5G System; Policy Control Event Exposure Service; Stage 3".

[21] 3GPP TS 29.514: "5G System; Policy Authorization Service; Stage 3".

[22] 3GPP TS 29.517: "5G System; Application Function (AF) event exposure service".

[23] 3GPP TS 29.503: "5G System; Unified Data Management Services; Stage 3".

[24] 3GPP TS 29.531: "5G System; Network Slice Selection Services; Stage 3".

[25] 3GPP TS 29.552: "5G System; Network Data Analytics signalling flows; Stage 3".

[26] 3GPP TS 29.574: "5G System; Data Collection Coordination Services; Stage 3".

[27] 3GPP TS 29.575: "5G System; Analytics Data Repository Services; Stage 3".

[28] 3GPP TS 29.576: "5G System; Messaging Framework Adaptor Services; Stage 3".

[29] 3GPP TS 29.508: "5G System; Session Management Event Exposure Service; Stage 3".

[30] 3GPP TS 29.572: "5G System; Location Management Services; Stage 3".

[31] IANA: "SMI Network Management Private Enterprise Codes", <http://www.iana.org/assignments/enterprise-numbers>.

[32] 3GPP TS 29.522: "5G System; Network Exposure Function Northbound APIs; Stage 3".

[33] IETF RFC 6733: "Diameter Base Protocol".

\*\*\* Next Change \*\*\*

#### 5.1.2.1 General

HTTP/2, IETF RFC 9113 [9], shall be used as specified in clause 5 of 3GPP TS 29.500 [6].

HTTP/2 shall be transported as specified in clause 5.3 of 3GPP TS 29.500 [6].

The OpenAPI [11] specification of HTTP messages and content bodies for the Nnwdaf\_EventsSubscription is contained in Annex A.

\*\*\* Next Change \*\*\*

##### 5.1.2.2.2 Content type

JSON, IETF RFC 8259 [10], shall be used as content type of the HTTP bodies specified in the present specification as specified in clause 5.4 of 3GPP TS 29.500 [6]. The use of the JSON format shall be signalled by the content type "application/json".

"Problem Details" JSON object shall be used to indicate additional details of the error in a HTTP response body and shall be signalled by the content type "application/problem+json", as defined in IETF RFC 9457 [15].

\*\*\* Next Change \*\*\*

#### 5.2.2.1 General

HTTP/2, IETF RFC 9113 [9], shall be used as specified in clause 5 of 3GPP TS 29.500 [6].

HTTP/2 shall be transported as specified in clause 5.3 of 3GPP TS 29.500 [6].

The OpenAPI [11] specification of HTTP messages and content bodies for the Nnwdaf\_AnalyticsInfo is contained in Annex A.

\*\*\* Next Change \*\*\*

##### 5.2.2.2.2 Content type

JSON, IETF RFC 8259 [10], shall be used as content type of the HTTP bodies specified in the present specification as specified in clause 5.4 of 3GPP TS 29.500 [6]. The use of the JSON format shall be signalled by the content type "application/json".

"Problem Details" JSON object shall be used to indicate additional details of the error in a HTTP response body and shall be signalled by the content type "application/problem+json", as defined in IETF RFC 9457 [15].

\*\*\* Next Change \*\*\*

#### 5.3.2.1 General

HTTP/2, IETF RFC 9113 [9], shall be used as specified in clause 5 of 3GPP TS 29.500 [6].

HTTP/2 shall be transported as specified in clause 5.3 of 3GPP TS 29.500 [6].

The OpenAPI [11] specification of HTTP messages and content bodies for the Nnwdaf\_DataManagement is contained in Annex A.

\*\*\* Next Change \*\*\*

##### 5.3.2.2.2 Content type

JSON, IETF RFC 8259 [10], shall be used as content type of the HTTP bodies specified in the present specification as specified in clause 5.4 of 3GPP TS 29.500 [6]. The use of the JSON format shall be signalled by the content type "application/json".

"Problem Details" JSON object shall be used to indicate additional details of the error in a HTTP response body and shall be signalled by the content type "application/problem+json", as defined in IETF RFC 9457 [15].

\*\*\* Next Change \*\*\*

#### 5.4.2.1 General

HTTP/2, IETF RFC 9113 [9], shall be used as specified in clause 5 of 3GPP TS 29.500 [6].

HTTP/2 shall be transported as specified in clause 5.3 of 3GPP TS 29.500 [6].

The OpenAPI [11] specification of HTTP messages and content bodies for the Nnwdaf\_MLModelProvision is contained in Annex A.

\*\*\* Next Change \*\*\*

##### 5.4.2.2.2 Content type

JSON, IETF RFC 8259 [10], shall be used as content type of the HTTP bodies specified in the present specification as specified in clause 5.4 of 3GPP TS 29.500 [6]. The use of the JSON format shall be signalled by the content type "application/json".

"Problem Details" JSON object shall be used to indicate additional details of the error in a HTTP response body and shall be signalled by the content type "application/problem+json", as defined in IETF RFC 9457 [15].

\*\*\* Next Change \*\*\*

#### 5.5.2.1 General

HTTP/2, IETF RFC 9113 [9], shall be used as specified in clause 5 of 3GPP TS 29.500 [6].

HTTP/2 shall be transported as specified in clause 5.3 of 3GPP TS 29.500 [6].

The OpenAPI [11] specification of HTTP messages and content bodies for the Nnwdaf\_MLModelTraining is contained in Annex A.

\*\*\* Next Change \*\*\*

##### 5.5.2.2.2 Content type

JSON, IETF RFC 8259 [10], shall be used as content type of the HTTP bodies specified in the present specification as specified in clause 5.4 of 3GPP TS 29.500 [6]. The use of the JSON format shall be signalled by the content type "application/json".

"Problem Details" JSON object shall be used to indicate additional details of the error in a HTTP response body and shall be signalled by the content type "application/problem+json", as defined in IETF RFC 9457 [15].

\*\*\* End of Changes \*\*\*