**3GPP TSG-CT WG3 Meeting #131C3-235425**

**Chicago, USA, 9 - 13 November, 2023**

|  |
| --- |
| *CR-Form-v12.2* |
| **CHANGE REQUEST** |
|  |
|  | **29.575** | **CR** | **0072** | **rev** | **-** | **Current version:** | **18.3.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **X** |

|  |
| --- |
|  |
| ***Title:***  | IETF RFC 7540 and 9457 obsoleted by RFC 9113 and 7807 |
|  |  |
| ***Source to WG:*** | China Mobile |
| ***Source to TSG:*** | CT3 |
|  |  |
| ***Work item code:*** | SBIProtoc18 |  | ***Date:*** | 2023-11-06 |
|  |  |  |  |  |
| ***Category:*** | **F** |  | ***Release:*** | Rel-18 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)Rel-19 (Release 19)* |
|  |  |
| ***Reason for change:*** | As indicated by C3-234018, IETF RFC 9113 ("HTTP/2", published in June 2022) obsoletes RFC 7540.IETF RFC 9457 ("Problem Details for HTTP APIs") obsoletes RFC 7807. |
|  |  |
| ***Summary of change:*** | * Update the RFC references.
 |
|  |  |
| ***Consequences if not approved:*** | Reference to a obsoleted RFC. |
|  |  |
| ***Clauses affected:*** | 2, 5.1.2.1, 5.1.2.2.2, 5.2.2.1, 5.2.2.2.2 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** | This CR does not impact the OpenAPI file. |
|  |  |
| ***This CR's revision history:*** |  |

**Additional discussion(if needed):**

**Proposed changes:**

\*\*\* 1st Change \*\*\*

# 2 References

The following documents contain provisions which, through reference in this text, constitute provisions of the present document.

- References are either specific (identified by date of publication, edition number, version number, etc.) or non‑specific.

- For a specific reference, subsequent revisions do not apply.

- For a non-specific reference, the latest version applies. In the case of a reference to a 3GPP document (including a GSM document), a non-specific reference implicitly refers to the latest version of that document *in the same Release as the present document*.

[1] 3GPP TR 21.905: "Vocabulary for 3GPP Specifications".

[2] 3GPP TS 23.501: "System Architecture for the 5G System; Stage 2".

[3] 3GPP TS 23.502: "Procedures for the 5G System; Stage 2".

[4] 3GPP TS 29.500: "5G System; Technical Realization of Service Based Architecture; Stage 3".

[5] 3GPP TS 29.501: "5G System; Principles and Guidelines for Services Definition; Stage 3".

[6] OpenAPI: "OpenAPI 3.0.0 Specification", <https://github.com/OAI/OpenAPI-Specification/blob/master/versions/3.0.0.md>.

[7] 3GPP TR 21.900: "Technical Specification Group working methods".

[8] 3GPP TS 33.501: "Security architecture and procedures for 5G system".

[9] IETF RFC 6749: "The OAuth 2.0 Authorization Framework".

[10] 3GPP TS 29.510: "5G System; Network Function Repository Services; Stage 3".

[11] IETF RFC 9113: "HTTP/2".

[12] IETF RFC 8259: "The JavaScript Object Notation (JSON) Data Interchange Format".

[13] IETF RFC 9457: "Problem Details for HTTP APIs".

[14] 3GPP TS 23.288: "Architecture enhancements for 5G System (5GS) to support network data analytics services".

[15] 3GPP TS 29.520: "5G System; Network Data Analytics Services; Stage 3".

[16] 3GPP TS 29.571: "5G System; Common Data Types for Service Based Interfaces; Stage 3".

[17] 3GPP TS 29.508: "5G System; Session Management Event Exposure Service; Stage 3".

[18] 3GPP TS 29.518: "5G System; Access and Mobility Management Services; Stage 3".

[19] 3GPP TS 29.503: "5G System; Unified Data Management Services; Stage 3".

[20] 3GPP TS 29.517: "5G System; Application Function Event Exposure Services; Stage 3".

[21] 3GPP TS 29.591: "5G System; Network Exposure Function Southbound Services; Stage 3".

[22] 3GPP TS 29.122: "T8 reference point for Northbound APIs".

[23] 3GPP TS 29.574: "5G System; Data Collection Coordination Services; Stage 3".

[24] 3GPP TS 29.576: "5G System; Messaging Framework Adaptor Services; Stage 3".

[25] 3GPP TS 29.536: "5G System; Network Slice Admission Control Services; Stage 3".

[26] 3GPP TS 29.564: "5G System; User Plane Function Services; Stage 3".

[27] 3GPP TS 29.515: "5G System; Gateway Mobile Location Services; Stage 3".

\*\*\* Next Change \*\*\*

#### 5.1.2.1 General

HTTP/2, IETF RFC 9113 [11], shall be used as specified in clause 5 of 3GPP TS 29.500 [4].

HTTP/2 shall be transported as specified in clause 5.3 of 3GPP TS 29.500 [4].

The OpenAPI [6] specification of HTTP messages and content bodies for the Nadrf\_DataManagement API is contained in Annex A.

\*\*\* Next Change \*\*\*

##### 5.1.2.2.2 Content type

JSON, IETF RFC 8259 [12], shall be used as content type of the HTTP bodies specified in the present specification as specified in clause 5.4 of 3GPP TS 29.500 [4]. The use of the JSON format shall be signalled by the content type "application/json".

"Problem Details" JSON object shall be used to indicate additional details of the error in a HTTP response body and shall be signalled by the content type "application/problem+json", as defined in IETF RFC 9457 [13].

\*\*\* Next Change \*\*\*

#### 5.2.2.1 General

HTTP/2, IETF RFC 9113 [11], shall be used as specified in clause 5 of 3GPP TS 29.500 [4].

HTTP/2 shall be transported as specified in clause 5.3 of 3GPP TS 29.500 [4].

The OpenAPI [6] specification of HTTP messages and content bodies for the Nadrf\_MLModelManagement API is contained in Annex A.

\*\*\* Next Change \*\*\*

##### 5.2.2.2.2 Content type

JSON, IETF RFC 8259 [12], shall be used as content type of the HTTP bodies specified in the present specification as specified in clause 5.4 of 3GPP TS 29.500 [4]. The use of the JSON format shall be signalled by the content type "application/json".

"Problem Details" JSON object shall be used to indicate additional details of the error in a HTTP response body and shall be signalled by the content type "application/problem+json", as defined in IETF RFC 9457 [13].

\*\*\* End of Changes \*\*\*