3GPP TSG RAN WG1 Meeting #100bis-e R1-20xxxxx

20th April– 30th April 2020

Agenda Item: 7.2.3.2

Source: Qualcomm Incorporated

Title: Summary #1 of 7.2.3.2 - Extensions of RACH occasions and periodicities for backhaul RACH resources

Document for: Discussion and decision

### Introduction

This contribution provides a summary of the proposals for agenda item 7.2.3.2 on the subject of extensions of RACH occasions and periodicities for backhaul RACH resources for planning the email discussion in RAN1 #100bis-e.

### Issues for discussion

There is one contribution [1] on this agenda item which addresses some issues with the current specifications in TS 38.211.

The issues relate to inaccuracies in the following paragraph of TS 38.211:

|  |
| --- |
| For the IAB-MT part of an IAB node, the following applies:  - if the higher-layer parameter *prach-ConfigurationPeriocScaling* is configured, the variable used in of Tables 6.3.3.2-2 to 6.3.3.2-4 shall be replaced by , where and is given by the higher-layer parameter *prach-ConfigurationPeriodScaling* and the IAB node does not expect to be larger than 64;  - if the higher-layer parameter *prach-ConfigurationFrameOffset* is configured, the variable used in of Tables 6.3.3.2-2 to 6.3.3.2-4 shall be replaced by where is given by the higher-layer parameter *prach-ConfigurationFrameOffset*, and ;  - if the higher-layer parameter *prach-ConfigurationSOffset* is configured, the subframe number in Tables 6.3.3.2-2 to 6.3.3.2-3 and the slot number in Table 6.3.3.2-4 shall be replaced by where is the slot or subframe number, is given by the higher-layer parameter *prach-ConfigurationSOffset*, and is the number of subframes in a frame in Tables 6.3.3.2-2 to 6.3.3.2-3 and the number of slots in a frame in Table 6.3.3.2-4. |

Specifically, the main issue is that the text “and is the number of subframes in a frame in Tables 6.3.3.2-2 to 6.3.3.2-3 and the number of slots in a frame in Table 6.3.3.2-4” seems to imply that L is provided in those tables. However, that interpretation would not be accurate and a reader not familiar with the IAB RAN1 context may get confused.

Moreover, a potential issue is that the text “the subframe number in Tables 6.3.3.2-2 to 6.3.3.2-3 and the slot number in Table 6.3.3.2-4 shall be replaced by (s\_n +Δs) mod L” may imply a value replacement in the tables while the previous two paragraphs describe a variable replacement in the equations using values from the tables.

A TP is proposed in [1] to address these issues.

A slightly simpler TP that minimizes the text changes is proposed:

**Proposal 1:**

**Adopt the following TP for section 6.3.3.2 of 38.211:**

|  |
| --- |
| **<**Unchanged text is omitted>  For the IAB-MT part of an IAB node, the following applies:  - if the higher-layer parameter *prach-ConfigurationPeriocScaling* is configured, the variable used in of Tables 6.3.3.2-2 to 6.3.3.2-4 shall be replaced by , where and is given by the higher-layer parameter *prach-ConfigurationPeriodScaling* and the IAB node does not expect to be larger than 64;  - if the higher-layer parameter *prach-ConfigurationFrameOffset* is configured, the variable used in of Tables 6.3.3.2-2 to 6.3.3.2-4 shall be replaced by where is given by the higher-layer parameter *prach-ConfigurationFrameOffset*, and ;  - if the higher-layer parameter *prach-ConfigurationSOffset* is configured, the subframe number from ~~in~~ Tables 6.3.3.2-2 to 6.3.3.2-3 and the slot number from ~~in~~ Table 6.3.3.2-4 shall be replaced by where ~~is the slot or subframe number,~~ is given by the higher-layer parameter *prach-ConfigurationSOffset*, and is the number of subframes in a frame when using ~~in~~ Tables 6.3.3.2-2 to 6.3.3.2-3 and the number of slots in a frame for SCS of 60 KHz when using ~~in~~ Table 6.3.3.2-4.  **<**Unchanged text is omitted> |

Discussion on Proposal 1:

|  |  |  |
| --- | --- | --- |
| **Company** | **Support Proposal 1? [Yes/No]** | **Comments** |
| Qualcomm | Yes | None. |
| ZTE, Sanechips | Yes | None. |
| LG | Yes | None. |
| Ericsson | Yes | None |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

### Conclusion

To be provided after completion of the email discussion.

### References

[1] R1-2001874 – “Remaining issues in IAB PRACH” – ZTE, Sanechips

### Appendix

##### Proposals from contributions:

|  |  |
| --- | --- |
| R1-2001874 | According to the discussion above, we provide the following proposal and text proposals on PRACH occasions of IAB node MT: 6.3.3.2 Mapping to physical resources **<Unchanged text is omitted>**  For the IAB-MT part of an IAB node, the following applies:  - if the higher-layer parameter *prach-ConfigurationPeriocScaling* is configured, the variable used in of Tables 6.3.3.2-2 to 6.3.3.2-4 shall be replaced by , where and is given by the higher-layer parameter *prach-ConfigurationPeriodScaling* and the IAB node does not expect to be larger than 64;  - if the higher-layer parameter *prach-ConfigurationFrameOffset* is configured, the variable used in of Tables 6.3.3.2-2 to 6.3.3.2-4 shall be replaced by where is given by the higher-layer parameter *prach-ConfigurationFrameOffset*, and is the value used in ;  - if the higher-layer parameter *prach-ConfigurationSOffset* is configured, the subframe number ~~in Tables 6.3.3.2-2 to 6.3.3.2-3~~ and the slot number ~~in Table 6.3.3.2-4~~ for PRACH time resources shall be replaced by where  ~~is the slot or subframe number,~~ is given by the higher-layer parameter *prach-ConfigurationSOffset*, and  ~~is the number of subframes in a frame in Tables 6.3.3.2-2 to 6.3.3.2-3 and the number of slots in a frame in Table 6.3.3.2-4.~~  - For subframe number determination, is the subframe number in Tables 6.3.3.2-2 to 6.3.3.2-3 and L equals to 10.  - For slot number determination, is the slot number in Tables 6.3.3.2-4 and L equals to 40. |