**3GPP TSG-RAN WG2 Meeting #110-e *DRAFT\_R2-2005158***

**Online, 01 – 12 June 2020**

|  |
| --- |
| *CR-Form-v12.0* |
| **CHANGE REQUEST** |
|  |
|  | **36.306** | **CR** | **1758** | **rev** | **1** | **Current version:** | **16.0.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **x** | Radio Access Network | **x** | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  | UE radio access capabilities introduction for IIOT WI (CR for 36.306) |
|  |  |
| ***Source to WG:*** | Nokia, Nokia Shanghai Bell |
| ***Source to TSG:*** | R2 |
|  |  |
| ***Work item code:*** | NR\_IIOT-Core |  | ***Date:*** | 2020-05 |
|  |  |  |  |  |
| ***Category:*** | **Cat B** |  | ***Release:*** | Rel-16 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)Rel-12 (Release 12)**Rel-13 (Release 13)Rel-14 (Release 14)Rel-15 (Release 15)Rel-16 (Release 16)* |
|  |  |
| ***Reason for change:*** | Finalization of IIOT WI requires introduction of related radio capabilities. |
|  |  |
| ***Summary of change:*** | CR captures UE radio capabilities related to Ethernet Header Compression agreed as part of IIOT WI. |
|  |  |
| ***Consequences if not approved:*** | UE radio features related to Ethernet Header Compression introdcued as part of NR IIOT WI are not specified and cannot be utilized. |
|  |  |
| ***Clauses affected:*** | 2, 3.3, 4.3 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** | **X** |  |  Other core specifications  | TS 36.300 CR 1276TS 36.323 CR 0278TS 36.331 CR 4228 |
| ***affected:*** |  |  |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  |  |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

*First Modified Subclause*

2 References

The following documents contain provisions which, through reference in this text, constitute provisions of the present document.

- References are either specific (identified by date of publication, edition number, version number, etc.) or non specific.

- For a specific reference, subsequent revisions do not apply.

- For a non-specific reference, the latest version applies. In the case of a reference to a 3GPP document (including a GSM document), a non-specific reference implicitly refers to the latest version of that document *in the same Release as the present document*.

[1] 3GPP TR 21.905: "Vocabulary for 3GPP Specifications".

[2] 3GPP TS 36.323: "Evolved Universal Terrestrial Radio Access (E-UTRA) Packet Data Convergence Protocol (PDCP) specification".

[3] 3GPP TS 36.322: "Evolved Universal Terrestrial Radio Access (E-UTRA) Radio Link Control (RLC) specification".

[4] 3GPP TS 36.321: "Evolved Universal Terrestrial Radio Access (E-UTRA) Medium Access Control (MAC) specification".

[5] 3GPP TS 36.331: "Evolved Universal Terrestrial Radio Access (E-UTRA) Radio Resource Control (RRC) specification".

[6] 3GPP TS 36.101: "Evolved Universal Terrestrial Radio Access (E-UTRA) radio transmission and reception".

[7] IETF RFC 5795: "The RObust Header Compression (ROHC) Framework".

[8] IETF RFC 6846: "RObust Header Compression (ROHC): A Profile for TCP/IP (ROHC-TCP)".

[9] IETF RFC 3095: "RObust Header Compression (RoHC): Framework and four profiles: RTP, UDP, ESP and uncompressed".

[10] IETF RFC 3843: "RObust Header Compression (RoHC): A Compression Profile for IP".

[11] IETF RFC 4815: "RObust Header Compression (ROHC): Corrections and Clarifications to RFC 3095".

[12] IETF RFC 5225: "RObust Header Compression (ROHC) Version 2: Profiles for RTP, UDP, IP, ESP and UDP Lite".

[13] 3GPP TS 36.355: "Evolved Universal Terrestrial Radio Access (E-UTRA) LTE Positioning Protocol (LPP)".

[14] 3GPP TS 36.304: "Evolved Universal Terrestrial Radio Access (E-UTRA); UE Procedures in Idle Mode".

[15] 3GPP TS 37.320: "Universal Terrestrial Radio Access (UTRA) and Evolved Universal Terrestrial Radio Access (E-UTRA); Radio measurement collection for Minimization of Drive Tests (MDT); Overall description; Stage 2".

[16] 3GPP TS 36.133: "Evolved Universal Terrestrial Radio Access (E-UTRA); Requirements for support of radio resource management".

[17] 3GPP TS 36.211: "Evolved Universal Terrestrial Radio Access (E-UTRA); Physical Channels and Modulation".

[18] 3GPP TS 23.401: "General Packet Radio Service (GPRS) enhancements for Evolved Universal Terrestrial Radio Access Network (E-UTRAN) access".

[19] 3GPP TS 23.216: "Single Radio Voice Call Continuity (SRVCC)".

[20] 3GPP TS 25.307: "Requirement on User Equipments (UEs) supporting a release-independent frequency band".

[21] 3GPP TS 24.312: "Access Network Discovery and Selection Function (ANDSF) Management Object (MO)".

[22] 3GPP TS 36.213: "Evolved Universal Terrestrial Radio Access (E-UTRA); Physical layer procedures".

[23] 3GPP TS 36.214: "Evolved Universal Terrestrial Radio Access (E-UTRA); Physical layer - Measurements".

[24] 3GPP TS 23.303: "Proximity-based services (ProSe); Stage 2".

[25] 3GPP TS 36.314: "Evolved Universal Terrestrial Radio Access (E-UTRA); Layer 2- Measurements".

[26] 3GPP TS 36.212: "Evolved Universal Terrestrial Radio Access (E-UTRA); Multiplexing and channel coding".

[27] 3GPP TS 36.307: "Evolved Universal Terrestrial Radio Access (E-UTRA); Requirements on User Equipments (UEs) supporting a release-independent frequency band".

[28] 3GPP TS 24.301: "Non-Access-Stratum (NAS) protocol for Evolved Packet System (EPS); Stage 3".

[29] 3GPP TS 23.285: "Technical Specification Group Services and System Aspects; Architecture enhancements for V2X services".

[30] 3GPP TS 36.300: "Evolved Universal Terrestrial Radio Access (E-UTRA) and Evolved Universal Terrestrial Radio Access (E-UTRAN); Overall description; Stage 2".

[31] 3GPP TS 23.246: "Multimedia Broadcast/Multicast Service (MBMS); Architecture and functional description".

[32] 3GPP TS 38.306 "NR; UE Radio Access Capabilities".

[33] 3GPP TS 38.101-1: "NR User Equipment (UE) radio transmission and reception Part 1: Range 1 Standalone".

[34] 3GPP TS 38.101-2: "NR User Equipment (UE) radio transmission and reception Part 2: Range 2 Standalone".

[35] 3GPP TS 38.331: "NR; Radio Resource Control (RRC) protocol specification".

[36] 3GPP TS 38.215: "NR; Physical layer measurements".

[37] 3GPP TS 38.133: "NR; Requirements for support of radio resource management".

[38] 3GPP TS 37.340: "Evolved Universal Terrestrial Radio Access (E-UTRA) and NR; Multi-connectivity".

[39] 3GPP TS 24.501: "Non-Access-Stratum (NAS) protocol for 5G System (5GS); Stage 3".

[x] 3GPP TS 38.323: "NR; Packet Data Convergence Protocol (PDCP) specification".

*Next Modified Subclause*

## 3.3 Abbreviations

For the purposes of the present document, the abbreviations given in TR 21.905 [1] and the following apply. An abbreviation defined in the present document takes precedence over the definition of the same abbreviation, if any, in TR 21.905 [1].

1xRTT CDMA2000 1x Radio Transmission Technology

ACK Acknowledgement

ACDC Application specific Congestion control for Data Communication

ANDSF Access Network Discovery and Selection Function

ANR Automatic Neighbour Relation

BCCH Broadcast Control Channel

CAS Cell Acquisition Subframes

CFI Control Format Indicator

CG Cell Group

CRS Cell-specific Rerefence Signal

CSG Closed Subscriber Group

CSI Channel State Information

DC Dual Connectivity

DCI Downlink Control Information

DL-SCH Downlink Shared Channel

EHC Ethernet Header Compression

E-UTRA Evolved Universal Terrestrial Radio Access

E-UTRAN Evolved Universal Terrestrial Radio Access Network

FDD Frequency Division Duplex

GERAN GSM/EDGE Radio Access Network

HARQ Hybrid Automatic Repeat Request

HRPD High Rate Packet Data

IRC Interference Rejection Combining

MAC Medium Access Control

MMSE Minimum Mean Squared Error

MO-EDT Mobile Originated Early Data Transmission

MRO Mobility Robustness Optimisation

MT-EDT Mobile Terminated Early Data Transmission

MTSI Multimedia Telephony Service for IMS

MUST MultiUser Superposition Transmission

NAICS Network Assisted Interference Cancellation/Suppression

NB-IoT Narrow Band Internet of Things

OS OFDM Symbol

PCell Primary Cell

PDCCH Physical Downlink Control Channel

PDCP Packet Data Convergence Protocol

PDSCH Physical Downlink Shared Channel

PHR Power Headroom Reporting

ProSe Proximity-based Services

PUCCH Physical Uplink Control Channel

PUR Preconfigured Uplink Resource

PUSCH Physical Uplink Shared Channel

QoE Quality of Experience

RACH Random Access CHannel

RAI Release Assistance Indication

RAT Radio Access Technology

RLC Radio Link Control

ROHC RObust Header Compression

RRC Radio Resource Control

SC-PTM Single Cell Point to Multipoint

SCC Secondary Component Carrier

SCell Secondary Cell

SI System Information

SL Sidelink

SL-DCH Sidelink Discovery CHannel

SL-SCH Sidelink Shared CHannel

SON Self Organizing Networks

SPT Short Processing Time

SR Scheduling Request

SSAC Service Specific Access Control

SSTD SFN and Subframe Timing Difference

STTI Short TTI

TDD Time Division Duplex

TTI Transmission Time Interval

UCI Uplink Control Information

UDC Uplink Data Compression

UE User Equipment

UL-SCH Uplink Shared Channel

UMTS Universal Mobile Telecommunications System

UTRA UMTS Terrestrial Radio Access

V2X Vehicle-to-Everything

WLAN Wireless Local Area Network

*Next Modified Subclause*

4.3 Parameters independent of the field *ue-Category* and *ue-CategoryDL / ue-CategoryUL*

4.3.1 PDCP Parameters

4.3.1.1 *supportedROHC-Profiles*

This field defines which ROHC profiles from the list below are supported by the UE.

- 0x0000 ROHC uncompressed (RFC 5795)

- 0x0001 ROHC RTP (RFC 3095, RFC 4815)

- 0x0002 ROHC UDP (RFC 3095, RFC 4815)

- 0x0003 ROHC ESP (RFC 3095, RFC 4815)

- 0x0004 ROHC IP (RFC 3843, RFC 4815)

- 0x0006 ROHC TCP (RFC 6846)

- 0x0101 ROHCv2 RTP (RFC 5225)

- 0x0102 ROHCv2 UDP (RFC 5225)

- 0x0103 ROHCv2 ESP (RFC 5225)

- 0x0104 ROHCv2 IP (RFC 5225)

A UE that supports one or more of the listed ROHC profiles shall support ROHC profile 0x0000 ROHC uncompressed (RFC 5795).

'IMS capable UEs supporting voice' shall support ROHC profiles 0x0000, 0x0001, 0x0002 and be able to compress and decompress headers of PDCP SDUs at a PDCP SDU rate corresponding to supported IMS voice codecs.

4.3.1.1A *supportedROHC-Profiles-r13*

This field defines which ROHC profiles from the list below are supported by the UE:

- 0x0000 ROHC uncompressed (RFC 5795)

- 0x0002 ROHC UDP (RFC 3095, RFC 4815)

- 0x0003 ROHC ESP (RFC 3095, RFC 4815)

- 0x0004 ROHC IP (RFC 3843, RFC 4815)

- 0x0006 ROHC TCP (RFC 6846)

- 0x0102 ROHCv2 UDP (RFC 5225)

- 0x0103 ROHCv2 ESP (RFC 5225)

- 0x0104 ROHCv2 IP (RFC 5225)

A UE that supports one or more of the listed ROHC profiles shall support ROHC profile 0x0000 ROHC uncompressed (RFC 5795). This field is only applicable if the UE supports S1-U data transfer or User plane CIoT EPS Optimisation, see TS 36.331 [5], and any *ue-Category-NB*.

4.3.1.2 *maxNumberROHC-ContextSessions*

This field defines the maximum number of header compression context sessions supported by the UE, excluding context sessions that leave all headers uncompressed.

4.3.1.2A *maxNumberROHC-ContextSessions-r13*

This field defines the maximum number of header compression context sessions supported by the UE, excluding context sessions that leave all headers uncompressed. This field is only applicable if the UE supports S1-U data transfer or User plane CIoT EPS Optimisation, see TS 36.331 [5], and any *ue-Category-NB*.

4.3.1.3 *pdcp-SN-Extension*

This field defines whether the UE supports 15 bit length of PDCP sequence number as specified in TS 36.323 [2]. It is mandatory for UEs supporting split bearers and UEs supporting 18 bit length of PDCP sequence number.

4.3.1.4 *supportRohcContextContinue*

This field defines whether the UE supports ROHC context continuation operation where the UE does not reset the current ROHC context upon handover.

4.3.1.5 *pdcp-SN-Extension-18bits-r13*

This field defines whether the UE supports 18 bit length of PDCP sequence number as specified in TS 36.323 [2].

4.3.1.6 *supportedUplinkOnlyROHC-Profiles*

This field defines which ROHC profile(s) from the list below are supported in uplink-only ROHC operation by the UE.

- 0x0006 ROHC TCP (RFC 6846)

A UE that supports uplink-only ROHC profile(s) shall support ROHC profile 0x0000 ROHC uncompressed (RFC 5795).

4.3.1.7 *supportedUDC-r15*

This field defines whether the UE supports the uplink data compression operation as specified in TS 36.323 [2].

A UE that supports the uplink data compression operation shall support 8192 bytes for compression buffer per UDC DRB and support up to 2 UDC DRBs.

4.3.1.8 *supportedStandardDic-r15*

This field defines whether the UE supports UL data compression with SIP static dictionary as defined in TS 36.323 [2].

4.3.1.9 *supportedOperatorDic-r15*

This field defines whether the UE supports UL data compression with operator defined dictionary. If UE supports operator defined dictionary, the UE shall report *versionOfDictionary*, the version number of the dictionary, and *associatedPLMN-ID*, the associated PLMN ID of this operator defined dictionary as defined in TS 36.331 [5]. Note this parameter is not required to be present if the UE is in VPLMN. In this release of specification, UE can only support one operator defined dictionary.

4.3.1.7 *pdcp-Duplication-r15*

This field defines whether the UE supports PDCP duplication.

4.3.1.X *ehc-r16*

Indicates that the UE supports Ethernet header compression and decompression using EHC protocol, as specified in TS 36.323 [2] and in Annex A of TS 38.323 [x]. The UE indicating this capability and indicating support for at least one ROHC profile, shall support simultaneous configuration of EHC and ROHC on different DRBs.

4.3.1.X+1 *maxNumberEHC-Contexts-r16*

Defines the maximum number of Ethernet header compression contexts supported by the UE across all DRBs and across UE’s EHC compressor and EHC decompressor. The indicated number defines the number of contexts in addition to CID = "all zeros" as specified in Annex A of TS 38.323 [x].

4.3.1.X+2 *continueEHC-Context-r16*

Indicates that the UE supports EHC context continuation operation where the UE keeps the established EHC context(s) upon PDCP re-establishment, as specified in TS 36.323 [2].

4.3.1.X+2 *jointEHC-ROHC-r16*

Indicates whether the UE supports simultaneous configuration of EHC and ROHC protocols for the same DRB.

*End of changes*