**3GPP TSG-RAN WG2 Meeting #130 R2-250xxxx**

**Saint Julian’s, Malta, 19 – 23 May 2025**

**Title: [DRAFT]** Reply LS on LS on RTP retransmission

**Response to:** R2-2503341 / S4-250739

**Release:** Release 19

**Work Item:** NR\_XR\_Ph3-Core

**Source:** Nokia [TSG RAN WG2]

**To:** TSG SA WG4

**Cc:** TSG SA WG2

**Contact Person:**

#### Name: Benoist Sébire

E-mail Address: benoist.sebire@nokia.com

**Send any reply LS to: 3GPP Liaisons Coordinator,** **mailto:3GPPLiaison@etsi.org**

**Attachments:** -

**1. Overall Description:**

RAN2 would like to thank SA4 for the LS on RTP retransmission. If the source stream and retransmission stream are mapped onto two different QoS flows, they can inherently be treated differently in RAN. This does not require new mechanisms in RAN and can be kept transparent to the RAN. RAN2 did not identify the need for receiving additional application layer retransmission information.

**2. Actions:**

**To SA4 group.**

**ACTION:** RAN2 respectfully asks SA4 to take RAN2 feedback into account.

**3. Date of Next TSG-RAN WG2 Meetings:**

RAN2#131 from 2025-08-25 to 2025-08-29 Bengaluru, IN

RAN2#131bis from 2025-10-13 to 2025-10-17 Prague, CZ