**3GPP TSG-RAN3 Meeting #108-e *R3-203208***

**E-meeting, 01 – 11 June 2020**

|  |
| --- |
| *CR-Form-v12.0* |
| **CHANGE REQUEST** |
|  |
|  | **38.413** | **CR** | **0391** | **rev** | **1** | **Current version:** | **15.7.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network | **x** | Core Network | **x** |

|  |
| --- |
|  |
| ***Title:***  | Selected PLMN ID for untrusted non-3GPP access |
|  |  |
| ***Source to WG:*** | Huawei |
| ***Source to TSG:*** | R3 |
|  |  |
| ***Work item code:*** | NR\_newRAT-Core |  | ***Date:*** | 2020-06-05 |
|  |  |  |  |  |
| ***Category:*** | **F** |  | ***Release:*** | Rel-15 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)Rel-12 (Release 12)**Rel-13 (Release 13)Rel-14 (Release 14)Rel-15 (Release 15)Rel-16 (Release 16)* |
|  |  |
| ***Reason for change:*** | As specificed in TS 23.502, Selected PLMNID should be provided fron RAN to AMF in section 4.12.2.2 step 6, but it is not supported in NGAP specification. |
|  |  |
| ***Summary of change:*** | Introduce Selected PLMN Identity in INITIAL UE MESSAGE message.Impact Analysis:Impact assessment towards the previous version of the specification (same release): This CR has isolated impact with the previous version of the specification (same release) because it corrects the Initial UE Message function only. |
|  |  |
| ***Consequences if not approved:*** | The Selected PLMN ID is not provided to AMF for untrusted non-3GPP access, not aligned with TS23.502. |
|  |  |
| ***Clauses affected:*** | 9.2.5.1, 9.4.4, 9.4.7 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** | **x** |  |  Other core specifications  | TS29.413 CR 0005  |
| ***affected:*** |  | **x** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **x** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** | Rev 1: add Semantics description for the new IE |

***----Start of the First Change----***

#### 9.2.5.1 INITIAL UE MESSAGE

This message is sent by the NG-RAN node to transfer the initial layer 3 message to the AMF over the NG interface.

Direction: NG-RAN node → AMF

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description | Criticality | Assigned Criticality |
| Message Type | M |  | 9.3.1.1 |  | YES | ignore |
| RAN UE NGAP ID | M |  | 9.3.3.2 |  | YES | reject |
| NAS-PDU | M |  | 9.3.3.4 |  | YES | reject |
| User Location Information | M |  | 9.3.1.16 |  | YES | reject |
| RRC Establishment Cause | M |  | 9.3.1.111 |  | YES | ignore |
| 5G-S-TMSI | O |  | 9.3.3.20 |  | YES | reject |
| AMF Set ID | O |  | 9.3.3.12 |  | YES | ignore |
| UE Context Request | O |  | ENUMERATED (requested, ...) |  | YES | ignore |
| Allowed NSSAI | O |  | 9.3.1.31 |  | YES | reject |
| Source to Target AMF Information Reroute | O |  | 9.3.3.27 |  | YES | ignore |
| Selected PLMN Identity | O |  | PLMN Identity9.3.3.5 | Indicates the selected PLMN id for the non-3GPP access. | YES | ignore |

***----Start of the Next Change----***

###

### 9.4.4 PDU Definitions

-- ASN1START

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- PDU definitions for NGAP.

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

NGAP-PDU-Contents {

itu-t (0) identified-organization (4) etsi (0) mobileDomain (0)

ngran-Access (22) modules (3) ngap (1) version1 (1) ngap-PDU-Contents (1) }

DEFINITIONS AUTOMATIC TAGS ::=

BEGIN

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- IE parameter types from other modules.

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

IMPORTS

 AllowedNSSAI,

 AMFName,

**//skip the unchanged part**

 PDUSessionResourceSetupListCxtReq,

 PDUSessionResourceSetupListCxtRes,

 PDUSessionResourceSetupListHOReq,

 PDUSessionResourceSetupListSUReq,

 PDUSessionResourceSetupListSURes,

 PDUSessionResourceSwitchedList,

 PDUSessionResourceToBeSwitchedDLList,

 PDUSessionResourceToReleaseListHOCmd,

 PDUSessionResourceToReleaseListRelCmd,

 PLMNIdentity,

 PLMNSupportList,

 PWSFailedCellIDList,

 RANNodeName,

 RANPagingPriority,

 RANStatusTransfer-TransparentContainer,

 RAN-UE-NGAP-ID,

 RedirectionVoiceFallback,

 RelativeAMFCapacity,

**//skip the unchanged part**

 id-RelativeAMFCapacity,

 id-RepetitionPeriod,

 id-ResetType,

 id-RoutingID,

 id-RRCEstablishmentCause,

 id-RRCInactiveTransitionReportRequest,

 id-RRCState,

 id-SecurityContext,

 id-SecurityKey,

 id-SelectedPLMNIdentity,

 id-SerialNumber,

 id-ServedGUAMIList,

 id-SliceSupportList,

 id-SONConfigurationTransferDL,

 id-SONConfigurationTransferUL,

 id-SourceAMF-UE-NGAP-ID,

 id-SourceToTarget-TransparentContainer,

 id-SourceToTarget-AMFInformationReroute,

 id-SupportedTAList,

 id-TAIListForPaging,

 id-TAIListForRestart,

 id-TargetID,

 id-TargetToSource-TransparentContainer,

 id-TimeToWait,

 id-TraceActivation,

 id-TraceCollectionEntityIPAddress,

 id-UEAggregateMaximumBitRate,

**//skip the unchanged part**

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- INITIAL UE MESSAGE

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

InitialUEMessage ::= SEQUENCE {

 protocolIEs ProtocolIE-Container { {InitialUEMessage-IEs} },

 ...

}

InitialUEMessage-IEs NGAP-PROTOCOL-IES ::= {

 { ID id-RAN-UE-NGAP-ID CRITICALITY reject TYPE RAN-UE-NGAP-ID PRESENCE mandatory }|

 { ID id-NAS-PDU CRITICALITY reject TYPE NAS-PDU PRESENCE mandatory }|

 { ID id-UserLocationInformation CRITICALITY reject TYPE UserLocationInformation PRESENCE mandatory }|

 { ID id-RRCEstablishmentCause CRITICALITY ignore TYPE RRCEstablishmentCause PRESENCE mandatory }|

 { ID id-FiveG-S-TMSI CRITICALITY reject TYPE FiveG-S-TMSI PRESENCE optional }|

 { ID id-AMFSetID CRITICALITY ignore TYPE AMFSetID PRESENCE optional }|

 { ID id-UEContextRequest CRITICALITY ignore TYPE UEContextRequest PRESENCE optional }|

 { ID id-AllowedNSSAI CRITICALITY reject TYPE AllowedNSSAI PRESENCE optional }|

 { ID id-SourceToTarget-AMFInformationReroute CRITICALITY ignore TYPE SourceToTarget-AMFInformationReroute PRESENCE optional }|

 { ID id-SelectedPLMNIdentity CRITICALITY ignore TYPE PLMNIdentity PRESENCE optional },

 ...

}

***----Start of the Next Change----***

### 9.4.7 Constant Definitions

-- ASN1START

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Constant definitions

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

NGAP-Constants {

itu-t (0) identified-organization (4) etsi (0) mobileDomain (0)

ngran-Access (22) modules (3) ngap (1) version1 (1) ngap-Constants (4) }

DEFINITIONS AUTOMATIC TAGS ::=

BEGIN

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- IE parameter types from other modules.

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

**//skip the unchanged part**

 id-CNAssistedRANTuning ProtocolIE-ID ::= 165

 id-CommonNetworkInstance ProtocolIE-ID ::= 166

 id-NGRAN-TNLAssociationToRemoveList ProtocolIE-ID ::= 167

 id-TNLAssociationTransportLayerAddressNGRAN ProtocolIE-ID ::= 168

 id-EndpointIPAddressAndPort ProtocolIE-ID ::= 169

 id-LocationReportingAdditionalInfo ProtocolIE-ID ::= 170

 id-SourceToTarget-AMFInformationReroute ProtocolIE-ID ::= 171

 id-AdditionalULForwardingUPTNLInformation ProtocolIE-ID ::= 172

 id-SCTP-TLAs ProtocolIE-ID ::= 173

 id-SelectedPLMNIdentity ProtocolIE-ID ::= xxx

END

-- ASN1STOP

***----Start of the Next Change----***