**3GPP TSG-RAN3 Meeting #108-e *R3-203718***

**E-meeting, 01 - 11 June 2020**

**Title:** (TP for NR\_IIOT BL CR for TS 38.473): Proposed rapporteur changes to the BL CR

**Source:** Huawei

**Agenda item:** 17.1

**Document for:** Other

# 1. Annex – TP

|  |
| --- |
| **Change Begins** |

#### 9.3.1.XX Reporting Request Type

This IE indicates the type of accurate reference time information reporting to be handled by the gNB-DU.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| Event Type | M |  | ENUMERATED (on demand, periodic, stop, …) |  |
| Report Periodicity Value | C-ifEventTypeisPeriodic |  | INTEGER (0..512, …) | Indicates the periodicity of accurate reference time information report. Unit in radio frame. |
|  |  |  |  |  |

|  |  |
| --- | --- |
| C-ifEventYpeisStop | Explanation |
| ifEventTypeisPeriodic | This IE shall be present if the *Event Type* IE is set to "periodic". |

<Unchanged Texts Omitted>

### 9.4.5 Information Element Definitions

-- ASN1START

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Information Element Definitions

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

<Unchanged Texts Omitted>

ReportingPeriodicityValue ::= INTEGER (0..512, ...)

Periodicity ::= INTEGER (0..640000, ...)

<Unchanged Texts Omitted>

ReportingRequestType ::= SEQUENCE {

 eventType EventType,

 reportingPeriodicityValue ReportingPeriodicityValue OPTIONAL,

 -- C-ifEventTypeisPeriodic: This IE shall be present if the Event Type IE is set to "periodic" in the Event Type IE.

 iE-Extensions ProtocolExtensionContainer { {ReportingRequestType-ExtIEs} } OPTIONAL

}

ReportingRequestType-ExtIEs F1AP-PROTOCOL-EXTENSION ::= {

 ...

}

|  |
| --- |
| **End Change** |