**3GPP TSG-RAN WG3 #111-e R3-211105**

**25 January – 4 February 2021**

**Online**

Agenda Item: 9.3.8.1

Source: Nokia (moderator)

Title: Summary of email Discussion on NG-RAN node behaviour when it receives the Xn Signalling TNL association address at source NG-C side IE

Document for: Approval

# Introduction

**CB: # 97\_SignalingTNLassocAddr**

**- issue is acknowledged, i.e. unclarity in relevant SA2 specs; need to fix this**

**- whether to liaise SA2 now? Attempt LS**

**- where to capture relevant st2 statements? whether to agree XnAP CR now?**

(Nok - moderator)

Summary of offline disc [R3-211105](Inbox%5CR3-211105.zip)

drLS to SA2: [R3-211106](Inbox%5CR3-211106.zip)

# For the Chairman’s Notes

Propose the following:

**Agree following proposals:**

…

**Continue discussion on following:**

# Discussion

Online discussion acknowledged the issue and the fix.

When the target NG-RAN node has an available TNL association towards the TNL address as indicated by the *Signalling TNL association address at source NG-C side* IE, the target NG-RAN node should select the TNL association to create an NGAP UE TNLA binding for the UE. Otherwise, the target NG-RAN node should select other available TNL association towards the same AMF or an AMF from the same AMF set to create an NGAP UE TNLA binding for the UE.

The main question is whether the fix should be captured in the XnAP spec ([2]), or should be captured in the SA2 spec (e.g. TS23.502)

* Option 1: Capture the fix in the XnAP spec, e.g. contribution ([2]) for Rel-15 and mirror CR ([3]) for Rel-16. Also LS SA2 to fix the error in TS23.502
* Option 2: No RAN3 CR. Only LS SA2 to fix the error in TS23.502.

**Q1: Please share your view on the two options above, e.g. the preferred option.**

|  |  |
| --- | --- |
| **Company** | **Comment** |
| Nokia | Option 1 is preferred. If the majority prefer Option 2, we are ok to adopt the majority view. |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |

**Q2: Please share your view on the draft LS to SA2.**

|  |  |
| --- | --- |
| **Company** | **Comment** |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |

**Q3: If company prefer Option 1, please share your comments on the draft CR (based on [2][3])**

|  |  |
| --- | --- |
| **Company** | **Comment** |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |

**Summary:**

*

**Potential Proposal:**

**...**

# Part II…[if needed]

If needed

# References

1. R3-210484, Discussion on NG-RAN node behaviour when it receives the Xn Signalling TNL association address at source NG-C side IE (Nokia, Nokia Shanghai Bell, China Telecom, Huawei)
2. R3-210485, Clarify NG-RAN node behavior upon the reception of the Signalling TNL association address at source NG-C side IE (Nokia, Nokia Shanghai Bell, China Telecom, Huawei)
3. R3-210486, Clarify NG-RAN node behavior upon the reception of the Signalling TNL association address at source NG-C side IE (Nokia, Nokia Shanghai Bell, China Telecom, Huawei)