**3GPP TSG-RAN WG3 #113-eR3-214374**

**Online, 16th - 26th August 2021 was R3-214250**

|  |
| --- |
| *CR-Form-v12.1* |
| **CHANGE REQUEST** |
|  |
|  |  | **CR** |  | **rev** | **3** | **Current version:** |  |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network | **X** | Core Network | **X** |

|  |
| --- |
|  |
| ***Title:***  | Correcting assigned criticality for IEs in transparent handover containers |
|  |  |
| ***Source to WG:*** | , Huawei |
| ***Source to TSG:*** |  |
|  |  |
| ***Work item code:*** | LTE\_feMob-Core |  | ***Date:*** | 2021-08-05 |
|  |  |  |  |  |
| ***Category:*** | **F** |  | ***Release:*** | Rel-16 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-15 (Release 15)Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)* |
|  |  |
| ***Reason for change:*** | The transparent handover containers do not provide means to communicate non-comprehended IEs with criticality set to “reject”. Furthermore, assigning “reject” in a response message should be well justified. |
|  |  |
| ***Summary of change:*** | The criticality for IEs in the transparent handover containers set to “reject” has been changed to “ignore”.Impact Analysis:Impact assessment towards the previous version of the specification (same release): This CR has isolated impact with the previous version of the specification (same release) because it corrects DAPS.The CR is backwards compatible from protocol point of view |
|  |  |
| ***Consequences if not approved:*** | Handover may fail although no functional reasons would exist to let it fail nor protocol means are available to provide information to the peer node why handover was failed. |
|  |  |
| ***Clauses affected:*** | 9.2.1.8, 9.3.4 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** | **X** |  |  Other core specifications  | TS 38.413 CR0641 |
| ***affected:*** |  | **X** |  Test specifications |  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications |  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** | r3: adding co-signing company and linked CRr2: correction of coverpage by MCCr1: re-submission to RAN3#113-er0: submission to RAN3#112-e |

<<<<<<<<<<<<<<<<<<<< First Change >>>>>>>>>>>>>>>>>>>>

#### 9.2.1.8 Target eNB to Source eNB Transparent Container

The *Target eNB to Source eNB Transparent Container* IE is an information element that is produced by the target eNB and is transmitted to the source eNB. For inter-system handovers to E-UTRAN, the IE is transmitted from the target eNB to the external relocation source.

This IE is transparent to EPC.

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description | Criticality | Assigned Criticality |
| RRC Container | M |  | OCTET STRING | Includes the RRC E-UTRA Handover Command message as defined in subclause 10.2.2 of TS 36.331 [16]. | - |  |
| DAPS Response Information List |  | *0..1* |  |  | YES | ignore |
| >DAPS Response Information Item |  | *1 .. <maxnoofE-RABs>* |  |  | EACH | ignore |
| >>E-RAB ID | M |  | 9.2.1.2 |  | - |  |
| >>DAPS Response Information | M |  | 9.2.1.156 | Indicates the response to a requested DAPS Handover | - |  |

|  |  |
| --- | --- |
| **Range bound** | **Explanation** |
| maxnoofE-RABs | Maximum no. of E-RABs for one UE. Value is 256. |

<<<<<<<<<<<<<<<<<<<< Next Change >>>>>>>>>>>>>>>>>>>>

<<<<<<<<<<<<<<<<<<<< Last Change >>>>>>>>>>>>>>>>>>>>

### 9.3.4 Information Element Definitions

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Information Element Definitions

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

<<<<<<<<<<<<<<<<<<<< Unmodified Text omitted >>>>>>>>>>>>>>>>>>>>

TargeteNB-ToSourceeNB-TransparentContainer ::= SEQUENCE {

 rRC-Container RRC-Container,

 iE-Extensions ProtocolExtensionContainer { {TargeteNB-ToSourceeNB-TransparentContainer-ExtIEs} } OPTIONAL,

 ...

}

TargeteNB-ToSourceeNB-TransparentContainer-ExtIEs S1AP-PROTOCOL-EXTENSION ::= {

 { ID id-DAPSResponseInfoList CRITICALITY ignore EXTENSION DAPSResponseInfoList PRESENCE optional},

 ...

}

<<<<<<<<<<<<<<<<<<<< End of Changes >>>>>>>>>>>>>>>>>>>>